(footprint "Micro_Mate-N-Lok_4p_vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 6 0)
		(layer "F.SilkS")
		(uuid "28c42959-8e72-4709-83e0-fbb99eade23c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Micro_Mate-N-Lok_4p_vertical"
		(at 0 -5.75 0)
		(layer "F.Fab")
		(uuid "83616a1b-53cb-4bc4-bfc7-a340c75ffaa4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "717f09b2-37e4-4065-ab9f-bd5b82883500")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "6b792804-3b53-4c15-a045-8be7dc697f38")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "0c97b29a-8a73-4fb2-a424-274df2c8800f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -8.25 1.25)
		(end -7 1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ce87f310-f0ba-406a-b736-4ce38509611a")
	)
	(fp_line
		(start -7 -2.5)
		(end -5.5 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9d599c6e-ce87-40a6-8808-1c09f41e6d87")
	)
	(fp_line
		(start -7 -1.25)
		(end -8.25 -1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f47134a4-be82-4ad4-a1ad-bf72ff4ae546")
	)
	(fp_line
		(start -7 -1.25)
		(end -7 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7867b632-d2fd-4db9-9675-d8279a64bbd8")
	)
	(fp_line
		(start -7 1.25)
		(end -7 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f2227206-4c84-434c-b85d-b3d50163b425")
	)
	(fp_line
		(start -7 2.5)
		(end 7 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c48a8f6a-aabd-46bb-b189-6c52e59ce28e")
	)
	(fp_line
		(start -3.5 -2.5)
		(end -2.5 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9264500c-9af3-4dc7-9fd6-bcf2403182e5")
	)
	(fp_line
		(start -0.5 -3.25)
		(end 0.5 -3.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9eb142f5-c818-4799-9b6e-f56193c12346")
	)
	(fp_line
		(start 2.5 -2.5)
		(end 3.5 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f744641e-4674-436f-97f8-bda7558362c2")
	)
	(fp_line
		(start 5.5 -2.5)
		(end 7 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6d0c9227-9fa4-4fdd-a7a1-f5cf102ac4cd")
	)
	(fp_line
		(start 7 -2.5)
		(end 7 -1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ca04d088-9d6e-44be-a42b-87756ac6b0e4")
	)
	(fp_line
		(start 7 1.25)
		(end 8.25 1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "23416e5d-9e80-4232-bc36-57f7ae89601a")
	)
	(fp_line
		(start 7 2.5)
		(end 7 1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "08f73a32-8b79-4586-8a34-9772d25ce1d2")
	)
	(fp_line
		(start 8.25 -1.25)
		(end 7 -1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b102087c-eb25-4b44-aa8b-3c782cbfd9bc")
	)
	(fp_circle
		(center 8 -3.5)
		(end 8.5 -3.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "89197813-1f34-412e-b0f2-543175929a5d")
	)
	(fp_rect
		(start -10 -4.75)
		(end 10 2.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "2e955124-6939-410c-81be-086896fd0cd7")
	)
	(pad "" smd roundrect
		(at -8.2 0)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "5f7505cc-53a6-463b-b397-33ff845b1ac0")
	)
	(pad "" smd roundrect
		(at 8.2 0)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "a1223b95-aa11-427a-b201-9190a86a68be")
	)
	(pad "1" smd roundrect
		(at 4.5 -3.2)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "e7f989f7-95da-4be3-9e33-743523ae1ee0")
	)
	(pad "2" smd roundrect
		(at 1.5 -3.2)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "35e13391-5257-46f3-93a5-87ffd4e862a4")
	)
	(pad "3" smd roundrect
		(at -1.5 -3.2)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "8a3381a5-19d1-47f5-85b0-cf20b0f3bb61")
	)
	(pad "4" smd roundrect
		(at -4.5 -3.2)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "cc93ecb4-fd7b-48b7-868d-89f294f07c27")
	)
)
