(footprint "SW_Wurth_WS-TOTV_472231010140_WITHLOCKING" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Ø 12 mm Panel Cut-Out Vertical Operation Toggle Switch with Screw Terminal, body 33.7x22.6x29mm, https://www.we-online.com/en/components/products/datasheet/472231010140?ki")
  (tags "THT")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -12.55 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2054d9eb-6276-4212-b6f0-9ee186fc5c60)
  )
  (fp_text value "SW_Wurth_WS-TOTV_472231010140_WITHLOCKING" (at 0 12.55 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a7bfd566-c68f-4329-9cea-a20976cc7c60)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3c251a0e-8478-416b-a0de-c0c4e4b0f589)
  )
  (fp_line (start -16.95 -11.4) (end 16.95 -11.4)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c87672fc-9ac2-4368-97e6-00f424305994))
  (fp_line (start -16.95 11.4) (end -16.95 -11.4)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp da24bf5f-e93a-4ced-a60c-6756b0da9cc7))
  (fp_line (start 16.95 -11.4) (end 16.95 11.4)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9ace5a63-67ea-43b7-9534-4cc915d7d23f))
  (fp_line (start 16.95 11.4) (end -16.95 11.4)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f59abdae-fc15-4282-8b48-46f1f2b8408c))
  (fp_rect (start 17.1 11.55) (end -17.1 -11.55)
    (stroke (width 0.05) (type default)) (fill none) (layer "B.CrtYd") (tstamp 5a3b1380-4d69-4557-81f8-d96ce31b1b35))
  (fp_rect (start 11.35 6.2) (end -6.2 -6.2)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp d2b2b9fc-d05b-4072-82e9-d1b1c650261f))
  (fp_line (start -16.85 -11.3) (end 16.85 -11.3)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp af46c1a6-a323-43d4-8e00-362b6b73e5fb))
  (fp_line (start -16.85 11.3) (end -16.85 -11.3)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3bd940cb-a392-4a50-987f-12bb8abb5460))
  (fp_line (start 16.85 -11.3) (end 16.85 11.3)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e6815902-3b44-4b29-b4f5-71b2cd608017))
  (fp_line (start 16.85 11.3) (end -16.85 11.3)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 31dbfde0-2e83-4a45-bb00-2397ccb399f5))
  (fp_circle (center 0 0) (end -5.95 0)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp ae46732d-6d1b-4fd3-84be-36e696072c46))
  (pad "" np_thru_hole circle (at 0 0) (size 12 12) (drill 12) (layers "F&B.Cu" "*.Mask") (tstamp 7009c851-7df8-46a7-adf5-e1270a540bfb))
  (pad "" np_thru_hole circle (at 9.5 0 180) (size 3.3 3.3) (drill 3.3) (layers "*.Cu" "*.Mask") (tstamp d505d037-2cd1-44ea-b0e3-1b9472f76537))
  (pad "1" thru_hole rect (at -3.81 -2.54 180) (size 1.108 1.108) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp c7d1ff2e-fa3a-40a9-bb5c-da69b42e5499))
  (pad "2" thru_hole circle (at 0 -2.54 180) (size 1.108 1.108) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp 5b6a7004-a58e-4156-9e35-59dc073f7945))
  (pad "3" thru_hole circle (at 3.81 -2.54 180) (size 1.108 1.108) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp f2cd16dd-cc91-4902-b615-03e501de9957))
  (pad "4" thru_hole circle (at -3.81 2.54 180) (size 1.108 1.108) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp 515915d1-0b21-485c-91e7-cd9b57816d04))
  (pad "5" thru_hole circle (at 0 2.54 180) (size 1.108 1.108) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp fc39e761-0d49-42f5-af07-40016e845209))
  (pad "6" thru_hole circle (at 3.81 2.54 180) (size 1.108 1.108) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp a3845d08-ab6b-4e3e-b7d3-69373a12018c))
  (model "${WE_3DMODEL_DIR}/Switch_THT_Wurth.3dshapes/SW_Wurth_WS-TOTV_472231010140.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
