(footprint "SW_Wurth_WS-ROTV_428527520910" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "IP67 Rotary Switch with Cross Type Actuator 10x10 mm, body 10x10x6.5mm, https://www.we-online.com/en/components/products/datasheet/428527520910?ki")
  (tags "THT")
  (attr smd)
  (fp_text reference "REF**" (at 3.81 -3.71 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b90b34b4-5f31-4994-93c3-c5748b052e29)
  )
  (fp_text value "SW_Wurth_WS-ROTV_428527520910" (at 3.81 8.79 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fa703c6b-d9cd-4364-9bdd-05b61a67740b)
  )
  (fp_text user "${REFERENCE}" (at 3.81 2.54 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    (tstamp e79aba0c-f375-4763-8b7e-f5bf076bb661)
  )
  (fp_line (start -1.525 -0.75) (end -1.525 0.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a5b67d16-f5b9-40e9-b7b3-11f38dec8b2b))
  (fp_line (start -1.3 -1.51) (end -0.24 -2.57)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 77115a40-d40d-4113-9c59-ed1eb2f09f88))
  (fp_line (start -1.3 7.65) (end -1.3 -1.51)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 8b33a15b-46a6-4000-938c-4bee9058bf9e))
  (fp_line (start -0.24 -2.57) (end 8.92 -2.57)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 7d0d9574-0341-4af3-8f6f-028362b2daa6))
  (fp_line (start 8.92 -2.57) (end 8.92 7.65)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp aae10fd9-5a49-455b-a016-bf841abd4f81))
  (fp_line (start 8.92 7.65) (end -1.3 7.65)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp c6118058-c965-4f6c-86d9-62ced5f4a53f))
  (fp_rect (start -1.44 -2.71) (end 9.06 7.79)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp df069671-a9d3-47d1-9d3d-9e695ed2a221))
  (fp_line (start -1.19 -1.46) (end -0.19 -2.46)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 332bf321-8038-47c4-ab6b-314e14dc1117))
  (fp_line (start -1.19 -0.75) (end -0.29 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 780ca69e-dfc6-4e5f-b3b4-b75a1ad7d751))
  (fp_line (start -1.19 0.75) (end -0.29 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e644f2d0-1a50-4f21-a053-a9e99969858e))
  (fp_line (start -1.19 7.54) (end -1.19 -1.46)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 584170b3-b94b-44ff-94c2-37595599c4f4))
  (fp_line (start -0.19 -2.46) (end 8.81 -2.46)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp a5f561c0-ff0e-4edc-97b0-b6759778ffa6))
  (fp_line (start 8.81 -2.46) (end 8.81 7.54)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp dec587a8-f447-433d-8038-7fb6839ca97d))
  (fp_line (start 8.81 7.54) (end -1.19 7.54)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp c6548c37-1b1a-41da-9e2c-aff1b9716b3e))
  (pad "1" thru_hole rect (at 0 0) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask") (tstamp c5b6c57e-1cad-4c10-80b3-b4a6a210400d))
  (pad "2" thru_hole circle (at 7.62 5.08) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask") (tstamp ec32eb3c-6138-431a-9848-f39eba41be0a))
  (pad "4" thru_hole circle (at 0 5.08) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 0606fc9d-8e44-43fb-a90a-aa47cf1eb8b1))
  (pad "8" thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 88eb2110-e6a6-4f7e-b529-6e3529c3dcb2))
  (pad "C1" thru_hole circle (at 0 2.54) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask") (tstamp bea492a8-1dab-4b7f-bcc3-789db84b6763))
  (pad "C2" thru_hole circle (at 7.62 2.54) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 3f49c619-5896-4477-a582-f25b8f6c4eab))
  (model "${WE_3DMODEL_DIR}/Switch_THT_Wurth.3dshapes/SW_Wurth_WS-ROTV_428527520910.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
