(footprint "SW_Wurth_WS-TOTV_472221010110_WITHLOCKING" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Ø 12 mm Panel Cut-Out Vertical Operation Toggle Switch with 6.3 mm quick-connect terminal, body 28.8x15.8x29mm, https://www.we-online.com/en/components/products/datasheet/472221010110?ki")
  (tags "THT")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -9.15 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 888f1d7d-e68b-4428-82af-2abc83337f39)
  )
  (fp_text value "SW_Wurth_WS-TOTV_472221010110_WITHLOCKING" (at 0 9.15 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 24fc21ad-22e1-4859-a94e-44ff6f3c31ad)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f2735e98-1cf7-475e-858b-b118875b8602)
  )
  (fp_line (start -14.5 -8) (end 14.5 -8)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d0560b0a-254b-4465-b8b2-543bc534988e))
  (fp_line (start -14.5 8) (end -14.5 -8)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7c2f7dd3-be69-4f8c-946f-57e923f5643d))
  (fp_line (start 14.5 -8) (end 14.5 8)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp cf9f18fb-34af-45fd-a69c-e5eb234b2c15))
  (fp_line (start 14.5 8) (end -14.5 8)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6400d092-efbd-4418-b11d-dae93c2dcb2f))
  (fp_rect (start 14.9 8.4) (end -14.9 -8.4)
    (stroke (width 0.05) (type default)) (fill none) (layer "B.CrtYd") (tstamp 508a3779-b1ae-49ec-b74c-4252bde459a0))
  (fp_rect (start 11.55 6.4) (end -6.4 -6.4)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 62a90b94-c0e6-4509-b25b-97a418c04f55))
  (fp_line (start -14.4 -7.9) (end 14.4 -7.9)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cd51a118-8383-40f9-abe2-b069d93724d8))
  (fp_line (start -14.4 7.9) (end -14.4 -7.9)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fcfed0e7-3f65-40f5-905a-001e64f72f3d))
  (fp_line (start 14.4 -7.9) (end 14.4 7.9)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0e338875-1259-46af-a6a0-022cbb61aad6))
  (fp_line (start 14.4 7.9) (end -14.4 7.9)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7a2c0ee9-71ad-43e2-9ba3-0c94701246f2))
  (fp_circle (center 0 0) (end -5.95 0)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 093d9e4e-f2ec-45d2-94d1-2aec5764837a))
  (pad "" np_thru_hole circle (at 0 0 180) (size 12 12) (drill 12) (layers "*.Cu" "*.Mask") (tstamp 3781a5a8-fd20-4f09-a339-1c7a7d81428e))
  (pad "" np_thru_hole circle (at 9.5 0 180) (size 3.3 3.3) (drill 3.3) (layers "*.Cu" "*.Mask") (tstamp 12671db7-3f62-4d91-b222-56dda0eaa035))
  (pad "1" thru_hole rect (at -3.81 0 180) (size 1.108 1.108) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp 601641b9-382d-477f-912d-04ade32a1e76))
  (pad "2" thru_hole circle (at 0 0 180) (size 1.108 1.108) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp 5effc530-27b4-4706-b104-d7c110ef107a))
  (pad "3" thru_hole circle (at 3.81 0 180) (size 1.108 1.108) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp 2bf850f2-de8b-4b75-a0d5-1b1c7b1f3c2d))
  (model "${WE_3DMODEL_DIR}/Switch_THT_Wurth.3dshapes/SW_Wurth_WS-TOTV_472221010110.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
