(footprint "SW_Wurth_WS-ROTV_428547320910" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "IP67 Rotary Switch with Arrow Type Actuator 7x7 mm, body 7.4x7.4x3.65mm, https://www.we-online.com/en/components/products/datasheet/428547320910?ki")
  (tags "THT")
  (attr smd)
  (fp_text reference "REF**" (at 3.81 -2.41 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2aef3f93-e74b-4b5d-a67f-2986ff0c1d97)
  )
  (fp_text value "SW_Wurth_WS-ROTV_428547320910" (at 3.81 7.49 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 49a4648f-577b-452c-859b-7d32fa65166b)
  )
  (fp_text user "${REFERENCE}" (at 3.81 2.54 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    (tstamp 9a7c6b2e-35a4-4f70-9c6d-7e86e876b9d7)
  )
  (fp_line (start -0.985 -0.65) (end -0.985 0.65)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ea81414e-7432-4396-82b8-4325267aada2))
  (fp_line (start 0 -1.27) (end 0 -0.91)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0b2ab567-3dc8-4753-ba01-c0aeb5905ede))
  (fp_line (start 0 -1.27) (end 7.62 -1.27)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4d95c076-78de-48a2-8c15-589f98b93a9f))
  (fp_line (start 0 0.91) (end 0 1.63)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp e521f0b2-162e-4cf8-8835-2358acb90947))
  (fp_line (start 0 3.45) (end 0 4.17)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6e3b42ee-be54-492c-85ac-3b91fe702d2f))
  (fp_line (start 0 6.35) (end 0 5.99)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8f6a5d84-f772-4d1a-a88a-6a00ddd4bd34))
  (fp_line (start 0 6.35) (end 7.62 6.35)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1701ad37-6863-4982-bd62-53cc9dd3d186))
  (fp_line (start 7.62 -1.27) (end 7.62 -0.91)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8527e9ef-5aa8-46c7-a33a-427157be5e8a))
  (fp_line (start 7.62 0.91) (end 7.62 1.63)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 3ba5505c-d653-4f61-abf1-5cd8c8301843))
  (fp_line (start 7.62 3.45) (end 7.62 4.17)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp cfc9db22-c50a-42a3-9e6a-fe7c0645e47d))
  (fp_line (start 7.62 6.35) (end 7.62 5.99)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c21fefa8-2b6b-4f5a-9b5e-5e3ffee32744))
  (fp_rect (start -0.9 -1.41) (end 8.52 6.49)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp c7ccbce5-a9f4-4f98-a580-425510d50672))
  (fp_line (start 0.11 -0.65) (end 0.89 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dece63c4-fdf5-4c11-a399-074817ecf7ab))
  (fp_line (start 0.11 0.65) (end 0.89 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d573e33c-f5c2-44fd-9bf6-275c92e5768b))
  (fp_rect (start 0.11 -1.16) (end 7.51 6.24)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp e014b504-6cdc-4858-a709-533afdce8064))
  (pad "1" thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 57ddbb1f-a7c0-487d-8680-7a87b4d4588e))
  (pad "2" thru_hole circle (at 7.62 5.08) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp f043c7d9-20e9-44eb-8c5d-f228603bc4e1))
  (pad "4" thru_hole circle (at 0 5.08) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 6877d816-fdba-4bd4-8b44-b7eda002c5ed))
  (pad "8" thru_hole circle (at 7.62 0) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 5c803ca7-5163-4de0-a86d-d0658071c12e))
  (pad "C1" thru_hole circle (at 0 2.54) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp b7b946ca-51ab-461b-aea2-6ee5631dec15))
  (pad "C2" thru_hole circle (at 7.62 2.54) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 19f6ff33-9c9d-4323-a79f-4e8e8a88dc99))
  (model "${WE_3DMODEL_DIR}/Switch_THT_Wurth.3dshapes/SW_Wurth_WS-ROTV_428547320910.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
