(footprint "SW_Wurth_WS-TOTV_472223010110_NOLOCKING" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Ø 12 mm Panel Cut-Out Vertical Operation Toggle Switch with 6.3 mm quick-connect terminal, body 28.8x15.8x29mm, https://www.we-online.com/en/components/products/datasheet/472223010110?ki")
  (tags "THT")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -9.15 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c0ef3f58-c96a-4e32-b823-dae65cf77f3b)
  )
  (fp_text value "SW_Wurth_WS-TOTV_472223010110_NOLOCKING" (at 0 9.15 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 148fb4c8-16a1-4418-b41e-7414d1b9b648)
  )
  (fp_text user "PCB Cutout Area" (at 0 -2.54) (layer "Edge.Cuts")
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    (tstamp d3ce782b-221a-4ccc-b19f-02c6b85e45dd)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cb093514-15c4-42c7-831c-bd36f478cd5b)
  )
  (fp_line (start -14.5 -8) (end 14.5 -8)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp eb3dcfb7-912e-45c7-89a5-e159d1ccec1f))
  (fp_line (start -14.5 8) (end -14.5 -8)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f8f1c8f8-2383-42df-ba93-2065862b9d05))
  (fp_line (start 14.5 -8) (end 14.5 8)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2777b6c4-0d81-4339-899b-1063e56a34a3))
  (fp_line (start 14.5 8) (end -14.5 8)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8819a373-be4b-4c0d-892d-559a85474c64))
  (fp_circle (center 0 0) (end 0.56 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 7a8c9a3e-0c5a-4ab6-a7f3-35c25c6b152e))
  (fp_poly
    (pts
      (arc (start 5.94 -0.85) (mid -6.000664 0) (end 5.94 0.85))
      (xy 5.14 0.85)
      (xy 5.14 -0.85)
    )

    (stroke (width 0.001) (type solid)) (fill none) (layer "Edge.Cuts") (tstamp 104f058e-3c38-4f95-be50-1e28a9b61a0f))
  (fp_rect (start 14.9 8.4) (end -14.9 -8.4)
    (stroke (width 0.05) (type default)) (fill none) (layer "B.CrtYd") (tstamp d65916e9-4fa6-4ef8-a91a-86aa1289e052))
  (fp_circle (center 0 0) (end -6.5 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp a33b1872-b4b7-4f32-808b-40dc74f33234))
  (fp_line (start -14.4 -7.9) (end 14.4 -7.9)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e9298a4b-c45f-4b3c-855b-90c745ca9c5b))
  (fp_line (start -14.4 7.9) (end -14.4 -7.9)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2bb68782-1c97-44a9-bfb9-6ed9ba738fc8))
  (fp_line (start 14.4 -7.9) (end 14.4 7.9)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e746e740-a3fe-4cba-badb-8c0dedfae6c4))
  (fp_line (start 14.4 7.9) (end -14.4 7.9)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ace8d213-a10b-4d6d-8db8-e1148c879dde))
  (fp_circle (center 0 0) (end -6 0)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp c5902e7e-7c83-4a74-9d7e-c4a74d8b2581))
  (pad "1" thru_hole rect (at -3.81 0 180) (size 1.108 1.108) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp b0b00d53-d994-4763-bfb7-4e5b56c3f447))
  (pad "2" thru_hole circle (at 0 0 180) (size 1.108 1.108) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp 9f97c465-155e-4869-8068-f2667000d4f7))
  (pad "3" thru_hole circle (at 3.81 0 180) (size 1.108 1.108) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp 20e7ac1b-9b98-41c7-b973-6c5baa7b3f81))
  (model "${WE_3DMODEL_DIR}/Switch_THT_Wurth.3dshapes/SW_Wurth_WS-TOTV_472223010110.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
