(footprint "SW_Wurth_WS-ROTV_428517310916" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "IP67 Rotary Switch 4x1 Terminal with Arrow Type Actuator 10x10 mm, body 10x10x6.5mm, https://www.we-online.com/en/components/products/datasheet/428517310916?ki")
  (tags "THT")
  (attr smd)
  (fp_text reference "REF**" (at 3.81 -2.44 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 37191f76-038e-4106-93dc-75e99dac0bf4)
  )
  (fp_text value "SW_Wurth_WS-ROTV_428517310916" (at 3.81 10.06 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 98c2b2a3-41f7-4779-bfd7-a7b7c63b4c40)
  )
  (fp_text user "${REFERENCE}" (at 3.81 3.81 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    (tstamp e7a59447-db55-4cc8-af82-38897d343386)
  )
  (fp_line (start -1.525 -0.75) (end -1.525 0.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 30a9451f-4d3b-4bc9-941f-141814ecaa80))
  (fp_line (start -1.3 -1.3) (end 7.86 -1.3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp d62fcf3b-ba5e-449a-937f-30299b3be25c))
  (fp_line (start -1.3 8.92) (end -1.3 -1.3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 2962ec59-74d2-4046-ba59-b55681669c3b))
  (fp_line (start 7.86 -1.3) (end 8.92 -0.24)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 11ab8858-dea4-4b93-ac10-9aa5de5cf9d7))
  (fp_line (start 8.92 -0.24) (end 8.92 8.92)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 3c872f14-4a1c-491d-944c-184891e9916d))
  (fp_line (start 8.92 8.92) (end -1.3 8.92)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 81421cae-744f-4bc1-a38b-68b14d247377))
  (fp_rect (start -1.44 -1.44) (end 9.06 9.06)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp d6f68e61-2d3d-4f0f-b6a3-b43f3be96152))
  (fp_line (start -1.19 -1.19) (end 7.81 -1.19)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 723ed215-042a-490e-b2e4-6aa796d260b8))
  (fp_line (start -1.19 -0.75) (end -0.29 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f66064be-b6f6-4dc4-b650-74455dffa85e))
  (fp_line (start -1.19 0.75) (end -0.29 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8433668c-60b3-4f7f-abbf-d0868bfe4c33))
  (fp_line (start -1.19 8.81) (end -1.19 -1.19)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp efe8c929-faaf-4750-b053-68d887702d8f))
  (fp_line (start 7.81 -1.19) (end 8.81 -0.19)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 7ec4cbdf-a1f8-49fd-9ea2-3495f39b0d8f))
  (fp_line (start 8.81 -0.19) (end 8.81 8.81)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp f7a3d2f6-02b2-4a37-8a6b-13b5358c8c93))
  (fp_line (start 8.81 8.81) (end -1.19 8.81)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 1bb6b320-4a85-46fd-9eb7-38c05554c71e))
  (pad "1" thru_hole rect (at 0 0) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask") (tstamp b2d21331-ada4-411f-9843-fe5304fab372))
  (pad "2" thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 2b7927b6-b9df-4a7e-a303-b3f206b5466c))
  (pad "4" thru_hole circle (at 5.08 0) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 8b53fe41-3245-48fa-9230-9c4aa38aa537))
  (pad "8" thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask") (tstamp ced097d8-4348-41ff-afb4-523b81595949))
  (pad "C" thru_hole circle (at 2.54 7.62) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask") (tstamp a7217d4e-e3b1-47ee-b7ad-ff35193e91c6))
  (model "${WE_3DMODEL_DIR}/Switch_THT_Wurth.3dshapes/SW_Wurth_WS-ROTV_428517310916.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
