(footprint "standard_WE_Quartz"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
	(tags "SMD SMT crystal")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(layer "F.SilkS")
		(uuid "c452c494-fda0-4205-9224-1ab75b383e9e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "standard_WE_Quartz"
		(at 0 2 0)
		(layer "F.Fab")
		(uuid "8d209d78-b899-4125-bec6-811aea420e7b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0e71a2f9-e374-4986-9335-563b6d14042f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "019b1c2c-b11e-4efc-b60d-8da2af912239")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "59621ca5-7fdb-4ffd-8fc9-b38e9f39aba8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.35 -1.15)
		(end -1.35 1.15)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0a3930a8-7834-4aa2-93a1-f8d9b5b6a3bb")
	)
	(fp_line
		(start -1.35 1.15)
		(end 1.35 1.15)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "55526c5f-9d1a-4cd6-a104-8e4d880f3fef")
	)
	(fp_line
		(start -1.4 -1.3)
		(end -1.4 1.3)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "34e63933-552c-48bb-95a7-b84b227a77a6")
	)
	(fp_line
		(start -1.4 1.3)
		(end 1.4 1.3)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "dc92ca90-ea2d-4950-a602-866d97075ba7")
	)
	(fp_line
		(start 1.4 -1.3)
		(end -1.4 -1.3)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e083f58a-71c3-4607-9968-d9dbc3421982")
	)
	(fp_line
		(start 1.4 1.3)
		(end 1.4 -1.3)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2b2e2644-c522-487c-ac4a-20069db06c43")
	)
	(fp_line
		(start -1 -0.7)
		(end -0.9 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8c7409d0-ae20-4cb8-a492-064cc9357d9b")
	)
	(fp_line
		(start -1 0.3)
		(end -0.5 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "db711fe0-1d12-4dc5-b7a1-e37c6b6ba4f9")
	)
	(fp_line
		(start -1 0.7)
		(end -1 -0.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c4e81ffc-7dae-4df1-aada-004c3364ba03")
	)
	(fp_line
		(start -0.9 -0.8)
		(end 0.9 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ef3a8dd1-57dd-48c5-be51-4e69f3027b56")
	)
	(fp_line
		(start -0.9 0.8)
		(end -1 0.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "13ed775b-79d6-44c1-86d9-7c0012c02949")
	)
	(fp_line
		(start 0.9 -0.8)
		(end 1 -0.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ad26dfe8-879b-41f7-82b1-778ba3037a47")
	)
	(fp_line
		(start 0.9 0.8)
		(end -0.9 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5db80ce5-985a-4aec-85dd-82b33b31b3cf")
	)
	(fp_line
		(start 1 -0.7)
		(end 1 0.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ead4fe2e-bb78-4771-9df1-66152da304c3")
	)
	(fp_line
		(start 1 0.7)
		(end 0.9 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a0e73119-5f1a-4020-b5ce-f892e58fa1d8")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "6b43f183-f370-4890-bacb-cec31a1a8e56")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(pad "1" smd rect
		(at -0.7 0.55)
		(size 0.9 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "22d45045-0de8-4c32-a49a-da556a53bbdd")
	)
	(pad "2" smd rect
		(at 0.9 0.55)
		(size 0.9 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "82ee7744-0249-4049-a9ae-bf50a9e86bd3")
	)
	(pad "3" smd rect
		(at 0.9 -0.75)
		(size 0.9 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "1259f0b9-907b-40e6-8ed8-60107d45b13c")
	)
	(pad "4" smd rect
		(at -0.7 -0.75)
		(size 0.9 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "cbc9241c-8606-4c07-9edc-64c2127bb1c2")
	)
	(model "${KIPRJMOD}/KiCAD_Libraries/FaSTTUBe_Crystals.pretty/3d_models/STP_830108178109.stp"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
