(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin 100 80)
    (grid_origin 100 80)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(D101-Pad1)")
  (net 2 "+12V")
  (net 3 "CAN_H")
  (net 4 "GND")
  (net 5 "CAN_L")
  (net 6 "+3V3")
  (net 7 "NRST")
  (net 8 "+5V")
  (net 9 "SCL")
  (net 10 "SDA")
  (net 11 "CAN_Tx")
  (net 12 "CAN_Rx")
  (net 13 "unconnected-(U104-Pad18)")
  (net 14 "unconnected-(U104-Pad19)")
  (net 15 "unconnected-(U103-Pad1)")
  (net 16 "unconnected-(U103-Pad2)")
  (net 17 "unconnected-(U103-Pad3)")
  (net 18 "unconnected-(U104-Pad20)")
  (net 19 "SWDIO")
  (net 20 "unconnected-(U103-Pad6)")
  (net 21 "unconnected-(U103-Pad7)")
  (net 22 "unconnected-(U103-Pad8)")
  (net 23 "unconnected-(U103-Pad9)")
  (net 24 "SWCLK")
  (net 25 "unconnected-(U104-Pad25)")
  (net 26 "unconnected-(U103-Pad12)")
  (net 27 "unconnected-(U103-Pad13)")
  (net 28 "unconnected-(U103-Pad14)")
  (net 29 "unconnected-(U103-Pad15)")
  (net 30 "unconnected-(U103-Pad16)")
  (net 31 "unconnected-(U104-Pad26)")
  (net 32 "unconnected-(U104-Pad27)")
  (net 33 "unconnected-(U104-Pad28)")
  (net 34 "unconnected-(U104-Pad29)")
  (net 35 "unconnected-(U104-Pad30)")
  (net 36 "unconnected-(U104-Pad31)")
  (net 37 "unconnected-(U104-Pad6)")
  (net 38 "unconnected-(U104-Pad7)")
  (net 39 "unconnected-(U104-Pad8)")
  (net 40 "unconnected-(U104-Pad9)")
  (net 41 "unconnected-(U104-Pad10)")
  (net 42 "unconnected-(U104-Pad11)")
  (net 43 "unconnected-(U104-Pad12)")
  (net 44 "unconnected-(U104-Pad13)")
  (net 45 "unconnected-(U104-Pad14)")
  (net 46 "unconnected-(U104-Pad15)")

  (footprint "Package_QFP:LQFP-32_7x7mm_P0.8mm" (layer "F.Cu")
    (tstamp 3836c63d-ca60-4e8e-a339-40980bdccc31)
    (at 127 69 180)
    (descr "LQFP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT358-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/8cee74f1-4063-4176-8a00-9f2e4a72af2e")
    (attr smd)
    (fp_text reference "U104" (at 0 -5.88) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d71f0cba-ee35-4c7d-8e36-e6e267833f6a)
    )
    (fp_text value "STM32F042K6Tx" (at 0 5.88) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f1084b0d-b992-4d4c-9074-1c148a908ad5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c09e814d-1e36-4717-a65f-fd59e1f66b26)
    )
    (fp_line (start -3.61 -3.61) (end -3.61 -3.31)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp da49333a-2ae3-46a7-85b7-29e867a658b0))
    (fp_line (start -3.61 -3.31) (end -4.925 -3.31)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 780076de-fb73-43f2-b5aa-1c95059ff25d))
    (fp_line (start -3.61 3.61) (end -3.61 3.31)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 475da62c-4191-4a2f-9bbc-249deb6d8df7))
    (fp_line (start -3.31 -3.61) (end -3.61 -3.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f7925461-00b9-45fa-8499-f4088f9215ce))
    (fp_line (start -3.31 3.61) (end -3.61 3.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 28a2cccb-c5e0-45cc-a452-0336e0813126))
    (fp_line (start 3.31 -3.61) (end 3.61 -3.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5413e9f0-4b25-4379-9452-5ca9a4dfa90a))
    (fp_line (start 3.31 3.61) (end 3.61 3.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 95ef5708-8f43-434f-b139-406a942bfd2d))
    (fp_line (start 3.61 -3.61) (end 3.61 -3.31)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 64940337-2175-44aa-ab05-e1e92e28a356))
    (fp_line (start 3.61 3.61) (end 3.61 3.31)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 52113c98-6292-463e-b72c-6132239a046a))
    (fp_line (start -5.18 -3.3) (end -5.18 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9a573a5f-16ed-4bac-a9aa-25b5d86e5dd3))
    (fp_line (start -5.18 3.3) (end -5.18 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d77aae80-2ebb-449c-8753-33e439daa878))
    (fp_line (start -3.75 -3.75) (end -3.75 -3.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d5a6653e-3f63-4910-afbc-8ebf149f0d3d))
    (fp_line (start -3.75 -3.3) (end -5.18 -3.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8ef3e563-c1f8-49c5-a3f8-41d88bb0ede4))
    (fp_line (start -3.75 3.3) (end -5.18 3.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 711f8627-5a3c-4396-84c3-6cf951de66c5))
    (fp_line (start -3.75 3.75) (end -3.75 3.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 22ebd635-5838-472e-8b50-03affaba3376))
    (fp_line (start -3.3 -5.18) (end -3.3 -3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dac75ca8-9fd9-4f25-9f22-82af6f3fdad2))
    (fp_line (start -3.3 -3.75) (end -3.75 -3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e6ba8e5a-5295-4d99-9539-f0f44fc4499c))
    (fp_line (start -3.3 3.75) (end -3.75 3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f0172b04-3281-4d5a-a911-69e210ac9ebd))
    (fp_line (start -3.3 5.18) (end -3.3 3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 32d1147a-7743-4223-ab67-db4aaf57b1b9))
    (fp_line (start 0 -5.18) (end -3.3 -5.18)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 518a4131-64e9-4ba1-a442-4691a53e2b81))
    (fp_line (start 0 -5.18) (end 3.3 -5.18)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 94dd7c58-d6bf-4547-ab6b-8de0e37bf355))
    (fp_line (start 0 5.18) (end -3.3 5.18)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 05ce1968-bece-4bfd-ade8-db196bc5f219))
    (fp_line (start 0 5.18) (end 3.3 5.18)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ca51fbb9-a837-4f97-892a-477f8b6ae176))
    (fp_line (start 3.3 -5.18) (end 3.3 -3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f09822c0-7fac-44ce-a87f-366f7a49f250))
    (fp_line (start 3.3 -3.75) (end 3.75 -3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 02b39166-9f7a-4094-8bda-785f43edf3d1))
    (fp_line (start 3.3 3.75) (end 3.75 3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4fffb586-b915-45cc-a9a2-02cc516bb571))
    (fp_line (start 3.3 5.18) (end 3.3 3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8b64729b-0793-4b75-90fd-6a59598d76c3))
    (fp_line (start 3.75 -3.75) (end 3.75 -3.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fed97871-4d75-4194-a3d3-5b61f2a948a5))
    (fp_line (start 3.75 -3.3) (end 5.18 -3.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4f489d12-440e-4cd0-933d-b6701961a6d6))
    (fp_line (start 3.75 3.3) (end 5.18 3.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6a7b2059-d977-4612-95c2-3fe01e6e1434))
    (fp_line (start 3.75 3.75) (end 3.75 3.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 21a00f46-105c-4e4b-a84f-ed4acb136567))
    (fp_line (start 5.18 -3.3) (end 5.18 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b656459b-45a8-4466-bf55-064e0e9bbeb4))
    (fp_line (start 5.18 3.3) (end 5.18 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 97c3e317-415d-4b4f-8101-e9340ae149a3))
    (fp_line (start -3.5 -2.5) (end -2.5 -3.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f6fee84b-bfc5-4648-8e13-9d6d04247a23))
    (fp_line (start -3.5 3.5) (end -3.5 -2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cf646d51-a95b-4acb-92eb-03438484ca3f))
    (fp_line (start -2.5 -3.5) (end 3.5 -3.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77b08f8f-0764-4619-ae58-4700c5781fa2))
    (fp_line (start 3.5 -3.5) (end 3.5 3.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1b097a20-994c-479c-9cb5-f236aa61c8fa))
    (fp_line (start 3.5 3.5) (end -3.5 3.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9273aad3-d4fd-4f46-88b0-3a63b54fdc41))
    (pad "1" smd roundrect (at -4.175 -2.8 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pinfunction "VDD") (pintype "power_in") (tstamp 288344de-d424-4b26-b740-94d18e9ae516))
    (pad "2" smd roundrect (at -4.175 -2 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "SDA") (pinfunction "PF0") (pintype "input") (tstamp eec00f97-9726-4990-8aef-95005e7267d9))
    (pad "3" smd roundrect (at -4.175 -1.2 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "SCL") (pinfunction "PF1") (pintype "input") (tstamp 1ddaccf1-4d0b-44e5-b2c4-dfcabfdb2934))
    (pad "4" smd roundrect (at -4.175 -0.4 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "NRST") (pinfunction "NRST") (pintype "input") (tstamp 58633a66-53a7-4a80-bb62-9adf9147da29))
    (pad "5" smd roundrect (at -4.175 0.4 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pinfunction "VDDA") (pintype "power_in") (tstamp d23ca5ac-bc4d-44a2-90ac-0b3eaa4af6f8))
    (pad "6" smd roundrect (at -4.175 1.2 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "unconnected-(U104-Pad6)") (pinfunction "PA0") (pintype "bidirectional+no_connect") (tstamp 89311f2b-7f4a-4f24-93ac-72dc2e834d5d))
    (pad "7" smd roundrect (at -4.175 2 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "unconnected-(U104-Pad7)") (pinfunction "PA1") (pintype "bidirectional+no_connect") (tstamp a7be9e53-3c65-4638-b824-3d5371aceb9f))
    (pad "8" smd roundrect (at -4.175 2.8 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "unconnected-(U104-Pad8)") (pinfunction "PA2") (pintype "bidirectional+no_connect") (tstamp fac37166-6544-4a5a-8523-75c307b4539f))
    (pad "9" smd roundrect (at -2.8 4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "unconnected-(U104-Pad9)") (pinfunction "PA3") (pintype "bidirectional+no_connect") (tstamp a658002a-8a7e-43ad-8acb-33b00307f4c4))
    (pad "10" smd roundrect (at -2 4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "unconnected-(U104-Pad10)") (pinfunction "PA4") (pintype "bidirectional+no_connect") (tstamp c065b0a4-0b93-48f2-9339-44d26009eb1c))
    (pad "11" smd roundrect (at -1.2 4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "unconnected-(U104-Pad11)") (pinfunction "PA5") (pintype "bidirectional+no_connect") (tstamp 8e73e860-7df5-47ee-9d85-a51cffff4073))
    (pad "12" smd roundrect (at -0.4 4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "unconnected-(U104-Pad12)") (pinfunction "PA6") (pintype "bidirectional+no_connect") (tstamp 9a1807dc-d64a-4457-9c2b-93b6612c3b2e))
    (pad "13" smd roundrect (at 0.4 4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "unconnected-(U104-Pad13)") (pinfunction "PA7") (pintype "bidirectional+no_connect") (tstamp 59e03393-006d-471e-9536-bbbd75e54503))
    (pad "14" smd roundrect (at 1.2 4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "unconnected-(U104-Pad14)") (pinfunction "PB0") (pintype "bidirectional+no_connect") (tstamp bc90f0c0-612e-411d-9c41-1a8ebb2b39fc))
    (pad "15" smd roundrect (at 2 4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "unconnected-(U104-Pad15)") (pinfunction "PB1") (pintype "bidirectional+no_connect") (tstamp e09508cd-85e8-48bb-9bcb-9bab32279ab6))
    (pad "16" smd roundrect (at 2.8 4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp d7cdfc88-84f0-4354-8fda-98af7b5493ec))
    (pad "17" smd roundrect (at 4.175 2.8 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pinfunction "VDDIO2") (pintype "power_in") (tstamp 86ed86f4-0151-45c5-905f-b4a048144531))
    (pad "18" smd roundrect (at 4.175 2 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "unconnected-(U104-Pad18)") (pinfunction "PA8") (pintype "bidirectional+no_connect") (tstamp 77a2b2d1-2483-4c81-b108-6030d548a09e))
    (pad "19" smd roundrect (at 4.175 1.2 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "unconnected-(U104-Pad19)") (pinfunction "PA9") (pintype "bidirectional+no_connect") (tstamp 9cb160c0-5456-4bd7-aa7f-b9388d25eb35))
    (pad "20" smd roundrect (at 4.175 0.4 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "unconnected-(U104-Pad20)") (pinfunction "PA10") (pintype "bidirectional+no_connect") (tstamp 66749c6a-b16f-43be-bab1-76caa7a8a44a))
    (pad "21" smd roundrect (at 4.175 -0.4 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "CAN_Rx") (pinfunction "PA11") (pintype "bidirectional") (tstamp 9ee66366-9074-4bc0-8447-8c0b7199acdf))
    (pad "22" smd roundrect (at 4.175 -1.2 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "CAN_Tx") (pinfunction "PA12") (pintype "bidirectional") (tstamp 06b57733-f545-49fc-900f-f90ae9b9047c))
    (pad "23" smd roundrect (at 4.175 -2 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "SWDIO") (pinfunction "PA13") (pintype "bidirectional") (tstamp 0d33a0a3-6701-41b8-8040-7340c4d8cd33))
    (pad "24" smd roundrect (at 4.175 -2.8 180) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "SWCLK") (pinfunction "PA14") (pintype "bidirectional") (tstamp b2837d6b-6cc1-45c4-aa75-fd2bb220208e))
    (pad "25" smd roundrect (at 2.8 -4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "unconnected-(U104-Pad25)") (pinfunction "PA15") (pintype "bidirectional") (tstamp 0bb36be2-ca53-49e2-aeb3-4c5728e3d819))
    (pad "26" smd roundrect (at 2 -4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "unconnected-(U104-Pad26)") (pinfunction "PB3") (pintype "bidirectional+no_connect") (tstamp a0fa8234-8777-4a66-8b79-9ecbb37d6605))
    (pad "27" smd roundrect (at 1.2 -4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "unconnected-(U104-Pad27)") (pinfunction "PB4") (pintype "bidirectional+no_connect") (tstamp 33aa4306-27d6-4090-96fe-2e0a2a713e0b))
    (pad "28" smd roundrect (at 0.4 -4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "unconnected-(U104-Pad28)") (pinfunction "PB5") (pintype "bidirectional+no_connect") (tstamp a631a287-dbe8-4491-9924-f1eeb226bfe0))
    (pad "29" smd roundrect (at -0.4 -4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "unconnected-(U104-Pad29)") (pinfunction "PB6") (pintype "bidirectional+no_connect") (tstamp 89bc2a9a-0459-4374-90b7-e699bb20f381))
    (pad "30" smd roundrect (at -1.2 -4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "unconnected-(U104-Pad30)") (pinfunction "PB7") (pintype "bidirectional+no_connect") (tstamp 956ad4a4-cb8d-4eef-aba4-03ec6d18e652))
    (pad "31" smd roundrect (at -2 -4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "unconnected-(U104-Pad31)") (pinfunction "PB8") (pintype "bidirectional+no_connect") (tstamp 1e3e2138-6822-4c2d-8218-89e25ffe3f06))
    (pad "32" smd roundrect (at -2.8 -4.175 180) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "VSSA") (pintype "power_in") (tstamp e7987f0c-e4c6-4aae-a5d6-e1cfea057719))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-32_7x7mm_P0.8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tstamp 58a29587-ce99-4765-b407-30c1ea49813b)
    (at 114 70 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/f9790b8d-d8b1-4ec5-b707-7beaab2f7d75")
    (attr smd)
    (fp_text reference "U102" (at 0 -3.4) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f23aaf25-de61-4f0e-9770-0b4e07746fe6)
    )
    (fp_text value "TLE9351VSJ" (at 0 3.4) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 75ada5c7-eed3-466b-a900-bb7cf3da6f9e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.98 0.98) (thickness 0.15)))
      (tstamp 09fb80d2-b024-4766-bca5-51e910d26f69)
    )
    (fp_line (start 0 -2.56) (end -3.45 -2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 56f922ba-5e6c-4b39-98b8-ceef758779a3))
    (fp_line (start 0 -2.56) (end 1.95 -2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 43ca08d4-846a-41b1-a610-aa6c41c9f133))
    (fp_line (start 0 2.56) (end -1.95 2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c933003a-40a8-41cc-a69c-ec19f80cd86d))
    (fp_line (start 0 2.56) (end 1.95 2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a8cefac6-64e1-41d0-bc58-04e647fd0fde))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 39ac7e3c-47f1-43e5-b70d-8dfebc468916))
    (fp_line (start -3.7 2.7) (end 3.7 2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5423c8e8-edb6-4a4c-b102-71ca45602660))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8659c80d-80a2-43b9-ad9c-32ad48891220))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e1f19822-404e-437b-a507-e38cc4c0bfe0))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 526a7a5e-afe2-4029-a038-8c14d846f3f2))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b0bd4229-67bb-4dc7-9d0c-fc6ab8405f53))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 908ce94b-b837-4c84-b759-ec4fbb006eea))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 50e6b88c-1bd3-4928-86fd-758de4de04a3))
    (fp_line (start 1.95 2.45) (end -1.95 2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cd48f1a3-c9ad-4bac-abff-bd98a26719eb))
    (pad "1" smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "CAN_Tx") (pinfunction "TXD") (pintype "input") (tstamp 73ede880-e7f5-4d7b-b9cb-33e82f1b044f))
    (pad "2" smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp aeeba41f-21f1-411c-816e-2bda876a1c79))
    (pad "3" smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+5V") (pinfunction "VDD") (pintype "power_in") (tstamp 06cccf2c-d0d0-41ad-bc61-a0c3e7cbae93))
    (pad "4" smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "CAN_Rx") (pinfunction "RXD") (pintype "output") (tstamp 51ce9675-eb70-4a97-98fd-269bf17eea73))
    (pad "5" smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pinfunction "Vio") (pintype "power_in") (tstamp d9b1315d-9c8a-4956-90df-e5669cf68010))
    (pad "6" smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "CAN_L") (pinfunction "CANL") (pintype "bidirectional") (tstamp 292ce6ba-0c6b-4913-be49-83f41145002d))
    (pad "7" smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "CAN_H") (pinfunction "CANH") (pintype "bidirectional") (tstamp 6ef5f8e0-5c2d-4349-9162-179c7c438d89))
    (pad "8" smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "STBY") (pintype "input") (tstamp 2d7fbff7-ad9e-4962-b4e0-56a226f3dd6a))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SSU_parts:SM7000_SOIC-16" (layer "F.Cu")
    (tstamp b37ba0e4-c660-44d5-bd24-47ff6d2ba9c7)
    (at 142 69)
    (tags "SOIC SO")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/d7122615-17b0-4821-b4c3-bdf15686e5b4")
    (attr smd)
    (fp_text reference "U103" (at 0 -6.1) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a4d49e7c-3f1b-4d80-bed7-772a82216d80)
    )
    (fp_text value "SM7331" (at 0 6.1) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 14fc535c-cb89-48aa-90fe-76e1fd47f505)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ce1926e7-aefc-4410-8ad7-0050d6aebd28)
    )
    (fp_line (start -3.86 -5.26) (end -3.86 -5.005)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7bafe9bc-eba9-4810-a855-8b4f34bb53ef))
    (fp_line (start -3.86 -5.005) (end -5.675 -5.005)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 466f8d1c-c448-4a97-87ec-4e94847952fc))
    (fp_line (start -3.86 5.26) (end -3.86 5.005)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1c72f17e-d445-4a58-842c-0dfdfce350d3))
    (fp_line (start 0 -5.26) (end -3.86 -5.26)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7f4c333e-95dd-4f0c-b8a5-bc57a1ff22fb))
    (fp_line (start 0 -5.26) (end 3.86 -5.26)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 594eb499-401a-4092-9a2b-1cc8f8989e5b))
    (fp_line (start 0 5.26) (end -3.86 5.26)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 22f1a18b-d140-451a-a871-4c11294da049))
    (fp_line (start 0 5.26) (end 3.86 5.26)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e8a5d0de-f294-42b4-a32d-95b01f36190d))
    (fp_line (start 3.86 -5.26) (end 3.86 -5.005)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7f251369-eace-44ab-848c-cd3c5957381c))
    (fp_line (start 3.86 5.26) (end 3.86 5.005)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 543a1648-5784-4e1c-9576-bc01c6ff98bf))
    (fp_line (start -5.93 -5.4) (end -5.93 5.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a3a4ba60-3271-4e9a-ba37-9a84bcaf9db5))
    (fp_line (start -5.93 5.4) (end 5.93 5.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ec5e2d7d-3bc6-4fcb-8261-5aceb45c3c19))
    (fp_line (start 5.93 -5.4) (end -5.93 -5.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2c913718-efbb-4ec8-bb76-bae88d46ed51))
    (fp_line (start 5.93 5.4) (end 5.93 -5.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 47472735-41ec-4096-96fb-ce611f148c4c))
    (fp_line (start -3.75 -4.15) (end -2.75 -5.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 947acefe-ac33-4206-9de3-25b50b4731dd))
    (fp_line (start -3.75 5.15) (end -3.75 -4.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1b0fa014-c61e-4314-8f3d-160bae26aa4c))
    (fp_line (start -2.75 -5.15) (end 3.75 -5.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f75ebc7d-c37e-40c2-a424-54729f414b88))
    (fp_line (start 3.75 -5.15) (end 3.75 5.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ec464e2c-70c1-4b51-8600-7384ed6e411a))
    (fp_line (start 3.75 5.15) (end -3.75 5.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a02008a9-68e1-4709-bfc0-24c27997889b))
    (pad "1" smd roundrect (at -4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "unconnected-(U103-Pad1)") (pintype "no_connect") (tstamp c484a812-1402-4e4a-b9af-2e216b21f631))
    (pad "2" smd roundrect (at -4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "unconnected-(U103-Pad2)") (pintype "no_connect") (tstamp 250e48fb-e2d3-44be-a21e-1a17c0d65000))
    (pad "3" smd roundrect (at -4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "unconnected-(U103-Pad3)") (pintype "no_connect") (tstamp 1418a8af-ecf9-4c29-a7a3-d0ed1e478705))
    (pad "4" smd roundrect (at -4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp fb134e24-116f-4c1a-a910-69e228b2dca7))
    (pad "5" smd roundrect (at -4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pinfunction "VDD") (pintype "power_in") (tstamp ab1e0f05-b1ba-418b-9e43-ba5776957f76))
    (pad "6" smd roundrect (at -4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "unconnected-(U103-Pad6)") (pintype "no_connect") (tstamp ada0013d-cfe2-4fa3-ae62-0cfc7e1da447))
    (pad "7" smd roundrect (at -4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "unconnected-(U103-Pad7)") (pintype "no_connect") (tstamp c8a3bad8-b631-46f3-ad1c-65cbb9e97856))
    (pad "8" smd roundrect (at -4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "unconnected-(U103-Pad8)") (pintype "no_connect") (tstamp 819f78e6-941f-4dad-85f1-b4c7c6b3f0f2))
    (pad "9" smd roundrect (at 4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "unconnected-(U103-Pad9)") (pintype "no_connect") (tstamp e99125d6-a0ca-4b37-842b-335296080c6e))
    (pad "10" smd roundrect (at 4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "SDA") (pinfunction "SDA") (pintype "bidirectional") (tstamp f69224be-c98a-48ad-a04c-1caaa0418333))
    (pad "11" smd roundrect (at 4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "SCL") (pinfunction "SCL") (pintype "input") (tstamp 25f1074a-6ae7-40ed-8106-5e5622cabe99))
    (pad "12" smd roundrect (at 4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "unconnected-(U103-Pad12)") (pintype "no_connect") (tstamp 36709ce8-feaf-4ca8-a999-4108fb101352))
    (pad "13" smd roundrect (at 4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "unconnected-(U103-Pad13)") (pintype "no_connect") (tstamp 078044b2-8672-471f-8af0-713545e8135d))
    (pad "14" smd roundrect (at 4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "unconnected-(U103-Pad14)") (pintype "no_connect") (tstamp c873fbd2-c35e-4523-8311-de379b125b9d))
    (pad "15" smd roundrect (at 4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "unconnected-(U103-Pad15)") (pintype "no_connect") (tstamp 75288219-cb62-4584-bfee-979eec5f882a))
    (pad "16" smd roundrect (at 4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "unconnected-(U103-Pad16)") (pintype "no_connect") (tstamp 179b931a-ee6e-4f42-a650-8fcc15be33cf))
    (model "${KIPRJMOD}/SSU_parts.pretty/3d_models/c-7331-bce-s-001-000-1-3d.stp"
      (offset (xyz 0 0 9.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (footprint "FaSTTUBe_connectors:M8_718_4pin_horizontal" (layer "F.Cu")
    (tstamp d3006e26-11be-4e7f-bb12-87a5d58c58e2)
    (at 105 70 -90)
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/221070d2-097a-4eec-8eb2-3f9858d8c92f")
    (attr through_hole)
    (fp_text reference "J101" (at 0 -4.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f3c28ff0-c3be-47ce-bf6f-f3061324a07d)
    )
    (fp_text value "M8_4pin_horizontal" (at 0 -7.62 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c665bf8f-ade8-4a9d-95ae-f4e3ccaa66bf)
    )
    (fp_line (start -6.5 7.5) (end -6.5 2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dc00fa94-a583-43b2-92cf-d179c920f4b4))
    (fp_line (start -5 16.5) (end -5 7.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a5c7f988-1d57-48d4-82d1-1deaeac9e184))
    (fp_line (start 5 7.5) (end 5 16.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 82a9a530-e248-4dc9-896c-25f6d73fe113))
    (fp_line (start 5 16.5) (end -5 16.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 159574a9-ecec-48bb-adb0-3dc9e65d4e79))
    (fp_line (start 6.5 2) (end 6.5 7.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp becc5b0d-0352-4ad7-ac5e-da033ca0b239))
    (fp_line (start 6.5 7.5) (end -6.5 7.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 853b4aa5-bf64-4f10-b1c5-492731c47e3b))
    (fp_rect (start -8.5 -3) (end 8.5 17.5)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 68d14432-223b-47bb-bd26-18873cfb3df2))
    (fp_line (start -6.5 7.5) (end -6.5 -3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5a1ce9b7-22a6-4b53-b971-3e729d539c8a))
    (fp_line (start -5 7.5) (end -6.5 7.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1cd4cd25-b3d1-4eb2-9ee3-b812e12c968e))
    (fp_line (start -5 7.5) (end -5 16.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 50d6612f-7f92-41c4-9e0a-c8c46e77f4d3))
    (fp_line (start -5 8.5) (end 5 8.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fe2c9782-2ff0-473c-98b0-ea9a985143fb))
    (fp_line (start -5 9) (end 5 8.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 97cc39d8-c871-4e37-a9ca-8f3a0ea043e7))
    (fp_line (start -5 10) (end 5 9.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ed2acee5-b6b0-4723-bb74-ad84b2a662e5))
    (fp_line (start -5 11) (end 5 10.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f7a980e1-d757-405b-965e-cb3c9b1ceca1))
    (fp_line (start -5 12) (end 5 11.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ca221485-8dbb-436e-8b3e-94c2d532aee3))
    (fp_line (start -5 13) (end 5 12.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3a2b4e4a-e4df-4836-8ba6-f50f59704c20))
    (fp_line (start -5 14) (end 5 13.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5bf810e2-0301-40b2-b0db-351f308659e8))
    (fp_line (start -5 15) (end 5 14.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4d44b129-c661-445a-acd1-16280b0de7da))
    (fp_line (start -5 16) (end 5 15.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c195be24-c988-452d-b72d-6611cbe671f7))
    (fp_line (start -5 16.5) (end 5 16.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 81ee098e-cdb0-4a5b-b358-35fb3f1d56ba))
    (fp_line (start 5 7.5) (end 6.5 7.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5351e629-ee47-4afd-b6e5-171421799e39))
    (fp_line (start 5 16.5) (end 5 7.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ba3030b2-37eb-4eb2-b7ee-c2f135251592))
    (fp_line (start 6.5 -3) (end -6.5 -3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a064c737-c686-4181-95db-c4c0eab13acb))
    (fp_line (start 6.5 7.5) (end 6.5 -3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2fdba96d-8ce8-4d3e-9e54-485e4b754b6d))
    (pad "1" thru_hole circle (at 1.7 0 270) (size 1.8 1.8) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D101-Pad1)") (pintype "passive") (tstamp 4fbf7295-52ca-4bf6-b81b-f54f8903681f))
    (pad "2" thru_hole circle (at 1.075 -1.95 270) (size 1.8 1.8) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 3 "CAN_H") (pintype "passive") (tstamp 98a311ac-38c5-418c-9c79-a5650558a468))
    (pad "3" thru_hole circle (at -1.7 0 270) (size 1.8 1.8) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pintype "passive") (tstamp 462f3238-fbc0-42d6-b76e-a63d29cc32e1))
    (pad "4" thru_hole circle (at -1.075 -1.95 270) (size 1.8 1.8) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 5 "CAN_L") (pintype "passive") (tstamp 0887e962-8f08-410d-9589-9308e22a7936))
    (pad "5" thru_hole circle (at -6.25 -0.5 270) (size 4 4) (drill 3) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pintype "passive") (tstamp 24edf58e-a5f8-4553-99c5-1a11459c3da5))
    (pad "5" thru_hole circle (at 6.25 -0.5 270) (size 4 4) (drill 3) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pintype "passive") (tstamp e4d2c258-274a-4398-b6a0-528d81ed8508))
    (model "${KIPRJMOD}/FT_libraries/FaSTTUBe_connectors.pretty/3d_models/M8_718_4pin_horizontal.stp"
      (offset (xyz 0 -2.65 6.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 90))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tstamp 096430c7-4642-4dae-bd6a-55fa18716ff7)
    (at 133.745 71.01 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/8e7dab79-cde7-492b-b9fd-12734ba0b893")
    (attr smd)
    (fp_text reference "C106" (at 0 1.43) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b72aaacf-4683-4df4-9e60-1a4b5785f973)
    )
    (fp_text value "100nF" (at 0 -1.43) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c8f52e79-1c85-4d36-abb4-161a4b988f81)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 1536a9db-5598-466b-a288-cb0c5770380a)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9c6b6a16-9b62-44e4-a22e-f145da2ae51d))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 267773a4-a2c0-4ca8-aaf8-96a2057e4fca))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e0fb141f-ab47-4acb-8b68-0bcddb2d7b34))
    (fp_line (start -1.48 0.73) (end 1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7c2e2eac-a58d-436d-b4b6-f12f3dce2920))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4195ec14-3bf5-4e68-87e2-0a491afa3525))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 72725c0e-7c55-454f-96ea-76e2f84cd5a5))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d630dcee-a3a9-4a04-97d4-d562419390a6))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d1663e97-6d89-466e-adc3-1c7d78b891e4))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bbfdf9c2-1fe0-4411-857d-4b555d7af160))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1d23a639-db64-4ae1-969f-8fb1d06e9d04))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pintype "passive") (tstamp 8f776595-7e2f-4ccf-b66f-8fcdf34a12ae))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 74c06c3f-ef67-4f23-a6ae-1802a20c59af))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tstamp 09ab9b2a-26ef-4942-ba61-f8a6673867aa)
    (at 111 74 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/188da065-3e29-4072-be10-31183ac43e16")
    (attr smd)
    (fp_text reference "D101" (at 0 2.4 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c36de2cd-62e2-4141-94ed-8598a4021bc0)
    )
    (fp_text value "BAT54S" (at 0 -2.4 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d0583253-7f1c-498c-afba-93bf9b28c781)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.32 0.32) (thickness 0.05)) (justify mirror))
      (tstamp debb48c2-0606-4abf-b967-c5cd55bd0d6c)
    )
    (fp_line (start 0 -1.56) (end -0.65 -1.56)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d3349b0a-8f2b-4222-bb13-fa4f0f887f4d))
    (fp_line (start 0 -1.56) (end 0.65 -1.56)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 84aac022-880b-473d-82ad-f2827a88892f))
    (fp_line (start 0 1.56) (end -1.675 1.56)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b4501435-1b74-4814-ac8d-457d48a8c57b))
    (fp_line (start 0 1.56) (end 0.65 1.56)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ef855f52-01db-4405-9940-c5f27401f345))
    (fp_line (start -1.92 -1.7) (end 1.92 -1.7)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4821a0f1-0757-49b5-bc91-a0ccf3e9f548))
    (fp_line (start -1.92 1.7) (end -1.92 -1.7)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a8f15f81-c64f-4a6a-8184-eabd4f5daa6f))
    (fp_line (start 1.92 -1.7) (end 1.92 1.7)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp bdd60e70-d069-432f-96bc-1e17050cb723))
    (fp_line (start 1.92 1.7) (end -1.92 1.7)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9e50feee-fd1e-48c9-aa44-dd6062da7f84))
    (fp_line (start -0.65 -1.45) (end -0.65 1.125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp feb38b83-6d1c-4038-a568-147252bfbe12))
    (fp_line (start -0.65 1.125) (end -0.325 1.45)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8217ca7d-977c-4985-a684-eea82e5113b4))
    (fp_line (start -0.325 1.45) (end 0.65 1.45)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1f3dd671-b973-4373-871e-23d23284bfad))
    (fp_line (start 0.65 -1.45) (end -0.65 -1.45)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d039718a-5f93-4d2d-b957-a40b11652989))
    (fp_line (start 0.65 1.45) (end 0.65 -1.45)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 51957904-d257-41c5-8124-dcc959977230))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(D101-Pad1)") (pintype "passive") (tstamp 0270c5c4-c68e-47b7-a6f1-50651981be2d))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "+12V") (pintype "passive") (tstamp 73917165-0d82-4691-91ca-2eb1b8bbe05e))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "+12V") (pintype "passive") (tstamp 2923d83c-3334-4b85-acfa-e9f2eb6f5eb5))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tstamp 13ee48b4-acdb-42d5-98e7-1f42231ad494)
    (at 137.725 68.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/20af30d6-dfaf-4a69-b935-e03497165543")
    (attr smd)
    (fp_text reference "C107" (at 0 1.43) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0d5168d0-f702-4a2a-82cd-d4cb9d3b9c60)
    )
    (fp_text value "100nF" (at 0 -1.43) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ecab30c4-546c-46da-8332-d218e09ac3ff)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp f20d5e2e-ece3-47e5-8160-12899cb8fddd)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp cde3b9d0-093e-498f-9000-b98af9c727a5))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3a42bce0-7657-48ba-87fb-f076f875d51e))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 94ade9c6-2ad4-4cf9-9c37-4d26de34f693))
    (fp_line (start -1.48 0.73) (end 1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 38b9ad92-1088-49ca-b5a8-49fe3e681f71))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2d38c491-1714-40e1-9666-09f1510e90ab))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1123e6a7-a30b-4196-a686-bcb5d98b0d05))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 99c7eb7c-a47e-40e7-ace7-a2d71007b07e))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 54f22ccb-d5ec-4e2b-8713-604575a5214e))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ceec7167-0834-4472-b45d-d666f60ac721))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 56569bd6-7178-44f0-bdce-f871566a1c1e))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pintype "passive") (tstamp bdc38e36-b9b1-46ba-865e-279da74e8098))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 7fa8a056-ce6b-467d-ba4f-e8fe61828733))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tstamp 25de8be3-f93a-440d-b827-58d13e33763b)
    (at 137.755 73.52 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/618e1e72-1c22-4784-8172-4b569d836999")
    (attr smd)
    (fp_text reference "C105" (at 0 1.43) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 15916668-965b-4fbb-90fe-6e8ea3eea0f3)
    )
    (fp_text value "100nF" (at 0 -1.43) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9349a2a6-9472-46c3-9139-de96a88c881b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp bc2ae153-e72d-4f62-822b-b8938bf03172)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp fd05c247-250a-4625-9a4c-ca0bf2aa3a5f))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5888e6c7-18c8-4d73-a59f-605e9b3f591b))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 223fcaa1-c8ee-4c8b-90b9-90bbdf7dc635))
    (fp_line (start -1.48 0.73) (end 1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2d89ce0b-4fd1-4caa-867e-d317d0ba5928))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 77bd4070-52a6-475f-bd6a-fadffe842c09))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 446bf39e-f653-4e79-b238-d1778bb60fa7))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp eb530003-727b-4ecc-8b8f-441a3d94f9e6))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c6ebbe38-c87a-4fe7-a38d-153487ea22e3))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8168321f-7a04-4522-8aef-2189470fd750))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 51df22b6-e057-4f99-b98b-50c5e8bcccf5))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pintype "passive") (tstamp 5d1822b4-80f4-45dd-9a73-6dfc5358949a))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 6fda8cc7-2c94-48a4-8a84-fdf231d4c8b3))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tstamp 3f4f770f-5e99-4a8e-b5af-7914e68b6289)
    (at 129.735 71.01 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/b39fb77b-8e5c-4366-9a8b-570ec6c90b66")
    (attr smd)
    (fp_text reference "C109" (at 0 1.43) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cb769dc3-c6fc-49f5-8be4-730baedaf59b)
    )
    (fp_text value "100nF" (at 0 -1.43) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cedc45bf-4e65-4017-b907-290cabf6a00e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 89d4d411-a5f7-4c6f-bc3b-ba27dd7732b0)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9292d21d-a1c5-4919-b2ca-d60a18782af4))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 683f2b56-fd10-4bb7-9ecd-e0730edba3f7))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 90ea5eff-61f5-42fd-9d09-8293d32f875f))
    (fp_line (start -1.48 0.73) (end 1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a907df6a-bb58-46d9-bf00-b6cc8cb33e12))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f2d65df2-f587-4815-81c9-d592863fe6fa))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6d0c0b5c-64f5-4edf-9b64-3692aee02f2f))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fb49aa4f-1335-4636-a802-241b030c2abc))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 73ae83a5-020a-4327-b90d-29cc0aab6a77))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 40a1d86a-f96b-4f7b-86b1-aaf716bb2d42))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f028bb9a-e844-4a65-be05-94031330ae0e))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "+5V") (pintype "passive") (tstamp 3b81d06a-ce18-4bca-803e-30b2703c3dd0))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 0494945d-30aa-4dfc-a7db-a76e4144928b))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tstamp 573b6166-477e-41d5-845b-278e224dda5a)
    (at 137.725 71 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/0e4195e9-6daf-4243-94bc-d2e481a82e9f")
    (attr smd)
    (fp_text reference "C104" (at 0 1.43) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4097878a-cc9a-406f-b588-261dcc1ab591)
    )
    (fp_text value "100nF" (at 0 -1.43) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c8d7a2ad-9c97-423f-b49f-a81f046c4e60)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp f43ee131-f516-4210-9dfe-a839a99357cc)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9445505b-8919-4033-8b09-2a0f18efee38))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 17814adf-14b5-4d47-ab6c-b17a29140993))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 577ae91e-cb35-46de-86b5-34d1ef80360a))
    (fp_line (start -1.48 0.73) (end 1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 78e1e19b-cb09-421d-a528-29ec2c7a7eb6))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 81b27a91-be7d-4df0-9ce9-5ad4390963e6))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 0c9bd2ab-c161-412a-85df-6305ab225d18))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a6c2d17b-77ab-4b23-acd0-b85ceca88b32))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp eb5177bb-f5e6-4a5e-a9fb-739ece3fd5a1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 40b3b4d7-ace0-45f3-a574-ca84379a4fbd))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a3892bed-2422-46c3-a2f7-c55c7ea6ac93))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pintype "passive") (tstamp 9c807c08-dfd9-4896-8b28-22732ec49d2f))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 66bf5db8-0d2c-4a41-a2b8-f7e4b1a0afc3))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tstamp 7781aae8-5d26-4046-9a09-adba2b97542e)
    (at 133.745 73.52 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/b3320132-69fc-49f0-88ee-6a3c7b7f3109")
    (attr smd)
    (fp_text reference "R103" (at 0 1.43) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e32eb75d-d030-4f22-ad16-b68334252a6f)
    )
    (fp_text value "10k" (at 0 -1.43) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ae3d04df-c395-4606-b5f2-9b08bc48fa82)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp df049df0-5bdf-493e-8325-4d313c798e35)
    )
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9bcc956e-c4f5-4588-9853-153c0a2fe704))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 491783cd-5231-406c-a894-1307926a4d32))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 695ccbcc-4a44-4a1f-b5e4-e7c0459755d8))
    (fp_line (start -1.48 0.73) (end 1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d7dabff1-d3e8-43d3-9166-fdc019d9e19a))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp dd24b3b7-fded-4c6a-9ae8-b40d092a7306))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f01717ce-5ea2-40bb-b345-2f1eb154ce2d))
    (fp_line (start -0.8 -0.4125) (end -0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e9e0135f-dc09-4297-aa43-2589d124f697))
    (fp_line (start -0.8 0.4125) (end 0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4f9e6c7f-c861-4fc9-8454-f86043fee0ad))
    (fp_line (start 0.8 -0.4125) (end -0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3abd0d27-4387-470f-9670-488149825e8a))
    (fp_line (start 0.8 0.4125) (end 0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1a8e6dd9-5188-4b8e-8817-9c427dc5f186))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pintype "passive") (tstamp 946820c0-3b54-4d49-8bf1-ece9fed82a51))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "SDA") (pintype "passive") (tstamp 0df8ac50-91ca-471c-a2bf-3fc9ebf81672))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (layer "B.Cu")
    (tstamp 86bb7e54-f037-47a0-b596-e108d6b4f269)
    (at 117 70 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/9821c558-58e3-47fb-b61f-2f1746d0a0c0")
    (attr smd)
    (fp_text reference "U101" (at 0 4.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5ee2adf0-1a71-404c-91ed-e0ee9563acff)
    )
    (fp_text value "AP1117-33" (at 0 -4.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ec94d7fb-8ff3-47fc-9bcb-6ab1990a40ec)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
      (tstamp 50804f87-f832-4c63-a5a7-b7f94bf6665d)
    )
    (fp_line (start -4.1 3.41) (end 1.91 3.41)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0bc86cc1-c86c-41e0-9315-281c18af05f0))
    (fp_line (start -1.85 -3.41) (end 1.91 -3.41)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b8dbe2de-283b-405e-95ac-e8f8950e16ea))
    (fp_line (start 1.91 -3.41) (end 1.91 -2.15)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp dd9691e0-5bea-4f21-9741-4d29638cd32d))
    (fp_line (start 1.91 3.41) (end 1.91 2.15)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 36cd765a-f621-46fc-9b88-d90e333169eb))
    (fp_line (start -4.4 -3.6) (end 4.4 -3.6)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 263e9b7e-c3cd-4442-851e-d2b54de99d8e))
    (fp_line (start -4.4 3.6) (end -4.4 -3.6)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 95ef25aa-dac6-44d9-90a0-efd49308b704))
    (fp_line (start 4.4 -3.6) (end 4.4 3.6)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 79a5a253-5ade-4145-9002-16ea61146340))
    (fp_line (start 4.4 3.6) (end -4.4 3.6)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp bc96b171-0e5f-4f36-b582-eb709cbba257))
    (fp_line (start -1.85 -3.35) (end 1.85 -3.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d547ab08-9a5d-4bc3-bdc6-eb70399817c6))
    (fp_line (start -1.85 2.35) (end -1.85 -3.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 75f01a69-5b72-43de-ae85-3f0e1d096e8d))
    (fp_line (start -1.85 2.35) (end -0.85 3.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b29a0e42-fd5a-49a8-8a01-edc4123e673b))
    (fp_line (start -0.85 3.35) (end 1.85 3.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e226f21d-d833-4b38-a2cd-20826072ac2f))
    (fp_line (start 1.85 3.35) (end 1.85 -3.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fd7e3921-456d-4e00-b0f0-baf8980505ac))
    (pad "1" smd rect (at -3.15 2.3 90) (size 2 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (tstamp cb61a608-4d4c-465e-98f1-04dc591a70ac))
    (pad "2" smd rect (at -3.15 0 90) (size 2 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "+3V3") (pinfunction "VO") (pintype "power_out") (tstamp 0ea296d6-5875-4618-860c-bfe68796f5b4))
    (pad "2" smd rect (at 3.15 0 90) (size 2 3.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "+3V3") (pinfunction "VO") (pintype "power_out") (tstamp 43b4c41e-2f8b-4ca3-9572-a148323b8957))
    (pad "3" smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "+12V") (pinfunction "VI") (pintype "power_in") (tstamp d3bd2f73-786f-472c-89b7-10fd054df22c))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tstamp b1e850bc-5b6a-4eb2-9c2f-3f1342925223)
    (at 129.735 68.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/9d9e2133-2b70-4805-878d-24188dcc4000")
    (attr smd)
    (fp_text reference "R102" (at 0 1.43) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2b7a0a38-c57b-4049-9459-6425e02babc9)
    )
    (fp_text value "10k" (at 0 -1.43) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 457dccbc-dfb4-410d-af24-85b1db346ea1)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 441c4051-7729-4c6b-b365-e314899e280d)
    )
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 34d0d5b5-2222-4d7c-b01b-790b6e1c93ac))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7d1eb56d-f0c3-47ad-a047-c3b152757acf))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9d241524-4f3d-403f-922c-c9ba77ea6dbe))
    (fp_line (start -1.48 0.73) (end 1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f51e8516-43d9-4968-ab7d-a1cfafe430cd))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 11e0f06a-7597-4384-8f57-89cae5157d93))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6e8132b0-bc04-403c-b348-bb0846356149))
    (fp_line (start -0.8 -0.4125) (end -0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 27bfdb5a-d4d9-4caf-821e-0fed526dbe2a))
    (fp_line (start -0.8 0.4125) (end 0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4c05367a-a32d-485a-8a68-33fce1124b1a))
    (fp_line (start 0.8 -0.4125) (end -0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8a7c6555-7cb9-41c2-91f0-a74568b7b0cd))
    (fp_line (start 0.8 0.4125) (end 0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b419826f-750b-431c-af7c-5c03c96204d7))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pintype "passive") (tstamp a1f24bd0-e3fa-4202-ae73-ed88fc1cca4f))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "SCL") (pintype "passive") (tstamp 26876a32-8807-4cfb-b77d-1e29e6d8b522))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tstamp bc40b764-3a73-4806-8523-1eda19817ca6)
    (at 129.735 73.52 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/e5df6708-97a0-4ca9-a79d-5b0a137ba390")
    (attr smd)
    (fp_text reference "R101" (at 0 1.43) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ce82fbda-e06d-49cc-a744-32ea5e870665)
    )
    (fp_text value "120" (at 0 -1.43) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8fb6774b-9ab0-47a5-9476-41708212d06d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 1a3cc24d-b360-48d7-92eb-163cb6c06b75)
    )
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 442ad714-c7a9-4440-933a-07208878b2c0))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 147d8636-f8cb-4d9a-9fe2-4658fd953f44))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c0b496dd-271f-4291-967f-f7d244b50133))
    (fp_line (start -1.48 0.73) (end 1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b827f110-2cf7-4092-a122-1d92290218c6))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 03129bca-6ccc-44e1-9824-68323f0f4da6))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp eef0dd68-ce93-4c5c-b0e1-289c240ecd5d))
    (fp_line (start -0.8 -0.4125) (end -0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 519577a3-6f4e-49bd-9931-91b1722446ce))
    (fp_line (start -0.8 0.4125) (end 0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6784fed8-33b9-4eae-a20b-898c7e9f9acd))
    (fp_line (start 0.8 -0.4125) (end -0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 08b72fac-3076-401e-9cc4-995667f4e96a))
    (fp_line (start 0.8 0.4125) (end 0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 904a2992-5785-4e29-8b72-389b2d02b9a8))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "CAN_H") (pintype "passive") (tstamp a26b0c01-8eb4-4d00-bbd9-9aa2b4bd9bf0))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "CAN_L") (pintype "passive") (tstamp 26ee0bb2-ad6d-413d-98eb-7ee5ee45f359))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tstamp d65df6c2-4899-4d81-bbd1-f9cd81497d96)
    (at 125.725 68.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/b6b87d06-bb02-483f-9470-6f1bf552d5bb")
    (attr smd)
    (fp_text reference "C103" (at 0 1.43) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4fd235c9-441a-4cba-9926-ccffceea63ef)
    )
    (fp_text value "100nF" (at 0 -1.43) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 548b04a1-d840-46eb-8046-ea6d5b847536)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 59c827fc-c46a-4f69-9645-701509830418)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 931f560b-b7e4-4812-93db-e50c077f321a))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e0e0225d-f3f4-4560-a40a-20beae2e800a))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 27f6f06c-6a6f-41aa-983e-2ed54faf57de))
    (fp_line (start -1.48 0.73) (end 1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 431a886f-0366-450e-9433-efecde94f72b))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d9370610-1fd8-4b82-a7bb-f499d18bbb76))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 76ac3625-a7e6-4715-9d90-ee7b97180dd8))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f479c339-3a5b-4069-8d93-2d7eb1cca77d))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bab68a84-450b-43fa-9a66-c03fffb0911f))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2dbaab6f-3c0a-40ae-8f5a-53d640e01991))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a18631ab-5079-4828-aa4f-f40d0d360ca1))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "NRST") (pintype "passive") (tstamp 461016e1-95fe-44ab-95ca-f0200c4375d7))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp fca26de5-9099-46f1-a650-97641a4fc54c))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tstamp ecdc6ed9-10dc-4d50-996f-96055667ab89)
    (at 133.745 68.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SSU_v3.kicad_sch")
    (property "Sheetname" "")
    (path "/35062d3a-422f-42d1-a609-9707938e547e")
    (attr smd)
    (fp_text reference "C108" (at 0 1.43) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6c6ef1f3-5895-46ee-9a7d-f355258d24e6)
    )
    (fp_text value "100nF" (at 0 -1.43) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 06ab3080-ead1-405d-8478-570f89e01714)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp e1005603-1844-4963-b59c-76ea294269ed)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp eeeeed59-f52b-4c93-bb8d-23b298f9db6b))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b88dbd92-5b5c-47a9-961f-fb08556db269))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1a2f8608-8214-4129-ad53-21bcf787c5c1))
    (fp_line (start -1.48 0.73) (end 1.48 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d1fa3f51-6079-429a-a0dd-de48371b0d21))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5b5bb662-aac7-42fe-9c27-aa68ef3065bc))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9eb48115-eaf6-491d-8ff0-7233ce6d32c1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4c515548-95bd-4716-a634-d9e5f53fea15))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e4a6398f-3925-412a-9af0-3ffbe269071a))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e44ed356-8143-4d95-bf6d-93364da9becd))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 35318176-26bc-4124-8d52-94cac88c25bb))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pintype "passive") (tstamp 6ff67214-2159-41a3-9523-3dd11277b364))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 30a97fa8-ff45-43e2-908c-02a05b8731dd))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 100 60) (end 150 80)
    (stroke (width 0.1) (type solid)) (fill none) (layer "Edge.Cuts") (tstamp c0c2bd35-5c61-47db-a8b8-e4249227472b))
  (dimension (type aligned) (layer "Cmts.User") (tstamp 11af36ff-3959-41d6-86f2-35df83d416be)
    (pts (xy 100 80) (xy 100 55))
    (height -8)
    (gr_text "25,0000 mm" (at 90.85 67.5 90) (layer "Cmts.User") (tstamp 11af36ff-3959-41d6-86f2-35df83d416be)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User") (tstamp 9a5fd4ec-6e7a-49cc-a40e-d6c92b4c48b2)
    (pts (xy 100 80) (xy 155 80))
    (height 5)
    (gr_text "55,0000 mm" (at 127.5 83.85) (layer "Cmts.User") (tstamp 9a5fd4ec-6e7a-49cc-a40e-d6c92b4c48b2)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )

)
