(footprint "SOT-23-BAT54FILM"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SOT TO_SOT_SMD")
	(property "Reference" "D2"
		(at 0.03 -2.43 0)
		(layer "F.SilkS")
		(uuid "fd2b6b18-5a33-42a6-98ce-1ad2761b7815")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "BAT54FILM"
		(at 0 2.4 0)
		(layer "F.Fab")
		(uuid "bce5f94f-595d-4b58-bbf9-7ec66fef3cb2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2b15c36e-1a82-40a1-8988-dd00d3479ff1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.mouser.de/datasheet/2/389/bat54-1849047.pdf"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "fb11451d-f56b-498f-9d06-b18f27ef0779")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Schottky diode"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7eb98bc3-5ae3-46a5-a8ed-1fb6439c5f82")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0 -1.56)
		(end -0.65 -1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e7e039af-98eb-43d6-8bd6-1a50b3aed995")
	)
	(fp_line
		(start 0 -1.56)
		(end 0.65 -1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ce4a5ff6-0534-483f-8b3c-1cbf422e0c45")
	)
	(fp_line
		(start 0 1.56)
		(end -0.65 1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0d52bad0-a7fb-40b4-afe4-cfb28f23c478")
	)
	(fp_line
		(start 0 1.56)
		(end 0.65 1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c67b72fe-2f74-4e05-88d0-53c5cddf768e")
	)
	(fp_poly
		(pts
			(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.84) (xy -1.1625 -1.51)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "85e28ae0-5759-498a-b3c5-49653e6ce6d7")
	)
	(fp_line
		(start -1.92 -1.7)
		(end -1.92 1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2888e2db-32b7-46a6-b27b-be63ad535c6a")
	)
	(fp_line
		(start -1.92 1.7)
		(end 1.92 1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ff1bc43b-0e5c-469a-a6d0-94f0985a3dbe")
	)
	(fp_line
		(start 1.92 -1.7)
		(end -1.92 -1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "29b75944-170f-4746-ac9d-4d80c0988669")
	)
	(fp_line
		(start 1.92 1.7)
		(end 1.92 -1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "48522168-1aec-4f43-a32e-7b4bf0368dff")
	)
	(fp_line
		(start -0.65 -1.125)
		(end -0.325 -1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8d1b0501-4922-45f2-aa7e-5d58f1bb278b")
	)
	(fp_line
		(start -0.65 1.45)
		(end -0.65 -1.125)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ad9c5576-241d-4d56-8869-0fca525338f9")
	)
	(fp_line
		(start -0.325 -1.45)
		(end 0.65 -1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a5519682-2082-4609-8a04-e509f60ce024")
	)
	(fp_line
		(start 0.65 -1.45)
		(end 0.65 1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6a65b1ff-f514-42c1-a720-35a3c81e7453")
	)
	(fp_line
		(start 0.65 1.45)
		(end -0.65 1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b08e7da9-b638-4313-9802-202c94d9d072")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "b37947a8-6a81-42c9-858f-c252ee831d65")
		(effects
			(font
				(size 0.32 0.32)
				(thickness 0.05)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.9375 -0.95)
		(size 1.475 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "456f2781-c6ed-4b4b-8a7e-29a1f2bd6012")
	)
	(pad "2" smd roundrect
		(at 0.9375 0)
		(size 1.475 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "963d4ddd-f26b-4635-81d2-804d42e5a733")
	)
	(pad "3" smd roundrect
		(at -0.9375 0.95)
		(size 1.475 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "df4080b4-f6b9-484d-957d-ff14d3209ca0")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
