Questionable use of curly braces in ".meas e_cond param {p_cond*(t_off/4)}"
    Error: undefined symbol in: "[p_cond]*(t_off/4)"
Questionable use of curly braces in ".meas e_off_uj param {e_off*1000000}"
    Error: undefined symbol in: "[e_off]*1000000"
Questionable use of curly braces in ".meas e_on_uj param {(e_on-e_cond)*1000000}"
    Error: undefined symbol in: "([e_on]-e_cond)*1000000"
LTspice 24.0.12 for Windows
Circuit: * C:\Users\Vincents Laptop\Documents\TU Berlin\Fasttube\Electronics\DCDC\Konzept\PSFB\FETs\Spice\DPT_Switching_Energies.asc
Start Time: Tue May 27 20:54:41 2025
solver = Normal
Maximum thread count: 16
tnom = 27
temp = 27
method = modified trap
abstol = 1e-10
reltol = 0.0001
chgtol = 1e-12
c1: Increased Cpar to 1e-10
c2: Increased Cpar to 1e-10
WARNING: Less than two connections to node tc.  This node is used by v5.
Direct Newton iteration for .op point succeeded.
Changing Tseed to 5e-14
Changing Tseed to 5e-16
Heightened Def Con from 7.32422e-16 to 1e-09
Heightened Def Con from 1e-07 to 1.045e-07
Heightened Def Con from 2.01671e-06 to 2.02176e-06

e_off: INTEG(v(phase)*ix(u3:drain))=1.37158e-06 FROM 9.16709e-07 TO 1.16671e-06
e_on: INTEG(v(phase)*ix(u3:drain))=1.64926e-05 FROM 1.91671e-06 TO 2.16671e-06
p_cond_on1: ix(u3:drain)*v(phase)=4.38208 at 2.16671e-06
p_cond_on_2: ix(u3:drain)*v(phase)=4.77517 at 2.21671e-06
p_cond: (p_cond_on1+p_cond_on_2)/2=4.57862
e_cond: (p_cond*(t_off/4))=1.14466e-06
e_off_uj: (e_off*1000000)=1.37158
e_on_uj: ((e_on-e_cond)*1000000)=15.348

Total elapsed time: 1.335 seconds.

