<?xml version="1.0" encoding="utf-8"?>
<!--/15743474/1031803/2.50/8/3/Integrated Circuit/-->
<!DOCTYPE curve SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;Digital Isolators Automotive, hot-swappable, robust-EMC bidirectional I2C isolator with bidirectional clock&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOIC127P600X175-8N">
<description>&lt;b&gt;D0008A&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="ISO1640BQDRQ1">
<pin name="VCC1" direction="io"/>
<pin name="SDA1" direction="io"/>
<pin name="SCL1" direction="io"/>
<pin name="GND1" direction="io"/>
<pin name="VCC2" direction="io"/>
<pin name="SDA2" direction="io"/>
<pin name="SCL2" direction="io"/>
<pin name="GND2" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ISO1640BQDRQ1" prefix="IC">
<description>&lt;b&gt;Digital Isolators Automotive, hot-swappable, robust-EMC bidirectional I2C isolator with bidirectional clock&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://www.ti.com/lit/ds/symlink/iso1640.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ISO1640BQDRQ1"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="G$1" pin="VCC1" pad="1"/>
<connect gate="G$1" pin="SDA1" pad="2"/>
<connect gate="G$1" pin="SCL1" pad="3"/>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="SCL2" pad="6"/>
<connect gate="G$1" pin="SDA2" pad="7"/>
<connect gate="G$1" pin="VCC2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="Mouser_Part_Number" value="595-ISO1640BQDRQ1"/>
<attribute name="Mouser_Price-Stock" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/ISO1640BQDRQ1?qs=QNEnbhJQKvat3Z1mRPODGw%3D%3D"/>
<attribute name="Manufacturer_Name" value="Texas Instruments"/>
<attribute name="Manufacturer_Part_Number" value="ISO1640BQDRQ1"/>
<attribute name="Description" value="Digital Isolators Automotive, hot-swappable, robust-EMC bidirectional I2C isolator with bidirectional clock"/>
<attribute name="Height" value="1.75mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
