(footprint "Littelfuse_485" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 6226A06B)
  (attr smd)
  (fp_text reference "REF**" (at 0 -4 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bb5999d5-f86c-445a-9ff9-2a1b539dc199)
  )
  (fp_text value "Littelfuse_485" (at 0 4.25 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8f03ae41-61bd-4463-bc12-db0dde34447c)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b5ea13a8-3e37-4201-b115-0647094f76a8)
  )
  (fp_line (start -2 2.5) (end 2 2.5) (layer "F.SilkS") (width 0.12) (tstamp 13f30964-a0e5-4b66-a3b0-82966c8576ce))
  (fp_line (start -2 -2.5) (end 2 -2.5) (layer "F.SilkS") (width 0.12) (tstamp 27ab07ca-24f6-4b98-9e32-937f5364edd2))
  (fp_rect (start -7.25 -3.25) (end 7.25 3.25) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp d854e56c-a962-466d-bce7-bfb3c9c54498))
  (fp_rect (start -6.05 -2.25) (end 6.05 2.25) (layer "F.Fab") (width 0.1) (fill none) (tstamp 3f494321-e87f-4a8e-bbe5-a937d805b012))
  (pad "1" smd roundrect (at -5.15 0) (size 3.5 5.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 9cb160c0-5456-4bd7-aa7f-b9388d25eb35))
  (pad "2" smd roundrect (at 5.15 0) (size 3.5 5.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 9ee66366-9074-4bc0-8447-8c0b7199acdf))
)
