(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "TLE7258SJ" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -10.16 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TLE7258SJ" (id 1) (at 1.27 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 0 -12.7 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/Infineon-TLE7258-DS-v01_10-EN.pdf?fileId=5546d46259d9a4bf015a3cff8dd85e6b" (id 3) (at -10.16 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "LIN 2.2A SAE J2602 Transceiver" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LIN 2.2A/SAE J2602 transceiver, 20kbps" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TLE7258SJ_0_1"
      (rectangle (start -10.16 7.62) (end 10.16 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TLE7258SJ_1_1"
      (pin open_collector line (at -12.7 5.08 0) (length 2.54)
        (name "RXD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -12.7 -5.08 0) (length 2.54) hide
        (name "N.C." (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 2.54)
        (name "TXD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
        (name "BUS" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 2.54 180) (length 2.54)
        (name "INH" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TLE9351VSJ" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -10.16 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TLE9351VSJ" (id 1) (at 2.54 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 0 -12.7 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/Infineon-TLE9351VSJ-DataSheet-v01_10-EN.pdf?fileId=5546d46276c4f5350176f6dd01371230" (id 3) (at 0 -15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Automotive CAN FD Transceiver" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Automotive CAN FD Transceiver, 5Mbps, 5V supply, Vio pin" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TLE9351VSJ_0_1"
      (rectangle (start -10.16 7.62) (end 10.16 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TLE9351VSJ_1_1"
      (pin input line (at -12.7 5.08 0) (length 2.54)
        (name "TXD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 2.54 0) (length 2.54)
        (name "RXD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 -2.54 0) (length 2.54)
        (name "Vio" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
        (name "CANL" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 2.54 180) (length 2.54)
        (name "CANH" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 2.54)
        (name "STBY" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
