(footprint "APEM-ISx3SAD" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61BA292D)
  (descr "Sealed pushbutton switch")
  (tags "ISR3AD, ISP3AD")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -9.33) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp faecce08-8f51-4f10-9f76-24557732a17c)
  )
  (fp_text value "SW_Push" (at 0 -11.43) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9f355912-b2a0-47c2-9480-f08e9b430c38)
  )
  (fp_circle (center 0 0) (end 8.75 0) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 3bacaf2e-6da8-4b29-841c-47b3ef14f69d))
  (pad "1" thru_hole roundrect (at -2.54 0) (size 1.6 4) (drill oval 1 3.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp f0eaca8d-f04b-43dc-bb41-c96d99e31523))
  (pad "2" thru_hole roundrect (at 2.54 0) (size 1.6 4) (drill oval 1 3.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp ff84004f-a3bb-4ea5-8adf-2c6fd652e9f1))
)
