(footprint "ST1L08"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "ce929630-f189-4a05-86c8-5f1460eddd88")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "ST1L08"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "74fd3911-0ac2-4cf0-a0d3-8409634064a1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6d28731f-bc3e-4beb-8469-5e36dda5279a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "088ddb5b-018a-4150-b550-d388d9c4fba4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "899947d9-c9a6-4f4a-859f-d8870b6937da")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -1.25 -2)
		(end 1.25 2)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "d5128ff1-6a27-4d11-a5f0-efb011accf59")
	)
	(fp_circle
		(center 1.75 -1.75)
		(end 1.9 -1.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "cc2c7194-ca79-469b-9a1e-d741b021b595")
	)
	(fp_rect
		(start -1.25 -2)
		(end 1.25 2)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "35d40a70-7369-4fc2-afc7-2dce07ce5021")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "4e2f5e90-d177-4033-bda5-8174c62ac57c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at 0.75 -1.4)
		(size 0.3 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "668d6769-6369-420c-ae0a-db117a63cc82")
	)
	(pad "2" smd roundrect
		(at 0.25 -1.4)
		(size 0.3 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "c51b4abc-a370-45f0-8f5e-270ce217b2be")
	)
	(pad "3" smd roundrect
		(at -0.25 -1.4)
		(size 0.3 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "e5df56f1-0310-4694-b3a2-116cb4756ce5")
	)
	(pad "4" smd roundrect
		(at -0.75 -1.4)
		(size 0.3 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "f245cb2d-50ba-418e-9e66-5c373bc6d5d9")
	)
	(pad "5" smd roundrect
		(at -0.75 1.4)
		(size 0.3 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0)
		(chamfer bottom_left bottom_right)
		(thermal_bridge_angle 45)
		(uuid "2e07bd35-0dbc-4011-ab81-5285db555a17")
	)
	(pad "6" smd roundrect
		(at -0.25 1.4)
		(size 0.3 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0)
		(chamfer bottom_left bottom_right)
		(thermal_bridge_angle 45)
		(uuid "5b2e619c-d833-4a33-8fe0-b1a71c647429")
	)
	(pad "7" smd roundrect
		(at 0.25 1.4)
		(size 0.3 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0)
		(chamfer bottom_left bottom_right)
		(thermal_bridge_angle 45)
		(uuid "98f0bf13-72af-4103-af62-4711bf5c175a")
	)
	(pad "8" smd roundrect
		(at 0.75 1.4)
		(size 0.3 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0)
		(chamfer bottom_left bottom_right)
		(thermal_bridge_angle 45)
		(uuid "31dd0864-656d-4a9d-822c-cc8cf0ac18f8")
	)
	(pad "EP" smd roundrect
		(at 0 0)
		(size 1.75 1.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(chamfer_ratio 0.25)
		(chamfer top_right)
		(thermal_bridge_angle 45)
		(uuid "d1dba1a0-32d2-464a-8361-61066a511851")
	)
)
