(footprint "WE_SOP-4" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 63617782)
  (descr "SOP, 4 Pin (http://www.ixysic.com/home/pdfs.nsf/www/CPC1017N.pdf/$file/CPC1017N.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "SOP SO")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.5) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e250304b-2864-4f44-b1e8-173cc34a2ac6)
  )
  (fp_text value "WE_SOP-4" (at 0 3) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 08bb8c58-1868-4a96-8aaa-36d9e141ec38)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 0.95 0.95) (thickness 0.14)))
    (tstamp 758f4e53-9507-488a-960b-2e8e487b7ac8)
  )
  (fp_line (start 0 -2.16) (end -2.25 -2.16) (layer "F.SilkS") (width 0.12) (tstamp 3f0c3fb9-57f0-4439-b2df-3c934842d7db))
  (fp_line (start -2.25 2.16) (end -2.25 1.805) (layer "F.SilkS") (width 0.12) (tstamp 581488ee-fe1f-43d1-a23d-526666571191))
  (fp_line (start 0 -2.16) (end 2.25 -2.16) (layer "F.SilkS") (width 0.12) (tstamp 58e02161-61cc-4d0f-bdc8-c497a25ae380))
  (fp_line (start 2.25 -2.16) (end 2.25 -1.8225) (layer "F.SilkS") (width 0.12) (tstamp 7da78911-dd6f-4bbd-9a74-8a3476ec1fb5))
  (fp_line (start 0 2.16) (end -2.25 2.16) (layer "F.SilkS") (width 0.12) (tstamp af35a153-e4cc-4cb5-9b0a-a247aa9a27b2))
  (fp_line (start 2.25 2.16) (end 2.25 1.805) (layer "F.SilkS") (width 0.12) (tstamp b6e7e52e-fa7c-4663-b29b-8d72461a55fb))
  (fp_line (start 0 2.16) (end 2.25 2.16) (layer "F.SilkS") (width 0.12) (tstamp dc9eba43-a0ae-45fc-b91c-9050201557b9))
  (fp_line (start -2.25 -1.805) (end -3.75 -1.805) (layer "F.SilkS") (width 0.12) (tstamp de91796c-56de-4405-8fcc-748bd6a08e86))
  (fp_line (start -2.25 -2.16) (end -2.25 -1.805) (layer "F.SilkS") (width 0.12) (tstamp f76f4233-905d-4cb5-a153-eed7fe8e458e))
  (fp_line (start 4 -2.3) (end -4 -2.3) (layer "F.CrtYd") (width 0.05) (tstamp 2a756062-4e0c-4114-bc6d-4d6635f2d703))
  (fp_line (start -4 -2.3) (end -4 2.3) (layer "F.CrtYd") (width 0.05) (tstamp 65d0582b-c8a1-45a8-a0e9-e797f01caa63))
  (fp_line (start -4 2.3) (end 4 2.3) (layer "F.CrtYd") (width 0.05) (tstamp 6e24aa9b-c7e6-40f2-905b-b9c541e0e2f6))
  (fp_line (start 4 2.3) (end 4 -2.3) (layer "F.CrtYd") (width 0.05) (tstamp 88f2670e-1113-4ed9-b644-cfdac6e8b249))
  (fp_line (start 2 2.05) (end -2 2.05) (layer "F.Fab") (width 0.1) (tstamp 1f70d207-e63d-4692-be1f-5b6fa8599d57))
  (fp_line (start -0.95 -2.05) (end 2 -2.05) (layer "F.Fab") (width 0.1) (tstamp d7de2887-c7b2-4bb7-a339-632f4f906224))
  (fp_line (start -2 -1.1) (end -0.95 -2.05) (layer "F.Fab") (width 0.1) (tstamp e978c208-72f4-4c78-b109-bcb5e56d4024))
  (fp_line (start -2 2.05) (end -2 -1.1) (layer "F.Fab") (width 0.1) (tstamp ea3cd08e-2d6a-4ba3-9c39-87a3d44d2015))
  (fp_line (start 2 -2.05) (end 2 2.05) (layer "F.Fab") (width 0.1) (tstamp f69de914-d2d4-4fcf-a7d6-ce76fea2e1a7))
  (pad "1" smd roundrect (at -3.15 -1.27) (size 1.1 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp dea30d29-44e9-47fc-bccc-6928d5c29cea))
  (pad "2" smd roundrect (at -3.15 1.27) (size 1.1 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 767e3782-90bf-4d7f-b1ef-719aa7013187))
  (pad "3" smd roundrect (at 3.15 1.27) (size 1.1 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c34f5129-9516-486b-b322-ada2d7baa6ba))
  (pad "4" smd roundrect (at 3.15 -1.27) (size 1.1 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 407d0cd8-54f8-47a8-90cb-42c8a441d04f))
  (model "${KIPRJMOD}/FT_libraries/FaSTTUBe_Isolators.pretty/3d_models/WL-OCPT_Serie356.stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
