(footprint "Micro_Mate-N-Lok_2p_horizontal" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 63617318)
  (attr smd)
  (fp_text reference "REF**" (at 0 -8.25 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 42713045-fffd-4b2d-ae1e-7232d705fb12)
  )
  (fp_text value "Micro_Mate-N-Lok_2p_horizontal" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c0515cd2-cdaa-467e-8354-0f6eadfa35c9)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1bf544e3-5940-4576-9291-2464e95c0ee2)
  )
  (fp_line (start -4 -4.5) (end -2.5 -4.5) (layer "F.SilkS") (width 0.12) (tstamp 2923d83c-3334-4b85-acfa-e9f2eb6f5eb5))
  (fp_line (start 4 4.75) (end 4 1.25) (layer "F.SilkS") (width 0.12) (tstamp 3836c63d-ca60-4e8e-a339-40980bdccc31))
  (fp_line (start -0.5 -4.5) (end 0.5 -4.5) (layer "F.SilkS") (width 0.12) (tstamp 5e066231-f8d2-43bf-bff3-80c6fb0c9c86))
  (fp_line (start -4 4.75) (end 4 4.75) (layer "F.SilkS") (width 0.12) (tstamp 638492c1-39c4-4e69-a3a1-232b324e5b21))
  (fp_line (start -4 -1.25) (end -4 -4.5) (layer "F.SilkS") (width 0.12) (tstamp 68d14432-223b-47bb-bd26-18873cfb3df2))
  (fp_line (start -4 -1.25) (end -5 -1.25) (layer "F.SilkS") (width 0.12) (tstamp 721eced1-7601-448b-b032-57ae840a5bc6))
  (fp_line (start -4 1.25) (end -4 4.75) (layer "F.SilkS") (width 0.12) (tstamp 75ada5c7-eed3-466b-a900-bb7cf3da6f9e))
  (fp_line (start 4 1.25) (end 5 1.25) (layer "F.SilkS") (width 0.12) (tstamp 8e73e860-7df5-47ee-9d85-a51cffff4073))
  (fp_line (start -5 1.25) (end -4 1.25) (layer "F.SilkS") (width 0.12) (tstamp 908ce94b-b837-4c84-b759-ec4fbb006eea))
  (fp_line (start 2.5 -4.5) (end 4 -4.5) (layer "F.SilkS") (width 0.12) (tstamp ba3030b2-37eb-4eb2-b7ee-c2f135251592))
  (fp_line (start 5 -1.25) (end 4 -1.25) (layer "F.SilkS") (width 0.12) (tstamp e7987f0c-e4c6-4aae-a5d6-e1cfea057719))
  (fp_line (start 4 -1.25) (end 4 -4.5) (layer "F.SilkS") (width 0.12) (tstamp f1084b0d-b992-4d4c-9074-1c148a908ad5))
  (fp_circle (center 5 -5.5) (end 5.5 -5.5) (layer "F.SilkS") (width 0.12) (fill solid) (tstamp 63489ebf-0f52-43a6-a0ab-158b1a7d4988))
  (fp_rect (start -7 -7) (end 7 4.75) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 312474c5-a081-4cd1-b2e6-730f0718514a))
  (fp_line (start 4.318 1.27) (end 5.08 1.27) (layer "F.Fab") (width 0.1) (tstamp c6462399-f2e4-4f1a-b34a-b49a04c8bdb9))
  (fp_line (start 4.318 1.778) (end 4.318 1.27) (layer "F.Fab") (width 0.1) (tstamp f284b1e2-75a4-4a3f-a5f4-6f05f15fb4f5))
  (pad "" smd roundrect (at -5.2 0) (size 3.43 1.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1f3003e6-dce5-420f-906b-3f1e92b67249))
  (pad "" smd roundrect (at 5.2 0) (size 3.43 1.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 378af8b4-af3d-46e7-89ae-deff12ca9067))
  (pad "1" smd roundrect (at 1.5 -5.48) (size 1.27 2.92) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ebd06df3-d52b-4cff-99a2-a771df6d3733))
  (pad "2" smd roundrect (at -1.5 -5.48) (size 1.27 2.92) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8c0807a7-765b-4fa5-baaa-e09a2b610e6b))
  (model "${KIPRJMOD}/FT_libraries/FaSTTUBe_connectors.pretty/3d_models/Micro_Mate-N-Lok_2p_horizontal.stp"
    (offset (xyz 0 -4.6 2.5))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
