(footprint "Micro_Mate-N-Lok_2x2p_vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "3-794636-4-1")
  (tags "Connector")
  (attr smd)
  (fp_text reference "J**" (at 0 0) (layer "F.SilkS")
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    (tstamp de6dbf15-ae79-4d66-abac-08480863616c)
  )
  (fp_text value "37946364" (at 0 0) (layer "F.SilkS") hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    (tstamp 73454dd1-5b2b-42e4-bdce-e925fb2d75ff)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    (tstamp d7049f25-a0b9-4b2a-a477-c08baaf2a2f1)
  )
  (fp_line (start -3.43 -3.43) (end -3.43 -1.5)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 3919c0b8-6dc3-4513-a330-0a8e3b796879))
  (fp_line (start -3.43 1.5) (end -3.43 3.43)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp e3e68613-03be-4857-8287-eb53d4cf9588))
  (fp_line (start -3.43 3.43) (end -2.5 3.43)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp dcf44124-9aed-4edf-b196-d989bdbd713f))
  (fp_line (start -2.5 -3.43) (end -3.43 -3.43)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp a588c100-9eca-40d6-8abd-e0275b930252))
  (fp_line (start 2.5 -3.43) (end 3.43 -3.43)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 556702ed-84d9-4a47-8332-8821b9cc612a))
  (fp_line (start 2.5 3.43) (end 3.43 3.43)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 9dc23f8e-47a7-4a21-bc6c-32ab048af2b4))
  (fp_line (start 3.43 -3.43) (end 3.43 -1.5)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 1af06253-8ae9-4f4f-8dfe-1d65d2498836))
  (fp_line (start 3.43 3.43) (end 3.43 1.5)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 5d70b46a-35e1-4fbe-a3be-0ff620fe9f5f))
  (fp_circle (center 4 5) (end 4.5 5)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 1d1c915d-d05a-49d2-98a2-39f7b79b9eed))
  (fp_line (start -7.85 -6.97) (end 7.85 -6.97)
    (stroke (width 0.1) (type solid)) (layer "F.CrtYd") (tstamp 46c86f80-ccb8-42ef-a07e-87ae7e134f6b))
  (fp_line (start -7.85 6.97) (end -7.85 -6.97)
    (stroke (width 0.1) (type solid)) (layer "F.CrtYd") (tstamp 06f3ff96-1ab8-4145-8420-bff1d8501e6d))
  (fp_line (start 7.85 -6.97) (end 7.85 6.97)
    (stroke (width 0.1) (type solid)) (layer "F.CrtYd") (tstamp 845cc01b-b5e3-40a0-ab45-c48320a01ad9))
  (fp_line (start 7.85 6.97) (end -7.85 6.97)
    (stroke (width 0.1) (type solid)) (layer "F.CrtYd") (tstamp 1229a783-aa67-4fe4-b14d-11556dfd076d))
  (fp_line (start -3.43 -3.43) (end 3.43 -3.43)
    (stroke (width 0.2) (type solid)) (layer "F.Fab") (tstamp 202aafd5-7f0f-467b-9759-31af9730614e))
  (fp_line (start -3.43 3.43) (end -3.43 -3.43)
    (stroke (width 0.2) (type solid)) (layer "F.Fab") (tstamp a068ed0e-d660-403e-b910-b1c022a00a69))
  (fp_line (start 3.43 -3.43) (end 3.43 3.43)
    (stroke (width 0.2) (type solid)) (layer "F.Fab") (tstamp d5ad8bbd-4dd2-495b-b849-ac6d164ceb16))
  (fp_line (start 3.43 3.43) (end -3.43 3.43)
    (stroke (width 0.2) (type solid)) (layer "F.Fab") (tstamp aac6c8a0-a060-4f96-a728-2df7576b52d6))
  (pad "" smd roundrect (at -5.135 0 90) (size 1.65 3.43) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f1fd847b-553f-4793-8589-45a8fa16a3ce))
  (pad "" smd roundrect (at 5.135 0 90) (size 1.65 3.43) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cfed0ea5-fd39-4247-8b3a-bf5d16127b8b))
  (pad "1" smd roundrect (at 1.5 4.7) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 853f8b0a-b990-4a1e-9c7c-c95aa5b7e1c3))
  (pad "2" smd roundrect (at 1.5 -4.7) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2daa1bc9-0082-4d28-a4bb-9c0be7c8ce3e))
  (pad "3" smd roundrect (at -1.5 4.7) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 751511a8-2e16-45eb-9dfa-a168babcfa59))
  (pad "4" smd roundrect (at -1.5 -4.7) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ced13875-cb54-4df8-8bea-b4199d3c0768))
  (model "${KIPRJMOD}/libraries/FaSTTUBe_connectors_3dmodels/Micro_Mate-N-Lok_2x2p_vertical.stp"
    (offset (xyz 0 0 9.25))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 180))
  )
)
