(footprint "Micro_Mate-N-Lok_2p_vertical" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 62086176)
  (attr smd)
  (fp_text reference "REF**" (at 0 3.81 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 42713045-fffd-4b2d-ae1e-7232d705fb12)
  )
  (fp_text value "Micro_Mate-N-Lok_2p_vertical" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c0515cd2-cdaa-467e-8354-0f6eadfa35c9)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1bf544e3-5940-4576-9291-2464e95c0ee2)
  )
  (fp_line (start -3.81 2.54) (end 3.81 2.54) (layer "F.SilkS") (width 0.12) (tstamp 1c052668-6749-425a-9a77-35f046c8aa39))
  (fp_line (start 3.81 2.54) (end 3.81 1.27) (layer "F.SilkS") (width 0.12) (tstamp 25ca9482-069d-43de-b77e-6f2ad77fa017))
  (fp_line (start 3.81 -2.54) (end 3.81 -1.27) (layer "F.SilkS") (width 0.12) (tstamp 2b894b8a-c098-4d9d-be0f-2ef41dea274e))
  (fp_line (start -3.81 -2.54) (end -2.54 -2.54) (layer "F.SilkS") (width 0.12) (tstamp 3742a313-c63e-4807-a7bf-be5a0ae2c781))
  (fp_line (start -0.508 -3.302) (end 0.508 -3.302) (layer "F.SilkS") (width 0.12) (tstamp 4ba06b66-7669-4c70-b585-f5d4c9c33527))
  (fp_line (start -3.81 -1.27) (end -3.81 -2.54) (layer "F.SilkS") (width 0.12) (tstamp 5e27f565-c85a-4f3b-9862-58c0accdd5e3))
  (fp_line (start -3.81 2.54) (end -3.81 1.27) (layer "F.SilkS") (width 0.12) (tstamp d35d7027-ac1b-44b2-9664-3d8a37ee0f4e))
  (fp_line (start 2.54 -2.54) (end 3.81 -2.54) (layer "F.SilkS") (width 0.12) (tstamp e8558fbd-ea42-43a6-966a-7bd304bdfaad))
  (fp_circle (center -5.08 -3.81) (end -4.58 -3.81) (layer "F.SilkS") (width 0.12) (fill solid) (tstamp 63489ebf-0f52-43a6-a0ab-158b1a7d4988))
  (fp_rect (start -7.62 -5.08) (end 7.62 2.54) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 312474c5-a081-4cd1-b2e6-730f0718514a))
  (fp_line (start 4.318 1.27) (end 5.08 1.27) (layer "F.Fab") (width 0.1) (tstamp c6462399-f2e4-4f1a-b34a-b49a04c8bdb9))
  (fp_line (start 4.318 1.778) (end 4.318 1.27) (layer "F.Fab") (width 0.1) (tstamp f284b1e2-75a4-4a3f-a5f4-6f05f15fb4f5))
  (pad "" smd roundrect (at -5.2 0) (size 3.43 1.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1f3003e6-dce5-420f-906b-3f1e92b67249))
  (pad "" smd roundrect (at 5.2 0) (size 3.43 1.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 378af8b4-af3d-46e7-89ae-deff12ca9067))
  (pad "1" smd roundrect (at -1.5 -3.2) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ebd06df3-d52b-4cff-99a2-a771df6d3733))
  (pad "2" smd roundrect (at 1.5 -3.2) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8c0807a7-765b-4fa5-baaa-e09a2b610e6b))
  (model "${KIPRJMOD}/libraries/FaSTTUBe_connectors_3dmodels/Micro_Mate-N-Lok_2p_vertical.stp"
    (offset (xyz 0 0 9.24))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 180))
  )
)
