(footprint "Micro_Mate-N-Lok_2x7p_vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "3-794636-4-1")
  (tags "Connector")
  (attr smd)
  (fp_text reference "J**" (at 0 0) (layer "F.SilkS")
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    (tstamp de6dbf15-ae79-4d66-abac-08480863616c)
  )
  (fp_text value "37946364" (at 0 0) (layer "F.SilkS") hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    (tstamp 73454dd1-5b2b-42e4-bdce-e925fb2d75ff)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    (tstamp d7049f25-a0b9-4b2a-a477-c08baaf2a2f1)
  )
  (fp_line (start -11 -3.5) (end -10.5 -3.5)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 1c3816c9-1ab2-442e-a37d-1fa89b99ef20))
  (fp_line (start -11 -1.5) (end -11 -3.5)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp c50f8af2-5d6f-4d3f-a2f8-fd554ddabeab))
  (fp_line (start -11 1.5) (end -11 3.5)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 5ae35a22-004a-4c7e-b216-2b2dfba0dbbc))
  (fp_line (start -11 3.5) (end -10.5 3.5)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp fc2cb4fe-ca3f-4542-9560-61d4474c8b02))
  (fp_line (start -1.5 -7) (end 1.5 -7)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 69b740c7-5940-445d-bc9f-c8d087095d12))
  (fp_line (start -1.5 -5.5) (end -1.5 -7)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 8fcbd669-0c29-4bfe-8b8e-03f456fdd863))
  (fp_line (start 1.5 -7) (end 1.5 -5.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6e52454f-a4d6-449d-8ebd-6cd913a5a917))
  (fp_line (start 11 -3.5) (end 10.5 -3.5)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp e5d87176-e66e-495c-ac35-552ca54cd269))
  (fp_line (start 11 -1.5) (end 11 -3.5)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp cb23f404-a40e-47c9-9c77-accca23f0fca))
  (fp_line (start 11 1.5) (end 11 3.5)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 57e12c2a-918f-4dbf-8176-f8f0a70168e6))
  (fp_line (start 11 3.5) (end 10.5 3.5)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp d87a040c-ea93-47db-a367-d4cf8b02004b))
  (fp_circle (center -11.5 -5.5) (end -11 -5.5)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp ab878989-630e-4841-8563-9a196bac4b6b))
  (fp_rect (start -15 -7) (end 15 7)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp aa6fb2d3-a1b1-4b14-9351-5b2e789571d8))
  (fp_rect (start -10.93 -3.43) (end 10.93 3.43)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 3d4cb86e-70a3-4db7-a644-c739816fba05))
  (pad "" smd roundrect (at -12.635 0 90) (size 1.65 3.43) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f1fd847b-553f-4793-8589-45a8fa16a3ce))
  (pad "" smd roundrect (at 12.635 0 90) (size 1.65 3.43) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cfed0ea5-fd39-4247-8b3a-bf5d16127b8b))
  (pad "1" smd roundrect (at -9 -4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 13ae4d4f-9d65-408a-88d3-c1027bd0f239))
  (pad "2" smd roundrect (at -9 4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8b516d46-5072-4874-85fa-eb9a17379a1c))
  (pad "3" smd roundrect (at -6 -4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9e57dcaf-5541-4b80-b13a-e843bd2d19cc))
  (pad "4" smd roundrect (at -6 4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 21e2f832-26b9-4cf7-9608-5c55a1923e80))
  (pad "5" smd roundrect (at -3 -4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2de4fb7f-3783-4a40-ae45-63734e55c9d0))
  (pad "6" smd roundrect (at -3 4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp eab4589e-73cb-4069-9242-a95ca593b423))
  (pad "7" smd roundrect (at 0 -4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f672e036-75cd-43ba-a95b-1ab8be664d16))
  (pad "8" smd roundrect (at 0 4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3cf7efe1-bc26-43b7-ac75-50cb26b5ab3d))
  (pad "9" smd roundrect (at 3 -4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3148770a-c28f-43a5-acf5-a3f822d5144f))
  (pad "10" smd roundrect (at 3 4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 28b48210-c1ad-4859-bbd7-4448f3c8dd1d))
  (pad "11" smd roundrect (at 6 -4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a4514241-16b5-4170-a3ae-bb18e5df7fbd))
  (pad "12" smd roundrect (at 6 4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b796d4ac-2db7-4038-befe-5db96b995d33))
  (pad "13" smd roundrect (at 9 -4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp feb75515-353a-45d1-a1bc-82b614a271b5))
  (pad "14" smd roundrect (at 9 4.7 180) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 170c8784-240a-4e5a-bfbf-27ce184ffe94))
  (model "${KIPRJMOD}/libraries/FaSTTUBe_connectors_3dmodels/Micro_Mate-N-Lok_2x7p_vertical.stp"
    (offset (xyz 0 0 9.25))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
