(footprint "SON50P200X200X80-9N" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "WSON-8-")
  (tags "Integrated Circuit")
  (attr smd)
  (fp_text reference "IC**" (at 0 -2.4384) (layer "F.SilkS")
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    (tstamp 5ca1bf46-849c-4a3c-80f9-4e5a5f421b34)
  )
  (fp_text value "SON50P200X200X80-9N" (at 0 0) (layer "F.SilkS") hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    (tstamp 0faa16bf-72b3-4f24-8a0a-35bf9fb32e7c)
  )
  (fp_text user "${REFERENCE}" (at 0 2.4892) (layer "F.Fab")
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    (tstamp b7c74a59-def6-4b91-a5be-2cc426d25188)
  )
  (fp_circle (center -1.4 -1.4) (end -1.4 -1.275)
    (stroke (width 0.25) (type solid)) (fill none) (layer "F.SilkS") (tstamp 1811ee21-048b-4984-b7c4-82f32f0e1731))
  (fp_line (start -1.625 -1.3) (end 1.625 -1.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e32d1711-2847-4e37-a365-d9d63c41e24b))
  (fp_line (start -1.625 1.3) (end -1.625 -1.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2c165beb-1302-4433-9492-d7fd87167e0b))
  (fp_line (start 1.625 -1.3) (end 1.625 1.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 960ff1bc-51df-436f-b509-607fa8d93cb5))
  (fp_line (start 1.625 1.3) (end -1.625 1.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f19a16dd-1595-4610-956f-0622c93aa46e))
  (fp_line (start -1 -1) (end 1 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e12c6330-e385-46b2-9440-a61e0f646017))
  (fp_line (start -1 -0.5) (end -0.5 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cd875602-faad-4c47-9291-85c252e6e53b))
  (fp_line (start -1 1) (end -1 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 526baa73-29e3-44d8-908d-6ecef880548a))
  (fp_line (start 1 -1) (end 1 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 21347ff4-fc7d-4db3-a1c7-7f097c1cce20))
  (fp_line (start 1 1) (end -1 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a767b35a-b0ec-427b-8022-fd978047235c))
  (pad "1" smd rect (at -1.05 -0.75 90) (size 0.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 9be8c794-303e-4d94-bd05-1e81ae92857e))
  (pad "2" smd rect (at -1.05 -0.25 90) (size 0.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3d4e05d3-645a-448c-9645-66cc2440c13d))
  (pad "3" smd rect (at -1.05 0.25 90) (size 0.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ab95ad87-9713-4f47-b057-0446fe683edc))
  (pad "4" smd rect (at -1.05 0.75 90) (size 0.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3342043c-85c5-46dc-bdd5-90273a3ae4a0))
  (pad "5" smd rect (at 1.05 0.75 90) (size 0.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 1d468ce5-7347-4d10-8b25-6be8259fd785))
  (pad "6" smd rect (at 1.05 0.25 90) (size 0.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c81a3c5c-499b-4387-bd7c-e19b738d3bd1))
  (pad "7" smd rect (at 1.05 -0.25 90) (size 0.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp bdc42e13-0846-4c5f-bafe-9b6fbe8dd23e))
  (pad "8" smd rect (at 1.05 -0.75 90) (size 0.3 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp df8de995-e395-418f-9866-cd47bc9a12cd))
  (pad "9" smd rect (at 0 0) (size 1 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 6e040b39-bbe1-4e73-be7b-fce7c32f071c))
  (model "${KIPRJMOD}/KiCAD_Lib/stp/TMP1075DSGR.stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
