(footprint "mvbms"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
	(tags "Through hole pin header THT 1x01 2.54mm single row")
	(property "Reference" "REF**"
		(at 0 -2.33 0)
		(layer "F.SilkS")
		(uuid "6c50d304-4606-47dc-966e-5ce9cce54912")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "mvbms"
		(at 0 2.33 0)
		(layer "F.Fab")
		(uuid "86a9f2cd-c84c-4f67-881e-c331171fcf5a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f533db6b-d87a-483d-8669-171e932359e2")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "79edd7bb-ff18-468b-a74c-de472aa41331")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a34fbf3c-c5d6-441f-ab34-787ec4073ba2")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Silkscreen" ""
		(at 0 -2.54 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "0bcc6461-dd1e-47f1-b5e8-46e281bb0b51")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.33 -1.33)
		(end 0 -1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0d1844d8-3968-40e8-a883-14d5e2cea336")
	)
	(fp_line
		(start -1.33 0)
		(end -1.33 -1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f0354a49-62ac-41dc-8301-329bb549fb27")
	)
	(fp_line
		(start -1.33 1.27)
		(end -1.33 1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9785722f-c04d-4c74-9491-126777973d65")
	)
	(fp_line
		(start -1.33 1.27)
		(end 1.33 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "11d7a6c3-221d-4331-b595-0d9130e005e7")
	)
	(fp_line
		(start -1.33 1.33)
		(end 1.33 1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "79e2f484-8526-4235-8ecf-1b6fc52267cb")
	)
	(fp_line
		(start 1.33 1.27)
		(end 1.33 1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8acdf3e9-f57b-4971-921b-addfdd7d3c94")
	)
	(fp_line
		(start -1.8 -1.8)
		(end -1.8 1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8f0947d6-3894-4eae-bf45-a32c3dc2459d")
	)
	(fp_line
		(start -1.8 1.8)
		(end 1.8 1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5044617d-a06e-4e10-8542-74d0bf808891")
	)
	(fp_line
		(start 1.8 -1.8)
		(end -1.8 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f85def44-6cb2-4b98-be73-bc1b5313c4b5")
	)
	(fp_line
		(start 1.8 1.8)
		(end 1.8 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5949315c-51f8-4819-b018-03e8f8c7909c")
	)
	(fp_line
		(start -1.27 -0.635)
		(end -0.635 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "adc10770-1723-488c-8232-7f0ad2c7cace")
	)
	(fp_line
		(start -1.27 1.27)
		(end -1.27 -0.635)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1e1e093d-57ed-4801-8603-c7acae013741")
	)
	(fp_line
		(start -0.635 -1.27)
		(end 1.27 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e7d64334-39df-49f8-834e-0ac93da15a5b")
	)
	(fp_line
		(start 1.27 -1.27)
		(end 1.27 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1033fa55-0d33-4394-8b55-78af68f26749")
	)
	(fp_line
		(start 1.27 1.27)
		(end -1.27 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f25c5088-ca29-4940-8a9f-a773d953f951")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "6976de06-a21f-4558-b5c2-96b2fac0f546")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bf29d5b2-1ed9-48cf-a932-2258e5e431d0")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)