(footprint "Micro_Mate-N-Lok_4p_horizontal"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 6 0)
		(layer "F.SilkS")
		(uuid "ef50d2c1-0e62-4706-8b68-e2452d9c5fd4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Micro Mate-N-Lok 4-Pol"
		(at 0 -8 0)
		(layer "F.Fab")
		(uuid "bb457229-68b4-4b83-945a-637be1401348")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Micro_Mate-N-Lok_4p_horizontal"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "079d8040-4210-4d42-adbf-78df5555486a")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fcf75b4d-cf31-4938-8d91-98c96913608b")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "02b7c0b7-f2bc-4c4a-bbb9-ee95bd4e13a4")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -8 -6.6)
		(end 0 -6.6)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f4cd1fce-b403-45a3-a92a-3857709cb56c")
	)
	(fp_line
		(start -8 4.6)
		(end -8 -6.6)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3526fd5d-a8e6-4a27-aa45-32fef10ed55f")
	)
	(fp_line
		(start 0 -6.6)
		(end 8 -6.6)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "03f4dd16-8a03-420f-8a68-36191a32ffe4")
	)
	(fp_line
		(start 8 -6.6)
		(end 8 4.6)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d49171d5-f3c7-45c1-9821-1d65b3ba6318")
	)
	(fp_line
		(start 8 4.6)
		(end -8 4.6)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e8c1a284-6a9b-4d71-98eb-f0dd08599d22")
	)
	(pad "" smd rect
		(at -8.2 0.4)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "0a7c31da-37e8-4b35-b91e-598647bff19a")
	)
	(pad "" smd rect
		(at 8.21 0.4)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "7ef71d41-fba9-437b-be73-fcee65569b67")
	)
	(pad "1" smd rect
		(at -4.5 -5.08)
		(size 1.27 3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "0a9dc2f2-40cc-4fe5-91eb-a00b39df41b5")
	)
	(pad "2" smd rect
		(at -1.5 -5.08)
		(size 1.27 3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "cc7d6477-c8fd-4981-8d4d-d9bb40027ea3")
	)
	(pad "3" smd rect
		(at 1.5 -5.08)
		(size 1.27 3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "cf4238fc-03a7-4d24-8e80-fbb9fbba7c6c")
	)
	(pad "4" smd rect
		(at 4.5 -5.08)
		(size 1.27 3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "b087509a-c9dc-41f9-aa80-5f770222a1d3")
	)
	(model "${KIPRJMOD}/Symbol_Library/FaSTTUBe_connectors_3dmodels/Micro_Mate-N-Lok_4p_horizontal.stp"
		(offset
			(xyz 0 -5 2.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
