(footprint "Micro_Mate-N-Lok_2p_horizontal"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 7.6 0)
		(layer "F.SilkS")
		(uuid "b3717aae-6e72-4c5e-8a33-b309bc4120fe")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Micro Mate-N-Lok 2-Pol"
		(at 0 -6.22 0)
		(layer "F.Fab")
		(uuid "36e4278e-3a17-4a30-b25f-b47e619d8e54")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4afde509-61aa-4495-bea4-931c6d300cdc")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e13156ef-c15d-4d24-b178-c187d3564ad3")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d7224dbc-1065-41b6-82a1-ff9de5b98743")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -5 -5.4)
		(end 0 -5.4)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1c02454f-e74b-4db5-89ce-8549d76c156b")
	)
	(fp_line
		(start -5 6.2)
		(end -5 -5.4)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "79b7e7a7-54a5-4f04-ada0-5a78f329fb69")
	)
	(fp_line
		(start 0 -5.4)
		(end 5 -5.4)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a3f5f53b-a0a9-4632-9850-54b7a6125d67")
	)
	(fp_line
		(start 5 -5.4)
		(end 5 6.2)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "52aa1cc1-965b-412c-a19e-6434cee1a6e3")
	)
	(fp_line
		(start 5 6.2)
		(end -5 6.2)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e50755df-05fe-403a-adf5-a2d6e7cc5677")
	)
	(pad "" smd rect
		(at -5.2 1.6)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "c98ad03f-45fb-4c08-925c-a798f952439a")
	)
	(pad "" smd rect
		(at 5.21 1.6)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "1d1a1370-ddd7-4bd7-8fbf-a91b362cb160")
	)
	(pad "1" smd rect
		(at -1.5 -3.88)
		(size 1.27 3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "2291a95f-cda2-4dc8-88fc-a9b0f19ba741")
	)
	(pad "2" smd rect
		(at 1.5 -3.88)
		(size 1.27 3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "6df97d6c-664b-46c7-9be8-e97b286ece26")
	)
	(model "${KIPRJMOD}/Symbol_Library/FaSTTUBe_connectors_3dmodels/Micro_Mate-N-Lok_2p_horizontal.stp"
		(offset
			(xyz 0 -6.2 2.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)