(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "74LV08D" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LV08D" (id 1) (at 7.62 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mouser.de/datasheet/2/916/74LV08-1388983.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "And" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Quad And" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LV08D_1_1"
      (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LV08D_1_2"
      (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 3.81)
          (xy -0.635 3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.635 3.81)
          (xy -3.81 3.81)
          (xy -3.81 3.81)
          (xy -3.556 3.4036)
          (xy -3.0226 2.2606)
          (xy -2.6924 1.0414)
          (xy -2.6162 -0.254)
          (xy -2.7686 -1.4986)
          (xy -3.175 -2.7178)
          (xy -3.81 -3.81)
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width -25.4) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input inverted (at -7.62 2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 -2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LV08D_2_1"
      (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LV08D_2_2"
      (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 3.81)
          (xy -0.635 3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.635 3.81)
          (xy -3.81 3.81)
          (xy -3.81 3.81)
          (xy -3.556 3.4036)
          (xy -3.0226 2.2606)
          (xy -2.6924 1.0414)
          (xy -2.6162 -0.254)
          (xy -2.7686 -1.4986)
          (xy -3.175 -2.7178)
          (xy -3.81 -3.81)
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width -25.4) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input inverted (at -7.62 2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 -2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LV08D_3_1"
      (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input line (at -7.62 -2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LV08D_3_2"
      (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 3.81)
          (xy -0.635 3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.635 3.81)
          (xy -3.81 3.81)
          (xy -3.81 3.81)
          (xy -3.556 3.4036)
          (xy -3.0226 2.2606)
          (xy -2.6924 1.0414)
          (xy -2.6162 -0.254)
          (xy -2.7686 -1.4986)
          (xy -3.175 -2.7178)
          (xy -3.81 -3.81)
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width -25.4) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input inverted (at -7.62 -2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LV08D_4_1"
      (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LV08D_4_2"
      (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 3.81)
          (xy -0.635 3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.635 3.81)
          (xy -3.81 3.81)
          (xy -3.81 3.81)
          (xy -3.556 3.4036)
          (xy -3.0226 2.2606)
          (xy -2.6924 1.0414)
          (xy -2.6162 -0.254)
          (xy -2.7686 -1.4986)
          (xy -3.175 -2.7178)
          (xy -3.81 -3.81)
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width -25.4) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin output inverted (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 -2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LV08D_5_0"
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LV08D_5_1"
      (rectangle (start -5.08 7.62) (end 5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
  )
  (symbol "74LS09" (extends "74LV08D")
    (property "Reference" "U" (id 0) (at 3.81 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LS09" (id 1) (at 7.62 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS09" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "TTL and2 OpenCol" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Quad 2-input AND Open Collect" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "AZ1117-3Pin" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -3.81 4.445 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AZ1117-3Pin" (id 1) (at -1.27 4.445 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 0 6.35 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1A 20V Fixed LDO Linear Regulator, 1.2V, SOT-89/SOT-223/TO-220/TO-252/TO-263" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AZ1117-3Pin_0_1"
      (rectangle (start -5.08 2.54) (end 5.08 -5.08)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "AZ1117-3Pin_1_1"
      (pin power_in line (at 0 -7.62 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 0 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 0 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "AZ1117-4Pin" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -3.81 4.445 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AZ1117-4Pin" (id 1) (at 2.54 4.445 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 0 6.35 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1A 20V Fixed LDO Linear Regulator, 1.2V, SOT-89/SOT-223/TO-220/TO-252/TO-263" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AZ1117-4Pin_0_1"
      (rectangle (start -5.08 2.54) (end 5.08 -5.08)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "AZ1117-4Pin_1_1"
      (pin power_in line (at 1.27 -7.62 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 0 180) (length 2.54)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 0 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -1.27 5.08 270) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "AZ1117-1.5" (extends "AZ1117-4Pin")
    (property "Reference" "U" (id 0) (at -3.81 4.445 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AZ1117-1.5" (id 1) (at 2.54 4.445 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 0 6.35 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1A 20V Fixed LDO Linear Regulator, 1.5V, SOT-89/SOT-223/TO-220/TO-252/TO-263" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "AZ1117-1.8" (extends "AZ1117-4Pin")
    (property "Reference" "U" (id 0) (at -3.81 4.445 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AZ1117-1.8" (id 1) (at 2.54 4.445 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 0 6.35 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1A 20V Fixed LDO Linear Regulator, 1.8V, SOT-89/SOT-223/TO-220/TO-252/TO-263" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "AZ1117-2.5" (extends "AZ1117-4Pin")
    (property "Reference" "U" (id 0) (at -3.81 4.445 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AZ1117-2.5" (id 1) (at 2.54 4.445 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 0 6.35 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1A 20V Fixed LDO Linear Regulator, 2.5V, SOT-89/SOT-223/TO-220/TO-252/TO-263" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "AZ1117-2.85" (extends "AZ1117-4Pin")
    (property "Reference" "U" (id 0) (at -3.81 4.445 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AZ1117-2.85" (id 1) (at 2.54 4.445 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 0 6.35 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1A 20V Fixed LDO Linear Regulator, 2.85V, SOT-89/SOT-223/TO-220/TO-252/TO-263" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "AZ1117-3.3" (extends "AZ1117-4Pin")
    (property "Reference" "U" (id 0) (at -3.81 4.445 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AZ1117-3.3" (id 1) (at 2.54 4.445 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 0 6.35 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1A 20V Fixed LDO Linear Regulator, 3.3V, SOT-89/SOT-223/TO-220/TO-252/TO-263" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "AZ1117-5.0" (extends "AZ1117-4Pin")
    (property "Reference" "U" (id 0) (at -3.81 4.445 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AZ1117-5.0" (id 1) (at 2.54 4.445 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 0 6.35 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1A 20V Fixed LDO Linear Regulator, 5.0V, SOT-89/SOT-223/TO-220/TO-252/TO-263" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Binder-M12-12P" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -6.985 -5.715 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Binder-M12-12P" (id 1) (at 4.572 6.858 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf" (id 3) (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "circular DIN connector" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "8-pin DIN connector" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIN*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Binder-M12-12P_0_1"
      (circle (center -3.81 2.032) (radius 0.508)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center -1.016 -1.524) (radius 0.508)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center 0 -3.81) (radius 0.508)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -8.89 -2.54)
          (xy -6.35 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -8.89 2.54)
          (xy -6.35 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -5.08)
          (xy -2.54 -8.89)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 6.35)
          (xy -2.54 7.62)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.2446 -1.9558)
          (xy -2.54 -5.08)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -4.318)
          (xy 0 -8.89)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 2.54)
          (xy 0 1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 2.54)
          (xy 0 7.62)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.2192 -1.9812)
          (xy 2.54 -5.08)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -5.08)
          (xy 2.54 -8.89)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 6.35)
          (xy 2.54 7.62)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.35 -2.54)
          (xy 7.62 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.35 2.54)
          (xy 7.62 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -6.35 2.54)
          (xy -5.588 2.54)
          (xy -4.318 2.286)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.35 2.54)
          (xy 5.588 2.54)
          (xy 4.318 2.286)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center 0 0) (radius 6.35)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (circle (center 0 0.762) (radius 0.508)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center 1.016 -1.524) (radius 0.508)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center 3.81 2.032) (radius 0.508)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "Binder-M12-12P_1_1"
      (circle (center -3.81 -2.032) (radius 0.508)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center -3.81 0) (radius 0.508)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center -2.032 3.81) (radius 0.508)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -4.318 0)
          (xy -8.89 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.318 0)
          (xy 8.89 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -6.35 -2.54)
          (xy -5.588 -2.54)
          (xy -4.318 -2.286)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 6.35)
          (xy -2.54 5.588)
          (xy -2.286 4.318)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 6.35)
          (xy 2.54 5.588)
          (xy 2.286 4.318)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.35 -2.54)
          (xy 5.588 -2.54)
          (xy 4.318 -2.286)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center 2.032 3.81) (radius 0.508)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center 3.81 -2.032) (radius 0.508)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center 3.81 0) (radius 0.508)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin passive line (at -2.54 10.16 270) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 10.16 270) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -11.43 90) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -11.43 90) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 10.16 270) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -11.43 90) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -2.54 0) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 0 0) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 2.54 0) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Conn_02x02_Staggered_2xMountingPin" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at 0 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Conn_02x02_Staggered_2xMountingPin" (id 1) (at -19.05 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -1.27 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at -1.27 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "connector" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Generic connectable mounting pin connector, double row, 02x02, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Connector*:*_2x??-1MP*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Conn_02x02_Staggered_2xMountingPin_0_1"
      (circle (center 0 0) (radius 2.8448)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (circle (center 1.27 -1.27) (radius 0.3048)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "Conn_02x02_Staggered_2xMountingPin_1_1"
      (circle (center -1.27 -1.27) (radius 0.3048)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center -1.27 1.27) (radius 0.3048)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.286 -3.302)
          (xy -0.254 -3.302)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.254 -3.302)
          (xy 2.286 -3.302)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center 1.27 1.27) (radius 0.3048)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (text "Mounting" (at 0 -2.921 0)
        (effects (font (size 0.381 0.381)))
      )
      (pin passive line (at 6.35 -1.27 180) (length 3.81)
        (name "Pin_1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 6.35 1.27 180) (length 3.81)
        (name "Pin_2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -6.35 -1.27 0) (length 3.81)
        (name "Pin_3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -6.35 1.27 0) (length 3.81)
        (name "Pin_4" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -1.27 -7.62 90) (length 4.191)
        (name "MountPin1" (effects (font (size 1.27 1.27))))
        (number "MP1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 1.27 -7.62 90) (length 4.191)
        (name "MountPin2" (effects (font (size 1.27 1.27))))
        (number "MP2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LM3880" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM3880" (id 1) (at 3.81 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-6" (id 2) (at 16.51 -6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3880.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Power Sequencer" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Simple Power Sequencer, SOT-23-6" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM3880_0_1"
      (rectangle (start -7.62 5.08) (end 7.62 -5.08)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "LM3880_1_1"
      (pin power_in line (at 0 7.62 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 10.16 -2.54 180) (length 2.54)
        (name "FLAG3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 10.16 0 180) (length 2.54)
        (name "FLAG2" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 10.16 2.54 180) (length 2.54)
        (name "FLAG1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LM809" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 2.54 12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM809" (id 1) (at 5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 7.62 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm809.pdf" (id 3) (at 7.62 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "reset supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microprocessor Reset (active-low) Circuit, SOT-23" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM809_0_1"
      (rectangle (start 5.08 7.62) (end -5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "LM809_1_1"
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LM810" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 2.54 12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM810" (id 1) (at 5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 7.62 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm809.pdf" (id 3) (at 7.62 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "reset supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microprocessor Reset (active-high) Circuit, SOT-23" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM810_0_1"
      (rectangle (start 5.08 7.62) (end -5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "LM810_1_1"
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MAX6355" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -13.97 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX6355" (id 1) (at 11.43 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-6" (id 2) (at 0 -13.97 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6351-MAX6360.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Power Supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Voltage μP Supervisory Circuits, SOT-23-6" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX6355_0_1"
      (rectangle (start -15.24 7.62) (end 15.24 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MAX6355_1_1"
      (pin open_collector line (at 17.78 0 180) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 -5.08 0) (length 2.54)
        (name "~{MR}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 5.08 180) (length 2.54)
        (name "VCC2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 0 0) (length 2.54)
        (name "RSTIN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 5.08 0) (length 2.54)
        (name "VCC1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MAX6369" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -3.556 13.462 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX6369" (id 1) (at -6.604 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-8" (id 2) (at 16.51 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6369-MAX6374.pdf" (id 3) (at 3.81 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "watchdog supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Precision Pin-Selectable Watchdog Timer, 200us to 60s, SOT-23-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX6369_0_1"
      (rectangle (start -7.62 10.16) (end 7.62 -10.16)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MAX6369_1_1"
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "WDI" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 -5.08 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "SET0" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "SET1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "SET2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 10.16 5.08 180) (length 2.54)
        (name "~{WDO}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MAX6371" (extends "MAX6369")
    (property "Reference" "U" (id 0) (at -3.556 13.462 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX6371" (id 1) (at -6.604 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-8" (id 2) (at 16.51 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6369-MAX6374.pdf" (id 3) (at 3.81 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "watchdog supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Precision Pin-Selectable Watchdog Timer, 200us to 60s, SOT-23-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MAX6373" (extends "MAX6369")
    (property "Reference" "U" (id 0) (at -3.556 13.462 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX6373" (id 1) (at -6.604 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-8" (id 2) (at 16.51 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6369-MAX6374.pdf" (id 3) (at 3.81 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "watchdog supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Precision Pin-Selectable Watchdog Timer, 200us to 60s, SOT-23-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MAX6370" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -3.556 13.462 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX6370" (id 1) (at -6.604 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-8" (id 2) (at 16.51 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6369-MAX6374.pdf" (id 3) (at 3.81 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "watchdog supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Precision Pin-Selectable Watchdog Timer, 200us to 60s, SOT-23-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX6370_0_1"
      (rectangle (start -7.62 10.16) (end 7.62 -10.16)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MAX6370_1_1"
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "WDI" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 -5.08 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "SET0" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "SET1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "SET2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 5.08 180) (length 2.54)
        (name "~{WDO}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MAX6372" (extends "MAX6370")
    (property "Reference" "U" (id 0) (at -3.556 13.462 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX6372" (id 1) (at -6.604 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-8" (id 2) (at 16.51 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6369-MAX6374.pdf" (id 3) (at 3.81 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "watchdog supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Precision Pin-Selectable Watchdog Timer, 200us to 60s, SOT-23-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MAX6374" (extends "MAX6370")
    (property "Reference" "U" (id 0) (at -3.556 13.462 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX6374" (id 1) (at -6.604 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-8" (id 2) (at 16.51 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6369-MAX6374.pdf" (id 3) (at 3.81 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "watchdog supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Precision Pin-Selectable Watchdog Timer, 200us to 60s, SOT-23-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MAX691xPE" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -15.24 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX691xPE" (id 1) (at 3.81 13.97 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DIP:DIP-16_W7.62mm" (id 2) (at 0 -21.59 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX690-MAX695.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Power Supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microprocessor Supervisory Circuit, DIP-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX691xPE_0_1"
      (rectangle (start 16.51 12.7) (end -16.51 -15.24)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MAX691xPE_1_1"
      (pin power_in line (at -19.05 -6.35 0) (length 2.54)
        (name "VBATT" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 2.54 180) (length 2.54)
        (name "~{PFO}" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -2.54 0) (length 2.54)
        (name "WDI" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 -10.16 180) (length 2.54)
        (name "~{CE_OUT}" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -10.16 0) (length 2.54)
        (name "~{CE_IN}" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 -2.54 180) (length 2.54)
        (name "~{WDO}" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 7.62 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 5.08 180) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 19.05 -7.62 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 15.24 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -17.78 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 -5.08 180) (length 2.54)
        (name "BATT_ON" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 0 180) (length 2.54)
        (name "~{LOW_LINE}" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 3.81 0) (length 2.54)
        (name "OSC_IN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 1.27 0) (length 2.54)
        (name "OSC_SEL" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 6.35 0) (length 2.54)
        (name "PFI" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MAX691xWE" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -15.24 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX691xWE" (id 1) (at 5.08 13.97 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm" (id 2) (at 0 -21.59 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX690-MAX695.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Power Supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microprocessor Supervisory Circuit, SOIC-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX691xWE_0_1"
      (rectangle (start 16.51 12.7) (end -16.51 -15.24)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MAX691xWE_1_1"
      (pin power_in line (at -19.05 -6.35 0) (length 2.54)
        (name "VBATT" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 2.54 180) (length 2.54)
        (name "~{PFO}" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -2.54 0) (length 2.54)
        (name "WDI" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 -10.16 180) (length 2.54)
        (name "~{CE_OUT}" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -10.16 0) (length 2.54)
        (name "~{CE_IN}" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 -2.54 180) (length 2.54)
        (name "~{WDO}" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 7.62 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 5.08 180) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 19.05 -7.62 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 15.24 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -17.78 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 -5.08 180) (length 2.54)
        (name "BATT_ON" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 0 180) (length 2.54)
        (name "~{LOW_LINE}" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 3.81 0) (length 2.54)
        (name "OSC_IN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 1.27 0) (length 2.54)
        (name "OSC_SEL" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 6.35 0) (length 2.54)
        (name "PFI" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MC34064D" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -3.81 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MC34064D" (id 1) (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 0 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC34064-D.PDF" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Power Supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Undervoltage Sensing Circuit, SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MC34064D_0_1"
      (rectangle (start -6.35 -3.81) (end 6.35 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MC34064D_1_1"
      (pin open_collector line (at 8.89 1.27 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 1.27 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 6.35 -2.54 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -6.35 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 3.81 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 3.81 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -6.35 -2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 3.81 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MC34064DM" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -3.81 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MC34064DM" (id 1) (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm" (id 2) (at 0 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC34064-D.PDF" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Power Supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Undervoltage Sensing Circuit, MSOP-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MC34064DM_0_1"
      (rectangle (start -6.35 -3.81) (end 6.35 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MC34064DM_1_1"
      (pin open_collector line (at 8.89 1.27 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 1.27 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 6.35 -2.54 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -6.35 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 3.81 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 3.81 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -6.35 -2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 3.81 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MC34064P" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MC34064P" (id 1) (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-92L_Inline" (id 2) (at 0 -12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC34064-D.PDF" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Power Supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Undervoltage Sensing Circuit, TO-92" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?92L?Inline*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MC34064P_0_1"
      (rectangle (start -6.35 -5.08) (end 6.35 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MC34064P_1_1"
      (pin open_collector line (at 8.89 1.27 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 1.27 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -7.62 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MC34064SN" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MC34064SN" (id 1) (at 6.35 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:TSOP-5_1.65x3.05mm_P0.95mm" (id 2) (at 0 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC34064-D.PDF" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Power Supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Undervoltage Sensing Circuit, TSOP-5" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TSOP*1.65x3.05mm*P0.95mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MC34064SN_0_1"
      (rectangle (start -6.35 -3.81) (end 6.35 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MC34064SN_1_1"
      (pin power_in line (at 0 -6.35 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 1.27 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 8.89 1.27 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 3.81 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 3.81 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MC74HC1G00" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MC74HC1G00" (id 1) (at 7.62 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mouser.de/datasheet/2/308/1/MC74HC1G00_D-2315437.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "nand" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single 2-input NAND gate" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm* SO14*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MC74HC1G00_1_1"
      (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -1.27 -6.35 90) (length 2.54)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 6.35 270) (length 2.54)
        (name "VCC" (effects (font (size 0.9906 0.9906))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "MC74HC1G00_1_2"
      (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 3.81)
          (xy -0.635 3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.635 3.81)
          (xy -3.81 3.81)
          (xy -3.81 3.81)
          (xy -3.556 3.4036)
          (xy -3.0226 2.2606)
          (xy -2.6924 1.0414)
          (xy -2.6162 -0.254)
          (xy -2.7686 -1.4986)
          (xy -3.175 -2.7178)
          (xy -3.81 -3.81)
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width -25.4) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input inverted (at -7.62 2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 -2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "7400" (extends "MC74HC1G00")
    (property "Reference" "U" (id 0) (at 1.27 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "7400" (id 1) (at 7.62 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn7400" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "TTL nand 2-input" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "quad 2-input NAND gate" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm* SO14*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74HC00" (extends "MC74HC1G00")
    (property "Reference" "U" (id 0) (at 1.27 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74HC00" (id 1) (at 7.62 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74hc00" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "HCMOS nand 2-input" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "quad 2-input NAND gate" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm* SO14*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74HCT00" (extends "MC74HC1G00")
    (property "Reference" "U" (id 0) (at 1.27 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74HCT00" (id 1) (at 7.62 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74hct00" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "HCTMOS nand 2-input" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "quad 2-input NAND gate" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm* SO14*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LS37" (extends "MC74HC1G00")
    (property "Reference" "U" (id 0) (at 1.27 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LS37" (id 1) (at 7.62 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74ls37" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "TTL nand 2-input buffer" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "quad 2-input NAND buffer" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm* SO14*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MC74HC1G32" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MC74HC1G32" (id 1) (at 8.89 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mouser.de/datasheet/2/308/1/MC74HC1G32_D-2315545.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Or" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single 2-input OR" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP?14*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MC74HC1G32_1_1"
      (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 3.81)
          (xy -0.635 3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.635 3.81)
          (xy -3.81 3.81)
          (xy -3.81 3.81)
          (xy -3.556 3.4036)
          (xy -3.0226 2.2606)
          (xy -2.6924 1.0414)
          (xy -2.6162 -0.254)
          (xy -2.7686 -1.4986)
          (xy -3.175 -2.7178)
          (xy -3.81 -3.81)
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width -25.4) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -1.27 -6.35 90) (length 2.54)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 6.35 270) (length 2.54)
        (name "VCC" (effects (font (size 0.9906 0.9906))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "MC74HC1G32_1_2"
      (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input inverted (at -7.62 2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 -2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MCP100-270D" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP100-270D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 2.70V threshold, active low output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MCP100-270D_1_1"
      (rectangle (start -5.08 7.62) (end 5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 10.16 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -10.16 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MCP100-300D" (extends "MCP100-270D")
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP100-300D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 3.00V threshold, active low output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP100-315D" (extends "MCP100-270D")
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP100-315D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 3.15V threshold, active low output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP100-450D" (extends "MCP100-270D")
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP100-450D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 4.50V threshold, active low output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP100-460D" (extends "MCP100-270D")
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP100-460D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 4.60V threshold, active low output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP100-475D" (extends "MCP100-270D")
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP100-475D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 4.75V threshold, active low output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP100-485D" (extends "MCP100-270D")
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP100-485D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 4.85V threshold, active low output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP101-270D" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP101-270D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 2.70V threshold, active high output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MCP101-270D_1_1"
      (rectangle (start -5.08 7.62) (end 5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "RST" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 10.16 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -10.16 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MCP101-300D" (extends "MCP101-270D")
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP101-300D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 3.00V threshold, active high output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP101-315D" (extends "MCP101-270D")
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP101-315D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 3.15V threshold, active high output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP101-450D" (extends "MCP101-270D")
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP101-450D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 4.50V threshold, active high output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP101-460D" (extends "MCP101-270D")
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP101-460D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 4.60V threshold, active high output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP101-475D" (extends "MCP101-270D")
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP101-475D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 4.75V threshold, active high output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP101-485D" (extends "MCP101-270D")
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP101-485D" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, 4.85V threshold, active high output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* TO?92*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP120-xxxDxTO" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.08 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MCP120-xxxDxTO" (id 1) (at 8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 16.51 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisory circuit" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller supervisory circuit, TO-92" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO*92*Inline*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MCP120-xxxDxTO_0_1"
      (rectangle (start 5.08 7.62) (end -5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "MCP120-xxxDxTO_1_1"
      (pin open_collector line (at 7.62 0 180) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MCP130-xxxDxTO" (extends "MCP120-xxxDxTO")
    (property "Reference" "U" (id 0) (at -5.08 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MCP130-xxxDxTO" (id 1) (at 8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 16.51 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisory circuit pull-up" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller supervisory circuit with internal 5 kΩ pull-up, TO-92" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO*92*Inline*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP120-xxxGxTO" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.08 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MCP120-xxxGxTO" (id 1) (at 8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 16.51 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisory circuit" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller supervisory circuit, TO-92" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO*92*Inline*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MCP120-xxxGxTO_0_1"
      (rectangle (start 5.08 7.62) (end -5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MCP120-xxxGxTO_1_1"
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 7.62 0 180) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MCP120-xxxHxTO" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.08 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MCP120-xxxHxTO" (id 1) (at 8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 16.51 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisory circuit" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller supervisory circuit, TO-92" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO*92*Inline*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MCP120-xxxHxTO_0_1"
      (rectangle (start 5.08 7.62) (end -5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MCP120-xxxHxTO_1_1"
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 7.62 0 180) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MCP130-xxxHxTO" (extends "MCP120-xxxHxTO")
    (property "Reference" "U" (id 0) (at -5.08 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MCP130-xxxHxTO" (id 1) (at 8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 16.51 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisory circuit pull-up" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller supervisory circuit with internal 5 kΩ pull-up, TO-92" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO*92*Inline*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP120-xxxxSN" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.08 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MCP120-xxxxSN" (id 1) (at 8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 20.32 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisory circuit" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller supervisory circuit, SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MCP120-xxxxSN_0_1"
      (rectangle (start 5.08 7.62) (end -5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MCP120-xxxxSN_1_1"
      (pin open_collector line (at 7.62 0 180) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -5.08 5.08 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -5.08 2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -5.08 0 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -5.08 -2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -5.08 -5.08 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MCP130-xxxxSN" (extends "MCP120-xxxxSN")
    (property "Reference" "U" (id 0) (at -5.08 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MCP130-xxxxSN" (id 1) (at 8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 20.32 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisory circuit pull-up" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller supervisory circuit with internal 5 kΩ pull-up, SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP120-xxxxTT" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.08 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MCP120-xxxxTT" (id 1) (at 8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 15.24 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisory circuit" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller supervisory circuit, SOT-23" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MCP120-xxxxTT_0_1"
      (rectangle (start 5.08 7.62) (end -5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MCP120-xxxxTT_1_1"
      (pin open_collector line (at 7.62 0 180) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MCP130-xxxxTT" (extends "MCP120-xxxxTT")
    (property "Reference" "U" (id 0) (at -5.08 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MCP130-xxxxTT" (id 1) (at 8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 15.24 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisory circuit pull-up" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller supervisory circuit with internal 5 kΩ pull-up, SOT-23" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MCP130-xxxFxTO" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.08 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MCP130-xxxFxTO" (id 1) (at 8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 16.51 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisory circuit pull-up" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller supervisory circuit with internal 5 kΩ pull-up, TO-92" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO*92*Inline*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MCP130-xxxFxTO_0_1"
      (rectangle (start 5.08 7.62) (end -5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "MCP130-xxxFxTO_1_1"
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 7.62 0 180) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MCP39F521" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -11.43 19.05 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MCP39F521" (id 1) (at 8.89 19.05 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm" (id 2) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005442A.pdf" (id 3) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "i2c power monitor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power Monitor, Calculation and Energy Accumulation, I2C, 16-bit, QFN-28" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MCP39F521_0_1"
      (rectangle (start -12.7 17.78) (end 12.7 -20.32)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MCP39F521_1_1"
      (pin output line (at 15.24 -2.54 180) (length 2.54)
        (name "EVENT" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 15.24 0) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 20.32 270) (length 2.54)
        (name "AVDD" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 10.16 180) (length 2.54)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 5.08 180) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 7.62 180) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 10.16 0) (length 2.54)
        (name "I1+" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 7.62 0) (length 2.54)
        (name "I1-" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 2.54 0) (length 2.54)
        (name "V1-" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 5.08 0) (length 2.54)
        (name "V1+" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -12.7 12.7 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -10.16 0) (length 2.54)
        (name "AN_IN" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -22.86 90) (length 2.54)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 -5.08 180) (length 2.54)
        (name "ZCD" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
        (name "REFIN+/OUT" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -22.86 90) (length 2.54)
        (name "DGND" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 20.32 270) (length 2.54)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 15.24 180) (length 2.54)
        (name "~{MCLR}" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -22.86 90) (length 2.54) hide
        (name "DGND" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 -15.24 180) (length 2.54)
        (name "~{DR}" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -22.86 90) (length 2.54) hide
        (name "DGND" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -12.7 0 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -15.24 -5.08 0) (length 2.54)
        (name "COMMON_B" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -15.24 -2.54 0) (length 2.54)
        (name "COMMON_A" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -15.24 0) (length 2.54)
        (name "OSCI" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -15.24 -17.78 0) (length 2.54)
        (name "OSCO" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 12.7 12.7 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 12.7 0 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MIC811LUY" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MIC811LUY" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic811.pdf" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 4.63V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MIC811LUY_0_1"
      (rectangle (start -7.62 5.08) (end 7.62 -5.08)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MIC811LUY_1_1"
      (pin power_in line (at 0 -7.62 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "~{MR}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 7.62 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "CAT811JTBI-GT3" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "CAT811JTBI-GT3" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 4.00V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "CAT811LTBI-GT3" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "CAT811LTBI-GT3" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 4.63V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "CAT811MTBI-GT3" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "CAT811MTBI-GT3" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 4.38V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "CAT811RTBI-GT3" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "CAT811RTBI-GT3" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 2.63V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "CAT811STBI-GT3" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "CAT811STBI-GT3" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 2.93V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "CAT811TTBI-GT3" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "CAT811TTBI-GT3" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 3.08V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "CAT811ZTBI-GT3" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "CAT811ZTBI-GT3" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 2.32V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MAX811LEUS-T" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MAX811LEUS-T" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX811-MAX812.pdf" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 4.63V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MAX811MEUS-T" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MAX811MEUS-T" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX811-MAX812.pdf" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 4.38V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MAX811REUS-T" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MAX811REUS-T" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX811-MAX812.pdf" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 2.63V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MAX811SEUS-T" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MAX811SEUS-T" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX811-MAX812.pdf" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 2.93V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MAX811TEUS-T" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MAX811TEUS-T" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX811-MAX812.pdf" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 3.08V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MIC811JUY" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MIC811JUY" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic811.pdf" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 4.00V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MIC811MUY" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MIC811MUY" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic811.pdf" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 4.38V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MIC811RUY" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MIC811RUY" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic811.pdf" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 2.63V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MIC811SUY" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MIC811SUY" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic811.pdf" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 2.93V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MIC811TUY" (extends "MIC811LUY")
    (property "Reference" "U" (id 0) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MIC811TUY" (id 1) (at 1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-143" (id 2) (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic811.pdf" (id 3) (at -8.89 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Supervisor Reset" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Power supply supervisor, Manual reset, Threshold 3.08V, SOT-143" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*143*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "NL17SZ157" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 15.24 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "NL17SZ157" (id 1) (at 0 12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "NL17SZ157_1_1"
      (rectangle (start -5.08 6.35) (end 5.08 -6.35)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input line (at -7.62 -3.81 0) (length 2.54)
        (name "I1" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 0 -8.89 90) (length 2.54)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -7.62 -1.27 0) (length 2.54)
        (name "I0" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "Z" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 0 8.89 270) (length 2.54)
        (name "VCC" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -7.62 3.81 0) (length 2.54)
        (name "S" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
    )
  )
  (symbol "TCM809" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TCM809" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21661E.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, active low output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* *SC?70*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TCM809_1_1"
      (rectangle (start -5.08 7.62) (end 5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at -2.54 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 10.16 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TCM810" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TCM810" (id 1) (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at -10.16 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21661E.pdf" (id 3) (at -7.62 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supervisor reset push-pull" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller reset monitor, active high output" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* *SC?70*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TCM810_1_1"
      (rectangle (start -5.08 7.62) (end 5.08 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at -2.54 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 10.16 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TL7702A" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TL7702A" (id 1) (at 10.16 8.89 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Supply-Voltage Supervisors, 2.53V, PDIP-8/SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TL7702A_0_1"
      (rectangle (start -10.16 7.62) (end 10.16 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TL7702A_1_1"
      (pin output line (at 12.7 -5.08 180) (length 2.54)
        (name "REF" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 2.54)
        (name "~{RESIN}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -5.08 0) (length 2.54)
        (name "CT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 12.7 5.08 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 12.7 0 180) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 2.54)
        (name "SENSE" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TL7702B" (extends "TL7702A")
    (property "Reference" "U" (id 0) (at -8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TL7702B" (id 1) (at 10.16 8.89 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705b.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Supply-Voltage Supervisors, 2.53V, PDIP-8/SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TL7705A" (extends "TL7702A")
    (property "Reference" "U" (id 0) (at -8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TL7705A" (id 1) (at 10.16 8.89 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Supply-Voltage Supervisors, 4.55V, PDIP-8/SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TL7705B" (extends "TL7702A")
    (property "Reference" "U" (id 0) (at -8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TL7705B" (id 1) (at 10.16 8.89 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705b.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Supply-Voltage Supervisors, 4.55V, PDIP-8/SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TL7709A" (extends "TL7702A")
    (property "Reference" "U" (id 0) (at -8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TL7709A" (id 1) (at 10.16 8.89 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Supply-Voltage Supervisors, 7.6V, PDIP-8/SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TL7712A" (extends "TL7702A")
    (property "Reference" "U" (id 0) (at -8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TL7712A" (id 1) (at 10.16 8.89 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Supply-Voltage Supervisors, 10.8V, PDIP-8/SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TL7715A" (extends "TL7702A")
    (property "Reference" "U" (id 0) (at -8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TL7715A" (id 1) (at 10.16 8.89 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Supply-Voltage Supervisors, 13.5V, PDIP-8/SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TL7733B" (extends "TL7702A")
    (property "Reference" "U" (id 0) (at -8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TL7733B" (id 1) (at 10.16 8.89 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705b.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Supply-Voltage Supervisors, 3.08V, PDIP-8/SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TL7705ACPSR" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -8.89 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TL7705ACPSR" (id 1) (at 10.16 8.89 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "Package_SO:SO-8_5.3x6.2mm_P1.27mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Supply-Voltage Supervisors, 4.55V, SO-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SO*5.3x6.2mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TL7705ACPSR_0_1"
      (rectangle (start -10.16 7.62) (end 10.16 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TL7705ACPSR_1_1"
      (pin output line (at 12.7 -5.08 180) (length 2.54)
        (name "REF" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 2.54)
        (name "~{RESIN}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -5.08 0) (length 2.54)
        (name "CT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 12.7 5.08 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 12.7 0 180) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 2.54)
        (name "SENSE" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TPS3702" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -6.35 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TPS3702" (id 1) (at 6.35 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-6" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps3702.pdf" (id 3) (at -10.16 10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "protection overvoltage unvervoltage monitor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "High-Accuracy, Overvoltage and Undervoltage Monitor, SOT-23-6" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS3702_0_1"
      (rectangle (start -7.62 5.08) (end 7.62 -5.08)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TPS3702_1_1"
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "UV" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "SENSE" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "SET" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 7.62 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 2.54 180) (length 2.54)
        (name "OV" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TPS3808DBV" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TPS3808DBV" (id 1) (at 0 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-6" (id 2) (at -2.54 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps3808.pdf" (id 3) (at -2.54 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supply voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low-Quiescent-Current, Programmable-Delay Supervisory Circuit, SOT-23-6" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS3808DBV_0_1"
      (rectangle (start -7.62 5.08) (end 7.62 -5.08)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TPS3808DBV_1_1"
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "~{MR}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "CT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "SENSE" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 7.62 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TPS3831" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 2.54 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TPS3831" (id 1) (at 2.54 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SON:Texas_X2SON-4_1x1mm_P0.65mm" (id 2) (at 0 -15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/sbvs193d/sbvs193d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supply voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "150-nA, Ultralow Power, Supply Voltage Monitor, X2SON-4" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Texas*X2SON*1x1mm*P0.65mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS3831_0_1"
      (rectangle (start -5.08 5.08) (end 7.62 -5.08)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TPS3831_1_1"
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "~{MR}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 7.62 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -7.62 90) (length 2.54)
        (name "TP" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TPS3839DBZ" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 2.54 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TPS3839DBZ" (id 1) (at 2.54 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/sbvs193d/sbvs193d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supply voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "150-nA, Ultralow Power, Supply Voltage Monitor, SOT-23" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS3839DBZ_0_1"
      (rectangle (start -2.54 5.08) (end 7.62 -5.08)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TPS3839DBZ_1_1"
      (pin power_in line (at 0 -7.62 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 7.62 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TPS3839DQN" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 2.54 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TPS3839DQN" (id 1) (at 2.54 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SON:Texas_X2SON-4_1x1mm_P0.65mm" (id 2) (at 0 -15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/sbvs193d/sbvs193d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "supply voltage supervisor" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "150-nA, Ultralow Power, Supply Voltage Monitor, X2SON-4" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Texas*X2SON*1x1mm*P0.65mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS3839DQN_0_1"
      (rectangle (start -2.54 5.08) (end 7.62 -5.08)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TPS3839DQN_1_1"
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 0 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 7.62 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -7.62 90) (length 2.54)
        (name "TP" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "UCC2946" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 15.24 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "UCC2946" (id 1) (at 0 12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "UCC2946_0_1"
      (rectangle (start -6.35 7.62) (end 6.35 -7.62)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "UCC2946_1_1"
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 5.08 0) (length 2.54)
        (name "RTH" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 8.89 3.81 180) (length 2.54)
        (name "~{RES}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 2.54 0) (length 2.54)
        (name "RP" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 8.89 -3.81 180) (length 2.54)
        (name "~{WDO}" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 -2.54 0) (length 2.54)
        (name "WP" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 -5.08 0) (length 2.54)
        (name "WDI" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
