(footprint "APEM-ISx3SAD_NoSilk" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61C621C8)
  (descr "Sealed pushbutton switch")
  (tags "ISR3AD, ISP3AD")
  (property "Sheetfile" "buttons.kicad_sch")
  (property "Sheetname" "Buttons")
  (attr through_hole)
  (fp_text reference "AMC1" (at 9 0.333334 90) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f4411b4c-3b05-437e-8121-f36a1e7385cc)
  )
  (fp_text value "SW_Push" (at 0 -11.43 180) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f7678448-59ce-423d-9ac9-1ab76125b847)
  )
  (fp_circle (center 0 0) (end 8 0) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 092b614f-ec5f-4c70-b62a-9a73c6a6093e))
  (pad "1" thru_hole roundrect (at -2.54 0) (size 1.6 4) (drill oval 1 3.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp c07c5d16-3194-4e72-b4b3-f4bf0a0e5afd))
  (pad "2" thru_hole roundrect (at 2.54 0) (size 1.6 4) (drill oval 1 3.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp a47a5593-e189-48e9-b869-6a1feeac1d20))
  (model "${KIPRJMOD}/packages3d/Binder.3dshapes/APEM-ISx3SAD.stp"
    (offset (xyz 0 0 10.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 180 0 0))
  )
)
