(footprint "APEM-ISx3SAD" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61C621C8)
  (descr "Sealed pushbutton switch")
  (tags "ISR3AD, ISP3AD")
  (attr through_hole)
  (fp_text reference "BTN501" (at 0 -9.33) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4bbb7a56-8979-4d46-b19f-b3fabc0536c5)
  )
  (fp_text value "SW_Push" (at 0 -11.43) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 734347db-23d4-41fa-9688-637554ee1b59)
  )
  (fp_circle (center 0 0) (end 0 -7.5) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 1068cfac-4c4c-4d8b-8b09-85cb7363f1d8))
  (fp_circle (center 0 0) (end 8 0) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp eb82c349-2a66-4750-936b-b1a6bacea06b))
  (pad "1" thru_hole roundrect (at -2.54 0) (size 1.6 4) (drill oval 1 3.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp ace15fec-d222-4d10-8b2d-a093a6c81fb8))
  (pad "2" thru_hole roundrect (at 2.54 0) (size 1.6 4) (drill oval 1 3.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 892f0ac5-b430-401b-a8db-74d309cd8e3e))
  (model "${KIPRJMOD}/packages3d/Binder.3dshapes/APEM-ISx3SAD.stp"
    (offset (xyz 0 0 10.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 180 0 0))
  )
)
