(footprint "CP_Combo_15.0mm_5mm_P2.00mm_Horizontal_Slotted" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 2 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp db485260-35d1-41c6-be48-e09046f649b8)
  )
  (fp_text value "CP_Combo_15.0mm_5mm_P2.00mm_Horizontal_Slotted" (at 0 3.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 246fc9a1-9c36-4bbf-9fff-b66f34fade67)
  )
  (fp_text user "+" (at 2.25 -0.5 180 unlocked) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp f8a2f6d5-a7f8-4fcb-85e8-9d7508ce0240)
  )
  (fp_text user "${REFERENCE}" (at 0 2 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c0abae27-2668-4ef9-8429-e39a830481bc)
  )
  (fp_line (start 3.75 -4.5) (end 3 -3.75) (layer "F.SilkS") (width 0.12) (tstamp 3f154e81-080a-4eac-94e2-a57b350c2978))
  (fp_line (start -1.25 -16.75) (end -1.25 -18.25) (layer "F.SilkS") (width 0.4) (tstamp 7b507eed-8efb-4822-8cc7-aadfe799d0bb))
  (fp_line (start -2.5 0.75) (end -2.5 -0.75) (layer "F.SilkS") (width 0.4) (tstamp 8146c854-8a94-460e-91f6-0d5e97e5069d))
  (fp_line (start -3.75 -3) (end -3 -3.75) (layer "F.SilkS") (width 0.12) (tstamp af55e5ed-2cb9-4283-916f-1f6f4377ede1))
  (fp_line (start 3 -3.75) (end 3.75 -3) (layer "F.SilkS") (width 0.12) (tstamp e0064674-cc27-4394-b555-ccf9d18d0f44))
  (fp_line (start -3 -3.75) (end -3.75 -4.5) (layer "F.SilkS") (width 0.12) (tstamp f90baa84-3a74-47be-99d1-5aa261a5b253))
  (fp_rect (start -2.75 -16.25) (end 2.75 -1.25) (layer "Edge.Cuts") (width 0.12) (fill none) (tstamp 45b4ef61-88f6-4eb4-8106-9ca3e87943e7))
  (fp_line (start -3 -16.5) (end -3 -1) (layer "F.CrtYd") (width 0.05) (tstamp 158a813d-1c38-493d-ae26-da4960da326a))
  (fp_line (start 2.25 -1) (end 3 -1) (layer "F.CrtYd") (width 0.05) (tstamp 20a46376-a7b0-4b8f-8d35-33fed3bd5c52))
  (fp_line (start 3 -1) (end 3 -16.5) (layer "F.CrtYd") (width 0.05) (tstamp 4e4564d4-30dc-42d8-9169-d8b4985bb924))
  (fp_line (start -1.25 -19) (end -1.25 -16.5) (layer "F.CrtYd") (width 0.05) (tstamp 5c14fbda-342b-4e02-9e99-f9a56ee4fbd2))
  (fp_line (start -3 -1) (end -2.5 -1) (layer "F.CrtYd") (width 0.05) (tstamp 63d523a4-bc5c-4bcf-8fbb-2e596efb2e15))
  (fp_line (start -1.25 -16.5) (end -3 -16.5) (layer "F.CrtYd") (width 0.05) (tstamp 6fe169c0-13c3-483a-abdc-523a9de1b1fb))
  (fp_line (start -2.5 1.5) (end 2.25 1.5) (layer "F.CrtYd") (width 0.05) (tstamp c15b8e1d-4556-4949-ab84-bbb9f7611ffe))
  (fp_line (start 2.25 1.5) (end 2.25 -1) (layer "F.CrtYd") (width 0.05) (tstamp ca531509-0e26-4dc6-acdc-cbf73428037b))
  (fp_line (start -2.5 -1) (end -2.5 1.5) (layer "F.CrtYd") (width 0.05) (tstamp d4fc26ad-e5f8-4a7c-9265-a8a2d5118e4f))
  (fp_line (start 1.25 -16.5) (end 1.25 -19) (layer "F.CrtYd") (width 0.05) (tstamp eb7f73eb-789c-4acc-b242-b7ee49bf7bcd))
  (fp_line (start 3 -16.5) (end 1.25 -16.5) (layer "F.CrtYd") (width 0.05) (tstamp f2492c82-6691-4ffa-bd53-1594e3108b16))
  (fp_line (start 1.25 -19) (end -1.25 -19) (layer "F.CrtYd") (width 0.05) (tstamp f5d4ca73-c617-49d6-a4f8-11478234f86f))
  (pad "1" smd roundrect (at 0.75 0 90) (size 2 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 78de7dd2-ad59-4066-a037-c0adc5c5f761))
  (pad "2" smd roundrect (at -1.25 0 90) (size 2 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 0b22ec7a-796a-44ce-a329-1d243662c897))
  (pad "2" smd roundrect (at 0 -17.5 90) (size 2 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 848ac8c0-db8e-4c72-a57f-78222a82f4cd))
  (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D5.0mm_P18.00mm_Horizontal.step"
    (offset (xyz 2.9 0 -0.8))
    (scale (xyz 1 1 1))
    (rotate (xyz 75 0 -93))
  )
)
