(footprint "CP_Radial_10.0mm_4.5mm_P2.00mm_Horizontal_Slotted" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 1 2 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp db485260-35d1-41c6-be48-e09046f649b8)
  )
  (fp_text value "CP_Radial_10.0mm_4.5mm_P2.00mm_Horizontal_Slotted" (at 1 3.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 246fc9a1-9c36-4bbf-9fff-b66f34fade67)
  )
  (fp_text user "+" (at 3.25 -0.5 unlocked) (layer "B.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
    (tstamp c78985b3-9572-4caf-b990-86ab9120fc63)
  )
  (fp_text user "+" (at 3.25 -0.5 unlocked) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp f8a2f6d5-a7f8-4fcb-85e8-9d7508ce0240)
  )
  (fp_text user "${REFERENCE}" (at 1 2 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c0abae27-2668-4ef9-8429-e39a830481bc)
  )
  (fp_line (start -1.25 -0.75) (end -1.25 0.75) (layer "B.SilkS") (width 0.4) (tstamp f1521435-82eb-4f42-a627-5dffbe900568))
  (fp_line (start -1.25 -0.75) (end -1.25 0.75) (layer "F.SilkS") (width 0.4) (tstamp 7b507eed-8efb-4822-8cc7-aadfe799d0bb))
  (fp_rect (start 3.75 -1.25) (end -1.75 -13.75) (layer "Edge.Cuts") (width 0.12) (fill none) (tstamp 45b4ef61-88f6-4eb4-8106-9ca3e87943e7))
  (pad "1" smd roundrect (at 2 0 270) (size 2 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 78de7dd2-ad59-4066-a037-c0adc5c5f761))
  (pad "2" smd roundrect (at 0 0 270) (size 2 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 848ac8c0-db8e-4c72-a57f-78222a82f4cd))
  (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D5.0mm_H11.0mm_P2.00mm.step"
    (offset (xyz 0 2 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 0 0))
  )
)
