(footprint "Pogo_pins"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "1a594914-9fb3-47d8-89c2-873a10f4c61e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Pogo_pins"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "bb936fe0-28d1-4cbf-8fd6-3aac44a7b2bf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6b0e922a-4b10-4960-a1b9-d0c54d86528d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c3824025-46d8-4e06-b01f-717014cd9c53")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "680d7bdd-bdbf-411f-bd5e-18ae6338edb9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a9139022-458d-4b3b-9c85-a9a82598219b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd circle
		(at -5 0)
		(size 2.2 2.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "b5d7b1c6-45e1-4bb7-8369-6a1829089cec")
	)
	(pad "2" smd circle
		(at -2.5 0)
		(size 2.2 2.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "0f393125-ffd9-4f54-be69-f3648c9e05d3")
	)
	(pad "3" smd circle
		(at 0 0)
		(size 2.2 2.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "b33886b0-aca4-4cd3-91cf-c581387b0117")
	)
	(pad "4" smd circle
		(at 2.5 0)
		(size 2.2 2.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "d90541ba-cdf6-4ff0-a920-de944c839a07")
	)
	(pad "5" smd circle
		(at 5 0)
		(size 2.2 2.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "ddabb402-b5c9-48f0-bab3-44fc66dc83ce")
	)
)