(module "SOP65P640X120-14N" (layer F.Cu)
  (descr "PW (R-PDSO-G14)")
  (tags "Integrated Circuit")
  (attr smd)
  (fp_text reference IC** (at 0 0) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text value "SOP65P640X120-14N" (at 0 0) (layer F.SilkS) hide
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_line (start -3.925 -2.8) (end 3.925 -2.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.925 -2.8) (end 3.925 2.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.925 2.8) (end -3.925 2.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.925 2.8) (end -3.925 -2.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.2 -2.5) (end 2.2 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start 2.2 -2.5) (end 2.2 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start 2.2 2.5) (end -2.2 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.2 2.5) (end -2.2 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.2 -1.85) (end -1.55 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.85 -2.5) (end 1.85 -2.5) (layer F.SilkS) (width 0.2))
  (fp_line (start 1.85 -2.5) (end 1.85 2.5) (layer F.SilkS) (width 0.2))
  (fp_line (start 1.85 2.5) (end -1.85 2.5) (layer F.SilkS) (width 0.2))
  (fp_line (start -1.85 2.5) (end -1.85 -2.5) (layer F.SilkS) (width 0.2))
  (fp_line (start -3.675 -2.525) (end -2.2 -2.525) (layer F.SilkS) (width 0.2))
  (pad 1 smd rect (at -2.938 -1.95 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.938 -1.3 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.938 -0.65 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.938 0 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -2.938 0.65 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -2.938 1.3 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -2.938 1.95 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 2.938 1.95 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 2.938 1.3 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 2.938 0.65 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 2.938 0 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 2.938 -0.65 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 2.938 -1.3 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 2.938 -1.95 90) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
  (model TLV9004IPWR.stp
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
