(footprint "CPG-03-SMT-TR"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "2f0755a1-3ac9-4ab6-bda9-87f2025d59c2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "CPG-03-SMT-TR"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "894bae94-a028-45d2-9934-d49cc105bbc3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a366a178-061e-4b15-92fb-2b2c570df59e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7f97ee51-461d-4e3c-a8bd-7d7b6c2f201f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6b69307d-75fd-494f-b369-2ffb01621cbd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -6.2 -1.3)
		(end -6.2 1.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ed10e991-8d1b-40fe-81c6-9d4a3cc3593b")
	)
	(fp_line
		(start 6.2 -1.3)
		(end 6.2 1.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d29d9e88-b7fa-40e3-b561-6fc0e828384a")
	)
	(fp_rect
		(start -6.2 -1.3)
		(end 6.2 1.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "7ad65d33-a0d3-4d43-a0fd-db25cde92826")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "fd2eb63f-c8c5-42bd-b3aa-6074ff863950")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -5 0)
		(size 1 2.2)
		(layers "F.Cu" "F.Mask")
		(uuid "9c9634a0-661e-4828-ad89-7bb55c2d2abb")
	)
	(pad "2" smd rect
		(at -2.5 0)
		(size 1 2.2)
		(layers "F.Cu" "F.Mask")
		(uuid "b5452b20-0828-4365-8970-1d99cb042c70")
	)
	(pad "3" smd rect
		(at 0 0)
		(size 1 2.2)
		(layers "F.Cu" "F.Mask")
		(uuid "bb122bf9-4163-43de-aac2-517c0720d0de")
	)
	(pad "4" smd rect
		(at 2.5 0)
		(size 1 2.2)
		(layers "F.Cu" "F.Mask")
		(uuid "94268d36-f310-421d-aa98-d0710f469885")
	)
	(pad "5" smd rect
		(at 5 0)
		(size 1 2.2)
		(layers "F.Cu" "F.Mask")
		(uuid "432c1108-9fe0-4a4b-971c-e21dae8c12ab")
	)
)