FILE_TYPE = MULTI_PHYS_TABLE;

PART 'REF35160QDBVR'
CLASS = IC
{========================================================================================}
:"MANUFACTURER_NAME", "MANUFACTURER_PART_NUMBER"= "PART_NUMBER", "JEDEC_TYPE", "PACK_TYPE", "MOUSER_PART_NUMBER", "MOUSER_PRICE/STOCK", "DESCRIPTION", "DATASHEET", "HEIGHT";
{========================================================================================}
 "Texas Instruments", "REF35160QDBVR" (!) = "", "SOT95P280X145-6N", "SOT23 (6-Pin)", "595-REF35160QDBVR", "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/REF35160QDBVR?qs=rQFj71Wb1eVJh8regkgQhg%3D%3D", "Voltage References 650-nA quiescent current, 12-ppm/C drift, ultra-low-power precision voltage reference", "https://www.ti.com/lit/ds/symlink/ref35.pdf?ts=1675771464754&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FREF35%252Fpart-details%252FREF35125QDBVR%253FkeyMatch%253DREF35125QDBVR%2526tisearch%253Dsearch-everything%2526usecase%253DOPN", "1.45 mm"
END_PART

END.
