(footprint "LED_WE-5630_HandSoldering" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.35 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d8b91dd3-abf8-406f-b87c-f28432cc023c)
  )
  (fp_text value "LED_WE-5630_HandSoldering" (at 0 2.65 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 23c6e6f2-f214-43e3-9d3f-7fcfbb7f54c3)
  )
  (fp_text user "${REFERENCE}" (at 0 4.15 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6d6c82f0-3b61-4d44-9983-5fe373fb2a6e)
  )
  (fp_line (start -4.3 -1.3) (end -4.3 1.1)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 0280dc32-0269-483c-8dee-a8f7e615b3bb))
  (fp_line (start -4.3 1.1) (end -4.1 1.3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp fc4d853f-b0ca-421c-888d-bfd72f3e89d0))
  (fp_line (start -4.1 1.3) (end -1.4 1.3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 8d2c3835-6336-49fb-b7e2-03f22806ac68))
  (fp_line (start -1.4 -1.3) (end -4.3 -1.3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp d4e87bc6-c2b3-41f5-83dc-12da6763479d))
  (fp_rect (start -4.3 -1.3) (end 4.3 1.3)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 5d160da0-ac39-43ff-8695-98803fa25b37))
  (pad "1" smd rect (at -2.7 -0.65) (size 2.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 76ae0151-8555-490a-b362-f8c5f9bfb035))
  (pad "1" smd rect (at -2.7 0.65) (size 2.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp c70cad60-cf9b-43e4-b089-d3826f13674e))
  (pad "2" smd custom (at 0.15 0) (size 2.1 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_rect (start 1.05 0.2) (end 3.95 1.1) (width 0.01) (fill yes))
      (gr_rect (start 1.05 -1.1) (end 3.95 -0.2) (width 0.01) (fill yes))
    ) (tstamp a50b8502-9744-4016-87b7-ec59feb41081))
  (model "${KIPRJMOD}/FT_Libraries/FaSTTUBe_LEDs.pretty/3d_models/STP_WL-SWTP_5630A (rev1).stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
