(footprint "Crystal_SMD_ECS_CSM-7X" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 63AD0BC2)
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.25 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 99e78964-1449-4321-ad33-c70620f1a12d)
  )
  (fp_text value "Crystal_SMD_ECS_CSM-7X" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 871784c6-10d1-4698-80e4-c571e86d0b8f)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8388ed1d-6564-4156-b47e-40ff74523401)
  )
  (fp_rect (start -7.75 -2.5) (end 7.75 2.5) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp f54301a6-e34e-4c8a-a6fe-2b7d44893692))
  (pad "1" smd rect (at -4.75 0) (size 5.5 2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 7821cb42-6184-478c-ad6a-d32093b0b8ee))
  (pad "2" smd rect (at 4.75 0) (size 5.5 2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 765f4fd0-f068-4d04-a953-8890777f159f))
)
