(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "PH600A280-24"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 20.32 -1.778 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "PH600A280-24"
			(at 17.272 3.302 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" "PH300A_thru_PH600A_TDK"
			(at -6.858 6.096 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "PH600A280-24"
			(at -2.032 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "ki_keywords" "PH600A280-24"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "PH300A_thru_PH600A_TDK"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "PH600A280-24_0_1"
			(polyline
				(pts
					(xy 7.62 -15.24) (xy 33.02 -15.24)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 5.08) (xy 7.62 -15.24)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 33.02 -15.24) (xy 33.02 5.08)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 33.02 5.08) (xy 7.62 5.08)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "PH600A280-24_1_1"
			(pin passive line
				(at 20.32 -17.78 90)
				(length 2.54)
				(name "BasePlate"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 -12.7 0)
				(length 7.62)
				(name "CNT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 40.64 -13.97 180)
				(length 7.62)
				(name "-Vout"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -7.62 0)
				(length 7.62)
				(name "-VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -2.54 0)
				(length 7.62)
				(name "+VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 40.64 3.81 180)
				(length 7.62)
				(name "+Vout"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 40.64 1.27 180)
				(length 7.62)
				(name "+Vout"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 40.64 -2.54 180)
				(length 7.62)
				(name "+S"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 40.64 -5.08 180)
				(length 7.62)
				(name "TRM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 40.64 -7.62 180)
				(length 7.62)
				(name "-S"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 40.64 -11.43 180)
				(length 7.62)
				(name "-Vout"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
)
