(footprint "SWD_Clamp_4p" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at -7 0 90 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 62882383-8ec7-42e8-aad5-f322f2cd0d4d)
  )
  (fp_text value "SWD_Clamp_4p" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9d6cd97a-d008-4865-bef5-ffc5fdfb1619)
  )
  (fp_text user "SWD" (at 0 -2 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify bottom))
    (tstamp 67358610-9f23-496c-8c3d-e7f741120abc)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a0ab3b37-62cb-44eb-9bba-e6d4df1c89ff)
  )
  (fp_line (start -4.31 -3) (end -3.31 -3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp a081c966-4d98-4c69-a61d-188eaefedee2))
  (fp_line (start -3.81 -2) (end -4.31 -3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 37a35db4-393d-4da3-9555-a88ad496793d))
  (fp_line (start -3.31 -3) (end -3.81 -2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 5d92d681-adc0-4a1b-a754-25f6dc606414))
  (fp_rect (start -5.5 -1.5) (end 5.5 1.5)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 5e5a2d49-f47e-4302-9762-eeb4cf3f26c6))
  (pad "1" smd circle (at -3.81 0) (size 2 2) (layers "F.Cu" "F.Mask") (tstamp 9da04288-8c27-40a6-8fc4-065d8c81aa72))
  (pad "2" smd circle (at -1.27 0) (size 2 2) (layers "F.Cu" "F.Mask") (tstamp 978dc140-d7a3-417b-8e18-c9822ac5c7e1))
  (pad "3" smd circle (at 1.27 0) (size 2 2) (layers "F.Cu" "F.Mask") (tstamp 41330d6b-9554-45e4-a6e8-a23a86bcb171))
  (pad "4" smd circle (at 3.81 0) (size 2 2) (layers "F.Cu" "F.Mask") (tstamp d5d228aa-d9c8-4c92-aecb-b0fb533a9f8a))
)
