(footprint "TO-39_sidemount"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "U2"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f3e4eb35-7f64-4002-a6f4-67e3651690ee")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Heimann_32x32"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b0bb462a-ed7d-47d1-be42-b2e01861e764")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "TTS:TO-39_sidemount"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "c68153f4-4730-4612-8fcc-bb90f6b0bfd9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://cloud.fasttube.de/f/3478875"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2130d60a-a4ae-41a6-8986-43af399db7a6")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "49fe5c30-acc3-4724-aa42-22d0163dc722")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5da0f151-e4ba-4cd6-885b-c86cae39d644")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2 -4)
		(end 2 -4)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "feca1e6d-90a6-4e26-87f1-9fd935446e31")
	)
	(fp_rect
		(start -3 -4)
		(end 3 4)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "3d245e62-f492-406d-936b-119b8cd3d4f2")
	)
	(fp_line
		(start 3 -4)
		(end 3 4)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.Fab")
		(uuid "be20de29-a9fc-46e2-9007-198630fedf39")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "3360a157-680d-448d-8bca-82da88ea1b53")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd oval
		(at 0 -2.7)
		(size 4 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "8462b3f3-9c8d-4e6a-8380-70a8065f346f")
	)
	(pad "2" smd oval
		(at 0 2.7)
		(size 4 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "67cb80ab-4643-4b02-ae23-ac03b222a627")
	)
	(pad "3" smd oval
		(at 0 2.7)
		(size 4 1)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(uuid "571bb847-4446-4323-a450-55db84ec34b7")
	)
	(pad "4" smd oval
		(at 0 -2.7)
		(size 4 1)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(uuid "8f041321-d344-4c4b-90bc-39668deabd30")
	)
	(model "${KIPRJMOD}/CAD/TO-39_Heimann.stp"
		(offset
			(xyz 3.5 0 -0.85)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 180 90 0)
		)
	)
)
