(footprint "SOT-23"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SOT TO_SOT_SMD")
	(property "Reference" "D4"
		(at 0 -2.4 0)
		(layer "F.SilkS")
		(uuid "e8673960-1949-4a2a-8f9c-4ff243fb3013")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "BAT54FILM"
		(at 0 2.4 0)
		(layer "F.Fab")
		(uuid "0f93caf0-5c51-47f7-96eb-c6758b78a8db")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "135d6f7c-eb8c-4719-86a3-c0dc1e3477c4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.mouser.de/datasheet/2/389/bat54-1849047.pdf"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "f9bb9add-d490-44a2-bd54-f0a775c36607")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Schottky diode"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "ace244fb-7728-4b56-9f2c-6dd5467d46e3")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0 -1.56)
		(end -0.65 -1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "339c149e-0837-41dd-9ed6-bc861aed82de")
	)
	(fp_line
		(start 0 -1.56)
		(end 0.65 -1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2bf6c8f9-0b30-4b00-b6d5-1aa3f43c45cf")
	)
	(fp_line
		(start 0 1.56)
		(end -0.65 1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2da49af8-18e8-4705-9b54-347d2c53a2b9")
	)
	(fp_line
		(start 0 1.56)
		(end 0.65 1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e368b48d-a244-46aa-83d7-c19ca3d1bb34")
	)
	(fp_poly
		(pts
			(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.84) (xy -1.1625 -1.51)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "bf817525-4ccf-4002-9402-ac7392685639")
	)
	(fp_line
		(start -1.92 -1.7)
		(end -1.92 1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "67b4b023-b144-4f1a-ad1d-e4168db2d292")
	)
	(fp_line
		(start -1.92 1.7)
		(end 1.92 1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e4999367-0d73-47fa-8fa4-a583cabcd74e")
	)
	(fp_line
		(start 1.92 -1.7)
		(end -1.92 -1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "efcd6404-e4c8-4b80-a30a-ac29d44b52fe")
	)
	(fp_line
		(start 1.92 1.7)
		(end 1.92 -1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e618ccea-a173-4580-a146-082258de1411")
	)
	(fp_line
		(start -0.65 -1.125)
		(end -0.325 -1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "07a3d11f-dc9e-41b4-a0f2-4289c3a8a37d")
	)
	(fp_line
		(start -0.65 1.45)
		(end -0.65 -1.125)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4b929fda-bd08-4735-acf1-3445c812fd29")
	)
	(fp_line
		(start -0.325 -1.45)
		(end 0.65 -1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e032854b-e74c-402b-9cf1-aadf07c35b1a")
	)
	(fp_line
		(start 0.65 -1.45)
		(end 0.65 1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d7bd4ee0-717e-48e9-89dc-8d1b4ca0e477")
	)
	(fp_line
		(start 0.65 1.45)
		(end -0.65 1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "dddab8f4-4fd8-42a1-8df9-22fefb5943d6")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "1e255205-899b-4e16-9def-9e749cd808c8")
		(effects
			(font
				(size 0.32 0.32)
				(thickness 0.05)
			)
		)
	)
	(pad "" smd roundrect
		(at -0.9375 0.95)
		(size 1.475 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "56f251e7-f756-4f1a-997b-ffc95b8c5cfc")
	)
	(pad "1" smd roundrect
		(at 0.9375 0)
		(size 1.475 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "a4aad8a6-19b9-4bbd-b9fd-8f0c723c4a8d")
	)
	(pad "2" smd roundrect
		(at -0.9375 -0.95)
		(size 1.475 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "acce8743-07f3-46aa-b809-fb9c41b71cb5")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
