(footprint "APEM-ISx3SAD_Harwin_S9091-46R_NoSilk" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Sealed pushbutton switch")
  (tags "ISR3AD, ISP3AD")
  (property "Sheetfile" "buttons.kicad_sch")
  (property "Sheetname" "Buttons")
  (fp_text reference "AMC1" (at 9 0.333334 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f4411b4c-3b05-437e-8121-f36a1e7385cc)
  )
  (fp_text value "SW_Push" (at 0 -11.43 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f7678448-59ce-423d-9ac9-1ab76125b847)
  )
  (fp_rect (start -3.79 3.25) (end -1.29 -3.25)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 1223bf0d-c22e-477b-95a1-3545b2024011))
  (fp_rect (start 1.25 3.25) (end 3.75 -3.25)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 012bd6fb-e35a-4ae9-af40-8d0c184a49e9))
  (fp_circle (center 0 0) (end 8 0)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 092b614f-ec5f-4c70-b62a-9a73c6a6093e))
  (pad "" np_thru_hole circle (at -2.54 0 90) (size 3.8 3.8) (drill 3.8) (layers "*.Mask") (tstamp 28ceebe1-79ac-4a63-9660-90c38b7a98cf))
  (pad "" np_thru_hole circle (at 2.5 0 90) (size 3.8 3.8) (drill 3.8) (layers "*.Mask") (tstamp 2213bc2a-f51d-4f4f-be50-444ceaee2e6a))
  (pad "1" smd roundrect (at -2.55 -2.6 180) (size 2 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp aa00010d-b319-412c-a448-033152234416))
  (pad "1" smd roundrect (at -2.55 2.6 180) (size 2 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp 3c2ac476-fc84-49a5-aad0-86ad9021bc64))
  (pad "2" smd roundrect (at 2.5 -2.6 180) (size 2 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp e11bcd78-e910-4ea0-9d13-0d5d0df1d23f))
  (pad "2" smd roundrect (at 2.5 2.6 180) (size 2 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp 7347a874-9f42-488c-8800-5283857fa454))
  (model "${KIPRJMOD}/FT_Libraries/FaSTTUBe_Switches.pretty/3d_models/APEM-ISx3SAD.stp"
    (offset (xyz 0 0 12.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 180 0 0))
  )
  (model "${KIPRJMOD}/FT_Libraries/FaSTTUBe_Switches.pretty/3d_models/s9091-46r.stp"
    (offset (xyz 2.5 0 -2))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
  (model "${KIPRJMOD}/FT_Libraries/FaSTTUBe_Switches.pretty/3d_models/s9091-46r.stp"
    (offset (xyz -2.5 0 -2))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
