ARM GAS  /tmp/cc5SiBtg.s 			page 1


   1              		.cpu cortex-m4
   2              		.arch armv7e-m
   3              		.fpu fpv4-sp-d16
   4              		.eabi_attribute 27, 1
   5              		.eabi_attribute 28, 1
   6              		.eabi_attribute 20, 1
   7              		.eabi_attribute 21, 1
   8              		.eabi_attribute 23, 3
   9              		.eabi_attribute 24, 1
  10              		.eabi_attribute 25, 1
  11              		.eabi_attribute 26, 1
  12              		.eabi_attribute 30, 1
  13              		.eabi_attribute 34, 1
  14              		.eabi_attribute 18, 4
  15              		.file	"stm32f3xx_hal_spi.c"
  16              		.text
  17              	.Ltext0:
  18              		.cfi_sections	.debug_frame
  19              		.file 1 "Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c"
  20              		.section	.text.SPI_WaitFlagStateUntilTimeout,"ax",%progbits
  21              		.align	1
  22              		.syntax unified
  23              		.thumb
  24              		.thumb_func
  26              	SPI_WaitFlagStateUntilTimeout:
  27              	.LVL0:
  28              	.LFB170:
   1:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
   2:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ******************************************************************************
   3:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @file    stm32f3xx_hal_spi.c
   4:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @author  MCD Application Team
   5:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief   SPI HAL module driver.
   6:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *          This file provides firmware functions to manage the following
   7:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *          functionalities of the Serial Peripheral Interface (SPI) peripheral:
   8:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           + Initialization and de-initialization functions
   9:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           + IO operation functions
  10:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           + Peripheral Control functions
  11:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           + Peripheral State functions
  12:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ******************************************************************************
  13:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @attention
  14:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
  15:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * Copyright (c) 2016 STMicroelectronics.
  16:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * All rights reserved.
  17:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
  18:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * This software is licensed under terms that can be found in the LICENSE file
  19:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * in the root directory of this software component.
  20:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * If no LICENSE file comes with this software, it is provided AS-IS.
  21:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
  22:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ******************************************************************************
  23:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   @verbatim
  24:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ==============================================================================
  25:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                         ##### How to use this driver #####
  26:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ==============================================================================
  27:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     [..]
  28:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       The SPI HAL driver can be used as follows:
  29:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  30:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) Declare a SPI_HandleTypeDef handle structure, for example:
ARM GAS  /tmp/cc5SiBtg.s 			page 2


  31:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SPI_HandleTypeDef  hspi;
  32:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  33:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#)Initialize the SPI low level resources by implementing the HAL_SPI_MspInit() API:
  34:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) Enable the SPIx interface clock
  35:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) SPI pins configuration
  36:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Enable the clock for the SPI GPIOs
  37:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Configure these SPI pins as alternate function push-pull
  38:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) NVIC configuration if you need to use interrupt process
  39:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Configure the SPIx interrupt priority
  40:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Enable the NVIC SPI IRQ handle
  41:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) DMA Configuration if you need to use DMA process
  42:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Declare a DMA_HandleTypeDef handle structure for the transmit or receive Stream
  43:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Enable the DMAx clock
  44:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Configure the DMA handle parameters
  45:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Configure the DMA Tx or Rx Stream/Channel
  46:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Associate the initialized hdma_tx(or _rx)  handle to the hspi DMA Tx or Rx hand
  47:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Configure the priority and enable the NVIC for the transfer complete interrupt 
  48:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  49:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) Program the Mode, BidirectionalMode , Data size, Baudrate Prescaler, NSS
  50:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           management, Clock polarity and phase, FirstBit and CRC configuration in the hspi Init str
  51:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  52:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) Initialize the SPI registers by calling the HAL_SPI_Init() API:
  53:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (++) This API configures also the low level Hardware GPIO, CLOCK, CORTEX...etc)
  54:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               by calling the customized HAL_SPI_MspInit() API.
  55:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      [..]
  56:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Circular mode restriction:
  57:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) The DMA circular mode cannot be used when the SPI is configured in these modes:
  58:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) Master 2Lines RxOnly
  59:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) Master 1Line Rx
  60:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) The CRC feature is not managed when the DMA circular mode is enabled
  61:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) When the SPI DMA Pause/Stop features are used, we must use the following APIs
  62:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           the HAL_SPI_DMAPause()/ HAL_SPI_DMAStop() only under the SPI callbacks
  63:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      [..]
  64:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Master Receive mode restriction:
  65:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) In Master unidirectional receive-only mode (MSTR =1, BIDIMODE=0, RXONLY=1) or
  66:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           bidirectional receive mode (MSTR=1, BIDIMODE=1, BIDIOE=0), to ensure that the SPI
  67:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           does not initiate a new transfer the following procedure has to be respected:
  68:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) HAL_SPI_DeInit()
  69:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) HAL_SPI_Init()
  70:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      [..]
  71:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Callback registration:
  72:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  73:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) The compilation flag USE_HAL_SPI_REGISTER_CALLBACKS when set to 1U
  74:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           allows the user to configure dynamically the driver callbacks.
  75:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           Use Functions HAL_SPI_RegisterCallback() to register an interrupt callback.
  76:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  77:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           Function HAL_SPI_RegisterCallback() allows to register following callbacks:
  78:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxCpltCallback        : SPI Tx Completed callback
  79:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) RxCpltCallback        : SPI Rx Completed callback
  80:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxRxCpltCallback      : SPI TxRx Completed callback
  81:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxHalfCpltCallback    : SPI Tx Half Completed callback
  82:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) RxHalfCpltCallback    : SPI Rx Half Completed callback
  83:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxRxHalfCpltCallback  : SPI TxRx Half Completed callback
  84:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) ErrorCallback         : SPI Error callback
  85:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) AbortCpltCallback     : SPI Abort callback
  86:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) MspInitCallback       : SPI Msp Init callback
  87:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) MspDeInitCallback     : SPI Msp DeInit callback
ARM GAS  /tmp/cc5SiBtg.s 			page 3


  88:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           This function takes as parameters the HAL peripheral handle, the Callback ID
  89:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           and a pointer to the user callback function.
  90:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  91:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  92:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) Use function HAL_SPI_UnRegisterCallback to reset a callback to the default
  93:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           weak function.
  94:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           HAL_SPI_UnRegisterCallback takes as parameters the HAL peripheral handle,
  95:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           and the Callback ID.
  96:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           This function allows to reset following callbacks:
  97:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxCpltCallback        : SPI Tx Completed callback
  98:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) RxCpltCallback        : SPI Rx Completed callback
  99:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxRxCpltCallback      : SPI TxRx Completed callback
 100:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxHalfCpltCallback    : SPI Tx Half Completed callback
 101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) RxHalfCpltCallback    : SPI Rx Half Completed callback
 102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxRxHalfCpltCallback  : SPI TxRx Half Completed callback
 103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) ErrorCallback         : SPI Error callback
 104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) AbortCpltCallback     : SPI Abort callback
 105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) MspInitCallback       : SPI Msp Init callback
 106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) MspDeInitCallback     : SPI Msp DeInit callback
 107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        [..]
 109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        By default, after the HAL_SPI_Init() and when the state is HAL_SPI_STATE_RESET
 110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        all callbacks are set to the corresponding weak functions:
 111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        examples HAL_SPI_MasterTxCpltCallback(), HAL_SPI_MasterRxCpltCallback().
 112:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Exception done for MspInit and MspDeInit functions that are
 113:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        reset to the legacy weak functions in the HAL_SPI_Init()/ HAL_SPI_DeInit() only when
 114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        these callbacks are null (not registered beforehand).
 115:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        If MspInit or MspDeInit are not null, the HAL_SPI_Init()/ HAL_SPI_DeInit()
 116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        keep and use the user MspInit/MspDeInit callbacks (registered beforehand) whatever the state
 117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        [..]
 119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Callbacks can be registered/unregistered in HAL_SPI_STATE_READY state only.
 120:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Exception done MspInit/MspDeInit functions that can be registered/unregistered
 121:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        in HAL_SPI_STATE_READY or HAL_SPI_STATE_RESET state,
 122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        thus registered (user) MspInit/DeInit callbacks can be used during the Init/DeInit.
 123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Then, the user first registers the MspInit/MspDeInit user callbacks
 124:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        using HAL_SPI_RegisterCallback() before calling HAL_SPI_DeInit()
 125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        or HAL_SPI_Init() function.
 126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        [..]
 128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        When the compilation define USE_HAL_PPP_REGISTER_CALLBACKS is set to 0 or
 129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        not defined, the callback registering feature is not available
 130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        and weak (surcharged) callbacks are used.
 131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      [..]
 133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Using the HAL it is not possible to reach all supported SPI frequency with the different SPI
 134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        the following table resume the max SPI frequency reached with data size 8bits/16bits,
 135:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****          according to frequency of the APBx Peripheral Clock (fPCLK) used by the SPI instance.
 136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 137:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   @endverbatim
 138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   Additional table :
 140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        DataSize = SPI_DATASIZE_8BIT:
 142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        +-------------------------------------------------------------------------------------------
 143:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |                | 2Lines Fullduplex   |     2Lines RxOnly    |         1Line     
 144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        | Process | Transfer mode  |---------------------|----------------------|-------------------
ARM GAS  /tmp/cc5SiBtg.s 			page 4


 145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |                |  Master  |  Slave   |  Master   |  Slave   |  Master   |  Slave
 146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |===========================================================================================
 147:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    T    |     Polling    | Fpclk/4  | Fpclk/8  |    NA     |    NA    |    NA     |   NA  
 148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |----------------|----------|----------|-----------|----------|-----------|-------
 149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    /    |     Interrupt  | Fpclk/4  | Fpclk/16 |    NA     |    NA    |    NA     |   NA  
 150:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    R    |----------------|----------|----------|-----------|----------|-----------|-------
 151:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |       DMA      | Fpclk/2  | Fpclk/2  |    NA     |    NA    |    NA     |   NA  
 152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |=========|================|==========|==========|===========|==========|===========|=======
 153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |     Polling    | Fpclk/4  | Fpclk/8  | Fpclk/16  | Fpclk/8  | Fpclk/8   | Fpclk/
 154:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |----------------|----------|----------|-----------|----------|-----------|-------
 155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    R    |     Interrupt  | Fpclk/8  | Fpclk/16 | Fpclk/8   | Fpclk/8  | Fpclk/8   | Fpclk/
 156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |----------------|----------|----------|-----------|----------|-----------|-------
 157:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |       DMA      | Fpclk/4  | Fpclk/2  | Fpclk/2   | Fpclk/16 | Fpclk/2   | Fpclk/
 158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |=========|================|==========|==========|===========|==========|===========|=======
 159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |     Polling    | Fpclk/8  | Fpclk/2  |     NA    |    NA    | Fpclk/8   | Fpclk/
 160:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |----------------|----------|----------|-----------|----------|-----------|-------
 161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    T    |     Interrupt  | Fpclk/2  | Fpclk/4  |     NA    |    NA    | Fpclk/16  | Fpclk/
 162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |----------------|----------|----------|-----------|----------|-----------|-------
 163:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |       DMA      | Fpclk/2  | Fpclk/2  |     NA    |    NA    | Fpclk/8   | Fpclk/
 164:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        +-------------------------------------------------------------------------------------------
 165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 166:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        DataSize = SPI_DATASIZE_16BIT:
 167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        +-------------------------------------------------------------------------------------------
 168:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |                | 2Lines Fullduplex   |     2Lines RxOnly    |         1Line     
 169:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        | Process | Transfer mode  |---------------------|----------------------|-------------------
 170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |                |  Master  |  Slave   |  Master   |  Slave   |  Master   |  Slave
 171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |===========================================================================================
 172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    T    |     Polling    | Fpclk/4  | Fpclk/8  |    NA     |    NA    |    NA     |   NA  
 173:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |----------------|----------|----------|-----------|----------|-----------|-------
 174:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    /    |     Interrupt  | Fpclk/4  | Fpclk/16 |    NA     |    NA    |    NA     |   NA  
 175:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    R    |----------------|----------|----------|-----------|----------|-----------|-------
 176:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |       DMA      | Fpclk/2  | Fpclk/2  |    NA     |    NA    |    NA     |   NA  
 177:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |=========|================|==========|==========|===========|==========|===========|=======
 178:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |     Polling    | Fpclk/4  | Fpclk/8  | Fpclk/16  | Fpclk/8  | Fpclk/8   | Fpclk/
 179:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |----------------|----------|----------|-----------|----------|-----------|-------
 180:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    R    |     Interrupt  | Fpclk/8  | Fpclk/16 | Fpclk/8   | Fpclk/8  | Fpclk/8   | Fpclk/
 181:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |----------------|----------|----------|-----------|----------|-----------|-------
 182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |       DMA      | Fpclk/4  | Fpclk/2  | Fpclk/2   | Fpclk/16 | Fpclk/2   | Fpclk/
 183:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |=========|================|==========|==========|===========|==========|===========|=======
 184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |     Polling    | Fpclk/8  | Fpclk/2  |     NA    |    NA    | Fpclk/8   | Fpclk/
 185:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |----------------|----------|----------|-----------|----------|-----------|-------
 186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    T    |     Interrupt  | Fpclk/2  | Fpclk/4  |     NA    |    NA    | Fpclk/16  | Fpclk/
 187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |----------------|----------|----------|-----------|----------|-----------|-------
 188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |       DMA      | Fpclk/2  | Fpclk/2  |     NA    |    NA    | Fpclk/8   | Fpclk/
 189:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        +-------------------------------------------------------------------------------------------
 190:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        @note The max SPI frequency depend on SPI data size (4bits, 5bits,..., 8bits,...15bits, 16bi
 191:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****              SPI mode(2 Lines fullduplex, 2 lines RxOnly, 1 line TX/RX) and Process mode (Polling, 
 192:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        @note
 193:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (#) TX/RX processes are HAL_SPI_TransmitReceive(), HAL_SPI_TransmitReceive_IT() and HAL
 194:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (#) RX processes are HAL_SPI_Receive(), HAL_SPI_Receive_IT() and HAL_SPI_Receive_DMA()
 195:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (#) TX processes are HAL_SPI_Transmit(), HAL_SPI_Transmit_IT() and HAL_SPI_Transmit_DMA
 196:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Includes ------------------------------------------------------------------*/
 200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #include "stm32f3xx_hal.h"
 201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 5


 202:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @addtogroup STM32F3xx_HAL_Driver
 203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 204:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI SPI
 207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief SPI HAL module driver
 208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #ifdef HAL_SPI_MODULE_ENABLED
 211:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Private typedef -----------------------------------------------------------*/
 213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Private defines -----------------------------------------------------------*/
 214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI_Private_Constants SPI Private Constants
 215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 216:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 217:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #define SPI_DEFAULT_TIMEOUT 100U
 218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @}
 220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Private macros ------------------------------------------------------------*/
 223:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Private variables ---------------------------------------------------------*/
 224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Private function prototypes -----------------------------------------------*/
 225:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI_Private_Functions SPI Private Functions
 226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 228:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMATransmitCplt(DMA_HandleTypeDef *hdma);
 229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAReceiveCplt(DMA_HandleTypeDef *hdma);
 230:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMATransmitReceiveCplt(DMA_HandleTypeDef *hdma);
 231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAHalfTransmitCplt(DMA_HandleTypeDef *hdma);
 232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAHalfReceiveCplt(DMA_HandleTypeDef *hdma);
 233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAHalfTransmitReceiveCplt(DMA_HandleTypeDef *hdma);
 234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAError(DMA_HandleTypeDef *hdma);
 235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAAbortOnError(DMA_HandleTypeDef *hdma);
 236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMATxAbortCallback(DMA_HandleTypeDef *hdma);
 237:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMARxAbortCallback(DMA_HandleTypeDef *hdma);
 238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_WaitFlagStateUntilTimeout(SPI_HandleTypeDef *hspi, uint32_t Flag, Flag
 239:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                        uint32_t Timeout, uint32_t Tickstart);
 240:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_WaitFifoStateUntilTimeout(SPI_HandleTypeDef *hspi, uint32_t Fifo, uint
 241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                        uint32_t Timeout, uint32_t Tickstart);
 242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_TxISR_8BIT(struct __SPI_HandleTypeDef *hspi);
 243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_TxISR_16BIT(struct __SPI_HandleTypeDef *hspi);
 244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_8BIT(struct __SPI_HandleTypeDef *hspi);
 245:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_16BIT(struct __SPI_HandleTypeDef *hspi);
 246:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_8BIT(struct __SPI_HandleTypeDef *hspi);
 247:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesTxISR_8BIT(struct __SPI_HandleTypeDef *hspi);
 248:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesTxISR_16BIT(struct __SPI_HandleTypeDef *hspi);
 249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_16BIT(struct __SPI_HandleTypeDef *hspi);
 250:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 251:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_8BITCRC(struct __SPI_HandleTypeDef *hspi);
 252:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_16BITCRC(struct __SPI_HandleTypeDef *hspi);
 253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_8BITCRC(struct __SPI_HandleTypeDef *hspi);
 254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_16BITCRC(struct __SPI_HandleTypeDef *hspi);
 255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_AbortRx_ISR(SPI_HandleTypeDef *hspi);
 257:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_AbortTx_ISR(SPI_HandleTypeDef *hspi);
 258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_CloseRxTx_ISR(SPI_HandleTypeDef *hspi);
ARM GAS  /tmp/cc5SiBtg.s 			page 6


 259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_CloseRx_ISR(SPI_HandleTypeDef *hspi);
 260:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_CloseTx_ISR(SPI_HandleTypeDef *hspi);
 261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_EndRxTransaction(SPI_HandleTypeDef *hspi, uint32_t Timeout, uint32_t T
 262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_EndRxTxTransaction(SPI_HandleTypeDef *hspi, uint32_t Timeout, uint32_t
 263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @}
 265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 267:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Exported functions --------------------------------------------------------*/
 268:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI_Exported_Functions SPI Exported Functions
 269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 270:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI_Exported_Functions_Group1 Initialization and de-initialization functions
 273:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *  @brief    Initialization and Configuration functions
 274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
 275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** @verbatim
 276:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****  ===============================================================================
 277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               ##### Initialization and de-initialization functions #####
 278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****  ===============================================================================
 279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     [..]  This subsection provides a set of functions allowing to initialize and
 280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           de-initialize the SPIx peripheral:
 281:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (+) User must implement HAL_SPI_MspInit() function in which he configures
 283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           all related peripherals resources (CLOCK, GPIO, DMA, IT and NVIC ).
 284:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 285:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (+) Call the function HAL_SPI_Init() to configure the selected device with
 286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           the selected configuration:
 287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) Mode
 288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) Direction
 289:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) Data Size
 290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) Clock Polarity and Phase
 291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) NSS Management
 292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) BaudRate Prescaler
 293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) FirstBit
 294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) TIMode
 295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) CRC Calculation
 296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) CRC Polynomial if CRC enabled
 297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) CRC Length, used only with Data8 and Data16
 298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) FIFO reception threshold
 299:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 300:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (+) Call the function HAL_SPI_DeInit() to restore the default configuration
 301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           of the selected SPIx peripheral.
 302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 303:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** @endverbatim
 304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Initialize the SPI according to the specified parameters
 309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         in the SPI_InitTypeDef and initialize the associated handle.
 310:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
 311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
 312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
 313:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Init(SPI_HandleTypeDef *hspi)
 315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
ARM GAS  /tmp/cc5SiBtg.s 			page 7


 316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t frxth;
 317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the SPI handle allocation */
 319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi == NULL)
 320:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_ERROR;
 322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the parameters */
 325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_ALL_INSTANCE(hspi->Instance));
 326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_MODE(hspi->Init.Mode));
 327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION(hspi->Init.Direction));
 328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DATASIZE(hspi->Init.DataSize));
 329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_NSS(hspi->Init.NSS));
 330:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_NSSP(hspi->Init.NSSPMode));
 331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_BAUDRATE_PRESCALER(hspi->Init.BaudRatePrescaler));
 332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_FIRST_BIT(hspi->Init.FirstBit));
 333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_TIMODE(hspi->Init.TIMode));
 334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.TIMode == SPI_TIMODE_DISABLE)
 335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_CPOL(hspi->Init.CLKPolarity));
 337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_CPHA(hspi->Init.CLKPhase));
 338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.Mode == SPI_MODE_MASTER)
 340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       assert_param(IS_SPI_BAUDRATE_PRESCALER(hspi->Init.BaudRatePrescaler));
 342:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
 344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 345:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Baudrate prescaler not use in Motoraola Slave mode. force to default value */
 346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->Init.BaudRatePrescaler = SPI_BAUDRATEPRESCALER_2;
 347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
 350:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_BAUDRATE_PRESCALER(hspi->Init.BaudRatePrescaler));
 352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Force polarity and phase to TI protocaol requirements */
 354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Init.CLKPolarity = SPI_POLARITY_LOW;
 355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Init.CLKPhase    = SPI_PHASE_1EDGE;
 356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_CRC_CALCULATION(hspi->Init.CRCCalculation));
 359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_CRC_POLYNOMIAL(hspi->Init.CRCPolynomial));
 362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_CRC_LENGTH(hspi->Init.CRCLength));
 363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 364:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
 365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->Init.CRCCalculation = SPI_CRCCALCULATION_DISABLE;
 366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State == HAL_SPI_STATE_RESET)
 369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Allocate lock resource and initialize it */
 371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Lock = HAL_UNLOCKED;
 372:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 8


 373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
 374:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Init the SPI Callback settings */
 375:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxCpltCallback       = HAL_SPI_TxCpltCallback;       /* Legacy weak TxCpltCallback       
 376:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxCpltCallback       = HAL_SPI_RxCpltCallback;       /* Legacy weak RxCpltCallback       
 377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxRxCpltCallback     = HAL_SPI_TxRxCpltCallback;     /* Legacy weak TxRxCpltCallback     
 378:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxHalfCpltCallback   = HAL_SPI_TxHalfCpltCallback;   /* Legacy weak TxHalfCpltCallback   
 379:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxHalfCpltCallback   = HAL_SPI_RxHalfCpltCallback;   /* Legacy weak RxHalfCpltCallback   
 380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxRxHalfCpltCallback = HAL_SPI_TxRxHalfCpltCallback; /* Legacy weak TxRxHalfCpltCallback 
 381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCallback        = HAL_SPI_ErrorCallback;        /* Legacy weak ErrorCallback        
 382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->AbortCpltCallback    = HAL_SPI_AbortCpltCallback;    /* Legacy weak AbortCpltCallback    
 383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->MspInitCallback == NULL)
 385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->MspInitCallback = HAL_SPI_MspInit; /* Legacy weak MspInit  */
 387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Init the low level hardware : GPIO, CLOCK, NVIC... */
 390:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->MspInitCallback(hspi);
 391:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
 392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Init the low level hardware : GPIO, CLOCK, NVIC... */
 393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     HAL_SPI_MspInit(hspi);
 394:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 395:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_BUSY;
 398:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the selected SPI peripheral */
 400:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
 401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 402:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Align by default the rs fifo threshold on the data size */
 403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
 404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     frxth = SPI_RXFIFO_THRESHOLD_HF;
 406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
 408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     frxth = SPI_RXFIFO_THRESHOLD_QF;
 410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 412:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* CRC calculation is valid only for 16Bit and 8 Bit */
 413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.DataSize != SPI_DATASIZE_16BIT) && (hspi->Init.DataSize != SPI_DATASIZE_8BIT))
 414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* CRC must be disabled */
 416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Init.CRCCalculation = SPI_CRCCALCULATION_DISABLE;
 417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*----------------------- SPIx CR1 & CR2 Configuration ---------------------*/
 420:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure : SPI Mode, Communication Mode, Clock polarity and phase, NSS management,
 421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   Communication speed, First bit and CRC calculation state */
 422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   WRITE_REG(hspi->Instance->CR1, ((hspi->Init.Mode & (SPI_CR1_MSTR | SPI_CR1_SSI)) |
 423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.Direction & (SPI_CR1_RXONLY | SPI_CR1_BIDIMODE)) |
 424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.CLKPolarity & SPI_CR1_CPOL) |
 425:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.CLKPhase & SPI_CR1_CPHA) |
 426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.NSS & SPI_CR1_SSM) |
 427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.BaudRatePrescaler & SPI_CR1_BR_Msk) |
 428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.FirstBit  & SPI_CR1_LSBFIRST) |
 429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.CRCCalculation & SPI_CR1_CRCEN)));
ARM GAS  /tmp/cc5SiBtg.s 			page 9


 430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*---------------------------- SPIx CRCL Configuration -------------------*/
 432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Align the CRC Length on the data size */
 435:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCLength == SPI_CRC_LENGTH_DATASIZE)
 436:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* CRC Length aligned on the data size : value set by default */
 438:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
 439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->Init.CRCLength = SPI_CRC_LENGTH_16BIT;
 441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 442:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
 443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->Init.CRCLength = SPI_CRC_LENGTH_8BIT;
 445:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 447:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 448:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Configure : CRC Length */
 449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCLength == SPI_CRC_LENGTH_16BIT)
 450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCL);
 452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 456:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure : NSS management, TI Mode, NSS Pulse, Data size and Rx Fifo threshold */
 457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   WRITE_REG(hspi->Instance->CR2, (((hspi->Init.NSS >> 16U) & SPI_CR2_SSOE) |
 458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.TIMode & SPI_CR2_FRF) |
 459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.NSSPMode & SPI_CR2_NSSP) |
 460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.DataSize & SPI_CR2_DS_Msk) |
 461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (frxth & SPI_CR2_FRXTH)));
 462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*---------------------------- SPIx CRCPOLY Configuration ------------------*/
 465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure : CRC Polynomial */
 466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 467:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     WRITE_REG(hspi->Instance->CRCPR, (hspi->Init.CRCPolynomial & SPI_CRCPR_CRCPOLY_Msk));
 469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 470:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 472:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if defined(SPI_I2SCFGR_I2SMOD)
 473:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Activate the SPI mode (Make sure that I2SMOD bit in I2SCFGR register is reset) */
 474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->I2SCFGR, SPI_I2SCFGR_I2SMOD);
 475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* SPI_I2SCFGR_I2SMOD */
 476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode = HAL_SPI_ERROR_NONE;
 478:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State     = HAL_SPI_STATE_READY;
 479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 480:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
 481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 482:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 483:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 484:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  De-Initialize the SPI peripheral.
 485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
 486:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
ARM GAS  /tmp/cc5SiBtg.s 			page 10


 487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
 488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 489:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_DeInit(SPI_HandleTypeDef *hspi)
 490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the SPI handle allocation */
 492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi == NULL)
 493:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_ERROR;
 495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 497:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check SPI Instance parameter */
 498:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_ALL_INSTANCE(hspi->Instance));
 499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_BUSY;
 501:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI Peripheral Clock */
 503:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
 504:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
 506:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->MspDeInitCallback == NULL)
 507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->MspDeInitCallback = HAL_SPI_MspDeInit; /* Legacy weak MspDeInit  */
 509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 511:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DeInit the low level hardware: GPIO, CLOCK, NVIC... */
 512:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->MspDeInitCallback(hspi);
 513:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
 514:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DeInit the low level hardware: GPIO, CLOCK, NVIC... */
 515:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_MspDeInit(hspi);
 516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode = HAL_SPI_ERROR_NONE;
 519:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_RESET;
 520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Release Lock */
 522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
 523:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
 525:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 526:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 528:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Initialize the SPI MSP.
 529:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
 530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
 531:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
 532:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 533:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_MspInit(SPI_HandleTypeDef *hspi)
 534:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 535:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
 537:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
 539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_MspInit should be implemented in the user file
 540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
 541:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 543:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
ARM GAS  /tmp/cc5SiBtg.s 			page 11


 544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  De-Initialize the SPI MSP.
 545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
 546:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
 547:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
 548:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 549:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_MspDeInit(SPI_HandleTypeDef *hspi)
 550:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 551:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
 553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
 555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_MspDeInit should be implemented in the user file
 556:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
 557:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
 560:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 561:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Register a User SPI Callback
 562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         To be used instead of the weak predefined callback
 563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi Pointer to a SPI_HandleTypeDef structure that contains
 564:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *                the configuration information for the specified SPI.
 565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  CallbackID ID of the callback to be registered
 566:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pCallback pointer to the Callback function
 567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
 568:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 569:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_RegisterCallback(SPI_HandleTypeDef *hspi, HAL_SPI_CallbackIDTypeDef Callb
 570:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                            pSPI_CallbackTypeDef pCallback)
 571:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 572:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef status = HAL_OK;
 573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (pCallback == NULL)
 575:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 576:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update the error code */
 577:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode |= HAL_SPI_ERROR_INVALID_CALLBACK;
 578:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 579:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_ERROR;
 580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 581:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process locked */
 582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
 583:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_SPI_STATE_READY == hspi->State)
 585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 586:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     switch (CallbackID)
 587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_COMPLETE_CB_ID :
 589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxCpltCallback = pCallback;
 590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 591:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 592:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_RX_COMPLETE_CB_ID :
 593:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxCpltCallback = pCallback;
 594:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 595:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 596:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_RX_COMPLETE_CB_ID :
 597:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxRxCpltCallback = pCallback;
 598:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_HALF_COMPLETE_CB_ID :
ARM GAS  /tmp/cc5SiBtg.s 			page 12


 601:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxHalfCpltCallback = pCallback;
 602:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 604:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_RX_HALF_COMPLETE_CB_ID :
 605:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxHalfCpltCallback = pCallback;
 606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 607:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_RX_HALF_COMPLETE_CB_ID :
 609:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxRxHalfCpltCallback = pCallback;
 610:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 611:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_ERROR_CB_ID :
 613:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCallback = pCallback;
 614:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 615:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_ABORT_CB_ID :
 617:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->AbortCpltCallback = pCallback;
 618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 619:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 620:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPINIT_CB_ID :
 621:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspInitCallback = pCallback;
 622:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 624:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPDEINIT_CB_ID :
 625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspDeInitCallback = pCallback;
 626:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       default :
 629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Update the error code */
 630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 631:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 632:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Return error status */
 633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         status =  HAL_ERROR;
 634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else if (HAL_SPI_STATE_RESET == hspi->State)
 638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 639:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     switch (CallbackID)
 640:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 641:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPINIT_CB_ID :
 642:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspInitCallback = pCallback;
 643:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 644:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPDEINIT_CB_ID :
 646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspDeInitCallback = pCallback;
 647:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 649:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       default :
 650:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Update the error code */
 651:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 652:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 653:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Return error status */
 654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         status =  HAL_ERROR;
 655:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 657:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
ARM GAS  /tmp/cc5SiBtg.s 			page 13


 658:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
 659:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 660:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update the error code */
 661:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 662:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Return error status */
 664:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     status =  HAL_ERROR;
 665:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 666:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 667:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Release Lock */
 668:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
 669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return status;
 670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Unregister an SPI Callback
 674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         SPI callback is redirected to the weak predefined callback
 675:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi Pointer to a SPI_HandleTypeDef structure that contains
 676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *                the configuration information for the specified SPI.
 677:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  CallbackID ID of the callback to be unregistered
 678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
 679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 680:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_UnRegisterCallback(SPI_HandleTypeDef *hspi, HAL_SPI_CallbackIDTypeDef Cal
 681:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef status = HAL_OK;
 683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 684:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process locked */
 685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
 686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 687:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_SPI_STATE_READY == hspi->State)
 688:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     switch (CallbackID)
 690:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_COMPLETE_CB_ID :
 692:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxCpltCallback = HAL_SPI_TxCpltCallback;             /* Legacy weak TxCpltCallback   
 693:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 694:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 695:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_RX_COMPLETE_CB_ID :
 696:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxCpltCallback = HAL_SPI_RxCpltCallback;             /* Legacy weak RxCpltCallback   
 697:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 698:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_RX_COMPLETE_CB_ID :
 700:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxRxCpltCallback = HAL_SPI_TxRxCpltCallback;         /* Legacy weak TxRxCpltCallback 
 701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 702:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_HALF_COMPLETE_CB_ID :
 704:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxHalfCpltCallback = HAL_SPI_TxHalfCpltCallback;     /* Legacy weak TxHalfCpltCallbac
 705:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 706:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 707:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_RX_HALF_COMPLETE_CB_ID :
 708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxHalfCpltCallback = HAL_SPI_RxHalfCpltCallback;     /* Legacy weak RxHalfCpltCallbac
 709:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 710:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 711:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_RX_HALF_COMPLETE_CB_ID :
 712:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxRxHalfCpltCallback = HAL_SPI_TxRxHalfCpltCallback; /* Legacy weak TxRxHalfCpltCallb
 713:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 14


 715:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_ERROR_CB_ID :
 716:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCallback = HAL_SPI_ErrorCallback;               /* Legacy weak ErrorCallback    
 717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_ABORT_CB_ID :
 720:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->AbortCpltCallback = HAL_SPI_AbortCpltCallback;       /* Legacy weak AbortCpltCallback
 721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 722:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 723:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPINIT_CB_ID :
 724:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspInitCallback = HAL_SPI_MspInit;                   /* Legacy weak MspInit          
 725:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 727:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPDEINIT_CB_ID :
 728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspDeInitCallback = HAL_SPI_MspDeInit;               /* Legacy weak MspDeInit        
 729:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 731:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       default :
 732:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Update the error code */
 733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 735:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Return error status */
 736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         status =  HAL_ERROR;
 737:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 738:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 739:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 740:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else if (HAL_SPI_STATE_RESET == hspi->State)
 741:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 742:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     switch (CallbackID)
 743:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 744:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPINIT_CB_ID :
 745:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspInitCallback = HAL_SPI_MspInit;                   /* Legacy weak MspInit          
 746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 748:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPDEINIT_CB_ID :
 749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspDeInitCallback = HAL_SPI_MspDeInit;               /* Legacy weak MspDeInit        
 750:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 751:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 752:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       default :
 753:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Update the error code */
 754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 755:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 756:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Return error status */
 757:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         status =  HAL_ERROR;
 758:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 760:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 761:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
 762:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 763:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update the error code */
 764:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Return error status */
 767:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     status =  HAL_ERROR;
 768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 769:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Release Lock */
 771:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
ARM GAS  /tmp/cc5SiBtg.s 			page 15


 772:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return status;
 773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 776:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @}
 777:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 778:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 779:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI_Exported_Functions_Group2 IO operation functions
 780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *  @brief   Data transfers functions
 781:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
 782:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** @verbatim
 783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ==============================================================================
 784:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                       ##### IO operation functions #####
 785:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****  ===============================================================================
 786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****  [..]
 787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     This subsection provides a set of functions allowing to manage the SPI
 788:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     data transfers.
 789:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     [..] The SPI supports master and slave mode :
 791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     (#) There are two modes of transfer:
 793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        (++) Blocking mode: The communication is performed in polling mode.
 794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             The HAL status of all data processing is returned by the same function
 795:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             after finishing transfer.
 796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        (++) No-Blocking mode: The communication is performed using Interrupts
 797:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             or DMA, These APIs return the HAL status.
 798:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             The end of the data processing will be indicated through the
 799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             dedicated SPI IRQ when using Interrupt mode or the DMA IRQ when
 800:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             using DMA mode.
 801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             The HAL_SPI_TxCpltCallback(), HAL_SPI_RxCpltCallback() and HAL_SPI_TxRxCpltCallback() u
 802:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             will be executed respectively at the end of the transmit or Receive process
 803:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             The HAL_SPI_ErrorCallback()user callback will be executed when a communication error is
 804:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 805:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     (#) APIs provided for these 2 transfer modes (Blocking mode or Non blocking mode using either I
 806:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         exist for 1Line (simplex) and 2Lines (full duplex) modes.
 807:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 808:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** @endverbatim
 809:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 811:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 812:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Transmit an amount of data in blocking mode.
 814:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
 815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
 816:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pData pointer to data buffer
 817:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent
 818:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
 819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
 820:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 821:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Transmit(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size, uint32_t
 822:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 825:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t initial_TxXferCount;
 826:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check Direction parameter */
 828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES_OR_1LINE(hspi->Init.Direction));
ARM GAS  /tmp/cc5SiBtg.s 			page 16


 829:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 830:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
 831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
 832:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
 834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
 835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
 836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
 838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
 840:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 841:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 842:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0U))
 844:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
 846:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 847:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
 850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_TX;
 851:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 852:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 853:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 856:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*Init field not used in handle to zero */
 857:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)NULL;
 858:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 862:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 863:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure communication direction : 1Line */
 864:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
 865:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI Peripheral before set 1Line direction (BIDIOE bit) */
 867:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
 868:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 870:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 872:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
 873:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 874:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 875:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
 876:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 877:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 878:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 879:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
 880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
 881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
 883:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
 884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 17


 886:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
 887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
 888:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.Mode == SPI_MODE_SLAVE) || (initial_TxXferCount == 0x01U))
 890:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
 892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Transmit data in 16 Bit mode */
 896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     while (hspi->TxXferCount > 0U)
 897:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Wait until TXE flag is set to send data */
 899:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXE))
 900:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
 902:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 904:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
 906:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Timeout management */
 908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
 909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           errorcode = HAL_TIMEOUT;
 911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 913:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 915:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 916:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 917:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 8 Bit mode */
 918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
 919:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.Mode == SPI_MODE_SLAVE) || (initial_TxXferCount == 0x01U))
 921:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->TxXferCount > 1U)
 923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 924:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* write on the data register in packing mode */
 925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
 926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 929:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
 930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         *((__IO uint8_t *)&hspi->Instance->DR) = (*hspi->pTxBuffPtr);
 932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr ++;
 933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 935:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     while (hspi->TxXferCount > 0U)
 937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 938:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Wait until TXE flag is set to send data */
 939:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXE))
 940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->TxXferCount > 1U)
 942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
ARM GAS  /tmp/cc5SiBtg.s 			page 18


 943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* write on the data register in packing mode */
 944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
 945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 948:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         else
 949:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           *((__IO uint8_t *)&hspi->Instance->DR) = (*hspi->pTxBuffPtr);
 951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 954:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 955:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
 956:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 957:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Timeout management */
 958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
 959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 960:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           errorcode = HAL_TIMEOUT;
 961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 963:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 964:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 965:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 966:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 967:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 968:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable CRC Transmission */
 969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 970:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
 972:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 973:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 974:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 975:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transaction */
 976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTxTransaction(hspi, Timeout, tickstart) != HAL_OK)
 977:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 978:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_FLAG;
 979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 980:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 981:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear overrun flag in 2 Lines communication mode because received is not read */
 982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_2LINES)
 983:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_OVRFLAG(hspi);
 985:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 986:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
 988:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 989:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
 990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 991:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
 992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 994:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 995:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 996:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error:
 997:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
 998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
 999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
ARM GAS  /tmp/cc5SiBtg.s 			page 19


1000:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
1001:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
1003:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Receive an amount of data in blocking mode.
1004:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1005:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
1006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pData pointer to data buffer
1007:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be received
1008:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
1009:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1011:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Receive(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size, uint32_t 
1012:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1013:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1014:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t tmpreg = 0U;
1015:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  *ptmpreg8;
1016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
1017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
1019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
1020:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1023:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
1024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1025:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES))
1028:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_BUSY_RX;
1030:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
1031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_SPI_TransmitReceive(hspi, pData, pData, Size, Timeout);
1032:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1034:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
1035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
1036:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1037:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
1038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
1039:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1040:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0U))
1041:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1045:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1046:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
1047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_RX;
1048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1049:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
1050:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
1051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
1052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*Init field not used in handle to zero */
1054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)NULL;
1055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
1056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
ARM GAS  /tmp/cc5SiBtg.s 			page 20


1057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
1058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
1059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1060:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1061:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
1062:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1063:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1064:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
1065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* this is done to handle the CRCNEXT before the latest data */
1066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount--;
1067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1070:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the Rx Fifo threshold */
1071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1073:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 16bit */
1074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1075:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1076:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1077:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1078:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 8bit */
1079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1081:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1082:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure communication direction: 1Line */
1083:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
1084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI Peripheral before set 1Line direction (BIDIOE bit) */
1086:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
1087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
1088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1089:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1090:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
1091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
1092:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
1094:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
1095:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1097:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in 8 Bit mode */
1098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize <= SPI_DATASIZE_8BIT)
1099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1100:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Transfer loop */
1101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     while (hspi->RxXferCount > 0U)
1102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Check the RXNE flag */
1104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXNE))
1105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* read the received data */
1107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (* (uint8_t *)hspi->pRxBuffPtr) = *(__IO uint8_t *)&hspi->Instance->DR;
1108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
1109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
1110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
1112:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1113:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Timeout management */
ARM GAS  /tmp/cc5SiBtg.s 			page 21


1114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
1115:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           errorcode = HAL_TIMEOUT;
1117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
1118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
1119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1120:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1121:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1124:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Transfer loop */
1126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     while (hspi->RxXferCount > 0U)
1127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Check the RXNE flag */
1129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXNE))
1130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)hspi->Instance->DR;
1132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
1133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
1134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1135:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
1136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1137:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Timeout management */
1138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
1139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           errorcode = HAL_TIMEOUT;
1141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
1142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
1143:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1147:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Handle the CRC Transmission */
1150:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1151:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* freeze the CRC before the latest data */
1153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
1154:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Read the latest data */
1156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, Timeout, tickstart) != HAL_OK)
1157:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* the latest data has not been received */
1159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_TIMEOUT;
1160:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       goto error;
1161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1163:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Receive last data in 16 Bit mode */
1164:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1166:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)hspi->Instance->DR;
1167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1168:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Receive last data in 8 Bit mode */
1169:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
1170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
ARM GAS  /tmp/cc5SiBtg.s 			page 22


1171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (*(uint8_t *)hspi->pRxBuffPtr) = *(__IO uint8_t *)&hspi->Instance->DR;
1172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1173:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1174:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait the CRC data */
1175:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, Timeout, tickstart) != HAL_OK)
1176:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1177:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
1178:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_TIMEOUT;
1179:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       goto error;
1180:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1181:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Read CRC to Flush DR and RXNE flag */
1183:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.DataSize == SPI_DATASIZE_16BIT)
1184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1185:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Read 16bit CRC */
1186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       tmpreg = READ_REG(hspi->Instance->DR);
1187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
1188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       UNUSED(tmpreg);
1189:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1190:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
1191:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1192:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Initialize the 8bit temporary pointer */
1193:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
1194:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Read 8bit CRC */
1195:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       tmpreg8 = *ptmpreg8;
1196:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
1197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       UNUSED(tmpreg8);
1198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((hspi->Init.DataSize == SPI_DATASIZE_8BIT) && (hspi->Init.CRCLength == SPI_CRC_LENGTH_16B
1200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, Timeout, tickstart) != HAL_OK)
1202:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Error on the CRC reception */
1204:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
1205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           errorcode = HAL_TIMEOUT;
1206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
1207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Read 8bit CRC again in case of 16bit CRC in 8bit Data mode */
1209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmpreg8 = *ptmpreg8;
1210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* To avoid GCC warning */
1211:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         UNUSED(tmpreg8);
1212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1216:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1217:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transaction */
1218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTransaction(hspi, Timeout, tickstart) != HAL_OK)
1219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_FLAG;
1221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1223:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if CRC error occurred */
1225:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_CRCERR))
1226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
ARM GAS  /tmp/cc5SiBtg.s 			page 23


1228:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
1229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1230:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
1233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1237:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
1239:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1240:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
1242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
1244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
1245:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1246:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
1247:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Transmit and Receive an amount of data in blocking mode.
1248:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
1250:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pTxData pointer to transmission data buffer
1251:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pRxData pointer to reception data buffer
1252:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent and received
1253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
1254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_TransmitReceive(SPI_HandleTypeDef *hspi, uint8_t *pTxData, uint8_t *pRxDa
1257:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                           uint32_t Timeout)
1258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t             initial_TxXferCount;
1260:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t             initial_RxXferCount;
1261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
1262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_StateTypeDef tmp_state;
1263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tickstart;
1264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t tmpreg = 0U;
1266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             spi_cr1;
1267:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             spi_cr2;
1268:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  *ptmpreg8;
1269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
1270:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Variable used to alternate Rx and Tx during transfer */
1273:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             txallowed = 1U;
1274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef    errorcode = HAL_OK;
1275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1276:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check Direction parameter */
1277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES(hspi->Init.Direction));
1278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
1280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
1281:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
1283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
1284:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 24


1285:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init temporary variables */
1286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_state           = hspi->State;
1287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
1288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
1289:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_RxXferCount = Size;
1290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   spi_cr1             = READ_REG(hspi->Instance->CR1);
1292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   spi_cr2             = READ_REG(hspi->Instance->CR2);
1293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (!((tmp_state == HAL_SPI_STATE_READY) || \
1296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
1297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
1299:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1300:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pTxData == NULL) || (pRxData == NULL) || (Size == 0U))
1303:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Don't overwrite in case of HAL_SPI_STATE_BUSY_RX */
1309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_BUSY_RX)
1310:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_BUSY_TX_RX;
1312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1313:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
1315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
1317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
1318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
1319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
1320:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
1321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
1322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*Init field not used in handle to zero */
1324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
1325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
1326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
1329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1330:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
1332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the Rx Fifo threshold */
1336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) || (initial_RxXferCount > 1U))
1337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set fiforxthreshold according the reception data length: 16bit */
1339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
ARM GAS  /tmp/cc5SiBtg.s 			page 25


1342:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set fiforxthreshold according the reception data length: 8bit */
1344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1345:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
1348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
1349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1350:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
1351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
1352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit and Receive data in 16 Bit mode */
1355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.Mode == SPI_MODE_SLAVE) || (initial_TxXferCount == 0x01U))
1358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
1360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
1361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
1362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1364:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Enable CRC Transmission */
1365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((hspi->TxXferCount == 0U) && (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE))
1366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Set NSS Soft to received correctly the CRC on slave mode with NSS pulse activated */
1368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((READ_BIT(spi_cr1, SPI_CR1_MSTR) == 0U) && (READ_BIT(spi_cr2, SPI_CR2_NSSP) == SPI_CR2_
1369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->Instance->CR1, SPI_CR1_SSM);
1371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1372:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
1373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1374:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1375:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1376:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     while ((hspi->TxXferCount > 0U) || (hspi->RxXferCount > 0U))
1378:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1379:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Check TXE flag */
1380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXE)) && (hspi->TxXferCount > 0U) && (txallowed == 1U)
1381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
1383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
1384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
1385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a reception (Rx). Tx not allowed */
1386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         txallowed = 0U;
1387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Enable CRC Transmission */
1390:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((hspi->TxXferCount == 0U) && (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE))
1391:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Set NSS Soft to received correctly the CRC on slave mode with NSS pulse activated */
1393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if ((READ_BIT(spi_cr1, SPI_CR1_MSTR) == 0U) && (READ_BIT(spi_cr2, SPI_CR2_NSSP) == SPI_CR
1394:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
1395:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->Instance->CR1, SPI_CR1_SSM);
1396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
1397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
1398:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
ARM GAS  /tmp/cc5SiBtg.s 			page 26


1399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1400:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1402:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Check RXNE flag */
1403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXNE)) && (hspi->RxXferCount > 0U))
1404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)hspi->Instance->DR;
1406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
1407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
1408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a Transmission (Tx). Tx is allowed */
1409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         txallowed = 1U;
1410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY))
1412:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         errorcode = HAL_TIMEOUT;
1414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
1415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         goto error;
1416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit and Receive data in 8 Bit mode */
1420:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.Mode == SPI_MODE_SLAVE) || (initial_TxXferCount == 0x01U))
1423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->TxXferCount > 1U)
1425:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
1427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
1428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
1429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
1431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         *(__IO uint8_t *)&hspi->Instance->DR = (*hspi->pTxBuffPtr);
1433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr++;
1434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
1435:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1436:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Enable CRC Transmission */
1438:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((hspi->TxXferCount == 0U) && (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE))
1439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Set NSS Soft to received correctly the CRC on slave mode with NSS pulse activated */
1441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if ((READ_BIT(spi_cr1, SPI_CR1_MSTR) == 0U) && (READ_BIT(spi_cr2, SPI_CR2_NSSP) == SPI_CR
1442:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
1443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->Instance->CR1, SPI_CR1_SSM);
1444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
1445:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
1446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1447:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1448:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     while ((hspi->TxXferCount > 0U) || (hspi->RxXferCount > 0U))
1451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Check TXE flag */
1453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXE)) && (hspi->TxXferCount > 0U) && (txallowed == 1U)
1454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->TxXferCount > 1U)
ARM GAS  /tmp/cc5SiBtg.s 			page 27


1456:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
1458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
1459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
1460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         else
1462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           *(__IO uint8_t *)&hspi->Instance->DR = (*hspi->pTxBuffPtr);
1464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
1465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
1466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1467:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a reception (Rx). Tx not allowed */
1468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         txallowed = 0U;
1469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1470:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Enable CRC Transmission */
1472:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((hspi->TxXferCount == 0U) && (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE))
1473:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Set NSS Soft to received correctly the CRC on slave mode with NSS pulse activated */
1475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if ((READ_BIT(spi_cr1, SPI_CR1_MSTR) == 0U) && (READ_BIT(spi_cr2, SPI_CR2_NSSP) == SPI_CR
1476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
1477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->Instance->CR1, SPI_CR1_SSM);
1478:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
1479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
1480:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1482:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1483:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1484:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Wait until RXNE flag is reset */
1485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXNE)) && (hspi->RxXferCount > 0U))
1486:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->RxXferCount > 1U)
1488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1489:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)hspi->Instance->DR;
1490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
1491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount -= 2U;
1492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (hspi->RxXferCount <= 1U)
1493:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
1494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             /* Set RX Fifo threshold before to switch on 8 bit data size */
1495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
1497:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1498:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         else
1499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (*(uint8_t *)hspi->pRxBuffPtr) = *(__IO uint8_t *)&hspi->Instance->DR;
1501:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr++;
1502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount--;
1503:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1504:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a Transmission (Tx). Tx is allowed */
1505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         txallowed = 1U;
1506:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((((HAL_GetTick() - tickstart) >=  Timeout) && ((Timeout != HAL_MAX_DELAY))) || (Timeout =
1508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         errorcode = HAL_TIMEOUT;
1510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
1511:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         goto error;
1512:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
ARM GAS  /tmp/cc5SiBtg.s 			page 28


1513:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1514:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1515:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Read CRC from DR to close CRC calculation process */
1518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1519:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait until TXE flag */
1521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, Timeout, tickstart) != HAL_OK)
1522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1523:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Error on the CRC reception */
1524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
1525:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_TIMEOUT;
1526:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       goto error;
1527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1528:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Read CRC */
1529:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.DataSize == SPI_DATASIZE_16BIT)
1530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1531:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Read 16bit CRC */
1532:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       tmpreg = READ_REG(hspi->Instance->DR);
1533:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
1534:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       UNUSED(tmpreg);
1535:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
1537:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Initialize the 8bit temporary pointer */
1539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
1540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Read 8bit CRC */
1541:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       tmpreg8 = *ptmpreg8;
1542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
1543:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       UNUSED(tmpreg8);
1544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->Init.CRCLength == SPI_CRC_LENGTH_16BIT)
1546:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1547:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, Timeout, tickstart) != HAL_OK)
1548:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1549:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Error on the CRC reception */
1550:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
1551:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           errorcode = HAL_TIMEOUT;
1552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
1553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Read 8bit CRC again in case of 16bit CRC in 8bit Data mode */
1555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmpreg8 = *ptmpreg8;
1556:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* To avoid GCC warning */
1557:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         UNUSED(tmpreg8);
1558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1560:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1561:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if CRC error occurred */
1563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_CRCERR))
1564:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
1566:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Clear CRC Flag */
1567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
1568:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1569:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
ARM GAS  /tmp/cc5SiBtg.s 			page 29


1570:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1571:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1572:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transaction */
1574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTxTransaction(hspi, Timeout, tickstart) != HAL_OK)
1575:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1576:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1577:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_FLAG;
1578:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1579:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
1581:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1583:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1586:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
1587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   
1589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
1590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1591:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
1592:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
1593:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1594:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
1595:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Transmit an amount of data in non-blocking mode with Interrupt.
1596:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1597:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
1598:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pData pointer to data buffer
1599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent
1600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1601:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1602:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Transmit_IT(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size)
1603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1604:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
1605:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check Direction parameter */
1607:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES_OR_1LINE(hspi->Init.Direction));
1608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1609:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1610:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0U))
1611:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1613:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1614:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1615:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1617:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
1619:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1620:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1621:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1622:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
1623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
1624:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
1626:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_TX;
ARM GAS  /tmp/cc5SiBtg.s 			page 30


1627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
1629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
1630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
1631:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1632:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init field not used in handle to zero */
1633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)NULL;
1634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
1635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
1636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
1637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the function for IT treatment */
1639:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1640:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1641:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR = SPI_TxISR_16BIT;
1642:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1643:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1644:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR = SPI_TxISR_8BIT;
1646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1647:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure communication direction : 1Line */
1649:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
1650:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1651:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI Peripheral before set 1Line direction (BIDIOE bit) */
1652:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
1653:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
1654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1655:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1657:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
1658:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1659:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1660:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
1661:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1662:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1664:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
1665:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
1666:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1667:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
1668:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
1669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
1672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable TXE and ERR interrupt */
1674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_TXE | SPI_IT_ERR));
1675:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
1677:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
1678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
1679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1680:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
1681:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Receive an amount of data in non-blocking mode with Interrupt.
1682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
ARM GAS  /tmp/cc5SiBtg.s 			page 31


1684:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pData pointer to data buffer
1685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent
1686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1687:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1688:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Receive_IT(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size)
1689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1690:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
1691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1692:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1693:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1694:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1695:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
1696:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1697:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1698:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Direction == SPI_DIRECTION_2LINES) && (hspi->Init.Mode == SPI_MODE_MASTER))
1700:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_BUSY_RX;
1702:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
1703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_SPI_TransmitReceive_IT(hspi, pData, pData, Size);
1704:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1705:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1706:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1707:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0U))
1708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1709:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1710:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1711:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1712:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1713:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
1714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
1715:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1716:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
1717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_RX;
1718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
1720:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
1721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
1722:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1723:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init field not used in handle to zero */
1724:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)NULL;
1725:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
1726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
1727:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
1728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1729:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the data size to adapt Rx threshold and the set the function for IT treatment */
1730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1731:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1732:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 16 bit */
1733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_16BIT;
1735:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1737:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1738:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 8 bit */
1739:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1740:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_8BIT;
ARM GAS  /tmp/cc5SiBtg.s 			page 32


1741:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1742:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1743:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure communication direction : 1Line */
1744:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
1745:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI Peripheral before set 1Line direction (BIDIOE bit) */
1747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
1748:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
1749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1750:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1751:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1752:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
1753:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1755:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->CRCSize = 1U;
1756:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.DataSize <= SPI_DATASIZE_8BIT) && (hspi->Init.CRCLength == SPI_CRC_LENGTH_16BIT
1757:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1758:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->CRCSize = 2U;
1759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1760:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
1761:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1762:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1763:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1764:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->CRCSize = 0U;
1765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1767:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Note : The SPI must be enabled after unlocking current process
1769:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             to avoid the risk of SPI interrupt handle execution before current
1770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             process unlock */
1771:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1772:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
1773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
1774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
1776:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
1777:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1778:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1779:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
1780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1781:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable RXNE and ERR interrupt */
1782:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_RXNE | SPI_IT_ERR));
1783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1784:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
1785:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
1786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
1787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1788:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
1789:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Transmit and Receive an amount of data in non-blocking mode with Interrupt.
1790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
1792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pTxData pointer to transmission data buffer
1793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pRxData pointer to reception data buffer
1794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent and received
1795:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1797:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_TransmitReceive_IT(SPI_HandleTypeDef *hspi, uint8_t *pTxData, uint8_t *pR
ARM GAS  /tmp/cc5SiBtg.s 			page 33


1798:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
1800:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_StateTypeDef tmp_state;
1801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef    errorcode = HAL_OK;
1802:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1803:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check Direction parameter */
1804:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES(hspi->Init.Direction));
1805:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1806:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init temporary variables */
1807:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_state           = hspi->State;
1808:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
1809:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (!((tmp_state == HAL_SPI_STATE_READY) || \
1811:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
1812:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
1814:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1816:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1817:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pTxData == NULL) || (pRxData == NULL) || (Size == 0U))
1818:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1820:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1821:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1822:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process locked */
1824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
1825:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1826:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Don't overwrite in case of HAL_SPI_STATE_BUSY_RX */
1827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_BUSY_RX)
1828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1829:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_BUSY_TX_RX;
1830:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1832:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
1833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
1835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
1836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
1837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
1838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
1839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
1840:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1841:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the function for IT treatment */
1842:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1844:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR     = SPI_2linesRxISR_16BIT;
1845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_16BIT;
1846:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1847:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR     = SPI_2linesRxISR_8BIT;
1850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_8BIT;
1851:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1852:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1853:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
ARM GAS  /tmp/cc5SiBtg.s 			page 34


1855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1856:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1857:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->CRCSize = 1U;
1858:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.DataSize <= SPI_DATASIZE_8BIT) && (hspi->Init.CRCLength == SPI_CRC_LENGTH_16BIT
1859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->CRCSize = 2U;
1861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1862:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
1863:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1864:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1865:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->CRCSize = 0U;
1867:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1868:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1870:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if packing mode is enabled and if there is more than 2 data to receive */
1871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) || (Size >= 2U))
1872:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1873:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 16 bit */
1874:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1875:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1876:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1877:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1878:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 8 bit */
1879:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1883:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
1884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
1885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1886:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
1887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
1888:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1890:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
1891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable TXE, RXNE and ERR interrupt */
1893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_TXE | SPI_IT_RXNE | SPI_IT_ERR));
1894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
1896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
1897:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
1898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1899:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
1900:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Transmit an amount of data in non-blocking mode with DMA.
1901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1902:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
1903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pData pointer to data buffer
1904:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent
1905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1906:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Transmit_DMA(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size)
1908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
1910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check tx dma handle */
ARM GAS  /tmp/cc5SiBtg.s 			page 35


1912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DMA_HANDLE(hspi->hdmatx));
1913:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check Direction parameter */
1915:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES_OR_1LINE(hspi->Init.Direction));
1916:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1917:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
1918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
1919:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1921:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
1923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1924:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0U))
1927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1929:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
1933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_TX;
1934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1935:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
1936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
1937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
1938:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1939:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init field not used in handle to zero */
1940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)NULL;
1941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
1942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
1943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
1944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
1945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure communication direction : 1Line */
1947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
1948:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1949:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI Peripheral before set 1Line direction (BIDIOE bit) */
1950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
1951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
1952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1954:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1955:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
1956:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1957:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
1959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1960:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the SPI TxDMA Half transfer complete callback */
1963:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferHalfCpltCallback = SPI_DMAHalfTransmitCplt;
1964:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1965:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the SPI TxDMA transfer complete callback */
1966:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback = SPI_DMATransmitCplt;
1967:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1968:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the DMA error callback */
ARM GAS  /tmp/cc5SiBtg.s 			page 36


1969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferErrorCallback = SPI_DMAError;
1970:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the DMA AbortCpltCallback */
1972:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback = NULL;
1973:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1974:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMATX);
1975:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Packing mode is enabled only if the DMA setting is HALWORD */
1976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.DataSize <= SPI_DATASIZE_8BIT) && (hspi->hdmatx->Init.MemDataAlignment == DMA_MDA
1977:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1978:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check the even/odd of the data size + crc if enabled */
1979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->TxXferCount & 0x1U) == 0U)
1980:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1981:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMATX);
1982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount >> 1U);
1983:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
1985:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1986:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR2, SPI_CR2_LDMATX);
1987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount >> 1U) + 1U;
1988:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1989:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1991:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the Tx DMA Stream/Channel */
1992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_OK != HAL_DMA_Start_IT(hspi->hdmatx, (uint32_t)hspi->pTxBuffPtr, (uint32_t)&hspi->Instanc
1993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
1994:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1995:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update SPI error code */
1996:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
1997:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2000:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2001:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
2003:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
2004:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2005:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
2006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
2007:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2008:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2009:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the SPI Error Interrupt Bit */
2010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_ERR));
2011:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2012:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable Tx DMA Request */
2013:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SET_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN);
2014:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2015:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
2016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
2017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
2018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
2019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2020:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Receive an amount of data in non-blocking mode with DMA.
2023:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   In case of MASTER mode and SPI_DIRECTION_2LINES direction, hdmatx shall be defined.
2024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2025:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
ARM GAS  /tmp/cc5SiBtg.s 			page 37


2026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pData pointer to data buffer
2027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   When the CRC feature is enabled the pData Length must be Size + 1.
2028:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent
2029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2030:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Receive_DMA(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size)
2032:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
2034:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check rx dma handle */
2036:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DMA_HANDLE(hspi->hdmarx));
2037:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
2039:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2040:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
2041:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Direction == SPI_DIRECTION_2LINES) && (hspi->Init.Mode == SPI_MODE_MASTER))
2045:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2046:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_BUSY_RX;
2047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check tx dma handle */
2049:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_DMA_HANDLE(hspi->hdmatx));
2050:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
2052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_SPI_TransmitReceive_DMA(hspi, pData, pData, Size);
2053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
2056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
2057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0U))
2059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2060:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2061:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2062:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2063:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2064:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
2065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_RX;
2066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
2067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
2068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
2069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
2070:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*Init field not used in handle to zero */
2072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
2073:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
2074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
2075:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
2076:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2077:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure communication direction : 1Line */
2078:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
2079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI Peripheral before set 1Line direction (BIDIOE bit) */
2081:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
2082:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
ARM GAS  /tmp/cc5SiBtg.s 			page 38


2083:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
2086:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
2087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
2088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2089:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
2090:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
2092:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if defined (STM32F302xC) || defined (STM32F303xC) || defined (STM32F373xC) || defined (STM32F358xx
2094:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Packing mode management is enabled by the DMA settings */
2095:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.DataSize <= SPI_DATASIZE_8BIT) && (hspi->hdmarx->Init.MemDataAlignment == DMA_MDA
2096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2097:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Restriction the DMA data received is not allowed in this mode */
2098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2100:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* STM32F302xC || STM32F303xC || STM32F373xC || STM32F358xx || STM32F378xx */
2102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMARX);
2104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
2105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 16bit */
2107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
2108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
2110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 8bit */
2112:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
2113:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmarx->Init.MemDataAlignment == DMA_MDATAALIGN_HALFWORD)
2115:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set RX Fifo threshold according the reception data length: 16bit */
2117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
2118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((hspi->RxXferCount & 0x1U) == 0x0U)
2120:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2121:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMARX);
2122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = hspi->RxXferCount >> 1U;
2123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2124:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->Instance->CR2, SPI_CR2_LDMARX);
2127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = (hspi->RxXferCount >> 1U) + 1U;
2128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the SPI RxDMA Half transfer complete callback */
2133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferHalfCpltCallback = SPI_DMAHalfReceiveCplt;
2134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2135:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the SPI Rx DMA transfer complete callback */
2136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferCpltCallback = SPI_DMAReceiveCplt;
2137:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the DMA error callback */
2139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferErrorCallback = SPI_DMAError;
ARM GAS  /tmp/cc5SiBtg.s 			page 39


2140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the DMA AbortCpltCallback */
2142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferAbortCallback = NULL;
2143:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the Rx DMA Stream/Channel  */
2145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_OK != HAL_DMA_Start_IT(hspi->hdmarx, (uint32_t)&hspi->Instance->DR, (uint32_t)hspi->pRxBu
2146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
2147:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update SPI error code */
2149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2150:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2151:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2154:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
2156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
2157:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
2159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
2160:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the SPI Error Interrupt Bit */
2163:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_ERR));
2164:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable Rx DMA Request */
2166:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SET_BIT(hspi->Instance->CR2, SPI_CR2_RXDMAEN);
2167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2168:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error:
2169:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
2170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
2171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
2172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2173:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2174:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2175:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Transmit and Receive an amount of data in non-blocking mode with DMA.
2176:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2177:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2178:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pTxData pointer to transmission data buffer
2179:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pRxData pointer to reception data buffer
2180:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   When the CRC feature is enabled the pRxData Length must be Size + 1
2181:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent
2182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2183:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_TransmitReceive_DMA(SPI_HandleTypeDef *hspi, uint8_t *pTxData, uint8_t *p
2185:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                               uint16_t Size)
2186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
2188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_StateTypeDef tmp_state;
2189:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
2190:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2191:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check rx & tx dma handles */
2192:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DMA_HANDLE(hspi->hdmarx));
2193:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DMA_HANDLE(hspi->hdmatx));
2194:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2195:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check Direction parameter */
2196:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES(hspi->Init.Direction));
ARM GAS  /tmp/cc5SiBtg.s 			page 40


2197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process locked */
2199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
2200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init temporary variables */
2202:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_state           = hspi->State;
2203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
2204:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (!((tmp_state == HAL_SPI_STATE_READY) ||
2206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
2207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
2209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2211:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pTxData == NULL) || (pRxData == NULL) || (Size == 0U))
2213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2216:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2217:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Don't overwrite in case of HAL_SPI_STATE_BUSY_RX */
2219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_BUSY_RX)
2220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_BUSY_TX_RX;
2222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2223:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
2225:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
2226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
2227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
2228:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
2229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
2230:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
2231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
2232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init field not used in handle to zero */
2234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
2235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
2236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2237:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
2238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
2239:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
2240:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
2242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
2244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2245:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if defined (STM32F302xC) || defined (STM32F303xC) || defined (STM32F373xC) || defined (STM32F358xx
2246:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Packing mode management is enabled by the DMA settings */
2247:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.DataSize <= SPI_DATASIZE_8BIT) && (hspi->hdmarx->Init.MemDataAlignment == DMA_MDA
2248:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Restriction the DMA data received is not allowed in this mode */
2250:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2251:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2252:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* STM32F302xC || STM32F303xC || STM32F373xC || STM32F358xx || STM32F378xx */
ARM GAS  /tmp/cc5SiBtg.s 			page 41


2254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset the threshold bit */
2256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMATX | SPI_CR2_LDMARX);
2257:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* The packing mode management is enabled by the DMA settings according the spi data size */
2259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
2260:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set fiforxthreshold according the reception data length: 16bit */
2262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
2263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
2265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 8bit */
2267:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
2268:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmatx->Init.MemDataAlignment == DMA_MDATAALIGN_HALFWORD)
2270:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((hspi->TxXferSize & 0x1U) == 0x0U)
2272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2273:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMATX);
2274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount = hspi->TxXferCount >> 1U;
2275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2276:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->Instance->CR2, SPI_CR2_LDMATX);
2279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount = (hspi->TxXferCount >> 1U) + 1U;
2280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2281:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmarx->Init.MemDataAlignment == DMA_MDATAALIGN_HALFWORD)
2284:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2285:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set RX Fifo threshold according the reception data length: 16bit */
2286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
2287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((hspi->RxXferCount & 0x1U) == 0x0U)
2289:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMARX);
2291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = hspi->RxXferCount >> 1U;
2292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->Instance->CR2, SPI_CR2_LDMARX);
2296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = (hspi->RxXferCount >> 1U) + 1U;
2297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2299:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2300:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if we are in Rx only or in Rx/Tx Mode and configure the DMA transfer complete callback *
2302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State == HAL_SPI_STATE_BUSY_RX)
2303:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set the SPI Rx DMA Half transfer complete callback */
2305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferHalfCpltCallback = SPI_DMAHalfReceiveCplt;
2306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMAReceiveCplt;
2307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
2309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2310:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set the SPI Tx/Rx DMA Half transfer complete callback */
ARM GAS  /tmp/cc5SiBtg.s 			page 42


2311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferHalfCpltCallback = SPI_DMAHalfTransmitReceiveCplt;
2312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMATransmitReceiveCplt;
2313:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the DMA error callback */
2316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferErrorCallback = SPI_DMAError;
2317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the DMA AbortCpltCallback */
2319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferAbortCallback = NULL;
2320:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the Rx DMA Stream/Channel  */
2322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_OK != HAL_DMA_Start_IT(hspi->hdmarx, (uint32_t)&hspi->Instance->DR, (uint32_t)hspi->pRxBu
2323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
2324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update SPI error code */
2326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2330:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable Rx DMA Request */
2333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SET_BIT(hspi->Instance->CR2, SPI_CR2_RXDMAEN);
2334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the SPI Tx DMA transfer complete callback as NULL because the communication closing
2336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   is performed in DMA reception complete callback  */
2337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferHalfCpltCallback = NULL;
2338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback     = NULL;
2339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferErrorCallback    = NULL;
2340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback    = NULL;
2341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2342:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the Tx DMA Stream/Channel  */
2343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_OK != HAL_DMA_Start_IT(hspi->hdmatx, (uint32_t)hspi->pTxBuffPtr, (uint32_t)&hspi->Instanc
2344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
2345:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update SPI error code */
2347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2350:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
2354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
2355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
2357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
2358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the SPI Error Interrupt Bit */
2360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_ERR));
2361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable Tx DMA Request */
2363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SET_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN);
2364:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
2366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
2367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
ARM GAS  /tmp/cc5SiBtg.s 			page 43


2368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
2369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2372:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Abort ongoing transfer (blocking mode).
2373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi SPI handle.
2374:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   This procedure could be used for aborting any ongoing transfer (Tx and Rx),
2375:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         started in Interrupt or DMA mode.
2376:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         This procedure performs following operations :
2377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Disable SPI Interrupts (depending of transfer direction)
2378:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Disable the DMA transfer in the peripheral register (if enabled)
2379:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Abort DMA transfer by calling HAL_DMA_Abort (in case of transfer in DMA mode)
2380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Set handle State to READY
2381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   This procedure is executed in blocking mode : when exiting function, Abort is considere
2382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Abort(SPI_HandleTypeDef *hspi)
2385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
2387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
2388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t resetcount;
2389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2390:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Initialized local variable  */
2391:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   errorcode = HAL_OK;
2392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
2393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
2394:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2395:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear ERRIE interrupt to avoid error interrupts generation during Abort procedure */
2396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_ERRIE);
2397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2398:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable TXEIE, RXNEIE and ERRIE(mode fault event, overrun error, TI frame error) interrupts */
2399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_TXEIE))
2400:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR = SPI_AbortTx_ISR;
2402:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
2403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     do
2404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (count == 0U)
2406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
2409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
2411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
2412:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
2413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     count = resetcount;
2414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXNEIE))
2417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_AbortRx_ISR;
2419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
2420:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     do
2421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (count == 0U)
2423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
ARM GAS  /tmp/cc5SiBtg.s 			page 44


2425:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
2426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
2428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
2429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
2430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     count = resetcount;
2431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI DMA Tx request if enabled */
2434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_TXDMAEN))
2435:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2436:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Abort the SPI DMA Tx Stream/Channel : use blocking DMA Abort API (no callback) */
2437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmatx != NULL)
2438:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set the SPI DMA Abort callback :
2440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       will lead to call HAL_SPI_AbortCpltCallback() at end of DMA abort procedure */
2441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->hdmatx->XferAbortCallback = NULL;
2442:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Abort DMA Tx Handle linked to SPI Peripheral */
2444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (HAL_DMA_Abort(hspi->hdmatx) != HAL_OK)
2445:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2447:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2448:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable Tx DMA Request */
2450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, (SPI_CR2_TXDMAEN));
2451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, HAL_GetTick()) != HAL_OK)
2453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2456:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable SPI Peripheral */
2458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_DISABLE(hspi);
2459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Empty the FRLVL fifo */
2461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT,
2462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2467:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI DMA Rx request if enabled */
2469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXDMAEN))
2470:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Abort the SPI DMA Rx Stream/Channel : use blocking DMA Abort API (no callback) */
2472:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmarx != NULL)
2473:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set the SPI DMA Abort callback :
2475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       will lead to call HAL_SPI_AbortCpltCallback() at end of DMA abort procedure */
2476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->hdmarx->XferAbortCallback = NULL;
2477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2478:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Abort DMA Rx Handle linked to SPI Peripheral */
2479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (HAL_DMA_Abort(hspi->hdmarx) != HAL_OK)
2480:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
ARM GAS  /tmp/cc5SiBtg.s 			page 45


2482:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2483:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2484:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable peripheral */
2485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_DISABLE(hspi);
2486:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Control the BSY flag */
2488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_BSY, RESET, SPI_DEFAULT_TIMEOUT, HAL_GetTick
2489:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2493:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Empty the FRLVL fifo */
2494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT,
2495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2497:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2498:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable Rx DMA Request */
2500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, (SPI_CR2_RXDMAEN));
2501:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2503:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset Tx and Rx transfer counters */
2504:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
2505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
2506:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check error during Abort procedure */
2508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode == HAL_SPI_ERROR_ABORT)
2509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* return HAL_Error in case of error during Abort procedure */
2511:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2512:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2513:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
2514:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2515:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset errorCode */
2516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_NONE;
2517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2519:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear the Error flags in the SR register */
2520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_OVRFLAG(hspi);
2521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
2522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2523:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Restore hspi->state to ready */
2524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
2525:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2526:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
2527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2528:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2529:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Abort ongoing transfer (Interrupt mode).
2531:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi SPI handle.
2532:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   This procedure could be used for aborting any ongoing transfer (Tx and Rx),
2533:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         started in Interrupt or DMA mode.
2534:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         This procedure performs following operations :
2535:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Disable SPI Interrupts (depending of transfer direction)
2536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Disable the DMA transfer in the peripheral register (if enabled)
2537:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Abort DMA transfer by calling HAL_DMA_Abort_IT (in case of transfer in DMA mode)
2538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Set handle State to READY
ARM GAS  /tmp/cc5SiBtg.s 			page 46


2539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - At abort completion, call user abort complete callback
2540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   This procedure is executed in Interrupt mode, meaning that abort procedure could be
2541:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         considered as completed only when user abort complete callback is executed (not when ex
2542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2543:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Abort_IT(SPI_HandleTypeDef *hspi)
2545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2546:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
2547:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t abortcplt ;
2548:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
2549:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t resetcount;
2550:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2551:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Initialized local variable  */
2552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   errorcode = HAL_OK;
2553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   abortcplt = 1U;
2554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
2555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
2556:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2557:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear ERRIE interrupt to avoid error interrupts generation during Abort procedure */
2558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_ERRIE);
2559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2560:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Change Rx and Tx Irq Handler to Disable TXEIE, RXNEIE and ERRIE interrupts */
2561:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_TXEIE))
2562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR = SPI_AbortTx_ISR;
2564:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
2565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     do
2566:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (count == 0U)
2568:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2569:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2570:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
2571:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2572:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
2573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
2574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
2575:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     count = resetcount;
2576:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2577:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2578:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXNEIE))
2579:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_AbortRx_ISR;
2581:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
2582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     do
2583:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (count == 0U)
2585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2586:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
2588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
2590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
2591:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
2592:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     count = resetcount;
2593:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2594:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2595:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* If DMA Tx and/or DMA Rx Handles are associated to SPI Handle, DMA Abort complete callbacks sho
ARM GAS  /tmp/cc5SiBtg.s 			page 47


2596:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      before any call to DMA Abort functions */
2597:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DMA Tx Handle is valid */
2598:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->hdmatx != NULL)
2599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set DMA Abort Complete callback if UART DMA Tx request if enabled.
2601:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Otherwise, set it to NULL */
2602:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_TXDMAEN))
2603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2604:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->hdmatx->XferAbortCallback = SPI_DMATxAbortCallback;
2605:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
2607:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->hdmatx->XferAbortCallback = NULL;
2609:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2610:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2611:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DMA Rx Handle is valid */
2612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->hdmarx != NULL)
2613:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2614:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set DMA Abort Complete callback if UART DMA Rx request if enabled.
2615:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Otherwise, set it to NULL */
2616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXDMAEN))
2617:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->hdmarx->XferAbortCallback = SPI_DMARxAbortCallback;
2619:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2620:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
2621:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2622:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->hdmarx->XferAbortCallback = NULL;
2623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2624:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2626:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI DMA Tx request if enabled */
2627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_TXDMAEN))
2628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Abort the SPI DMA Tx Stream/Channel */
2630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmatx != NULL)
2631:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2632:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Abort DMA Tx Handle linked to SPI Peripheral */
2633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (HAL_DMA_Abort_IT(hspi->hdmatx) != HAL_OK)
2634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->hdmatx->XferAbortCallback = NULL;
2636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2639:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2640:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         abortcplt = 0U;
2641:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2642:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2643:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2644:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI DMA Rx request if enabled */
2645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXDMAEN))
2646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2647:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Abort the SPI DMA Rx Stream/Channel */
2648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmarx != NULL)
2649:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2650:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Abort DMA Rx Handle linked to SPI Peripheral */
2651:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (HAL_DMA_Abort_IT(hspi->hdmarx) !=  HAL_OK)
2652:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
ARM GAS  /tmp/cc5SiBtg.s 			page 48


2653:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->hdmarx->XferAbortCallback = NULL;
2654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2655:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2657:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2658:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         abortcplt = 0U;
2659:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2660:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2661:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2662:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (abortcplt == 1U)
2664:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2665:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Tx and Rx transfer counters */
2666:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount = 0U;
2667:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount = 0U;
2668:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check error during Abort procedure */
2670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode == HAL_SPI_ERROR_ABORT)
2671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* return HAL_Error in case of error during Abort procedure */
2673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_ERROR;
2674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2675:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
2676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2677:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Reset errorCode */
2678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCode = HAL_SPI_ERROR_NONE;
2679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2680:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2681:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Clear the Error flags in the SR register */
2682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_OVRFLAG(hspi);
2683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
2684:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Restore hspi->State to Ready */
2686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
2687:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2688:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* As no DMA to be aborted, call directly user Abort complete callback */
2689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
2690:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->AbortCpltCallback(hspi);
2691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
2692:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     HAL_SPI_AbortCpltCallback(hspi);
2693:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
2694:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2695:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2696:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
2697:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2698:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2700:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Pause the DMA Transfer.
2701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2702:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified SPI module.
2703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2704:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2705:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_DMAPause(SPI_HandleTypeDef *hspi)
2706:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2707:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
2708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
2709:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 49


2710:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI DMA Tx & Rx requests */
2711:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN);
2712:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2713:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
2714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
2715:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2716:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
2717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2720:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Resume the DMA Transfer.
2721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2722:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified SPI module.
2723:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2724:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2725:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_DMAResume(SPI_HandleTypeDef *hspi)
2726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2727:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
2728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
2729:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the SPI DMA Tx & Rx requests */
2731:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SET_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN);
2732:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
2734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
2735:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
2737:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2738:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2739:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2740:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Stop the DMA Transfer.
2741:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2742:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified SPI module.
2743:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2744:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2745:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_DMAStop(SPI_HandleTypeDef *hspi)
2746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
2748:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* The Lock is not implemented on this API to allow the user application
2749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      to call the HAL SPI API under callbacks HAL_SPI_TxCpltCallback() or HAL_SPI_RxCpltCallback() o
2750:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      when calling HAL_DMA_Abort() API the DMA TX/RX Transfer complete interrupt is generated
2751:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      and the correspond call back is executed HAL_SPI_TxCpltCallback() or HAL_SPI_RxCpltCallback() 
2752:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      */
2753:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Abort the SPI DMA tx Stream/Channel  */
2755:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->hdmatx != NULL)
2756:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2757:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (HAL_OK != HAL_DMA_Abort(hspi->hdmatx))
2758:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2760:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_ERROR;
2761:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2762:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2763:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Abort the SPI DMA rx Stream/Channel  */
2764:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->hdmarx != NULL)
2765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (HAL_OK != HAL_DMA_Abort(hspi->hdmarx))
ARM GAS  /tmp/cc5SiBtg.s 			page 50


2767:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2769:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_ERROR;
2770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2771:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2772:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI DMA Tx & Rx requests */
2774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN);
2775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
2776:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
2777:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2778:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2779:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle SPI interrupt request.
2781:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2782:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified SPI module.
2783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2784:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2785:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** void HAL_SPI_IRQHandler(SPI_HandleTypeDef *hspi)
2786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itsource = hspi->Instance->CR2;
2788:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itflag   = hspi->Instance->SR;
2789:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* SPI in mode Receiver ----------------------------------------------------*/
2791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((SPI_CHECK_FLAG(itflag, SPI_FLAG_OVR) == RESET) &&
2792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (SPI_CHECK_FLAG(itflag, SPI_FLAG_RXNE) != RESET) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT_RXN
2793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR(hspi);
2795:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
2796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2797:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2798:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* SPI in mode Transmitter -------------------------------------------------*/
2799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((SPI_CHECK_FLAG(itflag, SPI_FLAG_TXE) != RESET) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT_TXE)
2800:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR(hspi);
2802:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
2803:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2804:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2805:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* SPI in Error Treatment --------------------------------------------------*/
2806:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (((SPI_CHECK_FLAG(itflag, SPI_FLAG_MODF) != RESET) || (SPI_CHECK_FLAG(itflag, SPI_FLAG_OVR) !=
2807:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        || (SPI_CHECK_FLAG(itflag, SPI_FLAG_FRE) != RESET)) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT
2808:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2809:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* SPI Overrun error interrupt occurred ----------------------------------*/
2810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_CHECK_FLAG(itflag, SPI_FLAG_OVR) != RESET)
2811:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2812:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->State != HAL_SPI_STATE_BUSY_TX)
2813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2814:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_OVR);
2815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_SPI_CLEAR_OVRFLAG(hspi);
2816:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2817:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2818:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_SPI_CLEAR_OVRFLAG(hspi);
2820:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
2821:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2822:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 51


2824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* SPI Mode Fault error interrupt occurred -------------------------------*/
2825:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_CHECK_FLAG(itflag, SPI_FLAG_MODF) != RESET)
2826:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_MODF);
2828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_MODFFLAG(hspi);
2829:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2830:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* SPI Frame error interrupt occurred ------------------------------------*/
2832:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_CHECK_FLAG(itflag, SPI_FLAG_FRE) != RESET)
2833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FRE);
2835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_FREFLAG(hspi);
2836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
2839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2840:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable all interrupts */
2841:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, SPI_IT_RXNE | SPI_IT_TXE | SPI_IT_ERR);
2842:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->State = HAL_SPI_STATE_READY;
2844:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable the SPI DMA requests if enabled */
2845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((HAL_IS_BIT_SET(itsource, SPI_CR2_TXDMAEN)) || (HAL_IS_BIT_SET(itsource, SPI_CR2_RXDMAEN)
2846:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2847:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         CLEAR_BIT(hspi->Instance->CR2, (SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN));
2848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Abort the SPI DMA Rx channel */
2850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->hdmarx != NULL)
2851:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
2852:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Set the SPI DMA Abort callback :
2853:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           will lead to call HAL_SPI_ErrorCallback() at end of DMA abort procedure */
2854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->hdmarx->XferAbortCallback = SPI_DMAAbortOnError;
2855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmarx))
2856:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
2857:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2858:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
2859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
2860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Abort the SPI DMA Tx channel */
2861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->hdmatx != NULL)
2862:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
2863:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Set the SPI DMA Abort callback :
2864:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           will lead to call HAL_SPI_ErrorCallback() at end of DMA abort procedure */
2865:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->hdmatx->XferAbortCallback = SPI_DMAAbortOnError;
2866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmatx))
2867:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
2868:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
2870:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
2871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2872:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2873:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2874:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user error callback */
2875:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
2876:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCallback(hspi);
2877:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
2878:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         HAL_SPI_ErrorCallback(hspi);
2879:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
2880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
ARM GAS  /tmp/cc5SiBtg.s 			page 52


2881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
2883:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2886:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Tx Transfer completed callback.
2888:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2890:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_TxCpltCallback(SPI_HandleTypeDef *hspi)
2893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2897:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_TxCpltCallback should be implemented in the user file
2899:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2900:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2902:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Rx Transfer completed callback.
2904:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2906:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_RxCpltCallback(SPI_HandleTypeDef *hspi)
2909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2913:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_RxCpltCallback should be implemented in the user file
2915:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2916:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2917:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2919:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Tx and Rx Transfer completed callback.
2920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2921:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2924:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_TxRxCpltCallback(SPI_HandleTypeDef *hspi)
2925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2929:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_TxRxCpltCallback should be implemented in the user file
2931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2935:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Tx Half Transfer completed callback.
2936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
ARM GAS  /tmp/cc5SiBtg.s 			page 53


2938:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2939:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_TxHalfCpltCallback(SPI_HandleTypeDef *hspi)
2941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_TxHalfCpltCallback should be implemented in the user file
2947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2948:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2949:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Rx Half Transfer completed callback.
2952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2954:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2955:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2956:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_RxHalfCpltCallback(SPI_HandleTypeDef *hspi)
2957:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2960:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_RxHalfCpltCallback() should be implemented in the user file
2963:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2964:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2965:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2966:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2967:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Tx and Rx Half Transfer callback.
2968:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2970:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2972:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_TxRxHalfCpltCallback(SPI_HandleTypeDef *hspi)
2973:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2974:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2975:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2977:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2978:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_TxRxHalfCpltCallback() should be implemented in the user file
2979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2980:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2981:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2983:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  SPI error callback.
2984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2985:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2986:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2988:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_ErrorCallback(SPI_HandleTypeDef *hspi)
2989:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2991:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2994:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_ErrorCallback should be implemented in the user file
ARM GAS  /tmp/cc5SiBtg.s 			page 54


2995:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2996:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : The ErrorCode parameter in the hspi handle is updated by the SPI processes
2997:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             and user can use HAL_SPI_GetError() API to check the latest error occurred
2998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3000:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3001:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  SPI Abort Complete callback.
3003:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi SPI handle.
3004:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3005:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_AbortCpltCallback(SPI_HandleTypeDef *hspi)
3007:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3008:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
3009:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
3010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3011:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
3012:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_AbortCpltCallback can be implemented in the user file.
3013:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
3014:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3015:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @}
3018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3020:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI_Exported_Functions_Group3 Peripheral State and Errors functions
3021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief   SPI control functions
3022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
3023:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** @verbatim
3024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****  ===============================================================================
3025:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                       ##### Peripheral State and Errors functions #####
3026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****  ===============================================================================
3027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     [..]
3028:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     This subsection provides a set of functions allowing to control the SPI.
3029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      (+) HAL_SPI_GetState() API can be helpful to check in run-time the state of the SPI peripheral
3030:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      (+) HAL_SPI_GetError() check in run-time Errors occurring during communication
3031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** @endverbatim
3032:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
3033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3034:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3036:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Return the SPI handle state.
3037:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3039:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval SPI state
3040:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3041:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_SPI_StateTypeDef HAL_SPI_GetState(SPI_HandleTypeDef *hspi)
3042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Return SPI handle state */
3044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return hspi->State;
3045:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3046:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Return the SPI error code.
3049:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3050:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval SPI error code in bitmap format
ARM GAS  /tmp/cc5SiBtg.s 			page 55


3052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** uint32_t HAL_SPI_GetError(SPI_HandleTypeDef *hspi)
3054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Return SPI ErrorCode */
3056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return hspi->ErrorCode;
3057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3060:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @}
3061:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3062:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3063:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3064:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @}
3065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @addtogroup SPI_Private_Functions
3068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief   Private functions
3069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
3070:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3073:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI transmit process complete callback.
3074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3075:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3076:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3077:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3078:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMATransmitCplt(DMA_HandleTypeDef *hdma)
3079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3081:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
3082:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3083:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
3084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
3085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3086:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DMA Normal Mode */
3087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hdma->Instance->CCR & DMA_CCR_CIRC) != DMA_CCR_CIRC)
3088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3089:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable ERR interrupt */
3090:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_ERR);
3091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3092:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable Tx DMA Request */
3093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN);
3094:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3095:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check the end of the transaction */
3096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, tickstart) != HAL_OK)
3097:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
3099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3100:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Clear overrun flag in 2 Lines communication mode because received data is not read */
3102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.Direction == SPI_DIRECTION_2LINES)
3103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_OVRFLAG(hspi);
3105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount = 0U;
3108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
ARM GAS  /tmp/cc5SiBtg.s 			page 56


3109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
3111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3112:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
3113:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCallback(hspi);
3115:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       HAL_SPI_ErrorCallback(hspi);
3117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3120:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3121:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user Tx complete callback */
3122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxCpltCallback(hspi);
3124:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_TxCpltCallback(hspi);
3126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI receive process complete callback.
3131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3135:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAReceiveCplt(DMA_HandleTypeDef *hdma)
3136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3137:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
3139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t tmpreg = 0U;
3141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  *ptmpreg8;
3142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
3143:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
3146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
3147:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DMA Normal Mode */
3149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hdma->Instance->CCR & DMA_CCR_CIRC) != DMA_CCR_CIRC)
3150:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3151:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable ERR interrupt */
3152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_ERR);
3153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3154:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* CRC handling */
3156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3157:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Wait until RXNE flag */
3159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, SPI_DEFAULT_TIMEOUT, tickstart) !
3160:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Error on the CRC reception */
3162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
3163:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
3164:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Read CRC */
3165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
ARM GAS  /tmp/cc5SiBtg.s 			page 57


3166:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Read 16bit CRC */
3168:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmpreg = READ_REG(hspi->Instance->DR);
3169:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* To avoid GCC warning */
3170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         UNUSED(tmpreg);
3171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
3172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
3173:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3174:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Initialize the 8bit temporary pointer */
3175:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
3176:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Read 8bit CRC */
3177:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmpreg8 = *ptmpreg8;
3178:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* To avoid GCC warning */
3179:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         UNUSED(tmpreg8);
3180:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3181:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->Init.CRCLength == SPI_CRC_LENGTH_16BIT)
3182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
3183:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, SPI_DEFAULT_TIMEOUT, tickstar
3184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
3185:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             /* Error on the CRC reception */
3186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
3187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
3188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Read 8bit CRC again in case of 16bit CRC in 8bit Data mode */
3189:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           tmpreg8 = *ptmpreg8;
3190:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* To avoid GCC warning */
3191:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           UNUSED(tmpreg8);
3192:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
3193:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
3194:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3195:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3196:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check if we are in Master RX 2 line mode */
3198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.Direction == SPI_DIRECTION_2LINES) && (hspi->Init.Mode == SPI_MODE_MASTER))
3199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable Rx/Tx DMA Request (done by default to handle the case master rx direction 2 lines)
3201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN);
3202:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
3204:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Normal case */
3206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_RXDMAEN);
3207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check the end of the transaction */
3210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_EndRxTransaction(hspi, SPI_DEFAULT_TIMEOUT, tickstart) != HAL_OK)
3211:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCode = HAL_SPI_ERROR_FLAG;
3213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount = 0U;
3216:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
3217:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check if CRC error occurred */
3220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_CRCERR))
3221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
ARM GAS  /tmp/cc5SiBtg.s 			page 58


3223:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
3224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3225:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
3228:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
3230:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCallback(hspi);
3232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       HAL_SPI_ErrorCallback(hspi);
3234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3237:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user Rx complete callback */
3239:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3240:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxCpltCallback(hspi);
3241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_RxCpltCallback(hspi);
3243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3245:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3246:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3247:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI transmit receive process complete callback.
3248:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3250:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3251:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3252:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMATransmitReceiveCplt(DMA_HandleTypeDef *hdma)
3253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
3256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3257:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t tmpreg = 0U;
3258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  *ptmpreg8;
3259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
3260:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
3263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
3264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DMA Normal Mode */
3266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hdma->Instance->CCR & DMA_CCR_CIRC) != DMA_CCR_CIRC)
3267:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3268:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable ERR interrupt */
3269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_ERR);
3270:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* CRC handling */
3273:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((hspi->Init.DataSize == SPI_DATASIZE_8BIT) && (hspi->Init.CRCLength == SPI_CRC_LENGTH_8BI
3276:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_QUARTER_FULL, SPI_DEFAULT
3278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                           tickstart) != HAL_OK)
3279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
ARM GAS  /tmp/cc5SiBtg.s 			page 59


3280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Error on the CRC reception */
3281:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
3282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
3283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Initialize the 8bit temporary pointer */
3284:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
3285:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Read 8bit CRC */
3286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmpreg8 = *ptmpreg8;
3287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* To avoid GCC warning */
3288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         UNUSED(tmpreg8);
3289:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
3290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
3291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_HALF_FULL, SPI_DEFAULT_TI
3293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
3294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Error on the CRC reception */
3295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
3296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
3297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Read CRC to Flush DR and RXNE flag */
3298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmpreg = READ_REG(hspi->Instance->DR);
3299:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* To avoid GCC warning */
3300:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         UNUSED(tmpreg);
3301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
3302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3303:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check the end of the transaction */
3306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, tickstart) != HAL_OK)
3307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
3309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3310:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable Rx/Tx DMA Request */
3312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN);
3313:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount = 0U;
3315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount = 0U;
3316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
3317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check if CRC error occurred */
3320:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_CRCERR))
3321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
3323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
3324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
3328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
3330:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCallback(hspi);
3332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       HAL_SPI_ErrorCallback(hspi);
3334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
ARM GAS  /tmp/cc5SiBtg.s 			page 60


3337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user TxRx complete callback */
3339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxRxCpltCallback(hspi);
3341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3342:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_TxRxCpltCallback(hspi);
3343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3345:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI half transmit process complete callback.
3348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3350:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAHalfTransmitCplt(DMA_HandleTypeDef *hdma)
3353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user Tx half complete callback */
3357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxHalfCpltCallback(hspi);
3359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_TxHalfCpltCallback(hspi);
3361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3364:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI half receive process complete callback
3366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAHalfReceiveCplt(DMA_HandleTypeDef *hdma)
3371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3372:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3374:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user Rx half complete callback */
3375:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3376:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxHalfCpltCallback(hspi);
3377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3378:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_RxHalfCpltCallback(hspi);
3379:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI half transmit receive process complete callback.
3384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAHalfTransmitReceiveCplt(DMA_HandleTypeDef *hdma)
3389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3390:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3391:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user TxRx half complete callback */
3393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
ARM GAS  /tmp/cc5SiBtg.s 			page 61


3394:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxRxHalfCpltCallback(hspi);
3395:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_TxRxHalfCpltCallback(hspi);
3397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3398:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3400:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI communication error callback.
3402:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAError(DMA_HandleTypeDef *hdma)
3407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Stop the disable DMA transfer on SPI side */
3411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN);
3412:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
3414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
3415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user error callback */
3416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCallback(hspi);
3418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_ErrorCallback(hspi);
3420:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI communication abort callback, when initiated by HAL services on Error
3425:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         (To be called at end of DMA Abort procedure following error occurrence).
3426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma DMA handle.
3427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAAbortOnError(DMA_HandleTypeDef *hdma)
3430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
3433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
3434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3435:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user error callback */
3436:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCallback(hspi);
3438:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_ErrorCallback(hspi);
3440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3442:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI Tx communication abort callback, when initiated by user
3445:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         (To be called at end of DMA Tx Abort procedure following user abort request).
3446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   When this callback is executed, User Abort complete call back is called only if no
3447:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         Abort still ongoing for Rx DMA Handle.
3448:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma DMA handle.
3449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
ARM GAS  /tmp/cc5SiBtg.s 			page 62


3451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMATxAbortCallback(DMA_HandleTypeDef *hdma)
3452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback = NULL;
3456:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable Tx DMA Request */
3458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN);
3459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, HAL_GetTick()) != HAL_OK)
3461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
3463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable SPI Peripheral */
3466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
3467:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Empty the FRLVL fifo */
3469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT, HAL
3470:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
3472:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3473:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if an Abort process is still ongoing */
3475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->hdmarx != NULL)
3476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmarx->XferAbortCallback != NULL)
3478:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3480:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3482:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3483:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* No Abort process still ongoing : All DMA Stream/Channel are aborted, call user Abort Complete 
3484:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
3485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
3486:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check no error during Abort procedure */
3488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_ABORT)
3489:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset errorCode */
3491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_NONE;
3492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3493:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear the Error flags in the SR register */
3495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_OVRFLAG(hspi);
3496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
3497:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3498:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Restore hspi->State to Ready */
3499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State  = HAL_SPI_STATE_READY;
3500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3501:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user Abort complete callback */
3502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3503:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->AbortCpltCallback(hspi);
3504:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_AbortCpltCallback(hspi);
3506:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
ARM GAS  /tmp/cc5SiBtg.s 			page 63


3508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI Rx communication abort callback, when initiated by user
3511:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         (To be called at end of DMA Rx Abort procedure following user abort request).
3512:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   When this callback is executed, User Abort complete call back is called only if no
3513:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         Abort still ongoing for Tx DMA Handle.
3514:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma DMA handle.
3515:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMARxAbortCallback(DMA_HandleTypeDef *hdma)
3518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3519:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable SPI Peripheral */
3522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
3523:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferAbortCallback = NULL;
3525:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3526:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable Rx DMA Request */
3527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_RXDMAEN);
3528:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3529:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Control the BSY flag */
3530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_BSY, RESET, SPI_DEFAULT_TIMEOUT, HAL_GetTick()) 
3531:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3532:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
3533:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3534:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3535:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Empty the FRLVL fifo */
3536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT, HAL
3537:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
3539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3541:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if an Abort process is still ongoing */
3542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->hdmatx != NULL)
3543:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmatx->XferAbortCallback != NULL)
3545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3546:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3547:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3548:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3549:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3550:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* No Abort process still ongoing : All DMA Stream/Channel are aborted, call user Abort Complete 
3551:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
3552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
3553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check no error during Abort procedure */
3555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_ABORT)
3556:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3557:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset errorCode */
3558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_NONE;
3559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3560:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3561:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear the Error flags in the SR register */
3562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_OVRFLAG(hspi);
3563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
3564:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 64


3565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Restore hspi->State to Ready */
3566:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State  = HAL_SPI_STATE_READY;
3567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3568:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user Abort complete callback */
3569:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3570:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->AbortCpltCallback(hspi);
3571:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3572:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_AbortCpltCallback(hspi);
3573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3575:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3576:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3577:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Rx 8-bit handler for Transmit and Receive in Interrupt mode.
3578:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3579:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3581:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_8BIT(struct __SPI_HandleTypeDef *hspi)
3583:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in packing mode */
3585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->RxXferCount > 1U)
3586:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)(hspi->Instance->DR);
3588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr += sizeof(uint16_t);
3589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount -= 2U;
3590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->RxXferCount == 1U)
3591:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3592:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set RX Fifo threshold according the reception data length: 8bit */
3593:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
3594:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3595:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3596:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in 8 Bit mode */
3597:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
3598:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     *hspi->pRxBuffPtr = *((__IO uint8_t *)&hspi->Instance->DR);
3600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr++;
3601:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount--;
3602:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3604:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check end of the reception */
3605:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->RxXferCount == 0U)
3606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3607:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3609:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3610:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
3611:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->RxISR =  SPI_2linesRxISR_8BITCRC;
3612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3613:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3614:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3615:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable RXNE  and ERR interrupt */
3617:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_RXNE | SPI_IT_ERR));
3618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3619:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->TxXferCount == 0U)
3620:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3621:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SPI_CloseRxTx_ISR(hspi);
ARM GAS  /tmp/cc5SiBtg.s 			page 65


3622:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3624:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3626:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Rx 8-bit handler for Transmit and Receive in Interrupt mode.
3629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3631:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3632:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_8BITCRC(struct __SPI_HandleTypeDef *hspi)
3634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  *ptmpreg8;
3636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
3637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Initialize the 8bit temporary pointer */
3639:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
3640:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Read 8bit CRC to flush Data Register */
3641:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmpreg8 = *ptmpreg8;
3642:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* To avoid GCC warning */
3643:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(tmpreg8);
3644:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->CRCSize--;
3646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3647:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check end of the reception */
3648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->CRCSize == 0U)
3649:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3650:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable RXNE and ERR interrupt */
3651:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_RXNE | SPI_IT_ERR));
3652:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3653:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->TxXferCount == 0U)
3654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3655:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SPI_CloseRxTx_ISR(hspi);
3656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3657:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3658:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3659:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3660:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3661:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3662:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Tx 8-bit handler for Transmit and Receive in Interrupt mode.
3663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3664:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3665:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3666:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3667:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesTxISR_8BIT(struct __SPI_HandleTypeDef *hspi)
3668:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in packing Bit mode */
3670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->TxXferCount >= 2U)
3671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
3673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr += sizeof(uint16_t);
3674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount -= 2U;
3675:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 8 Bit mode */
3677:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
3678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 66


3679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     *(__IO uint8_t *)&hspi->Instance->DR = (*hspi->pTxBuffPtr);
3680:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr++;
3681:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount--;
3682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3684:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transmission */
3685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->TxXferCount == 0U)
3686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3687:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3688:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3690:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set CRC Next Bit to send CRC */
3691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
3692:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable TXE interrupt */
3693:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXE);
3694:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3695:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3696:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3697:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3698:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable TXE interrupt */
3699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXE);
3700:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->RxXferCount == 0U)
3702:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SPI_CloseRxTx_ISR(hspi);
3704:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3705:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3706:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3707:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3709:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Rx 16-bit handler for Transmit and Receive in Interrupt mode.
3710:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3711:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3712:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3713:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_16BIT(struct __SPI_HandleTypeDef *hspi)
3715:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3716:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in 16 Bit mode */
3717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)(hspi->Instance->DR);
3718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
3719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
3720:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->RxXferCount == 0U)
3722:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3723:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3724:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3725:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->RxISR =  SPI_2linesRxISR_16BITCRC;
3727:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3729:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3731:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable RXNE interrupt */
3732:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_RXNE);
3733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->TxXferCount == 0U)
3735:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
ARM GAS  /tmp/cc5SiBtg.s 			page 67


3736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SPI_CloseRxTx_ISR(hspi);
3737:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3738:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3739:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3740:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3741:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3742:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3743:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Manage the CRC 16-bit receive for Transmit and Receive in Interrupt mode.
3744:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3745:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3748:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_16BITCRC(struct __SPI_HandleTypeDef *hspi)
3749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3750:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t tmpreg = 0U;
3751:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3752:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Read 16bit CRC to flush Data Register */
3753:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmpreg = READ_REG(hspi->Instance->DR);
3754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* To avoid GCC warning */
3755:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(tmpreg);
3756:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3757:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable RXNE interrupt */
3758:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE_IT(hspi, SPI_IT_RXNE);
3759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3760:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_CloseRxTx_ISR(hspi);
3761:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3762:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3763:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3764:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Tx 16-bit handler for Transmit and Receive in Interrupt mode.
3766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3767:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3769:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesTxISR_16BIT(struct __SPI_HandleTypeDef *hspi)
3771:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3772:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
3773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
3774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
3775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
3776:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3777:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable CRC Transmission */
3778:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->TxXferCount == 0U)
3779:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3781:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3782:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set CRC Next Bit to send CRC */
3784:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
3785:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable TXE interrupt */
3786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXE);
3787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3788:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3789:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable TXE interrupt */
3792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXE);
ARM GAS  /tmp/cc5SiBtg.s 			page 68


3793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->RxXferCount == 0U)
3795:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SPI_CloseRxTx_ISR(hspi);
3797:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3798:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3800:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3802:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3803:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Manage the CRC 8-bit receive in Interrupt context.
3804:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3805:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3806:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3807:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3808:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_8BITCRC(struct __SPI_HandleTypeDef *hspi)
3809:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  *ptmpreg8;
3811:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
3812:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Initialize the 8bit temporary pointer */
3814:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
3815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Read 8bit CRC to flush Data Register */
3816:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmpreg8 = *ptmpreg8;
3817:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* To avoid GCC warning */
3818:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(tmpreg8);
3819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3820:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->CRCSize--;
3821:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3822:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->CRCSize == 0U)
3823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_CloseRx_ISR(hspi);
3825:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3826:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3829:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3830:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Manage the receive 8-bit in Interrupt context.
3831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3832:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_8BIT(struct __SPI_HandleTypeDef *hspi)
3836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *hspi->pRxBuffPtr = (*(__IO uint8_t *)&hspi->Instance->DR);
3838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr++;
3839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
3840:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3841:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3842:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable CRC Transmission */
3843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->RxXferCount == 1U) && (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE))
3844:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
3846:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3847:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->RxXferCount == 0U)
ARM GAS  /tmp/cc5SiBtg.s 			page 69


3850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3851:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3852:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3853:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->RxISR =  SPI_RxISR_8BITCRC;
3855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3856:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3857:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3858:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_CloseRx_ISR(hspi);
3859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3862:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3863:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3864:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Manage the CRC 16-bit receive in Interrupt context.
3865:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3867:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3868:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_16BITCRC(struct __SPI_HandleTypeDef *hspi)
3870:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t tmpreg = 0U;
3872:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3873:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Read 16bit CRC to flush Data Register */
3874:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmpreg = READ_REG(hspi->Instance->DR);
3875:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* To avoid GCC warning */
3876:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(tmpreg);
3877:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3878:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable RXNE and ERR interrupt */
3879:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_RXNE | SPI_IT_ERR));
3880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_CloseRx_ISR(hspi);
3882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3883:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3886:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Manage the 16-bit receive in Interrupt context.
3887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3888:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3890:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_16BIT(struct __SPI_HandleTypeDef *hspi)
3892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)(hspi->Instance->DR);
3894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
3895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
3896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3897:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable CRC Transmission */
3899:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->RxXferCount == 1U) && (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE))
3900:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
3902:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3904:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->RxXferCount == 0U)
3906:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 70


3907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->RxISR = SPI_RxISR_16BITCRC;
3911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3913:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_CloseRx_ISR(hspi);
3915:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3916:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3917:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3919:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the data 8-bit transmit in Interrupt mode.
3920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3921:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3924:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_TxISR_8BIT(struct __SPI_HandleTypeDef *hspi)
3925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *(__IO uint8_t *)&hspi->Instance->DR = (*hspi->pTxBuffPtr);
3927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr++;
3928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
3929:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->TxXferCount == 0U)
3931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3935:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Enable CRC Transmission */
3936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
3937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3938:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3939:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_CloseTx_ISR(hspi);
3940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the data 16-bit transmit in Interrupt mode.
3945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3948:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3949:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_TxISR_16BIT(struct __SPI_HandleTypeDef *hspi)
3950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
3952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
3953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
3954:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
3955:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3956:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->TxXferCount == 0U)
3957:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3960:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Enable CRC Transmission */
3962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
3963:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
ARM GAS  /tmp/cc5SiBtg.s 			page 71


3964:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3965:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_CloseTx_ISR(hspi);
3966:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3967:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3968:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3970:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle SPI Communication Timeout.
3971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3972:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *              the configuration information for SPI module.
3973:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Flag SPI flag to check
3974:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  State flag state to check
3975:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
3976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Tickstart tick start value
3977:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
3978:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_WaitFlagStateUntilTimeout(SPI_HandleTypeDef *hspi, uint32_t Flag, Flag
3980:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                        uint32_t Timeout, uint32_t Tickstart)
3981:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
  29              		.loc 1 3981 1 view -0
  30              		.cfi_startproc
  31              		@ args = 4, pretend = 0, frame = 8
  32              		@ frame_needed = 0, uses_anonymous_args = 0
  33              		.loc 1 3981 1 is_stmt 0 view .LVU1
  34 0000 2DE9F047 		push	{r4, r5, r6, r7, r8, r9, r10, lr}
  35              		.cfi_def_cfa_offset 32
  36              		.cfi_offset 4, -32
  37              		.cfi_offset 5, -28
  38              		.cfi_offset 6, -24
  39              		.cfi_offset 7, -20
  40              		.cfi_offset 8, -16
  41              		.cfi_offset 9, -12
  42              		.cfi_offset 10, -8
  43              		.cfi_offset 14, -4
  44 0004 82B0     		sub	sp, sp, #8
  45              		.cfi_def_cfa_offset 40
  46 0006 0546     		mov	r5, r0
  47 0008 8846     		mov	r8, r1
  48 000a 1746     		mov	r7, r2
  49 000c 1E46     		mov	r6, r3
3982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
  50              		.loc 1 3982 3 is_stmt 1 view .LVU2
3983:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tmp_timeout;
  51              		.loc 1 3983 3 view .LVU3
3984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tmp_tickstart;
  52              		.loc 1 3984 3 view .LVU4
3985:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3986:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Adjust Timeout value  in case of end of transfer */
3987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_timeout   = Timeout - (HAL_GetTick() - Tickstart);
  53              		.loc 1 3987 3 view .LVU5
  54              		.loc 1 3987 30 is_stmt 0 view .LVU6
  55 000e FFF7FEFF 		bl	HAL_GetTick
  56              	.LVL1:
  57              		.loc 1 3987 44 discriminator 1 view .LVU7
  58 0012 0A9B     		ldr	r3, [sp, #40]
  59 0014 1B1A     		subs	r3, r3, r0
  60              		.loc 1 3987 17 discriminator 1 view .LVU8
  61 0016 03EB0609 		add	r9, r3, r6
ARM GAS  /tmp/cc5SiBtg.s 			page 72


  62              	.LVL2:
3988:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_tickstart = HAL_GetTick();
  63              		.loc 1 3988 3 is_stmt 1 view .LVU9
  64              		.loc 1 3988 19 is_stmt 0 view .LVU10
  65 001a FFF7FEFF 		bl	HAL_GetTick
  66              	.LVL3:
  67 001e 8246     		mov	r10, r0
  68              	.LVL4:
3989:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Calculate Timeout based on a software loop to avoid blocking issue if Systick is disabled */
3991:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = tmp_timeout * ((SystemCoreClock * 32U) >> 20U);
  69              		.loc 1 3991 3 is_stmt 1 view .LVU11
  70              		.loc 1 3991 43 is_stmt 0 view .LVU12
  71 0020 284B     		ldr	r3, .L16
  72 0022 1B68     		ldr	r3, [r3]
  73              		.loc 1 3991 50 view .LVU13
  74 0024 C3F3CB33 		ubfx	r3, r3, #15, #12
  75              		.loc 1 3991 23 view .LVU14
  76 0028 09FB03F3 		mul	r3, r9, r3
  77              		.loc 1 3991 9 view .LVU15
  78 002c 0193     		str	r3, [sp, #4]
3992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   while ((__HAL_SPI_GET_FLAG(hspi, Flag) ? SET : RESET) != State)
  79              		.loc 1 3993 3 is_stmt 1 view .LVU16
  80              	.LVL5:
  81              	.L3:
  82              		.loc 1 3993 57 view .LVU17
  83              		.loc 1 3993 11 is_stmt 0 view .LVU18
  84 002e 2B68     		ldr	r3, [r5]
  85 0030 9C68     		ldr	r4, [r3, #8]
  86              		.loc 1 3993 48 view .LVU19
  87 0032 38EA0404 		bics	r4, r8, r4
  88 0036 0CBF     		ite	eq
  89 0038 0123     		moveq	r3, #1
  90 003a 0023     		movne	r3, #0
  91              		.loc 1 3993 57 view .LVU20
  92 003c BB42     		cmp	r3, r7
  93 003e 3DD0     		beq	.L12
3994:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3995:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (Timeout != HAL_MAX_DELAY)
  94              		.loc 1 3995 5 is_stmt 1 view .LVU21
  95              		.loc 1 3995 8 is_stmt 0 view .LVU22
  96 0040 B6F1FF3F 		cmp	r6, #-1
  97 0044 F3D0     		beq	.L3
3996:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3997:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (((HAL_GetTick() - tmp_tickstart) >= tmp_timeout) || (tmp_timeout == 0U))
  98              		.loc 1 3997 7 is_stmt 1 view .LVU23
  99              		.loc 1 3997 13 is_stmt 0 view .LVU24
 100 0046 FFF7FEFF 		bl	HAL_GetTick
 101              	.LVL6:
 102              		.loc 1 3997 27 discriminator 1 view .LVU25
 103 004a A0EB0A00 		sub	r0, r0, r10
 104              		.loc 1 3997 10 discriminator 1 view .LVU26
 105 004e 4845     		cmp	r0, r9
 106 0050 07D2     		bcs	.L13
3998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Disable the SPI and reset the CRC: the CRC value should be cleared
ARM GAS  /tmp/cc5SiBtg.s 			page 73


4000:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****            on both master and slave sides in order to resynchronize the master
4001:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****            and slave for their respective CRC calculation */
4002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4003:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Disable TXE, RXNE and ERR interrupts for the interrupt process */
4004:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_TXE | SPI_IT_RXNE | SPI_IT_ERR));
4005:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((hspi->Init.Mode == SPI_MODE_MASTER) && ((hspi->Init.Direction == SPI_DIRECTION_1LINE)
4007:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
4008:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
4009:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Disable SPI peripheral */
4010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           __HAL_SPI_DISABLE(hspi);
4011:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
4012:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4013:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Reset CRC Calculation */
4014:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
4015:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
4016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SPI_RESET_CRC(hspi);
4017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
4018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
4020:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Process Unlocked */
4022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_UNLOCK(hspi);
4023:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return HAL_TIMEOUT;
4025:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
4026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* If Systick is disabled or not incremented, deactivate timeout to go in disable loop proced
4027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (count == 0U)
 107              		.loc 1 4027 7 is_stmt 1 view .LVU27
 108              		.loc 1 4027 17 is_stmt 0 view .LVU28
 109 0052 019A     		ldr	r2, [sp, #4]
 110              		.loc 1 4027 10 view .LVU29
 111 0054 02B1     		cbz	r2, .L9
 112 0056 4A46     		mov	r2, r9
 113              	.L9:
 114              	.LVL7:
4028:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
4029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmp_timeout = 0U;
4030:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
4031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
 115              		.loc 1 4031 7 is_stmt 1 view .LVU30
 116              		.loc 1 4031 12 is_stmt 0 view .LVU31
 117 0058 019B     		ldr	r3, [sp, #4]
 118 005a 013B     		subs	r3, r3, #1
 119 005c 0193     		str	r3, [sp, #4]
 120 005e 9146     		mov	r9, r2
 121 0060 E5E7     		b	.L3
 122              	.LVL8:
 123              	.L13:
4004:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 124              		.loc 1 4004 9 is_stmt 1 view .LVU32
 125 0062 2A68     		ldr	r2, [r5]
 126 0064 5368     		ldr	r3, [r2, #4]
 127 0066 23F0E003 		bic	r3, r3, #224
 128 006a 5360     		str	r3, [r2, #4]
4006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 129              		.loc 1 4006 9 view .LVU33
ARM GAS  /tmp/cc5SiBtg.s 			page 74


4006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 130              		.loc 1 4006 24 is_stmt 0 view .LVU34
 131 006c 6B68     		ldr	r3, [r5, #4]
4006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 132              		.loc 1 4006 12 view .LVU35
 133 006e B3F5827F 		cmp	r3, #260
 134 0072 0BD0     		beq	.L14
 135              	.L5:
4014:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 136              		.loc 1 4014 9 is_stmt 1 view .LVU36
4014:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 137              		.loc 1 4014 23 is_stmt 0 view .LVU37
 138 0074 AB6A     		ldr	r3, [r5, #40]
4014:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 139              		.loc 1 4014 12 view .LVU38
 140 0076 B3F5005F 		cmp	r3, #8192
 141 007a 14D0     		beq	.L15
 142              	.L7:
4016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 143              		.loc 1 4016 11 is_stmt 1 discriminator 1 view .LVU39
4019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 144              		.loc 1 4019 9 view .LVU40
4019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 145              		.loc 1 4019 21 is_stmt 0 view .LVU41
 146 007c 0123     		movs	r3, #1
 147 007e 85F85D30 		strb	r3, [r5, #93]
4022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 148              		.loc 1 4022 9 is_stmt 1 view .LVU42
4022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 149              		.loc 1 4022 9 view .LVU43
 150 0082 0023     		movs	r3, #0
 151 0084 85F85C30 		strb	r3, [r5, #92]
4022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 152              		.loc 1 4022 9 view .LVU44
4024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 153              		.loc 1 4024 9 view .LVU45
4024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 154              		.loc 1 4024 16 is_stmt 0 view .LVU46
 155 0088 0320     		movs	r0, #3
 156 008a 18E0     		b	.L8
 157              	.L14:
4006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 158              		.loc 1 4006 65 discriminator 1 view .LVU47
 159 008c AB68     		ldr	r3, [r5, #8]
4006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 160              		.loc 1 4006 50 discriminator 1 view .LVU48
 161 008e B3F5004F 		cmp	r3, #32768
 162 0092 02D0     		beq	.L6
4007:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 163              		.loc 1 4007 54 view .LVU49
 164 0094 B3F5806F 		cmp	r3, #1024
 165 0098 ECD1     		bne	.L5
 166              	.L6:
4010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 167              		.loc 1 4010 11 is_stmt 1 view .LVU50
 168 009a 2A68     		ldr	r2, [r5]
 169 009c 1368     		ldr	r3, [r2]
ARM GAS  /tmp/cc5SiBtg.s 			page 75


 170 009e 23F04003 		bic	r3, r3, #64
 171 00a2 1360     		str	r3, [r2]
 172 00a4 E6E7     		b	.L5
 173              	.L15:
4016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 174              		.loc 1 4016 11 view .LVU51
4016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 175              		.loc 1 4016 11 view .LVU52
 176 00a6 2A68     		ldr	r2, [r5]
 177 00a8 1368     		ldr	r3, [r2]
 178 00aa 23F40053 		bic	r3, r3, #8192
 179 00ae 1360     		str	r3, [r2]
4016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 180              		.loc 1 4016 11 view .LVU53
 181 00b0 2A68     		ldr	r2, [r5]
 182 00b2 1368     		ldr	r3, [r2]
 183 00b4 43F40053 		orr	r3, r3, #8192
 184 00b8 1360     		str	r3, [r2]
 185 00ba DFE7     		b	.L7
 186              	.L12:
4032:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4034:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
 187              		.loc 1 4035 10 is_stmt 0 view .LVU54
 188 00bc 0020     		movs	r0, #0
 189              	.L8:
4036:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 190              		.loc 1 4036 1 view .LVU55
 191 00be 02B0     		add	sp, sp, #8
 192              		.cfi_def_cfa_offset 32
 193              		@ sp needed
 194 00c0 BDE8F087 		pop	{r4, r5, r6, r7, r8, r9, r10, pc}
 195              	.LVL9:
 196              	.L17:
 197              		.loc 1 4036 1 view .LVU56
 198              		.align	2
 199              	.L16:
 200 00c4 00000000 		.word	SystemCoreClock
 201              		.cfi_endproc
 202              	.LFE170:
 204              		.section	.text.SPI_WaitFifoStateUntilTimeout,"ax",%progbits
 205              		.align	1
 206              		.syntax unified
 207              		.thumb
 208              		.thumb_func
 210              	SPI_WaitFifoStateUntilTimeout:
 211              	.LVL10:
 212              	.LFB171:
4037:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4039:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle SPI FIFO Communication Timeout.
4040:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4041:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *              the configuration information for SPI module.
4042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Fifo Fifo to check
4043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  State Fifo state to check
4044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
ARM GAS  /tmp/cc5SiBtg.s 			page 76


4045:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Tickstart tick start value
4046:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
4047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_WaitFifoStateUntilTimeout(SPI_HandleTypeDef *hspi, uint32_t Fifo, uint
4049:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                        uint32_t Timeout, uint32_t Tickstart)
4050:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 213              		.loc 1 4050 1 is_stmt 1 view -0
 214              		.cfi_startproc
 215              		@ args = 4, pretend = 0, frame = 8
 216              		@ frame_needed = 0, uses_anonymous_args = 0
 217              		.loc 1 4050 1 is_stmt 0 view .LVU58
 218 0000 2DE9F047 		push	{r4, r5, r6, r7, r8, r9, r10, lr}
 219              		.cfi_def_cfa_offset 32
 220              		.cfi_offset 4, -32
 221              		.cfi_offset 5, -28
 222              		.cfi_offset 6, -24
 223              		.cfi_offset 7, -20
 224              		.cfi_offset 8, -16
 225              		.cfi_offset 9, -12
 226              		.cfi_offset 10, -8
 227              		.cfi_offset 14, -4
 228 0004 82B0     		sub	sp, sp, #8
 229              		.cfi_def_cfa_offset 40
 230 0006 0646     		mov	r6, r0
 231 0008 0C46     		mov	r4, r1
 232 000a 1546     		mov	r5, r2
 233 000c 1F46     		mov	r7, r3
4051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
 234              		.loc 1 4051 3 is_stmt 1 view .LVU59
4052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tmp_timeout;
 235              		.loc 1 4052 3 view .LVU60
4053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tmp_tickstart;
 236              		.loc 1 4053 3 view .LVU61
4054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  *ptmpreg8;
 237              		.loc 1 4054 3 view .LVU62
4055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
 238              		.loc 1 4055 3 view .LVU63
 239              		.loc 1 4055 17 is_stmt 0 view .LVU64
 240 000e 0023     		movs	r3, #0
 241              	.LVL11:
 242              		.loc 1 4055 17 view .LVU65
 243 0010 8DF80330 		strb	r3, [sp, #3]
4056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Adjust Timeout value  in case of end of transfer */
4058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_timeout = Timeout - (HAL_GetTick() - Tickstart);
 244              		.loc 1 4058 3 is_stmt 1 view .LVU66
 245              		.loc 1 4058 28 is_stmt 0 view .LVU67
 246 0014 FFF7FEFF 		bl	HAL_GetTick
 247              	.LVL12:
 248              		.loc 1 4058 42 discriminator 1 view .LVU68
 249 0018 0A9B     		ldr	r3, [sp, #40]
 250 001a 1B1A     		subs	r3, r3, r0
 251              		.loc 1 4058 15 discriminator 1 view .LVU69
 252 001c 03EB0708 		add	r8, r3, r7
 253              	.LVL13:
4059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_tickstart = HAL_GetTick();
 254              		.loc 1 4059 3 is_stmt 1 view .LVU70
ARM GAS  /tmp/cc5SiBtg.s 			page 77


 255              		.loc 1 4059 19 is_stmt 0 view .LVU71
 256 0020 FFF7FEFF 		bl	HAL_GetTick
 257              	.LVL14:
 258 0024 8146     		mov	r9, r0
 259              	.LVL15:
4060:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4061:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Initialize the 8bit temporary pointer */
4062:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
 260              		.loc 1 4062 3 is_stmt 1 view .LVU72
 261              		.loc 1 4062 35 is_stmt 0 view .LVU73
 262 0026 D6F800A0 		ldr	r10, [r6]
 263              	.LVL16:
4063:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4064:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Calculate Timeout based on a software loop to avoid blocking issue if Systick is disabled */
4065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = tmp_timeout * ((SystemCoreClock * 35U) >> 20U);
 264              		.loc 1 4065 3 is_stmt 1 view .LVU74
 265              		.loc 1 4065 43 is_stmt 0 view .LVU75
 266 002a 304B     		ldr	r3, .L35
 267 002c 1B68     		ldr	r3, [r3]
 268 002e 03EB8303 		add	r3, r3, r3, lsl #2
 269 0032 C3EBC303 		rsb	r3, r3, r3, lsl #3
 270              		.loc 1 4065 50 view .LVU76
 271 0036 1B0D     		lsrs	r3, r3, #20
 272              		.loc 1 4065 23 view .LVU77
 273 0038 08FB03F3 		mul	r3, r8, r3
 274              		.loc 1 4065 9 view .LVU78
 275 003c 0193     		str	r3, [sp, #4]
4066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   while ((hspi->Instance->SR & Fifo) != State)
 276              		.loc 1 4067 3 is_stmt 1 view .LVU79
 277              		.loc 1 4067 9 is_stmt 0 view .LVU80
 278 003e 02E0     		b	.L21
 279              	.LVL17:
 280              	.L20:
4068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((Fifo == SPI_SR_FRLVL) && (State == SPI_FRLVL_EMPTY))
4070:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Flush Data Register by a blank read */
4072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       tmpreg8 = *ptmpreg8;
4073:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
4074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       UNUSED(tmpreg8);
4075:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4076:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4077:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (Timeout != HAL_MAX_DELAY)
 281              		.loc 1 4077 5 is_stmt 1 view .LVU81
 282              		.loc 1 4077 8 is_stmt 0 view .LVU82
 283 0040 B7F1FF3F 		cmp	r7, #-1
 284 0044 12D1     		bne	.L30
 285              	.L21:
4067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 286              		.loc 1 4067 38 is_stmt 1 view .LVU83
4067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 287              		.loc 1 4067 15 is_stmt 0 view .LVU84
 288 0046 3368     		ldr	r3, [r6]
4067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 289              		.loc 1 4067 25 view .LVU85
 290 0048 9B68     		ldr	r3, [r3, #8]
ARM GAS  /tmp/cc5SiBtg.s 			page 78


4067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 291              		.loc 1 4067 30 view .LVU86
 292 004a 03EA040C 		and	ip, r3, r4
4067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 293              		.loc 1 4067 38 view .LVU87
 294 004e AC45     		cmp	ip, r5
 295 0050 47D0     		beq	.L31
4069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 296              		.loc 1 4069 5 is_stmt 1 view .LVU88
4069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 297              		.loc 1 4069 8 is_stmt 0 view .LVU89
 298 0052 B4F5C06F 		cmp	r4, #1536
 299 0056 F3D1     		bne	.L20
4069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 300              		.loc 1 4069 32 discriminator 1 view .LVU90
 301 0058 002D     		cmp	r5, #0
 302 005a F1D1     		bne	.L20
4072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
 303              		.loc 1 4072 7 is_stmt 1 view .LVU91
4072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
 304              		.loc 1 4072 17 is_stmt 0 view .LVU92
 305 005c 9AF80C30 		ldrb	r3, [r10, #12]	@ zero_extendqisi2
 306 0060 DBB2     		uxtb	r3, r3
4072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
 307              		.loc 1 4072 15 view .LVU93
 308 0062 8DF80330 		strb	r3, [sp, #3]
4074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 309              		.loc 1 4074 7 is_stmt 1 view .LVU94
 310 0066 9DF80330 		ldrb	r3, [sp, #3]	@ zero_extendqisi2
 311 006a E9E7     		b	.L20
 312              	.L30:
4078:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (((HAL_GetTick() - tmp_tickstart) >= tmp_timeout) || (tmp_timeout == 0U))
 313              		.loc 1 4079 7 view .LVU95
 314              		.loc 1 4079 13 is_stmt 0 view .LVU96
 315 006c FFF7FEFF 		bl	HAL_GetTick
 316              	.LVL18:
 317              		.loc 1 4079 27 discriminator 1 view .LVU97
 318 0070 A0EB0900 		sub	r0, r0, r9
 319              		.loc 1 4079 10 discriminator 1 view .LVU98
 320 0074 4045     		cmp	r0, r8
 321 0076 07D2     		bcs	.L32
4080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
4081:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Disable the SPI and reset the CRC: the CRC value should be cleared
4082:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****            on both master and slave sides in order to resynchronize the master
4083:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****            and slave for their respective CRC calculation */
4084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Disable TXE, RXNE and ERR interrupts for the interrupt process */
4086:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_TXE | SPI_IT_RXNE | SPI_IT_ERR));
4087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((hspi->Init.Mode == SPI_MODE_MASTER) && ((hspi->Init.Direction == SPI_DIRECTION_1LINE)
4089:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
4090:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
4091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Disable SPI peripheral */
4092:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           __HAL_SPI_DISABLE(hspi);
4093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
4094:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 79


4095:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Reset CRC Calculation */
4096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
4097:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
4098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SPI_RESET_CRC(hspi);
4099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
4100:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
4102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Process Unlocked */
4104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_UNLOCK(hspi);
4105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return HAL_TIMEOUT;
4107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
4108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* If Systick is disabled or not incremented, deactivate timeout to go in disable loop proced
4109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (count == 0U)
 322              		.loc 1 4109 7 is_stmt 1 view .LVU99
 323              		.loc 1 4109 17 is_stmt 0 view .LVU100
 324 0078 019A     		ldr	r2, [sp, #4]
 325              		.loc 1 4109 10 view .LVU101
 326 007a 02B1     		cbz	r2, .L27
 327 007c 4246     		mov	r2, r8
 328              	.L27:
 329              	.LVL19:
4110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
4111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmp_timeout = 0U;
4112:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
4113:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
 330              		.loc 1 4113 7 is_stmt 1 view .LVU102
 331              		.loc 1 4113 12 is_stmt 0 view .LVU103
 332 007e 019B     		ldr	r3, [sp, #4]
 333 0080 013B     		subs	r3, r3, #1
 334 0082 0193     		str	r3, [sp, #4]
 335 0084 9046     		mov	r8, r2
 336 0086 DEE7     		b	.L21
 337              	.LVL20:
 338              	.L32:
4086:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 339              		.loc 1 4086 9 is_stmt 1 view .LVU104
 340 0088 3268     		ldr	r2, [r6]
 341 008a 5368     		ldr	r3, [r2, #4]
 342 008c 23F0E003 		bic	r3, r3, #224
 343 0090 5360     		str	r3, [r2, #4]
4088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 344              		.loc 1 4088 9 view .LVU105
4088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 345              		.loc 1 4088 24 is_stmt 0 view .LVU106
 346 0092 7368     		ldr	r3, [r6, #4]
4088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 347              		.loc 1 4088 12 view .LVU107
 348 0094 B3F5827F 		cmp	r3, #260
 349 0098 0BD0     		beq	.L33
 350              	.L23:
4096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 351              		.loc 1 4096 9 is_stmt 1 view .LVU108
4096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 352              		.loc 1 4096 23 is_stmt 0 view .LVU109
 353 009a B36A     		ldr	r3, [r6, #40]
ARM GAS  /tmp/cc5SiBtg.s 			page 80


4096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 354              		.loc 1 4096 12 view .LVU110
 355 009c B3F5005F 		cmp	r3, #8192
 356 00a0 14D0     		beq	.L34
 357              	.L25:
4098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 358              		.loc 1 4098 11 is_stmt 1 discriminator 1 view .LVU111
4101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 359              		.loc 1 4101 9 view .LVU112
4101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 360              		.loc 1 4101 21 is_stmt 0 view .LVU113
 361 00a2 0123     		movs	r3, #1
 362 00a4 86F85D30 		strb	r3, [r6, #93]
4104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 363              		.loc 1 4104 9 is_stmt 1 view .LVU114
4104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 364              		.loc 1 4104 9 view .LVU115
 365 00a8 0023     		movs	r3, #0
 366 00aa 86F85C30 		strb	r3, [r6, #92]
4104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 367              		.loc 1 4104 9 view .LVU116
4106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 368              		.loc 1 4106 9 view .LVU117
4106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 369              		.loc 1 4106 16 is_stmt 0 view .LVU118
 370 00ae 0320     		movs	r0, #3
 371 00b0 18E0     		b	.L26
 372              	.L33:
4088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 373              		.loc 1 4088 65 discriminator 1 view .LVU119
 374 00b2 B368     		ldr	r3, [r6, #8]
4088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 375              		.loc 1 4088 50 discriminator 1 view .LVU120
 376 00b4 B3F5004F 		cmp	r3, #32768
 377 00b8 02D0     		beq	.L24
4089:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 378              		.loc 1 4089 54 view .LVU121
 379 00ba B3F5806F 		cmp	r3, #1024
 380 00be ECD1     		bne	.L23
 381              	.L24:
4092:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 382              		.loc 1 4092 11 is_stmt 1 view .LVU122
 383 00c0 3268     		ldr	r2, [r6]
 384 00c2 1368     		ldr	r3, [r2]
 385 00c4 23F04003 		bic	r3, r3, #64
 386 00c8 1360     		str	r3, [r2]
 387 00ca E6E7     		b	.L23
 388              	.L34:
4098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 389              		.loc 1 4098 11 view .LVU123
4098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 390              		.loc 1 4098 11 view .LVU124
 391 00cc 3268     		ldr	r2, [r6]
 392 00ce 1368     		ldr	r3, [r2]
 393 00d0 23F40053 		bic	r3, r3, #8192
 394 00d4 1360     		str	r3, [r2]
4098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
ARM GAS  /tmp/cc5SiBtg.s 			page 81


 395              		.loc 1 4098 11 view .LVU125
 396 00d6 3268     		ldr	r2, [r6]
 397 00d8 1368     		ldr	r3, [r2]
 398 00da 43F40053 		orr	r3, r3, #8192
 399 00de 1360     		str	r3, [r2]
 400 00e0 DFE7     		b	.L25
 401              	.L31:
4114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4115:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
 402              		.loc 1 4117 10 is_stmt 0 view .LVU126
 403 00e2 0020     		movs	r0, #0
 404              	.L26:
4118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 405              		.loc 1 4118 1 view .LVU127
 406 00e4 02B0     		add	sp, sp, #8
 407              		.cfi_def_cfa_offset 32
 408              		@ sp needed
 409 00e6 BDE8F087 		pop	{r4, r5, r6, r7, r8, r9, r10, pc}
 410              	.LVL21:
 411              	.L36:
 412              		.loc 1 4118 1 view .LVU128
 413 00ea 00BF     		.align	2
 414              	.L35:
 415 00ec 00000000 		.word	SystemCoreClock
 416              		.cfi_endproc
 417              	.LFE171:
 419              		.section	.text.SPI_EndRxTxTransaction,"ax",%progbits
 420              		.align	1
 421              		.syntax unified
 422              		.thumb
 423              		.thumb_func
 425              	SPI_EndRxTxTransaction:
 426              	.LVL22:
 427              	.LFB173:
4119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4120:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4121:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the check of the RX transaction complete.
4122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
4124:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
4125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Tickstart tick start value
4126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
4127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_EndRxTransaction(SPI_HandleTypeDef *hspi,  uint32_t Timeout, uint32_t 
4129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
4130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Mode == SPI_MODE_MASTER) && ((hspi->Init.Direction == SPI_DIRECTION_1LINE)
4131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
4132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI peripheral */
4134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
4135:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4137:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Control the BSY flag */
4138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_BSY, RESET, Timeout, Tickstart) != HAL_OK)
4139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 82


4140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
4142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4143:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Mode == SPI_MODE_MASTER) && ((hspi->Init.Direction == SPI_DIRECTION_1LINE)
4145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
4146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4147:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Empty the FRLVL fifo */
4148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, Timeout, Tickstart) !=
4149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4150:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4151:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return HAL_TIMEOUT;
4152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4154:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
4155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
4156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4157:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the check of the RXTX or TX transaction complete.
4159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi SPI handle
4160:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
4161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Tickstart tick start value
4162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
4163:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4164:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_EndRxTxTransaction(SPI_HandleTypeDef *hspi, uint32_t Timeout, uint32_t
4165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 428              		.loc 1 4165 1 is_stmt 1 view -0
 429              		.cfi_startproc
 430              		@ args = 0, pretend = 0, frame = 0
 431              		@ frame_needed = 0, uses_anonymous_args = 0
 432              		.loc 1 4165 1 is_stmt 0 view .LVU130
 433 0000 70B5     		push	{r4, r5, r6, lr}
 434              		.cfi_def_cfa_offset 16
 435              		.cfi_offset 4, -16
 436              		.cfi_offset 5, -12
 437              		.cfi_offset 6, -8
 438              		.cfi_offset 14, -4
 439 0002 82B0     		sub	sp, sp, #8
 440              		.cfi_def_cfa_offset 24
 441 0004 0446     		mov	r4, r0
 442 0006 0D46     		mov	r5, r1
 443 0008 1646     		mov	r6, r2
4166:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Control if the TX fifo is empty */
4167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FTLVL, SPI_FTLVL_EMPTY, Timeout, Tickstart) != H
 444              		.loc 1 4167 3 is_stmt 1 view .LVU131
 445              		.loc 1 4167 7 is_stmt 0 view .LVU132
 446 000a 0092     		str	r2, [sp]
 447 000c 0B46     		mov	r3, r1
 448 000e 0022     		movs	r2, #0
 449              	.LVL23:
 450              		.loc 1 4167 7 view .LVU133
 451 0010 4FF4C051 		mov	r1, #6144
 452              	.LVL24:
 453              		.loc 1 4167 7 view .LVU134
 454 0014 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 455              	.LVL25:
 456              		.loc 1 4167 6 discriminator 1 view .LVU135
ARM GAS  /tmp/cc5SiBtg.s 			page 83


 457 0018 B0B9     		cbnz	r0, .L42
4168:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4169:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
4171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4173:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Control the BSY flag */
4174:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_BSY, RESET, Timeout, Tickstart) != HAL_OK)
 458              		.loc 1 4174 3 is_stmt 1 view .LVU136
 459              		.loc 1 4174 7 is_stmt 0 view .LVU137
 460 001a 0096     		str	r6, [sp]
 461 001c 2B46     		mov	r3, r5
 462 001e 0022     		movs	r2, #0
 463 0020 8021     		movs	r1, #128
 464 0022 2046     		mov	r0, r4
 465 0024 FFF7FEFF 		bl	SPI_WaitFlagStateUntilTimeout
 466              	.LVL26:
 467              		.loc 1 4174 6 discriminator 1 view .LVU138
 468 0028 A8B9     		cbnz	r0, .L43
4175:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4176:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4177:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
4178:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4179:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4180:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Control if the RX fifo is empty */
4181:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, Timeout, Tickstart) != H
 469              		.loc 1 4181 3 is_stmt 1 view .LVU139
 470              		.loc 1 4181 7 is_stmt 0 view .LVU140
 471 002a 0096     		str	r6, [sp]
 472 002c 2B46     		mov	r3, r5
 473 002e 0022     		movs	r2, #0
 474 0030 4FF4C061 		mov	r1, #1536
 475 0034 2046     		mov	r0, r4
 476 0036 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 477              	.LVL27:
 478              		.loc 1 4181 6 discriminator 1 view .LVU141
 479 003a 50B1     		cbz	r0, .L39
4182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4183:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
 480              		.loc 1 4183 5 is_stmt 1 view .LVU142
 481 003c 236E     		ldr	r3, [r4, #96]
 482 003e 43F02003 		orr	r3, r3, #32
 483 0042 2366     		str	r3, [r4, #96]
4184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
 484              		.loc 1 4184 5 view .LVU143
 485              		.loc 1 4184 12 is_stmt 0 view .LVU144
 486 0044 0320     		movs	r0, #3
 487 0046 04E0     		b	.L39
 488              	.L42:
4169:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
 489              		.loc 1 4169 5 is_stmt 1 view .LVU145
 490 0048 236E     		ldr	r3, [r4, #96]
 491 004a 43F02003 		orr	r3, r3, #32
 492 004e 2366     		str	r3, [r4, #96]
4170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 493              		.loc 1 4170 5 view .LVU146
4170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
ARM GAS  /tmp/cc5SiBtg.s 			page 84


 494              		.loc 1 4170 12 is_stmt 0 view .LVU147
 495 0050 0320     		movs	r0, #3
 496              	.L39:
4185:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
4188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 497              		.loc 1 4188 1 view .LVU148
 498 0052 02B0     		add	sp, sp, #8
 499              		.cfi_remember_state
 500              		.cfi_def_cfa_offset 16
 501              		@ sp needed
 502 0054 70BD     		pop	{r4, r5, r6, pc}
 503              	.LVL28:
 504              	.L43:
 505              		.cfi_restore_state
4176:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
 506              		.loc 1 4176 5 is_stmt 1 view .LVU149
 507 0056 236E     		ldr	r3, [r4, #96]
 508 0058 43F02003 		orr	r3, r3, #32
 509 005c 2366     		str	r3, [r4, #96]
4177:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 510              		.loc 1 4177 5 view .LVU150
4177:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 511              		.loc 1 4177 12 is_stmt 0 view .LVU151
 512 005e 0320     		movs	r0, #3
 513 0060 F7E7     		b	.L39
 514              		.cfi_endproc
 515              	.LFE173:
 517              		.section	.text.SPI_EndRxTransaction,"ax",%progbits
 518              		.align	1
 519              		.syntax unified
 520              		.thumb
 521              		.thumb_func
 523              	SPI_EndRxTransaction:
 524              	.LVL29:
 525              	.LFB172:
4129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Mode == SPI_MODE_MASTER) && ((hspi->Init.Direction == SPI_DIRECTION_1LINE)
 526              		.loc 1 4129 1 is_stmt 1 view -0
 527              		.cfi_startproc
 528              		@ args = 0, pretend = 0, frame = 0
 529              		@ frame_needed = 0, uses_anonymous_args = 0
4129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Mode == SPI_MODE_MASTER) && ((hspi->Init.Direction == SPI_DIRECTION_1LINE)
 530              		.loc 1 4129 1 is_stmt 0 view .LVU153
 531 0000 70B5     		push	{r4, r5, r6, lr}
 532              		.cfi_def_cfa_offset 16
 533              		.cfi_offset 4, -16
 534              		.cfi_offset 5, -12
 535              		.cfi_offset 6, -8
 536              		.cfi_offset 14, -4
 537 0002 82B0     		sub	sp, sp, #8
 538              		.cfi_def_cfa_offset 24
 539 0004 0446     		mov	r4, r0
 540 0006 0D46     		mov	r5, r1
 541 0008 1646     		mov	r6, r2
4130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 542              		.loc 1 4130 3 is_stmt 1 view .LVU154
ARM GAS  /tmp/cc5SiBtg.s 			page 85


4130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 543              		.loc 1 4130 18 is_stmt 0 view .LVU155
 544 000a 4368     		ldr	r3, [r0, #4]
4130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 545              		.loc 1 4130 6 view .LVU156
 546 000c B3F5827F 		cmp	r3, #260
 547 0010 0DD0     		beq	.L51
 548              	.LVL30:
 549              	.L45:
4138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 550              		.loc 1 4138 3 is_stmt 1 view .LVU157
4138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 551              		.loc 1 4138 7 is_stmt 0 view .LVU158
 552 0012 0096     		str	r6, [sp]
 553 0014 2B46     		mov	r3, r5
 554 0016 0022     		movs	r2, #0
 555 0018 8021     		movs	r1, #128
 556              	.LVL31:
4138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 557              		.loc 1 4138 7 view .LVU159
 558 001a 2046     		mov	r0, r4
 559              	.LVL32:
4138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 560              		.loc 1 4138 7 view .LVU160
 561 001c FFF7FEFF 		bl	SPI_WaitFlagStateUntilTimeout
 562              	.LVL33:
4138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 563              		.loc 1 4138 6 discriminator 1 view .LVU161
 564 0020 90B9     		cbnz	r0, .L52
4144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 565              		.loc 1 4144 3 is_stmt 1 view .LVU162
4144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 566              		.loc 1 4144 18 is_stmt 0 view .LVU163
 567 0022 6368     		ldr	r3, [r4, #4]
4144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 568              		.loc 1 4144 6 view .LVU164
 569 0024 B3F5827F 		cmp	r3, #260
 570 0028 14D0     		beq	.L53
 571              	.L48:
4155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 572              		.loc 1 4155 1 view .LVU165
 573 002a 02B0     		add	sp, sp, #8
 574              		.cfi_remember_state
 575              		.cfi_def_cfa_offset 16
 576              		@ sp needed
 577 002c 70BD     		pop	{r4, r5, r6, pc}
 578              	.LVL34:
 579              	.L51:
 580              		.cfi_restore_state
4130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 581              		.loc 1 4130 59 discriminator 1 view .LVU166
 582 002e 8368     		ldr	r3, [r0, #8]
4130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 583              		.loc 1 4130 44 discriminator 1 view .LVU167
 584 0030 B3F5004F 		cmp	r3, #32768
 585 0034 02D0     		beq	.L46
4131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 86


 586              		.loc 1 4131 48 view .LVU168
 587 0036 B3F5806F 		cmp	r3, #1024
 588 003a EAD1     		bne	.L45
 589              	.L46:
4134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 590              		.loc 1 4134 5 is_stmt 1 view .LVU169
 591 003c 2268     		ldr	r2, [r4]
 592              	.LVL35:
4134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 593              		.loc 1 4134 5 is_stmt 0 view .LVU170
 594 003e 1368     		ldr	r3, [r2]
 595 0040 23F04003 		bic	r3, r3, #64
 596 0044 1360     		str	r3, [r2]
 597 0046 E4E7     		b	.L45
 598              	.LVL36:
 599              	.L52:
4140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
 600              		.loc 1 4140 5 is_stmt 1 view .LVU171
 601 0048 236E     		ldr	r3, [r4, #96]
 602 004a 43F02003 		orr	r3, r3, #32
 603 004e 2366     		str	r3, [r4, #96]
4141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 604              		.loc 1 4141 5 view .LVU172
4141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 605              		.loc 1 4141 12 is_stmt 0 view .LVU173
 606 0050 0320     		movs	r0, #3
 607 0052 EAE7     		b	.L48
 608              	.L53:
4144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 609              		.loc 1 4144 59 discriminator 1 view .LVU174
 610 0054 A368     		ldr	r3, [r4, #8]
4144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 611              		.loc 1 4144 44 discriminator 1 view .LVU175
 612 0056 B3F5004F 		cmp	r3, #32768
 613 005a 02D0     		beq	.L49
4145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 614              		.loc 1 4145 48 view .LVU176
 615 005c B3F5806F 		cmp	r3, #1024
 616 0060 E3D1     		bne	.L48
 617              	.L49:
4148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 618              		.loc 1 4148 5 is_stmt 1 view .LVU177
4148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 619              		.loc 1 4148 9 is_stmt 0 view .LVU178
 620 0062 0096     		str	r6, [sp]
 621 0064 2B46     		mov	r3, r5
 622 0066 0022     		movs	r2, #0
 623 0068 4FF4C061 		mov	r1, #1536
 624 006c 2046     		mov	r0, r4
 625 006e FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 626              	.LVL37:
4148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 627              		.loc 1 4148 8 discriminator 1 view .LVU179
 628 0072 0028     		cmp	r0, #0
 629 0074 D9D0     		beq	.L48
4150:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return HAL_TIMEOUT;
 630              		.loc 1 4150 7 is_stmt 1 view .LVU180
ARM GAS  /tmp/cc5SiBtg.s 			page 87


 631 0076 236E     		ldr	r3, [r4, #96]
 632 0078 43F02003 		orr	r3, r3, #32
 633 007c 2366     		str	r3, [r4, #96]
4151:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 634              		.loc 1 4151 7 view .LVU181
4151:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 635              		.loc 1 4151 14 is_stmt 0 view .LVU182
 636 007e 0320     		movs	r0, #3
 637 0080 D3E7     		b	.L48
 638              		.cfi_endproc
 639              	.LFE172:
 641              		.section	.text.SPI_AbortRx_ISR,"ax",%progbits
 642              		.align	1
 643              		.syntax unified
 644              		.thumb
 645              		.thumb_func
 647              	SPI_AbortRx_ISR:
 648              	.LVL38:
 649              	.LFB177:
4189:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4190:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4191:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the end of the RXTX transaction.
4192:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4193:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
4194:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
4195:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4196:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_CloseRxTx_ISR(SPI_HandleTypeDef *hspi)
4197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
4198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
4199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management */
4201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
4202:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable ERR interrupt */
4204:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE_IT(hspi, SPI_IT_ERR);
4205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transaction */
4207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, tickstart) != HAL_OK)
4208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4211:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
4213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if CRC error occurred */
4214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_CRCERR) != RESET)
4215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4216:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
4217:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
4218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
4219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call user error callback */
4220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCallback(hspi);
4222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4223:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     HAL_SPI_ErrorCallback(hspi);
4224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4225:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
ARM GAS  /tmp/cc5SiBtg.s 			page 88


4227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4228:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
4229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode == HAL_SPI_ERROR_NONE)
4230:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->State == HAL_SPI_STATE_BUSY_RX)
4232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
4233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
4234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user Rx complete callback */
4235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxCpltCallback(hspi);
4237:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         HAL_SPI_RxCpltCallback(hspi);
4239:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4240:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
4241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
4242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
4243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
4244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user TxRx complete callback */
4245:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4246:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxRxCpltCallback(hspi);
4247:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4248:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         HAL_SPI_TxRxCpltCallback(hspi);
4249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4250:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
4251:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4252:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
4253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->State = HAL_SPI_STATE_READY;
4255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
4256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4257:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCallback(hspi);
4258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       HAL_SPI_ErrorCallback(hspi);
4260:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
4263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
4265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
4266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4267:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4268:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the end of the RX transaction.
4269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4270:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
4271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
4272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4273:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_CloseRx_ISR(SPI_HandleTypeDef *hspi)
4274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
4275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable RXNE and ERR interrupt */
4276:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_RXNE | SPI_IT_ERR));
4277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transaction */
4279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTransaction(hspi, SPI_DEFAULT_TIMEOUT, HAL_GetTick()) != HAL_OK)
4280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4281:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
ARM GAS  /tmp/cc5SiBtg.s 			page 89


4284:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4285:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
4286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if CRC error occurred */
4287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_CRCERR) != RESET)
4288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4289:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
4290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
4291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call user error callback */
4292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCallback(hspi);
4294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     HAL_SPI_ErrorCallback(hspi);
4296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
4299:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4300:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
4301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode == HAL_SPI_ERROR_NONE)
4302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4303:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user Rx complete callback */
4304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->RxCpltCallback(hspi);
4306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       HAL_SPI_RxCpltCallback(hspi);
4308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4310:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
4311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
4313:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCallback(hspi);
4315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       HAL_SPI_ErrorCallback(hspi);
4317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
4320:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
4322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
4323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the end of the TX transaction.
4326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
4328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
4329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4330:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_CloseTx_ISR(SPI_HandleTypeDef *hspi)
4331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
4332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
4333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
4335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
4336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable TXE and ERR interrupt */
4338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_TXE | SPI_IT_ERR));
4339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transaction */
ARM GAS  /tmp/cc5SiBtg.s 			page 90


4341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, tickstart) != HAL_OK)
4342:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4345:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear overrun flag in 2 Lines communication mode because received is not read */
4347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_2LINES)
4348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_OVRFLAG(hspi);
4350:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
4353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
4354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call user error callback */
4356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCallback(hspi);
4358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     HAL_SPI_ErrorCallback(hspi);
4360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
4363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4364:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call user Rx complete callback */
4365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxCpltCallback(hspi);
4367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     HAL_SPI_TxCpltCallback(hspi);
4369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
4372:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4374:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle abort a Rx transaction.
4375:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4376:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
4377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
4378:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4379:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_AbortRx_ISR(SPI_HandleTypeDef *hspi)
4380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 650              		.loc 1 4380 1 is_stmt 1 view -0
 651              		.cfi_startproc
 652              		@ args = 0, pretend = 0, frame = 8
 653              		@ frame_needed = 0, uses_anonymous_args = 0
 654              		.loc 1 4380 1 is_stmt 0 view .LVU184
 655 0000 10B5     		push	{r4, lr}
 656              		.cfi_def_cfa_offset 8
 657              		.cfi_offset 4, -8
 658              		.cfi_offset 14, -4
 659 0002 84B0     		sub	sp, sp, #16
 660              		.cfi_def_cfa_offset 24
 661 0004 0446     		mov	r4, r0
4381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
 662              		.loc 1 4381 3 is_stmt 1 view .LVU185
4382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable SPI Peripheral */
4384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
ARM GAS  /tmp/cc5SiBtg.s 			page 91


 663              		.loc 1 4384 3 view .LVU186
 664 0006 0268     		ldr	r2, [r0]
 665 0008 1368     		ldr	r3, [r2]
 666 000a 23F04003 		bic	r3, r3, #64
 667 000e 1360     		str	r3, [r2]
4385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 668              		.loc 1 4386 3 view .LVU187
 669              		.loc 1 4386 56 is_stmt 0 view .LVU188
 670 0010 1D4B     		ldr	r3, .L62
 671 0012 1B68     		ldr	r3, [r3]
 672 0014 1D4A     		ldr	r2, .L62+4
 673 0016 A2FB0323 		umull	r2, r3, r2, r3
 674 001a 5B0A     		lsrs	r3, r3, #9
 675              		.loc 1 4386 31 view .LVU189
 676 001c 6422     		movs	r2, #100
 677 001e 02FB03F3 		mul	r3, r2, r3
 678              		.loc 1 4386 9 view .LVU190
 679 0022 0393     		str	r3, [sp, #12]
4387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable RXNEIE interrupt */
4389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, (SPI_CR2_RXNEIE));
 680              		.loc 1 4389 3 is_stmt 1 view .LVU191
 681 0024 0268     		ldr	r2, [r0]
 682 0026 5368     		ldr	r3, [r2, #4]
 683 0028 23F04003 		bic	r3, r3, #64
 684 002c 5360     		str	r3, [r2, #4]
 685              	.L57:
4390:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4391:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check RXNEIE is disabled */
4392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   do
 686              		.loc 1 4392 3 view .LVU192
4393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4394:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (count == 0U)
 687              		.loc 1 4394 5 view .LVU193
 688              		.loc 1 4394 15 is_stmt 0 view .LVU194
 689 002e 039B     		ldr	r3, [sp, #12]
 690              		.loc 1 4394 8 view .LVU195
 691 0030 43B1     		cbz	r3, .L61
4395:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
4397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       break;
4398:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     count--;
 692              		.loc 1 4399 5 is_stmt 1 view .LVU196
 693              		.loc 1 4399 10 is_stmt 0 view .LVU197
 694 0032 039B     		ldr	r3, [sp, #12]
 695 0034 013B     		subs	r3, r3, #1
 696 0036 0393     		str	r3, [sp, #12]
4400:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   } while (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXNEIE));
 697              		.loc 1 4400 12 is_stmt 1 view .LVU198
 698 0038 2368     		ldr	r3, [r4]
 699 003a 5B68     		ldr	r3, [r3, #4]
 700 003c 13F0400F 		tst	r3, #64
 701 0040 F5D1     		bne	.L57
 702 0042 03E0     		b	.L56
 703              	.L61:
ARM GAS  /tmp/cc5SiBtg.s 			page 92


4396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       break;
 704              		.loc 1 4396 7 view .LVU199
 705 0044 236E     		ldr	r3, [r4, #96]
 706 0046 43F04003 		orr	r3, r3, #64
 707 004a 2366     		str	r3, [r4, #96]
4397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 708              		.loc 1 4397 7 view .LVU200
 709              	.L56:
4401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4402:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Control the BSY flag */
4403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_BSY, RESET, SPI_DEFAULT_TIMEOUT, HAL_GetTick()) 
 710              		.loc 1 4403 3 view .LVU201
 711              		.loc 1 4403 7 is_stmt 0 view .LVU202
 712 004c FFF7FEFF 		bl	HAL_GetTick
 713              	.LVL39:
 714              		.loc 1 4403 7 discriminator 1 view .LVU203
 715 0050 0090     		str	r0, [sp]
 716 0052 6423     		movs	r3, #100
 717 0054 0022     		movs	r2, #0
 718 0056 8021     		movs	r1, #128
 719 0058 2046     		mov	r0, r4
 720 005a FFF7FEFF 		bl	SPI_WaitFlagStateUntilTimeout
 721              	.LVL40:
 722              		.loc 1 4403 6 discriminator 2 view .LVU204
 723 005e 08B1     		cbz	r0, .L58
4404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 724              		.loc 1 4405 5 is_stmt 1 view .LVU205
 725              		.loc 1 4405 21 is_stmt 0 view .LVU206
 726 0060 4023     		movs	r3, #64
 727 0062 2366     		str	r3, [r4, #96]
 728              	.L58:
4406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Empty the FRLVL fifo */
4409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT, HAL
 729              		.loc 1 4409 3 is_stmt 1 view .LVU207
 730              		.loc 1 4409 7 is_stmt 0 view .LVU208
 731 0064 FFF7FEFF 		bl	HAL_GetTick
 732              	.LVL41:
 733              		.loc 1 4409 7 discriminator 1 view .LVU209
 734 0068 0090     		str	r0, [sp]
 735 006a 6423     		movs	r3, #100
 736 006c 0022     		movs	r2, #0
 737 006e 4FF4C061 		mov	r1, #1536
 738 0072 2046     		mov	r0, r4
 739 0074 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 740              	.LVL42:
 741              		.loc 1 4409 6 discriminator 2 view .LVU210
 742 0078 08B1     		cbz	r0, .L59
4410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 743              		.loc 1 4411 5 is_stmt 1 view .LVU211
 744              		.loc 1 4411 21 is_stmt 0 view .LVU212
 745 007a 4023     		movs	r3, #64
 746 007c 2366     		str	r3, [r4, #96]
 747              	.L59:
ARM GAS  /tmp/cc5SiBtg.s 			page 93


4412:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_ABORT;
 748              		.loc 1 4414 3 is_stmt 1 view .LVU213
 749              		.loc 1 4414 15 is_stmt 0 view .LVU214
 750 007e 0723     		movs	r3, #7
 751 0080 84F85D30 		strb	r3, [r4, #93]
4415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 752              		.loc 1 4415 1 view .LVU215
 753 0084 04B0     		add	sp, sp, #16
 754              		.cfi_def_cfa_offset 8
 755              		@ sp needed
 756 0086 10BD     		pop	{r4, pc}
 757              	.LVL43:
 758              	.L63:
 759              		.loc 1 4415 1 view .LVU216
 760              		.align	2
 761              	.L62:
 762 0088 00000000 		.word	SystemCoreClock
 763 008c F1197605 		.word	91625969
 764              		.cfi_endproc
 765              	.LFE177:
 767              		.section	.text.SPI_AbortTx_ISR,"ax",%progbits
 768              		.align	1
 769              		.syntax unified
 770              		.thumb
 771              		.thumb_func
 773              	SPI_AbortTx_ISR:
 774              	.LVL44:
 775              	.LFB178:
4416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle abort a Tx or Rx/Tx transaction.
4419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4420:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
4421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
4422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_AbortTx_ISR(SPI_HandleTypeDef *hspi)
4424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 776              		.loc 1 4424 1 is_stmt 1 view -0
 777              		.cfi_startproc
 778              		@ args = 0, pretend = 0, frame = 8
 779              		@ frame_needed = 0, uses_anonymous_args = 0
 780              		.loc 1 4424 1 is_stmt 0 view .LVU218
 781 0000 10B5     		push	{r4, lr}
 782              		.cfi_def_cfa_offset 8
 783              		.cfi_offset 4, -8
 784              		.cfi_offset 14, -4
 785 0002 84B0     		sub	sp, sp, #16
 786              		.cfi_def_cfa_offset 24
 787 0004 0446     		mov	r4, r0
4425:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
 788              		.loc 1 4425 3 is_stmt 1 view .LVU219
4426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 789              		.loc 1 4427 3 view .LVU220
 790              		.loc 1 4427 56 is_stmt 0 view .LVU221
ARM GAS  /tmp/cc5SiBtg.s 			page 94


 791 0006 384B     		ldr	r3, .L78
 792 0008 1B68     		ldr	r3, [r3]
 793 000a 384A     		ldr	r2, .L78+4
 794 000c A2FB0323 		umull	r2, r3, r2, r3
 795 0010 5B0A     		lsrs	r3, r3, #9
 796              		.loc 1 4427 31 view .LVU222
 797 0012 6422     		movs	r2, #100
 798 0014 02FB03F3 		mul	r3, r2, r3
 799              		.loc 1 4427 9 view .LVU223
 800 0018 0393     		str	r3, [sp, #12]
4428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable TXEIE interrupt */
4430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, (SPI_CR2_TXEIE));
 801              		.loc 1 4430 3 is_stmt 1 view .LVU224
 802 001a 0268     		ldr	r2, [r0]
 803 001c 5368     		ldr	r3, [r2, #4]
 804 001e 23F08003 		bic	r3, r3, #128
 805 0022 5360     		str	r3, [r2, #4]
 806              	.L67:
4431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check TXEIE is disabled */
4433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   do
 807              		.loc 1 4433 3 view .LVU225
4434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4435:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (count == 0U)
 808              		.loc 1 4435 5 view .LVU226
 809              		.loc 1 4435 15 is_stmt 0 view .LVU227
 810 0024 039B     		ldr	r3, [sp, #12]
 811              		.loc 1 4435 8 view .LVU228
 812 0026 43B1     		cbz	r3, .L76
4436:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
4438:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       break;
4439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     count--;
 813              		.loc 1 4440 5 is_stmt 1 view .LVU229
 814              		.loc 1 4440 10 is_stmt 0 view .LVU230
 815 0028 039B     		ldr	r3, [sp, #12]
 816 002a 013B     		subs	r3, r3, #1
 817 002c 0393     		str	r3, [sp, #12]
4441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   } while (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_TXEIE));
 818              		.loc 1 4441 12 is_stmt 1 view .LVU231
 819 002e 2368     		ldr	r3, [r4]
 820 0030 5B68     		ldr	r3, [r3, #4]
 821 0032 13F0800F 		tst	r3, #128
 822 0036 F5D1     		bne	.L67
 823 0038 03E0     		b	.L66
 824              	.L76:
4437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       break;
 825              		.loc 1 4437 7 view .LVU232
 826 003a 236E     		ldr	r3, [r4, #96]
 827 003c 43F04003 		orr	r3, r3, #64
 828 0040 2366     		str	r3, [r4, #96]
4438:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 829              		.loc 1 4438 7 view .LVU233
 830              	.L66:
4442:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 95


4443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, HAL_GetTick()) != HAL_OK)
 831              		.loc 1 4443 3 view .LVU234
 832              		.loc 1 4443 7 is_stmt 0 view .LVU235
 833 0042 FFF7FEFF 		bl	HAL_GetTick
 834              	.LVL45:
 835              		.loc 1 4443 7 view .LVU236
 836 0046 0246     		mov	r2, r0
 837              		.loc 1 4443 7 discriminator 1 view .LVU237
 838 0048 6421     		movs	r1, #100
 839 004a 2046     		mov	r0, r4
 840 004c FFF7FEFF 		bl	SPI_EndRxTxTransaction
 841              	.LVL46:
 842              		.loc 1 4443 6 discriminator 2 view .LVU238
 843 0050 08B1     		cbz	r0, .L68
4444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4445:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 844              		.loc 1 4445 5 is_stmt 1 view .LVU239
 845              		.loc 1 4445 21 is_stmt 0 view .LVU240
 846 0052 4023     		movs	r3, #64
 847 0054 2366     		str	r3, [r4, #96]
 848              	.L68:
4446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4447:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4448:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable SPI Peripheral */
4449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
 849              		.loc 1 4449 3 is_stmt 1 view .LVU241
 850 0056 2268     		ldr	r2, [r4]
 851 0058 1368     		ldr	r3, [r2]
 852 005a 23F04003 		bic	r3, r3, #64
 853 005e 1360     		str	r3, [r2]
4450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Empty the FRLVL fifo */
4452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT, HAL
 854              		.loc 1 4452 3 view .LVU242
 855              		.loc 1 4452 7 is_stmt 0 view .LVU243
 856 0060 FFF7FEFF 		bl	HAL_GetTick
 857              	.LVL47:
 858              		.loc 1 4452 7 discriminator 1 view .LVU244
 859 0064 0090     		str	r0, [sp]
 860 0066 6423     		movs	r3, #100
 861 0068 0022     		movs	r2, #0
 862 006a 4FF4C061 		mov	r1, #1536
 863 006e 2046     		mov	r0, r4
 864 0070 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 865              	.LVL48:
 866              		.loc 1 4452 6 discriminator 2 view .LVU245
 867 0074 08B1     		cbz	r0, .L69
4453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 868              		.loc 1 4454 5 is_stmt 1 view .LVU246
 869              		.loc 1 4454 21 is_stmt 0 view .LVU247
 870 0076 4023     		movs	r3, #64
 871 0078 2366     		str	r3, [r4, #96]
 872              	.L69:
4455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4456:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check case of Full-Duplex Mode and disable directly RXNEIE interrupt */
ARM GAS  /tmp/cc5SiBtg.s 			page 96


4458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXNEIE))
 873              		.loc 1 4458 3 is_stmt 1 view .LVU248
 874              		.loc 1 4458 7 is_stmt 0 view .LVU249
 875 007a 2368     		ldr	r3, [r4]
 876 007c 5A68     		ldr	r2, [r3, #4]
 877              		.loc 1 4458 6 view .LVU250
 878 007e 12F0400F 		tst	r2, #64
 879 0082 2BD0     		beq	.L70
4459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable RXNEIE interrupt */
4461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, (SPI_CR2_RXNEIE));
 880              		.loc 1 4461 5 is_stmt 1 view .LVU251
 881 0084 5A68     		ldr	r2, [r3, #4]
 882 0086 22F04002 		bic	r2, r2, #64
 883 008a 5A60     		str	r2, [r3, #4]
 884              	.L73:
4462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check RXNEIE is disabled */
4464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     do
 885              		.loc 1 4464 5 view .LVU252
4465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (count == 0U)
 886              		.loc 1 4466 7 view .LVU253
 887              		.loc 1 4466 17 is_stmt 0 view .LVU254
 888 008c 039B     		ldr	r3, [sp, #12]
 889              		.loc 1 4466 10 view .LVU255
 890 008e 43B1     		cbz	r3, .L77
4467:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
4468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
4469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
4470:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
4471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
 891              		.loc 1 4471 7 is_stmt 1 view .LVU256
 892              		.loc 1 4471 12 is_stmt 0 view .LVU257
 893 0090 039B     		ldr	r3, [sp, #12]
 894 0092 013B     		subs	r3, r3, #1
 895 0094 0393     		str	r3, [sp, #12]
4472:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXNEIE));
 896              		.loc 1 4472 14 is_stmt 1 view .LVU258
 897 0096 2368     		ldr	r3, [r4]
 898 0098 5B68     		ldr	r3, [r3, #4]
 899 009a 13F0400F 		tst	r3, #64
 900 009e F5D1     		bne	.L73
 901 00a0 03E0     		b	.L72
 902              	.L77:
4468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 903              		.loc 1 4468 9 view .LVU259
 904 00a2 236E     		ldr	r3, [r4, #96]
 905 00a4 43F04003 		orr	r3, r3, #64
 906 00a8 2366     		str	r3, [r4, #96]
4469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 907              		.loc 1 4469 9 view .LVU260
 908              	.L72:
4473:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Control the BSY flag */
4475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_BSY, RESET, SPI_DEFAULT_TIMEOUT, HAL_GetTick()
 909              		.loc 1 4475 5 view .LVU261
ARM GAS  /tmp/cc5SiBtg.s 			page 97


 910              		.loc 1 4475 9 is_stmt 0 view .LVU262
 911 00aa FFF7FEFF 		bl	HAL_GetTick
 912              	.LVL49:
 913              		.loc 1 4475 9 discriminator 1 view .LVU263
 914 00ae 0090     		str	r0, [sp]
 915 00b0 6423     		movs	r3, #100
 916 00b2 0022     		movs	r2, #0
 917 00b4 8021     		movs	r1, #128
 918 00b6 2046     		mov	r0, r4
 919 00b8 FFF7FEFF 		bl	SPI_WaitFlagStateUntilTimeout
 920              	.LVL50:
 921              		.loc 1 4475 8 discriminator 2 view .LVU264
 922 00bc 08B1     		cbz	r0, .L74
4476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 923              		.loc 1 4477 7 is_stmt 1 view .LVU265
 924              		.loc 1 4477 23 is_stmt 0 view .LVU266
 925 00be 4023     		movs	r3, #64
 926 00c0 2366     		str	r3, [r4, #96]
 927              	.L74:
4478:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4480:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Empty the FRLVL fifo */
4481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT, H
 928              		.loc 1 4481 5 is_stmt 1 view .LVU267
 929              		.loc 1 4481 9 is_stmt 0 view .LVU268
 930 00c2 FFF7FEFF 		bl	HAL_GetTick
 931              	.LVL51:
 932              		.loc 1 4481 9 discriminator 1 view .LVU269
 933 00c6 0090     		str	r0, [sp]
 934 00c8 6423     		movs	r3, #100
 935 00ca 0022     		movs	r2, #0
 936 00cc 4FF4C061 		mov	r1, #1536
 937 00d0 2046     		mov	r0, r4
 938 00d2 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 939              	.LVL52:
 940              		.loc 1 4481 8 discriminator 2 view .LVU270
 941 00d6 08B1     		cbz	r0, .L70
4482:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4483:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 942              		.loc 1 4483 7 is_stmt 1 view .LVU271
 943              		.loc 1 4483 23 is_stmt 0 view .LVU272
 944 00d8 4023     		movs	r3, #64
 945 00da 2366     		str	r3, [r4, #96]
 946              	.L70:
4484:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4486:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_ABORT;
 947              		.loc 1 4486 3 is_stmt 1 view .LVU273
 948              		.loc 1 4486 15 is_stmt 0 view .LVU274
 949 00dc 0723     		movs	r3, #7
 950 00de 84F85D30 		strb	r3, [r4, #93]
4487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 951              		.loc 1 4487 1 view .LVU275
 952 00e2 04B0     		add	sp, sp, #16
 953              		.cfi_def_cfa_offset 8
 954              		@ sp needed
ARM GAS  /tmp/cc5SiBtg.s 			page 98


 955 00e4 10BD     		pop	{r4, pc}
 956              	.LVL53:
 957              	.L79:
 958              		.loc 1 4487 1 view .LVU276
 959 00e6 00BF     		.align	2
 960              	.L78:
 961 00e8 00000000 		.word	SystemCoreClock
 962 00ec F1197605 		.word	91625969
 963              		.cfi_endproc
 964              	.LFE178:
 966              		.section	.text.HAL_SPI_MspInit,"ax",%progbits
 967              		.align	1
 968              		.weak	HAL_SPI_MspInit
 969              		.syntax unified
 970              		.thumb
 971              		.thumb_func
 973              	HAL_SPI_MspInit:
 974              	.LVL54:
 975              	.LFB125:
 534:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 976              		.loc 1 534 1 is_stmt 1 view -0
 977              		.cfi_startproc
 978              		@ args = 0, pretend = 0, frame = 0
 979              		@ frame_needed = 0, uses_anonymous_args = 0
 980              		@ link register save eliminated.
 536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 981              		.loc 1 536 3 view .LVU278
 541:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 982              		.loc 1 541 1 is_stmt 0 view .LVU279
 983 0000 7047     		bx	lr
 984              		.cfi_endproc
 985              	.LFE125:
 987              		.section	.text.HAL_SPI_Init,"ax",%progbits
 988              		.align	1
 989              		.global	HAL_SPI_Init
 990              		.syntax unified
 991              		.thumb
 992              		.thumb_func
 994              	HAL_SPI_Init:
 995              	.LVL55:
 996              	.LFB123:
 315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t frxth;
 997              		.loc 1 315 1 is_stmt 1 view -0
 998              		.cfi_startproc
 999              		@ args = 0, pretend = 0, frame = 0
 1000              		@ frame_needed = 0, uses_anonymous_args = 0
 316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1001              		.loc 1 316 3 view .LVU281
 319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1002              		.loc 1 319 3 view .LVU282
 319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1003              		.loc 1 319 6 is_stmt 0 view .LVU283
 1004 0000 0028     		cmp	r0, #0
 1005 0002 6FD0     		beq	.L88
 315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t frxth;
 1006              		.loc 1 315 1 view .LVU284
 1007 0004 10B5     		push	{r4, lr}
ARM GAS  /tmp/cc5SiBtg.s 			page 99


 1008              		.cfi_def_cfa_offset 8
 1009              		.cfi_offset 4, -8
 1010              		.cfi_offset 14, -4
 1011 0006 0446     		mov	r4, r0
 325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_MODE(hspi->Init.Mode));
 1012              		.loc 1 325 3 is_stmt 1 view .LVU285
 326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION(hspi->Init.Direction));
 1013              		.loc 1 326 3 view .LVU286
 327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DATASIZE(hspi->Init.DataSize));
 1014              		.loc 1 327 3 view .LVU287
 328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_NSS(hspi->Init.NSS));
 1015              		.loc 1 328 3 view .LVU288
 329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_NSSP(hspi->Init.NSSPMode));
 1016              		.loc 1 329 3 view .LVU289
 330:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_BAUDRATE_PRESCALER(hspi->Init.BaudRatePrescaler));
 1017              		.loc 1 330 3 view .LVU290
 331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_FIRST_BIT(hspi->Init.FirstBit));
 1018              		.loc 1 331 3 view .LVU291
 332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_TIMODE(hspi->Init.TIMode));
 1019              		.loc 1 332 3 view .LVU292
 333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.TIMode == SPI_TIMODE_DISABLE)
 1020              		.loc 1 333 3 view .LVU293
 334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1021              		.loc 1 334 3 view .LVU294
 334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1022              		.loc 1 334 17 is_stmt 0 view .LVU295
 1023 0008 436A     		ldr	r3, [r0, #36]
 334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1024              		.loc 1 334 6 view .LVU296
 1025 000a 33B9     		cbnz	r3, .L83
 336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_CPHA(hspi->Init.CLKPhase));
 1026              		.loc 1 336 5 is_stmt 1 view .LVU297
 337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1027              		.loc 1 337 5 view .LVU298
 339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1028              		.loc 1 339 5 view .LVU299
 339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1029              		.loc 1 339 19 is_stmt 0 view .LVU300
 1030 000c 4368     		ldr	r3, [r0, #4]
 339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1031              		.loc 1 339 8 view .LVU301
 1032 000e B3F5827F 		cmp	r3, #260
 1033 0012 05D0     		beq	.L84
 346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1034              		.loc 1 346 7 is_stmt 1 view .LVU302
 346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1035              		.loc 1 346 36 is_stmt 0 view .LVU303
 1036 0014 0023     		movs	r3, #0
 1037 0016 C361     		str	r3, [r0, #28]
 1038 0018 02E0     		b	.L84
 1039              	.L83:
 351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1040              		.loc 1 351 5 is_stmt 1 view .LVU304
 354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Init.CLKPhase    = SPI_PHASE_1EDGE;
 1041              		.loc 1 354 5 view .LVU305
 354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Init.CLKPhase    = SPI_PHASE_1EDGE;
 1042              		.loc 1 354 28 is_stmt 0 view .LVU306
ARM GAS  /tmp/cc5SiBtg.s 			page 100


 1043 001a 0023     		movs	r3, #0
 1044 001c 0361     		str	r3, [r0, #16]
 355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1045              		.loc 1 355 5 is_stmt 1 view .LVU307
 355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1046              		.loc 1 355 28 is_stmt 0 view .LVU308
 1047 001e 4361     		str	r3, [r0, #20]
 1048              	.L84:
 365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 1049              		.loc 1 365 3 is_stmt 1 view .LVU309
 365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 1050              		.loc 1 365 29 is_stmt 0 view .LVU310
 1051 0020 0023     		movs	r3, #0
 1052 0022 A362     		str	r3, [r4, #40]
 368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1053              		.loc 1 368 3 is_stmt 1 view .LVU311
 368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1054              		.loc 1 368 11 is_stmt 0 view .LVU312
 1055 0024 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1056              		.loc 1 368 6 view .LVU313
 1057 0028 002B     		cmp	r3, #0
 1058 002a 52D0     		beq	.L94
 1059              	.LVL56:
 1060              	.L85:
 397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1061              		.loc 1 397 3 is_stmt 1 view .LVU314
 397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1062              		.loc 1 397 15 is_stmt 0 view .LVU315
 1063 002c 0223     		movs	r3, #2
 1064 002e 84F85D30 		strb	r3, [r4, #93]
 400:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1065              		.loc 1 400 3 is_stmt 1 view .LVU316
 1066 0032 2268     		ldr	r2, [r4]
 1067 0034 1368     		ldr	r3, [r2]
 1068 0036 23F04003 		bic	r3, r3, #64
 1069 003a 1360     		str	r3, [r2]
 403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1070              		.loc 1 403 3 view .LVU317
 403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1071              		.loc 1 403 17 is_stmt 0 view .LVU318
 1072 003c E368     		ldr	r3, [r4, #12]
 403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1073              		.loc 1 403 6 view .LVU319
 1074 003e B3F5E06F 		cmp	r3, #1792
 1075 0042 4CD9     		bls	.L89
 405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1076              		.loc 1 405 11 view .LVU320
 1077 0044 0022     		movs	r2, #0
 1078              	.L86:
 1079              	.LVL57:
 413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1080              		.loc 1 413 3 is_stmt 1 view .LVU321
 413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1081              		.loc 1 413 6 is_stmt 0 view .LVU322
 1082 0046 B3F5706F 		cmp	r3, #3840
 1083 004a 04D0     		beq	.L87
ARM GAS  /tmp/cc5SiBtg.s 			page 101


 413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1084              		.loc 1 413 51 discriminator 1 view .LVU323
 1085 004c B3F5E06F 		cmp	r3, #1792
 1086 0050 01D0     		beq	.L87
 416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1087              		.loc 1 416 5 is_stmt 1 view .LVU324
 416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1088              		.loc 1 416 31 is_stmt 0 view .LVU325
 1089 0052 0023     		movs	r3, #0
 1090 0054 A362     		str	r3, [r4, #40]
 1091              	.L87:
 422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.Direction & (SPI_CR1_RXONLY | SPI_CR1_BIDIMODE)) |
 1092              		.loc 1 422 3 is_stmt 1 view .LVU326
 1093 0056 6368     		ldr	r3, [r4, #4]
 1094 0058 03F48273 		and	r3, r3, #260
 1095 005c A168     		ldr	r1, [r4, #8]
 1096 005e 01F40441 		and	r1, r1, #33792
 1097 0062 0B43     		orrs	r3, r3, r1
 1098 0064 2169     		ldr	r1, [r4, #16]
 1099 0066 01F00201 		and	r1, r1, #2
 1100 006a 0B43     		orrs	r3, r3, r1
 1101 006c 6169     		ldr	r1, [r4, #20]
 1102 006e 01F00101 		and	r1, r1, #1
 1103 0072 0B43     		orrs	r3, r3, r1
 1104 0074 A169     		ldr	r1, [r4, #24]
 1105 0076 01F40071 		and	r1, r1, #512
 1106 007a 0B43     		orrs	r3, r3, r1
 1107 007c E169     		ldr	r1, [r4, #28]
 1108 007e 01F03801 		and	r1, r1, #56
 1109 0082 0B43     		orrs	r3, r3, r1
 1110 0084 216A     		ldr	r1, [r4, #32]
 1111 0086 01F08001 		and	r1, r1, #128
 1112 008a 0B43     		orrs	r3, r3, r1
 1113 008c A16A     		ldr	r1, [r4, #40]
 1114 008e 01F40051 		and	r1, r1, #8192
 1115 0092 2068     		ldr	r0, [r4]
 1116 0094 0B43     		orrs	r3, r3, r1
 1117 0096 0360     		str	r3, [r0]
 457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.TIMode & SPI_CR2_FRF) |
 1118              		.loc 1 457 3 view .LVU327
 1119 0098 638B     		ldrh	r3, [r4, #26]
 1120 009a 03F00403 		and	r3, r3, #4
 1121 009e 616A     		ldr	r1, [r4, #36]
 1122 00a0 01F01001 		and	r1, r1, #16
 1123 00a4 0B43     		orrs	r3, r3, r1
 1124 00a6 616B     		ldr	r1, [r4, #52]
 1125 00a8 01F00801 		and	r1, r1, #8
 1126 00ac 0B43     		orrs	r3, r3, r1
 1127 00ae E168     		ldr	r1, [r4, #12]
 1128 00b0 01F47061 		and	r1, r1, #3840
 1129 00b4 0B43     		orrs	r3, r3, r1
 1130 00b6 2168     		ldr	r1, [r4]
 1131 00b8 1343     		orrs	r3, r3, r2
 1132 00ba 4B60     		str	r3, [r1, #4]
 474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* SPI_I2SCFGR_I2SMOD */
 1133              		.loc 1 474 3 view .LVU328
 1134 00bc 2268     		ldr	r2, [r4]
ARM GAS  /tmp/cc5SiBtg.s 			page 102


 1135              	.LVL58:
 474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* SPI_I2SCFGR_I2SMOD */
 1136              		.loc 1 474 3 is_stmt 0 view .LVU329
 1137 00be D369     		ldr	r3, [r2, #28]
 1138 00c0 23F40063 		bic	r3, r3, #2048
 1139 00c4 D361     		str	r3, [r2, #28]
 477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State     = HAL_SPI_STATE_READY;
 1140              		.loc 1 477 3 is_stmt 1 view .LVU330
 477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State     = HAL_SPI_STATE_READY;
 1141              		.loc 1 477 19 is_stmt 0 view .LVU331
 1142 00c6 0020     		movs	r0, #0
 1143 00c8 2066     		str	r0, [r4, #96]
 478:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1144              		.loc 1 478 3 is_stmt 1 view .LVU332
 478:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1145              		.loc 1 478 19 is_stmt 0 view .LVU333
 1146 00ca 0123     		movs	r3, #1
 1147 00cc 84F85D30 		strb	r3, [r4, #93]
 480:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 1148              		.loc 1 480 3 is_stmt 1 view .LVU334
 481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1149              		.loc 1 481 1 is_stmt 0 view .LVU335
 1150 00d0 10BD     		pop	{r4, pc}
 1151              	.LVL59:
 1152              	.L94:
 371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1153              		.loc 1 371 5 is_stmt 1 view .LVU336
 371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1154              		.loc 1 371 16 is_stmt 0 view .LVU337
 1155 00d2 84F85C30 		strb	r3, [r4, #92]
 393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 1156              		.loc 1 393 5 is_stmt 1 view .LVU338
 1157 00d6 2046     		mov	r0, r4
 1158              	.LVL60:
 393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 1159              		.loc 1 393 5 is_stmt 0 view .LVU339
 1160 00d8 FFF7FEFF 		bl	HAL_SPI_MspInit
 1161              	.LVL61:
 1162 00dc A6E7     		b	.L85
 1163              	.L89:
 409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1164              		.loc 1 409 11 view .LVU340
 1165 00de 4FF48052 		mov	r2, #4096
 1166 00e2 B0E7     		b	.L86
 1167              	.LVL62:
 1168              	.L88:
 1169              		.cfi_def_cfa_offset 0
 1170              		.cfi_restore 4
 1171              		.cfi_restore 14
 321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1172              		.loc 1 321 12 view .LVU341
 1173 00e4 0120     		movs	r0, #1
 1174              	.LVL63:
 481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1175              		.loc 1 481 1 view .LVU342
 1176 00e6 7047     		bx	lr
 1177              		.cfi_endproc
ARM GAS  /tmp/cc5SiBtg.s 			page 103


 1178              	.LFE123:
 1180              		.section	.text.HAL_SPI_MspDeInit,"ax",%progbits
 1181              		.align	1
 1182              		.weak	HAL_SPI_MspDeInit
 1183              		.syntax unified
 1184              		.thumb
 1185              		.thumb_func
 1187              	HAL_SPI_MspDeInit:
 1188              	.LVL64:
 1189              	.LFB126:
 550:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 1190              		.loc 1 550 1 is_stmt 1 view -0
 1191              		.cfi_startproc
 1192              		@ args = 0, pretend = 0, frame = 0
 1193              		@ frame_needed = 0, uses_anonymous_args = 0
 1194              		@ link register save eliminated.
 552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1195              		.loc 1 552 3 view .LVU344
 557:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1196              		.loc 1 557 1 is_stmt 0 view .LVU345
 1197 0000 7047     		bx	lr
 1198              		.cfi_endproc
 1199              	.LFE126:
 1201              		.section	.text.HAL_SPI_DeInit,"ax",%progbits
 1202              		.align	1
 1203              		.global	HAL_SPI_DeInit
 1204              		.syntax unified
 1205              		.thumb
 1206              		.thumb_func
 1208              	HAL_SPI_DeInit:
 1209              	.LVL65:
 1210              	.LFB124:
 490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the SPI handle allocation */
 1211              		.loc 1 490 1 is_stmt 1 view -0
 1212              		.cfi_startproc
 1213              		@ args = 0, pretend = 0, frame = 0
 1214              		@ frame_needed = 0, uses_anonymous_args = 0
 492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1215              		.loc 1 492 3 view .LVU347
 492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1216              		.loc 1 492 6 is_stmt 0 view .LVU348
 1217 0000 90B1     		cbz	r0, .L98
 490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the SPI handle allocation */
 1218              		.loc 1 490 1 view .LVU349
 1219 0002 10B5     		push	{r4, lr}
 1220              		.cfi_def_cfa_offset 8
 1221              		.cfi_offset 4, -8
 1222              		.cfi_offset 14, -4
 1223 0004 0446     		mov	r4, r0
 498:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1224              		.loc 1 498 3 is_stmt 1 view .LVU350
 500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1225              		.loc 1 500 3 view .LVU351
 500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1226              		.loc 1 500 15 is_stmt 0 view .LVU352
 1227 0006 0223     		movs	r3, #2
 1228 0008 80F85D30 		strb	r3, [r0, #93]
ARM GAS  /tmp/cc5SiBtg.s 			page 104


 503:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1229              		.loc 1 503 3 is_stmt 1 view .LVU353
 1230 000c 0268     		ldr	r2, [r0]
 1231 000e 1368     		ldr	r3, [r2]
 1232 0010 23F04003 		bic	r3, r3, #64
 1233 0014 1360     		str	r3, [r2]
 515:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 1234              		.loc 1 515 3 view .LVU354
 1235 0016 FFF7FEFF 		bl	HAL_SPI_MspDeInit
 1236              	.LVL66:
 518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_RESET;
 1237              		.loc 1 518 3 view .LVU355
 518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_RESET;
 1238              		.loc 1 518 19 is_stmt 0 view .LVU356
 1239 001a 0020     		movs	r0, #0
 1240 001c 2066     		str	r0, [r4, #96]
 519:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1241              		.loc 1 519 3 is_stmt 1 view .LVU357
 519:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1242              		.loc 1 519 15 is_stmt 0 view .LVU358
 1243 001e 84F85D00 		strb	r0, [r4, #93]
 522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1244              		.loc 1 522 3 is_stmt 1 view .LVU359
 522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1245              		.loc 1 522 3 view .LVU360
 1246 0022 84F85C00 		strb	r0, [r4, #92]
 522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1247              		.loc 1 522 3 view .LVU361
 524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 1248              		.loc 1 524 3 view .LVU362
 525:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1249              		.loc 1 525 1 is_stmt 0 view .LVU363
 1250 0026 10BD     		pop	{r4, pc}
 1251              	.LVL67:
 1252              	.L98:
 1253              		.cfi_def_cfa_offset 0
 1254              		.cfi_restore 4
 1255              		.cfi_restore 14
 494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1256              		.loc 1 494 12 view .LVU364
 1257 0028 0120     		movs	r0, #1
 1258              	.LVL68:
 525:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1259              		.loc 1 525 1 view .LVU365
 1260 002a 7047     		bx	lr
 1261              		.cfi_endproc
 1262              	.LFE124:
 1264              		.section	.text.HAL_SPI_Transmit,"ax",%progbits
 1265              		.align	1
 1266              		.global	HAL_SPI_Transmit
 1267              		.syntax unified
 1268              		.thumb
 1269              		.thumb_func
 1271              	HAL_SPI_Transmit:
 1272              	.LVL69:
 1273              	.LFB127:
 822:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
ARM GAS  /tmp/cc5SiBtg.s 			page 105


 1274              		.loc 1 822 1 is_stmt 1 view -0
 1275              		.cfi_startproc
 1276              		@ args = 0, pretend = 0, frame = 8
 1277              		@ frame_needed = 0, uses_anonymous_args = 0
 822:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 1278              		.loc 1 822 1 is_stmt 0 view .LVU367
 1279 0000 2DE9F043 		push	{r4, r5, r6, r7, r8, r9, lr}
 1280              		.cfi_def_cfa_offset 28
 1281              		.cfi_offset 4, -28
 1282              		.cfi_offset 5, -24
 1283              		.cfi_offset 6, -20
 1284              		.cfi_offset 7, -16
 1285              		.cfi_offset 8, -12
 1286              		.cfi_offset 9, -8
 1287              		.cfi_offset 14, -4
 1288 0004 83B0     		sub	sp, sp, #12
 1289              		.cfi_def_cfa_offset 40
 1290 0006 1D46     		mov	r5, r3
 823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 1291              		.loc 1 823 3 is_stmt 1 view .LVU368
 824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t initial_TxXferCount;
 1292              		.loc 1 824 3 view .LVU369
 1293              	.LVL70:
 825:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1294              		.loc 1 825 3 view .LVU370
 828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1295              		.loc 1 828 3 view .LVU371
 831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1296              		.loc 1 831 3 view .LVU372
 831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1297              		.loc 1 831 3 view .LVU373
 1298 0008 90F85C30 		ldrb	r3, [r0, #92]	@ zero_extendqisi2
 1299              	.LVL71:
 831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1300              		.loc 1 831 3 is_stmt 0 view .LVU374
 1301 000c 012B     		cmp	r3, #1
 1302 000e 00F0F480 		beq	.L130
 1303 0012 0446     		mov	r4, r0
 1304 0014 8846     		mov	r8, r1
 1305 0016 9146     		mov	r9, r2
 831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1306              		.loc 1 831 3 is_stmt 1 discriminator 2 view .LVU375
 1307 0018 0123     		movs	r3, #1
 1308 001a 80F85C30 		strb	r3, [r0, #92]
 831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1309              		.loc 1 831 3 discriminator 2 view .LVU376
 834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
 1310              		.loc 1 834 3 view .LVU377
 834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
 1311              		.loc 1 834 15 is_stmt 0 view .LVU378
 1312 001e FFF7FEFF 		bl	HAL_GetTick
 1313              	.LVL72:
 834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
 1314              		.loc 1 834 15 view .LVU379
 1315 0022 0746     		mov	r7, r0
 1316              	.LVL73:
 835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 106


 1317              		.loc 1 835 3 is_stmt 1 view .LVU380
 837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1318              		.loc 1 837 3 view .LVU381
 837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1319              		.loc 1 837 11 is_stmt 0 view .LVU382
 1320 0024 94F85D60 		ldrb	r6, [r4, #93]	@ zero_extendqisi2
 1321 0028 F6B2     		uxtb	r6, r6
 837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1322              		.loc 1 837 6 view .LVU383
 1323 002a 012E     		cmp	r6, #1
 1324 002c 40F0DD80 		bne	.L131
 843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1325              		.loc 1 843 3 is_stmt 1 view .LVU384
 843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1326              		.loc 1 843 6 is_stmt 0 view .LVU385
 1327 0030 B8F1000F 		cmp	r8, #0
 1328 0034 00F0DA80 		beq	.L105
 843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1329              		.loc 1 843 23 discriminator 1 view .LVU386
 1330 0038 B9F1000F 		cmp	r9, #0
 1331 003c 00F0D680 		beq	.L105
 850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 1332              		.loc 1 850 3 is_stmt 1 view .LVU387
 850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 1333              		.loc 1 850 21 is_stmt 0 view .LVU388
 1334 0040 0323     		movs	r3, #3
 1335 0042 84F85D30 		strb	r3, [r4, #93]
 851:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 1336              		.loc 1 851 3 is_stmt 1 view .LVU389
 851:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 1337              		.loc 1 851 21 is_stmt 0 view .LVU390
 1338 0046 0023     		movs	r3, #0
 1339 0048 2366     		str	r3, [r4, #96]
 852:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 1340              		.loc 1 852 3 is_stmt 1 view .LVU391
 852:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 1341              		.loc 1 852 21 is_stmt 0 view .LVU392
 1342 004a C4F83880 		str	r8, [r4, #56]
 853:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 1343              		.loc 1 853 3 is_stmt 1 view .LVU393
 853:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 1344              		.loc 1 853 21 is_stmt 0 view .LVU394
 1345 004e A4F83C90 		strh	r9, [r4, #60]	@ movhi
 854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1346              		.loc 1 854 3 is_stmt 1 view .LVU395
 854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1347              		.loc 1 854 21 is_stmt 0 view .LVU396
 1348 0052 A4F83E90 		strh	r9, [r4, #62]	@ movhi
 857:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 1349              		.loc 1 857 3 is_stmt 1 view .LVU397
 857:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 1350              		.loc 1 857 21 is_stmt 0 view .LVU398
 1351 0056 2364     		str	r3, [r4, #64]
 858:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 1352              		.loc 1 858 3 is_stmt 1 view .LVU399
 858:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 1353              		.loc 1 858 21 is_stmt 0 view .LVU400
ARM GAS  /tmp/cc5SiBtg.s 			page 107


 1354 0058 A4F84430 		strh	r3, [r4, #68]	@ movhi
 859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 1355              		.loc 1 859 3 is_stmt 1 view .LVU401
 859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 1356              		.loc 1 859 21 is_stmt 0 view .LVU402
 1357 005c A4F84630 		strh	r3, [r4, #70]	@ movhi
 860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 1358              		.loc 1 860 3 is_stmt 1 view .LVU403
 860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 1359              		.loc 1 860 21 is_stmt 0 view .LVU404
 1360 0060 2365     		str	r3, [r4, #80]
 861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1361              		.loc 1 861 3 is_stmt 1 view .LVU405
 861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1362              		.loc 1 861 21 is_stmt 0 view .LVU406
 1363 0062 E364     		str	r3, [r4, #76]
 864:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1364              		.loc 1 864 3 is_stmt 1 view .LVU407
 864:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1365              		.loc 1 864 17 is_stmt 0 view .LVU408
 1366 0064 A368     		ldr	r3, [r4, #8]
 864:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1367              		.loc 1 864 6 view .LVU409
 1368 0066 B3F5004F 		cmp	r3, #32768
 1369 006a 1ED0     		beq	.L133
 1370              	.L106:
 880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1371              		.loc 1 880 3 is_stmt 1 view .LVU410
 880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1372              		.loc 1 880 12 is_stmt 0 view .LVU411
 1373 006c 2368     		ldr	r3, [r4]
 880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1374              		.loc 1 880 22 view .LVU412
 1375 006e 1A68     		ldr	r2, [r3]
 880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1376              		.loc 1 880 6 view .LVU413
 1377 0070 12F0400F 		tst	r2, #64
 1378 0074 03D1     		bne	.L107
 883:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1379              		.loc 1 883 5 is_stmt 1 view .LVU414
 1380 0076 1A68     		ldr	r2, [r3]
 1381 0078 42F04002 		orr	r2, r2, #64
 1382 007c 1A60     		str	r2, [r3]
 1383              	.L107:
 887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1384              		.loc 1 887 3 view .LVU415
 887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1385              		.loc 1 887 17 is_stmt 0 view .LVU416
 1386 007e E368     		ldr	r3, [r4, #12]
 887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1387              		.loc 1 887 6 view .LVU417
 1388 0080 B3F5E06F 		cmp	r3, #1792
 1389 0084 44D9     		bls	.L108
 889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1390              		.loc 1 889 5 is_stmt 1 view .LVU418
 889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1391              		.loc 1 889 20 is_stmt 0 view .LVU419
ARM GAS  /tmp/cc5SiBtg.s 			page 108


 1392 0086 6368     		ldr	r3, [r4, #4]
 889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1393              		.loc 1 889 8 view .LVU420
 1394 0088 13B1     		cbz	r3, .L109
 889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1395              		.loc 1 889 45 discriminator 1 view .LVU421
 1396 008a B9F1010F 		cmp	r9, #1
 1397 008e 20D1     		bne	.L111
 1398              	.L109:
 891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1399              		.loc 1 891 7 is_stmt 1 view .LVU422
 891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1400              		.loc 1 891 46 is_stmt 0 view .LVU423
 1401 0090 A26B     		ldr	r2, [r4, #56]
 891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1402              		.loc 1 891 11 view .LVU424
 1403 0092 2368     		ldr	r3, [r4]
 891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1404              		.loc 1 891 28 view .LVU425
 1405 0094 1288     		ldrh	r2, [r2]
 891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1406              		.loc 1 891 26 view .LVU426
 1407 0096 DA60     		str	r2, [r3, #12]
 892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 1408              		.loc 1 892 7 is_stmt 1 view .LVU427
 892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 1409              		.loc 1 892 11 is_stmt 0 view .LVU428
 1410 0098 A36B     		ldr	r3, [r4, #56]
 892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 1411              		.loc 1 892 24 view .LVU429
 1412 009a 0233     		adds	r3, r3, #2
 1413 009c A363     		str	r3, [r4, #56]
 893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1414              		.loc 1 893 7 is_stmt 1 view .LVU430
 893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1415              		.loc 1 893 11 is_stmt 0 view .LVU431
 1416 009e E38F     		ldrh	r3, [r4, #62]
 1417 00a0 9BB2     		uxth	r3, r3
 893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1418              		.loc 1 893 24 view .LVU432
 1419 00a2 013B     		subs	r3, r3, #1
 1420 00a4 9BB2     		uxth	r3, r3
 1421 00a6 E387     		strh	r3, [r4, #62]	@ movhi
 1422 00a8 13E0     		b	.L111
 1423              	.L133:
 867:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 1424              		.loc 1 867 5 is_stmt 1 view .LVU433
 1425 00aa 2268     		ldr	r2, [r4]
 1426 00ac 1368     		ldr	r3, [r2]
 1427 00ae 23F04003 		bic	r3, r3, #64
 1428 00b2 1360     		str	r3, [r2]
 868:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1429              		.loc 1 868 5 view .LVU434
 1430 00b4 2268     		ldr	r2, [r4]
 1431 00b6 1368     		ldr	r3, [r2]
 1432 00b8 43F48043 		orr	r3, r3, #16384
 1433 00bc 1360     		str	r3, [r2]
ARM GAS  /tmp/cc5SiBtg.s 			page 109


 1434 00be D5E7     		b	.L106
 1435              	.LVL74:
 1436              	.L112:
 908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1437              		.loc 1 908 9 view .LVU435
 908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1438              		.loc 1 908 16 is_stmt 0 view .LVU436
 1439 00c0 FFF7FEFF 		bl	HAL_GetTick
 1440              	.LVL75:
 908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1441              		.loc 1 908 30 discriminator 1 view .LVU437
 1442 00c4 C01B     		subs	r0, r0, r7
 908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1443              		.loc 1 908 12 discriminator 1 view .LVU438
 1444 00c6 A842     		cmp	r0, r5
 1445 00c8 02D3     		bcc	.L114
 908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1446              		.loc 1 908 56 discriminator 1 view .LVU439
 1447 00ca B5F1FF3F 		cmp	r5, #-1
 1448 00ce 1AD1     		bne	.L115
 1449              	.L114:
 908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1450              		.loc 1 908 87 discriminator 3 view .LVU440
 1451 00d0 CDB1     		cbz	r5, .L115
 1452              	.L111:
 896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1453              		.loc 1 896 30 is_stmt 1 view .LVU441
 896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1454              		.loc 1 896 16 is_stmt 0 view .LVU442
 1455 00d2 E38F     		ldrh	r3, [r4, #62]
 1456 00d4 9BB2     		uxth	r3, r3
 896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1457              		.loc 1 896 30 view .LVU443
 1458 00d6 002B     		cmp	r3, #0
 1459 00d8 6FD0     		beq	.L117
 899:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1460              		.loc 1 899 7 is_stmt 1 view .LVU444
 899:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1461              		.loc 1 899 11 is_stmt 0 view .LVU445
 1462 00da 2368     		ldr	r3, [r4]
 1463 00dc 9A68     		ldr	r2, [r3, #8]
 899:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1464              		.loc 1 899 10 view .LVU446
 1465 00de 12F0020F 		tst	r2, #2
 1466 00e2 EDD0     		beq	.L112
 901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1467              		.loc 1 901 9 is_stmt 1 view .LVU447
 901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1468              		.loc 1 901 48 is_stmt 0 view .LVU448
 1469 00e4 A26B     		ldr	r2, [r4, #56]
 901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1470              		.loc 1 901 30 view .LVU449
 1471 00e6 1288     		ldrh	r2, [r2]
 901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1472              		.loc 1 901 28 view .LVU450
 1473 00e8 DA60     		str	r2, [r3, #12]
 902:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
ARM GAS  /tmp/cc5SiBtg.s 			page 110


 1474              		.loc 1 902 9 is_stmt 1 view .LVU451
 902:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1475              		.loc 1 902 13 is_stmt 0 view .LVU452
 1476 00ea A36B     		ldr	r3, [r4, #56]
 902:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1477              		.loc 1 902 26 view .LVU453
 1478 00ec 0233     		adds	r3, r3, #2
 1479 00ee A363     		str	r3, [r4, #56]
 903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1480              		.loc 1 903 9 is_stmt 1 view .LVU454
 903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1481              		.loc 1 903 13 is_stmt 0 view .LVU455
 1482 00f0 B4F83EC0 		ldrh	ip, [r4, #62]
 1483 00f4 1FFA8CFC 		uxth	ip, ip
 903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1484              		.loc 1 903 26 view .LVU456
 1485 00f8 0CF1FF3C 		add	ip, ip, #-1
 1486 00fc 1FFA8CFC 		uxth	ip, ip
 1487 0100 A4F83EC0 		strh	ip, [r4, #62]	@ movhi
 1488 0104 E5E7     		b	.L111
 1489              	.L115:
 910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 1490              		.loc 1 910 11 is_stmt 1 view .LVU457
 1491              	.LVL76:
 911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 1492              		.loc 1 911 11 view .LVU458
 911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 1493              		.loc 1 911 23 is_stmt 0 view .LVU459
 1494 0106 0123     		movs	r3, #1
 1495 0108 84F85D30 		strb	r3, [r4, #93]
 912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1496              		.loc 1 912 11 is_stmt 1 view .LVU460
 910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 1497              		.loc 1 910 21 is_stmt 0 view .LVU461
 1498 010c 0326     		movs	r6, #3
 912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1499              		.loc 1 912 11 view .LVU462
 1500 010e 6DE0     		b	.L105
 1501              	.LVL77:
 1502              	.L108:
 920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1503              		.loc 1 920 5 is_stmt 1 view .LVU463
 920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1504              		.loc 1 920 20 is_stmt 0 view .LVU464
 1505 0110 6368     		ldr	r3, [r4, #4]
 920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1506              		.loc 1 920 8 view .LVU465
 1507 0112 13B1     		cbz	r3, .L118
 920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1508              		.loc 1 920 45 discriminator 1 view .LVU466
 1509 0114 B9F1010F 		cmp	r9, #1
 1510 0118 32D1     		bne	.L121
 1511              	.L118:
 922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1512              		.loc 1 922 7 is_stmt 1 view .LVU467
 922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1513              		.loc 1 922 15 is_stmt 0 view .LVU468
ARM GAS  /tmp/cc5SiBtg.s 			page 111


 1514 011a E38F     		ldrh	r3, [r4, #62]
 1515 011c 9BB2     		uxth	r3, r3
 922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1516              		.loc 1 922 10 view .LVU469
 1517 011e 012B     		cmp	r3, #1
 1518 0120 0CD9     		bls	.L120
 925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1519              		.loc 1 925 9 is_stmt 1 view .LVU470
 925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1520              		.loc 1 925 48 is_stmt 0 view .LVU471
 1521 0122 A26B     		ldr	r2, [r4, #56]
 925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1522              		.loc 1 925 13 view .LVU472
 1523 0124 2368     		ldr	r3, [r4]
 925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1524              		.loc 1 925 30 view .LVU473
 1525 0126 1288     		ldrh	r2, [r2]
 925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1526              		.loc 1 925 28 view .LVU474
 1527 0128 DA60     		str	r2, [r3, #12]
 926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 1528              		.loc 1 926 9 is_stmt 1 view .LVU475
 926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 1529              		.loc 1 926 13 is_stmt 0 view .LVU476
 1530 012a A36B     		ldr	r3, [r4, #56]
 926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 1531              		.loc 1 926 26 view .LVU477
 1532 012c 0233     		adds	r3, r3, #2
 1533 012e A363     		str	r3, [r4, #56]
 927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1534              		.loc 1 927 9 is_stmt 1 view .LVU478
 927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1535              		.loc 1 927 13 is_stmt 0 view .LVU479
 1536 0130 E38F     		ldrh	r3, [r4, #62]
 1537 0132 9BB2     		uxth	r3, r3
 927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1538              		.loc 1 927 27 view .LVU480
 1539 0134 023B     		subs	r3, r3, #2
 1540 0136 9BB2     		uxth	r3, r3
 1541 0138 E387     		strh	r3, [r4, #62]	@ movhi
 1542 013a 21E0     		b	.L121
 1543              	.L120:
 931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr ++;
 1544              		.loc 1 931 9 is_stmt 1 view .LVU481
 931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr ++;
 1545              		.loc 1 931 56 is_stmt 0 view .LVU482
 1546 013c A26B     		ldr	r2, [r4, #56]
 931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr ++;
 1547              		.loc 1 931 32 view .LVU483
 1548 013e 2368     		ldr	r3, [r4]
 931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr ++;
 1549              		.loc 1 931 51 view .LVU484
 1550 0140 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
 931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr ++;
 1551              		.loc 1 931 48 view .LVU485
 1552 0142 1A73     		strb	r2, [r3, #12]
 932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
ARM GAS  /tmp/cc5SiBtg.s 			page 112


 1553              		.loc 1 932 9 is_stmt 1 view .LVU486
 932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1554              		.loc 1 932 13 is_stmt 0 view .LVU487
 1555 0144 A36B     		ldr	r3, [r4, #56]
 932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1556              		.loc 1 932 26 view .LVU488
 1557 0146 0133     		adds	r3, r3, #1
 1558 0148 A363     		str	r3, [r4, #56]
 933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1559              		.loc 1 933 9 is_stmt 1 view .LVU489
 933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1560              		.loc 1 933 13 is_stmt 0 view .LVU490
 1561 014a E38F     		ldrh	r3, [r4, #62]
 1562 014c 9BB2     		uxth	r3, r3
 933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1563              		.loc 1 933 26 view .LVU491
 1564 014e 013B     		subs	r3, r3, #1
 1565 0150 9BB2     		uxth	r3, r3
 1566 0152 E387     		strh	r3, [r4, #62]	@ movhi
 1567 0154 14E0     		b	.L121
 1568              	.LVL78:
 1569              	.L123:
 950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 1570              		.loc 1 950 11 is_stmt 1 view .LVU492
 950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 1571              		.loc 1 950 58 is_stmt 0 view .LVU493
 1572 0156 A36B     		ldr	r3, [r4, #56]
 950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 1573              		.loc 1 950 53 view .LVU494
 1574 0158 1B78     		ldrb	r3, [r3]	@ zero_extendqisi2
 950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 1575              		.loc 1 950 50 view .LVU495
 1576 015a 1373     		strb	r3, [r2, #12]
 951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 1577              		.loc 1 951 11 is_stmt 1 view .LVU496
 951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 1578              		.loc 1 951 15 is_stmt 0 view .LVU497
 1579 015c A36B     		ldr	r3, [r4, #56]
 951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 1580              		.loc 1 951 27 view .LVU498
 1581 015e 0133     		adds	r3, r3, #1
 1582 0160 A363     		str	r3, [r4, #56]
 952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1583              		.loc 1 952 11 is_stmt 1 view .LVU499
 952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1584              		.loc 1 952 15 is_stmt 0 view .LVU500
 1585 0162 E38F     		ldrh	r3, [r4, #62]
 1586 0164 9BB2     		uxth	r3, r3
 952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1587              		.loc 1 952 28 view .LVU501
 1588 0166 013B     		subs	r3, r3, #1
 1589 0168 9BB2     		uxth	r3, r3
 1590 016a E387     		strh	r3, [r4, #62]	@ movhi
 1591 016c 08E0     		b	.L121
 1592              	.L122:
 958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1593              		.loc 1 958 9 is_stmt 1 view .LVU502
ARM GAS  /tmp/cc5SiBtg.s 			page 113


 958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1594              		.loc 1 958 16 is_stmt 0 view .LVU503
 1595 016e FFF7FEFF 		bl	HAL_GetTick
 1596              	.LVL79:
 958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1597              		.loc 1 958 30 discriminator 1 view .LVU504
 1598 0172 C01B     		subs	r0, r0, r7
 958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1599              		.loc 1 958 12 discriminator 1 view .LVU505
 1600 0174 A842     		cmp	r0, r5
 1601 0176 02D3     		bcc	.L125
 958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1602              		.loc 1 958 56 discriminator 1 view .LVU506
 1603 0178 B5F1FF3F 		cmp	r5, #-1
 1604 017c 18D1     		bne	.L126
 1605              	.L125:
 958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1606              		.loc 1 958 87 discriminator 3 view .LVU507
 1607 017e BDB1     		cbz	r5, .L126
 1608              	.L121:
 936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1609              		.loc 1 936 30 is_stmt 1 view .LVU508
 936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1610              		.loc 1 936 16 is_stmt 0 view .LVU509
 1611 0180 E38F     		ldrh	r3, [r4, #62]
 1612 0182 9BB2     		uxth	r3, r3
 936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1613              		.loc 1 936 30 view .LVU510
 1614 0184 CBB1     		cbz	r3, .L117
 939:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1615              		.loc 1 939 7 is_stmt 1 view .LVU511
 939:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1616              		.loc 1 939 11 is_stmt 0 view .LVU512
 1617 0186 2268     		ldr	r2, [r4]
 1618 0188 9368     		ldr	r3, [r2, #8]
 939:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1619              		.loc 1 939 10 view .LVU513
 1620 018a 13F0020F 		tst	r3, #2
 1621 018e EED0     		beq	.L122
 941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1622              		.loc 1 941 9 is_stmt 1 view .LVU514
 941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1623              		.loc 1 941 17 is_stmt 0 view .LVU515
 1624 0190 E38F     		ldrh	r3, [r4, #62]
 1625 0192 9BB2     		uxth	r3, r3
 941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1626              		.loc 1 941 12 view .LVU516
 1627 0194 012B     		cmp	r3, #1
 1628 0196 DED9     		bls	.L123
 944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 1629              		.loc 1 944 11 is_stmt 1 view .LVU517
 944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 1630              		.loc 1 944 50 is_stmt 0 view .LVU518
 1631 0198 A36B     		ldr	r3, [r4, #56]
 944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 1632              		.loc 1 944 32 view .LVU519
 1633 019a 1B88     		ldrh	r3, [r3]
ARM GAS  /tmp/cc5SiBtg.s 			page 114


 944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 1634              		.loc 1 944 30 view .LVU520
 1635 019c D360     		str	r3, [r2, #12]
 945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 1636              		.loc 1 945 11 is_stmt 1 view .LVU521
 945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 1637              		.loc 1 945 15 is_stmt 0 view .LVU522
 1638 019e A36B     		ldr	r3, [r4, #56]
 945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 1639              		.loc 1 945 28 view .LVU523
 1640 01a0 0233     		adds	r3, r3, #2
 1641 01a2 A363     		str	r3, [r4, #56]
 946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1642              		.loc 1 946 11 is_stmt 1 view .LVU524
 946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1643              		.loc 1 946 15 is_stmt 0 view .LVU525
 1644 01a4 E38F     		ldrh	r3, [r4, #62]
 1645 01a6 9BB2     		uxth	r3, r3
 946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1646              		.loc 1 946 29 view .LVU526
 1647 01a8 023B     		subs	r3, r3, #2
 1648 01aa 9BB2     		uxth	r3, r3
 1649 01ac E387     		strh	r3, [r4, #62]	@ movhi
 1650 01ae E7E7     		b	.L121
 1651              	.L126:
 960:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 1652              		.loc 1 960 11 is_stmt 1 view .LVU527
 1653              	.LVL80:
 961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 1654              		.loc 1 961 11 view .LVU528
 961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 1655              		.loc 1 961 23 is_stmt 0 view .LVU529
 1656 01b0 0123     		movs	r3, #1
 1657 01b2 84F85D30 		strb	r3, [r4, #93]
 962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1658              		.loc 1 962 11 is_stmt 1 view .LVU530
 960:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 1659              		.loc 1 960 21 is_stmt 0 view .LVU531
 1660 01b6 0326     		movs	r6, #3
 962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1661              		.loc 1 962 11 view .LVU532
 1662 01b8 18E0     		b	.L105
 1663              	.LVL81:
 1664              	.L117:
 976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1665              		.loc 1 976 3 is_stmt 1 view .LVU533
 976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1666              		.loc 1 976 7 is_stmt 0 view .LVU534
 1667 01ba 3A46     		mov	r2, r7
 1668 01bc 2946     		mov	r1, r5
 1669 01be 2046     		mov	r0, r4
 1670 01c0 FFF7FEFF 		bl	SPI_EndRxTxTransaction
 1671              	.LVL82:
 976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1672              		.loc 1 976 6 discriminator 1 view .LVU535
 1673 01c4 08B1     		cbz	r0, .L128
 978:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
ARM GAS  /tmp/cc5SiBtg.s 			page 115


 1674              		.loc 1 978 5 is_stmt 1 view .LVU536
 978:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1675              		.loc 1 978 21 is_stmt 0 view .LVU537
 1676 01c6 2023     		movs	r3, #32
 1677 01c8 2366     		str	r3, [r4, #96]
 1678              	.L128:
 982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1679              		.loc 1 982 3 is_stmt 1 view .LVU538
 982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1680              		.loc 1 982 17 is_stmt 0 view .LVU539
 1681 01ca A368     		ldr	r3, [r4, #8]
 982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1682              		.loc 1 982 6 view .LVU540
 1683 01cc 33B9     		cbnz	r3, .L129
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1684              		.loc 1 984 5 is_stmt 1 view .LVU541
 1685              	.LBB2:
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1686              		.loc 1 984 5 view .LVU542
 1687 01ce 0193     		str	r3, [sp, #4]
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1688              		.loc 1 984 5 view .LVU543
 1689 01d0 2368     		ldr	r3, [r4]
 1690 01d2 DA68     		ldr	r2, [r3, #12]
 1691 01d4 0192     		str	r2, [sp, #4]
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1692              		.loc 1 984 5 view .LVU544
 1693 01d6 9B68     		ldr	r3, [r3, #8]
 1694 01d8 0193     		str	r3, [sp, #4]
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1695              		.loc 1 984 5 view .LVU545
 1696 01da 019B     		ldr	r3, [sp, #4]
 1697              	.L129:
 1698              	.LBE2:
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1699              		.loc 1 984 5 discriminator 1 view .LVU546
 987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1700              		.loc 1 987 3 view .LVU547
 987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1701              		.loc 1 987 11 is_stmt 0 view .LVU548
 1702 01dc 236E     		ldr	r3, [r4, #96]
 987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1703              		.loc 1 987 6 view .LVU549
 1704 01de 2BB9     		cbnz	r3, .L105
 993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1705              		.loc 1 993 5 is_stmt 1 view .LVU550
 993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1706              		.loc 1 993 17 is_stmt 0 view .LVU551
 1707 01e0 0123     		movs	r3, #1
 1708 01e2 84F85D30 		strb	r3, [r4, #93]
 824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t initial_TxXferCount;
 1709              		.loc 1 824 21 view .LVU552
 1710 01e6 0026     		movs	r6, #0
 1711 01e8 00E0     		b	.L105
 1712              	.LVL83:
 1713              	.L131:
 839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
ARM GAS  /tmp/cc5SiBtg.s 			page 116


 1714              		.loc 1 839 15 view .LVU553
 1715 01ea 0226     		movs	r6, #2
 1716              	.LVL84:
 1717              	.L105:
 998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 1718              		.loc 1 998 3 is_stmt 1 view .LVU554
 998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 1719              		.loc 1 998 3 view .LVU555
 1720 01ec 0023     		movs	r3, #0
 1721 01ee 84F85C30 		strb	r3, [r4, #92]
 998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 1722              		.loc 1 998 3 view .LVU556
 999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 1723              		.loc 1 999 3 view .LVU557
 1724              	.LVL85:
 1725              	.L104:
1000:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1726              		.loc 1 1000 1 is_stmt 0 view .LVU558
 1727 01f2 3046     		mov	r0, r6
 1728 01f4 03B0     		add	sp, sp, #12
 1729              		.cfi_remember_state
 1730              		.cfi_def_cfa_offset 28
 1731              		@ sp needed
 1732 01f6 BDE8F083 		pop	{r4, r5, r6, r7, r8, r9, pc}
 1733              	.LVL86:
 1734              	.L130:
 1735              		.cfi_restore_state
 831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1736              		.loc 1 831 3 discriminator 1 view .LVU559
 1737 01fa 0226     		movs	r6, #2
 1738 01fc F9E7     		b	.L104
 1739              		.cfi_endproc
 1740              	.LFE127:
 1742              		.section	.text.HAL_SPI_TransmitReceive,"ax",%progbits
 1743              		.align	1
 1744              		.global	HAL_SPI_TransmitReceive
 1745              		.syntax unified
 1746              		.thumb
 1747              		.thumb_func
 1749              	HAL_SPI_TransmitReceive:
 1750              	.LVL87:
 1751              	.LFB129:
1258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t             initial_TxXferCount;
 1752              		.loc 1 1258 1 is_stmt 1 view -0
 1753              		.cfi_startproc
 1754              		@ args = 4, pretend = 0, frame = 0
 1755              		@ frame_needed = 0, uses_anonymous_args = 0
1258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t             initial_TxXferCount;
 1756              		.loc 1 1258 1 is_stmt 0 view .LVU561
 1757 0000 2DE9F843 		push	{r3, r4, r5, r6, r7, r8, r9, lr}
 1758              		.cfi_def_cfa_offset 32
 1759              		.cfi_offset 3, -32
 1760              		.cfi_offset 4, -28
 1761              		.cfi_offset 5, -24
 1762              		.cfi_offset 6, -20
 1763              		.cfi_offset 7, -16
 1764              		.cfi_offset 8, -12
ARM GAS  /tmp/cc5SiBtg.s 			page 117


 1765              		.cfi_offset 9, -8
 1766              		.cfi_offset 14, -4
 1767 0004 1F46     		mov	r7, r3
 1768 0006 089D     		ldr	r5, [sp, #32]
1259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t             initial_RxXferCount;
 1769              		.loc 1 1259 3 is_stmt 1 view .LVU562
1260:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
 1770              		.loc 1 1260 3 view .LVU563
1261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_StateTypeDef tmp_state;
 1771              		.loc 1 1261 3 view .LVU564
1262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tickstart;
 1772              		.loc 1 1262 3 view .LVU565
1263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 1773              		.loc 1 1263 3 view .LVU566
1273:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef    errorcode = HAL_OK;
 1774              		.loc 1 1273 3 view .LVU567
 1775              	.LVL88:
1274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1776              		.loc 1 1274 3 view .LVU568
1277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1777              		.loc 1 1277 3 view .LVU569
1280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1778              		.loc 1 1280 3 view .LVU570
1280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1779              		.loc 1 1280 3 view .LVU571
 1780 0008 90F85C30 		ldrb	r3, [r0, #92]	@ zero_extendqisi2
 1781              	.LVL89:
1280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1782              		.loc 1 1280 3 is_stmt 0 view .LVU572
 1783 000c 012B     		cmp	r3, #1
 1784 000e 00F06B81 		beq	.L163
 1785 0012 0446     		mov	r4, r0
 1786 0014 8846     		mov	r8, r1
 1787 0016 9146     		mov	r9, r2
1280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1788              		.loc 1 1280 3 is_stmt 1 discriminator 2 view .LVU573
 1789 0018 0123     		movs	r3, #1
 1790 001a 80F85C30 		strb	r3, [r0, #92]
1280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1791              		.loc 1 1280 3 discriminator 2 view .LVU574
1283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1792              		.loc 1 1283 3 view .LVU575
1283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1793              		.loc 1 1283 15 is_stmt 0 view .LVU576
 1794 001e FFF7FEFF 		bl	HAL_GetTick
 1795              	.LVL90:
1283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1796              		.loc 1 1283 15 view .LVU577
 1797 0022 0646     		mov	r6, r0
 1798              	.LVL91:
1286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
 1799              		.loc 1 1286 3 is_stmt 1 view .LVU578
1286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
 1800              		.loc 1 1286 23 is_stmt 0 view .LVU579
 1801 0024 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 1802 0028 DBB2     		uxtb	r3, r3
 1803              	.LVL92:
ARM GAS  /tmp/cc5SiBtg.s 			page 118


1287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
 1804              		.loc 1 1287 3 is_stmt 1 view .LVU580
1287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
 1805              		.loc 1 1287 23 is_stmt 0 view .LVU581
 1806 002a 6268     		ldr	r2, [r4, #4]
 1807              	.LVL93:
1288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_RxXferCount = Size;
 1808              		.loc 1 1288 3 is_stmt 1 view .LVU582
1289:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 1809              		.loc 1 1289 3 view .LVU583
1295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 1810              		.loc 1 1295 3 view .LVU584
1295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 1811              		.loc 1 1295 6 is_stmt 0 view .LVU585
 1812 002c 012B     		cmp	r3, #1
 1813 002e 0AD0     		beq	.L136
1295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 1814              		.loc 1 1295 7 discriminator 1 view .LVU586
 1815 0030 B2F5827F 		cmp	r2, #260
 1816 0034 40F04681 		bne	.L164
1296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1817              		.loc 1 1296 54 view .LVU587
 1818 0038 A268     		ldr	r2, [r4, #8]
 1819              	.LVL94:
1296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1820              		.loc 1 1296 40 view .LVU588
 1821 003a 002A     		cmp	r2, #0
 1822 003c 40F04881 		bne	.L165
1296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1823              		.loc 1 1296 90 discriminator 1 view .LVU589
 1824 0040 042B     		cmp	r3, #4
 1825 0042 40F04781 		bne	.L166
 1826              	.L136:
1302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1827              		.loc 1 1302 3 is_stmt 1 view .LVU590
1302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1828              		.loc 1 1302 6 is_stmt 0 view .LVU591
 1829 0046 B8F1000F 		cmp	r8, #0
 1830 004a 00F04581 		beq	.L167
1302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1831              		.loc 1 1302 25 discriminator 1 view .LVU592
 1832 004e B9F1000F 		cmp	r9, #0
 1833 0052 00F04381 		beq	.L168
1302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1834              		.loc 1 1302 46 discriminator 2 view .LVU593
 1835 0056 002F     		cmp	r7, #0
 1836 0058 00F04281 		beq	.L169
1309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1837              		.loc 1 1309 3 is_stmt 1 view .LVU594
1309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1838              		.loc 1 1309 11 is_stmt 0 view .LVU595
 1839 005c 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 1840              	.LVL95:
1309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1841              		.loc 1 1309 11 view .LVU596
 1842 0060 DBB2     		uxtb	r3, r3
1309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 119


 1843              		.loc 1 1309 6 view .LVU597
 1844 0062 042B     		cmp	r3, #4
 1845 0064 02D0     		beq	.L138
1311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1846              		.loc 1 1311 5 is_stmt 1 view .LVU598
1311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1847              		.loc 1 1311 17 is_stmt 0 view .LVU599
 1848 0066 0523     		movs	r3, #5
 1849 0068 84F85D30 		strb	r3, [r4, #93]
 1850              	.L138:
1315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 1851              		.loc 1 1315 3 is_stmt 1 view .LVU600
1315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 1852              		.loc 1 1315 21 is_stmt 0 view .LVU601
 1853 006c 0023     		movs	r3, #0
 1854 006e 2366     		str	r3, [r4, #96]
1316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 1855              		.loc 1 1316 3 is_stmt 1 view .LVU602
1316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 1856              		.loc 1 1316 21 is_stmt 0 view .LVU603
 1857 0070 C4F84090 		str	r9, [r4, #64]
1317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 1858              		.loc 1 1317 3 is_stmt 1 view .LVU604
1317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 1859              		.loc 1 1317 21 is_stmt 0 view .LVU605
 1860 0074 A4F84670 		strh	r7, [r4, #70]	@ movhi
1318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
 1861              		.loc 1 1318 3 is_stmt 1 view .LVU606
1318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
 1862              		.loc 1 1318 21 is_stmt 0 view .LVU607
 1863 0078 A4F84470 		strh	r7, [r4, #68]	@ movhi
1319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 1864              		.loc 1 1319 3 is_stmt 1 view .LVU608
1319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 1865              		.loc 1 1319 21 is_stmt 0 view .LVU609
 1866 007c C4F83880 		str	r8, [r4, #56]
1320:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 1867              		.loc 1 1320 3 is_stmt 1 view .LVU610
1320:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 1868              		.loc 1 1320 21 is_stmt 0 view .LVU611
 1869 0080 E787     		strh	r7, [r4, #62]	@ movhi
1321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1870              		.loc 1 1321 3 is_stmt 1 view .LVU612
1321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1871              		.loc 1 1321 21 is_stmt 0 view .LVU613
 1872 0082 A787     		strh	r7, [r4, #60]	@ movhi
1324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 1873              		.loc 1 1324 3 is_stmt 1 view .LVU614
1324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 1874              		.loc 1 1324 21 is_stmt 0 view .LVU615
 1875 0084 E364     		str	r3, [r4, #76]
1325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1876              		.loc 1 1325 3 is_stmt 1 view .LVU616
1325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1877              		.loc 1 1325 21 is_stmt 0 view .LVU617
 1878 0086 2365     		str	r3, [r4, #80]
1336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 120


 1879              		.loc 1 1336 3 is_stmt 1 view .LVU618
1336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1880              		.loc 1 1336 18 is_stmt 0 view .LVU619
 1881 0088 E368     		ldr	r3, [r4, #12]
1336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1882              		.loc 1 1336 6 view .LVU620
 1883 008a B3F5E06F 		cmp	r3, #1792
 1884 008e 01D8     		bhi	.L139
1336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1885              		.loc 1 1336 49 discriminator 1 view .LVU621
 1886 0090 012F     		cmp	r7, #1
 1887 0092 23D9     		bls	.L140
 1888              	.L139:
1339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1889              		.loc 1 1339 5 is_stmt 1 view .LVU622
 1890 0094 2268     		ldr	r2, [r4]
 1891 0096 5368     		ldr	r3, [r2, #4]
 1892 0098 23F48053 		bic	r3, r3, #4096
 1893 009c 5360     		str	r3, [r2, #4]
 1894              	.LVL96:
 1895              	.L141:
1348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1896              		.loc 1 1348 3 view .LVU623
1348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1897              		.loc 1 1348 12 is_stmt 0 view .LVU624
 1898 009e 2368     		ldr	r3, [r4]
1348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1899              		.loc 1 1348 22 view .LVU625
 1900 00a0 1A68     		ldr	r2, [r3]
1348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1901              		.loc 1 1348 6 view .LVU626
 1902 00a2 12F0400F 		tst	r2, #64
 1903 00a6 03D1     		bne	.L142
1351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1904              		.loc 1 1351 5 is_stmt 1 view .LVU627
 1905 00a8 1A68     		ldr	r2, [r3]
 1906 00aa 42F04002 		orr	r2, r2, #64
 1907 00ae 1A60     		str	r2, [r3]
 1908              	.L142:
1355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1909              		.loc 1 1355 3 view .LVU628
1355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1910              		.loc 1 1355 17 is_stmt 0 view .LVU629
 1911 00b0 E368     		ldr	r3, [r4, #12]
1355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1912              		.loc 1 1355 6 view .LVU630
 1913 00b2 B3F5E06F 		cmp	r3, #1792
 1914 00b6 5CD9     		bls	.L143
1357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1915              		.loc 1 1357 5 is_stmt 1 view .LVU631
1357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1916              		.loc 1 1357 20 is_stmt 0 view .LVU632
 1917 00b8 6368     		ldr	r3, [r4, #4]
1357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1918              		.loc 1 1357 8 view .LVU633
 1919 00ba 0BB1     		cbz	r3, .L144
1357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
ARM GAS  /tmp/cc5SiBtg.s 			page 121


 1920              		.loc 1 1357 45 discriminator 1 view .LVU634
 1921 00bc 012F     		cmp	r7, #1
 1922 00be 0BD1     		bne	.L145
 1923              	.L144:
1359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1924              		.loc 1 1359 7 is_stmt 1 view .LVU635
1359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1925              		.loc 1 1359 46 is_stmt 0 view .LVU636
 1926 00c0 A26B     		ldr	r2, [r4, #56]
1359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1927              		.loc 1 1359 11 view .LVU637
 1928 00c2 2368     		ldr	r3, [r4]
1359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1929              		.loc 1 1359 28 view .LVU638
 1930 00c4 1288     		ldrh	r2, [r2]
1359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1931              		.loc 1 1359 26 view .LVU639
 1932 00c6 DA60     		str	r2, [r3, #12]
1360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 1933              		.loc 1 1360 7 is_stmt 1 view .LVU640
1360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 1934              		.loc 1 1360 11 is_stmt 0 view .LVU641
 1935 00c8 A36B     		ldr	r3, [r4, #56]
1360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 1936              		.loc 1 1360 24 view .LVU642
 1937 00ca 0233     		adds	r3, r3, #2
 1938 00cc A363     		str	r3, [r4, #56]
1361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1939              		.loc 1 1361 7 is_stmt 1 view .LVU643
1361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1940              		.loc 1 1361 11 is_stmt 0 view .LVU644
 1941 00ce E38F     		ldrh	r3, [r4, #62]
 1942 00d0 9BB2     		uxth	r3, r3
1361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1943              		.loc 1 1361 24 view .LVU645
 1944 00d2 013B     		subs	r3, r3, #1
 1945 00d4 9BB2     		uxth	r3, r3
 1946 00d6 E387     		strh	r3, [r4, #62]	@ movhi
 1947              	.L145:
1409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1948              		.loc 1 1409 19 view .LVU646
 1949 00d8 0127     		movs	r7, #1
 1950              	.LVL97:
1409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1951              		.loc 1 1409 19 view .LVU647
 1952 00da 30E0     		b	.L146
 1953              	.LVL98:
 1954              	.L140:
1344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1955              		.loc 1 1344 5 is_stmt 1 view .LVU648
 1956 00dc 2268     		ldr	r2, [r4]
 1957 00de 5368     		ldr	r3, [r2, #4]
 1958 00e0 43F48053 		orr	r3, r3, #4096
 1959 00e4 5360     		str	r3, [r2, #4]
 1960              	.LVL99:
1344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1961              		.loc 1 1344 5 is_stmt 0 view .LVU649
ARM GAS  /tmp/cc5SiBtg.s 			page 122


 1962 00e6 DAE7     		b	.L141
 1963              	.LVL100:
 1964              	.L174:
1382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1965              		.loc 1 1382 9 is_stmt 1 view .LVU650
1382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1966              		.loc 1 1382 48 is_stmt 0 view .LVU651
 1967 00e8 A26B     		ldr	r2, [r4, #56]
1382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1968              		.loc 1 1382 30 view .LVU652
 1969 00ea 1288     		ldrh	r2, [r2]
1382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1970              		.loc 1 1382 28 view .LVU653
 1971 00ec DA60     		str	r2, [r3, #12]
1383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1972              		.loc 1 1383 9 is_stmt 1 view .LVU654
1383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1973              		.loc 1 1383 13 is_stmt 0 view .LVU655
 1974 00ee A36B     		ldr	r3, [r4, #56]
1383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1975              		.loc 1 1383 26 view .LVU656
 1976 00f0 0233     		adds	r3, r3, #2
 1977 00f2 A363     		str	r3, [r4, #56]
1384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a reception (Rx). Tx not allowed */
 1978              		.loc 1 1384 9 is_stmt 1 view .LVU657
1384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a reception (Rx). Tx not allowed */
 1979              		.loc 1 1384 13 is_stmt 0 view .LVU658
 1980 00f4 E38F     		ldrh	r3, [r4, #62]
 1981 00f6 9BB2     		uxth	r3, r3
1384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a reception (Rx). Tx not allowed */
 1982              		.loc 1 1384 26 view .LVU659
 1983 00f8 013B     		subs	r3, r3, #1
 1984 00fa 9BB2     		uxth	r3, r3
 1985 00fc E387     		strh	r3, [r4, #62]	@ movhi
1386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1986              		.loc 1 1386 9 is_stmt 1 view .LVU660
 1987              	.LVL101:
1386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1988              		.loc 1 1386 19 is_stmt 0 view .LVU661
 1989 00fe 0027     		movs	r7, #0
 1990              	.LVL102:
 1991              	.L147:
1403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1992              		.loc 1 1403 7 is_stmt 1 view .LVU662
1403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1993              		.loc 1 1403 12 is_stmt 0 view .LVU663
 1994 0100 2368     		ldr	r3, [r4]
 1995 0102 9A68     		ldr	r2, [r3, #8]
1403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1996              		.loc 1 1403 10 view .LVU664
 1997 0104 12F0010F 		tst	r2, #1
 1998 0108 11D0     		beq	.L148
1403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1999              		.loc 1 1403 61 discriminator 1 view .LVU665
 2000 010a B4F84620 		ldrh	r2, [r4, #70]
 2001 010e 92B2     		uxth	r2, r2
1403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
ARM GAS  /tmp/cc5SiBtg.s 			page 123


 2002              		.loc 1 1403 53 discriminator 1 view .LVU666
 2003 0110 6AB1     		cbz	r2, .L148
1405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 2004              		.loc 1 1405 9 is_stmt 1 view .LVU667
1405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 2005              		.loc 1 1405 67 is_stmt 0 view .LVU668
 2006 0112 DA68     		ldr	r2, [r3, #12]
1405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 2007              		.loc 1 1405 27 view .LVU669
 2008 0114 236C     		ldr	r3, [r4, #64]
1405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 2009              		.loc 1 1405 41 view .LVU670
 2010 0116 1A80     		strh	r2, [r3]	@ movhi
1406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2011              		.loc 1 1406 9 is_stmt 1 view .LVU671
1406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2012              		.loc 1 1406 13 is_stmt 0 view .LVU672
 2013 0118 236C     		ldr	r3, [r4, #64]
1406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2014              		.loc 1 1406 26 view .LVU673
 2015 011a 0233     		adds	r3, r3, #2
 2016 011c 2364     		str	r3, [r4, #64]
1407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a Transmission (Tx). Tx is allowed */
 2017              		.loc 1 1407 9 is_stmt 1 view .LVU674
1407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a Transmission (Tx). Tx is allowed */
 2018              		.loc 1 1407 13 is_stmt 0 view .LVU675
 2019 011e B4F84630 		ldrh	r3, [r4, #70]
 2020 0122 9BB2     		uxth	r3, r3
1407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a Transmission (Tx). Tx is allowed */
 2021              		.loc 1 1407 26 view .LVU676
 2022 0124 013B     		subs	r3, r3, #1
 2023 0126 9BB2     		uxth	r3, r3
 2024 0128 A4F84630 		strh	r3, [r4, #70]	@ movhi
1409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2025              		.loc 1 1409 9 is_stmt 1 view .LVU677
 2026              	.LVL103:
1409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2027              		.loc 1 1409 19 is_stmt 0 view .LVU678
 2028 012c 0127     		movs	r7, #1
 2029              	.LVL104:
 2030              	.L148:
1411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2031              		.loc 1 1411 7 is_stmt 1 view .LVU679
1411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2032              		.loc 1 1411 13 is_stmt 0 view .LVU680
 2033 012e FFF7FEFF 		bl	HAL_GetTick
 2034              	.LVL105:
1411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2035              		.loc 1 1411 27 discriminator 1 view .LVU681
 2036 0132 831B     		subs	r3, r0, r6
1411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2037              		.loc 1 1411 10 discriminator 1 view .LVU682
 2038 0134 AB42     		cmp	r3, r5
 2039 0136 02D3     		bcc	.L146
1411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2040              		.loc 1 1411 53 discriminator 1 view .LVU683
 2041 0138 B5F1FF3F 		cmp	r5, #-1
ARM GAS  /tmp/cc5SiBtg.s 			page 124


 2042 013c 14D1     		bne	.L173
 2043              	.LVL106:
 2044              	.L146:
1377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2045              		.loc 1 1377 37 is_stmt 1 view .LVU684
1377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2046              		.loc 1 1377 17 is_stmt 0 view .LVU685
 2047 013e E38F     		ldrh	r3, [r4, #62]
 2048 0140 9BB2     		uxth	r3, r3
1377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2049              		.loc 1 1377 37 view .LVU686
 2050 0142 2BB9     		cbnz	r3, .L149
1377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2051              		.loc 1 1377 45 discriminator 1 view .LVU687
 2052 0144 B4F84630 		ldrh	r3, [r4, #70]
 2053 0148 9BB2     		uxth	r3, r3
1377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2054              		.loc 1 1377 37 discriminator 1 view .LVU688
 2055 014a 002B     		cmp	r3, #0
 2056 014c 00F0AB80 		beq	.L150
 2057              	.L149:
1380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2058              		.loc 1 1380 7 is_stmt 1 view .LVU689
1380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2059              		.loc 1 1380 12 is_stmt 0 view .LVU690
 2060 0150 2368     		ldr	r3, [r4]
 2061 0152 9A68     		ldr	r2, [r3, #8]
1380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2062              		.loc 1 1380 10 view .LVU691
 2063 0154 12F0020F 		tst	r2, #2
 2064 0158 D2D0     		beq	.L147
1380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2065              		.loc 1 1380 60 discriminator 1 view .LVU692
 2066 015a E28F     		ldrh	r2, [r4, #62]
 2067 015c 92B2     		uxth	r2, r2
1380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2068              		.loc 1 1380 52 discriminator 1 view .LVU693
 2069 015e 002A     		cmp	r2, #0
 2070 0160 CED0     		beq	.L147
1380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2071              		.loc 1 1380 80 discriminator 2 view .LVU694
 2072 0162 002F     		cmp	r7, #0
 2073 0164 CCD0     		beq	.L147
 2074 0166 BFE7     		b	.L174
 2075              	.L173:
1413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
 2076              		.loc 1 1413 9 is_stmt 1 view .LVU695
 2077              	.LVL107:
1414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         goto error;
 2078              		.loc 1 1414 9 view .LVU696
1414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         goto error;
 2079              		.loc 1 1414 21 is_stmt 0 view .LVU697
 2080 0168 0123     		movs	r3, #1
 2081 016a 84F85D30 		strb	r3, [r4, #93]
1415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2082              		.loc 1 1415 9 is_stmt 1 view .LVU698
1413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
ARM GAS  /tmp/cc5SiBtg.s 			page 125


 2083              		.loc 1 1413 19 is_stmt 0 view .LVU699
 2084 016e 0320     		movs	r0, #3
1415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2085              		.loc 1 1415 9 view .LVU700
 2086 0170 A9E0     		b	.L137
 2087              	.LVL108:
 2088              	.L143:
1422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2089              		.loc 1 1422 5 is_stmt 1 view .LVU701
1422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2090              		.loc 1 1422 20 is_stmt 0 view .LVU702
 2091 0172 6368     		ldr	r3, [r4, #4]
1422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2092              		.loc 1 1422 8 view .LVU703
 2093 0174 0BB1     		cbz	r3, .L151
1422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2094              		.loc 1 1422 45 discriminator 1 view .LVU704
 2095 0176 012F     		cmp	r7, #1
 2096 0178 0FD1     		bne	.L152
 2097              	.L151:
1424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2098              		.loc 1 1424 7 is_stmt 1 view .LVU705
1424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2099              		.loc 1 1424 15 is_stmt 0 view .LVU706
 2100 017a E38F     		ldrh	r3, [r4, #62]
 2101 017c 9BB2     		uxth	r3, r3
1424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2102              		.loc 1 1424 10 view .LVU707
 2103 017e 012B     		cmp	r3, #1
 2104 0180 0DD9     		bls	.L153
1426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 2105              		.loc 1 1426 9 is_stmt 1 view .LVU708
1426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 2106              		.loc 1 1426 48 is_stmt 0 view .LVU709
 2107 0182 A26B     		ldr	r2, [r4, #56]
1426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 2108              		.loc 1 1426 13 view .LVU710
 2109 0184 2368     		ldr	r3, [r4]
1426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 2110              		.loc 1 1426 30 view .LVU711
 2111 0186 1288     		ldrh	r2, [r2]
1426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 2112              		.loc 1 1426 28 view .LVU712
 2113 0188 DA60     		str	r2, [r3, #12]
1427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 2114              		.loc 1 1427 9 is_stmt 1 view .LVU713
1427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 2115              		.loc 1 1427 13 is_stmt 0 view .LVU714
 2116 018a A36B     		ldr	r3, [r4, #56]
1427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 2117              		.loc 1 1427 26 view .LVU715
 2118 018c 0233     		adds	r3, r3, #2
 2119 018e A363     		str	r3, [r4, #56]
1428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2120              		.loc 1 1428 9 is_stmt 1 view .LVU716
1428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2121              		.loc 1 1428 13 is_stmt 0 view .LVU717
ARM GAS  /tmp/cc5SiBtg.s 			page 126


 2122 0190 E38F     		ldrh	r3, [r4, #62]
 2123 0192 9BB2     		uxth	r3, r3
1428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2124              		.loc 1 1428 27 view .LVU718
 2125 0194 023B     		subs	r3, r3, #2
 2126 0196 9BB2     		uxth	r3, r3
 2127 0198 E387     		strh	r3, [r4, #62]	@ movhi
 2128              	.L152:
1505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2129              		.loc 1 1505 19 view .LVU719
 2130 019a 0127     		movs	r7, #1
 2131              	.LVL109:
1505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2132              		.loc 1 1505 19 view .LVU720
 2133 019c 49E0     		b	.L160
 2134              	.LVL110:
 2135              	.L153:
1432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr++;
 2136              		.loc 1 1432 9 is_stmt 1 view .LVU721
1432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr++;
 2137              		.loc 1 1432 54 is_stmt 0 view .LVU722
 2138 019e A26B     		ldr	r2, [r4, #56]
1432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr++;
 2139              		.loc 1 1432 31 view .LVU723
 2140 01a0 2368     		ldr	r3, [r4]
1432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr++;
 2141              		.loc 1 1432 49 view .LVU724
 2142 01a2 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
1432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr++;
 2143              		.loc 1 1432 46 view .LVU725
 2144 01a4 1A73     		strb	r2, [r3, #12]
1433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 2145              		.loc 1 1433 9 is_stmt 1 view .LVU726
1433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 2146              		.loc 1 1433 13 is_stmt 0 view .LVU727
 2147 01a6 A36B     		ldr	r3, [r4, #56]
1433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 2148              		.loc 1 1433 25 view .LVU728
 2149 01a8 0133     		adds	r3, r3, #1
 2150 01aa A363     		str	r3, [r4, #56]
1434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2151              		.loc 1 1434 9 is_stmt 1 view .LVU729
1434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2152              		.loc 1 1434 13 is_stmt 0 view .LVU730
 2153 01ac E38F     		ldrh	r3, [r4, #62]
 2154 01ae 9BB2     		uxth	r3, r3
1434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2155              		.loc 1 1434 26 view .LVU731
 2156 01b0 013B     		subs	r3, r3, #1
 2157 01b2 9BB2     		uxth	r3, r3
 2158 01b4 E387     		strh	r3, [r4, #62]	@ movhi
 2159 01b6 F0E7     		b	.L152
 2160              	.LVL111:
 2161              	.L175:
1455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2162              		.loc 1 1455 9 is_stmt 1 view .LVU732
1455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
ARM GAS  /tmp/cc5SiBtg.s 			page 127


 2163              		.loc 1 1455 17 is_stmt 0 view .LVU733
 2164 01b8 E28F     		ldrh	r2, [r4, #62]
 2165 01ba 92B2     		uxth	r2, r2
1455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2166              		.loc 1 1455 12 view .LVU734
 2167 01bc 012A     		cmp	r2, #1
 2168 01be 0CD9     		bls	.L155
1457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 2169              		.loc 1 1457 11 is_stmt 1 view .LVU735
1457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 2170              		.loc 1 1457 50 is_stmt 0 view .LVU736
 2171 01c0 A26B     		ldr	r2, [r4, #56]
1457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 2172              		.loc 1 1457 32 view .LVU737
 2173 01c2 1288     		ldrh	r2, [r2]
1457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 2174              		.loc 1 1457 30 view .LVU738
 2175 01c4 DA60     		str	r2, [r3, #12]
1458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 2176              		.loc 1 1458 11 is_stmt 1 view .LVU739
1458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 2177              		.loc 1 1458 15 is_stmt 0 view .LVU740
 2178 01c6 A36B     		ldr	r3, [r4, #56]
1458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 2179              		.loc 1 1458 28 view .LVU741
 2180 01c8 0233     		adds	r3, r3, #2
 2181 01ca A363     		str	r3, [r4, #56]
1459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2182              		.loc 1 1459 11 is_stmt 1 view .LVU742
1459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2183              		.loc 1 1459 15 is_stmt 0 view .LVU743
 2184 01cc E38F     		ldrh	r3, [r4, #62]
 2185 01ce 9BB2     		uxth	r3, r3
1459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2186              		.loc 1 1459 29 view .LVU744
 2187 01d0 023B     		subs	r3, r3, #2
 2188 01d2 9BB2     		uxth	r3, r3
 2189 01d4 E387     		strh	r3, [r4, #62]	@ movhi
1468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2190              		.loc 1 1468 19 view .LVU745
 2191 01d6 0027     		movs	r7, #0
 2192              	.LVL112:
1468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2193              		.loc 1 1468 19 view .LVU746
 2194 01d8 3DE0     		b	.L154
 2195              	.LVL113:
 2196              	.L155:
1463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 2197              		.loc 1 1463 11 is_stmt 1 view .LVU747
1463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 2198              		.loc 1 1463 56 is_stmt 0 view .LVU748
 2199 01da A26B     		ldr	r2, [r4, #56]
1463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 2200              		.loc 1 1463 51 view .LVU749
 2201 01dc 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
1463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 2202              		.loc 1 1463 48 view .LVU750
ARM GAS  /tmp/cc5SiBtg.s 			page 128


 2203 01de 1A73     		strb	r2, [r3, #12]
1464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 2204              		.loc 1 1464 11 is_stmt 1 view .LVU751
1464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 2205              		.loc 1 1464 15 is_stmt 0 view .LVU752
 2206 01e0 A36B     		ldr	r3, [r4, #56]
1464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 2207              		.loc 1 1464 27 view .LVU753
 2208 01e2 0133     		adds	r3, r3, #1
 2209 01e4 A363     		str	r3, [r4, #56]
1465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2210              		.loc 1 1465 11 is_stmt 1 view .LVU754
1465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2211              		.loc 1 1465 15 is_stmt 0 view .LVU755
 2212 01e6 E38F     		ldrh	r3, [r4, #62]
 2213 01e8 9BB2     		uxth	r3, r3
1465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2214              		.loc 1 1465 28 view .LVU756
 2215 01ea 013B     		subs	r3, r3, #1
 2216 01ec 9BB2     		uxth	r3, r3
 2217 01ee E387     		strh	r3, [r4, #62]	@ movhi
1468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2218              		.loc 1 1468 19 view .LVU757
 2219 01f0 0027     		movs	r7, #0
 2220              	.LVL114:
1468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2221              		.loc 1 1468 19 view .LVU758
 2222 01f2 30E0     		b	.L154
 2223              	.LVL115:
 2224              	.L176:
1495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
 2225              		.loc 1 1495 13 is_stmt 1 view .LVU759
 2226 01f4 2268     		ldr	r2, [r4]
 2227 01f6 5368     		ldr	r3, [r2, #4]
 2228 01f8 43F48053 		orr	r3, r3, #4096
 2229 01fc 5360     		str	r3, [r2, #4]
1505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2230              		.loc 1 1505 19 is_stmt 0 view .LVU760
 2231 01fe 0127     		movs	r7, #1
 2232              	.LVL116:
1505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2233              		.loc 1 1505 19 view .LVU761
 2234 0200 0DE0     		b	.L156
 2235              	.LVL117:
 2236              	.L157:
1500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr++;
 2237              		.loc 1 1500 11 is_stmt 1 view .LVU762
1500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr++;
 2238              		.loc 1 1500 28 is_stmt 0 view .LVU763
 2239 0202 226C     		ldr	r2, [r4, #64]
1500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr++;
 2240              		.loc 1 1500 44 view .LVU764
 2241 0204 1B7B     		ldrb	r3, [r3, #12]	@ zero_extendqisi2
1500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr++;
 2242              		.loc 1 1500 42 view .LVU765
 2243 0206 1370     		strb	r3, [r2]
1501:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount--;
ARM GAS  /tmp/cc5SiBtg.s 			page 129


 2244              		.loc 1 1501 11 is_stmt 1 view .LVU766
1501:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount--;
 2245              		.loc 1 1501 15 is_stmt 0 view .LVU767
 2246 0208 236C     		ldr	r3, [r4, #64]
1501:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount--;
 2247              		.loc 1 1501 27 view .LVU768
 2248 020a 0133     		adds	r3, r3, #1
 2249 020c 2364     		str	r3, [r4, #64]
1502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2250              		.loc 1 1502 11 is_stmt 1 view .LVU769
1502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2251              		.loc 1 1502 15 is_stmt 0 view .LVU770
 2252 020e B4F84630 		ldrh	r3, [r4, #70]
 2253 0212 9BB2     		uxth	r3, r3
1502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2254              		.loc 1 1502 28 view .LVU771
 2255 0214 013B     		subs	r3, r3, #1
 2256 0216 9BB2     		uxth	r3, r3
 2257 0218 A4F84630 		strh	r3, [r4, #70]	@ movhi
1505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2258              		.loc 1 1505 19 view .LVU772
 2259 021c 0127     		movs	r7, #1
 2260              	.LVL118:
 2261              	.L156:
1507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2262              		.loc 1 1507 7 is_stmt 1 view .LVU773
1507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2263              		.loc 1 1507 14 is_stmt 0 view .LVU774
 2264 021e FFF7FEFF 		bl	HAL_GetTick
 2265              	.LVL119:
1507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2266              		.loc 1 1507 28 discriminator 1 view .LVU775
 2267 0222 801B     		subs	r0, r0, r6
1507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2268              		.loc 1 1507 10 discriminator 1 view .LVU776
 2269 0224 A842     		cmp	r0, r5
 2270 0226 02D3     		bcc	.L158
1507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2271              		.loc 1 1507 54 discriminator 1 view .LVU777
 2272 0228 B5F1FF3F 		cmp	r5, #-1
 2273 022c 36D1     		bne	.L159
 2274              	.L158:
1507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2275              		.loc 1 1507 87 discriminator 3 view .LVU778
 2276 022e 002D     		cmp	r5, #0
 2277 0230 34D0     		beq	.L159
 2278              	.LVL120:
 2279              	.L160:
1450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2280              		.loc 1 1450 37 is_stmt 1 view .LVU779
1450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2281              		.loc 1 1450 17 is_stmt 0 view .LVU780
 2282 0232 E38F     		ldrh	r3, [r4, #62]
 2283 0234 9BB2     		uxth	r3, r3
1450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2284              		.loc 1 1450 37 view .LVU781
 2285 0236 23B9     		cbnz	r3, .L161
ARM GAS  /tmp/cc5SiBtg.s 			page 130


1450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2286              		.loc 1 1450 45 discriminator 1 view .LVU782
 2287 0238 B4F84630 		ldrh	r3, [r4, #70]
 2288 023c 9BB2     		uxth	r3, r3
1450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2289              		.loc 1 1450 37 discriminator 1 view .LVU783
 2290 023e 002B     		cmp	r3, #0
 2291 0240 31D0     		beq	.L150
 2292              	.L161:
1453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2293              		.loc 1 1453 7 is_stmt 1 view .LVU784
1453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2294              		.loc 1 1453 12 is_stmt 0 view .LVU785
 2295 0242 2368     		ldr	r3, [r4]
 2296 0244 9A68     		ldr	r2, [r3, #8]
1453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2297              		.loc 1 1453 10 view .LVU786
 2298 0246 12F0020F 		tst	r2, #2
 2299 024a 04D0     		beq	.L154
1453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2300              		.loc 1 1453 60 discriminator 1 view .LVU787
 2301 024c E28F     		ldrh	r2, [r4, #62]
 2302 024e 92B2     		uxth	r2, r2
1453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2303              		.loc 1 1453 52 discriminator 1 view .LVU788
 2304 0250 0AB1     		cbz	r2, .L154
1453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2305              		.loc 1 1453 80 discriminator 2 view .LVU789
 2306 0252 002F     		cmp	r7, #0
 2307 0254 B0D1     		bne	.L175
 2308              	.LVL121:
 2309              	.L154:
1485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2310              		.loc 1 1485 7 is_stmt 1 view .LVU790
1485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2311              		.loc 1 1485 12 is_stmt 0 view .LVU791
 2312 0256 2368     		ldr	r3, [r4]
 2313 0258 9A68     		ldr	r2, [r3, #8]
1485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2314              		.loc 1 1485 10 view .LVU792
 2315 025a 12F0010F 		tst	r2, #1
 2316 025e DED0     		beq	.L156
1485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2317              		.loc 1 1485 61 discriminator 1 view .LVU793
 2318 0260 B4F84620 		ldrh	r2, [r4, #70]
 2319 0264 92B2     		uxth	r2, r2
1485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2320              		.loc 1 1485 53 discriminator 1 view .LVU794
 2321 0266 002A     		cmp	r2, #0
 2322 0268 D9D0     		beq	.L156
1487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2323              		.loc 1 1487 9 is_stmt 1 view .LVU795
1487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2324              		.loc 1 1487 17 is_stmt 0 view .LVU796
 2325 026a B4F84620 		ldrh	r2, [r4, #70]
 2326 026e 92B2     		uxth	r2, r2
1487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
ARM GAS  /tmp/cc5SiBtg.s 			page 131


 2327              		.loc 1 1487 12 view .LVU797
 2328 0270 012A     		cmp	r2, #1
 2329 0272 C6D9     		bls	.L157
1489:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
 2330              		.loc 1 1489 11 is_stmt 1 view .LVU798
1489:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
 2331              		.loc 1 1489 69 is_stmt 0 view .LVU799
 2332 0274 DA68     		ldr	r2, [r3, #12]
1489:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
 2333              		.loc 1 1489 29 view .LVU800
 2334 0276 236C     		ldr	r3, [r4, #64]
1489:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
 2335              		.loc 1 1489 43 view .LVU801
 2336 0278 1A80     		strh	r2, [r3]	@ movhi
1490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount -= 2U;
 2337              		.loc 1 1490 11 is_stmt 1 view .LVU802
1490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount -= 2U;
 2338              		.loc 1 1490 15 is_stmt 0 view .LVU803
 2339 027a 236C     		ldr	r3, [r4, #64]
1490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount -= 2U;
 2340              		.loc 1 1490 28 view .LVU804
 2341 027c 0233     		adds	r3, r3, #2
 2342 027e 2364     		str	r3, [r4, #64]
1491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (hspi->RxXferCount <= 1U)
 2343              		.loc 1 1491 11 is_stmt 1 view .LVU805
1491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (hspi->RxXferCount <= 1U)
 2344              		.loc 1 1491 15 is_stmt 0 view .LVU806
 2345 0280 B4F84630 		ldrh	r3, [r4, #70]
 2346 0284 9BB2     		uxth	r3, r3
1491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (hspi->RxXferCount <= 1U)
 2347              		.loc 1 1491 29 view .LVU807
 2348 0286 023B     		subs	r3, r3, #2
 2349 0288 9BB2     		uxth	r3, r3
 2350 028a A4F84630 		strh	r3, [r4, #70]	@ movhi
1492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 2351              		.loc 1 1492 11 is_stmt 1 view .LVU808
1492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 2352              		.loc 1 1492 19 is_stmt 0 view .LVU809
 2353 028e B4F84630 		ldrh	r3, [r4, #70]
 2354 0292 9BB2     		uxth	r3, r3
1492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 2355              		.loc 1 1492 14 view .LVU810
 2356 0294 012B     		cmp	r3, #1
 2357 0296 ADD9     		bls	.L176
1505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2358              		.loc 1 1505 19 view .LVU811
 2359 0298 0127     		movs	r7, #1
 2360              	.LVL122:
1505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2361              		.loc 1 1505 19 view .LVU812
 2362 029a C0E7     		b	.L156
 2363              	.LVL123:
 2364              	.L159:
1509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
 2365              		.loc 1 1509 9 is_stmt 1 view .LVU813
1510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         goto error;
 2366              		.loc 1 1510 9 view .LVU814
ARM GAS  /tmp/cc5SiBtg.s 			page 132


1510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         goto error;
 2367              		.loc 1 1510 21 is_stmt 0 view .LVU815
 2368 029c 0123     		movs	r3, #1
 2369 029e 84F85D30 		strb	r3, [r4, #93]
1511:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2370              		.loc 1 1511 9 is_stmt 1 view .LVU816
1509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
 2371              		.loc 1 1509 19 is_stmt 0 view .LVU817
 2372 02a2 0320     		movs	r0, #3
1511:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2373              		.loc 1 1511 9 view .LVU818
 2374 02a4 0FE0     		b	.L137
 2375              	.LVL124:
 2376              	.L150:
1574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2377              		.loc 1 1574 3 is_stmt 1 view .LVU819
1574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2378              		.loc 1 1574 7 is_stmt 0 view .LVU820
 2379 02a6 3246     		mov	r2, r6
 2380 02a8 2946     		mov	r1, r5
 2381 02aa 2046     		mov	r0, r4
 2382 02ac FFF7FEFF 		bl	SPI_EndRxTxTransaction
 2383              	.LVL125:
1574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2384              		.loc 1 1574 6 discriminator 1 view .LVU821
 2385 02b0 10B1     		cbz	r0, .L162
1576:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_FLAG;
 2386              		.loc 1 1576 5 is_stmt 1 view .LVU822
 2387              	.LVL126:
1577:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2388              		.loc 1 1577 5 view .LVU823
1577:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2389              		.loc 1 1577 21 is_stmt 0 view .LVU824
 2390 02b2 2023     		movs	r3, #32
 2391 02b4 2366     		str	r3, [r4, #96]
1576:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_FLAG;
 2392              		.loc 1 1576 15 view .LVU825
 2393 02b6 0120     		movs	r0, #1
 2394              	.LVL127:
 2395              	.L162:
1580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2396              		.loc 1 1580 3 is_stmt 1 view .LVU826
1580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2397              		.loc 1 1580 11 is_stmt 0 view .LVU827
 2398 02b8 236E     		ldr	r3, [r4, #96]
1580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2399              		.loc 1 1580 6 view .LVU828
 2400 02ba 9BB9     		cbnz	r3, .L171
1586:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2401              		.loc 1 1586 5 is_stmt 1 view .LVU829
1586:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2402              		.loc 1 1586 17 is_stmt 0 view .LVU830
 2403 02bc 0123     		movs	r3, #1
 2404 02be 84F85D30 		strb	r3, [r4, #93]
 2405 02c2 00E0     		b	.L137
 2406              	.LVL128:
 2407              	.L164:
ARM GAS  /tmp/cc5SiBtg.s 			page 133


1298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2408              		.loc 1 1298 15 view .LVU831
 2409 02c4 0220     		movs	r0, #2
 2410              	.LVL129:
 2411              	.L137:
1590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2412              		.loc 1 1590 3 is_stmt 1 view .LVU832
1590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2413              		.loc 1 1590 3 view .LVU833
 2414 02c6 0023     		movs	r3, #0
 2415 02c8 84F85C30 		strb	r3, [r4, #92]
1590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2416              		.loc 1 1590 3 view .LVU834
1591:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 2417              		.loc 1 1591 3 view .LVU835
 2418              	.LVL130:
 2419              	.L135:
1592:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2420              		.loc 1 1592 1 is_stmt 0 view .LVU836
 2421 02cc BDE8F883 		pop	{r3, r4, r5, r6, r7, r8, r9, pc}
 2422              	.LVL131:
 2423              	.L165:
1298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2424              		.loc 1 1298 15 view .LVU837
 2425 02d0 0220     		movs	r0, #2
 2426              	.LVL132:
1298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2427              		.loc 1 1298 15 view .LVU838
 2428 02d2 F8E7     		b	.L137
 2429              	.LVL133:
 2430              	.L166:
1298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2431              		.loc 1 1298 15 view .LVU839
 2432 02d4 0220     		movs	r0, #2
 2433              	.LVL134:
1298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2434              		.loc 1 1298 15 view .LVU840
 2435 02d6 F6E7     		b	.L137
 2436              	.LVL135:
 2437              	.L167:
1304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2438              		.loc 1 1304 15 view .LVU841
 2439 02d8 0120     		movs	r0, #1
 2440              	.LVL136:
1304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2441              		.loc 1 1304 15 view .LVU842
 2442 02da F4E7     		b	.L137
 2443              	.LVL137:
 2444              	.L168:
1304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2445              		.loc 1 1304 15 view .LVU843
 2446 02dc 0120     		movs	r0, #1
 2447              	.LVL138:
1304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2448              		.loc 1 1304 15 view .LVU844
 2449 02de F2E7     		b	.L137
 2450              	.LVL139:
ARM GAS  /tmp/cc5SiBtg.s 			page 134


 2451              	.L169:
1304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2452              		.loc 1 1304 15 view .LVU845
 2453 02e0 0120     		movs	r0, #1
 2454              	.LVL140:
1304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2455              		.loc 1 1304 15 view .LVU846
 2456 02e2 F0E7     		b	.L137
 2457              	.LVL141:
 2458              	.L171:
1582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2459              		.loc 1 1582 15 view .LVU847
 2460 02e4 0120     		movs	r0, #1
 2461              	.LVL142:
1582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2462              		.loc 1 1582 15 view .LVU848
 2463 02e6 EEE7     		b	.L137
 2464              	.LVL143:
 2465              	.L163:
1280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2466              		.loc 1 1280 3 discriminator 1 view .LVU849
 2467 02e8 0220     		movs	r0, #2
 2468              	.LVL144:
1280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2469              		.loc 1 1280 3 discriminator 1 view .LVU850
 2470 02ea EFE7     		b	.L135
 2471              		.cfi_endproc
 2472              	.LFE129:
 2474              		.section	.text.HAL_SPI_Receive,"ax",%progbits
 2475              		.align	1
 2476              		.global	HAL_SPI_Receive
 2477              		.syntax unified
 2478              		.thumb
 2479              		.thumb_func
 2481              	HAL_SPI_Receive:
 2482              	.LVL145:
 2483              	.LFB128:
1012:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 2484              		.loc 1 1012 1 is_stmt 1 view -0
 2485              		.cfi_startproc
 2486              		@ args = 0, pretend = 0, frame = 0
 2487              		@ frame_needed = 0, uses_anonymous_args = 0
1012:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 2488              		.loc 1 1012 1 is_stmt 0 view .LVU852
 2489 0000 2DE9F043 		push	{r4, r5, r6, r7, r8, r9, lr}
 2490              		.cfi_def_cfa_offset 28
 2491              		.cfi_offset 4, -28
 2492              		.cfi_offset 5, -24
 2493              		.cfi_offset 6, -20
 2494              		.cfi_offset 7, -16
 2495              		.cfi_offset 8, -12
 2496              		.cfi_offset 9, -8
 2497              		.cfi_offset 14, -4
 2498 0004 83B0     		sub	sp, sp, #12
 2499              		.cfi_def_cfa_offset 40
 2500 0006 0446     		mov	r4, r0
1018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
ARM GAS  /tmp/cc5SiBtg.s 			page 135


 2501              		.loc 1 1018 3 is_stmt 1 view .LVU853
1019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2502              		.loc 1 1019 3 view .LVU854
 2503              	.LVL146:
1021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2504              		.loc 1 1021 3 view .LVU855
1021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2505              		.loc 1 1021 11 is_stmt 0 view .LVU856
 2506 0008 90F85D60 		ldrb	r6, [r0, #93]	@ zero_extendqisi2
 2507 000c F6B2     		uxtb	r6, r6
1021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2508              		.loc 1 1021 6 view .LVU857
 2509 000e 012E     		cmp	r6, #1
 2510 0010 40F0C080 		bne	.L199
 2511 0014 8846     		mov	r8, r1
 2512 0016 9146     		mov	r9, r2
 2513 0018 1D46     		mov	r5, r3
1027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2514              		.loc 1 1027 3 is_stmt 1 view .LVU858
1027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2515              		.loc 1 1027 18 is_stmt 0 view .LVU859
 2516 001a 4368     		ldr	r3, [r0, #4]
 2517              	.LVL147:
1027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2518              		.loc 1 1027 6 view .LVU860
 2519 001c B3F5827F 		cmp	r3, #260
 2520 0020 3DD0     		beq	.L202
 2521              	.L179:
1035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2522              		.loc 1 1035 3 is_stmt 1 view .LVU861
1035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2523              		.loc 1 1035 3 view .LVU862
 2524 0022 94F85C30 		ldrb	r3, [r4, #92]	@ zero_extendqisi2
 2525 0026 012B     		cmp	r3, #1
 2526 0028 00F0BC80 		beq	.L200
1035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2527              		.loc 1 1035 3 discriminator 2 view .LVU863
 2528 002c 0123     		movs	r3, #1
 2529 002e 84F85C30 		strb	r3, [r4, #92]
1035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2530              		.loc 1 1035 3 discriminator 2 view .LVU864
1038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2531              		.loc 1 1038 3 view .LVU865
1038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2532              		.loc 1 1038 15 is_stmt 0 view .LVU866
 2533 0032 FFF7FEFF 		bl	HAL_GetTick
 2534              	.LVL148:
1038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2535              		.loc 1 1038 15 view .LVU867
 2536 0036 0746     		mov	r7, r0
 2537              	.LVL149:
1040:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2538              		.loc 1 1040 3 is_stmt 1 view .LVU868
1040:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2539              		.loc 1 1040 6 is_stmt 0 view .LVU869
 2540 0038 B8F1000F 		cmp	r8, #0
 2541 003c 00F0AB80 		beq	.L178
ARM GAS  /tmp/cc5SiBtg.s 			page 136


1040:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2542              		.loc 1 1040 23 discriminator 1 view .LVU870
 2543 0040 B9F1000F 		cmp	r9, #0
 2544 0044 00F0A780 		beq	.L178
1047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 2545              		.loc 1 1047 3 is_stmt 1 view .LVU871
1047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 2546              		.loc 1 1047 21 is_stmt 0 view .LVU872
 2547 0048 0423     		movs	r3, #4
 2548 004a 84F85D30 		strb	r3, [r4, #93]
1048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 2549              		.loc 1 1048 3 is_stmt 1 view .LVU873
1048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 2550              		.loc 1 1048 21 is_stmt 0 view .LVU874
 2551 004e 0023     		movs	r3, #0
 2552 0050 2366     		str	r3, [r4, #96]
1049:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 2553              		.loc 1 1049 3 is_stmt 1 view .LVU875
1049:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 2554              		.loc 1 1049 21 is_stmt 0 view .LVU876
 2555 0052 C4F84080 		str	r8, [r4, #64]
1050:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 2556              		.loc 1 1050 3 is_stmt 1 view .LVU877
1050:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 2557              		.loc 1 1050 21 is_stmt 0 view .LVU878
 2558 0056 A4F84490 		strh	r9, [r4, #68]	@ movhi
1051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2559              		.loc 1 1051 3 is_stmt 1 view .LVU879
1051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2560              		.loc 1 1051 21 is_stmt 0 view .LVU880
 2561 005a A4F84690 		strh	r9, [r4, #70]	@ movhi
1054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
 2562              		.loc 1 1054 3 is_stmt 1 view .LVU881
1054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
 2563              		.loc 1 1054 21 is_stmt 0 view .LVU882
 2564 005e A363     		str	r3, [r4, #56]
1055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 2565              		.loc 1 1055 3 is_stmt 1 view .LVU883
1055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 2566              		.loc 1 1055 21 is_stmt 0 view .LVU884
 2567 0060 A387     		strh	r3, [r4, #60]	@ movhi
1056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 2568              		.loc 1 1056 3 is_stmt 1 view .LVU885
1056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 2569              		.loc 1 1056 21 is_stmt 0 view .LVU886
 2570 0062 E387     		strh	r3, [r4, #62]	@ movhi
1057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 2571              		.loc 1 1057 3 is_stmt 1 view .LVU887
1057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 2572              		.loc 1 1057 21 is_stmt 0 view .LVU888
 2573 0064 E364     		str	r3, [r4, #76]
1058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2574              		.loc 1 1058 3 is_stmt 1 view .LVU889
1058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2575              		.loc 1 1058 21 is_stmt 0 view .LVU890
 2576 0066 2365     		str	r3, [r4, #80]
1071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 137


 2577              		.loc 1 1071 3 is_stmt 1 view .LVU891
1071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2578              		.loc 1 1071 17 is_stmt 0 view .LVU892
 2579 0068 E368     		ldr	r3, [r4, #12]
1071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2580              		.loc 1 1071 6 view .LVU893
 2581 006a B3F5E06F 		cmp	r3, #1792
 2582 006e 23D9     		bls	.L181
1074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2583              		.loc 1 1074 5 is_stmt 1 view .LVU894
 2584 0070 2268     		ldr	r2, [r4]
 2585 0072 5368     		ldr	r3, [r2, #4]
 2586 0074 23F48053 		bic	r3, r3, #4096
 2587 0078 5360     		str	r3, [r2, #4]
 2588              	.L182:
1083:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2589              		.loc 1 1083 3 view .LVU895
1083:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2590              		.loc 1 1083 17 is_stmt 0 view .LVU896
 2591 007a A368     		ldr	r3, [r4, #8]
1083:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2592              		.loc 1 1083 6 view .LVU897
 2593 007c B3F5004F 		cmp	r3, #32768
 2594 0080 20D0     		beq	.L203
 2595              	.L183:
1091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2596              		.loc 1 1091 3 is_stmt 1 view .LVU898
1091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2597              		.loc 1 1091 12 is_stmt 0 view .LVU899
 2598 0082 2368     		ldr	r3, [r4]
1091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2599              		.loc 1 1091 22 view .LVU900
 2600 0084 1A68     		ldr	r2, [r3]
1091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2601              		.loc 1 1091 6 view .LVU901
 2602 0086 12F0400F 		tst	r2, #64
 2603 008a 03D1     		bne	.L184
1094:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2604              		.loc 1 1094 5 is_stmt 1 view .LVU902
 2605 008c 1A68     		ldr	r2, [r3]
 2606 008e 42F04002 		orr	r2, r2, #64
 2607 0092 1A60     		str	r2, [r3]
 2608              	.L184:
1098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2609              		.loc 1 1098 3 view .LVU903
1098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2610              		.loc 1 1098 17 is_stmt 0 view .LVU904
 2611 0094 E368     		ldr	r3, [r4, #12]
1098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2612              		.loc 1 1098 6 view .LVU905
 2613 0096 B3F5E06F 		cmp	r3, #1792
 2614 009a 27D9     		bls	.L185
 2615 009c 4CE0     		b	.L186
 2616              	.LVL150:
 2617              	.L202:
1027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2618              		.loc 1 1027 58 discriminator 1 view .LVU906
ARM GAS  /tmp/cc5SiBtg.s 			page 138


 2619 009e 8368     		ldr	r3, [r0, #8]
1027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2620              		.loc 1 1027 44 discriminator 1 view .LVU907
 2621 00a0 002B     		cmp	r3, #0
 2622 00a2 BED1     		bne	.L179
1029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
 2623              		.loc 1 1029 5 is_stmt 1 view .LVU908
1029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
 2624              		.loc 1 1029 17 is_stmt 0 view .LVU909
 2625 00a4 0423     		movs	r3, #4
 2626 00a6 80F85D30 		strb	r3, [r0, #93]
1031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2627              		.loc 1 1031 5 is_stmt 1 view .LVU910
1031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2628              		.loc 1 1031 12 is_stmt 0 view .LVU911
 2629 00aa 0095     		str	r5, [sp]
 2630 00ac 1346     		mov	r3, r2
 2631 00ae 0A46     		mov	r2, r1
 2632              	.LVL151:
1031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2633              		.loc 1 1031 12 view .LVU912
 2634 00b0 FFF7FEFF 		bl	HAL_SPI_TransmitReceive
 2635              	.LVL152:
1031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2636              		.loc 1 1031 12 view .LVU913
 2637 00b4 0646     		mov	r6, r0
 2638 00b6 71E0     		b	.L180
 2639              	.LVL153:
 2640              	.L181:
1079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2641              		.loc 1 1079 5 is_stmt 1 view .LVU914
 2642 00b8 2268     		ldr	r2, [r4]
 2643 00ba 5368     		ldr	r3, [r2, #4]
 2644 00bc 43F48053 		orr	r3, r3, #4096
 2645 00c0 5360     		str	r3, [r2, #4]
 2646 00c2 DAE7     		b	.L182
 2647              	.L203:
1086:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
 2648              		.loc 1 1086 5 view .LVU915
 2649 00c4 2268     		ldr	r2, [r4]
 2650 00c6 1368     		ldr	r3, [r2]
 2651 00c8 23F04003 		bic	r3, r3, #64
 2652 00cc 1360     		str	r3, [r2]
1087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2653              		.loc 1 1087 5 view .LVU916
 2654 00ce 2268     		ldr	r2, [r4]
 2655 00d0 1368     		ldr	r3, [r2]
 2656 00d2 23F48043 		bic	r3, r3, #16384
 2657 00d6 1360     		str	r3, [r2]
 2658 00d8 D3E7     		b	.L183
 2659              	.LVL154:
 2660              	.L187:
1114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2661              		.loc 1 1114 9 view .LVU917
1114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2662              		.loc 1 1114 16 is_stmt 0 view .LVU918
 2663 00da FFF7FEFF 		bl	HAL_GetTick
ARM GAS  /tmp/cc5SiBtg.s 			page 139


 2664              	.LVL155:
1114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2665              		.loc 1 1114 30 discriminator 1 view .LVU919
 2666 00de C01B     		subs	r0, r0, r7
1114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2667              		.loc 1 1114 12 discriminator 1 view .LVU920
 2668 00e0 A842     		cmp	r0, r5
 2669 00e2 02D3     		bcc	.L189
1114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2670              		.loc 1 1114 56 discriminator 1 view .LVU921
 2671 00e4 B5F1FF3F 		cmp	r5, #-1
 2672 00e8 18D1     		bne	.L190
 2673              	.L189:
1114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2674              		.loc 1 1114 87 discriminator 3 view .LVU922
 2675 00ea BDB1     		cbz	r5, .L190
 2676              	.L185:
1101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2677              		.loc 1 1101 30 is_stmt 1 view .LVU923
1101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2678              		.loc 1 1101 16 is_stmt 0 view .LVU924
 2679 00ec B4F84630 		ldrh	r3, [r4, #70]
 2680 00f0 9BB2     		uxth	r3, r3
1101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2681              		.loc 1 1101 30 view .LVU925
 2682 00f2 002B     		cmp	r3, #0
 2683 00f4 3FD0     		beq	.L192
1104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2684              		.loc 1 1104 7 is_stmt 1 view .LVU926
1104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2685              		.loc 1 1104 11 is_stmt 0 view .LVU927
 2686 00f6 2368     		ldr	r3, [r4]
 2687 00f8 9A68     		ldr	r2, [r3, #8]
1104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2688              		.loc 1 1104 10 view .LVU928
 2689 00fa 12F0010F 		tst	r2, #1
 2690 00fe ECD0     		beq	.L187
1107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2691              		.loc 1 1107 9 is_stmt 1 view .LVU929
1107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2692              		.loc 1 1107 27 is_stmt 0 view .LVU930
 2693 0100 226C     		ldr	r2, [r4, #64]
1107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2694              		.loc 1 1107 43 view .LVU931
 2695 0102 1B7B     		ldrb	r3, [r3, #12]	@ zero_extendqisi2
1107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2696              		.loc 1 1107 41 view .LVU932
 2697 0104 1370     		strb	r3, [r2]
1108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2698              		.loc 1 1108 9 is_stmt 1 view .LVU933
1108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2699              		.loc 1 1108 13 is_stmt 0 view .LVU934
 2700 0106 236C     		ldr	r3, [r4, #64]
1108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2701              		.loc 1 1108 26 view .LVU935
 2702 0108 0133     		adds	r3, r3, #1
 2703 010a 2364     		str	r3, [r4, #64]
ARM GAS  /tmp/cc5SiBtg.s 			page 140


1109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2704              		.loc 1 1109 9 is_stmt 1 view .LVU936
1109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2705              		.loc 1 1109 13 is_stmt 0 view .LVU937
 2706 010c B4F84630 		ldrh	r3, [r4, #70]
 2707 0110 9BB2     		uxth	r3, r3
1109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2708              		.loc 1 1109 26 view .LVU938
 2709 0112 013B     		subs	r3, r3, #1
 2710 0114 9BB2     		uxth	r3, r3
 2711 0116 A4F84630 		strh	r3, [r4, #70]	@ movhi
 2712 011a E7E7     		b	.L185
 2713              	.L190:
1116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 2714              		.loc 1 1116 11 is_stmt 1 view .LVU939
 2715              	.LVL156:
1117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 2716              		.loc 1 1117 11 view .LVU940
1117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 2717              		.loc 1 1117 23 is_stmt 0 view .LVU941
 2718 011c 0123     		movs	r3, #1
 2719 011e 84F85D30 		strb	r3, [r4, #93]
1118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2720              		.loc 1 1118 11 is_stmt 1 view .LVU942
1116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 2721              		.loc 1 1116 21 is_stmt 0 view .LVU943
 2722 0122 0326     		movs	r6, #3
1118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2723              		.loc 1 1118 11 view .LVU944
 2724 0124 37E0     		b	.L178
 2725              	.LVL157:
 2726              	.L193:
1138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2727              		.loc 1 1138 9 is_stmt 1 view .LVU945
1138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2728              		.loc 1 1138 16 is_stmt 0 view .LVU946
 2729 0126 FFF7FEFF 		bl	HAL_GetTick
 2730              	.LVL158:
1138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2731              		.loc 1 1138 30 discriminator 1 view .LVU947
 2732 012a C01B     		subs	r0, r0, r7
1138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2733              		.loc 1 1138 12 discriminator 1 view .LVU948
 2734 012c A842     		cmp	r0, r5
 2735 012e 02D3     		bcc	.L195
1138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2736              		.loc 1 1138 56 discriminator 1 view .LVU949
 2737 0130 B5F1FF3F 		cmp	r5, #-1
 2738 0134 1AD1     		bne	.L196
 2739              	.L195:
1138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2740              		.loc 1 1138 87 discriminator 3 view .LVU950
 2741 0136 CDB1     		cbz	r5, .L196
 2742              	.L186:
1126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2743              		.loc 1 1126 30 is_stmt 1 view .LVU951
1126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
ARM GAS  /tmp/cc5SiBtg.s 			page 141


 2744              		.loc 1 1126 16 is_stmt 0 view .LVU952
 2745 0138 B4F84630 		ldrh	r3, [r4, #70]
 2746 013c 9BB2     		uxth	r3, r3
1126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2747              		.loc 1 1126 30 view .LVU953
 2748 013e D3B1     		cbz	r3, .L192
1129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2749              		.loc 1 1129 7 is_stmt 1 view .LVU954
1129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2750              		.loc 1 1129 11 is_stmt 0 view .LVU955
 2751 0140 2368     		ldr	r3, [r4]
 2752 0142 9A68     		ldr	r2, [r3, #8]
1129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2753              		.loc 1 1129 10 view .LVU956
 2754 0144 12F0010F 		tst	r2, #1
 2755 0148 EDD0     		beq	.L193
1131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 2756              		.loc 1 1131 9 is_stmt 1 view .LVU957
1131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 2757              		.loc 1 1131 67 is_stmt 0 view .LVU958
 2758 014a DA68     		ldr	r2, [r3, #12]
1131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 2759              		.loc 1 1131 27 view .LVU959
 2760 014c 236C     		ldr	r3, [r4, #64]
1131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 2761              		.loc 1 1131 41 view .LVU960
 2762 014e 1A80     		strh	r2, [r3]	@ movhi
1132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2763              		.loc 1 1132 9 is_stmt 1 view .LVU961
1132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2764              		.loc 1 1132 13 is_stmt 0 view .LVU962
 2765 0150 236C     		ldr	r3, [r4, #64]
1132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2766              		.loc 1 1132 26 view .LVU963
 2767 0152 0233     		adds	r3, r3, #2
 2768 0154 2364     		str	r3, [r4, #64]
1133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2769              		.loc 1 1133 9 is_stmt 1 view .LVU964
1133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2770              		.loc 1 1133 13 is_stmt 0 view .LVU965
 2771 0156 B4F846C0 		ldrh	ip, [r4, #70]
 2772 015a 1FFA8CFC 		uxth	ip, ip
1133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2773              		.loc 1 1133 26 view .LVU966
 2774 015e 0CF1FF3C 		add	ip, ip, #-1
 2775 0162 1FFA8CFC 		uxth	ip, ip
 2776 0166 A4F846C0 		strh	ip, [r4, #70]	@ movhi
 2777 016a E5E7     		b	.L186
 2778              	.L196:
1140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 2779              		.loc 1 1140 11 is_stmt 1 view .LVU967
 2780              	.LVL159:
1141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 2781              		.loc 1 1141 11 view .LVU968
1141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 2782              		.loc 1 1141 23 is_stmt 0 view .LVU969
 2783 016c 0123     		movs	r3, #1
ARM GAS  /tmp/cc5SiBtg.s 			page 142


 2784 016e 84F85D30 		strb	r3, [r4, #93]
1142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2785              		.loc 1 1142 11 is_stmt 1 view .LVU970
1140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 2786              		.loc 1 1140 21 is_stmt 0 view .LVU971
 2787 0172 0326     		movs	r6, #3
1142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2788              		.loc 1 1142 11 view .LVU972
 2789 0174 0FE0     		b	.L178
 2790              	.LVL160:
 2791              	.L192:
1218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2792              		.loc 1 1218 3 is_stmt 1 view .LVU973
1218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2793              		.loc 1 1218 7 is_stmt 0 view .LVU974
 2794 0176 3A46     		mov	r2, r7
 2795 0178 2946     		mov	r1, r5
 2796 017a 2046     		mov	r0, r4
 2797 017c FFF7FEFF 		bl	SPI_EndRxTransaction
 2798              	.LVL161:
1218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2799              		.loc 1 1218 6 discriminator 1 view .LVU975
 2800 0180 08B1     		cbz	r0, .L198
1220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2801              		.loc 1 1220 5 is_stmt 1 view .LVU976
1220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2802              		.loc 1 1220 21 is_stmt 0 view .LVU977
 2803 0182 2023     		movs	r3, #32
 2804 0184 2366     		str	r3, [r4, #96]
 2805              	.L198:
1232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2806              		.loc 1 1232 3 is_stmt 1 view .LVU978
1232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2807              		.loc 1 1232 11 is_stmt 0 view .LVU979
 2808 0186 236E     		ldr	r3, [r4, #96]
1232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2809              		.loc 1 1232 6 view .LVU980
 2810 0188 2BB9     		cbnz	r3, .L178
1238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2811              		.loc 1 1238 5 is_stmt 1 view .LVU981
1238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2812              		.loc 1 1238 17 is_stmt 0 view .LVU982
 2813 018a 0123     		movs	r3, #1
 2814 018c 84F85D30 		strb	r3, [r4, #93]
1019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2815              		.loc 1 1019 21 view .LVU983
 2816 0190 0026     		movs	r6, #0
 2817 0192 00E0     		b	.L178
 2818              	.LVL162:
 2819              	.L199:
1023:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2820              		.loc 1 1023 15 view .LVU984
 2821 0194 0226     		movs	r6, #2
 2822              	.LVL163:
 2823              	.L178:
1242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2824              		.loc 1 1242 3 is_stmt 1 view .LVU985
ARM GAS  /tmp/cc5SiBtg.s 			page 143


1242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2825              		.loc 1 1242 3 view .LVU986
 2826 0196 0023     		movs	r3, #0
 2827 0198 84F85C30 		strb	r3, [r4, #92]
1242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2828              		.loc 1 1242 3 view .LVU987
1243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 2829              		.loc 1 1243 3 view .LVU988
 2830              	.LVL164:
 2831              	.L180:
1244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2832              		.loc 1 1244 1 is_stmt 0 view .LVU989
 2833 019c 3046     		mov	r0, r6
 2834 019e 03B0     		add	sp, sp, #12
 2835              		.cfi_remember_state
 2836              		.cfi_def_cfa_offset 28
 2837              		@ sp needed
 2838 01a0 BDE8F083 		pop	{r4, r5, r6, r7, r8, r9, pc}
 2839              	.LVL165:
 2840              	.L200:
 2841              		.cfi_restore_state
1035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2842              		.loc 1 1035 3 discriminator 1 view .LVU990
 2843 01a4 0226     		movs	r6, #2
 2844 01a6 F9E7     		b	.L180
 2845              		.cfi_endproc
 2846              	.LFE128:
 2848              		.section	.text.HAL_SPI_Transmit_IT,"ax",%progbits
 2849              		.align	1
 2850              		.global	HAL_SPI_Transmit_IT
 2851              		.syntax unified
 2852              		.thumb
 2853              		.thumb_func
 2855              	HAL_SPI_Transmit_IT:
 2856              	.LVL166:
 2857              	.LFB130:
1603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 2858              		.loc 1 1603 1 is_stmt 1 view -0
 2859              		.cfi_startproc
 2860              		@ args = 0, pretend = 0, frame = 0
 2861              		@ frame_needed = 0, uses_anonymous_args = 0
 2862              		@ link register save eliminated.
1604:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2863              		.loc 1 1604 3 view .LVU992
1607:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2864              		.loc 1 1607 3 view .LVU993
1610:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2865              		.loc 1 1610 3 view .LVU994
1610:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2866              		.loc 1 1610 6 is_stmt 0 view .LVU995
 2867 0000 0029     		cmp	r1, #0
 2868 0002 49D0     		beq	.L210
1603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 2869              		.loc 1 1603 1 view .LVU996
 2870 0004 10B4     		push	{r4}
 2871              		.cfi_def_cfa_offset 4
 2872              		.cfi_offset 4, -4
ARM GAS  /tmp/cc5SiBtg.s 			page 144


1610:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2873              		.loc 1 1610 23 discriminator 1 view .LVU997
 2874 0006 002A     		cmp	r2, #0
 2875 0008 48D0     		beq	.L211
1616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2876              		.loc 1 1616 3 is_stmt 1 view .LVU998
1616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2877              		.loc 1 1616 11 is_stmt 0 view .LVU999
 2878 000a 90F85D30 		ldrb	r3, [r0, #93]	@ zero_extendqisi2
 2879 000e DBB2     		uxtb	r3, r3
1616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2880              		.loc 1 1616 6 view .LVU1000
 2881 0010 012B     		cmp	r3, #1
 2882 0012 45D1     		bne	.L212
1623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2883              		.loc 1 1623 3 is_stmt 1 view .LVU1001
1623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2884              		.loc 1 1623 3 view .LVU1002
 2885 0014 90F85C30 		ldrb	r3, [r0, #92]	@ zero_extendqisi2
 2886 0018 012B     		cmp	r3, #1
 2887 001a 43D0     		beq	.L213
1623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2888              		.loc 1 1623 3 discriminator 2 view .LVU1003
 2889 001c 0123     		movs	r3, #1
 2890 001e 80F85C30 		strb	r3, [r0, #92]
1623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2891              		.loc 1 1623 3 discriminator 2 view .LVU1004
1626:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 2892              		.loc 1 1626 3 view .LVU1005
1626:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 2893              		.loc 1 1626 21 is_stmt 0 view .LVU1006
 2894 0022 0323     		movs	r3, #3
 2895 0024 80F85D30 		strb	r3, [r0, #93]
1627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 2896              		.loc 1 1627 3 is_stmt 1 view .LVU1007
1627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 2897              		.loc 1 1627 21 is_stmt 0 view .LVU1008
 2898 0028 0023     		movs	r3, #0
 2899 002a 0366     		str	r3, [r0, #96]
1628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 2900              		.loc 1 1628 3 is_stmt 1 view .LVU1009
1628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 2901              		.loc 1 1628 21 is_stmt 0 view .LVU1010
 2902 002c 8163     		str	r1, [r0, #56]
1629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 2903              		.loc 1 1629 3 is_stmt 1 view .LVU1011
1629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 2904              		.loc 1 1629 21 is_stmt 0 view .LVU1012
 2905 002e 8287     		strh	r2, [r0, #60]	@ movhi
1630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2906              		.loc 1 1630 3 is_stmt 1 view .LVU1013
1630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2907              		.loc 1 1630 21 is_stmt 0 view .LVU1014
 2908 0030 C287     		strh	r2, [r0, #62]	@ movhi
1633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 2909              		.loc 1 1633 3 is_stmt 1 view .LVU1015
1633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
ARM GAS  /tmp/cc5SiBtg.s 			page 145


 2910              		.loc 1 1633 21 is_stmt 0 view .LVU1016
 2911 0032 0364     		str	r3, [r0, #64]
1634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 2912              		.loc 1 1634 3 is_stmt 1 view .LVU1017
1634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 2913              		.loc 1 1634 21 is_stmt 0 view .LVU1018
 2914 0034 A0F84430 		strh	r3, [r0, #68]	@ movhi
1635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 2915              		.loc 1 1635 3 is_stmt 1 view .LVU1019
1635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 2916              		.loc 1 1635 21 is_stmt 0 view .LVU1020
 2917 0038 A0F84630 		strh	r3, [r0, #70]	@ movhi
1636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2918              		.loc 1 1636 3 is_stmt 1 view .LVU1021
1636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2919              		.loc 1 1636 21 is_stmt 0 view .LVU1022
 2920 003c C364     		str	r3, [r0, #76]
1639:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2921              		.loc 1 1639 3 is_stmt 1 view .LVU1023
1639:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2922              		.loc 1 1639 17 is_stmt 0 view .LVU1024
 2923 003e C368     		ldr	r3, [r0, #12]
1639:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2924              		.loc 1 1639 6 view .LVU1025
 2925 0040 B3F5E06F 		cmp	r3, #1792
 2926 0044 1AD9     		bls	.L206
1641:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2927              		.loc 1 1641 5 is_stmt 1 view .LVU1026
1641:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2928              		.loc 1 1641 17 is_stmt 0 view .LVU1027
 2929 0046 184B     		ldr	r3, .L219
 2930 0048 0365     		str	r3, [r0, #80]
 2931              	.L207:
1649:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2932              		.loc 1 1649 3 is_stmt 1 view .LVU1028
1649:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2933              		.loc 1 1649 17 is_stmt 0 view .LVU1029
 2934 004a 8368     		ldr	r3, [r0, #8]
1649:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2935              		.loc 1 1649 6 view .LVU1030
 2936 004c B3F5004F 		cmp	r3, #32768
 2937 0050 17D0     		beq	.L218
 2938              	.LVL167:
 2939              	.L208:
1665:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2940              		.loc 1 1665 3 is_stmt 1 view .LVU1031
1665:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2941              		.loc 1 1665 12 is_stmt 0 view .LVU1032
 2942 0052 0368     		ldr	r3, [r0]
1665:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2943              		.loc 1 1665 22 view .LVU1033
 2944 0054 1A68     		ldr	r2, [r3]
1665:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2945              		.loc 1 1665 6 view .LVU1034
 2946 0056 12F0400F 		tst	r2, #64
 2947 005a 03D1     		bne	.L209
1668:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
ARM GAS  /tmp/cc5SiBtg.s 			page 146


 2948              		.loc 1 1668 5 is_stmt 1 view .LVU1035
 2949 005c 1A68     		ldr	r2, [r3]
 2950 005e 42F04002 		orr	r2, r2, #64
 2951 0062 1A60     		str	r2, [r3]
 2952              	.L209:
1672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable TXE and ERR interrupt */
 2953              		.loc 1 1672 3 view .LVU1036
1672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable TXE and ERR interrupt */
 2954              		.loc 1 1672 3 view .LVU1037
 2955 0064 0023     		movs	r3, #0
 2956 0066 80F85C30 		strb	r3, [r0, #92]
1672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable TXE and ERR interrupt */
 2957              		.loc 1 1672 3 view .LVU1038
1674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2958              		.loc 1 1674 3 view .LVU1039
 2959 006a 0168     		ldr	r1, [r0]
 2960              	.LVL168:
1674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2961              		.loc 1 1674 3 is_stmt 0 view .LVU1040
 2962 006c 4A68     		ldr	r2, [r1, #4]
 2963 006e 42F0A002 		orr	r2, r2, #160
 2964 0072 4A60     		str	r2, [r1, #4]
1604:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2965              		.loc 1 1604 21 view .LVU1041
 2966 0074 1846     		mov	r0, r3
 2967              	.LVL169:
 2968              	.L205:
1678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2969              		.loc 1 1678 1 view .LVU1042
 2970 0076 5DF8044B 		ldr	r4, [sp], #4
 2971              		.cfi_remember_state
 2972              		.cfi_restore 4
 2973              		.cfi_def_cfa_offset 0
 2974 007a 7047     		bx	lr
 2975              	.LVL170:
 2976              	.L206:
 2977              		.cfi_restore_state
1645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2978              		.loc 1 1645 5 is_stmt 1 view .LVU1043
1645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2979              		.loc 1 1645 17 is_stmt 0 view .LVU1044
 2980 007c 0B4B     		ldr	r3, .L219+4
 2981 007e 0365     		str	r3, [r0, #80]
 2982 0080 E3E7     		b	.L207
 2983              	.L218:
1652:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 2984              		.loc 1 1652 5 is_stmt 1 view .LVU1045
 2985 0082 0268     		ldr	r2, [r0]
 2986              	.LVL171:
1652:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 2987              		.loc 1 1652 5 is_stmt 0 view .LVU1046
 2988 0084 1368     		ldr	r3, [r2]
 2989 0086 23F04003 		bic	r3, r3, #64
 2990 008a 1360     		str	r3, [r2]
 2991              	.LVL172:
1653:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2992              		.loc 1 1653 5 is_stmt 1 view .LVU1047
ARM GAS  /tmp/cc5SiBtg.s 			page 147


 2993 008c 0268     		ldr	r2, [r0]
 2994 008e 1368     		ldr	r3, [r2]
 2995 0090 43F48043 		orr	r3, r3, #16384
 2996 0094 1360     		str	r3, [r2]
 2997 0096 DCE7     		b	.L208
 2998              	.LVL173:
 2999              	.L210:
 3000              		.cfi_def_cfa_offset 0
 3001              		.cfi_restore 4
1612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3002              		.loc 1 1612 15 is_stmt 0 view .LVU1048
 3003 0098 0120     		movs	r0, #1
 3004              	.LVL174:
1678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3005              		.loc 1 1678 1 view .LVU1049
 3006 009a 7047     		bx	lr
 3007              	.LVL175:
 3008              	.L211:
 3009              		.cfi_def_cfa_offset 4
 3010              		.cfi_offset 4, -4
1612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3011              		.loc 1 1612 15 view .LVU1050
 3012 009c 0120     		movs	r0, #1
 3013              	.LVL176:
1612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3014              		.loc 1 1612 15 view .LVU1051
 3015 009e EAE7     		b	.L205
 3016              	.LVL177:
 3017              	.L212:
1618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3018              		.loc 1 1618 15 view .LVU1052
 3019 00a0 0220     		movs	r0, #2
 3020              	.LVL178:
1618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3021              		.loc 1 1618 15 view .LVU1053
 3022 00a2 E8E7     		b	.L205
 3023              	.LVL179:
 3024              	.L213:
1623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3025              		.loc 1 1623 3 discriminator 1 view .LVU1054
 3026 00a4 0220     		movs	r0, #2
 3027              	.LVL180:
1623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3028              		.loc 1 1623 3 discriminator 1 view .LVU1055
 3029 00a6 E6E7     		b	.L205
 3030              	.L220:
 3031              		.align	2
 3032              	.L219:
 3033 00a8 00000000 		.word	SPI_TxISR_16BIT
 3034 00ac 00000000 		.word	SPI_TxISR_8BIT
 3035              		.cfi_endproc
 3036              	.LFE130:
 3038              		.section	.text.HAL_SPI_TransmitReceive_IT,"ax",%progbits
 3039              		.align	1
 3040              		.global	HAL_SPI_TransmitReceive_IT
 3041              		.syntax unified
 3042              		.thumb
ARM GAS  /tmp/cc5SiBtg.s 			page 148


 3043              		.thumb_func
 3045              	HAL_SPI_TransmitReceive_IT:
 3046              	.LVL181:
 3047              	.LFB132:
1798:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
 3048              		.loc 1 1798 1 is_stmt 1 view -0
 3049              		.cfi_startproc
 3050              		@ args = 0, pretend = 0, frame = 0
 3051              		@ frame_needed = 0, uses_anonymous_args = 0
 3052              		@ link register save eliminated.
1798:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
 3053              		.loc 1 1798 1 is_stmt 0 view .LVU1057
 3054 0000 10B4     		push	{r4}
 3055              		.cfi_def_cfa_offset 4
 3056              		.cfi_offset 4, -4
1799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_StateTypeDef tmp_state;
 3057              		.loc 1 1799 3 is_stmt 1 view .LVU1058
1800:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef    errorcode = HAL_OK;
 3058              		.loc 1 1800 3 view .LVU1059
1801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3059              		.loc 1 1801 3 view .LVU1060
 3060              	.LVL182:
1804:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3061              		.loc 1 1804 3 view .LVU1061
1807:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
 3062              		.loc 1 1807 3 view .LVU1062
1807:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
 3063              		.loc 1 1807 23 is_stmt 0 view .LVU1063
 3064 0002 90F85DC0 		ldrb	ip, [r0, #93]	@ zero_extendqisi2
 3065 0006 5FFA8CFC 		uxtb	ip, ip
 3066              	.LVL183:
1808:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3067              		.loc 1 1808 3 is_stmt 1 view .LVU1064
1808:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3068              		.loc 1 1808 23 is_stmt 0 view .LVU1065
 3069 000a 4468     		ldr	r4, [r0, #4]
 3070              	.LVL184:
1810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 3071              		.loc 1 1810 3 is_stmt 1 view .LVU1066
1810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 3072              		.loc 1 1810 6 is_stmt 0 view .LVU1067
 3073 000c BCF1010F 		cmp	ip, #1
 3074 0010 08D0     		beq	.L222
1810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 3075              		.loc 1 1810 7 discriminator 1 view .LVU1068
 3076 0012 B4F5827F 		cmp	r4, #260
 3077 0016 54D1     		bne	.L231
1811:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3078              		.loc 1 1811 54 view .LVU1069
 3079 0018 8468     		ldr	r4, [r0, #8]
 3080              	.LVL185:
1811:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3081              		.loc 1 1811 40 view .LVU1070
 3082 001a 002C     		cmp	r4, #0
 3083 001c 55D1     		bne	.L232
1811:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3084              		.loc 1 1811 90 discriminator 1 view .LVU1071
ARM GAS  /tmp/cc5SiBtg.s 			page 149


 3085 001e BCF1040F 		cmp	ip, #4
 3086 0022 54D1     		bne	.L233
 3087              	.L222:
1817:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3088              		.loc 1 1817 3 is_stmt 1 view .LVU1072
1817:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3089              		.loc 1 1817 6 is_stmt 0 view .LVU1073
 3090 0024 0029     		cmp	r1, #0
 3091 0026 54D0     		beq	.L234
1817:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3092              		.loc 1 1817 25 discriminator 1 view .LVU1074
 3093 0028 002A     		cmp	r2, #0
 3094 002a 54D0     		beq	.L235
1817:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3095              		.loc 1 1817 46 discriminator 2 view .LVU1075
 3096 002c 002B     		cmp	r3, #0
 3097 002e 54D0     		beq	.L236
1824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3098              		.loc 1 1824 3 is_stmt 1 view .LVU1076
1824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3099              		.loc 1 1824 3 view .LVU1077
 3100 0030 90F85C40 		ldrb	r4, [r0, #92]	@ zero_extendqisi2
 3101 0034 012C     		cmp	r4, #1
 3102 0036 52D0     		beq	.L237
1824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3103              		.loc 1 1824 3 discriminator 2 view .LVU1078
 3104 0038 0124     		movs	r4, #1
 3105 003a 80F85C40 		strb	r4, [r0, #92]
1824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3106              		.loc 1 1824 3 discriminator 2 view .LVU1079
1827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3107              		.loc 1 1827 3 view .LVU1080
1827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3108              		.loc 1 1827 11 is_stmt 0 view .LVU1081
 3109 003e 90F85D40 		ldrb	r4, [r0, #93]	@ zero_extendqisi2
 3110 0042 E4B2     		uxtb	r4, r4
1827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3111              		.loc 1 1827 6 view .LVU1082
 3112 0044 042C     		cmp	r4, #4
 3113 0046 02D0     		beq	.L224
1829:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3114              		.loc 1 1829 5 is_stmt 1 view .LVU1083
1829:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3115              		.loc 1 1829 17 is_stmt 0 view .LVU1084
 3116 0048 0524     		movs	r4, #5
 3117 004a 80F85D40 		strb	r4, [r0, #93]
 3118              	.L224:
1833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
 3119              		.loc 1 1833 3 is_stmt 1 view .LVU1085
1833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
 3120              		.loc 1 1833 21 is_stmt 0 view .LVU1086
 3121 004e 0024     		movs	r4, #0
 3122 0050 0466     		str	r4, [r0, #96]
1834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3123              		.loc 1 1834 3 is_stmt 1 view .LVU1087
1834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3124              		.loc 1 1834 21 is_stmt 0 view .LVU1088
ARM GAS  /tmp/cc5SiBtg.s 			page 150


 3125 0052 8163     		str	r1, [r0, #56]
1835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3126              		.loc 1 1835 3 is_stmt 1 view .LVU1089
1835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3127              		.loc 1 1835 21 is_stmt 0 view .LVU1090
 3128 0054 8387     		strh	r3, [r0, #60]	@ movhi
1836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 3129              		.loc 1 1836 3 is_stmt 1 view .LVU1091
1836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 3130              		.loc 1 1836 21 is_stmt 0 view .LVU1092
 3131 0056 C387     		strh	r3, [r0, #62]	@ movhi
1837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3132              		.loc 1 1837 3 is_stmt 1 view .LVU1093
1837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3133              		.loc 1 1837 21 is_stmt 0 view .LVU1094
 3134 0058 0264     		str	r2, [r0, #64]
1838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3135              		.loc 1 1838 3 is_stmt 1 view .LVU1095
1838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3136              		.loc 1 1838 21 is_stmt 0 view .LVU1096
 3137 005a A0F84430 		strh	r3, [r0, #68]	@ movhi
1839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3138              		.loc 1 1839 3 is_stmt 1 view .LVU1097
1839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3139              		.loc 1 1839 21 is_stmt 0 view .LVU1098
 3140 005e A0F84630 		strh	r3, [r0, #70]	@ movhi
1842:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3141              		.loc 1 1842 3 is_stmt 1 view .LVU1099
1842:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3142              		.loc 1 1842 17 is_stmt 0 view .LVU1100
 3143 0062 C268     		ldr	r2, [r0, #12]
 3144              	.LVL186:
1842:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3145              		.loc 1 1842 6 view .LVU1101
 3146 0064 B2F5E06F 		cmp	r2, #1792
 3147 0068 20D9     		bls	.L225
1844:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_16BIT;
 3148              		.loc 1 1844 5 is_stmt 1 view .LVU1102
1844:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_16BIT;
 3149              		.loc 1 1844 21 is_stmt 0 view .LVU1103
 3150 006a 1E49     		ldr	r1, .L239
 3151              	.LVL187:
1844:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_16BIT;
 3152              		.loc 1 1844 21 view .LVU1104
 3153 006c C164     		str	r1, [r0, #76]
1845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3154              		.loc 1 1845 5 is_stmt 1 view .LVU1105
1845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3155              		.loc 1 1845 21 is_stmt 0 view .LVU1106
 3156 006e 1E49     		ldr	r1, .L239+4
 3157 0070 0165     		str	r1, [r0, #80]
 3158              	.L226:
1871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3159              		.loc 1 1871 3 is_stmt 1 view .LVU1107
1871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3160              		.loc 1 1871 6 is_stmt 0 view .LVU1108
 3161 0072 B2F5E06F 		cmp	r2, #1792
ARM GAS  /tmp/cc5SiBtg.s 			page 151


 3162 0076 01D8     		bhi	.L227
1871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3163              		.loc 1 1871 49 discriminator 1 view .LVU1109
 3164 0078 012B     		cmp	r3, #1
 3165 007a 1CD9     		bls	.L228
 3166              	.L227:
1874:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3167              		.loc 1 1874 5 is_stmt 1 view .LVU1110
 3168 007c 0268     		ldr	r2, [r0]
 3169 007e 5368     		ldr	r3, [r2, #4]
 3170              	.LVL188:
1874:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3171              		.loc 1 1874 5 is_stmt 0 view .LVU1111
 3172 0080 23F48053 		bic	r3, r3, #4096
 3173 0084 5360     		str	r3, [r2, #4]
 3174              	.LVL189:
 3175              	.L229:
1884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3176              		.loc 1 1884 3 is_stmt 1 view .LVU1112
1884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3177              		.loc 1 1884 12 is_stmt 0 view .LVU1113
 3178 0086 0368     		ldr	r3, [r0]
1884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3179              		.loc 1 1884 22 view .LVU1114
 3180 0088 1A68     		ldr	r2, [r3]
1884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3181              		.loc 1 1884 6 view .LVU1115
 3182 008a 12F0400F 		tst	r2, #64
 3183 008e 03D1     		bne	.L230
1887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3184              		.loc 1 1887 5 is_stmt 1 view .LVU1116
 3185 0090 1A68     		ldr	r2, [r3]
 3186 0092 42F04002 		orr	r2, r2, #64
 3187 0096 1A60     		str	r2, [r3]
 3188              	.L230:
1891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable TXE, RXNE and ERR interrupt */
 3189              		.loc 1 1891 3 view .LVU1117
1891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable TXE, RXNE and ERR interrupt */
 3190              		.loc 1 1891 3 view .LVU1118
 3191 0098 0023     		movs	r3, #0
 3192 009a 80F85C30 		strb	r3, [r0, #92]
1891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable TXE, RXNE and ERR interrupt */
 3193              		.loc 1 1891 3 view .LVU1119
1893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3194              		.loc 1 1893 3 view .LVU1120
 3195 009e 0168     		ldr	r1, [r0]
 3196 00a0 4A68     		ldr	r2, [r1, #4]
 3197 00a2 42F0E002 		orr	r2, r2, #224
 3198 00a6 4A60     		str	r2, [r1, #4]
1801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3199              		.loc 1 1801 24 is_stmt 0 view .LVU1121
 3200 00a8 1846     		mov	r0, r3
 3201              	.LVL190:
1801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3202              		.loc 1 1801 24 view .LVU1122
 3203 00aa 0BE0     		b	.L223
 3204              	.LVL191:
ARM GAS  /tmp/cc5SiBtg.s 			page 152


 3205              	.L225:
1849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_8BIT;
 3206              		.loc 1 1849 5 is_stmt 1 view .LVU1123
1849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_8BIT;
 3207              		.loc 1 1849 21 is_stmt 0 view .LVU1124
 3208 00ac 0F49     		ldr	r1, .L239+8
 3209              	.LVL192:
1849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_8BIT;
 3210              		.loc 1 1849 21 view .LVU1125
 3211 00ae C164     		str	r1, [r0, #76]
1850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3212              		.loc 1 1850 5 is_stmt 1 view .LVU1126
1850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3213              		.loc 1 1850 21 is_stmt 0 view .LVU1127
 3214 00b0 0F49     		ldr	r1, .L239+12
 3215 00b2 0165     		str	r1, [r0, #80]
 3216 00b4 DDE7     		b	.L226
 3217              	.L228:
1879:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3218              		.loc 1 1879 5 is_stmt 1 view .LVU1128
 3219 00b6 0268     		ldr	r2, [r0]
 3220 00b8 5368     		ldr	r3, [r2, #4]
 3221              	.LVL193:
1879:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3222              		.loc 1 1879 5 is_stmt 0 view .LVU1129
 3223 00ba 43F48053 		orr	r3, r3, #4096
 3224 00be 5360     		str	r3, [r2, #4]
 3225              	.LVL194:
1879:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3226              		.loc 1 1879 5 view .LVU1130
 3227 00c0 E1E7     		b	.L229
 3228              	.LVL195:
 3229              	.L231:
1813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3230              		.loc 1 1813 15 view .LVU1131
 3231 00c2 0220     		movs	r0, #2
 3232              	.LVL196:
 3233              	.L223:
1897:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3234              		.loc 1 1897 1 view .LVU1132
 3235 00c4 5DF8044B 		ldr	r4, [sp], #4
 3236              		.cfi_remember_state
 3237              		.cfi_restore 4
 3238              		.cfi_def_cfa_offset 0
 3239 00c8 7047     		bx	lr
 3240              	.LVL197:
 3241              	.L232:
 3242              		.cfi_restore_state
1813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3243              		.loc 1 1813 15 view .LVU1133
 3244 00ca 0220     		movs	r0, #2
 3245              	.LVL198:
1813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3246              		.loc 1 1813 15 view .LVU1134
 3247 00cc FAE7     		b	.L223
 3248              	.LVL199:
 3249              	.L233:
ARM GAS  /tmp/cc5SiBtg.s 			page 153


1813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3250              		.loc 1 1813 15 view .LVU1135
 3251 00ce 0220     		movs	r0, #2
 3252              	.LVL200:
1813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3253              		.loc 1 1813 15 view .LVU1136
 3254 00d0 F8E7     		b	.L223
 3255              	.LVL201:
 3256              	.L234:
1819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3257              		.loc 1 1819 15 view .LVU1137
 3258 00d2 0120     		movs	r0, #1
 3259              	.LVL202:
1819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3260              		.loc 1 1819 15 view .LVU1138
 3261 00d4 F6E7     		b	.L223
 3262              	.LVL203:
 3263              	.L235:
1819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3264              		.loc 1 1819 15 view .LVU1139
 3265 00d6 0120     		movs	r0, #1
 3266              	.LVL204:
1819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3267              		.loc 1 1819 15 view .LVU1140
 3268 00d8 F4E7     		b	.L223
 3269              	.LVL205:
 3270              	.L236:
1819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3271              		.loc 1 1819 15 view .LVU1141
 3272 00da 0120     		movs	r0, #1
 3273              	.LVL206:
1819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3274              		.loc 1 1819 15 view .LVU1142
 3275 00dc F2E7     		b	.L223
 3276              	.LVL207:
 3277              	.L237:
1824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3278              		.loc 1 1824 3 discriminator 1 view .LVU1143
 3279 00de 0220     		movs	r0, #2
 3280              	.LVL208:
1824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3281              		.loc 1 1824 3 discriminator 1 view .LVU1144
 3282 00e0 F0E7     		b	.L223
 3283              	.L240:
 3284 00e2 00BF     		.align	2
 3285              	.L239:
 3286 00e4 00000000 		.word	SPI_2linesRxISR_16BIT
 3287 00e8 00000000 		.word	SPI_2linesTxISR_16BIT
 3288 00ec 00000000 		.word	SPI_2linesRxISR_8BIT
 3289 00f0 00000000 		.word	SPI_2linesTxISR_8BIT
 3290              		.cfi_endproc
 3291              	.LFE132:
 3293              		.section	.text.HAL_SPI_Receive_IT,"ax",%progbits
 3294              		.align	1
 3295              		.global	HAL_SPI_Receive_IT
 3296              		.syntax unified
 3297              		.thumb
ARM GAS  /tmp/cc5SiBtg.s 			page 154


 3298              		.thumb_func
 3300              	HAL_SPI_Receive_IT:
 3301              	.LVL209:
 3302              	.LFB131:
1689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 3303              		.loc 1 1689 1 is_stmt 1 view -0
 3304              		.cfi_startproc
 3305              		@ args = 0, pretend = 0, frame = 0
 3306              		@ frame_needed = 0, uses_anonymous_args = 0
1689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 3307              		.loc 1 1689 1 is_stmt 0 view .LVU1146
 3308 0000 8446     		mov	ip, r0
1690:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3309              		.loc 1 1690 3 is_stmt 1 view .LVU1147
 3310              	.LVL210:
1693:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3311              		.loc 1 1693 3 view .LVU1148
1693:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3312              		.loc 1 1693 11 is_stmt 0 view .LVU1149
 3313 0002 90F85D00 		ldrb	r0, [r0, #93]	@ zero_extendqisi2
 3314              	.LVL211:
1693:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3315              		.loc 1 1693 11 view .LVU1150
 3316 0006 C0B2     		uxtb	r0, r0
1693:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3317              		.loc 1 1693 6 view .LVU1151
 3318 0008 0128     		cmp	r0, #1
 3319 000a 6ED1     		bne	.L248
1689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 3320              		.loc 1 1689 1 view .LVU1152
 3321 000c 08B5     		push	{r3, lr}
 3322              		.cfi_def_cfa_offset 8
 3323              		.cfi_offset 3, -8
 3324              		.cfi_offset 14, -4
1699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3325              		.loc 1 1699 3 is_stmt 1 view .LVU1153
1699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3326              		.loc 1 1699 18 is_stmt 0 view .LVU1154
 3327 000e DCF80830 		ldr	r3, [ip, #8]
1699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3328              		.loc 1 1699 6 view .LVU1155
 3329 0012 23B9     		cbnz	r3, .L243
1699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3330              		.loc 1 1699 68 discriminator 1 view .LVU1156
 3331 0014 DCF80430 		ldr	r3, [ip, #4]
1699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3332              		.loc 1 1699 54 discriminator 1 view .LVU1157
 3333 0018 B3F5827F 		cmp	r3, #260
 3334 001c 45D0     		beq	.L254
 3335              	.L243:
1707:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3336              		.loc 1 1707 3 is_stmt 1 view .LVU1158
1707:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3337              		.loc 1 1707 6 is_stmt 0 view .LVU1159
 3338 001e 0029     		cmp	r1, #0
 3339 0020 42D0     		beq	.L242
1707:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 155


 3340              		.loc 1 1707 23 discriminator 1 view .LVU1160
 3341 0022 002A     		cmp	r2, #0
 3342 0024 40D0     		beq	.L242
1714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3343              		.loc 1 1714 3 is_stmt 1 view .LVU1161
1714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3344              		.loc 1 1714 3 view .LVU1162
 3345 0026 9CF85C30 		ldrb	r3, [ip, #92]	@ zero_extendqisi2
 3346 002a 012B     		cmp	r3, #1
 3347 002c 5FD0     		beq	.L249
1714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3348              		.loc 1 1714 3 discriminator 2 view .LVU1163
 3349 002e 0123     		movs	r3, #1
 3350 0030 8CF85C30 		strb	r3, [ip, #92]
1714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3351              		.loc 1 1714 3 discriminator 2 view .LVU1164
1717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3352              		.loc 1 1717 3 view .LVU1165
1717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3353              		.loc 1 1717 21 is_stmt 0 view .LVU1166
 3354 0034 0423     		movs	r3, #4
 3355 0036 8CF85D30 		strb	r3, [ip, #93]
1718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 3356              		.loc 1 1718 3 is_stmt 1 view .LVU1167
1718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 3357              		.loc 1 1718 21 is_stmt 0 view .LVU1168
 3358 003a 0023     		movs	r3, #0
 3359 003c CCF86030 		str	r3, [ip, #96]
1719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3360              		.loc 1 1719 3 is_stmt 1 view .LVU1169
1719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3361              		.loc 1 1719 21 is_stmt 0 view .LVU1170
 3362 0040 CCF84010 		str	r1, [ip, #64]
1720:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3363              		.loc 1 1720 3 is_stmt 1 view .LVU1171
1720:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3364              		.loc 1 1720 21 is_stmt 0 view .LVU1172
 3365 0044 ACF84420 		strh	r2, [ip, #68]	@ movhi
1721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3366              		.loc 1 1721 3 is_stmt 1 view .LVU1173
1721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3367              		.loc 1 1721 21 is_stmt 0 view .LVU1174
 3368 0048 ACF84620 		strh	r2, [ip, #70]	@ movhi
1724:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
 3369              		.loc 1 1724 3 is_stmt 1 view .LVU1175
1724:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
 3370              		.loc 1 1724 21 is_stmt 0 view .LVU1176
 3371 004c CCF83830 		str	r3, [ip, #56]
1725:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 3372              		.loc 1 1725 3 is_stmt 1 view .LVU1177
1725:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 3373              		.loc 1 1725 21 is_stmt 0 view .LVU1178
 3374 0050 ACF83C30 		strh	r3, [ip, #60]	@ movhi
1726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3375              		.loc 1 1726 3 is_stmt 1 view .LVU1179
1726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3376              		.loc 1 1726 21 is_stmt 0 view .LVU1180
ARM GAS  /tmp/cc5SiBtg.s 			page 156


 3377 0054 ACF83E30 		strh	r3, [ip, #62]	@ movhi
1727:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3378              		.loc 1 1727 3 is_stmt 1 view .LVU1181
1727:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3379              		.loc 1 1727 21 is_stmt 0 view .LVU1182
 3380 0058 CCF85030 		str	r3, [ip, #80]
1730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3381              		.loc 1 1730 3 is_stmt 1 view .LVU1183
1730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3382              		.loc 1 1730 17 is_stmt 0 view .LVU1184
 3383 005c DCF80C30 		ldr	r3, [ip, #12]
1730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3384              		.loc 1 1730 6 view .LVU1185
 3385 0060 B3F5E06F 		cmp	r3, #1792
 3386 0064 2AD9     		bls	.L244
1733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_16BIT;
 3387              		.loc 1 1733 5 is_stmt 1 view .LVU1186
 3388 0066 DCF80020 		ldr	r2, [ip]
 3389              	.LVL212:
1733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_16BIT;
 3390              		.loc 1 1733 5 is_stmt 0 view .LVU1187
 3391 006a 5368     		ldr	r3, [r2, #4]
 3392 006c 23F48053 		bic	r3, r3, #4096
 3393 0070 5360     		str	r3, [r2, #4]
 3394              	.LVL213:
1734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3395              		.loc 1 1734 5 is_stmt 1 view .LVU1188
1734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3396              		.loc 1 1734 17 is_stmt 0 view .LVU1189
 3397 0072 204B     		ldr	r3, .L256
 3398 0074 CCF84C30 		str	r3, [ip, #76]
 3399              	.L245:
1744:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3400              		.loc 1 1744 3 is_stmt 1 view .LVU1190
1744:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3401              		.loc 1 1744 17 is_stmt 0 view .LVU1191
 3402 0078 DCF80830 		ldr	r3, [ip, #8]
1744:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3403              		.loc 1 1744 6 view .LVU1192
 3404 007c B3F5004F 		cmp	r3, #32768
 3405 0080 26D0     		beq	.L255
 3406              	.L246:
1773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3407              		.loc 1 1773 3 is_stmt 1 view .LVU1193
1773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3408              		.loc 1 1773 12 is_stmt 0 view .LVU1194
 3409 0082 DCF80030 		ldr	r3, [ip]
1773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3410              		.loc 1 1773 22 view .LVU1195
 3411 0086 1A68     		ldr	r2, [r3]
1773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3412              		.loc 1 1773 6 view .LVU1196
 3413 0088 12F0400F 		tst	r2, #64
 3414 008c 03D1     		bne	.L247
1776:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3415              		.loc 1 1776 5 is_stmt 1 view .LVU1197
 3416 008e 1A68     		ldr	r2, [r3]
ARM GAS  /tmp/cc5SiBtg.s 			page 157


 3417 0090 42F04002 		orr	r2, r2, #64
 3418 0094 1A60     		str	r2, [r3]
 3419              	.L247:
1780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable RXNE and ERR interrupt */
 3420              		.loc 1 1780 3 view .LVU1198
1780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable RXNE and ERR interrupt */
 3421              		.loc 1 1780 3 view .LVU1199
 3422 0096 0020     		movs	r0, #0
 3423 0098 8CF85C00 		strb	r0, [ip, #92]
1780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable RXNE and ERR interrupt */
 3424              		.loc 1 1780 3 view .LVU1200
1782:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3425              		.loc 1 1782 3 view .LVU1201
 3426 009c DCF80020 		ldr	r2, [ip]
 3427 00a0 5368     		ldr	r3, [r2, #4]
 3428 00a2 43F06003 		orr	r3, r3, #96
 3429 00a6 5360     		str	r3, [r2, #4]
 3430              	.LVL214:
 3431              	.L242:
1786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3432              		.loc 1 1786 1 is_stmt 0 view .LVU1202
 3433 00a8 08BD     		pop	{r3, pc}
 3434              	.LVL215:
 3435              	.L254:
1701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
 3436              		.loc 1 1701 5 is_stmt 1 view .LVU1203
1701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
 3437              		.loc 1 1701 17 is_stmt 0 view .LVU1204
 3438 00aa 0423     		movs	r3, #4
 3439 00ac 8CF85D30 		strb	r3, [ip, #93]
1703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3440              		.loc 1 1703 5 is_stmt 1 view .LVU1205
1703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3441              		.loc 1 1703 12 is_stmt 0 view .LVU1206
 3442 00b0 1346     		mov	r3, r2
 3443 00b2 0A46     		mov	r2, r1
 3444              	.LVL216:
1703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3445              		.loc 1 1703 12 view .LVU1207
 3446 00b4 6046     		mov	r0, ip
 3447 00b6 FFF7FEFF 		bl	HAL_SPI_TransmitReceive_IT
 3448              	.LVL217:
1703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3449              		.loc 1 1703 12 view .LVU1208
 3450 00ba F5E7     		b	.L242
 3451              	.LVL218:
 3452              	.L244:
1739:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_8BIT;
 3453              		.loc 1 1739 5 is_stmt 1 view .LVU1209
 3454 00bc DCF80020 		ldr	r2, [ip]
 3455              	.LVL219:
1739:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_8BIT;
 3456              		.loc 1 1739 5 is_stmt 0 view .LVU1210
 3457 00c0 5368     		ldr	r3, [r2, #4]
 3458 00c2 43F48053 		orr	r3, r3, #4096
 3459 00c6 5360     		str	r3, [r2, #4]
 3460              	.LVL220:
ARM GAS  /tmp/cc5SiBtg.s 			page 158


1740:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3461              		.loc 1 1740 5 is_stmt 1 view .LVU1211
1740:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3462              		.loc 1 1740 17 is_stmt 0 view .LVU1212
 3463 00c8 0B4B     		ldr	r3, .L256+4
 3464 00ca CCF84C30 		str	r3, [ip, #76]
 3465 00ce D3E7     		b	.L245
 3466              	.L255:
1747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
 3467              		.loc 1 1747 5 is_stmt 1 view .LVU1213
 3468 00d0 DCF80020 		ldr	r2, [ip]
 3469 00d4 1368     		ldr	r3, [r2]
 3470 00d6 23F04003 		bic	r3, r3, #64
 3471 00da 1360     		str	r3, [r2]
1748:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3472              		.loc 1 1748 5 view .LVU1214
 3473 00dc DCF80020 		ldr	r2, [ip]
 3474 00e0 1368     		ldr	r3, [r2]
 3475 00e2 23F48043 		bic	r3, r3, #16384
 3476 00e6 1360     		str	r3, [r2]
 3477 00e8 CBE7     		b	.L246
 3478              	.LVL221:
 3479              	.L248:
 3480              		.cfi_def_cfa_offset 0
 3481              		.cfi_restore 3
 3482              		.cfi_restore 14
1695:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3483              		.loc 1 1695 15 is_stmt 0 view .LVU1215
 3484 00ea 0220     		movs	r0, #2
 3485              	.LVL222:
1786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3486              		.loc 1 1786 1 view .LVU1216
 3487 00ec 7047     		bx	lr
 3488              	.LVL223:
 3489              	.L249:
 3490              		.cfi_def_cfa_offset 8
 3491              		.cfi_offset 3, -8
 3492              		.cfi_offset 14, -4
1714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3493              		.loc 1 1714 3 discriminator 1 view .LVU1217
 3494 00ee 0220     		movs	r0, #2
 3495 00f0 DAE7     		b	.L242
 3496              	.L257:
 3497 00f2 00BF     		.align	2
 3498              	.L256:
 3499 00f4 00000000 		.word	SPI_RxISR_16BIT
 3500 00f8 00000000 		.word	SPI_RxISR_8BIT
 3501              		.cfi_endproc
 3502              	.LFE131:
 3504              		.section	.text.HAL_SPI_Transmit_DMA,"ax",%progbits
 3505              		.align	1
 3506              		.global	HAL_SPI_Transmit_DMA
 3507              		.syntax unified
 3508              		.thumb
 3509              		.thumb_func
 3511              	HAL_SPI_Transmit_DMA:
 3512              	.LVL224:
ARM GAS  /tmp/cc5SiBtg.s 			page 159


 3513              	.LFB133:
1908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 3514              		.loc 1 1908 1 is_stmt 1 view -0
 3515              		.cfi_startproc
 3516              		@ args = 0, pretend = 0, frame = 0
 3517              		@ frame_needed = 0, uses_anonymous_args = 0
1908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 3518              		.loc 1 1908 1 is_stmt 0 view .LVU1219
 3519 0000 38B5     		push	{r3, r4, r5, lr}
 3520              		.cfi_def_cfa_offset 16
 3521              		.cfi_offset 3, -16
 3522              		.cfi_offset 4, -12
 3523              		.cfi_offset 5, -8
 3524              		.cfi_offset 14, -4
1909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3525              		.loc 1 1909 3 is_stmt 1 view .LVU1220
 3526              	.LVL225:
1912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3527              		.loc 1 1912 3 view .LVU1221
1915:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3528              		.loc 1 1915 3 view .LVU1222
1918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3529              		.loc 1 1918 3 view .LVU1223
1918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3530              		.loc 1 1918 3 view .LVU1224
 3531 0002 90F85C30 		ldrb	r3, [r0, #92]	@ zero_extendqisi2
 3532 0006 012B     		cmp	r3, #1
 3533 0008 00F08980 		beq	.L266
 3534 000c 0446     		mov	r4, r0
1918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3535              		.loc 1 1918 3 discriminator 2 view .LVU1225
 3536 000e 0123     		movs	r3, #1
 3537 0010 80F85C30 		strb	r3, [r0, #92]
1918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3538              		.loc 1 1918 3 discriminator 2 view .LVU1226
1920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3539              		.loc 1 1920 3 view .LVU1227
1920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3540              		.loc 1 1920 11 is_stmt 0 view .LVU1228
 3541 0014 90F85D50 		ldrb	r5, [r0, #93]	@ zero_extendqisi2
 3542 0018 EDB2     		uxtb	r5, r5
1920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3543              		.loc 1 1920 6 view .LVU1229
 3544 001a 9D42     		cmp	r5, r3
 3545 001c 79D1     		bne	.L267
1926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3546              		.loc 1 1926 3 is_stmt 1 view .LVU1230
1926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3547              		.loc 1 1926 6 is_stmt 0 view .LVU1231
 3548 001e 0029     		cmp	r1, #0
 3549 0020 78D0     		beq	.L260
1926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3550              		.loc 1 1926 23 discriminator 1 view .LVU1232
 3551 0022 002A     		cmp	r2, #0
 3552 0024 76D0     		beq	.L260
1933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3553              		.loc 1 1933 3 is_stmt 1 view .LVU1233
ARM GAS  /tmp/cc5SiBtg.s 			page 160


1933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3554              		.loc 1 1933 21 is_stmt 0 view .LVU1234
 3555 0026 0323     		movs	r3, #3
 3556 0028 80F85D30 		strb	r3, [r0, #93]
1934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 3557              		.loc 1 1934 3 is_stmt 1 view .LVU1235
1934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 3558              		.loc 1 1934 21 is_stmt 0 view .LVU1236
 3559 002c 0023     		movs	r3, #0
 3560 002e 0366     		str	r3, [r0, #96]
1935:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3561              		.loc 1 1935 3 is_stmt 1 view .LVU1237
1935:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3562              		.loc 1 1935 21 is_stmt 0 view .LVU1238
 3563 0030 8163     		str	r1, [r0, #56]
1936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3564              		.loc 1 1936 3 is_stmt 1 view .LVU1239
1936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3565              		.loc 1 1936 21 is_stmt 0 view .LVU1240
 3566 0032 8287     		strh	r2, [r0, #60]	@ movhi
1937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3567              		.loc 1 1937 3 is_stmt 1 view .LVU1241
1937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3568              		.loc 1 1937 21 is_stmt 0 view .LVU1242
 3569 0034 C287     		strh	r2, [r0, #62]	@ movhi
1940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3570              		.loc 1 1940 3 is_stmt 1 view .LVU1243
1940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3571              		.loc 1 1940 21 is_stmt 0 view .LVU1244
 3572 0036 0364     		str	r3, [r0, #64]
1941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 3573              		.loc 1 1941 3 is_stmt 1 view .LVU1245
1941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 3574              		.loc 1 1941 21 is_stmt 0 view .LVU1246
 3575 0038 0365     		str	r3, [r0, #80]
1942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 3576              		.loc 1 1942 3 is_stmt 1 view .LVU1247
1942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 3577              		.loc 1 1942 21 is_stmt 0 view .LVU1248
 3578 003a C364     		str	r3, [r0, #76]
1943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 3579              		.loc 1 1943 3 is_stmt 1 view .LVU1249
1943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 3580              		.loc 1 1943 21 is_stmt 0 view .LVU1250
 3581 003c A0F84430 		strh	r3, [r0, #68]	@ movhi
1944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3582              		.loc 1 1944 3 is_stmt 1 view .LVU1251
1944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3583              		.loc 1 1944 21 is_stmt 0 view .LVU1252
 3584 0040 A0F84630 		strh	r3, [r0, #70]	@ movhi
1947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3585              		.loc 1 1947 3 is_stmt 1 view .LVU1253
1947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3586              		.loc 1 1947 17 is_stmt 0 view .LVU1254
 3587 0044 8368     		ldr	r3, [r0, #8]
1947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3588              		.loc 1 1947 6 view .LVU1255
ARM GAS  /tmp/cc5SiBtg.s 			page 161


 3589 0046 B3F5004F 		cmp	r3, #32768
 3590 004a 39D0     		beq	.L269
 3591              	.LVL226:
 3592              	.L261:
1963:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3593              		.loc 1 1963 3 is_stmt 1 view .LVU1256
1963:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3594              		.loc 1 1963 7 is_stmt 0 view .LVU1257
 3595 004c 636D     		ldr	r3, [r4, #84]
1963:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3596              		.loc 1 1963 38 view .LVU1258
 3597 004e 354A     		ldr	r2, .L272
 3598 0050 DA62     		str	r2, [r3, #44]
1966:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3599              		.loc 1 1966 3 is_stmt 1 view .LVU1259
1966:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3600              		.loc 1 1966 7 is_stmt 0 view .LVU1260
 3601 0052 636D     		ldr	r3, [r4, #84]
1966:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3602              		.loc 1 1966 34 view .LVU1261
 3603 0054 344A     		ldr	r2, .L272+4
 3604 0056 9A62     		str	r2, [r3, #40]
1969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3605              		.loc 1 1969 3 is_stmt 1 view .LVU1262
1969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3606              		.loc 1 1969 7 is_stmt 0 view .LVU1263
 3607 0058 636D     		ldr	r3, [r4, #84]
1969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3608              		.loc 1 1969 35 view .LVU1264
 3609 005a 344A     		ldr	r2, .L272+8
 3610 005c 1A63     		str	r2, [r3, #48]
1972:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3611              		.loc 1 1972 3 is_stmt 1 view .LVU1265
1972:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3612              		.loc 1 1972 7 is_stmt 0 view .LVU1266
 3613 005e 636D     		ldr	r3, [r4, #84]
1972:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3614              		.loc 1 1972 35 view .LVU1267
 3615 0060 0022     		movs	r2, #0
 3616 0062 5A63     		str	r2, [r3, #52]
1974:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Packing mode is enabled only if the DMA setting is HALWORD */
 3617              		.loc 1 1974 3 is_stmt 1 view .LVU1268
 3618 0064 2268     		ldr	r2, [r4]
 3619 0066 5368     		ldr	r3, [r2, #4]
 3620 0068 23F48043 		bic	r3, r3, #16384
 3621 006c 5360     		str	r3, [r2, #4]
1976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3622              		.loc 1 1976 3 view .LVU1269
1976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3623              		.loc 1 1976 18 is_stmt 0 view .LVU1270
 3624 006e E368     		ldr	r3, [r4, #12]
1976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3625              		.loc 1 1976 6 view .LVU1271
 3626 0070 B3F5E06F 		cmp	r3, #1792
 3627 0074 04D8     		bhi	.L262
1976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3628              		.loc 1 1976 58 discriminator 1 view .LVU1272
ARM GAS  /tmp/cc5SiBtg.s 			page 162


 3629 0076 636D     		ldr	r3, [r4, #84]
1976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3630              		.loc 1 1976 72 discriminator 1 view .LVU1273
 3631 0078 5B69     		ldr	r3, [r3, #20]
1976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3632              		.loc 1 1976 50 discriminator 1 view .LVU1274
 3633 007a B3F5806F 		cmp	r3, #1024
 3634 007e 2AD0     		beq	.L270
 3635              	.L262:
1992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 3636              		.loc 1 1992 3 is_stmt 1 view .LVU1275
1992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 3637              		.loc 1 1992 91 is_stmt 0 view .LVU1276
 3638 0080 2268     		ldr	r2, [r4]
1993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3639              		.loc 1 1993 38 view .LVU1277
 3640 0082 E38F     		ldrh	r3, [r4, #62]
1992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 3641              		.loc 1 1992 17 view .LVU1278
 3642 0084 9BB2     		uxth	r3, r3
 3643 0086 0C32     		adds	r2, r2, #12
 3644 0088 A16B     		ldr	r1, [r4, #56]
 3645              	.LVL227:
1992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 3646              		.loc 1 1992 17 view .LVU1279
 3647 008a 606D     		ldr	r0, [r4, #84]
 3648              	.LVL228:
1992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 3649              		.loc 1 1992 17 view .LVU1280
 3650 008c FFF7FEFF 		bl	HAL_DMA_Start_IT
 3651              	.LVL229:
1992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 3652              		.loc 1 1992 6 discriminator 1 view .LVU1281
 3653 0090 0146     		mov	r1, r0
 3654 0092 0028     		cmp	r0, #0
 3655 0094 38D1     		bne	.L271
2003:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3656              		.loc 1 2003 3 is_stmt 1 view .LVU1282
2003:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3657              		.loc 1 2003 12 is_stmt 0 view .LVU1283
 3658 0096 2368     		ldr	r3, [r4]
2003:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3659              		.loc 1 2003 22 view .LVU1284
 3660 0098 1A68     		ldr	r2, [r3]
2003:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3661              		.loc 1 2003 6 view .LVU1285
 3662 009a 12F0400F 		tst	r2, #64
 3663 009e 03D1     		bne	.L265
2006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3664              		.loc 1 2006 5 is_stmt 1 view .LVU1286
 3665 00a0 1A68     		ldr	r2, [r3]
 3666 00a2 42F04002 		orr	r2, r2, #64
 3667 00a6 1A60     		str	r2, [r3]
 3668              	.L265:
2010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3669              		.loc 1 2010 3 view .LVU1287
 3670 00a8 2268     		ldr	r2, [r4]
ARM GAS  /tmp/cc5SiBtg.s 			page 163


 3671 00aa 5368     		ldr	r3, [r2, #4]
 3672 00ac 43F02003 		orr	r3, r3, #32
 3673 00b0 5360     		str	r3, [r2, #4]
2013:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3674              		.loc 1 2013 3 view .LVU1288
 3675 00b2 2268     		ldr	r2, [r4]
 3676 00b4 5368     		ldr	r3, [r2, #4]
 3677 00b6 43F00203 		orr	r3, r3, #2
 3678 00ba 5360     		str	r3, [r2, #4]
1909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3679              		.loc 1 1909 21 is_stmt 0 view .LVU1289
 3680 00bc 0D46     		mov	r5, r1
 3681 00be 29E0     		b	.L260
 3682              	.LVL230:
 3683              	.L269:
1950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 3684              		.loc 1 1950 5 is_stmt 1 view .LVU1290
 3685 00c0 0268     		ldr	r2, [r0]
 3686              	.LVL231:
1950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 3687              		.loc 1 1950 5 is_stmt 0 view .LVU1291
 3688 00c2 1368     		ldr	r3, [r2]
 3689 00c4 23F04003 		bic	r3, r3, #64
 3690 00c8 1360     		str	r3, [r2]
 3691              	.LVL232:
1951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3692              		.loc 1 1951 5 is_stmt 1 view .LVU1292
 3693 00ca 0268     		ldr	r2, [r0]
 3694 00cc 1368     		ldr	r3, [r2]
 3695 00ce 43F48043 		orr	r3, r3, #16384
 3696 00d2 1360     		str	r3, [r2]
 3697 00d4 BAE7     		b	.L261
 3698              	.L270:
1979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3699              		.loc 1 1979 5 view .LVU1293
1979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3700              		.loc 1 1979 14 is_stmt 0 view .LVU1294
 3701 00d6 E38F     		ldrh	r3, [r4, #62]
1979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3702              		.loc 1 1979 8 view .LVU1295
 3703 00d8 13F0010F 		tst	r3, #1
 3704 00dc 09D1     		bne	.L263
1981:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount >> 1U);
 3705              		.loc 1 1981 7 is_stmt 1 view .LVU1296
 3706 00de 2268     		ldr	r2, [r4]
 3707 00e0 5368     		ldr	r3, [r2, #4]
 3708 00e2 23F48043 		bic	r3, r3, #16384
 3709 00e6 5360     		str	r3, [r2, #4]
1982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3710              		.loc 1 1982 7 view .LVU1297
1982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3711              		.loc 1 1982 32 is_stmt 0 view .LVU1298
 3712 00e8 E38F     		ldrh	r3, [r4, #62]
1982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3713              		.loc 1 1982 25 view .LVU1299
 3714 00ea C3F34E03 		ubfx	r3, r3, #1, #15
 3715 00ee E387     		strh	r3, [r4, #62]	@ movhi
ARM GAS  /tmp/cc5SiBtg.s 			page 164


 3716 00f0 C6E7     		b	.L262
 3717              	.L263:
1986:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount >> 1U) + 1U;
 3718              		.loc 1 1986 7 is_stmt 1 view .LVU1300
 3719 00f2 2268     		ldr	r2, [r4]
 3720 00f4 5368     		ldr	r3, [r2, #4]
 3721 00f6 43F48043 		orr	r3, r3, #16384
 3722 00fa 5360     		str	r3, [r2, #4]
1987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3723              		.loc 1 1987 7 view .LVU1301
1987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3724              		.loc 1 1987 32 is_stmt 0 view .LVU1302
 3725 00fc E38F     		ldrh	r3, [r4, #62]
1987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3726              		.loc 1 1987 53 view .LVU1303
 3727 00fe C3F34E03 		ubfx	r3, r3, #1, #15
 3728 0102 0133     		adds	r3, r3, #1
1987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3729              		.loc 1 1987 25 view .LVU1304
 3730 0104 E387     		strh	r3, [r4, #62]	@ movhi
 3731 0106 BBE7     		b	.L262
 3732              	.LVL233:
 3733              	.L271:
1996:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
 3734              		.loc 1 1996 5 is_stmt 1 view .LVU1305
 3735 0108 236E     		ldr	r3, [r4, #96]
 3736 010a 43F01003 		orr	r3, r3, #16
 3737 010e 2366     		str	r3, [r4, #96]
1997:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3738              		.loc 1 1997 5 view .LVU1306
 3739              	.LVL234:
1999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3740              		.loc 1 1999 5 view .LVU1307
 3741 0110 00E0     		b	.L260
 3742              	.LVL235:
 3743              	.L267:
1922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3744              		.loc 1 1922 15 is_stmt 0 view .LVU1308
 3745 0112 0225     		movs	r5, #2
 3746              	.LVL236:
 3747              	.L260:
2017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 3748              		.loc 1 2017 3 is_stmt 1 view .LVU1309
2017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 3749              		.loc 1 2017 3 view .LVU1310
 3750 0114 0023     		movs	r3, #0
 3751 0116 84F85C30 		strb	r3, [r4, #92]
2017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 3752              		.loc 1 2017 3 view .LVU1311
2018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 3753              		.loc 1 2018 3 view .LVU1312
 3754              	.LVL237:
 3755              	.L259:
2019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3756              		.loc 1 2019 1 is_stmt 0 view .LVU1313
 3757 011a 2846     		mov	r0, r5
 3758 011c 38BD     		pop	{r3, r4, r5, pc}
ARM GAS  /tmp/cc5SiBtg.s 			page 165


 3759              	.LVL238:
 3760              	.L266:
1918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3761              		.loc 1 1918 3 discriminator 1 view .LVU1314
 3762 011e 0225     		movs	r5, #2
 3763 0120 FBE7     		b	.L259
 3764              	.L273:
 3765 0122 00BF     		.align	2
 3766              	.L272:
 3767 0124 00000000 		.word	SPI_DMAHalfTransmitCplt
 3768 0128 00000000 		.word	SPI_DMATransmitCplt
 3769 012c 00000000 		.word	SPI_DMAError
 3770              		.cfi_endproc
 3771              	.LFE133:
 3773              		.section	.text.HAL_SPI_TransmitReceive_DMA,"ax",%progbits
 3774              		.align	1
 3775              		.global	HAL_SPI_TransmitReceive_DMA
 3776              		.syntax unified
 3777              		.thumb
 3778              		.thumb_func
 3780              	HAL_SPI_TransmitReceive_DMA:
 3781              	.LVL239:
 3782              	.LFB135:
2186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
 3783              		.loc 1 2186 1 is_stmt 1 view -0
 3784              		.cfi_startproc
 3785              		@ args = 0, pretend = 0, frame = 0
 3786              		@ frame_needed = 0, uses_anonymous_args = 0
2186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
 3787              		.loc 1 2186 1 is_stmt 0 view .LVU1316
 3788 0000 38B5     		push	{r3, r4, r5, lr}
 3789              		.cfi_def_cfa_offset 16
 3790              		.cfi_offset 3, -16
 3791              		.cfi_offset 4, -12
 3792              		.cfi_offset 5, -8
 3793              		.cfi_offset 14, -4
 3794 0002 0446     		mov	r4, r0
2187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_StateTypeDef tmp_state;
 3795              		.loc 1 2187 3 is_stmt 1 view .LVU1317
2188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 3796              		.loc 1 2188 3 view .LVU1318
2189:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3797              		.loc 1 2189 3 view .LVU1319
 3798              	.LVL240:
2192:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DMA_HANDLE(hspi->hdmatx));
 3799              		.loc 1 2192 3 view .LVU1320
2193:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3800              		.loc 1 2193 3 view .LVU1321
2196:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3801              		.loc 1 2196 3 view .LVU1322
2199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3802              		.loc 1 2199 3 view .LVU1323
2199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3803              		.loc 1 2199 3 view .LVU1324
 3804 0004 90F85C00 		ldrb	r0, [r0, #92]	@ zero_extendqisi2
 3805              	.LVL241:
2199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 166


 3806              		.loc 1 2199 3 is_stmt 0 view .LVU1325
 3807 0008 0128     		cmp	r0, #1
 3808 000a 00F0F380 		beq	.L289
2199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3809              		.loc 1 2199 3 is_stmt 1 discriminator 2 view .LVU1326
 3810 000e 0120     		movs	r0, #1
 3811 0010 84F85C00 		strb	r0, [r4, #92]
2199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3812              		.loc 1 2199 3 discriminator 2 view .LVU1327
2202:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
 3813              		.loc 1 2202 3 view .LVU1328
2202:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
 3814              		.loc 1 2202 23 is_stmt 0 view .LVU1329
 3815 0014 94F85D00 		ldrb	r0, [r4, #93]	@ zero_extendqisi2
 3816 0018 C0B2     		uxtb	r0, r0
 3817              	.LVL242:
2203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3818              		.loc 1 2203 3 is_stmt 1 view .LVU1330
2203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3819              		.loc 1 2203 23 is_stmt 0 view .LVU1331
 3820 001a 6568     		ldr	r5, [r4, #4]
 3821              	.LVL243:
2205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 3822              		.loc 1 2205 3 is_stmt 1 view .LVU1332
2205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 3823              		.loc 1 2205 6 is_stmt 0 view .LVU1333
 3824 001c 0128     		cmp	r0, #1
 3825 001e 0AD0     		beq	.L276
2205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 3826              		.loc 1 2205 7 discriminator 1 view .LVU1334
 3827 0020 B5F5827F 		cmp	r5, #260
 3828 0024 40F0D780 		bne	.L290
2206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3829              		.loc 1 2206 54 view .LVU1335
 3830 0028 A568     		ldr	r5, [r4, #8]
 3831              	.LVL244:
2206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3832              		.loc 1 2206 40 view .LVU1336
 3833 002a 002D     		cmp	r5, #0
 3834 002c 40F0D880 		bne	.L291
2206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3835              		.loc 1 2206 90 discriminator 1 view .LVU1337
 3836 0030 0428     		cmp	r0, #4
 3837 0032 40F0D780 		bne	.L292
 3838              	.L276:
2212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3839              		.loc 1 2212 3 is_stmt 1 view .LVU1338
2212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3840              		.loc 1 2212 6 is_stmt 0 view .LVU1339
 3841 0036 0029     		cmp	r1, #0
 3842 0038 00F0D680 		beq	.L293
2212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3843              		.loc 1 2212 25 discriminator 1 view .LVU1340
 3844 003c 002A     		cmp	r2, #0
 3845 003e 00F0D580 		beq	.L294
2212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3846              		.loc 1 2212 46 discriminator 2 view .LVU1341
ARM GAS  /tmp/cc5SiBtg.s 			page 167


 3847 0042 002B     		cmp	r3, #0
 3848 0044 00F0D480 		beq	.L295
2219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3849              		.loc 1 2219 3 is_stmt 1 view .LVU1342
2219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3850              		.loc 1 2219 11 is_stmt 0 view .LVU1343
 3851 0048 94F85D00 		ldrb	r0, [r4, #93]	@ zero_extendqisi2
 3852              	.LVL245:
2219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3853              		.loc 1 2219 11 view .LVU1344
 3854 004c C0B2     		uxtb	r0, r0
2219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3855              		.loc 1 2219 6 view .LVU1345
 3856 004e 0428     		cmp	r0, #4
 3857 0050 02D0     		beq	.L278
2221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3858              		.loc 1 2221 5 is_stmt 1 view .LVU1346
2221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3859              		.loc 1 2221 17 is_stmt 0 view .LVU1347
 3860 0052 0520     		movs	r0, #5
 3861 0054 84F85D00 		strb	r0, [r4, #93]
 3862              	.L278:
2225:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
 3863              		.loc 1 2225 3 is_stmt 1 view .LVU1348
2225:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
 3864              		.loc 1 2225 21 is_stmt 0 view .LVU1349
 3865 0058 0020     		movs	r0, #0
 3866 005a 2066     		str	r0, [r4, #96]
2226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3867              		.loc 1 2226 3 is_stmt 1 view .LVU1350
2226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3868              		.loc 1 2226 21 is_stmt 0 view .LVU1351
 3869 005c A163     		str	r1, [r4, #56]
2227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3870              		.loc 1 2227 3 is_stmt 1 view .LVU1352
2227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3871              		.loc 1 2227 21 is_stmt 0 view .LVU1353
 3872 005e A387     		strh	r3, [r4, #60]	@ movhi
2228:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 3873              		.loc 1 2228 3 is_stmt 1 view .LVU1354
2228:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 3874              		.loc 1 2228 21 is_stmt 0 view .LVU1355
 3875 0060 E387     		strh	r3, [r4, #62]	@ movhi
2229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3876              		.loc 1 2229 3 is_stmt 1 view .LVU1356
2229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3877              		.loc 1 2229 21 is_stmt 0 view .LVU1357
 3878 0062 2264     		str	r2, [r4, #64]
2230:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3879              		.loc 1 2230 3 is_stmt 1 view .LVU1358
2230:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3880              		.loc 1 2230 21 is_stmt 0 view .LVU1359
 3881 0064 A4F84430 		strh	r3, [r4, #68]	@ movhi
2231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3882              		.loc 1 2231 3 is_stmt 1 view .LVU1360
2231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3883              		.loc 1 2231 21 is_stmt 0 view .LVU1361
ARM GAS  /tmp/cc5SiBtg.s 			page 168


 3884 0068 A4F84630 		strh	r3, [r4, #70]	@ movhi
2234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3885              		.loc 1 2234 3 is_stmt 1 view .LVU1362
2234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3886              		.loc 1 2234 21 is_stmt 0 view .LVU1363
 3887 006c E064     		str	r0, [r4, #76]
2235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3888              		.loc 1 2235 3 is_stmt 1 view .LVU1364
2235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3889              		.loc 1 2235 21 is_stmt 0 view .LVU1365
 3890 006e 2065     		str	r0, [r4, #80]
2256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3891              		.loc 1 2256 3 is_stmt 1 view .LVU1366
 3892 0070 2268     		ldr	r2, [r4]
 3893              	.LVL246:
2256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3894              		.loc 1 2256 3 is_stmt 0 view .LVU1367
 3895 0072 5368     		ldr	r3, [r2, #4]
 3896              	.LVL247:
2256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3897              		.loc 1 2256 3 view .LVU1368
 3898 0074 23F4C043 		bic	r3, r3, #24576
 3899 0078 5360     		str	r3, [r2, #4]
 3900              	.LVL248:
2259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3901              		.loc 1 2259 3 is_stmt 1 view .LVU1369
2259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3902              		.loc 1 2259 17 is_stmt 0 view .LVU1370
 3903 007a E368     		ldr	r3, [r4, #12]
2259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3904              		.loc 1 2259 6 view .LVU1371
 3905 007c B3F5E06F 		cmp	r3, #1792
 3906 0080 26D9     		bls	.L279
2262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3907              		.loc 1 2262 5 is_stmt 1 view .LVU1372
 3908 0082 2268     		ldr	r2, [r4]
 3909 0084 5368     		ldr	r3, [r2, #4]
 3910 0086 23F48053 		bic	r3, r3, #4096
 3911 008a 5360     		str	r3, [r2, #4]
 3912              	.L280:
2302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3913              		.loc 1 2302 3 view .LVU1373
2302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3914              		.loc 1 2302 11 is_stmt 0 view .LVU1374
 3915 008c 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 3916 0090 DBB2     		uxtb	r3, r3
2302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3917              		.loc 1 2302 6 view .LVU1375
 3918 0092 042B     		cmp	r3, #4
 3919 0094 67D0     		beq	.L297
2311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMATransmitReceiveCplt;
 3920              		.loc 1 2311 5 is_stmt 1 view .LVU1376
2311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMATransmitReceiveCplt;
 3921              		.loc 1 2311 9 is_stmt 0 view .LVU1377
 3922 0096 A36D     		ldr	r3, [r4, #88]
2311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMATransmitReceiveCplt;
 3923              		.loc 1 2311 40 view .LVU1378
ARM GAS  /tmp/cc5SiBtg.s 			page 169


 3924 0098 574A     		ldr	r2, .L300
 3925 009a DA62     		str	r2, [r3, #44]
2312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3926              		.loc 1 2312 5 is_stmt 1 view .LVU1379
2312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3927              		.loc 1 2312 9 is_stmt 0 view .LVU1380
 3928 009c A36D     		ldr	r3, [r4, #88]
2312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3929              		.loc 1 2312 40 view .LVU1381
 3930 009e 574A     		ldr	r2, .L300+4
 3931 00a0 9A62     		str	r2, [r3, #40]
 3932              	.L285:
2316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3933              		.loc 1 2316 3 is_stmt 1 view .LVU1382
2316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3934              		.loc 1 2316 7 is_stmt 0 view .LVU1383
 3935 00a2 A36D     		ldr	r3, [r4, #88]
2316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3936              		.loc 1 2316 35 view .LVU1384
 3937 00a4 564A     		ldr	r2, .L300+8
 3938 00a6 1A63     		str	r2, [r3, #48]
2319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3939              		.loc 1 2319 3 is_stmt 1 view .LVU1385
2319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3940              		.loc 1 2319 7 is_stmt 0 view .LVU1386
 3941 00a8 A36D     		ldr	r3, [r4, #88]
2319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3942              		.loc 1 2319 35 view .LVU1387
 3943 00aa 0022     		movs	r2, #0
 3944 00ac 5A63     		str	r2, [r3, #52]
2322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 3945              		.loc 1 2322 3 is_stmt 1 view .LVU1388
2322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 3946              		.loc 1 2322 63 is_stmt 0 view .LVU1389
 3947 00ae 2168     		ldr	r1, [r4]
 3948              	.LVL249:
2323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3949              		.loc 1 2323 38 view .LVU1390
 3950 00b0 B4F84630 		ldrh	r3, [r4, #70]
2322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 3951              		.loc 1 2322 17 view .LVU1391
 3952 00b4 9BB2     		uxth	r3, r3
 3953 00b6 226C     		ldr	r2, [r4, #64]
 3954 00b8 0C31     		adds	r1, r1, #12
 3955 00ba A06D     		ldr	r0, [r4, #88]
 3956 00bc FFF7FEFF 		bl	HAL_DMA_Start_IT
 3957              	.LVL250:
2322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 3958              		.loc 1 2322 6 discriminator 1 view .LVU1392
 3959 00c0 0028     		cmp	r0, #0
 3960 00c2 57D0     		beq	.L286
2326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
 3961              		.loc 1 2326 5 is_stmt 1 view .LVU1393
 3962 00c4 236E     		ldr	r3, [r4, #96]
 3963 00c6 43F01003 		orr	r3, r3, #16
 3964 00ca 2366     		str	r3, [r4, #96]
2327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 170


 3965              		.loc 1 2327 5 view .LVU1394
 3966              	.LVL251:
2329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3967              		.loc 1 2329 5 view .LVU1395
2327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3968              		.loc 1 2327 15 is_stmt 0 view .LVU1396
 3969 00cc 0120     		movs	r0, #1
2329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3970              		.loc 1 2329 5 view .LVU1397
 3971 00ce 83E0     		b	.L277
 3972              	.LVL252:
 3973              	.L279:
2267:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3974              		.loc 1 2267 5 is_stmt 1 view .LVU1398
 3975 00d0 2268     		ldr	r2, [r4]
 3976 00d2 5368     		ldr	r3, [r2, #4]
 3977 00d4 43F48053 		orr	r3, r3, #4096
 3978 00d8 5360     		str	r3, [r2, #4]
2269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3979              		.loc 1 2269 5 view .LVU1399
2269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3980              		.loc 1 2269 13 is_stmt 0 view .LVU1400
 3981 00da 636D     		ldr	r3, [r4, #84]
2269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3982              		.loc 1 2269 27 view .LVU1401
 3983 00dc 5B69     		ldr	r3, [r3, #20]
2269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3984              		.loc 1 2269 8 view .LVU1402
 3985 00de B3F5806F 		cmp	r3, #1024
 3986 00e2 1AD0     		beq	.L298
 3987              	.L281:
2283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3988              		.loc 1 2283 5 is_stmt 1 view .LVU1403
2283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3989              		.loc 1 2283 13 is_stmt 0 view .LVU1404
 3990 00e4 A36D     		ldr	r3, [r4, #88]
2283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3991              		.loc 1 2283 27 view .LVU1405
 3992 00e6 5B69     		ldr	r3, [r3, #20]
2283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3993              		.loc 1 2283 8 view .LVU1406
 3994 00e8 B3F5806F 		cmp	r3, #1024
 3995 00ec CED1     		bne	.L280
2286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3996              		.loc 1 2286 7 is_stmt 1 view .LVU1407
 3997 00ee 2268     		ldr	r2, [r4]
 3998 00f0 5368     		ldr	r3, [r2, #4]
 3999 00f2 23F48053 		bic	r3, r3, #4096
 4000 00f6 5360     		str	r3, [r2, #4]
2288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4001              		.loc 1 2288 7 view .LVU1408
2288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4002              		.loc 1 2288 16 is_stmt 0 view .LVU1409
 4003 00f8 B4F84630 		ldrh	r3, [r4, #70]
2288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4004              		.loc 1 2288 10 view .LVU1410
 4005 00fc 13F0010F 		tst	r3, #1
ARM GAS  /tmp/cc5SiBtg.s 			page 171


 4006 0100 24D1     		bne	.L283
2290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = hspi->RxXferCount >> 1U;
 4007              		.loc 1 2290 9 is_stmt 1 view .LVU1411
 4008 0102 2268     		ldr	r2, [r4]
 4009 0104 5368     		ldr	r3, [r2, #4]
 4010 0106 23F40053 		bic	r3, r3, #8192
 4011 010a 5360     		str	r3, [r2, #4]
2291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4012              		.loc 1 2291 9 view .LVU1412
2291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4013              		.loc 1 2291 33 is_stmt 0 view .LVU1413
 4014 010c B4F84630 		ldrh	r3, [r4, #70]
2291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4015              		.loc 1 2291 27 view .LVU1414
 4016 0110 C3F34E03 		ubfx	r3, r3, #1, #15
 4017 0114 A4F84630 		strh	r3, [r4, #70]	@ movhi
 4018 0118 B8E7     		b	.L280
 4019              	.L298:
2271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4020              		.loc 1 2271 7 is_stmt 1 view .LVU1415
2271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4021              		.loc 1 2271 16 is_stmt 0 view .LVU1416
 4022 011a A38F     		ldrh	r3, [r4, #60]
2271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4023              		.loc 1 2271 10 view .LVU1417
 4024 011c 13F0010F 		tst	r3, #1
 4025 0120 09D1     		bne	.L282
2273:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount = hspi->TxXferCount >> 1U;
 4026              		.loc 1 2273 9 is_stmt 1 view .LVU1418
 4027 0122 2268     		ldr	r2, [r4]
 4028 0124 5368     		ldr	r3, [r2, #4]
 4029 0126 23F48043 		bic	r3, r3, #16384
 4030 012a 5360     		str	r3, [r2, #4]
2274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4031              		.loc 1 2274 9 view .LVU1419
2274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4032              		.loc 1 2274 33 is_stmt 0 view .LVU1420
 4033 012c E38F     		ldrh	r3, [r4, #62]
2274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4034              		.loc 1 2274 27 view .LVU1421
 4035 012e C3F34E03 		ubfx	r3, r3, #1, #15
 4036 0132 E387     		strh	r3, [r4, #62]	@ movhi
 4037 0134 D6E7     		b	.L281
 4038              	.L282:
2278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount = (hspi->TxXferCount >> 1U) + 1U;
 4039              		.loc 1 2278 9 is_stmt 1 view .LVU1422
 4040 0136 2268     		ldr	r2, [r4]
 4041 0138 5368     		ldr	r3, [r2, #4]
 4042 013a 43F48043 		orr	r3, r3, #16384
 4043 013e 5360     		str	r3, [r2, #4]
2279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4044              		.loc 1 2279 9 view .LVU1423
2279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4045              		.loc 1 2279 34 is_stmt 0 view .LVU1424
 4046 0140 E38F     		ldrh	r3, [r4, #62]
2279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4047              		.loc 1 2279 55 view .LVU1425
ARM GAS  /tmp/cc5SiBtg.s 			page 172


 4048 0142 C3F34E03 		ubfx	r3, r3, #1, #15
 4049 0146 0133     		adds	r3, r3, #1
2279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4050              		.loc 1 2279 27 view .LVU1426
 4051 0148 E387     		strh	r3, [r4, #62]	@ movhi
 4052 014a CBE7     		b	.L281
 4053              	.L283:
2295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = (hspi->RxXferCount >> 1U) + 1U;
 4054              		.loc 1 2295 9 is_stmt 1 view .LVU1427
 4055 014c 2268     		ldr	r2, [r4]
 4056 014e 5368     		ldr	r3, [r2, #4]
 4057 0150 43F40053 		orr	r3, r3, #8192
 4058 0154 5360     		str	r3, [r2, #4]
2296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4059              		.loc 1 2296 9 view .LVU1428
2296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4060              		.loc 1 2296 34 is_stmt 0 view .LVU1429
 4061 0156 B4F84630 		ldrh	r3, [r4, #70]
2296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4062              		.loc 1 2296 55 view .LVU1430
 4063 015a C3F34E03 		ubfx	r3, r3, #1, #15
 4064 015e 0133     		adds	r3, r3, #1
2296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4065              		.loc 1 2296 27 view .LVU1431
 4066 0160 A4F84630 		strh	r3, [r4, #70]	@ movhi
 4067 0164 92E7     		b	.L280
 4068              	.L297:
2305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMAReceiveCplt;
 4069              		.loc 1 2305 5 is_stmt 1 view .LVU1432
2305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMAReceiveCplt;
 4070              		.loc 1 2305 9 is_stmt 0 view .LVU1433
 4071 0166 A36D     		ldr	r3, [r4, #88]
2305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMAReceiveCplt;
 4072              		.loc 1 2305 40 view .LVU1434
 4073 0168 264A     		ldr	r2, .L300+12
 4074 016a DA62     		str	r2, [r3, #44]
2306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4075              		.loc 1 2306 5 is_stmt 1 view .LVU1435
2306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4076              		.loc 1 2306 9 is_stmt 0 view .LVU1436
 4077 016c A36D     		ldr	r3, [r4, #88]
2306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4078              		.loc 1 2306 40 view .LVU1437
 4079 016e 264A     		ldr	r2, .L300+16
 4080 0170 9A62     		str	r2, [r3, #40]
 4081 0172 96E7     		b	.L285
 4082              	.LVL253:
 4083              	.L286:
2333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4084              		.loc 1 2333 3 is_stmt 1 view .LVU1438
 4085 0174 2268     		ldr	r2, [r4]
 4086 0176 5368     		ldr	r3, [r2, #4]
 4087 0178 43F00103 		orr	r3, r3, #1
 4088 017c 5360     		str	r3, [r2, #4]
2337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback     = NULL;
 4089              		.loc 1 2337 3 view .LVU1439
2337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback     = NULL;
ARM GAS  /tmp/cc5SiBtg.s 			page 173


 4090              		.loc 1 2337 7 is_stmt 0 view .LVU1440
 4091 017e 626D     		ldr	r2, [r4, #84]
2337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback     = NULL;
 4092              		.loc 1 2337 38 view .LVU1441
 4093 0180 0023     		movs	r3, #0
 4094 0182 D362     		str	r3, [r2, #44]
2338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferErrorCallback    = NULL;
 4095              		.loc 1 2338 3 is_stmt 1 view .LVU1442
2338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferErrorCallback    = NULL;
 4096              		.loc 1 2338 7 is_stmt 0 view .LVU1443
 4097 0184 626D     		ldr	r2, [r4, #84]
2338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferErrorCallback    = NULL;
 4098              		.loc 1 2338 38 view .LVU1444
 4099 0186 9362     		str	r3, [r2, #40]
2339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback    = NULL;
 4100              		.loc 1 2339 3 is_stmt 1 view .LVU1445
2339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback    = NULL;
 4101              		.loc 1 2339 7 is_stmt 0 view .LVU1446
 4102 0188 626D     		ldr	r2, [r4, #84]
2339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback    = NULL;
 4103              		.loc 1 2339 38 view .LVU1447
 4104 018a 1363     		str	r3, [r2, #48]
2340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4105              		.loc 1 2340 3 is_stmt 1 view .LVU1448
2340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4106              		.loc 1 2340 7 is_stmt 0 view .LVU1449
 4107 018c 626D     		ldr	r2, [r4, #84]
2340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4108              		.loc 1 2340 38 view .LVU1450
 4109 018e 5363     		str	r3, [r2, #52]
2343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 4110              		.loc 1 2343 3 is_stmt 1 view .LVU1451
2343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 4111              		.loc 1 2343 91 is_stmt 0 view .LVU1452
 4112 0190 2268     		ldr	r2, [r4]
2344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4113              		.loc 1 2344 38 view .LVU1453
 4114 0192 E38F     		ldrh	r3, [r4, #62]
2343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 4115              		.loc 1 2343 17 view .LVU1454
 4116 0194 9BB2     		uxth	r3, r3
 4117 0196 0C32     		adds	r2, r2, #12
 4118 0198 A16B     		ldr	r1, [r4, #56]
 4119 019a 606D     		ldr	r0, [r4, #84]
 4120 019c FFF7FEFF 		bl	HAL_DMA_Start_IT
 4121              	.LVL254:
2343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 4122              		.loc 1 2343 6 discriminator 1 view .LVU1455
 4123 01a0 98B9     		cbnz	r0, .L299
2354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4124              		.loc 1 2354 3 is_stmt 1 view .LVU1456
2354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4125              		.loc 1 2354 12 is_stmt 0 view .LVU1457
 4126 01a2 2368     		ldr	r3, [r4]
2354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4127              		.loc 1 2354 22 view .LVU1458
 4128 01a4 1A68     		ldr	r2, [r3]
ARM GAS  /tmp/cc5SiBtg.s 			page 174


2354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4129              		.loc 1 2354 6 view .LVU1459
 4130 01a6 12F0400F 		tst	r2, #64
 4131 01aa 03D1     		bne	.L288
2357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4132              		.loc 1 2357 5 is_stmt 1 view .LVU1460
 4133 01ac 1A68     		ldr	r2, [r3]
 4134 01ae 42F04002 		orr	r2, r2, #64
 4135 01b2 1A60     		str	r2, [r3]
 4136              	.L288:
2360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4137              		.loc 1 2360 3 view .LVU1461
 4138 01b4 2268     		ldr	r2, [r4]
 4139 01b6 5368     		ldr	r3, [r2, #4]
 4140 01b8 43F02003 		orr	r3, r3, #32
 4141 01bc 5360     		str	r3, [r2, #4]
2363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4142              		.loc 1 2363 3 view .LVU1462
 4143 01be 2268     		ldr	r2, [r4]
 4144 01c0 5368     		ldr	r3, [r2, #4]
 4145 01c2 43F00203 		orr	r3, r3, #2
 4146 01c6 5360     		str	r3, [r2, #4]
 4147 01c8 06E0     		b	.L277
 4148              	.L299:
2347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
 4149              		.loc 1 2347 5 view .LVU1463
 4150 01ca 236E     		ldr	r3, [r4, #96]
 4151 01cc 43F01003 		orr	r3, r3, #16
 4152 01d0 2366     		str	r3, [r4, #96]
2348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4153              		.loc 1 2348 5 view .LVU1464
 4154              	.LVL255:
2350:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4155              		.loc 1 2350 5 view .LVU1465
2348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4156              		.loc 1 2348 15 is_stmt 0 view .LVU1466
 4157 01d2 0120     		movs	r0, #1
2350:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4158              		.loc 1 2350 5 view .LVU1467
 4159 01d4 00E0     		b	.L277
 4160              	.LVL256:
 4161              	.L290:
2208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4162              		.loc 1 2208 15 view .LVU1468
 4163 01d6 0220     		movs	r0, #2
 4164              	.LVL257:
 4165              	.L277:
2367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 4166              		.loc 1 2367 3 is_stmt 1 view .LVU1469
2367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 4167              		.loc 1 2367 3 view .LVU1470
 4168 01d8 0023     		movs	r3, #0
 4169 01da 84F85C30 		strb	r3, [r4, #92]
2367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 4170              		.loc 1 2367 3 view .LVU1471
2368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4171              		.loc 1 2368 3 view .LVU1472
ARM GAS  /tmp/cc5SiBtg.s 			page 175


 4172              	.LVL258:
 4173              	.L275:
2369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4174              		.loc 1 2369 1 is_stmt 0 view .LVU1473
 4175 01de 38BD     		pop	{r3, r4, r5, pc}
 4176              	.LVL259:
 4177              	.L291:
2208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4178              		.loc 1 2208 15 view .LVU1474
 4179 01e0 0220     		movs	r0, #2
 4180              	.LVL260:
2208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4181              		.loc 1 2208 15 view .LVU1475
 4182 01e2 F9E7     		b	.L277
 4183              	.LVL261:
 4184              	.L292:
2208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4185              		.loc 1 2208 15 view .LVU1476
 4186 01e4 0220     		movs	r0, #2
 4187              	.LVL262:
2208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4188              		.loc 1 2208 15 view .LVU1477
 4189 01e6 F7E7     		b	.L277
 4190              	.LVL263:
 4191              	.L293:
2214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4192              		.loc 1 2214 15 view .LVU1478
 4193 01e8 0120     		movs	r0, #1
 4194              	.LVL264:
2214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4195              		.loc 1 2214 15 view .LVU1479
 4196 01ea F5E7     		b	.L277
 4197              	.LVL265:
 4198              	.L294:
2214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4199              		.loc 1 2214 15 view .LVU1480
 4200 01ec 0120     		movs	r0, #1
 4201              	.LVL266:
2214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4202              		.loc 1 2214 15 view .LVU1481
 4203 01ee F3E7     		b	.L277
 4204              	.LVL267:
 4205              	.L295:
2214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4206              		.loc 1 2214 15 view .LVU1482
 4207 01f0 0120     		movs	r0, #1
 4208              	.LVL268:
2214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4209              		.loc 1 2214 15 view .LVU1483
 4210 01f2 F1E7     		b	.L277
 4211              	.LVL269:
 4212              	.L289:
2199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4213              		.loc 1 2199 3 discriminator 1 view .LVU1484
 4214 01f4 0220     		movs	r0, #2
 4215 01f6 F2E7     		b	.L275
 4216              	.L301:
ARM GAS  /tmp/cc5SiBtg.s 			page 176


 4217              		.align	2
 4218              	.L300:
 4219 01f8 00000000 		.word	SPI_DMAHalfTransmitReceiveCplt
 4220 01fc 00000000 		.word	SPI_DMATransmitReceiveCplt
 4221 0200 00000000 		.word	SPI_DMAError
 4222 0204 00000000 		.word	SPI_DMAHalfReceiveCplt
 4223 0208 00000000 		.word	SPI_DMAReceiveCplt
 4224              		.cfi_endproc
 4225              	.LFE135:
 4227              		.section	.text.HAL_SPI_Receive_DMA,"ax",%progbits
 4228              		.align	1
 4229              		.global	HAL_SPI_Receive_DMA
 4230              		.syntax unified
 4231              		.thumb
 4232              		.thumb_func
 4234              	HAL_SPI_Receive_DMA:
 4235              	.LVL270:
 4236              	.LFB134:
2032:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 4237              		.loc 1 2032 1 is_stmt 1 view -0
 4238              		.cfi_startproc
 4239              		@ args = 0, pretend = 0, frame = 0
 4240              		@ frame_needed = 0, uses_anonymous_args = 0
2032:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 4241              		.loc 1 2032 1 is_stmt 0 view .LVU1486
 4242 0000 38B5     		push	{r3, r4, r5, lr}
 4243              		.cfi_def_cfa_offset 16
 4244              		.cfi_offset 3, -16
 4245              		.cfi_offset 4, -12
 4246              		.cfi_offset 5, -8
 4247              		.cfi_offset 14, -4
 4248 0002 0446     		mov	r4, r0
2033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4249              		.loc 1 2033 3 is_stmt 1 view .LVU1487
 4250              	.LVL271:
2036:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4251              		.loc 1 2036 3 view .LVU1488
2038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4252              		.loc 1 2038 3 view .LVU1489
2038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4253              		.loc 1 2038 11 is_stmt 0 view .LVU1490
 4254 0004 90F85D50 		ldrb	r5, [r0, #93]	@ zero_extendqisi2
 4255 0008 EDB2     		uxtb	r5, r5
2038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4256              		.loc 1 2038 6 view .LVU1491
 4257 000a 012D     		cmp	r5, #1
 4258 000c 40F0A780 		bne	.L312
2044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4259              		.loc 1 2044 3 is_stmt 1 view .LVU1492
2044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4260              		.loc 1 2044 18 is_stmt 0 view .LVU1493
 4261 0010 8068     		ldr	r0, [r0, #8]
 4262              	.LVL272:
2044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4263              		.loc 1 2044 6 view .LVU1494
 4264 0012 18B9     		cbnz	r0, .L304
2044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 177


 4265              		.loc 1 2044 68 discriminator 1 view .LVU1495
 4266 0014 6368     		ldr	r3, [r4, #4]
2044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4267              		.loc 1 2044 54 discriminator 1 view .LVU1496
 4268 0016 B3F5827F 		cmp	r3, #260
 4269 001a 59D0     		beq	.L315
 4270              	.L304:
2056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4271              		.loc 1 2056 3 is_stmt 1 view .LVU1497
2056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4272              		.loc 1 2056 3 view .LVU1498
 4273 001c 94F85C30 		ldrb	r3, [r4, #92]	@ zero_extendqisi2
 4274 0020 012B     		cmp	r3, #1
 4275 0022 00F0A280 		beq	.L313
2056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4276              		.loc 1 2056 3 discriminator 2 view .LVU1499
 4277 0026 0123     		movs	r3, #1
 4278 0028 84F85C30 		strb	r3, [r4, #92]
2056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4279              		.loc 1 2056 3 discriminator 2 view .LVU1500
2058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4280              		.loc 1 2058 3 view .LVU1501
2058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4281              		.loc 1 2058 6 is_stmt 0 view .LVU1502
 4282 002c 0029     		cmp	r1, #0
 4283 002e 00F09780 		beq	.L303
2058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4284              		.loc 1 2058 23 discriminator 1 view .LVU1503
 4285 0032 002A     		cmp	r2, #0
 4286 0034 00F09480 		beq	.L303
2065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 4287              		.loc 1 2065 3 is_stmt 1 view .LVU1504
2065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 4288              		.loc 1 2065 21 is_stmt 0 view .LVU1505
 4289 0038 0423     		movs	r3, #4
 4290 003a 84F85D30 		strb	r3, [r4, #93]
2066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 4291              		.loc 1 2066 3 is_stmt 1 view .LVU1506
2066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 4292              		.loc 1 2066 21 is_stmt 0 view .LVU1507
 4293 003e 0023     		movs	r3, #0
 4294 0040 2366     		str	r3, [r4, #96]
2067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 4295              		.loc 1 2067 3 is_stmt 1 view .LVU1508
2067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 4296              		.loc 1 2067 21 is_stmt 0 view .LVU1509
 4297 0042 2164     		str	r1, [r4, #64]
2068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 4298              		.loc 1 2068 3 is_stmt 1 view .LVU1510
2068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 4299              		.loc 1 2068 21 is_stmt 0 view .LVU1511
 4300 0044 A4F84420 		strh	r2, [r4, #68]	@ movhi
2069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4301              		.loc 1 2069 3 is_stmt 1 view .LVU1512
2069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4302              		.loc 1 2069 21 is_stmt 0 view .LVU1513
 4303 0048 A4F84620 		strh	r2, [r4, #70]	@ movhi
ARM GAS  /tmp/cc5SiBtg.s 			page 178


2072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 4304              		.loc 1 2072 3 is_stmt 1 view .LVU1514
2072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 4305              		.loc 1 2072 21 is_stmt 0 view .LVU1515
 4306 004c E364     		str	r3, [r4, #76]
2073:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
 4307              		.loc 1 2073 3 is_stmt 1 view .LVU1516
2073:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
 4308              		.loc 1 2073 21 is_stmt 0 view .LVU1517
 4309 004e 2365     		str	r3, [r4, #80]
2074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 4310              		.loc 1 2074 3 is_stmt 1 view .LVU1518
2074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 4311              		.loc 1 2074 21 is_stmt 0 view .LVU1519
 4312 0050 A387     		strh	r3, [r4, #60]	@ movhi
2075:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4313              		.loc 1 2075 3 is_stmt 1 view .LVU1520
2075:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4314              		.loc 1 2075 21 is_stmt 0 view .LVU1521
 4315 0052 E387     		strh	r3, [r4, #62]	@ movhi
2078:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4316              		.loc 1 2078 3 is_stmt 1 view .LVU1522
2078:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4317              		.loc 1 2078 6 is_stmt 0 view .LVU1523
 4318 0054 B0F5004F 		cmp	r0, #32768
 4319 0058 44D0     		beq	.L316
 4320              	.LVL273:
 4321              	.L306:
2103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
 4322              		.loc 1 2103 3 is_stmt 1 view .LVU1524
 4323 005a 2268     		ldr	r2, [r4]
 4324 005c 5368     		ldr	r3, [r2, #4]
 4325 005e 23F40053 		bic	r3, r3, #8192
 4326 0062 5360     		str	r3, [r2, #4]
2104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4327              		.loc 1 2104 3 view .LVU1525
2104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4328              		.loc 1 2104 17 is_stmt 0 view .LVU1526
 4329 0064 E368     		ldr	r3, [r4, #12]
2104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4330              		.loc 1 2104 6 view .LVU1527
 4331 0066 B3F5E06F 		cmp	r3, #1792
 4332 006a 46D9     		bls	.L307
2107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4333              		.loc 1 2107 5 is_stmt 1 view .LVU1528
 4334 006c 2268     		ldr	r2, [r4]
 4335 006e 5368     		ldr	r3, [r2, #4]
 4336 0070 23F48053 		bic	r3, r3, #4096
 4337 0074 5360     		str	r3, [r2, #4]
 4338              	.L308:
2133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4339              		.loc 1 2133 3 view .LVU1529
2133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4340              		.loc 1 2133 7 is_stmt 0 view .LVU1530
 4341 0076 A36D     		ldr	r3, [r4, #88]
2133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4342              		.loc 1 2133 38 view .LVU1531
ARM GAS  /tmp/cc5SiBtg.s 			page 179


 4343 0078 3D4A     		ldr	r2, .L318
 4344 007a DA62     		str	r2, [r3, #44]
2136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4345              		.loc 1 2136 3 is_stmt 1 view .LVU1532
2136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4346              		.loc 1 2136 7 is_stmt 0 view .LVU1533
 4347 007c A36D     		ldr	r3, [r4, #88]
2136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4348              		.loc 1 2136 34 view .LVU1534
 4349 007e 3D4A     		ldr	r2, .L318+4
 4350 0080 9A62     		str	r2, [r3, #40]
2139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4351              		.loc 1 2139 3 is_stmt 1 view .LVU1535
2139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4352              		.loc 1 2139 7 is_stmt 0 view .LVU1536
 4353 0082 A36D     		ldr	r3, [r4, #88]
2139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4354              		.loc 1 2139 35 view .LVU1537
 4355 0084 3C4A     		ldr	r2, .L318+8
 4356 0086 1A63     		str	r2, [r3, #48]
2142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4357              		.loc 1 2142 3 is_stmt 1 view .LVU1538
2142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4358              		.loc 1 2142 7 is_stmt 0 view .LVU1539
 4359 0088 A36D     		ldr	r3, [r4, #88]
2142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4360              		.loc 1 2142 35 view .LVU1540
 4361 008a 0022     		movs	r2, #0
 4362 008c 5A63     		str	r2, [r3, #52]
2145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 4363              		.loc 1 2145 3 is_stmt 1 view .LVU1541
2145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 4364              		.loc 1 2145 63 is_stmt 0 view .LVU1542
 4365 008e 2168     		ldr	r1, [r4]
 4366              	.LVL274:
2146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4367              		.loc 1 2146 38 view .LVU1543
 4368 0090 B4F84630 		ldrh	r3, [r4, #70]
2145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 4369              		.loc 1 2145 17 view .LVU1544
 4370 0094 9BB2     		uxth	r3, r3
 4371 0096 226C     		ldr	r2, [r4, #64]
 4372 0098 0C31     		adds	r1, r1, #12
 4373 009a A06D     		ldr	r0, [r4, #88]
 4374 009c FFF7FEFF 		bl	HAL_DMA_Start_IT
 4375              	.LVL275:
2145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 4376              		.loc 1 2145 6 discriminator 1 view .LVU1545
 4377 00a0 0146     		mov	r1, r0
 4378 00a2 0028     		cmp	r0, #0
 4379 00a4 56D1     		bne	.L317
2156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4380              		.loc 1 2156 3 is_stmt 1 view .LVU1546
2156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4381              		.loc 1 2156 12 is_stmt 0 view .LVU1547
 4382 00a6 2368     		ldr	r3, [r4]
2156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 180


 4383              		.loc 1 2156 22 view .LVU1548
 4384 00a8 1A68     		ldr	r2, [r3]
2156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4385              		.loc 1 2156 6 view .LVU1549
 4386 00aa 12F0400F 		tst	r2, #64
 4387 00ae 03D1     		bne	.L311
2159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4388              		.loc 1 2159 5 is_stmt 1 view .LVU1550
 4389 00b0 1A68     		ldr	r2, [r3]
 4390 00b2 42F04002 		orr	r2, r2, #64
 4391 00b6 1A60     		str	r2, [r3]
 4392              	.L311:
2163:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4393              		.loc 1 2163 3 view .LVU1551
 4394 00b8 2268     		ldr	r2, [r4]
 4395 00ba 5368     		ldr	r3, [r2, #4]
 4396 00bc 43F02003 		orr	r3, r3, #32
 4397 00c0 5360     		str	r3, [r2, #4]
2166:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4398              		.loc 1 2166 3 view .LVU1552
 4399 00c2 2268     		ldr	r2, [r4]
 4400 00c4 5368     		ldr	r3, [r2, #4]
 4401 00c6 43F00103 		orr	r3, r3, #1
 4402 00ca 5360     		str	r3, [r2, #4]
2033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4403              		.loc 1 2033 21 is_stmt 0 view .LVU1553
 4404 00cc 0D46     		mov	r5, r1
 4405 00ce 47E0     		b	.L303
 4406              	.LVL276:
 4407              	.L315:
2046:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4408              		.loc 1 2046 5 is_stmt 1 view .LVU1554
2046:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4409              		.loc 1 2046 17 is_stmt 0 view .LVU1555
 4410 00d0 0423     		movs	r3, #4
 4411 00d2 84F85D30 		strb	r3, [r4, #93]
2049:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4412              		.loc 1 2049 5 is_stmt 1 view .LVU1556
2052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4413              		.loc 1 2052 5 view .LVU1557
2052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4414              		.loc 1 2052 12 is_stmt 0 view .LVU1558
 4415 00d6 1346     		mov	r3, r2
 4416 00d8 0A46     		mov	r2, r1
 4417              	.LVL277:
2052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4418              		.loc 1 2052 12 view .LVU1559
 4419 00da 2046     		mov	r0, r4
 4420 00dc FFF7FEFF 		bl	HAL_SPI_TransmitReceive_DMA
 4421              	.LVL278:
2052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4422              		.loc 1 2052 12 view .LVU1560
 4423 00e0 0546     		mov	r5, r0
 4424 00e2 40E0     		b	.L305
 4425              	.LVL279:
 4426              	.L316:
2081:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
ARM GAS  /tmp/cc5SiBtg.s 			page 181


 4427              		.loc 1 2081 5 is_stmt 1 view .LVU1561
 4428 00e4 2268     		ldr	r2, [r4]
 4429              	.LVL280:
2081:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
 4430              		.loc 1 2081 5 is_stmt 0 view .LVU1562
 4431 00e6 1368     		ldr	r3, [r2]
 4432 00e8 23F04003 		bic	r3, r3, #64
 4433 00ec 1360     		str	r3, [r2]
 4434              	.LVL281:
2082:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4435              		.loc 1 2082 5 is_stmt 1 view .LVU1563
 4436 00ee 2268     		ldr	r2, [r4]
 4437 00f0 1368     		ldr	r3, [r2]
 4438 00f2 23F48043 		bic	r3, r3, #16384
 4439 00f6 1360     		str	r3, [r2]
 4440 00f8 AFE7     		b	.L306
 4441              	.L307:
2112:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4442              		.loc 1 2112 5 view .LVU1564
 4443 00fa 2268     		ldr	r2, [r4]
 4444 00fc 5368     		ldr	r3, [r2, #4]
 4445 00fe 43F48053 		orr	r3, r3, #4096
 4446 0102 5360     		str	r3, [r2, #4]
2114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4447              		.loc 1 2114 5 view .LVU1565
2114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4448              		.loc 1 2114 13 is_stmt 0 view .LVU1566
 4449 0104 A36D     		ldr	r3, [r4, #88]
2114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4450              		.loc 1 2114 27 view .LVU1567
 4451 0106 5B69     		ldr	r3, [r3, #20]
2114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4452              		.loc 1 2114 8 view .LVU1568
 4453 0108 B3F5806F 		cmp	r3, #1024
 4454 010c B3D1     		bne	.L308
2117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4455              		.loc 1 2117 7 is_stmt 1 view .LVU1569
 4456 010e 2268     		ldr	r2, [r4]
 4457 0110 5368     		ldr	r3, [r2, #4]
 4458 0112 23F48053 		bic	r3, r3, #4096
 4459 0116 5360     		str	r3, [r2, #4]
2119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4460              		.loc 1 2119 7 view .LVU1570
2119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4461              		.loc 1 2119 16 is_stmt 0 view .LVU1571
 4462 0118 B4F84630 		ldrh	r3, [r4, #70]
2119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4463              		.loc 1 2119 10 view .LVU1572
 4464 011c 13F0010F 		tst	r3, #1
 4465 0120 0BD1     		bne	.L309
2121:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = hspi->RxXferCount >> 1U;
 4466              		.loc 1 2121 9 is_stmt 1 view .LVU1573
 4467 0122 2268     		ldr	r2, [r4]
 4468 0124 5368     		ldr	r3, [r2, #4]
 4469 0126 23F40053 		bic	r3, r3, #8192
 4470 012a 5360     		str	r3, [r2, #4]
2122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
ARM GAS  /tmp/cc5SiBtg.s 			page 182


 4471              		.loc 1 2122 9 view .LVU1574
2122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4472              		.loc 1 2122 33 is_stmt 0 view .LVU1575
 4473 012c B4F84630 		ldrh	r3, [r4, #70]
2122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4474              		.loc 1 2122 27 view .LVU1576
 4475 0130 C3F34E03 		ubfx	r3, r3, #1, #15
 4476 0134 A4F84630 		strh	r3, [r4, #70]	@ movhi
 4477 0138 9DE7     		b	.L308
 4478              	.L309:
2126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = (hspi->RxXferCount >> 1U) + 1U;
 4479              		.loc 1 2126 9 is_stmt 1 view .LVU1577
 4480 013a 2268     		ldr	r2, [r4]
 4481 013c 5368     		ldr	r3, [r2, #4]
 4482 013e 43F40053 		orr	r3, r3, #8192
 4483 0142 5360     		str	r3, [r2, #4]
2127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4484              		.loc 1 2127 9 view .LVU1578
2127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4485              		.loc 1 2127 34 is_stmt 0 view .LVU1579
 4486 0144 B4F84630 		ldrh	r3, [r4, #70]
2127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4487              		.loc 1 2127 55 view .LVU1580
 4488 0148 C3F34E03 		ubfx	r3, r3, #1, #15
 4489 014c 0133     		adds	r3, r3, #1
2127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4490              		.loc 1 2127 27 view .LVU1581
 4491 014e A4F84630 		strh	r3, [r4, #70]	@ movhi
 4492 0152 90E7     		b	.L308
 4493              	.LVL282:
 4494              	.L317:
2149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
 4495              		.loc 1 2149 5 is_stmt 1 view .LVU1582
 4496 0154 236E     		ldr	r3, [r4, #96]
 4497 0156 43F01003 		orr	r3, r3, #16
 4498 015a 2366     		str	r3, [r4, #96]
2150:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4499              		.loc 1 2150 5 view .LVU1583
 4500              	.LVL283:
2152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4501              		.loc 1 2152 5 view .LVU1584
 4502 015c 00E0     		b	.L303
 4503              	.LVL284:
 4504              	.L312:
2040:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4505              		.loc 1 2040 15 is_stmt 0 view .LVU1585
 4506 015e 0225     		movs	r5, #2
 4507              	.LVL285:
 4508              	.L303:
2170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 4509              		.loc 1 2170 3 is_stmt 1 view .LVU1586
2170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 4510              		.loc 1 2170 3 view .LVU1587
 4511 0160 0023     		movs	r3, #0
 4512 0162 84F85C30 		strb	r3, [r4, #92]
2170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 4513              		.loc 1 2170 3 view .LVU1588
ARM GAS  /tmp/cc5SiBtg.s 			page 183


2171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4514              		.loc 1 2171 3 view .LVU1589
 4515              	.LVL286:
 4516              	.L305:
2172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4517              		.loc 1 2172 1 is_stmt 0 view .LVU1590
 4518 0166 2846     		mov	r0, r5
 4519 0168 38BD     		pop	{r3, r4, r5, pc}
 4520              	.LVL287:
 4521              	.L313:
2056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4522              		.loc 1 2056 3 discriminator 1 view .LVU1591
 4523 016a 0225     		movs	r5, #2
 4524 016c FBE7     		b	.L305
 4525              	.L319:
 4526 016e 00BF     		.align	2
 4527              	.L318:
 4528 0170 00000000 		.word	SPI_DMAHalfReceiveCplt
 4529 0174 00000000 		.word	SPI_DMAReceiveCplt
 4530 0178 00000000 		.word	SPI_DMAError
 4531              		.cfi_endproc
 4532              	.LFE134:
 4534              		.section	.text.HAL_SPI_Abort,"ax",%progbits
 4535              		.align	1
 4536              		.global	HAL_SPI_Abort
 4537              		.syntax unified
 4538              		.thumb
 4539              		.thumb_func
 4541              	HAL_SPI_Abort:
 4542              	.LVL288:
 4543              	.LFB136:
2385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
 4544              		.loc 1 2385 1 is_stmt 1 view -0
 4545              		.cfi_startproc
 4546              		@ args = 0, pretend = 0, frame = 16
 4547              		@ frame_needed = 0, uses_anonymous_args = 0
2385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
 4548              		.loc 1 2385 1 is_stmt 0 view .LVU1593
 4549 0000 10B5     		push	{r4, lr}
 4550              		.cfi_def_cfa_offset 8
 4551              		.cfi_offset 4, -8
 4552              		.cfi_offset 14, -4
 4553 0002 86B0     		sub	sp, sp, #24
 4554              		.cfi_def_cfa_offset 32
 4555 0004 0446     		mov	r4, r0
2386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
 4556              		.loc 1 2386 3 is_stmt 1 view .LVU1594
2387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t resetcount;
 4557              		.loc 1 2387 3 view .LVU1595
2388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4558              		.loc 1 2388 3 view .LVU1596
2391:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 4559              		.loc 1 2391 3 view .LVU1597
 4560              	.LVL289:
2392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 4561              		.loc 1 2392 3 view .LVU1598
2392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
ARM GAS  /tmp/cc5SiBtg.s 			page 184


 4562              		.loc 1 2392 61 is_stmt 0 view .LVU1599
 4563 0006 5E4B     		ldr	r3, .L341
 4564 0008 1B68     		ldr	r3, [r3]
 4565 000a 5E4A     		ldr	r2, .L341+4
 4566 000c A2FB0323 		umull	r2, r3, r2, r3
 4567 0010 5B0A     		lsrs	r3, r3, #9
2392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 4568              		.loc 1 2392 36 view .LVU1600
 4569 0012 6422     		movs	r2, #100
 4570 0014 02FB03F3 		mul	r3, r2, r3
2392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 4571              		.loc 1 2392 14 view .LVU1601
 4572 0018 0493     		str	r3, [sp, #16]
2393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4573              		.loc 1 2393 3 is_stmt 1 view .LVU1602
2393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4574              		.loc 1 2393 9 is_stmt 0 view .LVU1603
 4575 001a 049B     		ldr	r3, [sp, #16]
 4576 001c 0593     		str	r3, [sp, #20]
2396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4577              		.loc 1 2396 3 is_stmt 1 view .LVU1604
 4578 001e 0268     		ldr	r2, [r0]
 4579 0020 5368     		ldr	r3, [r2, #4]
 4580 0022 23F02003 		bic	r3, r3, #32
 4581 0026 5360     		str	r3, [r2, #4]
2399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4582              		.loc 1 2399 3 view .LVU1605
2399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4583              		.loc 1 2399 7 is_stmt 0 view .LVU1606
 4584 0028 0268     		ldr	r2, [r0]
 4585 002a 5368     		ldr	r3, [r2, #4]
2399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4586              		.loc 1 2399 6 view .LVU1607
 4587 002c 13F0800F 		tst	r3, #128
 4588 0030 12D0     		beq	.L321
2401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 4589              		.loc 1 2401 5 is_stmt 1 view .LVU1608
2401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 4590              		.loc 1 2401 17 is_stmt 0 view .LVU1609
 4591 0032 554B     		ldr	r3, .L341+8
 4592 0034 0365     		str	r3, [r0, #80]
 4593              	.L324:
2403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4594              		.loc 1 2403 5 is_stmt 1 view .LVU1610
2405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4595              		.loc 1 2405 7 view .LVU1611
2405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4596              		.loc 1 2405 17 is_stmt 0 view .LVU1612
 4597 0036 059B     		ldr	r3, [sp, #20]
2405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4598              		.loc 1 2405 10 view .LVU1613
 4599 0038 43B1     		cbz	r3, .L339
2410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 4600              		.loc 1 2410 7 is_stmt 1 view .LVU1614
2410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 4601              		.loc 1 2410 12 is_stmt 0 view .LVU1615
 4602 003a 059B     		ldr	r3, [sp, #20]
ARM GAS  /tmp/cc5SiBtg.s 			page 185


 4603 003c 013B     		subs	r3, r3, #1
 4604 003e 0593     		str	r3, [sp, #20]
2411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 4605              		.loc 1 2411 26 is_stmt 1 view .LVU1616
2411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 4606              		.loc 1 2411 18 is_stmt 0 view .LVU1617
 4607 0040 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 4608 0044 DBB2     		uxtb	r3, r3
2411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 4609              		.loc 1 2411 26 view .LVU1618
 4610 0046 072B     		cmp	r3, #7
 4611 0048 F5D1     		bne	.L324
 4612 004a 03E0     		b	.L323
 4613              	.L339:
2407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 4614              		.loc 1 2407 9 is_stmt 1 view .LVU1619
 4615 004c 236E     		ldr	r3, [r4, #96]
 4616 004e 43F04003 		orr	r3, r3, #64
 4617 0052 2366     		str	r3, [r4, #96]
2408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4618              		.loc 1 2408 9 view .LVU1620
 4619              	.L323:
2413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4620              		.loc 1 2413 5 view .LVU1621
2413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4621              		.loc 1 2413 11 is_stmt 0 view .LVU1622
 4622 0054 049B     		ldr	r3, [sp, #16]
 4623 0056 0593     		str	r3, [sp, #20]
 4624              	.L321:
2416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4625              		.loc 1 2416 3 is_stmt 1 view .LVU1623
2416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4626              		.loc 1 2416 7 is_stmt 0 view .LVU1624
 4627 0058 5368     		ldr	r3, [r2, #4]
2416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4628              		.loc 1 2416 6 view .LVU1625
 4629 005a 13F0400F 		tst	r3, #64
 4630 005e 12D0     		beq	.L325
2418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 4631              		.loc 1 2418 5 is_stmt 1 view .LVU1626
2418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 4632              		.loc 1 2418 17 is_stmt 0 view .LVU1627
 4633 0060 4A4B     		ldr	r3, .L341+12
 4634 0062 E364     		str	r3, [r4, #76]
 4635              	.L328:
2420:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4636              		.loc 1 2420 5 is_stmt 1 view .LVU1628
2422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4637              		.loc 1 2422 7 view .LVU1629
2422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4638              		.loc 1 2422 17 is_stmt 0 view .LVU1630
 4639 0064 059B     		ldr	r3, [sp, #20]
2422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4640              		.loc 1 2422 10 view .LVU1631
 4641 0066 43B1     		cbz	r3, .L340
2427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 4642              		.loc 1 2427 7 is_stmt 1 view .LVU1632
ARM GAS  /tmp/cc5SiBtg.s 			page 186


2427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 4643              		.loc 1 2427 12 is_stmt 0 view .LVU1633
 4644 0068 059B     		ldr	r3, [sp, #20]
 4645 006a 013B     		subs	r3, r3, #1
 4646 006c 0593     		str	r3, [sp, #20]
2428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 4647              		.loc 1 2428 26 is_stmt 1 view .LVU1634
2428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 4648              		.loc 1 2428 18 is_stmt 0 view .LVU1635
 4649 006e 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 4650 0072 DBB2     		uxtb	r3, r3
2428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 4651              		.loc 1 2428 26 view .LVU1636
 4652 0074 072B     		cmp	r3, #7
 4653 0076 F5D1     		bne	.L328
 4654 0078 03E0     		b	.L327
 4655              	.L340:
2424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 4656              		.loc 1 2424 9 is_stmt 1 view .LVU1637
 4657 007a 236E     		ldr	r3, [r4, #96]
 4658 007c 43F04003 		orr	r3, r3, #64
 4659 0080 2366     		str	r3, [r4, #96]
2425:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4660              		.loc 1 2425 9 view .LVU1638
 4661              	.L327:
2430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4662              		.loc 1 2430 5 view .LVU1639
2430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4663              		.loc 1 2430 11 is_stmt 0 view .LVU1640
 4664 0082 049B     		ldr	r3, [sp, #16]
 4665 0084 0593     		str	r3, [sp, #20]
 4666              	.L325:
2434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4667              		.loc 1 2434 3 is_stmt 1 view .LVU1641
2434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4668              		.loc 1 2434 7 is_stmt 0 view .LVU1642
 4669 0086 5368     		ldr	r3, [r2, #4]
2434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4670              		.loc 1 2434 6 view .LVU1643
 4671 0088 13F0020F 		tst	r3, #2
 4672 008c 2AD0     		beq	.L329
2437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4673              		.loc 1 2437 5 is_stmt 1 view .LVU1644
2437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4674              		.loc 1 2437 13 is_stmt 0 view .LVU1645
 4675 008e 636D     		ldr	r3, [r4, #84]
2437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4676              		.loc 1 2437 8 view .LVU1646
 4677 0090 43B3     		cbz	r3, .L329
2441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4678              		.loc 1 2441 7 is_stmt 1 view .LVU1647
2441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4679              		.loc 1 2441 39 is_stmt 0 view .LVU1648
 4680 0092 0022     		movs	r2, #0
 4681 0094 5A63     		str	r2, [r3, #52]
2444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4682              		.loc 1 2444 7 is_stmt 1 view .LVU1649
ARM GAS  /tmp/cc5SiBtg.s 			page 187


2444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4683              		.loc 1 2444 11 is_stmt 0 view .LVU1650
 4684 0096 606D     		ldr	r0, [r4, #84]
 4685              	.LVL290:
2444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4686              		.loc 1 2444 11 view .LVU1651
 4687 0098 FFF7FEFF 		bl	HAL_DMA_Abort
 4688              	.LVL291:
2444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4689              		.loc 1 2444 10 discriminator 1 view .LVU1652
 4690 009c 08B1     		cbz	r0, .L330
2446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4691              		.loc 1 2446 9 is_stmt 1 view .LVU1653
2446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4692              		.loc 1 2446 25 is_stmt 0 view .LVU1654
 4693 009e 4023     		movs	r3, #64
 4694 00a0 2366     		str	r3, [r4, #96]
 4695              	.L330:
2450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4696              		.loc 1 2450 7 is_stmt 1 view .LVU1655
 4697 00a2 2268     		ldr	r2, [r4]
 4698 00a4 5368     		ldr	r3, [r2, #4]
 4699 00a6 23F00203 		bic	r3, r3, #2
 4700 00aa 5360     		str	r3, [r2, #4]
2452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4701              		.loc 1 2452 7 view .LVU1656
2452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4702              		.loc 1 2452 11 is_stmt 0 view .LVU1657
 4703 00ac FFF7FEFF 		bl	HAL_GetTick
 4704              	.LVL292:
 4705 00b0 0246     		mov	r2, r0
2452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4706              		.loc 1 2452 11 discriminator 1 view .LVU1658
 4707 00b2 6421     		movs	r1, #100
 4708 00b4 2046     		mov	r0, r4
 4709 00b6 FFF7FEFF 		bl	SPI_EndRxTxTransaction
 4710              	.LVL293:
2452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4711              		.loc 1 2452 10 discriminator 2 view .LVU1659
 4712 00ba 08B1     		cbz	r0, .L331
2454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4713              		.loc 1 2454 9 is_stmt 1 view .LVU1660
2454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4714              		.loc 1 2454 25 is_stmt 0 view .LVU1661
 4715 00bc 4023     		movs	r3, #64
 4716 00be 2366     		str	r3, [r4, #96]
 4717              	.L331:
2458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4718              		.loc 1 2458 7 is_stmt 1 view .LVU1662
 4719 00c0 2268     		ldr	r2, [r4]
 4720 00c2 1368     		ldr	r3, [r2]
 4721 00c4 23F04003 		bic	r3, r3, #64
 4722 00c8 1360     		str	r3, [r2]
2461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4723              		.loc 1 2461 7 view .LVU1663
2461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4724              		.loc 1 2461 11 is_stmt 0 view .LVU1664
ARM GAS  /tmp/cc5SiBtg.s 			page 188


 4725 00ca FFF7FEFF 		bl	HAL_GetTick
 4726              	.LVL294:
2461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4727              		.loc 1 2461 11 discriminator 1 view .LVU1665
 4728 00ce 0090     		str	r0, [sp]
 4729 00d0 6423     		movs	r3, #100
 4730 00d2 0022     		movs	r2, #0
 4731 00d4 4FF4C061 		mov	r1, #1536
 4732 00d8 2046     		mov	r0, r4
 4733 00da FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 4734              	.LVL295:
2461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4735              		.loc 1 2461 10 discriminator 2 view .LVU1666
 4736 00de 08B1     		cbz	r0, .L329
2463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4737              		.loc 1 2463 9 is_stmt 1 view .LVU1667
2463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4738              		.loc 1 2463 25 is_stmt 0 view .LVU1668
 4739 00e0 4023     		movs	r3, #64
 4740 00e2 2366     		str	r3, [r4, #96]
 4741              	.L329:
2469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4742              		.loc 1 2469 3 is_stmt 1 view .LVU1669
2469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4743              		.loc 1 2469 7 is_stmt 0 view .LVU1670
 4744 00e4 2368     		ldr	r3, [r4]
 4745 00e6 5B68     		ldr	r3, [r3, #4]
2469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4746              		.loc 1 2469 6 view .LVU1671
 4747 00e8 13F0010F 		tst	r3, #1
 4748 00ec 2CD0     		beq	.L332
2472:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4749              		.loc 1 2472 5 is_stmt 1 view .LVU1672
2472:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4750              		.loc 1 2472 13 is_stmt 0 view .LVU1673
 4751 00ee A36D     		ldr	r3, [r4, #88]
2472:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4752              		.loc 1 2472 8 view .LVU1674
 4753 00f0 53B3     		cbz	r3, .L332
2476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4754              		.loc 1 2476 7 is_stmt 1 view .LVU1675
2476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4755              		.loc 1 2476 39 is_stmt 0 view .LVU1676
 4756 00f2 0022     		movs	r2, #0
 4757 00f4 5A63     		str	r2, [r3, #52]
2479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4758              		.loc 1 2479 7 is_stmt 1 view .LVU1677
2479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4759              		.loc 1 2479 11 is_stmt 0 view .LVU1678
 4760 00f6 A06D     		ldr	r0, [r4, #88]
 4761 00f8 FFF7FEFF 		bl	HAL_DMA_Abort
 4762              	.LVL296:
2479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4763              		.loc 1 2479 10 discriminator 1 view .LVU1679
 4764 00fc 08B1     		cbz	r0, .L333
2481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4765              		.loc 1 2481 9 is_stmt 1 view .LVU1680
ARM GAS  /tmp/cc5SiBtg.s 			page 189


2481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4766              		.loc 1 2481 25 is_stmt 0 view .LVU1681
 4767 00fe 4023     		movs	r3, #64
 4768 0100 2366     		str	r3, [r4, #96]
 4769              	.L333:
2485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4770              		.loc 1 2485 7 is_stmt 1 view .LVU1682
 4771 0102 2268     		ldr	r2, [r4]
 4772 0104 1368     		ldr	r3, [r2]
 4773 0106 23F04003 		bic	r3, r3, #64
 4774 010a 1360     		str	r3, [r2]
2488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4775              		.loc 1 2488 7 view .LVU1683
2488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4776              		.loc 1 2488 11 is_stmt 0 view .LVU1684
 4777 010c FFF7FEFF 		bl	HAL_GetTick
 4778              	.LVL297:
2488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4779              		.loc 1 2488 11 discriminator 1 view .LVU1685
 4780 0110 0090     		str	r0, [sp]
 4781 0112 6423     		movs	r3, #100
 4782 0114 0022     		movs	r2, #0
 4783 0116 8021     		movs	r1, #128
 4784 0118 2046     		mov	r0, r4
 4785 011a FFF7FEFF 		bl	SPI_WaitFlagStateUntilTimeout
 4786              	.LVL298:
2488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4787              		.loc 1 2488 10 discriminator 2 view .LVU1686
 4788 011e 08B1     		cbz	r0, .L334
2490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4789              		.loc 1 2490 9 is_stmt 1 view .LVU1687
2490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4790              		.loc 1 2490 25 is_stmt 0 view .LVU1688
 4791 0120 4023     		movs	r3, #64
 4792 0122 2366     		str	r3, [r4, #96]
 4793              	.L334:
2494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4794              		.loc 1 2494 7 is_stmt 1 view .LVU1689
2494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4795              		.loc 1 2494 11 is_stmt 0 view .LVU1690
 4796 0124 FFF7FEFF 		bl	HAL_GetTick
 4797              	.LVL299:
2494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4798              		.loc 1 2494 11 discriminator 1 view .LVU1691
 4799 0128 0090     		str	r0, [sp]
 4800 012a 6423     		movs	r3, #100
 4801 012c 0022     		movs	r2, #0
 4802 012e 4FF4C061 		mov	r1, #1536
 4803 0132 2046     		mov	r0, r4
 4804 0134 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 4805              	.LVL300:
2494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4806              		.loc 1 2494 10 discriminator 2 view .LVU1692
 4807 0138 08B1     		cbz	r0, .L335
2496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4808              		.loc 1 2496 9 is_stmt 1 view .LVU1693
2496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
ARM GAS  /tmp/cc5SiBtg.s 			page 190


 4809              		.loc 1 2496 25 is_stmt 0 view .LVU1694
 4810 013a 4023     		movs	r3, #64
 4811 013c 2366     		str	r3, [r4, #96]
 4812              	.L335:
2500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 4813              		.loc 1 2500 7 is_stmt 1 view .LVU1695
 4814 013e 2268     		ldr	r2, [r4]
 4815 0140 5368     		ldr	r3, [r2, #4]
 4816 0142 23F00103 		bic	r3, r3, #1
 4817 0146 5360     		str	r3, [r2, #4]
 4818              	.L332:
2504:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 4819              		.loc 1 2504 3 view .LVU1696
2504:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 4820              		.loc 1 2504 21 is_stmt 0 view .LVU1697
 4821 0148 0023     		movs	r3, #0
 4822 014a A4F84630 		strh	r3, [r4, #70]	@ movhi
2505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4823              		.loc 1 2505 3 is_stmt 1 view .LVU1698
2505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4824              		.loc 1 2505 21 is_stmt 0 view .LVU1699
 4825 014e E387     		strh	r3, [r4, #62]	@ movhi
2508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4826              		.loc 1 2508 3 is_stmt 1 view .LVU1700
2508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4827              		.loc 1 2508 11 is_stmt 0 view .LVU1701
 4828 0150 236E     		ldr	r3, [r4, #96]
2508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4829              		.loc 1 2508 6 view .LVU1702
 4830 0152 402B     		cmp	r3, #64
 4831 0154 12D0     		beq	.L337
2516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4832              		.loc 1 2516 5 is_stmt 1 view .LVU1703
2516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4833              		.loc 1 2516 21 is_stmt 0 view .LVU1704
 4834 0156 0020     		movs	r0, #0
 4835 0158 2066     		str	r0, [r4, #96]
 4836              	.L336:
 4837              	.LVL301:
2520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 4838              		.loc 1 2520 3 is_stmt 1 view .LVU1705
 4839              	.LBB3:
2520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 4840              		.loc 1 2520 3 view .LVU1706
 4841 015a 0022     		movs	r2, #0
 4842 015c 0292     		str	r2, [sp, #8]
2520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 4843              		.loc 1 2520 3 view .LVU1707
 4844 015e 2368     		ldr	r3, [r4]
 4845 0160 D968     		ldr	r1, [r3, #12]
 4846 0162 0291     		str	r1, [sp, #8]
2520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 4847              		.loc 1 2520 3 view .LVU1708
 4848 0164 9968     		ldr	r1, [r3, #8]
 4849 0166 0291     		str	r1, [sp, #8]
2520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 4850              		.loc 1 2520 3 view .LVU1709
ARM GAS  /tmp/cc5SiBtg.s 			page 191


 4851 0168 0299     		ldr	r1, [sp, #8]
 4852              	.LBE3:
2520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 4853              		.loc 1 2520 3 view .LVU1710
2521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4854              		.loc 1 2521 3 view .LVU1711
 4855              	.LBB4:
2521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4856              		.loc 1 2521 3 view .LVU1712
 4857 016a 0392     		str	r2, [sp, #12]
2521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4858              		.loc 1 2521 3 view .LVU1713
 4859 016c 9B68     		ldr	r3, [r3, #8]
 4860 016e 0393     		str	r3, [sp, #12]
2521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4861              		.loc 1 2521 3 view .LVU1714
 4862 0170 039B     		ldr	r3, [sp, #12]
 4863              	.LBE4:
2521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4864              		.loc 1 2521 3 view .LVU1715
2524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4865              		.loc 1 2524 3 view .LVU1716
2524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4866              		.loc 1 2524 15 is_stmt 0 view .LVU1717
 4867 0172 0123     		movs	r3, #1
 4868 0174 84F85D30 		strb	r3, [r4, #93]
2526:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4869              		.loc 1 2526 3 is_stmt 1 view .LVU1718
2527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4870              		.loc 1 2527 1 is_stmt 0 view .LVU1719
 4871 0178 06B0     		add	sp, sp, #24
 4872              		.cfi_remember_state
 4873              		.cfi_def_cfa_offset 8
 4874              		@ sp needed
 4875 017a 10BD     		pop	{r4, pc}
 4876              	.LVL302:
 4877              	.L337:
 4878              		.cfi_restore_state
2511:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4879              		.loc 1 2511 15 view .LVU1720
 4880 017c 0120     		movs	r0, #1
 4881 017e ECE7     		b	.L336
 4882              	.L342:
 4883              		.align	2
 4884              	.L341:
 4885 0180 00000000 		.word	SystemCoreClock
 4886 0184 F1197605 		.word	91625969
 4887 0188 00000000 		.word	SPI_AbortTx_ISR
 4888 018c 00000000 		.word	SPI_AbortRx_ISR
 4889              		.cfi_endproc
 4890              	.LFE136:
 4892              		.section	.text.HAL_SPI_DMAPause,"ax",%progbits
 4893              		.align	1
 4894              		.global	HAL_SPI_DMAPause
 4895              		.syntax unified
 4896              		.thumb
 4897              		.thumb_func
ARM GAS  /tmp/cc5SiBtg.s 			page 192


 4899              	HAL_SPI_DMAPause:
 4900              	.LVL303:
 4901              	.LFB138:
2706:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
 4902              		.loc 1 2706 1 is_stmt 1 view -0
 4903              		.cfi_startproc
 4904              		@ args = 0, pretend = 0, frame = 0
 4905              		@ frame_needed = 0, uses_anonymous_args = 0
 4906              		@ link register save eliminated.
2708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4907              		.loc 1 2708 3 view .LVU1722
2708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4908              		.loc 1 2708 3 view .LVU1723
 4909 0000 90F85C30 		ldrb	r3, [r0, #92]	@ zero_extendqisi2
 4910 0004 012B     		cmp	r3, #1
 4911 0006 0CD0     		beq	.L345
2708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4912              		.loc 1 2708 3 discriminator 2 view .LVU1724
 4913 0008 0123     		movs	r3, #1
 4914 000a 80F85C30 		strb	r3, [r0, #92]
2708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4915              		.loc 1 2708 3 discriminator 2 view .LVU1725
2711:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4916              		.loc 1 2711 3 view .LVU1726
 4917 000e 0268     		ldr	r2, [r0]
 4918 0010 5368     		ldr	r3, [r2, #4]
 4919 0012 23F00303 		bic	r3, r3, #3
 4920 0016 5360     		str	r3, [r2, #4]
2714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4921              		.loc 1 2714 3 view .LVU1727
2714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4922              		.loc 1 2714 3 view .LVU1728
 4923 0018 0023     		movs	r3, #0
 4924 001a 80F85C30 		strb	r3, [r0, #92]
2714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4925              		.loc 1 2714 3 view .LVU1729
2716:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4926              		.loc 1 2716 3 view .LVU1730
2716:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4927              		.loc 1 2716 10 is_stmt 0 view .LVU1731
 4928 001e 1846     		mov	r0, r3
 4929              	.LVL304:
2716:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4930              		.loc 1 2716 10 view .LVU1732
 4931 0020 7047     		bx	lr
 4932              	.LVL305:
 4933              	.L345:
2708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4934              		.loc 1 2708 3 discriminator 1 view .LVU1733
 4935 0022 0220     		movs	r0, #2
 4936              	.LVL306:
2717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4937              		.loc 1 2717 1 view .LVU1734
 4938 0024 7047     		bx	lr
 4939              		.cfi_endproc
 4940              	.LFE138:
 4942              		.section	.text.HAL_SPI_DMAResume,"ax",%progbits
ARM GAS  /tmp/cc5SiBtg.s 			page 193


 4943              		.align	1
 4944              		.global	HAL_SPI_DMAResume
 4945              		.syntax unified
 4946              		.thumb
 4947              		.thumb_func
 4949              	HAL_SPI_DMAResume:
 4950              	.LVL307:
 4951              	.LFB139:
2726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
 4952              		.loc 1 2726 1 is_stmt 1 view -0
 4953              		.cfi_startproc
 4954              		@ args = 0, pretend = 0, frame = 0
 4955              		@ frame_needed = 0, uses_anonymous_args = 0
 4956              		@ link register save eliminated.
2728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4957              		.loc 1 2728 3 view .LVU1736
2728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4958              		.loc 1 2728 3 view .LVU1737
 4959 0000 90F85C30 		ldrb	r3, [r0, #92]	@ zero_extendqisi2
 4960 0004 012B     		cmp	r3, #1
 4961 0006 0CD0     		beq	.L348
2728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4962              		.loc 1 2728 3 discriminator 2 view .LVU1738
 4963 0008 0123     		movs	r3, #1
 4964 000a 80F85C30 		strb	r3, [r0, #92]
2728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4965              		.loc 1 2728 3 discriminator 2 view .LVU1739
2731:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4966              		.loc 1 2731 3 view .LVU1740
 4967 000e 0268     		ldr	r2, [r0]
 4968 0010 5368     		ldr	r3, [r2, #4]
 4969 0012 43F00303 		orr	r3, r3, #3
 4970 0016 5360     		str	r3, [r2, #4]
2734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4971              		.loc 1 2734 3 view .LVU1741
2734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4972              		.loc 1 2734 3 view .LVU1742
 4973 0018 0023     		movs	r3, #0
 4974 001a 80F85C30 		strb	r3, [r0, #92]
2734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4975              		.loc 1 2734 3 view .LVU1743
2736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4976              		.loc 1 2736 3 view .LVU1744
2736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4977              		.loc 1 2736 10 is_stmt 0 view .LVU1745
 4978 001e 1846     		mov	r0, r3
 4979              	.LVL308:
2736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4980              		.loc 1 2736 10 view .LVU1746
 4981 0020 7047     		bx	lr
 4982              	.LVL309:
 4983              	.L348:
2728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4984              		.loc 1 2728 3 discriminator 1 view .LVU1747
 4985 0022 0220     		movs	r0, #2
 4986              	.LVL310:
2737:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 194


 4987              		.loc 1 2737 1 view .LVU1748
 4988 0024 7047     		bx	lr
 4989              		.cfi_endproc
 4990              	.LFE139:
 4992              		.section	.text.HAL_SPI_DMAStop,"ax",%progbits
 4993              		.align	1
 4994              		.global	HAL_SPI_DMAStop
 4995              		.syntax unified
 4996              		.thumb
 4997              		.thumb_func
 4999              	HAL_SPI_DMAStop:
 5000              	.LVL311:
 5001              	.LFB140:
2746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 5002              		.loc 1 2746 1 is_stmt 1 view -0
 5003              		.cfi_startproc
 5004              		@ args = 0, pretend = 0, frame = 0
 5005              		@ frame_needed = 0, uses_anonymous_args = 0
2746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 5006              		.loc 1 2746 1 is_stmt 0 view .LVU1750
 5007 0000 38B5     		push	{r3, r4, r5, lr}
 5008              		.cfi_def_cfa_offset 16
 5009              		.cfi_offset 3, -16
 5010              		.cfi_offset 4, -12
 5011              		.cfi_offset 5, -8
 5012              		.cfi_offset 14, -4
 5013 0002 0446     		mov	r4, r0
2747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* The Lock is not implemented on this API to allow the user application
 5014              		.loc 1 2747 3 is_stmt 1 view .LVU1751
 5015              	.LVL312:
2755:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5016              		.loc 1 2755 3 view .LVU1752
2755:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5017              		.loc 1 2755 11 is_stmt 0 view .LVU1753
 5018 0004 406D     		ldr	r0, [r0, #84]
 5019              	.LVL313:
2755:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5020              		.loc 1 2755 6 view .LVU1754
 5021 0006 48B1     		cbz	r0, .L352
2757:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5022              		.loc 1 2757 5 is_stmt 1 view .LVU1755
2757:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5023              		.loc 1 2757 19 is_stmt 0 view .LVU1756
 5024 0008 FFF7FEFF 		bl	HAL_DMA_Abort
 5025              	.LVL314:
2757:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5026              		.loc 1 2757 8 discriminator 1 view .LVU1757
 5027 000c 0546     		mov	r5, r0
 5028 000e 30B1     		cbz	r0, .L350
2759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_ERROR;
 5029              		.loc 1 2759 7 is_stmt 1 view .LVU1758
 5030 0010 236E     		ldr	r3, [r4, #96]
 5031 0012 43F01003 		orr	r3, r3, #16
 5032 0016 2366     		str	r3, [r4, #96]
2760:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 5033              		.loc 1 2760 7 view .LVU1759
 5034              	.LVL315:
ARM GAS  /tmp/cc5SiBtg.s 			page 195


2760:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 5035              		.loc 1 2760 17 is_stmt 0 view .LVU1760
 5036 0018 0125     		movs	r5, #1
 5037 001a 00E0     		b	.L350
 5038              	.LVL316:
 5039              	.L352:
2747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* The Lock is not implemented on this API to allow the user application
 5040              		.loc 1 2747 21 view .LVU1761
 5041 001c 0025     		movs	r5, #0
 5042              	.LVL317:
 5043              	.L350:
2764:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5044              		.loc 1 2764 3 is_stmt 1 view .LVU1762
2764:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5045              		.loc 1 2764 11 is_stmt 0 view .LVU1763
 5046 001e A06D     		ldr	r0, [r4, #88]
2764:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5047              		.loc 1 2764 6 view .LVU1764
 5048 0020 38B1     		cbz	r0, .L351
2766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5049              		.loc 1 2766 5 is_stmt 1 view .LVU1765
2766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5050              		.loc 1 2766 19 is_stmt 0 view .LVU1766
 5051 0022 FFF7FEFF 		bl	HAL_DMA_Abort
 5052              	.LVL318:
2766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5053              		.loc 1 2766 8 discriminator 1 view .LVU1767
 5054 0026 20B1     		cbz	r0, .L351
2768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_ERROR;
 5055              		.loc 1 2768 7 is_stmt 1 view .LVU1768
 5056 0028 236E     		ldr	r3, [r4, #96]
 5057 002a 43F01003 		orr	r3, r3, #16
 5058 002e 2366     		str	r3, [r4, #96]
2769:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 5059              		.loc 1 2769 7 view .LVU1769
 5060              	.LVL319:
2769:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 5061              		.loc 1 2769 17 is_stmt 0 view .LVU1770
 5062 0030 0125     		movs	r5, #1
 5063              	.LVL320:
 5064              	.L351:
2774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
 5065              		.loc 1 2774 3 is_stmt 1 view .LVU1771
 5066 0032 2268     		ldr	r2, [r4]
 5067 0034 5368     		ldr	r3, [r2, #4]
 5068 0036 23F00303 		bic	r3, r3, #3
 5069 003a 5360     		str	r3, [r2, #4]
2775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 5070              		.loc 1 2775 3 view .LVU1772
2775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 5071              		.loc 1 2775 15 is_stmt 0 view .LVU1773
 5072 003c 0123     		movs	r3, #1
 5073 003e 84F85D30 		strb	r3, [r4, #93]
2776:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 5074              		.loc 1 2776 3 is_stmt 1 view .LVU1774
2777:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5075              		.loc 1 2777 1 is_stmt 0 view .LVU1775
ARM GAS  /tmp/cc5SiBtg.s 			page 196


 5076 0042 2846     		mov	r0, r5
 5077 0044 38BD     		pop	{r3, r4, r5, pc}
2777:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5078              		.loc 1 2777 1 view .LVU1776
 5079              		.cfi_endproc
 5080              	.LFE140:
 5082              		.section	.text.HAL_SPI_TxCpltCallback,"ax",%progbits
 5083              		.align	1
 5084              		.weak	HAL_SPI_TxCpltCallback
 5085              		.syntax unified
 5086              		.thumb
 5087              		.thumb_func
 5089              	HAL_SPI_TxCpltCallback:
 5090              	.LVL321:
 5091              	.LFB142:
2893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5092              		.loc 1 2893 1 is_stmt 1 view -0
 5093              		.cfi_startproc
 5094              		@ args = 0, pretend = 0, frame = 0
 5095              		@ frame_needed = 0, uses_anonymous_args = 0
 5096              		@ link register save eliminated.
2895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5097              		.loc 1 2895 3 view .LVU1778
2900:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5098              		.loc 1 2900 1 is_stmt 0 view .LVU1779
 5099 0000 7047     		bx	lr
 5100              		.cfi_endproc
 5101              	.LFE142:
 5103              		.section	.text.HAL_SPI_RxCpltCallback,"ax",%progbits
 5104              		.align	1
 5105              		.weak	HAL_SPI_RxCpltCallback
 5106              		.syntax unified
 5107              		.thumb
 5108              		.thumb_func
 5110              	HAL_SPI_RxCpltCallback:
 5111              	.LVL322:
 5112              	.LFB143:
2909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5113              		.loc 1 2909 1 is_stmt 1 view -0
 5114              		.cfi_startproc
 5115              		@ args = 0, pretend = 0, frame = 0
 5116              		@ frame_needed = 0, uses_anonymous_args = 0
 5117              		@ link register save eliminated.
2911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5118              		.loc 1 2911 3 view .LVU1781
2916:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5119              		.loc 1 2916 1 is_stmt 0 view .LVU1782
 5120 0000 7047     		bx	lr
 5121              		.cfi_endproc
 5122              	.LFE143:
 5124              		.section	.text.HAL_SPI_TxRxCpltCallback,"ax",%progbits
 5125              		.align	1
 5126              		.weak	HAL_SPI_TxRxCpltCallback
 5127              		.syntax unified
 5128              		.thumb
 5129              		.thumb_func
 5131              	HAL_SPI_TxRxCpltCallback:
ARM GAS  /tmp/cc5SiBtg.s 			page 197


 5132              	.LVL323:
 5133              	.LFB144:
2925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5134              		.loc 1 2925 1 is_stmt 1 view -0
 5135              		.cfi_startproc
 5136              		@ args = 0, pretend = 0, frame = 0
 5137              		@ frame_needed = 0, uses_anonymous_args = 0
 5138              		@ link register save eliminated.
2927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5139              		.loc 1 2927 3 view .LVU1784
2932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5140              		.loc 1 2932 1 is_stmt 0 view .LVU1785
 5141 0000 7047     		bx	lr
 5142              		.cfi_endproc
 5143              	.LFE144:
 5145              		.section	.text.HAL_SPI_TxHalfCpltCallback,"ax",%progbits
 5146              		.align	1
 5147              		.weak	HAL_SPI_TxHalfCpltCallback
 5148              		.syntax unified
 5149              		.thumb
 5150              		.thumb_func
 5152              	HAL_SPI_TxHalfCpltCallback:
 5153              	.LVL324:
 5154              	.LFB145:
2941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5155              		.loc 1 2941 1 is_stmt 1 view -0
 5156              		.cfi_startproc
 5157              		@ args = 0, pretend = 0, frame = 0
 5158              		@ frame_needed = 0, uses_anonymous_args = 0
 5159              		@ link register save eliminated.
2943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5160              		.loc 1 2943 3 view .LVU1787
2948:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5161              		.loc 1 2948 1 is_stmt 0 view .LVU1788
 5162 0000 7047     		bx	lr
 5163              		.cfi_endproc
 5164              	.LFE145:
 5166              		.section	.text.SPI_DMAHalfTransmitCplt,"ax",%progbits
 5167              		.align	1
 5168              		.syntax unified
 5169              		.thumb
 5170              		.thumb_func
 5172              	SPI_DMAHalfTransmitCplt:
 5173              	.LVL325:
 5174              	.LFB155:
3353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 5175              		.loc 1 3353 1 is_stmt 1 view -0
 5176              		.cfi_startproc
 5177              		@ args = 0, pretend = 0, frame = 0
 5178              		@ frame_needed = 0, uses_anonymous_args = 0
3353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 5179              		.loc 1 3353 1 is_stmt 0 view .LVU1790
 5180 0000 08B5     		push	{r3, lr}
 5181              		.cfi_def_cfa_offset 8
 5182              		.cfi_offset 3, -8
 5183              		.cfi_offset 14, -4
3354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 198


 5184              		.loc 1 3354 3 is_stmt 1 view .LVU1791
 5185              	.LVL326:
3360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5186              		.loc 1 3360 3 view .LVU1792
 5187 0002 406A     		ldr	r0, [r0, #36]
 5188              	.LVL327:
3360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5189              		.loc 1 3360 3 is_stmt 0 view .LVU1793
 5190 0004 FFF7FEFF 		bl	HAL_SPI_TxHalfCpltCallback
 5191              	.LVL328:
3362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5192              		.loc 1 3362 1 view .LVU1794
 5193 0008 08BD     		pop	{r3, pc}
 5194              		.cfi_endproc
 5195              	.LFE155:
 5197              		.section	.text.HAL_SPI_RxHalfCpltCallback,"ax",%progbits
 5198              		.align	1
 5199              		.weak	HAL_SPI_RxHalfCpltCallback
 5200              		.syntax unified
 5201              		.thumb
 5202              		.thumb_func
 5204              	HAL_SPI_RxHalfCpltCallback:
 5205              	.LVL329:
 5206              	.LFB146:
2957:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5207              		.loc 1 2957 1 is_stmt 1 view -0
 5208              		.cfi_startproc
 5209              		@ args = 0, pretend = 0, frame = 0
 5210              		@ frame_needed = 0, uses_anonymous_args = 0
 5211              		@ link register save eliminated.
2959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5212              		.loc 1 2959 3 view .LVU1796
2964:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5213              		.loc 1 2964 1 is_stmt 0 view .LVU1797
 5214 0000 7047     		bx	lr
 5215              		.cfi_endproc
 5216              	.LFE146:
 5218              		.section	.text.SPI_DMAHalfReceiveCplt,"ax",%progbits
 5219              		.align	1
 5220              		.syntax unified
 5221              		.thumb
 5222              		.thumb_func
 5224              	SPI_DMAHalfReceiveCplt:
 5225              	.LVL330:
 5226              	.LFB156:
3371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 5227              		.loc 1 3371 1 is_stmt 1 view -0
 5228              		.cfi_startproc
 5229              		@ args = 0, pretend = 0, frame = 0
 5230              		@ frame_needed = 0, uses_anonymous_args = 0
3371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 5231              		.loc 1 3371 1 is_stmt 0 view .LVU1799
 5232 0000 08B5     		push	{r3, lr}
 5233              		.cfi_def_cfa_offset 8
 5234              		.cfi_offset 3, -8
 5235              		.cfi_offset 14, -4
3372:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 199


 5236              		.loc 1 3372 3 is_stmt 1 view .LVU1800
 5237              	.LVL331:
3378:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5238              		.loc 1 3378 3 view .LVU1801
 5239 0002 406A     		ldr	r0, [r0, #36]
 5240              	.LVL332:
3378:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5241              		.loc 1 3378 3 is_stmt 0 view .LVU1802
 5242 0004 FFF7FEFF 		bl	HAL_SPI_RxHalfCpltCallback
 5243              	.LVL333:
3380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5244              		.loc 1 3380 1 view .LVU1803
 5245 0008 08BD     		pop	{r3, pc}
 5246              		.cfi_endproc
 5247              	.LFE156:
 5249              		.section	.text.HAL_SPI_TxRxHalfCpltCallback,"ax",%progbits
 5250              		.align	1
 5251              		.weak	HAL_SPI_TxRxHalfCpltCallback
 5252              		.syntax unified
 5253              		.thumb
 5254              		.thumb_func
 5256              	HAL_SPI_TxRxHalfCpltCallback:
 5257              	.LVL334:
 5258              	.LFB147:
2973:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5259              		.loc 1 2973 1 is_stmt 1 view -0
 5260              		.cfi_startproc
 5261              		@ args = 0, pretend = 0, frame = 0
 5262              		@ frame_needed = 0, uses_anonymous_args = 0
 5263              		@ link register save eliminated.
2975:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5264              		.loc 1 2975 3 view .LVU1805
2980:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5265              		.loc 1 2980 1 is_stmt 0 view .LVU1806
 5266 0000 7047     		bx	lr
 5267              		.cfi_endproc
 5268              	.LFE147:
 5270              		.section	.text.SPI_DMAHalfTransmitReceiveCplt,"ax",%progbits
 5271              		.align	1
 5272              		.syntax unified
 5273              		.thumb
 5274              		.thumb_func
 5276              	SPI_DMAHalfTransmitReceiveCplt:
 5277              	.LVL335:
 5278              	.LFB157:
3389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 5279              		.loc 1 3389 1 is_stmt 1 view -0
 5280              		.cfi_startproc
 5281              		@ args = 0, pretend = 0, frame = 0
 5282              		@ frame_needed = 0, uses_anonymous_args = 0
3389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 5283              		.loc 1 3389 1 is_stmt 0 view .LVU1808
 5284 0000 08B5     		push	{r3, lr}
 5285              		.cfi_def_cfa_offset 8
 5286              		.cfi_offset 3, -8
 5287              		.cfi_offset 14, -4
3390:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 200


 5288              		.loc 1 3390 3 is_stmt 1 view .LVU1809
 5289              	.LVL336:
3396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5290              		.loc 1 3396 3 view .LVU1810
 5291 0002 406A     		ldr	r0, [r0, #36]
 5292              	.LVL337:
3396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5293              		.loc 1 3396 3 is_stmt 0 view .LVU1811
 5294 0004 FFF7FEFF 		bl	HAL_SPI_TxRxHalfCpltCallback
 5295              	.LVL338:
3398:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5296              		.loc 1 3398 1 view .LVU1812
 5297 0008 08BD     		pop	{r3, pc}
 5298              		.cfi_endproc
 5299              	.LFE157:
 5301              		.section	.text.HAL_SPI_ErrorCallback,"ax",%progbits
 5302              		.align	1
 5303              		.weak	HAL_SPI_ErrorCallback
 5304              		.syntax unified
 5305              		.thumb
 5306              		.thumb_func
 5308              	HAL_SPI_ErrorCallback:
 5309              	.LVL339:
 5310              	.LFB148:
2989:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5311              		.loc 1 2989 1 is_stmt 1 view -0
 5312              		.cfi_startproc
 5313              		@ args = 0, pretend = 0, frame = 0
 5314              		@ frame_needed = 0, uses_anonymous_args = 0
 5315              		@ link register save eliminated.
2991:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5316              		.loc 1 2991 3 view .LVU1814
2999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5317              		.loc 1 2999 1 is_stmt 0 view .LVU1815
 5318 0000 7047     		bx	lr
 5319              		.cfi_endproc
 5320              	.LFE148:
 5322              		.section	.text.SPI_CloseTx_ISR,"ax",%progbits
 5323              		.align	1
 5324              		.syntax unified
 5325              		.thumb
 5326              		.thumb_func
 5328              	SPI_CloseTx_ISR:
 5329              	.LVL340:
 5330              	.LFB176:
4331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 5331              		.loc 1 4331 1 is_stmt 1 view -0
 5332              		.cfi_startproc
 5333              		@ args = 0, pretend = 0, frame = 8
 5334              		@ frame_needed = 0, uses_anonymous_args = 0
4331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 5335              		.loc 1 4331 1 is_stmt 0 view .LVU1817
 5336 0000 10B5     		push	{r4, lr}
 5337              		.cfi_def_cfa_offset 8
 5338              		.cfi_offset 4, -8
 5339              		.cfi_offset 14, -4
 5340 0002 82B0     		sub	sp, sp, #8
ARM GAS  /tmp/cc5SiBtg.s 			page 201


 5341              		.cfi_def_cfa_offset 16
 5342 0004 0446     		mov	r4, r0
4332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5343              		.loc 1 4332 3 is_stmt 1 view .LVU1818
4335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5344              		.loc 1 4335 3 view .LVU1819
4335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5345              		.loc 1 4335 15 is_stmt 0 view .LVU1820
 5346 0006 FFF7FEFF 		bl	HAL_GetTick
 5347              	.LVL341:
4335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5348              		.loc 1 4335 15 view .LVU1821
 5349 000a 0246     		mov	r2, r0
 5350              	.LVL342:
4338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5351              		.loc 1 4338 3 is_stmt 1 view .LVU1822
 5352 000c 2168     		ldr	r1, [r4]
 5353 000e 4B68     		ldr	r3, [r1, #4]
 5354 0010 23F0A003 		bic	r3, r3, #160
 5355 0014 4B60     		str	r3, [r1, #4]
4341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5356              		.loc 1 4341 3 view .LVU1823
4341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5357              		.loc 1 4341 7 is_stmt 0 view .LVU1824
 5358 0016 6421     		movs	r1, #100
 5359 0018 2046     		mov	r0, r4
 5360              	.LVL343:
4341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5361              		.loc 1 4341 7 view .LVU1825
 5362 001a FFF7FEFF 		bl	SPI_EndRxTxTransaction
 5363              	.LVL344:
4341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5364              		.loc 1 4341 6 discriminator 1 view .LVU1826
 5365 001e 18B1     		cbz	r0, .L368
4343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5366              		.loc 1 4343 5 is_stmt 1 view .LVU1827
 5367 0020 236E     		ldr	r3, [r4, #96]
 5368 0022 43F02003 		orr	r3, r3, #32
 5369 0026 2366     		str	r3, [r4, #96]
 5370              	.L368:
4347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5371              		.loc 1 4347 3 view .LVU1828
4347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5372              		.loc 1 4347 17 is_stmt 0 view .LVU1829
 5373 0028 A368     		ldr	r3, [r4, #8]
4347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5374              		.loc 1 4347 6 view .LVU1830
 5375 002a 33B9     		cbnz	r3, .L369
4349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5376              		.loc 1 4349 5 is_stmt 1 view .LVU1831
 5377              	.LBB5:
4349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5378              		.loc 1 4349 5 view .LVU1832
 5379 002c 0193     		str	r3, [sp, #4]
4349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5380              		.loc 1 4349 5 view .LVU1833
 5381 002e 2368     		ldr	r3, [r4]
ARM GAS  /tmp/cc5SiBtg.s 			page 202


 5382 0030 DA68     		ldr	r2, [r3, #12]
 5383 0032 0192     		str	r2, [sp, #4]
4349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5384              		.loc 1 4349 5 view .LVU1834
 5385 0034 9B68     		ldr	r3, [r3, #8]
 5386 0036 0193     		str	r3, [sp, #4]
4349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5387              		.loc 1 4349 5 view .LVU1835
 5388 0038 019B     		ldr	r3, [sp, #4]
 5389              	.L369:
 5390              	.LBE5:
4349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5391              		.loc 1 4349 5 discriminator 1 view .LVU1836
4352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
 5392              		.loc 1 4352 3 view .LVU1837
4352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
 5393              		.loc 1 4352 15 is_stmt 0 view .LVU1838
 5394 003a 0123     		movs	r3, #1
 5395 003c 84F85D30 		strb	r3, [r4, #93]
4353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5396              		.loc 1 4353 3 is_stmt 1 view .LVU1839
4353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5397              		.loc 1 4353 11 is_stmt 0 view .LVU1840
 5398 0040 236E     		ldr	r3, [r4, #96]
4353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5399              		.loc 1 4353 6 view .LVU1841
 5400 0042 23B1     		cbz	r3, .L370
4359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5401              		.loc 1 4359 5 is_stmt 1 view .LVU1842
 5402 0044 2046     		mov	r0, r4
 5403 0046 FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 5404              	.LVL345:
 5405              	.L367:
4371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5406              		.loc 1 4371 1 is_stmt 0 view .LVU1843
 5407 004a 02B0     		add	sp, sp, #8
 5408              		.cfi_remember_state
 5409              		.cfi_def_cfa_offset 8
 5410              		@ sp needed
 5411 004c 10BD     		pop	{r4, pc}
 5412              	.LVL346:
 5413              	.L370:
 5414              		.cfi_restore_state
4368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5415              		.loc 1 4368 5 is_stmt 1 view .LVU1844
 5416 004e 2046     		mov	r0, r4
 5417 0050 FFF7FEFF 		bl	HAL_SPI_TxCpltCallback
 5418              	.LVL347:
4371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5419              		.loc 1 4371 1 is_stmt 0 view .LVU1845
 5420 0054 F9E7     		b	.L367
 5421              		.cfi_endproc
 5422              	.LFE176:
 5424              		.section	.text.SPI_TxISR_8BIT,"ax",%progbits
 5425              		.align	1
 5426              		.syntax unified
 5427              		.thumb
ARM GAS  /tmp/cc5SiBtg.s 			page 203


 5428              		.thumb_func
 5430              	SPI_TxISR_8BIT:
 5431              	.LVL348:
 5432              	.LFB168:
3925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *(__IO uint8_t *)&hspi->Instance->DR = (*hspi->pTxBuffPtr);
 5433              		.loc 1 3925 1 is_stmt 1 view -0
 5434              		.cfi_startproc
 5435              		@ args = 0, pretend = 0, frame = 0
 5436              		@ frame_needed = 0, uses_anonymous_args = 0
3925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *(__IO uint8_t *)&hspi->Instance->DR = (*hspi->pTxBuffPtr);
 5437              		.loc 1 3925 1 is_stmt 0 view .LVU1847
 5438 0000 08B5     		push	{r3, lr}
 5439              		.cfi_def_cfa_offset 8
 5440              		.cfi_offset 3, -8
 5441              		.cfi_offset 14, -4
3926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr++;
 5442              		.loc 1 3926 3 is_stmt 1 view .LVU1848
3926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr++;
 5443              		.loc 1 3926 48 is_stmt 0 view .LVU1849
 5444 0002 826B     		ldr	r2, [r0, #56]
3926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr++;
 5445              		.loc 1 3926 25 view .LVU1850
 5446 0004 0368     		ldr	r3, [r0]
3926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr++;
 5447              		.loc 1 3926 43 view .LVU1851
 5448 0006 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
3926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr++;
 5449              		.loc 1 3926 40 view .LVU1852
 5450 0008 1A73     		strb	r2, [r3, #12]
3927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 5451              		.loc 1 3927 3 is_stmt 1 view .LVU1853
3927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 5452              		.loc 1 3927 7 is_stmt 0 view .LVU1854
 5453 000a 836B     		ldr	r3, [r0, #56]
3927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 5454              		.loc 1 3927 19 view .LVU1855
 5455 000c 0133     		adds	r3, r3, #1
 5456 000e 8363     		str	r3, [r0, #56]
3928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5457              		.loc 1 3928 3 is_stmt 1 view .LVU1856
3928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5458              		.loc 1 3928 7 is_stmt 0 view .LVU1857
 5459 0010 C38F     		ldrh	r3, [r0, #62]
 5460 0012 9BB2     		uxth	r3, r3
3928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5461              		.loc 1 3928 20 view .LVU1858
 5462 0014 013B     		subs	r3, r3, #1
 5463 0016 9BB2     		uxth	r3, r3
 5464 0018 C387     		strh	r3, [r0, #62]	@ movhi
3930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5465              		.loc 1 3930 3 is_stmt 1 view .LVU1859
3930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5466              		.loc 1 3930 11 is_stmt 0 view .LVU1860
 5467 001a C38F     		ldrh	r3, [r0, #62]
 5468 001c 9BB2     		uxth	r3, r3
3930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5469              		.loc 1 3930 6 view .LVU1861
ARM GAS  /tmp/cc5SiBtg.s 			page 204


 5470 001e 03B1     		cbz	r3, .L376
 5471              	.LVL349:
 5472              	.L373:
3941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5473              		.loc 1 3941 1 view .LVU1862
 5474 0020 08BD     		pop	{r3, pc}
 5475              	.LVL350:
 5476              	.L376:
3939:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5477              		.loc 1 3939 5 is_stmt 1 view .LVU1863
 5478 0022 FFF7FEFF 		bl	SPI_CloseTx_ISR
 5479              	.LVL351:
3941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5480              		.loc 1 3941 1 is_stmt 0 view .LVU1864
 5481 0026 FBE7     		b	.L373
 5482              		.cfi_endproc
 5483              	.LFE168:
 5485              		.section	.text.SPI_TxISR_16BIT,"ax",%progbits
 5486              		.align	1
 5487              		.syntax unified
 5488              		.thumb
 5489              		.thumb_func
 5491              	SPI_TxISR_16BIT:
 5492              	.LVL352:
 5493              	.LFB169:
3950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
 5494              		.loc 1 3950 1 is_stmt 1 view -0
 5495              		.cfi_startproc
 5496              		@ args = 0, pretend = 0, frame = 0
 5497              		@ frame_needed = 0, uses_anonymous_args = 0
3950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
 5498              		.loc 1 3950 1 is_stmt 0 view .LVU1866
 5499 0000 08B5     		push	{r3, lr}
 5500              		.cfi_def_cfa_offset 8
 5501              		.cfi_offset 3, -8
 5502              		.cfi_offset 14, -4
3952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 5503              		.loc 1 3952 3 is_stmt 1 view .LVU1867
3952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 5504              		.loc 1 3952 42 is_stmt 0 view .LVU1868
 5505 0002 826B     		ldr	r2, [r0, #56]
3952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 5506              		.loc 1 3952 7 view .LVU1869
 5507 0004 0368     		ldr	r3, [r0]
3952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 5508              		.loc 1 3952 24 view .LVU1870
 5509 0006 1288     		ldrh	r2, [r2]
3952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 5510              		.loc 1 3952 22 view .LVU1871
 5511 0008 DA60     		str	r2, [r3, #12]
3953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 5512              		.loc 1 3953 3 is_stmt 1 view .LVU1872
3953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 5513              		.loc 1 3953 7 is_stmt 0 view .LVU1873
 5514 000a 836B     		ldr	r3, [r0, #56]
3953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 5515              		.loc 1 3953 20 view .LVU1874
ARM GAS  /tmp/cc5SiBtg.s 			page 205


 5516 000c 0233     		adds	r3, r3, #2
 5517 000e 8363     		str	r3, [r0, #56]
3954:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5518              		.loc 1 3954 3 is_stmt 1 view .LVU1875
3954:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5519              		.loc 1 3954 7 is_stmt 0 view .LVU1876
 5520 0010 C38F     		ldrh	r3, [r0, #62]
 5521 0012 9BB2     		uxth	r3, r3
3954:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5522              		.loc 1 3954 20 view .LVU1877
 5523 0014 013B     		subs	r3, r3, #1
 5524 0016 9BB2     		uxth	r3, r3
 5525 0018 C387     		strh	r3, [r0, #62]	@ movhi
3956:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5526              		.loc 1 3956 3 is_stmt 1 view .LVU1878
3956:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5527              		.loc 1 3956 11 is_stmt 0 view .LVU1879
 5528 001a C38F     		ldrh	r3, [r0, #62]
 5529 001c 9BB2     		uxth	r3, r3
3956:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5530              		.loc 1 3956 6 view .LVU1880
 5531 001e 03B1     		cbz	r3, .L380
 5532              	.LVL353:
 5533              	.L377:
3967:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5534              		.loc 1 3967 1 view .LVU1881
 5535 0020 08BD     		pop	{r3, pc}
 5536              	.LVL354:
 5537              	.L380:
3965:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5538              		.loc 1 3965 5 is_stmt 1 view .LVU1882
 5539 0022 FFF7FEFF 		bl	SPI_CloseTx_ISR
 5540              	.LVL355:
3967:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5541              		.loc 1 3967 1 is_stmt 0 view .LVU1883
 5542 0026 FBE7     		b	.L377
 5543              		.cfi_endproc
 5544              	.LFE169:
 5546              		.section	.text.SPI_CloseRx_ISR,"ax",%progbits
 5547              		.align	1
 5548              		.syntax unified
 5549              		.thumb
 5550              		.thumb_func
 5552              	SPI_CloseRx_ISR:
 5553              	.LVL356:
 5554              	.LFB175:
4274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable RXNE and ERR interrupt */
 5555              		.loc 1 4274 1 is_stmt 1 view -0
 5556              		.cfi_startproc
 5557              		@ args = 0, pretend = 0, frame = 0
 5558              		@ frame_needed = 0, uses_anonymous_args = 0
4274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable RXNE and ERR interrupt */
 5559              		.loc 1 4274 1 is_stmt 0 view .LVU1885
 5560 0000 10B5     		push	{r4, lr}
 5561              		.cfi_def_cfa_offset 8
 5562              		.cfi_offset 4, -8
 5563              		.cfi_offset 14, -4
ARM GAS  /tmp/cc5SiBtg.s 			page 206


 5564 0002 0446     		mov	r4, r0
4276:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5565              		.loc 1 4276 3 is_stmt 1 view .LVU1886
 5566 0004 0268     		ldr	r2, [r0]
 5567 0006 5368     		ldr	r3, [r2, #4]
 5568 0008 23F06003 		bic	r3, r3, #96
 5569 000c 5360     		str	r3, [r2, #4]
4279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5570              		.loc 1 4279 3 view .LVU1887
4279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5571              		.loc 1 4279 7 is_stmt 0 view .LVU1888
 5572 000e FFF7FEFF 		bl	HAL_GetTick
 5573              	.LVL357:
4279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5574              		.loc 1 4279 7 view .LVU1889
 5575 0012 0246     		mov	r2, r0
4279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5576              		.loc 1 4279 7 discriminator 1 view .LVU1890
 5577 0014 6421     		movs	r1, #100
 5578 0016 2046     		mov	r0, r4
 5579 0018 FFF7FEFF 		bl	SPI_EndRxTransaction
 5580              	.LVL358:
4279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5581              		.loc 1 4279 6 discriminator 2 view .LVU1891
 5582 001c 18B1     		cbz	r0, .L382
4281:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5583              		.loc 1 4281 5 is_stmt 1 view .LVU1892
 5584 001e 236E     		ldr	r3, [r4, #96]
 5585 0020 43F02003 		orr	r3, r3, #32
 5586 0024 2366     		str	r3, [r4, #96]
 5587              	.L382:
4283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5588              		.loc 1 4283 3 view .LVU1893
4283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5589              		.loc 1 4283 15 is_stmt 0 view .LVU1894
 5590 0026 0123     		movs	r3, #1
 5591 0028 84F85D30 		strb	r3, [r4, #93]
4301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5592              		.loc 1 4301 5 is_stmt 1 view .LVU1895
4301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5593              		.loc 1 4301 13 is_stmt 0 view .LVU1896
 5594 002c 236E     		ldr	r3, [r4, #96]
4301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5595              		.loc 1 4301 8 view .LVU1897
 5596 002e 1BB9     		cbnz	r3, .L383
4307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5597              		.loc 1 4307 7 is_stmt 1 view .LVU1898
 5598 0030 2046     		mov	r0, r4
 5599 0032 FFF7FEFF 		bl	HAL_SPI_RxCpltCallback
 5600              	.LVL359:
 5601              	.L381:
4322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5602              		.loc 1 4322 1 is_stmt 0 view .LVU1899
 5603 0036 10BD     		pop	{r4, pc}
 5604              	.LVL360:
 5605              	.L383:
4316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
ARM GAS  /tmp/cc5SiBtg.s 			page 207


 5606              		.loc 1 4316 7 is_stmt 1 view .LVU1900
 5607 0038 2046     		mov	r0, r4
 5608 003a FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 5609              	.LVL361:
4322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5610              		.loc 1 4322 1 is_stmt 0 view .LVU1901
 5611 003e FAE7     		b	.L381
 5612              		.cfi_endproc
 5613              	.LFE175:
 5615              		.section	.text.SPI_RxISR_8BIT,"ax",%progbits
 5616              		.align	1
 5617              		.syntax unified
 5618              		.thumb
 5619              		.thumb_func
 5621              	SPI_RxISR_8BIT:
 5622              	.LVL362:
 5623              	.LFB166:
3836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *hspi->pRxBuffPtr = (*(__IO uint8_t *)&hspi->Instance->DR);
 5624              		.loc 1 3836 1 is_stmt 1 view -0
 5625              		.cfi_startproc
 5626              		@ args = 0, pretend = 0, frame = 0
 5627              		@ frame_needed = 0, uses_anonymous_args = 0
3836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *hspi->pRxBuffPtr = (*(__IO uint8_t *)&hspi->Instance->DR);
 5628              		.loc 1 3836 1 is_stmt 0 view .LVU1903
 5629 0000 08B5     		push	{r3, lr}
 5630              		.cfi_def_cfa_offset 8
 5631              		.cfi_offset 3, -8
 5632              		.cfi_offset 14, -4
3837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr++;
 5633              		.loc 1 3837 3 is_stmt 1 view .LVU1904
3837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr++;
 5634              		.loc 1 3837 46 is_stmt 0 view .LVU1905
 5635 0002 0268     		ldr	r2, [r0]
3837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr++;
 5636              		.loc 1 3837 8 view .LVU1906
 5637 0004 036C     		ldr	r3, [r0, #64]
3837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr++;
 5638              		.loc 1 3837 24 view .LVU1907
 5639 0006 127B     		ldrb	r2, [r2, #12]	@ zero_extendqisi2
3837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr++;
 5640              		.loc 1 3837 21 view .LVU1908
 5641 0008 1A70     		strb	r2, [r3]
3838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 5642              		.loc 1 3838 3 is_stmt 1 view .LVU1909
3838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 5643              		.loc 1 3838 7 is_stmt 0 view .LVU1910
 5644 000a 036C     		ldr	r3, [r0, #64]
3838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 5645              		.loc 1 3838 19 view .LVU1911
 5646 000c 0133     		adds	r3, r3, #1
 5647 000e 0364     		str	r3, [r0, #64]
3839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5648              		.loc 1 3839 3 is_stmt 1 view .LVU1912
3839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5649              		.loc 1 3839 7 is_stmt 0 view .LVU1913
 5650 0010 B0F84630 		ldrh	r3, [r0, #70]
 5651 0014 9BB2     		uxth	r3, r3
ARM GAS  /tmp/cc5SiBtg.s 			page 208


3839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5652              		.loc 1 3839 20 view .LVU1914
 5653 0016 013B     		subs	r3, r3, #1
 5654 0018 9BB2     		uxth	r3, r3
 5655 001a A0F84630 		strh	r3, [r0, #70]	@ movhi
3849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5656              		.loc 1 3849 3 is_stmt 1 view .LVU1915
3849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5657              		.loc 1 3849 11 is_stmt 0 view .LVU1916
 5658 001e B0F84630 		ldrh	r3, [r0, #70]
 5659 0022 9BB2     		uxth	r3, r3
3849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5660              		.loc 1 3849 6 view .LVU1917
 5661 0024 03B1     		cbz	r3, .L389
 5662              	.LVL363:
 5663              	.L386:
3860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5664              		.loc 1 3860 1 view .LVU1918
 5665 0026 08BD     		pop	{r3, pc}
 5666              	.LVL364:
 5667              	.L389:
3858:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5668              		.loc 1 3858 5 is_stmt 1 view .LVU1919
 5669 0028 FFF7FEFF 		bl	SPI_CloseRx_ISR
 5670              	.LVL365:
3860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5671              		.loc 1 3860 1 is_stmt 0 view .LVU1920
 5672 002c FBE7     		b	.L386
 5673              		.cfi_endproc
 5674              	.LFE166:
 5676              		.section	.text.SPI_RxISR_16BIT,"ax",%progbits
 5677              		.align	1
 5678              		.syntax unified
 5679              		.thumb
 5680              		.thumb_func
 5682              	SPI_RxISR_16BIT:
 5683              	.LVL366:
 5684              	.LFB167:
3892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)(hspi->Instance->DR);
 5685              		.loc 1 3892 1 is_stmt 1 view -0
 5686              		.cfi_startproc
 5687              		@ args = 0, pretend = 0, frame = 0
 5688              		@ frame_needed = 0, uses_anonymous_args = 0
3892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)(hspi->Instance->DR);
 5689              		.loc 1 3892 1 is_stmt 0 view .LVU1922
 5690 0000 08B5     		push	{r3, lr}
 5691              		.cfi_def_cfa_offset 8
 5692              		.cfi_offset 3, -8
 5693              		.cfi_offset 14, -4
3893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 5694              		.loc 1 3893 3 is_stmt 1 view .LVU1923
3893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 5695              		.loc 1 3893 52 is_stmt 0 view .LVU1924
 5696 0002 0368     		ldr	r3, [r0]
3893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 5697              		.loc 1 3893 62 view .LVU1925
 5698 0004 DA68     		ldr	r2, [r3, #12]
ARM GAS  /tmp/cc5SiBtg.s 			page 209


3893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 5699              		.loc 1 3893 21 view .LVU1926
 5700 0006 036C     		ldr	r3, [r0, #64]
3893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 5701              		.loc 1 3893 35 view .LVU1927
 5702 0008 1A80     		strh	r2, [r3]	@ movhi
3894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 5703              		.loc 1 3894 3 is_stmt 1 view .LVU1928
3894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 5704              		.loc 1 3894 7 is_stmt 0 view .LVU1929
 5705 000a 036C     		ldr	r3, [r0, #64]
3894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 5706              		.loc 1 3894 20 view .LVU1930
 5707 000c 0233     		adds	r3, r3, #2
 5708 000e 0364     		str	r3, [r0, #64]
3895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5709              		.loc 1 3895 3 is_stmt 1 view .LVU1931
3895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5710              		.loc 1 3895 7 is_stmt 0 view .LVU1932
 5711 0010 B0F84630 		ldrh	r3, [r0, #70]
 5712 0014 9BB2     		uxth	r3, r3
3895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5713              		.loc 1 3895 20 view .LVU1933
 5714 0016 013B     		subs	r3, r3, #1
 5715 0018 9BB2     		uxth	r3, r3
 5716 001a A0F84630 		strh	r3, [r0, #70]	@ movhi
3905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5717              		.loc 1 3905 3 is_stmt 1 view .LVU1934
3905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5718              		.loc 1 3905 11 is_stmt 0 view .LVU1935
 5719 001e B0F84630 		ldrh	r3, [r0, #70]
 5720 0022 9BB2     		uxth	r3, r3
3905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5721              		.loc 1 3905 6 view .LVU1936
 5722 0024 03B1     		cbz	r3, .L393
 5723              	.LVL367:
 5724              	.L390:
3916:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5725              		.loc 1 3916 1 view .LVU1937
 5726 0026 08BD     		pop	{r3, pc}
 5727              	.LVL368:
 5728              	.L393:
3914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5729              		.loc 1 3914 5 is_stmt 1 view .LVU1938
 5730 0028 FFF7FEFF 		bl	SPI_CloseRx_ISR
 5731              	.LVL369:
3916:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5732              		.loc 1 3916 1 is_stmt 0 view .LVU1939
 5733 002c FBE7     		b	.L390
 5734              		.cfi_endproc
 5735              	.LFE167:
 5737              		.section	.text.SPI_CloseRxTx_ISR,"ax",%progbits
 5738              		.align	1
 5739              		.syntax unified
 5740              		.thumb
 5741              		.thumb_func
 5743              	SPI_CloseRxTx_ISR:
ARM GAS  /tmp/cc5SiBtg.s 			page 210


 5744              	.LVL370:
 5745              	.LFB174:
4197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 5746              		.loc 1 4197 1 is_stmt 1 view -0
 5747              		.cfi_startproc
 5748              		@ args = 0, pretend = 0, frame = 0
 5749              		@ frame_needed = 0, uses_anonymous_args = 0
4197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 5750              		.loc 1 4197 1 is_stmt 0 view .LVU1941
 5751 0000 10B5     		push	{r4, lr}
 5752              		.cfi_def_cfa_offset 8
 5753              		.cfi_offset 4, -8
 5754              		.cfi_offset 14, -4
 5755 0002 0446     		mov	r4, r0
4198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5756              		.loc 1 4198 3 is_stmt 1 view .LVU1942
4201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5757              		.loc 1 4201 3 view .LVU1943
4201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5758              		.loc 1 4201 15 is_stmt 0 view .LVU1944
 5759 0004 FFF7FEFF 		bl	HAL_GetTick
 5760              	.LVL371:
4201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5761              		.loc 1 4201 15 view .LVU1945
 5762 0008 0246     		mov	r2, r0
 5763              	.LVL372:
4204:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5764              		.loc 1 4204 3 is_stmt 1 view .LVU1946
 5765 000a 2168     		ldr	r1, [r4]
 5766 000c 4B68     		ldr	r3, [r1, #4]
 5767 000e 23F02003 		bic	r3, r3, #32
 5768 0012 4B60     		str	r3, [r1, #4]
4207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5769              		.loc 1 4207 3 view .LVU1947
4207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5770              		.loc 1 4207 7 is_stmt 0 view .LVU1948
 5771 0014 6421     		movs	r1, #100
 5772 0016 2046     		mov	r0, r4
 5773              	.LVL373:
4207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5774              		.loc 1 4207 7 view .LVU1949
 5775 0018 FFF7FEFF 		bl	SPI_EndRxTxTransaction
 5776              	.LVL374:
4207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5777              		.loc 1 4207 6 discriminator 1 view .LVU1950
 5778 001c 18B1     		cbz	r0, .L395
4209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5779              		.loc 1 4209 5 is_stmt 1 view .LVU1951
 5780 001e 236E     		ldr	r3, [r4, #96]
 5781 0020 43F02003 		orr	r3, r3, #32
 5782 0024 2366     		str	r3, [r4, #96]
 5783              	.L395:
4229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5784              		.loc 1 4229 5 view .LVU1952
4229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5785              		.loc 1 4229 13 is_stmt 0 view .LVU1953
 5786 0026 236E     		ldr	r3, [r4, #96]
ARM GAS  /tmp/cc5SiBtg.s 			page 211


4229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5787              		.loc 1 4229 8 view .LVU1954
 5788 0028 93B9     		cbnz	r3, .L396
4231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 5789              		.loc 1 4231 7 is_stmt 1 view .LVU1955
4231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 5790              		.loc 1 4231 15 is_stmt 0 view .LVU1956
 5791 002a 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 5792 002e DBB2     		uxtb	r3, r3
4231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 5793              		.loc 1 4231 10 view .LVU1957
 5794 0030 042B     		cmp	r3, #4
 5795 0032 06D0     		beq	.L400
4243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user TxRx complete callback */
 5796              		.loc 1 4243 9 is_stmt 1 view .LVU1958
4243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user TxRx complete callback */
 5797              		.loc 1 4243 21 is_stmt 0 view .LVU1959
 5798 0034 0123     		movs	r3, #1
 5799 0036 84F85D30 		strb	r3, [r4, #93]
4248:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5800              		.loc 1 4248 9 is_stmt 1 view .LVU1960
 5801 003a 2046     		mov	r0, r4
 5802 003c FFF7FEFF 		bl	HAL_SPI_TxRxCpltCallback
 5803              	.LVL375:
 5804              	.L394:
4265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5805              		.loc 1 4265 1 is_stmt 0 view .LVU1961
 5806 0040 10BD     		pop	{r4, pc}
 5807              	.LVL376:
 5808              	.L400:
4233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user Rx complete callback */
 5809              		.loc 1 4233 9 is_stmt 1 view .LVU1962
4233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user Rx complete callback */
 5810              		.loc 1 4233 21 is_stmt 0 view .LVU1963
 5811 0042 0123     		movs	r3, #1
 5812 0044 84F85D30 		strb	r3, [r4, #93]
4238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5813              		.loc 1 4238 9 is_stmt 1 view .LVU1964
 5814 0048 2046     		mov	r0, r4
 5815 004a FFF7FEFF 		bl	HAL_SPI_RxCpltCallback
 5816              	.LVL377:
 5817 004e F7E7     		b	.L394
 5818              	.L396:
4254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
 5819              		.loc 1 4254 7 view .LVU1965
4254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
 5820              		.loc 1 4254 19 is_stmt 0 view .LVU1966
 5821 0050 0123     		movs	r3, #1
 5822 0052 84F85D30 		strb	r3, [r4, #93]
4259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5823              		.loc 1 4259 7 is_stmt 1 view .LVU1967
 5824 0056 2046     		mov	r0, r4
 5825 0058 FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 5826              	.LVL378:
4265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5827              		.loc 1 4265 1 is_stmt 0 view .LVU1968
 5828 005c F0E7     		b	.L394
ARM GAS  /tmp/cc5SiBtg.s 			page 212


 5829              		.cfi_endproc
 5830              	.LFE174:
 5832              		.section	.text.SPI_2linesTxISR_8BIT,"ax",%progbits
 5833              		.align	1
 5834              		.syntax unified
 5835              		.thumb
 5836              		.thumb_func
 5838              	SPI_2linesTxISR_8BIT:
 5839              	.LVL379:
 5840              	.LFB163:
3668:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in packing Bit mode */
 5841              		.loc 1 3668 1 is_stmt 1 view -0
 5842              		.cfi_startproc
 5843              		@ args = 0, pretend = 0, frame = 0
 5844              		@ frame_needed = 0, uses_anonymous_args = 0
3668:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in packing Bit mode */
 5845              		.loc 1 3668 1 is_stmt 0 view .LVU1970
 5846 0000 08B5     		push	{r3, lr}
 5847              		.cfi_def_cfa_offset 8
 5848              		.cfi_offset 3, -8
 5849              		.cfi_offset 14, -4
3670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5850              		.loc 1 3670 3 is_stmt 1 view .LVU1971
3670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5851              		.loc 1 3670 11 is_stmt 0 view .LVU1972
 5852 0002 C38F     		ldrh	r3, [r0, #62]
 5853 0004 9BB2     		uxth	r3, r3
3670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5854              		.loc 1 3670 6 view .LVU1973
 5855 0006 012B     		cmp	r3, #1
 5856 0008 18D9     		bls	.L402
3672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr += sizeof(uint16_t);
 5857              		.loc 1 3672 5 is_stmt 1 view .LVU1974
3672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr += sizeof(uint16_t);
 5858              		.loc 1 3672 44 is_stmt 0 view .LVU1975
 5859 000a 826B     		ldr	r2, [r0, #56]
3672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr += sizeof(uint16_t);
 5860              		.loc 1 3672 9 view .LVU1976
 5861 000c 0368     		ldr	r3, [r0]
3672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr += sizeof(uint16_t);
 5862              		.loc 1 3672 26 view .LVU1977
 5863 000e 1288     		ldrh	r2, [r2]
3672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr += sizeof(uint16_t);
 5864              		.loc 1 3672 24 view .LVU1978
 5865 0010 DA60     		str	r2, [r3, #12]
3673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount -= 2U;
 5866              		.loc 1 3673 5 is_stmt 1 view .LVU1979
3673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount -= 2U;
 5867              		.loc 1 3673 9 is_stmt 0 view .LVU1980
 5868 0012 836B     		ldr	r3, [r0, #56]
3673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount -= 2U;
 5869              		.loc 1 3673 22 view .LVU1981
 5870 0014 0233     		adds	r3, r3, #2
 5871 0016 8363     		str	r3, [r0, #56]
3674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5872              		.loc 1 3674 5 is_stmt 1 view .LVU1982
3674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
ARM GAS  /tmp/cc5SiBtg.s 			page 213


 5873              		.loc 1 3674 9 is_stmt 0 view .LVU1983
 5874 0018 C38F     		ldrh	r3, [r0, #62]
 5875 001a 9BB2     		uxth	r3, r3
3674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5876              		.loc 1 3674 23 view .LVU1984
 5877 001c 023B     		subs	r3, r3, #2
 5878 001e 9BB2     		uxth	r3, r3
 5879 0020 C387     		strh	r3, [r0, #62]	@ movhi
 5880              	.L403:
3685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5881              		.loc 1 3685 3 is_stmt 1 view .LVU1985
3685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5882              		.loc 1 3685 11 is_stmt 0 view .LVU1986
 5883 0022 C38F     		ldrh	r3, [r0, #62]
 5884 0024 9BB2     		uxth	r3, r3
3685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5885              		.loc 1 3685 6 view .LVU1987
 5886 0026 43B9     		cbnz	r3, .L401
3699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5887              		.loc 1 3699 5 is_stmt 1 view .LVU1988
 5888 0028 0268     		ldr	r2, [r0]
 5889 002a 5368     		ldr	r3, [r2, #4]
 5890 002c 23F08003 		bic	r3, r3, #128
 5891 0030 5360     		str	r3, [r2, #4]
3701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5892              		.loc 1 3701 5 view .LVU1989
3701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5893              		.loc 1 3701 13 is_stmt 0 view .LVU1990
 5894 0032 B0F84630 		ldrh	r3, [r0, #70]
 5895 0036 9BB2     		uxth	r3, r3
3701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5896              		.loc 1 3701 8 view .LVU1991
 5897 0038 6BB1     		cbz	r3, .L406
 5898              	.LVL380:
 5899              	.L401:
3706:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5900              		.loc 1 3706 1 view .LVU1992
 5901 003a 08BD     		pop	{r3, pc}
 5902              	.LVL381:
 5903              	.L402:
3679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr++;
 5904              		.loc 1 3679 5 is_stmt 1 view .LVU1993
3679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr++;
 5905              		.loc 1 3679 50 is_stmt 0 view .LVU1994
 5906 003c 826B     		ldr	r2, [r0, #56]
3679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr++;
 5907              		.loc 1 3679 27 view .LVU1995
 5908 003e 0368     		ldr	r3, [r0]
3679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr++;
 5909              		.loc 1 3679 45 view .LVU1996
 5910 0040 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
3679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr++;
 5911              		.loc 1 3679 42 view .LVU1997
 5912 0042 1A73     		strb	r2, [r3, #12]
3680:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount--;
 5913              		.loc 1 3680 5 is_stmt 1 view .LVU1998
3680:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount--;
ARM GAS  /tmp/cc5SiBtg.s 			page 214


 5914              		.loc 1 3680 9 is_stmt 0 view .LVU1999
 5915 0044 836B     		ldr	r3, [r0, #56]
3680:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount--;
 5916              		.loc 1 3680 21 view .LVU2000
 5917 0046 0133     		adds	r3, r3, #1
 5918 0048 8363     		str	r3, [r0, #56]
3681:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5919              		.loc 1 3681 5 is_stmt 1 view .LVU2001
3681:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5920              		.loc 1 3681 9 is_stmt 0 view .LVU2002
 5921 004a C38F     		ldrh	r3, [r0, #62]
 5922 004c 9BB2     		uxth	r3, r3
3681:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5923              		.loc 1 3681 22 view .LVU2003
 5924 004e 013B     		subs	r3, r3, #1
 5925 0050 9BB2     		uxth	r3, r3
 5926 0052 C387     		strh	r3, [r0, #62]	@ movhi
 5927 0054 E5E7     		b	.L403
 5928              	.L406:
3703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 5929              		.loc 1 3703 7 is_stmt 1 view .LVU2004
 5930 0056 FFF7FEFF 		bl	SPI_CloseRxTx_ISR
 5931              	.LVL382:
3706:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5932              		.loc 1 3706 1 is_stmt 0 view .LVU2005
 5933 005a EEE7     		b	.L401
 5934              		.cfi_endproc
 5935              	.LFE163:
 5937              		.section	.text.SPI_2linesRxISR_8BIT,"ax",%progbits
 5938              		.align	1
 5939              		.syntax unified
 5940              		.thumb
 5941              		.thumb_func
 5943              	SPI_2linesRxISR_8BIT:
 5944              	.LVL383:
 5945              	.LFB162:
3583:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in packing mode */
 5946              		.loc 1 3583 1 is_stmt 1 view -0
 5947              		.cfi_startproc
 5948              		@ args = 0, pretend = 0, frame = 0
 5949              		@ frame_needed = 0, uses_anonymous_args = 0
3583:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in packing mode */
 5950              		.loc 1 3583 1 is_stmt 0 view .LVU2007
 5951 0000 08B5     		push	{r3, lr}
 5952              		.cfi_def_cfa_offset 8
 5953              		.cfi_offset 3, -8
 5954              		.cfi_offset 14, -4
3585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5955              		.loc 1 3585 3 is_stmt 1 view .LVU2008
3585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5956              		.loc 1 3585 11 is_stmt 0 view .LVU2009
 5957 0002 B0F84630 		ldrh	r3, [r0, #70]
 5958 0006 9BB2     		uxth	r3, r3
3585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5959              		.loc 1 3585 6 view .LVU2010
 5960 0008 012B     		cmp	r3, #1
 5961 000a 18D9     		bls	.L408
ARM GAS  /tmp/cc5SiBtg.s 			page 215


3587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr += sizeof(uint16_t);
 5962              		.loc 1 3587 5 is_stmt 1 view .LVU2011
3587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr += sizeof(uint16_t);
 5963              		.loc 1 3587 54 is_stmt 0 view .LVU2012
 5964 000c 0368     		ldr	r3, [r0]
3587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr += sizeof(uint16_t);
 5965              		.loc 1 3587 64 view .LVU2013
 5966 000e DA68     		ldr	r2, [r3, #12]
3587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr += sizeof(uint16_t);
 5967              		.loc 1 3587 23 view .LVU2014
 5968 0010 036C     		ldr	r3, [r0, #64]
3587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr += sizeof(uint16_t);
 5969              		.loc 1 3587 37 view .LVU2015
 5970 0012 1A80     		strh	r2, [r3]	@ movhi
3588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount -= 2U;
 5971              		.loc 1 3588 5 is_stmt 1 view .LVU2016
3588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount -= 2U;
 5972              		.loc 1 3588 9 is_stmt 0 view .LVU2017
 5973 0014 036C     		ldr	r3, [r0, #64]
3588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount -= 2U;
 5974              		.loc 1 3588 22 view .LVU2018
 5975 0016 0233     		adds	r3, r3, #2
 5976 0018 0364     		str	r3, [r0, #64]
3589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->RxXferCount == 1U)
 5977              		.loc 1 3589 5 is_stmt 1 view .LVU2019
3589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->RxXferCount == 1U)
 5978              		.loc 1 3589 9 is_stmt 0 view .LVU2020
 5979 001a B0F84630 		ldrh	r3, [r0, #70]
 5980 001e 9BB2     		uxth	r3, r3
3589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->RxXferCount == 1U)
 5981              		.loc 1 3589 23 view .LVU2021
 5982 0020 023B     		subs	r3, r3, #2
 5983 0022 9BB2     		uxth	r3, r3
 5984 0024 A0F84630 		strh	r3, [r0, #70]	@ movhi
3590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5985              		.loc 1 3590 5 is_stmt 1 view .LVU2022
3590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5986              		.loc 1 3590 13 is_stmt 0 view .LVU2023
 5987 0028 B0F84630 		ldrh	r3, [r0, #70]
 5988 002c 9BB2     		uxth	r3, r3
3590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5989              		.loc 1 3590 8 view .LVU2024
 5990 002e 012B     		cmp	r3, #1
 5991 0030 13D1     		bne	.L409
3593:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 5992              		.loc 1 3593 7 is_stmt 1 view .LVU2025
 5993 0032 0268     		ldr	r2, [r0]
 5994 0034 5368     		ldr	r3, [r2, #4]
 5995 0036 43F48053 		orr	r3, r3, #4096
 5996 003a 5360     		str	r3, [r2, #4]
 5997 003c 0DE0     		b	.L409
 5998              	.L408:
3599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr++;
 5999              		.loc 1 3599 5 view .LVU2026
3599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr++;
 6000              		.loc 1 3599 48 is_stmt 0 view .LVU2027
 6001 003e 0268     		ldr	r2, [r0]
ARM GAS  /tmp/cc5SiBtg.s 			page 216


3599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr++;
 6002              		.loc 1 3599 10 view .LVU2028
 6003 0040 036C     		ldr	r3, [r0, #64]
3599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr++;
 6004              		.loc 1 3599 25 view .LVU2029
 6005 0042 127B     		ldrb	r2, [r2, #12]	@ zero_extendqisi2
3599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr++;
 6006              		.loc 1 3599 23 view .LVU2030
 6007 0044 1A70     		strb	r2, [r3]
3600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount--;
 6008              		.loc 1 3600 5 is_stmt 1 view .LVU2031
3600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount--;
 6009              		.loc 1 3600 9 is_stmt 0 view .LVU2032
 6010 0046 036C     		ldr	r3, [r0, #64]
3600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount--;
 6011              		.loc 1 3600 21 view .LVU2033
 6012 0048 0133     		adds	r3, r3, #1
 6013 004a 0364     		str	r3, [r0, #64]
3601:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6014              		.loc 1 3601 5 is_stmt 1 view .LVU2034
3601:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6015              		.loc 1 3601 9 is_stmt 0 view .LVU2035
 6016 004c B0F84630 		ldrh	r3, [r0, #70]
 6017 0050 9BB2     		uxth	r3, r3
3601:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6018              		.loc 1 3601 22 view .LVU2036
 6019 0052 013B     		subs	r3, r3, #1
 6020 0054 9BB2     		uxth	r3, r3
 6021 0056 A0F84630 		strh	r3, [r0, #70]	@ movhi
 6022              	.L409:
3605:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6023              		.loc 1 3605 3 is_stmt 1 view .LVU2037
3605:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6024              		.loc 1 3605 11 is_stmt 0 view .LVU2038
 6025 005a B0F84630 		ldrh	r3, [r0, #70]
 6026 005e 9BB2     		uxth	r3, r3
3605:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6027              		.loc 1 3605 6 view .LVU2039
 6028 0060 3BB9     		cbnz	r3, .L407
3617:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6029              		.loc 1 3617 5 is_stmt 1 view .LVU2040
 6030 0062 0268     		ldr	r2, [r0]
 6031 0064 5368     		ldr	r3, [r2, #4]
 6032 0066 23F06003 		bic	r3, r3, #96
 6033 006a 5360     		str	r3, [r2, #4]
3619:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6034              		.loc 1 3619 5 view .LVU2041
3619:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6035              		.loc 1 3619 13 is_stmt 0 view .LVU2042
 6036 006c C38F     		ldrh	r3, [r0, #62]
 6037 006e 9BB2     		uxth	r3, r3
3619:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6038              		.loc 1 3619 8 view .LVU2043
 6039 0070 03B1     		cbz	r3, .L412
 6040              	.LVL384:
 6041              	.L407:
3624:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/cc5SiBtg.s 			page 217


 6042              		.loc 1 3624 1 view .LVU2044
 6043 0072 08BD     		pop	{r3, pc}
 6044              	.LVL385:
 6045              	.L412:
3621:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6046              		.loc 1 3621 7 is_stmt 1 view .LVU2045
 6047 0074 FFF7FEFF 		bl	SPI_CloseRxTx_ISR
 6048              	.LVL386:
3624:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6049              		.loc 1 3624 1 is_stmt 0 view .LVU2046
 6050 0078 FBE7     		b	.L407
 6051              		.cfi_endproc
 6052              	.LFE162:
 6054              		.section	.text.SPI_2linesTxISR_16BIT,"ax",%progbits
 6055              		.align	1
 6056              		.syntax unified
 6057              		.thumb
 6058              		.thumb_func
 6060              	SPI_2linesTxISR_16BIT:
 6061              	.LVL387:
 6062              	.LFB165:
3771:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
 6063              		.loc 1 3771 1 is_stmt 1 view -0
 6064              		.cfi_startproc
 6065              		@ args = 0, pretend = 0, frame = 0
 6066              		@ frame_needed = 0, uses_anonymous_args = 0
3771:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
 6067              		.loc 1 3771 1 is_stmt 0 view .LVU2048
 6068 0000 08B5     		push	{r3, lr}
 6069              		.cfi_def_cfa_offset 8
 6070              		.cfi_offset 3, -8
 6071              		.cfi_offset 14, -4
3773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 6072              		.loc 1 3773 3 is_stmt 1 view .LVU2049
3773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 6073              		.loc 1 3773 42 is_stmt 0 view .LVU2050
 6074 0002 826B     		ldr	r2, [r0, #56]
3773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 6075              		.loc 1 3773 7 view .LVU2051
 6076 0004 0368     		ldr	r3, [r0]
3773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 6077              		.loc 1 3773 24 view .LVU2052
 6078 0006 1288     		ldrh	r2, [r2]
3773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 6079              		.loc 1 3773 22 view .LVU2053
 6080 0008 DA60     		str	r2, [r3, #12]
3774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 6081              		.loc 1 3774 3 is_stmt 1 view .LVU2054
3774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 6082              		.loc 1 3774 7 is_stmt 0 view .LVU2055
 6083 000a 836B     		ldr	r3, [r0, #56]
3774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 6084              		.loc 1 3774 20 view .LVU2056
 6085 000c 0233     		adds	r3, r3, #2
 6086 000e 8363     		str	r3, [r0, #56]
3775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6087              		.loc 1 3775 3 is_stmt 1 view .LVU2057
ARM GAS  /tmp/cc5SiBtg.s 			page 218


3775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6088              		.loc 1 3775 7 is_stmt 0 view .LVU2058
 6089 0010 C38F     		ldrh	r3, [r0, #62]
 6090 0012 9BB2     		uxth	r3, r3
3775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6091              		.loc 1 3775 20 view .LVU2059
 6092 0014 013B     		subs	r3, r3, #1
 6093 0016 9BB2     		uxth	r3, r3
 6094 0018 C387     		strh	r3, [r0, #62]	@ movhi
3778:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6095              		.loc 1 3778 3 is_stmt 1 view .LVU2060
3778:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6096              		.loc 1 3778 11 is_stmt 0 view .LVU2061
 6097 001a C38F     		ldrh	r3, [r0, #62]
 6098 001c 9BB2     		uxth	r3, r3
3778:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6099              		.loc 1 3778 6 view .LVU2062
 6100 001e 43B9     		cbnz	r3, .L413
3792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6101              		.loc 1 3792 5 is_stmt 1 view .LVU2063
 6102 0020 0268     		ldr	r2, [r0]
 6103 0022 5368     		ldr	r3, [r2, #4]
 6104 0024 23F08003 		bic	r3, r3, #128
 6105 0028 5360     		str	r3, [r2, #4]
3794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6106              		.loc 1 3794 5 view .LVU2064
3794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6107              		.loc 1 3794 13 is_stmt 0 view .LVU2065
 6108 002a B0F84630 		ldrh	r3, [r0, #70]
 6109 002e 9BB2     		uxth	r3, r3
3794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6110              		.loc 1 3794 8 view .LVU2066
 6111 0030 03B1     		cbz	r3, .L416
 6112              	.LVL388:
 6113              	.L413:
3799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6114              		.loc 1 3799 1 view .LVU2067
 6115 0032 08BD     		pop	{r3, pc}
 6116              	.LVL389:
 6117              	.L416:
3796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6118              		.loc 1 3796 7 is_stmt 1 view .LVU2068
 6119 0034 FFF7FEFF 		bl	SPI_CloseRxTx_ISR
 6120              	.LVL390:
3799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6121              		.loc 1 3799 1 is_stmt 0 view .LVU2069
 6122 0038 FBE7     		b	.L413
 6123              		.cfi_endproc
 6124              	.LFE165:
 6126              		.section	.text.SPI_2linesRxISR_16BIT,"ax",%progbits
 6127              		.align	1
 6128              		.syntax unified
 6129              		.thumb
 6130              		.thumb_func
 6132              	SPI_2linesRxISR_16BIT:
 6133              	.LVL391:
 6134              	.LFB164:
ARM GAS  /tmp/cc5SiBtg.s 			page 219


3715:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in 16 Bit mode */
 6135              		.loc 1 3715 1 is_stmt 1 view -0
 6136              		.cfi_startproc
 6137              		@ args = 0, pretend = 0, frame = 0
 6138              		@ frame_needed = 0, uses_anonymous_args = 0
3715:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in 16 Bit mode */
 6139              		.loc 1 3715 1 is_stmt 0 view .LVU2071
 6140 0000 08B5     		push	{r3, lr}
 6141              		.cfi_def_cfa_offset 8
 6142              		.cfi_offset 3, -8
 6143              		.cfi_offset 14, -4
3717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 6144              		.loc 1 3717 3 is_stmt 1 view .LVU2072
3717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 6145              		.loc 1 3717 52 is_stmt 0 view .LVU2073
 6146 0002 0368     		ldr	r3, [r0]
3717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 6147              		.loc 1 3717 62 view .LVU2074
 6148 0004 DA68     		ldr	r2, [r3, #12]
3717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 6149              		.loc 1 3717 21 view .LVU2075
 6150 0006 036C     		ldr	r3, [r0, #64]
3717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 6151              		.loc 1 3717 35 view .LVU2076
 6152 0008 1A80     		strh	r2, [r3]	@ movhi
3718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 6153              		.loc 1 3718 3 is_stmt 1 view .LVU2077
3718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 6154              		.loc 1 3718 7 is_stmt 0 view .LVU2078
 6155 000a 036C     		ldr	r3, [r0, #64]
3718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 6156              		.loc 1 3718 20 view .LVU2079
 6157 000c 0233     		adds	r3, r3, #2
 6158 000e 0364     		str	r3, [r0, #64]
3719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6159              		.loc 1 3719 3 is_stmt 1 view .LVU2080
3719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6160              		.loc 1 3719 7 is_stmt 0 view .LVU2081
 6161 0010 B0F84630 		ldrh	r3, [r0, #70]
 6162 0014 9BB2     		uxth	r3, r3
3719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6163              		.loc 1 3719 20 view .LVU2082
 6164 0016 013B     		subs	r3, r3, #1
 6165 0018 9BB2     		uxth	r3, r3
 6166 001a A0F84630 		strh	r3, [r0, #70]	@ movhi
3721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6167              		.loc 1 3721 3 is_stmt 1 view .LVU2083
3721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6168              		.loc 1 3721 11 is_stmt 0 view .LVU2084
 6169 001e B0F84630 		ldrh	r3, [r0, #70]
 6170 0022 9BB2     		uxth	r3, r3
3721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6171              		.loc 1 3721 6 view .LVU2085
 6172 0024 3BB9     		cbnz	r3, .L417
3732:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6173              		.loc 1 3732 5 is_stmt 1 view .LVU2086
 6174 0026 0268     		ldr	r2, [r0]
ARM GAS  /tmp/cc5SiBtg.s 			page 220


 6175 0028 5368     		ldr	r3, [r2, #4]
 6176 002a 23F04003 		bic	r3, r3, #64
 6177 002e 5360     		str	r3, [r2, #4]
3734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6178              		.loc 1 3734 5 view .LVU2087
3734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6179              		.loc 1 3734 13 is_stmt 0 view .LVU2088
 6180 0030 C38F     		ldrh	r3, [r0, #62]
 6181 0032 9BB2     		uxth	r3, r3
3734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6182              		.loc 1 3734 8 view .LVU2089
 6183 0034 03B1     		cbz	r3, .L420
 6184              	.LVL392:
 6185              	.L417:
3739:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6186              		.loc 1 3739 1 view .LVU2090
 6187 0036 08BD     		pop	{r3, pc}
 6188              	.LVL393:
 6189              	.L420:
3736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6190              		.loc 1 3736 7 is_stmt 1 view .LVU2091
 6191 0038 FFF7FEFF 		bl	SPI_CloseRxTx_ISR
 6192              	.LVL394:
3739:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6193              		.loc 1 3739 1 is_stmt 0 view .LVU2092
 6194 003c FBE7     		b	.L417
 6195              		.cfi_endproc
 6196              	.LFE164:
 6198              		.section	.text.SPI_DMAError,"ax",%progbits
 6199              		.align	1
 6200              		.syntax unified
 6201              		.thumb
 6202              		.thumb_func
 6204              	SPI_DMAError:
 6205              	.LVL395:
 6206              	.LFB158:
3407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6207              		.loc 1 3407 1 is_stmt 1 view -0
 6208              		.cfi_startproc
 6209              		@ args = 0, pretend = 0, frame = 0
 6210              		@ frame_needed = 0, uses_anonymous_args = 0
3407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6211              		.loc 1 3407 1 is_stmt 0 view .LVU2094
 6212 0000 08B5     		push	{r3, lr}
 6213              		.cfi_def_cfa_offset 8
 6214              		.cfi_offset 3, -8
 6215              		.cfi_offset 14, -4
3408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6216              		.loc 1 3408 3 is_stmt 1 view .LVU2095
3408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6217              		.loc 1 3408 22 is_stmt 0 view .LVU2096
 6218 0002 406A     		ldr	r0, [r0, #36]
 6219              	.LVL396:
3411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6220              		.loc 1 3411 3 is_stmt 1 view .LVU2097
 6221 0004 0268     		ldr	r2, [r0]
 6222 0006 5368     		ldr	r3, [r2, #4]
ARM GAS  /tmp/cc5SiBtg.s 			page 221


 6223 0008 23F00303 		bic	r3, r3, #3
 6224 000c 5360     		str	r3, [r2, #4]
3413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
 6225              		.loc 1 3413 3 view .LVU2098
 6226 000e 036E     		ldr	r3, [r0, #96]
 6227 0010 43F01003 		orr	r3, r3, #16
 6228 0014 0366     		str	r3, [r0, #96]
3414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user error callback */
 6229              		.loc 1 3414 3 view .LVU2099
3414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user error callback */
 6230              		.loc 1 3414 15 is_stmt 0 view .LVU2100
 6231 0016 0123     		movs	r3, #1
 6232 0018 80F85D30 		strb	r3, [r0, #93]
3419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6233              		.loc 1 3419 3 is_stmt 1 view .LVU2101
 6234 001c FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6235              	.LVL397:
3421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6236              		.loc 1 3421 1 is_stmt 0 view .LVU2102
 6237 0020 08BD     		pop	{r3, pc}
 6238              		.cfi_endproc
 6239              	.LFE158:
 6241              		.section	.text.SPI_DMATransmitCplt,"ax",%progbits
 6242              		.align	1
 6243              		.syntax unified
 6244              		.thumb
 6245              		.thumb_func
 6247              	SPI_DMATransmitCplt:
 6248              	.LVL398:
 6249              	.LFB152:
3079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6250              		.loc 1 3079 1 is_stmt 1 view -0
 6251              		.cfi_startproc
 6252              		@ args = 0, pretend = 0, frame = 8
 6253              		@ frame_needed = 0, uses_anonymous_args = 0
3079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6254              		.loc 1 3079 1 is_stmt 0 view .LVU2104
 6255 0000 30B5     		push	{r4, r5, lr}
 6256              		.cfi_def_cfa_offset 12
 6257              		.cfi_offset 4, -12
 6258              		.cfi_offset 5, -8
 6259              		.cfi_offset 14, -4
 6260 0002 83B0     		sub	sp, sp, #12
 6261              		.cfi_def_cfa_offset 24
 6262 0004 0546     		mov	r5, r0
3080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 6263              		.loc 1 3080 3 is_stmt 1 view .LVU2105
3080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 6264              		.loc 1 3080 22 is_stmt 0 view .LVU2106
 6265 0006 446A     		ldr	r4, [r0, #36]
 6266              	.LVL399:
3081:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6267              		.loc 1 3081 3 is_stmt 1 view .LVU2107
3084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6268              		.loc 1 3084 3 view .LVU2108
3084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6269              		.loc 1 3084 15 is_stmt 0 view .LVU2109
ARM GAS  /tmp/cc5SiBtg.s 			page 222


 6270 0008 FFF7FEFF 		bl	HAL_GetTick
 6271              	.LVL400:
3087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6272              		.loc 1 3087 3 is_stmt 1 view .LVU2110
3087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6273              		.loc 1 3087 12 is_stmt 0 view .LVU2111
 6274 000c 2B68     		ldr	r3, [r5]
3087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6275              		.loc 1 3087 22 view .LVU2112
 6276 000e 1B68     		ldr	r3, [r3]
3087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6277              		.loc 1 3087 6 view .LVU2113
 6278 0010 13F0200F 		tst	r3, #32
 6279 0014 23D1     		bne	.L424
 6280 0016 0246     		mov	r2, r0
3090:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6281              		.loc 1 3090 5 is_stmt 1 view .LVU2114
 6282 0018 2168     		ldr	r1, [r4]
 6283 001a 4B68     		ldr	r3, [r1, #4]
 6284 001c 23F02003 		bic	r3, r3, #32
 6285 0020 4B60     		str	r3, [r1, #4]
3093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6286              		.loc 1 3093 5 view .LVU2115
 6287 0022 2168     		ldr	r1, [r4]
 6288 0024 4B68     		ldr	r3, [r1, #4]
 6289 0026 23F00203 		bic	r3, r3, #2
 6290 002a 4B60     		str	r3, [r1, #4]
3096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6291              		.loc 1 3096 5 view .LVU2116
3096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6292              		.loc 1 3096 9 is_stmt 0 view .LVU2117
 6293 002c 6421     		movs	r1, #100
 6294 002e 2046     		mov	r0, r4
 6295              	.LVL401:
3096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6296              		.loc 1 3096 9 view .LVU2118
 6297 0030 FFF7FEFF 		bl	SPI_EndRxTxTransaction
 6298              	.LVL402:
3096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6299              		.loc 1 3096 8 discriminator 1 view .LVU2119
 6300 0034 18B1     		cbz	r0, .L425
3098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6301              		.loc 1 3098 7 is_stmt 1 view .LVU2120
 6302 0036 236E     		ldr	r3, [r4, #96]
 6303 0038 43F02003 		orr	r3, r3, #32
 6304 003c 2366     		str	r3, [r4, #96]
 6305              	.L425:
3102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6306              		.loc 1 3102 5 view .LVU2121
3102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6307              		.loc 1 3102 19 is_stmt 0 view .LVU2122
 6308 003e A368     		ldr	r3, [r4, #8]
3102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6309              		.loc 1 3102 8 view .LVU2123
 6310 0040 33B9     		cbnz	r3, .L426
3104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6311              		.loc 1 3104 7 is_stmt 1 view .LVU2124
ARM GAS  /tmp/cc5SiBtg.s 			page 223


 6312              	.LBB6:
3104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6313              		.loc 1 3104 7 view .LVU2125
 6314 0042 0193     		str	r3, [sp, #4]
3104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6315              		.loc 1 3104 7 view .LVU2126
 6316 0044 2368     		ldr	r3, [r4]
 6317 0046 DA68     		ldr	r2, [r3, #12]
 6318 0048 0192     		str	r2, [sp, #4]
3104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6319              		.loc 1 3104 7 view .LVU2127
 6320 004a 9B68     		ldr	r3, [r3, #8]
 6321 004c 0193     		str	r3, [sp, #4]
3104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6322              		.loc 1 3104 7 view .LVU2128
 6323 004e 019B     		ldr	r3, [sp, #4]
 6324              	.L426:
 6325              	.LBE6:
3104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6326              		.loc 1 3104 7 discriminator 1 view .LVU2129
3107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 6327              		.loc 1 3107 5 view .LVU2130
3107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 6328              		.loc 1 3107 23 is_stmt 0 view .LVU2131
 6329 0050 0023     		movs	r3, #0
 6330 0052 E387     		strh	r3, [r4, #62]	@ movhi
3108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6331              		.loc 1 3108 5 is_stmt 1 view .LVU2132
3108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6332              		.loc 1 3108 17 is_stmt 0 view .LVU2133
 6333 0054 0123     		movs	r3, #1
 6334 0056 84F85D30 		strb	r3, [r4, #93]
3110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6335              		.loc 1 3110 5 is_stmt 1 view .LVU2134
3110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6336              		.loc 1 3110 13 is_stmt 0 view .LVU2135
 6337 005a 236E     		ldr	r3, [r4, #96]
3110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6338              		.loc 1 3110 8 view .LVU2136
 6339 005c 23B9     		cbnz	r3, .L429
 6340              	.L424:
3125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6341              		.loc 1 3125 3 is_stmt 1 view .LVU2137
 6342 005e 2046     		mov	r0, r4
 6343 0060 FFF7FEFF 		bl	HAL_SPI_TxCpltCallback
 6344              	.LVL403:
 6345              	.L423:
3127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6346              		.loc 1 3127 1 is_stmt 0 view .LVU2138
 6347 0064 03B0     		add	sp, sp, #12
 6348              		.cfi_remember_state
 6349              		.cfi_def_cfa_offset 12
 6350              		@ sp needed
 6351 0066 30BD     		pop	{r4, r5, pc}
 6352              	.LVL404:
 6353              	.L429:
 6354              		.cfi_restore_state
ARM GAS  /tmp/cc5SiBtg.s 			page 224


3116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6355              		.loc 1 3116 7 is_stmt 1 view .LVU2139
 6356 0068 2046     		mov	r0, r4
 6357 006a FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6358              	.LVL405:
3118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6359              		.loc 1 3118 7 view .LVU2140
 6360 006e F9E7     		b	.L423
 6361              		.cfi_endproc
 6362              	.LFE152:
 6364              		.section	.text.SPI_DMAReceiveCplt,"ax",%progbits
 6365              		.align	1
 6366              		.syntax unified
 6367              		.thumb
 6368              		.thumb_func
 6370              	SPI_DMAReceiveCplt:
 6371              	.LVL406:
 6372              	.LFB153:
3136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6373              		.loc 1 3136 1 view -0
 6374              		.cfi_startproc
 6375              		@ args = 0, pretend = 0, frame = 0
 6376              		@ frame_needed = 0, uses_anonymous_args = 0
3136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6377              		.loc 1 3136 1 is_stmt 0 view .LVU2142
 6378 0000 38B5     		push	{r3, r4, r5, lr}
 6379              		.cfi_def_cfa_offset 16
 6380              		.cfi_offset 3, -16
 6381              		.cfi_offset 4, -12
 6382              		.cfi_offset 5, -8
 6383              		.cfi_offset 14, -4
 6384 0002 0546     		mov	r5, r0
3137:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 6385              		.loc 1 3137 3 is_stmt 1 view .LVU2143
3137:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 6386              		.loc 1 3137 22 is_stmt 0 view .LVU2144
 6387 0004 446A     		ldr	r4, [r0, #36]
 6388              	.LVL407:
3138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 6389              		.loc 1 3138 3 is_stmt 1 view .LVU2145
3146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6390              		.loc 1 3146 3 view .LVU2146
3146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6391              		.loc 1 3146 15 is_stmt 0 view .LVU2147
 6392 0006 FFF7FEFF 		bl	HAL_GetTick
 6393              	.LVL408:
3149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6394              		.loc 1 3149 3 is_stmt 1 view .LVU2148
3149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6395              		.loc 1 3149 12 is_stmt 0 view .LVU2149
 6396 000a 2B68     		ldr	r3, [r5]
3149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6397              		.loc 1 3149 22 view .LVU2150
 6398 000c 1B68     		ldr	r3, [r3]
3149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6399              		.loc 1 3149 6 view .LVU2151
 6400 000e 13F0200F 		tst	r3, #32
ARM GAS  /tmp/cc5SiBtg.s 			page 225


 6401 0012 1FD1     		bne	.L431
 6402 0014 0246     		mov	r2, r0
3152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6403              		.loc 1 3152 5 is_stmt 1 view .LVU2152
 6404 0016 2168     		ldr	r1, [r4]
 6405 0018 4B68     		ldr	r3, [r1, #4]
 6406 001a 23F02003 		bic	r3, r3, #32
 6407 001e 4B60     		str	r3, [r1, #4]
3198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6408              		.loc 1 3198 5 view .LVU2153
3198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6409              		.loc 1 3198 20 is_stmt 0 view .LVU2154
 6410 0020 A368     		ldr	r3, [r4, #8]
3198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6411              		.loc 1 3198 8 view .LVU2155
 6412 0022 1BB9     		cbnz	r3, .L432
3198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6413              		.loc 1 3198 70 discriminator 1 view .LVU2156
 6414 0024 6368     		ldr	r3, [r4, #4]
3198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6415              		.loc 1 3198 56 discriminator 1 view .LVU2157
 6416 0026 B3F5827F 		cmp	r3, #260
 6417 002a 17D0     		beq	.L437
 6418              	.L432:
3206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6419              		.loc 1 3206 7 is_stmt 1 view .LVU2158
 6420 002c 2168     		ldr	r1, [r4]
 6421 002e 4B68     		ldr	r3, [r1, #4]
 6422 0030 23F00103 		bic	r3, r3, #1
 6423 0034 4B60     		str	r3, [r1, #4]
 6424              	.L433:
3210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6425              		.loc 1 3210 5 view .LVU2159
3210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6426              		.loc 1 3210 9 is_stmt 0 view .LVU2160
 6427 0036 6421     		movs	r1, #100
 6428 0038 2046     		mov	r0, r4
 6429              	.LVL409:
3210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6430              		.loc 1 3210 9 view .LVU2161
 6431 003a FFF7FEFF 		bl	SPI_EndRxTransaction
 6432              	.LVL410:
3210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6433              		.loc 1 3210 8 discriminator 1 view .LVU2162
 6434 003e 08B1     		cbz	r0, .L434
3212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6435              		.loc 1 3212 7 is_stmt 1 view .LVU2163
3212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6436              		.loc 1 3212 23 is_stmt 0 view .LVU2164
 6437 0040 2023     		movs	r3, #32
 6438 0042 2366     		str	r3, [r4, #96]
 6439              	.L434:
3215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 6440              		.loc 1 3215 5 is_stmt 1 view .LVU2165
3215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 6441              		.loc 1 3215 23 is_stmt 0 view .LVU2166
 6442 0044 0023     		movs	r3, #0
ARM GAS  /tmp/cc5SiBtg.s 			page 226


 6443 0046 A4F84630 		strh	r3, [r4, #70]	@ movhi
3216:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6444              		.loc 1 3216 5 is_stmt 1 view .LVU2167
3216:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6445              		.loc 1 3216 17 is_stmt 0 view .LVU2168
 6446 004a 0123     		movs	r3, #1
 6447 004c 84F85D30 		strb	r3, [r4, #93]
3227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6448              		.loc 1 3227 5 is_stmt 1 view .LVU2169
3227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6449              		.loc 1 3227 13 is_stmt 0 view .LVU2170
 6450 0050 236E     		ldr	r3, [r4, #96]
3227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6451              		.loc 1 3227 8 view .LVU2171
 6452 0052 4BB9     		cbnz	r3, .L438
 6453              	.L431:
3242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6454              		.loc 1 3242 3 is_stmt 1 view .LVU2172
 6455 0054 2046     		mov	r0, r4
 6456 0056 FFF7FEFF 		bl	HAL_SPI_RxCpltCallback
 6457              	.LVL411:
 6458              	.L430:
3244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6459              		.loc 1 3244 1 is_stmt 0 view .LVU2173
 6460 005a 38BD     		pop	{r3, r4, r5, pc}
 6461              	.LVL412:
 6462              	.L437:
3201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6463              		.loc 1 3201 7 is_stmt 1 view .LVU2174
 6464 005c 2168     		ldr	r1, [r4]
 6465 005e 4B68     		ldr	r3, [r1, #4]
 6466 0060 23F00303 		bic	r3, r3, #3
 6467 0064 4B60     		str	r3, [r1, #4]
 6468 0066 E6E7     		b	.L433
 6469              	.LVL413:
 6470              	.L438:
3233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6471              		.loc 1 3233 7 view .LVU2175
 6472 0068 2046     		mov	r0, r4
 6473 006a FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6474              	.LVL414:
3235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6475              		.loc 1 3235 7 view .LVU2176
 6476 006e F4E7     		b	.L430
 6477              		.cfi_endproc
 6478              	.LFE153:
 6480              		.section	.text.SPI_DMATransmitReceiveCplt,"ax",%progbits
 6481              		.align	1
 6482              		.syntax unified
 6483              		.thumb
 6484              		.thumb_func
 6486              	SPI_DMATransmitReceiveCplt:
 6487              	.LVL415:
 6488              	.LFB154:
3253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6489              		.loc 1 3253 1 view -0
 6490              		.cfi_startproc
ARM GAS  /tmp/cc5SiBtg.s 			page 227


 6491              		@ args = 0, pretend = 0, frame = 0
 6492              		@ frame_needed = 0, uses_anonymous_args = 0
3253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6493              		.loc 1 3253 1 is_stmt 0 view .LVU2178
 6494 0000 38B5     		push	{r3, r4, r5, lr}
 6495              		.cfi_def_cfa_offset 16
 6496              		.cfi_offset 3, -16
 6497              		.cfi_offset 4, -12
 6498              		.cfi_offset 5, -8
 6499              		.cfi_offset 14, -4
 6500 0002 0546     		mov	r5, r0
3254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 6501              		.loc 1 3254 3 is_stmt 1 view .LVU2179
3254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 6502              		.loc 1 3254 22 is_stmt 0 view .LVU2180
 6503 0004 446A     		ldr	r4, [r0, #36]
 6504              	.LVL416:
3255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 6505              		.loc 1 3255 3 is_stmt 1 view .LVU2181
3263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6506              		.loc 1 3263 3 view .LVU2182
3263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6507              		.loc 1 3263 15 is_stmt 0 view .LVU2183
 6508 0006 FFF7FEFF 		bl	HAL_GetTick
 6509              	.LVL417:
3266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6510              		.loc 1 3266 3 is_stmt 1 view .LVU2184
3266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6511              		.loc 1 3266 12 is_stmt 0 view .LVU2185
 6512 000a 2B68     		ldr	r3, [r5]
3266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6513              		.loc 1 3266 22 view .LVU2186
 6514 000c 1B68     		ldr	r3, [r3]
3266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6515              		.loc 1 3266 6 view .LVU2187
 6516 000e 13F0200F 		tst	r3, #32
 6517 0012 1CD1     		bne	.L440
 6518 0014 0246     		mov	r2, r0
3269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6519              		.loc 1 3269 5 is_stmt 1 view .LVU2188
 6520 0016 2168     		ldr	r1, [r4]
 6521 0018 4B68     		ldr	r3, [r1, #4]
 6522 001a 23F02003 		bic	r3, r3, #32
 6523 001e 4B60     		str	r3, [r1, #4]
3306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6524              		.loc 1 3306 5 view .LVU2189
3306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6525              		.loc 1 3306 9 is_stmt 0 view .LVU2190
 6526 0020 6421     		movs	r1, #100
 6527 0022 2046     		mov	r0, r4
 6528              	.LVL418:
3306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6529              		.loc 1 3306 9 view .LVU2191
 6530 0024 FFF7FEFF 		bl	SPI_EndRxTxTransaction
 6531              	.LVL419:
3306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6532              		.loc 1 3306 8 discriminator 1 view .LVU2192
ARM GAS  /tmp/cc5SiBtg.s 			page 228


 6533 0028 18B1     		cbz	r0, .L441
3308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6534              		.loc 1 3308 7 is_stmt 1 view .LVU2193
 6535 002a 236E     		ldr	r3, [r4, #96]
 6536 002c 43F02003 		orr	r3, r3, #32
 6537 0030 2366     		str	r3, [r4, #96]
 6538              	.L441:
3312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6539              		.loc 1 3312 5 view .LVU2194
 6540 0032 2268     		ldr	r2, [r4]
 6541 0034 5368     		ldr	r3, [r2, #4]
 6542 0036 23F00303 		bic	r3, r3, #3
 6543 003a 5360     		str	r3, [r2, #4]
3314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount = 0U;
 6544              		.loc 1 3314 5 view .LVU2195
3314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount = 0U;
 6545              		.loc 1 3314 23 is_stmt 0 view .LVU2196
 6546 003c 0023     		movs	r3, #0
 6547 003e E387     		strh	r3, [r4, #62]	@ movhi
3315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 6548              		.loc 1 3315 5 is_stmt 1 view .LVU2197
3315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 6549              		.loc 1 3315 23 is_stmt 0 view .LVU2198
 6550 0040 A4F84630 		strh	r3, [r4, #70]	@ movhi
3316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6551              		.loc 1 3316 5 is_stmt 1 view .LVU2199
3316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6552              		.loc 1 3316 17 is_stmt 0 view .LVU2200
 6553 0044 0123     		movs	r3, #1
 6554 0046 84F85D30 		strb	r3, [r4, #93]
3327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6555              		.loc 1 3327 5 is_stmt 1 view .LVU2201
3327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6556              		.loc 1 3327 13 is_stmt 0 view .LVU2202
 6557 004a 236E     		ldr	r3, [r4, #96]
3327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6558              		.loc 1 3327 8 view .LVU2203
 6559 004c 1BB9     		cbnz	r3, .L444
 6560              	.L440:
3342:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6561              		.loc 1 3342 3 is_stmt 1 view .LVU2204
 6562 004e 2046     		mov	r0, r4
 6563 0050 FFF7FEFF 		bl	HAL_SPI_TxRxCpltCallback
 6564              	.LVL420:
 6565              	.L439:
3344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6566              		.loc 1 3344 1 is_stmt 0 view .LVU2205
 6567 0054 38BD     		pop	{r3, r4, r5, pc}
 6568              	.LVL421:
 6569              	.L444:
3333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6570              		.loc 1 3333 7 is_stmt 1 view .LVU2206
 6571 0056 2046     		mov	r0, r4
 6572 0058 FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6573              	.LVL422:
3335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6574              		.loc 1 3335 7 view .LVU2207
ARM GAS  /tmp/cc5SiBtg.s 			page 229


 6575 005c FAE7     		b	.L439
 6576              		.cfi_endproc
 6577              	.LFE154:
 6579              		.section	.text.HAL_SPI_IRQHandler,"ax",%progbits
 6580              		.align	1
 6581              		.global	HAL_SPI_IRQHandler
 6582              		.syntax unified
 6583              		.thumb
 6584              		.thumb_func
 6586              	HAL_SPI_IRQHandler:
 6587              	.LVL423:
 6588              	.LFB141:
2786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itsource = hspi->Instance->CR2;
 6589              		.loc 1 2786 1 view -0
 6590              		.cfi_startproc
 6591              		@ args = 0, pretend = 0, frame = 16
 6592              		@ frame_needed = 0, uses_anonymous_args = 0
2786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itsource = hspi->Instance->CR2;
 6593              		.loc 1 2786 1 is_stmt 0 view .LVU2209
 6594 0000 30B5     		push	{r4, r5, lr}
 6595              		.cfi_def_cfa_offset 12
 6596              		.cfi_offset 4, -12
 6597              		.cfi_offset 5, -8
 6598              		.cfi_offset 14, -4
 6599 0002 85B0     		sub	sp, sp, #20
 6600              		.cfi_def_cfa_offset 32
 6601 0004 0446     		mov	r4, r0
2787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itflag   = hspi->Instance->SR;
 6602              		.loc 1 2787 3 is_stmt 1 view .LVU2210
2787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itflag   = hspi->Instance->SR;
 6603              		.loc 1 2787 27 is_stmt 0 view .LVU2211
 6604 0006 0268     		ldr	r2, [r0]
2787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itflag   = hspi->Instance->SR;
 6605              		.loc 1 2787 12 view .LVU2212
 6606 0008 5168     		ldr	r1, [r2, #4]
 6607              	.LVL424:
2788:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6608              		.loc 1 2788 3 is_stmt 1 view .LVU2213
2788:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6609              		.loc 1 2788 12 is_stmt 0 view .LVU2214
 6610 000a 9368     		ldr	r3, [r2, #8]
 6611              	.LVL425:
2791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (SPI_CHECK_FLAG(itflag, SPI_FLAG_RXNE) != RESET) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT_RXN
 6612              		.loc 1 2791 3 is_stmt 1 view .LVU2215
 6613 000c C3F38010 		ubfx	r0, r3, #6, #1
 6614              	.LVL426:
2791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (SPI_CHECK_FLAG(itflag, SPI_FLAG_RXNE) != RESET) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT_RXN
 6615              		.loc 1 2791 6 is_stmt 0 view .LVU2216
 6616 0010 13F0400F 		tst	r3, #64
 6617 0014 05D1     		bne	.L446
2791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (SPI_CHECK_FLAG(itflag, SPI_FLAG_RXNE) != RESET) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT_RXN
 6618              		.loc 1 2791 55 discriminator 1 view .LVU2217
 6619 0016 13F0010F 		tst	r3, #1
 6620 001a 02D0     		beq	.L446
2792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6621              		.loc 1 2792 56 view .LVU2218
 6622 001c 11F0400F 		tst	r1, #64
ARM GAS  /tmp/cc5SiBtg.s 			page 230


 6623 0020 69D1     		bne	.L458
 6624              	.L446:
2799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6625              		.loc 1 2799 3 is_stmt 1 view .LVU2219
2799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6626              		.loc 1 2799 6 is_stmt 0 view .LVU2220
 6627 0022 13F0020F 		tst	r3, #2
 6628 0026 02D0     		beq	.L448
2799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6629              		.loc 1 2799 55 discriminator 1 view .LVU2221
 6630 0028 11F0800F 		tst	r1, #128
 6631 002c 67D1     		bne	.L459
 6632              	.L448:
2806:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        || (SPI_CHECK_FLAG(itflag, SPI_FLAG_FRE) != RESET)) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT
 6633              		.loc 1 2806 3 is_stmt 1 view .LVU2222
 6634 002e C3F34015 		ubfx	r5, r3, #5, #1
2806:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        || (SPI_CHECK_FLAG(itflag, SPI_FLAG_FRE) != RESET)) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT
 6635              		.loc 1 2806 6 is_stmt 0 view .LVU2223
 6636 0032 13F0200F 		tst	r3, #32
 6637 0036 03D1     		bne	.L449
2806:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        || (SPI_CHECK_FLAG(itflag, SPI_FLAG_FRE) != RESET)) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT
 6638              		.loc 1 2806 57 discriminator 1 view .LVU2224
 6639 0038 10B9     		cbnz	r0, .L449
2807:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6640              		.loc 1 2807 8 view .LVU2225
 6641 003a 13F4807F 		tst	r3, #256
 6642 003e 61D0     		beq	.L445
 6643              	.L449:
2807:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6644              		.loc 1 2807 60 discriminator 1 view .LVU2226
 6645 0040 11F0200F 		tst	r1, #32
 6646 0044 5ED0     		beq	.L445
2810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6647              		.loc 1 2810 5 is_stmt 1 view .LVU2227
2810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6648              		.loc 1 2810 8 is_stmt 0 view .LVU2228
 6649 0046 78B1     		cbz	r0, .L450
2812:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6650              		.loc 1 2812 7 is_stmt 1 view .LVU2229
2812:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6651              		.loc 1 2812 15 is_stmt 0 view .LVU2230
 6652 0048 94F85D00 		ldrb	r0, [r4, #93]	@ zero_extendqisi2
 6653 004c C0B2     		uxtb	r0, r0
2812:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6654              		.loc 1 2812 10 view .LVU2231
 6655 004e 0328     		cmp	r0, #3
 6656 0050 5AD0     		beq	.L451
2814:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_SPI_CLEAR_OVRFLAG(hspi);
 6657              		.loc 1 2814 9 is_stmt 1 view .LVU2232
 6658 0052 206E     		ldr	r0, [r4, #96]
 6659 0054 40F00400 		orr	r0, r0, #4
 6660 0058 2066     		str	r0, [r4, #96]
2815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6661              		.loc 1 2815 9 view .LVU2233
 6662              	.LBB7:
2815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6663              		.loc 1 2815 9 view .LVU2234
ARM GAS  /tmp/cc5SiBtg.s 			page 231


 6664 005a 0020     		movs	r0, #0
 6665 005c 0090     		str	r0, [sp]
2815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6666              		.loc 1 2815 9 view .LVU2235
 6667 005e D068     		ldr	r0, [r2, #12]
 6668 0060 0090     		str	r0, [sp]
2815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6669              		.loc 1 2815 9 view .LVU2236
 6670 0062 9068     		ldr	r0, [r2, #8]
 6671 0064 0090     		str	r0, [sp]
2815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6672              		.loc 1 2815 9 view .LVU2237
 6673 0066 0098     		ldr	r0, [sp]
 6674              	.LBE7:
2815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6675              		.loc 1 2815 9 view .LVU2238
 6676              	.L450:
2825:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6677              		.loc 1 2825 5 view .LVU2239
2825:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6678              		.loc 1 2825 8 is_stmt 0 view .LVU2240
 6679 0068 65B1     		cbz	r5, .L452
2827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_MODFFLAG(hspi);
 6680              		.loc 1 2827 7 is_stmt 1 view .LVU2241
 6681 006a 206E     		ldr	r0, [r4, #96]
 6682 006c 40F00100 		orr	r0, r0, #1
 6683 0070 2066     		str	r0, [r4, #96]
2828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6684              		.loc 1 2828 7 view .LVU2242
 6685              	.LBB8:
2828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6686              		.loc 1 2828 7 view .LVU2243
 6687 0072 0020     		movs	r0, #0
 6688 0074 0290     		str	r0, [sp, #8]
2828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6689              		.loc 1 2828 7 view .LVU2244
 6690 0076 9068     		ldr	r0, [r2, #8]
 6691 0078 0290     		str	r0, [sp, #8]
2828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6692              		.loc 1 2828 7 view .LVU2245
 6693 007a 1068     		ldr	r0, [r2]
 6694 007c 20F04000 		bic	r0, r0, #64
 6695 0080 1060     		str	r0, [r2]
2828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6696              		.loc 1 2828 7 view .LVU2246
 6697 0082 029A     		ldr	r2, [sp, #8]
 6698              	.L452:
2828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6699              		.loc 1 2828 7 is_stmt 0 view .LVU2247
 6700              	.LBE8:
2828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6701              		.loc 1 2828 7 is_stmt 1 discriminator 1 view .LVU2248
2832:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6702              		.loc 1 2832 5 view .LVU2249
2832:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6703              		.loc 1 2832 8 is_stmt 0 view .LVU2250
 6704 0084 13F4807F 		tst	r3, #256
ARM GAS  /tmp/cc5SiBtg.s 			page 232


 6705 0088 09D0     		beq	.L453
2834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_FREFLAG(hspi);
 6706              		.loc 1 2834 7 is_stmt 1 view .LVU2251
 6707 008a 236E     		ldr	r3, [r4, #96]
 6708              	.LVL427:
2834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_FREFLAG(hspi);
 6709              		.loc 1 2834 7 is_stmt 0 view .LVU2252
 6710 008c 43F00803 		orr	r3, r3, #8
 6711 0090 2366     		str	r3, [r4, #96]
2835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6712              		.loc 1 2835 7 is_stmt 1 view .LVU2253
 6713              	.LBB9:
2835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6714              		.loc 1 2835 7 view .LVU2254
 6715 0092 0023     		movs	r3, #0
 6716 0094 0393     		str	r3, [sp, #12]
2835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6717              		.loc 1 2835 7 view .LVU2255
 6718 0096 2368     		ldr	r3, [r4]
 6719 0098 9B68     		ldr	r3, [r3, #8]
 6720 009a 0393     		str	r3, [sp, #12]
2835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6721              		.loc 1 2835 7 view .LVU2256
 6722 009c 039B     		ldr	r3, [sp, #12]
 6723              	.L453:
2835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6724              		.loc 1 2835 7 is_stmt 0 view .LVU2257
 6725              	.LBE9:
2835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6726              		.loc 1 2835 7 is_stmt 1 discriminator 1 view .LVU2258
2838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6727              		.loc 1 2838 5 view .LVU2259
2838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6728              		.loc 1 2838 13 is_stmt 0 view .LVU2260
 6729 009e 236E     		ldr	r3, [r4, #96]
2838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6730              		.loc 1 2838 8 view .LVU2261
 6731 00a0 002B     		cmp	r3, #0
 6732 00a2 2FD0     		beq	.L445
2841:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6733              		.loc 1 2841 7 is_stmt 1 view .LVU2262
 6734 00a4 2268     		ldr	r2, [r4]
 6735 00a6 5368     		ldr	r3, [r2, #4]
 6736 00a8 23F0E003 		bic	r3, r3, #224
 6737 00ac 5360     		str	r3, [r2, #4]
2843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable the SPI DMA requests if enabled */
 6738              		.loc 1 2843 7 view .LVU2263
2843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable the SPI DMA requests if enabled */
 6739              		.loc 1 2843 19 is_stmt 0 view .LVU2264
 6740 00ae 0123     		movs	r3, #1
 6741 00b0 84F85D30 		strb	r3, [r4, #93]
2845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6742              		.loc 1 2845 7 is_stmt 1 view .LVU2265
2845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6743              		.loc 1 2845 10 is_stmt 0 view .LVU2266
 6744 00b4 11F0030F 		tst	r1, #3
 6745 00b8 2ED0     		beq	.L455
ARM GAS  /tmp/cc5SiBtg.s 			page 233


2847:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6746              		.loc 1 2847 9 is_stmt 1 view .LVU2267
 6747 00ba 2268     		ldr	r2, [r4]
 6748 00bc 5368     		ldr	r3, [r2, #4]
 6749 00be 23F00303 		bic	r3, r3, #3
 6750 00c2 5360     		str	r3, [r2, #4]
2850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 6751              		.loc 1 2850 9 view .LVU2268
2850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 6752              		.loc 1 2850 17 is_stmt 0 view .LVU2269
 6753 00c4 A36D     		ldr	r3, [r4, #88]
2850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 6754              		.loc 1 2850 12 view .LVU2270
 6755 00c6 4BB1     		cbz	r3, .L456
2854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmarx))
 6756              		.loc 1 2854 11 is_stmt 1 view .LVU2271
2854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmarx))
 6757              		.loc 1 2854 43 is_stmt 0 view .LVU2272
 6758 00c8 154A     		ldr	r2, .L460
 6759 00ca 5A63     		str	r2, [r3, #52]
2855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 6760              		.loc 1 2855 11 is_stmt 1 view .LVU2273
2855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 6761              		.loc 1 2855 25 is_stmt 0 view .LVU2274
 6762 00cc A06D     		ldr	r0, [r4, #88]
 6763 00ce FFF7FEFF 		bl	HAL_DMA_Abort_IT
 6764              	.LVL428:
2855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 6765              		.loc 1 2855 14 discriminator 1 view .LVU2275
 6766 00d2 18B1     		cbz	r0, .L456
2857:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
 6767              		.loc 1 2857 13 is_stmt 1 view .LVU2276
 6768 00d4 236E     		ldr	r3, [r4, #96]
 6769 00d6 43F04003 		orr	r3, r3, #64
 6770 00da 2366     		str	r3, [r4, #96]
 6771              	.L456:
2861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 6772              		.loc 1 2861 9 view .LVU2277
2861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 6773              		.loc 1 2861 17 is_stmt 0 view .LVU2278
 6774 00dc 636D     		ldr	r3, [r4, #84]
2861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 6775              		.loc 1 2861 12 view .LVU2279
 6776 00de 8BB1     		cbz	r3, .L445
2865:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmatx))
 6777              		.loc 1 2865 11 is_stmt 1 view .LVU2280
2865:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmatx))
 6778              		.loc 1 2865 43 is_stmt 0 view .LVU2281
 6779 00e0 0F4A     		ldr	r2, .L460
 6780 00e2 5A63     		str	r2, [r3, #52]
2866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 6781              		.loc 1 2866 11 is_stmt 1 view .LVU2282
2866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 6782              		.loc 1 2866 25 is_stmt 0 view .LVU2283
 6783 00e4 606D     		ldr	r0, [r4, #84]
 6784 00e6 FFF7FEFF 		bl	HAL_DMA_Abort_IT
 6785              	.LVL429:
ARM GAS  /tmp/cc5SiBtg.s 			page 234


2866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 6786              		.loc 1 2866 14 discriminator 1 view .LVU2284
 6787 00ea 58B1     		cbz	r0, .L445
2868:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
 6788              		.loc 1 2868 13 is_stmt 1 view .LVU2285
 6789 00ec 236E     		ldr	r3, [r4, #96]
 6790 00ee 43F04003 		orr	r3, r3, #64
 6791 00f2 2366     		str	r3, [r4, #96]
 6792 00f4 06E0     		b	.L445
 6793              	.LVL430:
 6794              	.L458:
2794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
 6795              		.loc 1 2794 5 view .LVU2286
2794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
 6796              		.loc 1 2794 9 is_stmt 0 view .LVU2287
 6797 00f6 E36C     		ldr	r3, [r4, #76]
 6798              	.LVL431:
2794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
 6799              		.loc 1 2794 5 view .LVU2288
 6800 00f8 2046     		mov	r0, r4
 6801 00fa 9847     		blx	r3
 6802              	.LVL432:
2795:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6803              		.loc 1 2795 5 is_stmt 1 view .LVU2289
 6804 00fc 02E0     		b	.L445
 6805              	.LVL433:
 6806              	.L459:
2801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
 6807              		.loc 1 2801 5 view .LVU2290
2801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
 6808              		.loc 1 2801 9 is_stmt 0 view .LVU2291
 6809 00fe 236D     		ldr	r3, [r4, #80]
 6810              	.LVL434:
2801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
 6811              		.loc 1 2801 5 view .LVU2292
 6812 0100 2046     		mov	r0, r4
 6813 0102 9847     		blx	r3
 6814              	.LVL435:
2802:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6815              		.loc 1 2802 5 is_stmt 1 view .LVU2293
 6816              	.L445:
2884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6817              		.loc 1 2884 1 is_stmt 0 view .LVU2294
 6818 0104 05B0     		add	sp, sp, #20
 6819              		.cfi_remember_state
 6820              		.cfi_def_cfa_offset 12
 6821              		@ sp needed
 6822 0106 30BD     		pop	{r4, r5, pc}
 6823              	.LVL436:
 6824              	.L451:
 6825              		.cfi_restore_state
2819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6826              		.loc 1 2819 9 is_stmt 1 view .LVU2295
 6827              	.LBB10:
2819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6828              		.loc 1 2819 9 view .LVU2296
 6829 0108 0023     		movs	r3, #0
ARM GAS  /tmp/cc5SiBtg.s 			page 235


 6830              	.LVL437:
2819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6831              		.loc 1 2819 9 is_stmt 0 view .LVU2297
 6832 010a 0193     		str	r3, [sp, #4]
2819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6833              		.loc 1 2819 9 is_stmt 1 view .LVU2298
 6834 010c D368     		ldr	r3, [r2, #12]
 6835 010e 0193     		str	r3, [sp, #4]
2819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6836              		.loc 1 2819 9 view .LVU2299
 6837 0110 9368     		ldr	r3, [r2, #8]
 6838 0112 0193     		str	r3, [sp, #4]
2819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6839              		.loc 1 2819 9 view .LVU2300
 6840 0114 019B     		ldr	r3, [sp, #4]
 6841              	.LBE10:
2819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6842              		.loc 1 2819 9 view .LVU2301
2820:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6843              		.loc 1 2820 9 view .LVU2302
 6844 0116 F5E7     		b	.L445
 6845              	.L455:
2878:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6846              		.loc 1 2878 9 view .LVU2303
 6847 0118 2046     		mov	r0, r4
 6848 011a FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6849              	.LVL438:
2882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6850              		.loc 1 2882 5 view .LVU2304
 6851 011e F1E7     		b	.L445
 6852              	.L461:
 6853              		.align	2
 6854              	.L460:
 6855 0120 00000000 		.word	SPI_DMAAbortOnError
 6856              		.cfi_endproc
 6857              	.LFE141:
 6859              		.section	.text.SPI_DMAAbortOnError,"ax",%progbits
 6860              		.align	1
 6861              		.syntax unified
 6862              		.thumb
 6863              		.thumb_func
 6865              	SPI_DMAAbortOnError:
 6866              	.LVL439:
 6867              	.LFB159:
3430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6868              		.loc 1 3430 1 view -0
 6869              		.cfi_startproc
 6870              		@ args = 0, pretend = 0, frame = 0
 6871              		@ frame_needed = 0, uses_anonymous_args = 0
3430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6872              		.loc 1 3430 1 is_stmt 0 view .LVU2306
 6873 0000 08B5     		push	{r3, lr}
 6874              		.cfi_def_cfa_offset 8
 6875              		.cfi_offset 3, -8
 6876              		.cfi_offset 14, -4
3431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 6877              		.loc 1 3431 3 is_stmt 1 view .LVU2307
ARM GAS  /tmp/cc5SiBtg.s 			page 236


3431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 6878              		.loc 1 3431 22 is_stmt 0 view .LVU2308
 6879 0002 406A     		ldr	r0, [r0, #36]
 6880              	.LVL440:
3432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 6881              		.loc 1 3432 3 is_stmt 1 view .LVU2309
3432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 6882              		.loc 1 3432 21 is_stmt 0 view .LVU2310
 6883 0004 0023     		movs	r3, #0
 6884 0006 A0F84630 		strh	r3, [r0, #70]	@ movhi
3433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6885              		.loc 1 3433 3 is_stmt 1 view .LVU2311
3433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6886              		.loc 1 3433 21 is_stmt 0 view .LVU2312
 6887 000a C387     		strh	r3, [r0, #62]	@ movhi
3439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6888              		.loc 1 3439 3 is_stmt 1 view .LVU2313
 6889 000c FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6890              	.LVL441:
3441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6891              		.loc 1 3441 1 is_stmt 0 view .LVU2314
 6892 0010 08BD     		pop	{r3, pc}
 6893              		.cfi_endproc
 6894              	.LFE159:
 6896              		.section	.text.HAL_SPI_AbortCpltCallback,"ax",%progbits
 6897              		.align	1
 6898              		.weak	HAL_SPI_AbortCpltCallback
 6899              		.syntax unified
 6900              		.thumb
 6901              		.thumb_func
 6903              	HAL_SPI_AbortCpltCallback:
 6904              	.LVL442:
 6905              	.LFB149:
3007:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 6906              		.loc 1 3007 1 is_stmt 1 view -0
 6907              		.cfi_startproc
 6908              		@ args = 0, pretend = 0, frame = 0
 6909              		@ frame_needed = 0, uses_anonymous_args = 0
 6910              		@ link register save eliminated.
3009:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6911              		.loc 1 3009 3 view .LVU2316
3014:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6912              		.loc 1 3014 1 is_stmt 0 view .LVU2317
 6913 0000 7047     		bx	lr
 6914              		.cfi_endproc
 6915              	.LFE149:
 6917              		.section	.text.HAL_SPI_Abort_IT,"ax",%progbits
 6918              		.align	1
 6919              		.global	HAL_SPI_Abort_IT
 6920              		.syntax unified
 6921              		.thumb
 6922              		.thumb_func
 6924              	HAL_SPI_Abort_IT:
 6925              	.LVL443:
 6926              	.LFB137:
2545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
 6927              		.loc 1 2545 1 is_stmt 1 view -0
ARM GAS  /tmp/cc5SiBtg.s 			page 237


 6928              		.cfi_startproc
 6929              		@ args = 0, pretend = 0, frame = 16
 6930              		@ frame_needed = 0, uses_anonymous_args = 0
2545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
 6931              		.loc 1 2545 1 is_stmt 0 view .LVU2319
 6932 0000 70B5     		push	{r4, r5, r6, lr}
 6933              		.cfi_def_cfa_offset 16
 6934              		.cfi_offset 4, -16
 6935              		.cfi_offset 5, -12
 6936              		.cfi_offset 6, -8
 6937              		.cfi_offset 14, -4
 6938 0002 84B0     		sub	sp, sp, #16
 6939              		.cfi_def_cfa_offset 32
 6940 0004 0446     		mov	r4, r0
2546:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t abortcplt ;
 6941              		.loc 1 2546 3 is_stmt 1 view .LVU2320
2547:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
 6942              		.loc 1 2547 3 view .LVU2321
2548:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t resetcount;
 6943              		.loc 1 2548 3 view .LVU2322
2549:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6944              		.loc 1 2549 3 view .LVU2323
2552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   abortcplt = 1U;
 6945              		.loc 1 2552 3 view .LVU2324
 6946              	.LVL444:
2553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 6947              		.loc 1 2553 3 view .LVU2325
2554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 6948              		.loc 1 2554 3 view .LVU2326
2554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 6949              		.loc 1 2554 61 is_stmt 0 view .LVU2327
 6950 0006 504B     		ldr	r3, .L491
 6951 0008 1B68     		ldr	r3, [r3]
 6952 000a 504A     		ldr	r2, .L491+4
 6953 000c A2FB0323 		umull	r2, r3, r2, r3
 6954 0010 5B0A     		lsrs	r3, r3, #9
2554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 6955              		.loc 1 2554 36 view .LVU2328
 6956 0012 6422     		movs	r2, #100
 6957 0014 02FB03F3 		mul	r3, r2, r3
2554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 6958              		.loc 1 2554 14 view .LVU2329
 6959 0018 0293     		str	r3, [sp, #8]
2555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6960              		.loc 1 2555 3 is_stmt 1 view .LVU2330
2555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6961              		.loc 1 2555 9 is_stmt 0 view .LVU2331
 6962 001a 029B     		ldr	r3, [sp, #8]
 6963 001c 0393     		str	r3, [sp, #12]
2558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6964              		.loc 1 2558 3 is_stmt 1 view .LVU2332
 6965 001e 0268     		ldr	r2, [r0]
 6966 0020 5368     		ldr	r3, [r2, #4]
 6967 0022 23F02003 		bic	r3, r3, #32
 6968 0026 5360     		str	r3, [r2, #4]
2561:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6969              		.loc 1 2561 3 view .LVU2333
ARM GAS  /tmp/cc5SiBtg.s 			page 238


2561:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6970              		.loc 1 2561 7 is_stmt 0 view .LVU2334
 6971 0028 0268     		ldr	r2, [r0]
 6972 002a 5368     		ldr	r3, [r2, #4]
2561:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6973              		.loc 1 2561 6 view .LVU2335
 6974 002c 13F0800F 		tst	r3, #128
 6975 0030 12D0     		beq	.L466
2563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 6976              		.loc 1 2563 5 is_stmt 1 view .LVU2336
2563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 6977              		.loc 1 2563 17 is_stmt 0 view .LVU2337
 6978 0032 474B     		ldr	r3, .L491+8
 6979 0034 0365     		str	r3, [r0, #80]
 6980              	.L469:
2565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6981              		.loc 1 2565 5 is_stmt 1 view .LVU2338
2567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6982              		.loc 1 2567 7 view .LVU2339
2567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6983              		.loc 1 2567 17 is_stmt 0 view .LVU2340
 6984 0036 039B     		ldr	r3, [sp, #12]
2567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6985              		.loc 1 2567 10 view .LVU2341
 6986 0038 43B1     		cbz	r3, .L488
2572:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 6987              		.loc 1 2572 7 is_stmt 1 view .LVU2342
2572:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 6988              		.loc 1 2572 12 is_stmt 0 view .LVU2343
 6989 003a 039B     		ldr	r3, [sp, #12]
 6990 003c 013B     		subs	r3, r3, #1
 6991 003e 0393     		str	r3, [sp, #12]
2573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 6992              		.loc 1 2573 26 is_stmt 1 view .LVU2344
2573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 6993              		.loc 1 2573 18 is_stmt 0 view .LVU2345
 6994 0040 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 6995 0044 DBB2     		uxtb	r3, r3
2573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 6996              		.loc 1 2573 26 view .LVU2346
 6997 0046 072B     		cmp	r3, #7
 6998 0048 F5D1     		bne	.L469
 6999 004a 03E0     		b	.L468
 7000              	.L488:
2569:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 7001              		.loc 1 2569 9 is_stmt 1 view .LVU2347
 7002 004c 236E     		ldr	r3, [r4, #96]
 7003 004e 43F04003 		orr	r3, r3, #64
 7004 0052 2366     		str	r3, [r4, #96]
2570:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7005              		.loc 1 2570 9 view .LVU2348
 7006              	.L468:
2575:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7007              		.loc 1 2575 5 view .LVU2349
2575:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7008              		.loc 1 2575 11 is_stmt 0 view .LVU2350
 7009 0054 029B     		ldr	r3, [sp, #8]
ARM GAS  /tmp/cc5SiBtg.s 			page 239


 7010 0056 0393     		str	r3, [sp, #12]
 7011              	.L466:
2578:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7012              		.loc 1 2578 3 is_stmt 1 view .LVU2351
2578:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7013              		.loc 1 2578 7 is_stmt 0 view .LVU2352
 7014 0058 5368     		ldr	r3, [r2, #4]
2578:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7015              		.loc 1 2578 6 view .LVU2353
 7016 005a 13F0400F 		tst	r3, #64
 7017 005e 12D0     		beq	.L470
2580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 7018              		.loc 1 2580 5 is_stmt 1 view .LVU2354
2580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 7019              		.loc 1 2580 17 is_stmt 0 view .LVU2355
 7020 0060 3C4B     		ldr	r3, .L491+12
 7021 0062 E364     		str	r3, [r4, #76]
 7022              	.L473:
2582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7023              		.loc 1 2582 5 is_stmt 1 view .LVU2356
2584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7024              		.loc 1 2584 7 view .LVU2357
2584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7025              		.loc 1 2584 17 is_stmt 0 view .LVU2358
 7026 0064 039B     		ldr	r3, [sp, #12]
2584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7027              		.loc 1 2584 10 view .LVU2359
 7028 0066 43B1     		cbz	r3, .L489
2589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 7029              		.loc 1 2589 7 is_stmt 1 view .LVU2360
2589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 7030              		.loc 1 2589 12 is_stmt 0 view .LVU2361
 7031 0068 039B     		ldr	r3, [sp, #12]
 7032 006a 013B     		subs	r3, r3, #1
 7033 006c 0393     		str	r3, [sp, #12]
2590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 7034              		.loc 1 2590 26 is_stmt 1 view .LVU2362
2590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 7035              		.loc 1 2590 18 is_stmt 0 view .LVU2363
 7036 006e 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 7037 0072 DBB2     		uxtb	r3, r3
2590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 7038              		.loc 1 2590 26 view .LVU2364
 7039 0074 072B     		cmp	r3, #7
 7040 0076 F5D1     		bne	.L473
 7041 0078 03E0     		b	.L472
 7042              	.L489:
2586:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 7043              		.loc 1 2586 9 is_stmt 1 view .LVU2365
 7044 007a 236E     		ldr	r3, [r4, #96]
 7045 007c 43F04003 		orr	r3, r3, #64
 7046 0080 2366     		str	r3, [r4, #96]
2587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7047              		.loc 1 2587 9 view .LVU2366
 7048              	.L472:
2592:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7049              		.loc 1 2592 5 view .LVU2367
ARM GAS  /tmp/cc5SiBtg.s 			page 240


2592:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7050              		.loc 1 2592 11 is_stmt 0 view .LVU2368
 7051 0082 029B     		ldr	r3, [sp, #8]
 7052 0084 0393     		str	r3, [sp, #12]
 7053              	.L470:
2598:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7054              		.loc 1 2598 3 is_stmt 1 view .LVU2369
2598:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7055              		.loc 1 2598 11 is_stmt 0 view .LVU2370
 7056 0086 636D     		ldr	r3, [r4, #84]
2598:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7057              		.loc 1 2598 6 view .LVU2371
 7058 0088 2BB1     		cbz	r3, .L474
2602:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7059              		.loc 1 2602 5 is_stmt 1 view .LVU2372
2602:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7060              		.loc 1 2602 9 is_stmt 0 view .LVU2373
 7061 008a 5268     		ldr	r2, [r2, #4]
2602:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7062              		.loc 1 2602 8 view .LVU2374
 7063 008c 12F0020F 		tst	r2, #2
 7064 0090 1BD0     		beq	.L475
2604:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7065              		.loc 1 2604 7 is_stmt 1 view .LVU2375
2604:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7066              		.loc 1 2604 39 is_stmt 0 view .LVU2376
 7067 0092 314A     		ldr	r2, .L491+16
 7068 0094 5A63     		str	r2, [r3, #52]
 7069              	.L474:
2612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7070              		.loc 1 2612 3 is_stmt 1 view .LVU2377
2612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7071              		.loc 1 2612 11 is_stmt 0 view .LVU2378
 7072 0096 A36D     		ldr	r3, [r4, #88]
2612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7073              		.loc 1 2612 6 view .LVU2379
 7074 0098 33B1     		cbz	r3, .L476
2616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7075              		.loc 1 2616 5 is_stmt 1 view .LVU2380
2616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7076              		.loc 1 2616 9 is_stmt 0 view .LVU2381
 7077 009a 2268     		ldr	r2, [r4]
 7078 009c 5268     		ldr	r2, [r2, #4]
2616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7079              		.loc 1 2616 8 view .LVU2382
 7080 009e 12F0010F 		tst	r2, #1
 7081 00a2 15D0     		beq	.L477
2618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7082              		.loc 1 2618 7 is_stmt 1 view .LVU2383
2618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7083              		.loc 1 2618 39 is_stmt 0 view .LVU2384
 7084 00a4 2D4A     		ldr	r2, .L491+20
 7085 00a6 5A63     		str	r2, [r3, #52]
 7086              	.L476:
2627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7087              		.loc 1 2627 3 is_stmt 1 view .LVU2385
2627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 241


 7088              		.loc 1 2627 7 is_stmt 0 view .LVU2386
 7089 00a8 2368     		ldr	r3, [r4]
 7090 00aa 5B68     		ldr	r3, [r3, #4]
2627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7091              		.loc 1 2627 6 view .LVU2387
 7092 00ac 13F0020F 		tst	r3, #2
 7093 00b0 11D0     		beq	.L482
2630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7094              		.loc 1 2630 5 is_stmt 1 view .LVU2388
2630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7095              		.loc 1 2630 13 is_stmt 0 view .LVU2389
 7096 00b2 606D     		ldr	r0, [r4, #84]
 7097              	.LVL445:
2630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7098              		.loc 1 2630 8 view .LVU2390
 7099 00b4 28B3     		cbz	r0, .L483
2633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7100              		.loc 1 2633 7 is_stmt 1 view .LVU2391
2633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7101              		.loc 1 2633 11 is_stmt 0 view .LVU2392
 7102 00b6 FFF7FEFF 		bl	HAL_DMA_Abort_IT
 7103              	.LVL446:
2633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7104              		.loc 1 2633 10 discriminator 1 view .LVU2393
 7105 00ba 20B3     		cbz	r0, .L484
2635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 7106              		.loc 1 2635 9 is_stmt 1 view .LVU2394
2635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 7107              		.loc 1 2635 13 is_stmt 0 view .LVU2395
 7108 00bc 636D     		ldr	r3, [r4, #84]
2635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 7109              		.loc 1 2635 41 view .LVU2396
 7110 00be 0022     		movs	r2, #0
 7111 00c0 5A63     		str	r2, [r3, #52]
2636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7112              		.loc 1 2636 9 is_stmt 1 view .LVU2397
2636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7113              		.loc 1 2636 25 is_stmt 0 view .LVU2398
 7114 00c2 4023     		movs	r3, #64
 7115 00c4 2366     		str	r3, [r4, #96]
2553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 7116              		.loc 1 2553 13 view .LVU2399
 7117 00c6 0126     		movs	r6, #1
 7118 00c8 06E0     		b	.L478
 7119              	.LVL447:
 7120              	.L475:
2608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7121              		.loc 1 2608 7 is_stmt 1 view .LVU2400
2608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7122              		.loc 1 2608 39 is_stmt 0 view .LVU2401
 7123 00ca 0022     		movs	r2, #0
 7124 00cc 5A63     		str	r2, [r3, #52]
 7125 00ce E2E7     		b	.L474
 7126              	.L477:
2622:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7127              		.loc 1 2622 7 is_stmt 1 view .LVU2402
2622:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
ARM GAS  /tmp/cc5SiBtg.s 			page 242


 7128              		.loc 1 2622 39 is_stmt 0 view .LVU2403
 7129 00d0 0022     		movs	r2, #0
 7130 00d2 5A63     		str	r2, [r3, #52]
 7131 00d4 E8E7     		b	.L476
 7132              	.L482:
2553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 7133              		.loc 1 2553 13 view .LVU2404
 7134 00d6 0126     		movs	r6, #1
 7135              	.LVL448:
 7136              	.L478:
2645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7137              		.loc 1 2645 3 is_stmt 1 view .LVU2405
2645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7138              		.loc 1 2645 7 is_stmt 0 view .LVU2406
 7139 00d8 2368     		ldr	r3, [r4]
 7140 00da 5B68     		ldr	r3, [r3, #4]
2645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7141              		.loc 1 2645 6 view .LVU2407
 7142 00dc 13F0010F 		tst	r3, #1
 7143 00e0 0AD0     		beq	.L479
2648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7144              		.loc 1 2648 5 is_stmt 1 view .LVU2408
2648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7145              		.loc 1 2648 13 is_stmt 0 view .LVU2409
 7146 00e2 A06D     		ldr	r0, [r4, #88]
2648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7147              		.loc 1 2648 8 view .LVU2410
 7148 00e4 40B1     		cbz	r0, .L479
2651:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7149              		.loc 1 2651 7 is_stmt 1 view .LVU2411
2651:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7150              		.loc 1 2651 11 is_stmt 0 view .LVU2412
 7151 00e6 FFF7FEFF 		bl	HAL_DMA_Abort_IT
 7152              	.LVL449:
2651:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7153              		.loc 1 2651 10 discriminator 1 view .LVU2413
 7154 00ea 0546     		mov	r5, r0
 7155 00ec 30B1     		cbz	r0, .L480
2653:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 7156              		.loc 1 2653 9 is_stmt 1 view .LVU2414
2653:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 7157              		.loc 1 2653 13 is_stmt 0 view .LVU2415
 7158 00ee A36D     		ldr	r3, [r4, #88]
2653:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 7159              		.loc 1 2653 41 view .LVU2416
 7160 00f0 0022     		movs	r2, #0
 7161 00f2 5A63     		str	r2, [r3, #52]
2654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7162              		.loc 1 2654 9 is_stmt 1 view .LVU2417
2654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7163              		.loc 1 2654 25 is_stmt 0 view .LVU2418
 7164 00f4 4023     		movs	r3, #64
 7165 00f6 2366     		str	r3, [r4, #96]
 7166              	.L479:
2663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7167              		.loc 1 2663 3 is_stmt 1 view .LVU2419
2663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 243


 7168              		.loc 1 2663 6 is_stmt 0 view .LVU2420
 7169 00f8 3EB9     		cbnz	r6, .L490
2552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   abortcplt = 1U;
 7170              		.loc 1 2552 13 view .LVU2421
 7171 00fa 0025     		movs	r5, #0
 7172              	.LVL450:
 7173              	.L480:
2696:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 7174              		.loc 1 2696 3 is_stmt 1 view .LVU2422
2697:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7175              		.loc 1 2697 1 is_stmt 0 view .LVU2423
 7176 00fc 2846     		mov	r0, r5
 7177 00fe 04B0     		add	sp, sp, #16
 7178              		.cfi_remember_state
 7179              		.cfi_def_cfa_offset 16
 7180              		@ sp needed
 7181 0100 70BD     		pop	{r4, r5, r6, pc}
 7182              	.LVL451:
 7183              	.L483:
 7184              		.cfi_restore_state
2553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 7185              		.loc 1 2553 13 view .LVU2424
 7186 0102 0126     		movs	r6, #1
 7187 0104 E8E7     		b	.L478
 7188              	.L484:
2640:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7189              		.loc 1 2640 19 view .LVU2425
 7190 0106 0026     		movs	r6, #0
 7191 0108 E6E7     		b	.L478
 7192              	.LVL452:
 7193              	.L490:
2666:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount = 0U;
 7194              		.loc 1 2666 5 is_stmt 1 view .LVU2426
2666:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount = 0U;
 7195              		.loc 1 2666 23 is_stmt 0 view .LVU2427
 7196 010a 0023     		movs	r3, #0
 7197 010c A4F84630 		strh	r3, [r4, #70]	@ movhi
2667:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7198              		.loc 1 2667 5 is_stmt 1 view .LVU2428
2667:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7199              		.loc 1 2667 23 is_stmt 0 view .LVU2429
 7200 0110 E387     		strh	r3, [r4, #62]	@ movhi
2670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7201              		.loc 1 2670 5 is_stmt 1 view .LVU2430
2670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7202              		.loc 1 2670 13 is_stmt 0 view .LVU2431
 7203 0112 236E     		ldr	r3, [r4, #96]
2670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7204              		.loc 1 2670 8 view .LVU2432
 7205 0114 402B     		cmp	r3, #64
 7206 0116 14D0     		beq	.L486
2678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7207              		.loc 1 2678 7 is_stmt 1 view .LVU2433
2678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7208              		.loc 1 2678 23 is_stmt 0 view .LVU2434
 7209 0118 0025     		movs	r5, #0
 7210 011a 2566     		str	r5, [r4, #96]
ARM GAS  /tmp/cc5SiBtg.s 			page 244


 7211              	.L481:
 7212              	.LVL453:
2682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 7213              		.loc 1 2682 5 is_stmt 1 view .LVU2435
 7214              	.LBB11:
2682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 7215              		.loc 1 2682 5 view .LVU2436
 7216 011c 0022     		movs	r2, #0
 7217 011e 0092     		str	r2, [sp]
2682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 7218              		.loc 1 2682 5 view .LVU2437
 7219 0120 2368     		ldr	r3, [r4]
 7220 0122 D968     		ldr	r1, [r3, #12]
 7221 0124 0091     		str	r1, [sp]
2682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 7222              		.loc 1 2682 5 view .LVU2438
 7223 0126 9968     		ldr	r1, [r3, #8]
 7224 0128 0091     		str	r1, [sp]
2682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 7225              		.loc 1 2682 5 view .LVU2439
 7226 012a 0099     		ldr	r1, [sp]
 7227              	.LBE11:
2682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 7228              		.loc 1 2682 5 view .LVU2440
2683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7229              		.loc 1 2683 5 view .LVU2441
 7230              	.LBB12:
2683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7231              		.loc 1 2683 5 view .LVU2442
 7232 012c 0192     		str	r2, [sp, #4]
2683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7233              		.loc 1 2683 5 view .LVU2443
 7234 012e 9B68     		ldr	r3, [r3, #8]
 7235 0130 0193     		str	r3, [sp, #4]
2683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7236              		.loc 1 2683 5 view .LVU2444
 7237 0132 019B     		ldr	r3, [sp, #4]
 7238              	.LBE12:
2683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7239              		.loc 1 2683 5 view .LVU2445
2686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7240              		.loc 1 2686 5 view .LVU2446
2686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7241              		.loc 1 2686 17 is_stmt 0 view .LVU2447
 7242 0134 0123     		movs	r3, #1
 7243 0136 84F85D30 		strb	r3, [r4, #93]
2692:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 7244              		.loc 1 2692 5 is_stmt 1 view .LVU2448
 7245 013a 2046     		mov	r0, r4
 7246 013c FFF7FEFF 		bl	HAL_SPI_AbortCpltCallback
 7247              	.LVL454:
 7248 0140 DCE7     		b	.L480
 7249              	.LVL455:
 7250              	.L486:
2673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7251              		.loc 1 2673 17 is_stmt 0 view .LVU2449
 7252 0142 0125     		movs	r5, #1
ARM GAS  /tmp/cc5SiBtg.s 			page 245


 7253 0144 EAE7     		b	.L481
 7254              	.L492:
 7255 0146 00BF     		.align	2
 7256              	.L491:
 7257 0148 00000000 		.word	SystemCoreClock
 7258 014c F1197605 		.word	91625969
 7259 0150 00000000 		.word	SPI_AbortTx_ISR
 7260 0154 00000000 		.word	SPI_AbortRx_ISR
 7261 0158 00000000 		.word	SPI_DMATxAbortCallback
 7262 015c 00000000 		.word	SPI_DMARxAbortCallback
 7263              		.cfi_endproc
 7264              	.LFE137:
 7266              		.section	.text.SPI_DMARxAbortCallback,"ax",%progbits
 7267              		.align	1
 7268              		.syntax unified
 7269              		.thumb
 7270              		.thumb_func
 7272              	SPI_DMARxAbortCallback:
 7273              	.LVL456:
 7274              	.LFB161:
3518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 7275              		.loc 1 3518 1 is_stmt 1 view -0
 7276              		.cfi_startproc
 7277              		@ args = 0, pretend = 0, frame = 8
 7278              		@ frame_needed = 0, uses_anonymous_args = 0
3518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 7279              		.loc 1 3518 1 is_stmt 0 view .LVU2451
 7280 0000 30B5     		push	{r4, r5, lr}
 7281              		.cfi_def_cfa_offset 12
 7282              		.cfi_offset 4, -12
 7283              		.cfi_offset 5, -8
 7284              		.cfi_offset 14, -4
 7285 0002 85B0     		sub	sp, sp, #20
 7286              		.cfi_def_cfa_offset 32
3519:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7287              		.loc 1 3519 3 is_stmt 1 view .LVU2452
3519:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7288              		.loc 1 3519 22 is_stmt 0 view .LVU2453
 7289 0004 446A     		ldr	r4, [r0, #36]
 7290              	.LVL457:
3522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7291              		.loc 1 3522 3 is_stmt 1 view .LVU2454
 7292 0006 2268     		ldr	r2, [r4]
 7293 0008 1368     		ldr	r3, [r2]
 7294 000a 23F04003 		bic	r3, r3, #64
 7295 000e 1360     		str	r3, [r2]
3524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7296              		.loc 1 3524 3 view .LVU2455
3524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7297              		.loc 1 3524 7 is_stmt 0 view .LVU2456
 7298 0010 A36D     		ldr	r3, [r4, #88]
3524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7299              		.loc 1 3524 35 view .LVU2457
 7300 0012 0025     		movs	r5, #0
 7301 0014 5D63     		str	r5, [r3, #52]
3527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7302              		.loc 1 3527 3 is_stmt 1 view .LVU2458
ARM GAS  /tmp/cc5SiBtg.s 			page 246


 7303 0016 2268     		ldr	r2, [r4]
 7304 0018 5368     		ldr	r3, [r2, #4]
 7305 001a 23F00103 		bic	r3, r3, #1
 7306 001e 5360     		str	r3, [r2, #4]
3530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7307              		.loc 1 3530 3 view .LVU2459
3530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7308              		.loc 1 3530 7 is_stmt 0 view .LVU2460
 7309 0020 FFF7FEFF 		bl	HAL_GetTick
 7310              	.LVL458:
3530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7311              		.loc 1 3530 7 discriminator 1 view .LVU2461
 7312 0024 0090     		str	r0, [sp]
 7313 0026 6423     		movs	r3, #100
 7314 0028 2A46     		mov	r2, r5
 7315 002a 8021     		movs	r1, #128
 7316 002c 2046     		mov	r0, r4
 7317 002e FFF7FEFF 		bl	SPI_WaitFlagStateUntilTimeout
 7318              	.LVL459:
3530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7319              		.loc 1 3530 6 discriminator 2 view .LVU2462
 7320 0032 08B1     		cbz	r0, .L494
3532:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7321              		.loc 1 3532 5 is_stmt 1 view .LVU2463
3532:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7322              		.loc 1 3532 21 is_stmt 0 view .LVU2464
 7323 0034 4023     		movs	r3, #64
 7324 0036 2366     		str	r3, [r4, #96]
 7325              	.L494:
3536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7326              		.loc 1 3536 3 is_stmt 1 view .LVU2465
3536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7327              		.loc 1 3536 7 is_stmt 0 view .LVU2466
 7328 0038 FFF7FEFF 		bl	HAL_GetTick
 7329              	.LVL460:
3536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7330              		.loc 1 3536 7 discriminator 1 view .LVU2467
 7331 003c 0090     		str	r0, [sp]
 7332 003e 6423     		movs	r3, #100
 7333 0040 0022     		movs	r2, #0
 7334 0042 4FF4C061 		mov	r1, #1536
 7335 0046 2046     		mov	r0, r4
 7336 0048 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 7337              	.LVL461:
3536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7338              		.loc 1 3536 6 discriminator 2 view .LVU2468
 7339 004c 08B1     		cbz	r0, .L495
3538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7340              		.loc 1 3538 5 is_stmt 1 view .LVU2469
3538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7341              		.loc 1 3538 21 is_stmt 0 view .LVU2470
 7342 004e 4023     		movs	r3, #64
 7343 0050 2366     		str	r3, [r4, #96]
 7344              	.L495:
3542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7345              		.loc 1 3542 3 is_stmt 1 view .LVU2471
3542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 247


 7346              		.loc 1 3542 11 is_stmt 0 view .LVU2472
 7347 0052 636D     		ldr	r3, [r4, #84]
3542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7348              		.loc 1 3542 6 view .LVU2473
 7349 0054 0BB1     		cbz	r3, .L496
3544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7350              		.loc 1 3544 5 is_stmt 1 view .LVU2474
3544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7351              		.loc 1 3544 21 is_stmt 0 view .LVU2475
 7352 0056 5B6B     		ldr	r3, [r3, #52]
3544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7353              		.loc 1 3544 8 view .LVU2476
 7354 0058 D3B9     		cbnz	r3, .L493
 7355              	.L496:
3551:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 7356              		.loc 1 3551 3 is_stmt 1 view .LVU2477
3551:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 7357              		.loc 1 3551 21 is_stmt 0 view .LVU2478
 7358 005a 0023     		movs	r3, #0
 7359 005c A4F84630 		strh	r3, [r4, #70]	@ movhi
3552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7360              		.loc 1 3552 3 is_stmt 1 view .LVU2479
3552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7361              		.loc 1 3552 21 is_stmt 0 view .LVU2480
 7362 0060 E387     		strh	r3, [r4, #62]	@ movhi
3555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7363              		.loc 1 3555 3 is_stmt 1 view .LVU2481
3555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7364              		.loc 1 3555 11 is_stmt 0 view .LVU2482
 7365 0062 236E     		ldr	r3, [r4, #96]
3555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7366              		.loc 1 3555 6 view .LVU2483
 7367 0064 402B     		cmp	r3, #64
 7368 0066 01D0     		beq	.L498
3558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7369              		.loc 1 3558 5 is_stmt 1 view .LVU2484
3558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7370              		.loc 1 3558 21 is_stmt 0 view .LVU2485
 7371 0068 0023     		movs	r3, #0
 7372 006a 2366     		str	r3, [r4, #96]
 7373              	.L498:
3562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7374              		.loc 1 3562 3 is_stmt 1 view .LVU2486
 7375              	.LBB13:
3562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7376              		.loc 1 3562 3 view .LVU2487
 7377 006c 0022     		movs	r2, #0
 7378 006e 0292     		str	r2, [sp, #8]
3562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7379              		.loc 1 3562 3 view .LVU2488
 7380 0070 2368     		ldr	r3, [r4]
 7381 0072 D968     		ldr	r1, [r3, #12]
 7382 0074 0291     		str	r1, [sp, #8]
3562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7383              		.loc 1 3562 3 view .LVU2489
 7384 0076 9968     		ldr	r1, [r3, #8]
 7385 0078 0291     		str	r1, [sp, #8]
ARM GAS  /tmp/cc5SiBtg.s 			page 248


3562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7386              		.loc 1 3562 3 view .LVU2490
 7387 007a 0299     		ldr	r1, [sp, #8]
 7388              	.LBE13:
3562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7389              		.loc 1 3562 3 view .LVU2491
3563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7390              		.loc 1 3563 3 view .LVU2492
 7391              	.LBB14:
3563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7392              		.loc 1 3563 3 view .LVU2493
 7393 007c 0392     		str	r2, [sp, #12]
3563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7394              		.loc 1 3563 3 view .LVU2494
 7395 007e 9B68     		ldr	r3, [r3, #8]
 7396 0080 0393     		str	r3, [sp, #12]
3563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7397              		.loc 1 3563 3 view .LVU2495
 7398 0082 039B     		ldr	r3, [sp, #12]
 7399              	.LBE14:
3563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7400              		.loc 1 3563 3 view .LVU2496
3566:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7401              		.loc 1 3566 3 view .LVU2497
3566:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7402              		.loc 1 3566 16 is_stmt 0 view .LVU2498
 7403 0084 0123     		movs	r3, #1
 7404 0086 84F85D30 		strb	r3, [r4, #93]
3572:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 7405              		.loc 1 3572 3 is_stmt 1 view .LVU2499
 7406 008a 2046     		mov	r0, r4
 7407 008c FFF7FEFF 		bl	HAL_SPI_AbortCpltCallback
 7408              	.LVL462:
 7409              	.L493:
3574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7410              		.loc 1 3574 1 is_stmt 0 view .LVU2500
 7411 0090 05B0     		add	sp, sp, #20
 7412              		.cfi_def_cfa_offset 12
 7413              		@ sp needed
 7414 0092 30BD     		pop	{r4, r5, pc}
3574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7415              		.loc 1 3574 1 view .LVU2501
 7416              		.cfi_endproc
 7417              	.LFE161:
 7419              		.section	.text.SPI_DMATxAbortCallback,"ax",%progbits
 7420              		.align	1
 7421              		.syntax unified
 7422              		.thumb
 7423              		.thumb_func
 7425              	SPI_DMATxAbortCallback:
 7426              	.LVL463:
 7427              	.LFB160:
3452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 7428              		.loc 1 3452 1 is_stmt 1 view -0
 7429              		.cfi_startproc
 7430              		@ args = 0, pretend = 0, frame = 8
 7431              		@ frame_needed = 0, uses_anonymous_args = 0
ARM GAS  /tmp/cc5SiBtg.s 			page 249


3452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 7432              		.loc 1 3452 1 is_stmt 0 view .LVU2503
 7433 0000 10B5     		push	{r4, lr}
 7434              		.cfi_def_cfa_offset 8
 7435              		.cfi_offset 4, -8
 7436              		.cfi_offset 14, -4
 7437 0002 84B0     		sub	sp, sp, #16
 7438              		.cfi_def_cfa_offset 24
3453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7439              		.loc 1 3453 3 is_stmt 1 view .LVU2504
3453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7440              		.loc 1 3453 22 is_stmt 0 view .LVU2505
 7441 0004 446A     		ldr	r4, [r0, #36]
 7442              	.LVL464:
3455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7443              		.loc 1 3455 3 is_stmt 1 view .LVU2506
3455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7444              		.loc 1 3455 7 is_stmt 0 view .LVU2507
 7445 0006 636D     		ldr	r3, [r4, #84]
3455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7446              		.loc 1 3455 35 view .LVU2508
 7447 0008 0022     		movs	r2, #0
 7448 000a 5A63     		str	r2, [r3, #52]
3458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7449              		.loc 1 3458 3 is_stmt 1 view .LVU2509
 7450 000c 2268     		ldr	r2, [r4]
 7451 000e 5368     		ldr	r3, [r2, #4]
 7452 0010 23F00203 		bic	r3, r3, #2
 7453 0014 5360     		str	r3, [r2, #4]
3460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7454              		.loc 1 3460 3 view .LVU2510
3460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7455              		.loc 1 3460 7 is_stmt 0 view .LVU2511
 7456 0016 FFF7FEFF 		bl	HAL_GetTick
 7457              	.LVL465:
3460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7458              		.loc 1 3460 7 view .LVU2512
 7459 001a 0246     		mov	r2, r0
3460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7460              		.loc 1 3460 7 discriminator 1 view .LVU2513
 7461 001c 6421     		movs	r1, #100
 7462 001e 2046     		mov	r0, r4
 7463 0020 FFF7FEFF 		bl	SPI_EndRxTxTransaction
 7464              	.LVL466:
3460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7465              		.loc 1 3460 6 discriminator 2 view .LVU2514
 7466 0024 08B1     		cbz	r0, .L501
3462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7467              		.loc 1 3462 5 is_stmt 1 view .LVU2515
3462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7468              		.loc 1 3462 21 is_stmt 0 view .LVU2516
 7469 0026 4023     		movs	r3, #64
 7470 0028 2366     		str	r3, [r4, #96]
 7471              	.L501:
3466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7472              		.loc 1 3466 3 is_stmt 1 view .LVU2517
 7473 002a 2268     		ldr	r2, [r4]
ARM GAS  /tmp/cc5SiBtg.s 			page 250


 7474 002c 1368     		ldr	r3, [r2]
 7475 002e 23F04003 		bic	r3, r3, #64
 7476 0032 1360     		str	r3, [r2]
3469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7477              		.loc 1 3469 3 view .LVU2518
3469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7478              		.loc 1 3469 7 is_stmt 0 view .LVU2519
 7479 0034 FFF7FEFF 		bl	HAL_GetTick
 7480              	.LVL467:
3469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7481              		.loc 1 3469 7 discriminator 1 view .LVU2520
 7482 0038 0090     		str	r0, [sp]
 7483 003a 6423     		movs	r3, #100
 7484 003c 0022     		movs	r2, #0
 7485 003e 4FF4C061 		mov	r1, #1536
 7486 0042 2046     		mov	r0, r4
 7487 0044 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 7488              	.LVL468:
3469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7489              		.loc 1 3469 6 discriminator 2 view .LVU2521
 7490 0048 08B1     		cbz	r0, .L502
3471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7491              		.loc 1 3471 5 is_stmt 1 view .LVU2522
3471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7492              		.loc 1 3471 21 is_stmt 0 view .LVU2523
 7493 004a 4023     		movs	r3, #64
 7494 004c 2366     		str	r3, [r4, #96]
 7495              	.L502:
3475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7496              		.loc 1 3475 3 is_stmt 1 view .LVU2524
3475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7497              		.loc 1 3475 11 is_stmt 0 view .LVU2525
 7498 004e A36D     		ldr	r3, [r4, #88]
3475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7499              		.loc 1 3475 6 view .LVU2526
 7500 0050 0BB1     		cbz	r3, .L503
3477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7501              		.loc 1 3477 5 is_stmt 1 view .LVU2527
3477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7502              		.loc 1 3477 21 is_stmt 0 view .LVU2528
 7503 0052 5B6B     		ldr	r3, [r3, #52]
3477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7504              		.loc 1 3477 8 view .LVU2529
 7505 0054 D3B9     		cbnz	r3, .L500
 7506              	.L503:
3484:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 7507              		.loc 1 3484 3 is_stmt 1 view .LVU2530
3484:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 7508              		.loc 1 3484 21 is_stmt 0 view .LVU2531
 7509 0056 0023     		movs	r3, #0
 7510 0058 A4F84630 		strh	r3, [r4, #70]	@ movhi
3485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7511              		.loc 1 3485 3 is_stmt 1 view .LVU2532
3485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7512              		.loc 1 3485 21 is_stmt 0 view .LVU2533
 7513 005c E387     		strh	r3, [r4, #62]	@ movhi
3488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/cc5SiBtg.s 			page 251


 7514              		.loc 1 3488 3 is_stmt 1 view .LVU2534
3488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7515              		.loc 1 3488 11 is_stmt 0 view .LVU2535
 7516 005e 236E     		ldr	r3, [r4, #96]
3488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7517              		.loc 1 3488 6 view .LVU2536
 7518 0060 402B     		cmp	r3, #64
 7519 0062 01D0     		beq	.L505
3491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7520              		.loc 1 3491 5 is_stmt 1 view .LVU2537
3491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7521              		.loc 1 3491 21 is_stmt 0 view .LVU2538
 7522 0064 0023     		movs	r3, #0
 7523 0066 2366     		str	r3, [r4, #96]
 7524              	.L505:
3495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7525              		.loc 1 3495 3 is_stmt 1 view .LVU2539
 7526              	.LBB15:
3495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7527              		.loc 1 3495 3 view .LVU2540
 7528 0068 0022     		movs	r2, #0
 7529 006a 0292     		str	r2, [sp, #8]
3495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7530              		.loc 1 3495 3 view .LVU2541
 7531 006c 2368     		ldr	r3, [r4]
 7532 006e D968     		ldr	r1, [r3, #12]
 7533 0070 0291     		str	r1, [sp, #8]
3495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7534              		.loc 1 3495 3 view .LVU2542
 7535 0072 9968     		ldr	r1, [r3, #8]
 7536 0074 0291     		str	r1, [sp, #8]
3495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7537              		.loc 1 3495 3 view .LVU2543
 7538 0076 0299     		ldr	r1, [sp, #8]
 7539              	.LBE15:
3495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7540              		.loc 1 3495 3 view .LVU2544
3496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7541              		.loc 1 3496 3 view .LVU2545
 7542              	.LBB16:
3496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7543              		.loc 1 3496 3 view .LVU2546
 7544 0078 0392     		str	r2, [sp, #12]
3496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7545              		.loc 1 3496 3 view .LVU2547
 7546 007a 9B68     		ldr	r3, [r3, #8]
 7547 007c 0393     		str	r3, [sp, #12]
3496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7548              		.loc 1 3496 3 view .LVU2548
 7549 007e 039B     		ldr	r3, [sp, #12]
 7550              	.LBE16:
3496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7551              		.loc 1 3496 3 view .LVU2549
3499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7552              		.loc 1 3499 3 view .LVU2550
3499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7553              		.loc 1 3499 16 is_stmt 0 view .LVU2551
ARM GAS  /tmp/cc5SiBtg.s 			page 252


 7554 0080 0123     		movs	r3, #1
 7555 0082 84F85D30 		strb	r3, [r4, #93]
3505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 7556              		.loc 1 3505 3 is_stmt 1 view .LVU2552
 7557 0086 2046     		mov	r0, r4
 7558 0088 FFF7FEFF 		bl	HAL_SPI_AbortCpltCallback
 7559              	.LVL469:
 7560              	.L500:
3507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7561              		.loc 1 3507 1 is_stmt 0 view .LVU2553
 7562 008c 04B0     		add	sp, sp, #16
 7563              		.cfi_def_cfa_offset 8
 7564              		@ sp needed
 7565 008e 10BD     		pop	{r4, pc}
3507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7566              		.loc 1 3507 1 view .LVU2554
 7567              		.cfi_endproc
 7568              	.LFE160:
 7570              		.section	.text.HAL_SPI_GetState,"ax",%progbits
 7571              		.align	1
 7572              		.global	HAL_SPI_GetState
 7573              		.syntax unified
 7574              		.thumb
 7575              		.thumb_func
 7577              	HAL_SPI_GetState:
 7578              	.LVL470:
 7579              	.LFB150:
3042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Return SPI handle state */
 7580              		.loc 1 3042 1 is_stmt 1 view -0
 7581              		.cfi_startproc
 7582              		@ args = 0, pretend = 0, frame = 0
 7583              		@ frame_needed = 0, uses_anonymous_args = 0
 7584              		@ link register save eliminated.
3044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 7585              		.loc 1 3044 3 view .LVU2556
3044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 7586              		.loc 1 3044 14 is_stmt 0 view .LVU2557
 7587 0000 90F85D00 		ldrb	r0, [r0, #93]	@ zero_extendqisi2
 7588              	.LVL471:
3045:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7589              		.loc 1 3045 1 view .LVU2558
 7590 0004 7047     		bx	lr
 7591              		.cfi_endproc
 7592              	.LFE150:
 7594              		.section	.text.HAL_SPI_GetError,"ax",%progbits
 7595              		.align	1
 7596              		.global	HAL_SPI_GetError
 7597              		.syntax unified
 7598              		.thumb
 7599              		.thumb_func
 7601              	HAL_SPI_GetError:
 7602              	.LVL472:
 7603              	.LFB151:
3054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Return SPI ErrorCode */
 7604              		.loc 1 3054 1 is_stmt 1 view -0
 7605              		.cfi_startproc
 7606              		@ args = 0, pretend = 0, frame = 0
ARM GAS  /tmp/cc5SiBtg.s 			page 253


 7607              		@ frame_needed = 0, uses_anonymous_args = 0
 7608              		@ link register save eliminated.
3056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 7609              		.loc 1 3056 3 view .LVU2560
3056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 7610              		.loc 1 3056 14 is_stmt 0 view .LVU2561
 7611 0000 006E     		ldr	r0, [r0, #96]
 7612              	.LVL473:
3057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7613              		.loc 1 3057 1 view .LVU2562
 7614 0002 7047     		bx	lr
 7615              		.cfi_endproc
 7616              	.LFE151:
 7618              		.text
 7619              	.Letext0:
 7620              		.file 2 "/home/chiangni/.config/Code/User/globalStorage/bmd.stm32-for-vscode/@xpack-dev-tools/arm-
 7621              		.file 3 "/home/chiangni/.config/Code/User/globalStorage/bmd.stm32-for-vscode/@xpack-dev-tools/arm-
 7622              		.file 4 "Drivers/CMSIS/Device/ST/STM32F3xx/Include/stm32f302x8.h"
 7623              		.file 5 "Drivers/CMSIS/Device/ST/STM32F3xx/Include/stm32f3xx.h"
 7624              		.file 6 "Drivers/STM32F3xx_HAL_Driver/Inc/stm32f3xx_hal_def.h"
 7625              		.file 7 "Drivers/STM32F3xx_HAL_Driver/Inc/stm32f3xx_hal_dma.h"
 7626              		.file 8 "Drivers/STM32F3xx_HAL_Driver/Inc/stm32f3xx_hal_spi.h"
 7627              		.file 9 "Drivers/CMSIS/Device/ST/STM32F3xx/Include/system_stm32f3xx.h"
 7628              		.file 10 "Drivers/STM32F3xx_HAL_Driver/Inc/stm32f3xx_hal.h"
ARM GAS  /tmp/cc5SiBtg.s 			page 254


DEFINED SYMBOLS
                            *ABS*:00000000 stm32f3xx_hal_spi.c
     /tmp/cc5SiBtg.s:21     .text.SPI_WaitFlagStateUntilTimeout:00000000 $t
     /tmp/cc5SiBtg.s:26     .text.SPI_WaitFlagStateUntilTimeout:00000000 SPI_WaitFlagStateUntilTimeout
     /tmp/cc5SiBtg.s:200    .text.SPI_WaitFlagStateUntilTimeout:000000c4 $d
     /tmp/cc5SiBtg.s:205    .text.SPI_WaitFifoStateUntilTimeout:00000000 $t
     /tmp/cc5SiBtg.s:210    .text.SPI_WaitFifoStateUntilTimeout:00000000 SPI_WaitFifoStateUntilTimeout
     /tmp/cc5SiBtg.s:415    .text.SPI_WaitFifoStateUntilTimeout:000000ec $d
     /tmp/cc5SiBtg.s:420    .text.SPI_EndRxTxTransaction:00000000 $t
     /tmp/cc5SiBtg.s:425    .text.SPI_EndRxTxTransaction:00000000 SPI_EndRxTxTransaction
     /tmp/cc5SiBtg.s:518    .text.SPI_EndRxTransaction:00000000 $t
     /tmp/cc5SiBtg.s:523    .text.SPI_EndRxTransaction:00000000 SPI_EndRxTransaction
     /tmp/cc5SiBtg.s:642    .text.SPI_AbortRx_ISR:00000000 $t
     /tmp/cc5SiBtg.s:647    .text.SPI_AbortRx_ISR:00000000 SPI_AbortRx_ISR
     /tmp/cc5SiBtg.s:762    .text.SPI_AbortRx_ISR:00000088 $d
     /tmp/cc5SiBtg.s:768    .text.SPI_AbortTx_ISR:00000000 $t
     /tmp/cc5SiBtg.s:773    .text.SPI_AbortTx_ISR:00000000 SPI_AbortTx_ISR
     /tmp/cc5SiBtg.s:961    .text.SPI_AbortTx_ISR:000000e8 $d
     /tmp/cc5SiBtg.s:967    .text.HAL_SPI_MspInit:00000000 $t
     /tmp/cc5SiBtg.s:973    .text.HAL_SPI_MspInit:00000000 HAL_SPI_MspInit
     /tmp/cc5SiBtg.s:988    .text.HAL_SPI_Init:00000000 $t
     /tmp/cc5SiBtg.s:994    .text.HAL_SPI_Init:00000000 HAL_SPI_Init
     /tmp/cc5SiBtg.s:1181   .text.HAL_SPI_MspDeInit:00000000 $t
     /tmp/cc5SiBtg.s:1187   .text.HAL_SPI_MspDeInit:00000000 HAL_SPI_MspDeInit
     /tmp/cc5SiBtg.s:1202   .text.HAL_SPI_DeInit:00000000 $t
     /tmp/cc5SiBtg.s:1208   .text.HAL_SPI_DeInit:00000000 HAL_SPI_DeInit
     /tmp/cc5SiBtg.s:1265   .text.HAL_SPI_Transmit:00000000 $t
     /tmp/cc5SiBtg.s:1271   .text.HAL_SPI_Transmit:00000000 HAL_SPI_Transmit
     /tmp/cc5SiBtg.s:1743   .text.HAL_SPI_TransmitReceive:00000000 $t
     /tmp/cc5SiBtg.s:1749   .text.HAL_SPI_TransmitReceive:00000000 HAL_SPI_TransmitReceive
     /tmp/cc5SiBtg.s:2475   .text.HAL_SPI_Receive:00000000 $t
     /tmp/cc5SiBtg.s:2481   .text.HAL_SPI_Receive:00000000 HAL_SPI_Receive
     /tmp/cc5SiBtg.s:2849   .text.HAL_SPI_Transmit_IT:00000000 $t
     /tmp/cc5SiBtg.s:2855   .text.HAL_SPI_Transmit_IT:00000000 HAL_SPI_Transmit_IT
     /tmp/cc5SiBtg.s:3033   .text.HAL_SPI_Transmit_IT:000000a8 $d
     /tmp/cc5SiBtg.s:5491   .text.SPI_TxISR_16BIT:00000000 SPI_TxISR_16BIT
     /tmp/cc5SiBtg.s:5430   .text.SPI_TxISR_8BIT:00000000 SPI_TxISR_8BIT
     /tmp/cc5SiBtg.s:3039   .text.HAL_SPI_TransmitReceive_IT:00000000 $t
     /tmp/cc5SiBtg.s:3045   .text.HAL_SPI_TransmitReceive_IT:00000000 HAL_SPI_TransmitReceive_IT
     /tmp/cc5SiBtg.s:3286   .text.HAL_SPI_TransmitReceive_IT:000000e4 $d
     /tmp/cc5SiBtg.s:6132   .text.SPI_2linesRxISR_16BIT:00000000 SPI_2linesRxISR_16BIT
     /tmp/cc5SiBtg.s:6060   .text.SPI_2linesTxISR_16BIT:00000000 SPI_2linesTxISR_16BIT
     /tmp/cc5SiBtg.s:5943   .text.SPI_2linesRxISR_8BIT:00000000 SPI_2linesRxISR_8BIT
     /tmp/cc5SiBtg.s:5838   .text.SPI_2linesTxISR_8BIT:00000000 SPI_2linesTxISR_8BIT
     /tmp/cc5SiBtg.s:3294   .text.HAL_SPI_Receive_IT:00000000 $t
     /tmp/cc5SiBtg.s:3300   .text.HAL_SPI_Receive_IT:00000000 HAL_SPI_Receive_IT
     /tmp/cc5SiBtg.s:3499   .text.HAL_SPI_Receive_IT:000000f4 $d
     /tmp/cc5SiBtg.s:5682   .text.SPI_RxISR_16BIT:00000000 SPI_RxISR_16BIT
     /tmp/cc5SiBtg.s:5621   .text.SPI_RxISR_8BIT:00000000 SPI_RxISR_8BIT
     /tmp/cc5SiBtg.s:3505   .text.HAL_SPI_Transmit_DMA:00000000 $t
     /tmp/cc5SiBtg.s:3511   .text.HAL_SPI_Transmit_DMA:00000000 HAL_SPI_Transmit_DMA
     /tmp/cc5SiBtg.s:3767   .text.HAL_SPI_Transmit_DMA:00000124 $d
     /tmp/cc5SiBtg.s:5172   .text.SPI_DMAHalfTransmitCplt:00000000 SPI_DMAHalfTransmitCplt
     /tmp/cc5SiBtg.s:6247   .text.SPI_DMATransmitCplt:00000000 SPI_DMATransmitCplt
     /tmp/cc5SiBtg.s:6204   .text.SPI_DMAError:00000000 SPI_DMAError
     /tmp/cc5SiBtg.s:3774   .text.HAL_SPI_TransmitReceive_DMA:00000000 $t
     /tmp/cc5SiBtg.s:3780   .text.HAL_SPI_TransmitReceive_DMA:00000000 HAL_SPI_TransmitReceive_DMA
ARM GAS  /tmp/cc5SiBtg.s 			page 255


     /tmp/cc5SiBtg.s:4219   .text.HAL_SPI_TransmitReceive_DMA:000001f8 $d
     /tmp/cc5SiBtg.s:5276   .text.SPI_DMAHalfTransmitReceiveCplt:00000000 SPI_DMAHalfTransmitReceiveCplt
     /tmp/cc5SiBtg.s:6486   .text.SPI_DMATransmitReceiveCplt:00000000 SPI_DMATransmitReceiveCplt
     /tmp/cc5SiBtg.s:5224   .text.SPI_DMAHalfReceiveCplt:00000000 SPI_DMAHalfReceiveCplt
     /tmp/cc5SiBtg.s:6370   .text.SPI_DMAReceiveCplt:00000000 SPI_DMAReceiveCplt
     /tmp/cc5SiBtg.s:4228   .text.HAL_SPI_Receive_DMA:00000000 $t
     /tmp/cc5SiBtg.s:4234   .text.HAL_SPI_Receive_DMA:00000000 HAL_SPI_Receive_DMA
     /tmp/cc5SiBtg.s:4528   .text.HAL_SPI_Receive_DMA:00000170 $d
     /tmp/cc5SiBtg.s:4535   .text.HAL_SPI_Abort:00000000 $t
     /tmp/cc5SiBtg.s:4541   .text.HAL_SPI_Abort:00000000 HAL_SPI_Abort
     /tmp/cc5SiBtg.s:4885   .text.HAL_SPI_Abort:00000180 $d
     /tmp/cc5SiBtg.s:4893   .text.HAL_SPI_DMAPause:00000000 $t
     /tmp/cc5SiBtg.s:4899   .text.HAL_SPI_DMAPause:00000000 HAL_SPI_DMAPause
     /tmp/cc5SiBtg.s:4943   .text.HAL_SPI_DMAResume:00000000 $t
     /tmp/cc5SiBtg.s:4949   .text.HAL_SPI_DMAResume:00000000 HAL_SPI_DMAResume
     /tmp/cc5SiBtg.s:4993   .text.HAL_SPI_DMAStop:00000000 $t
     /tmp/cc5SiBtg.s:4999   .text.HAL_SPI_DMAStop:00000000 HAL_SPI_DMAStop
     /tmp/cc5SiBtg.s:5083   .text.HAL_SPI_TxCpltCallback:00000000 $t
     /tmp/cc5SiBtg.s:5089   .text.HAL_SPI_TxCpltCallback:00000000 HAL_SPI_TxCpltCallback
     /tmp/cc5SiBtg.s:5104   .text.HAL_SPI_RxCpltCallback:00000000 $t
     /tmp/cc5SiBtg.s:5110   .text.HAL_SPI_RxCpltCallback:00000000 HAL_SPI_RxCpltCallback
     /tmp/cc5SiBtg.s:5125   .text.HAL_SPI_TxRxCpltCallback:00000000 $t
     /tmp/cc5SiBtg.s:5131   .text.HAL_SPI_TxRxCpltCallback:00000000 HAL_SPI_TxRxCpltCallback
     /tmp/cc5SiBtg.s:5146   .text.HAL_SPI_TxHalfCpltCallback:00000000 $t
     /tmp/cc5SiBtg.s:5152   .text.HAL_SPI_TxHalfCpltCallback:00000000 HAL_SPI_TxHalfCpltCallback
     /tmp/cc5SiBtg.s:5167   .text.SPI_DMAHalfTransmitCplt:00000000 $t
     /tmp/cc5SiBtg.s:5198   .text.HAL_SPI_RxHalfCpltCallback:00000000 $t
     /tmp/cc5SiBtg.s:5204   .text.HAL_SPI_RxHalfCpltCallback:00000000 HAL_SPI_RxHalfCpltCallback
     /tmp/cc5SiBtg.s:5219   .text.SPI_DMAHalfReceiveCplt:00000000 $t
     /tmp/cc5SiBtg.s:5250   .text.HAL_SPI_TxRxHalfCpltCallback:00000000 $t
     /tmp/cc5SiBtg.s:5256   .text.HAL_SPI_TxRxHalfCpltCallback:00000000 HAL_SPI_TxRxHalfCpltCallback
     /tmp/cc5SiBtg.s:5271   .text.SPI_DMAHalfTransmitReceiveCplt:00000000 $t
     /tmp/cc5SiBtg.s:5302   .text.HAL_SPI_ErrorCallback:00000000 $t
     /tmp/cc5SiBtg.s:5308   .text.HAL_SPI_ErrorCallback:00000000 HAL_SPI_ErrorCallback
     /tmp/cc5SiBtg.s:5323   .text.SPI_CloseTx_ISR:00000000 $t
     /tmp/cc5SiBtg.s:5328   .text.SPI_CloseTx_ISR:00000000 SPI_CloseTx_ISR
     /tmp/cc5SiBtg.s:5425   .text.SPI_TxISR_8BIT:00000000 $t
     /tmp/cc5SiBtg.s:5486   .text.SPI_TxISR_16BIT:00000000 $t
     /tmp/cc5SiBtg.s:5547   .text.SPI_CloseRx_ISR:00000000 $t
     /tmp/cc5SiBtg.s:5552   .text.SPI_CloseRx_ISR:00000000 SPI_CloseRx_ISR
     /tmp/cc5SiBtg.s:5616   .text.SPI_RxISR_8BIT:00000000 $t
     /tmp/cc5SiBtg.s:5677   .text.SPI_RxISR_16BIT:00000000 $t
     /tmp/cc5SiBtg.s:5738   .text.SPI_CloseRxTx_ISR:00000000 $t
     /tmp/cc5SiBtg.s:5743   .text.SPI_CloseRxTx_ISR:00000000 SPI_CloseRxTx_ISR
     /tmp/cc5SiBtg.s:5833   .text.SPI_2linesTxISR_8BIT:00000000 $t
     /tmp/cc5SiBtg.s:5938   .text.SPI_2linesRxISR_8BIT:00000000 $t
     /tmp/cc5SiBtg.s:6055   .text.SPI_2linesTxISR_16BIT:00000000 $t
     /tmp/cc5SiBtg.s:6127   .text.SPI_2linesRxISR_16BIT:00000000 $t
     /tmp/cc5SiBtg.s:6199   .text.SPI_DMAError:00000000 $t
     /tmp/cc5SiBtg.s:6242   .text.SPI_DMATransmitCplt:00000000 $t
     /tmp/cc5SiBtg.s:6365   .text.SPI_DMAReceiveCplt:00000000 $t
     /tmp/cc5SiBtg.s:6481   .text.SPI_DMATransmitReceiveCplt:00000000 $t
     /tmp/cc5SiBtg.s:6580   .text.HAL_SPI_IRQHandler:00000000 $t
     /tmp/cc5SiBtg.s:6586   .text.HAL_SPI_IRQHandler:00000000 HAL_SPI_IRQHandler
     /tmp/cc5SiBtg.s:6855   .text.HAL_SPI_IRQHandler:00000120 $d
     /tmp/cc5SiBtg.s:6865   .text.SPI_DMAAbortOnError:00000000 SPI_DMAAbortOnError
     /tmp/cc5SiBtg.s:6860   .text.SPI_DMAAbortOnError:00000000 $t
ARM GAS  /tmp/cc5SiBtg.s 			page 256


     /tmp/cc5SiBtg.s:6897   .text.HAL_SPI_AbortCpltCallback:00000000 $t
     /tmp/cc5SiBtg.s:6903   .text.HAL_SPI_AbortCpltCallback:00000000 HAL_SPI_AbortCpltCallback
     /tmp/cc5SiBtg.s:6918   .text.HAL_SPI_Abort_IT:00000000 $t
     /tmp/cc5SiBtg.s:6924   .text.HAL_SPI_Abort_IT:00000000 HAL_SPI_Abort_IT
     /tmp/cc5SiBtg.s:7257   .text.HAL_SPI_Abort_IT:00000148 $d
     /tmp/cc5SiBtg.s:7425   .text.SPI_DMATxAbortCallback:00000000 SPI_DMATxAbortCallback
     /tmp/cc5SiBtg.s:7272   .text.SPI_DMARxAbortCallback:00000000 SPI_DMARxAbortCallback
     /tmp/cc5SiBtg.s:7267   .text.SPI_DMARxAbortCallback:00000000 $t
     /tmp/cc5SiBtg.s:7420   .text.SPI_DMATxAbortCallback:00000000 $t
     /tmp/cc5SiBtg.s:7571   .text.HAL_SPI_GetState:00000000 $t
     /tmp/cc5SiBtg.s:7577   .text.HAL_SPI_GetState:00000000 HAL_SPI_GetState
     /tmp/cc5SiBtg.s:7595   .text.HAL_SPI_GetError:00000000 $t
     /tmp/cc5SiBtg.s:7601   .text.HAL_SPI_GetError:00000000 HAL_SPI_GetError

UNDEFINED SYMBOLS
HAL_GetTick
SystemCoreClock
HAL_DMA_Start_IT
HAL_DMA_Abort
HAL_DMA_Abort_IT
