(module Micro-Mate-N-Lok-16pin-2row (layer F.Cu) (tedit 5D12244A)
  (fp_text reference REF** (at 0 -5.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Micro-Mate-N-Lok-16pin-2row (at 0 10.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 13.5 0) (end 13.5 9) (layer F.CrtYd) (width 0.15))
  (fp_line (start -13.5 0) (end -13.5 9) (layer F.CrtYd) (width 0.15))
  (fp_line (start -13.5 9) (end 13.5 9) (layer F.CrtYd) (width 0.15))
  (fp_line (start -13.5 0) (end -13.5 -4) (layer F.CrtYd) (width 0.15))
  (fp_line (start -13.5 -4) (end 13.5 -4) (layer F.CrtYd) (width 0.15))
  (fp_line (start 13.5 -4) (end 13.5 0.2) (layer F.CrtYd) (width 0.15))
  (fp_line (start -13.7 0.4) (end -13.7 -4.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -13.7 -4.2) (end 13.7 -4.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 13.7 -4.2) (end 13.7 0.4) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at -10.5 0) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -7.5 0) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -4.5 0) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -1.5 0) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 1.5 0) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 4.5 0) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 7.5 0) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 10.5 0) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 10.5 -3) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 7.5 -3) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 4.5 -3) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 1.5 -3) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at -1.5 -3) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at -4.5 -3) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at -7.5 -3) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at -10.5 -3) (size 1.8 1.8) (drill 1.02) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -8.34 4.32) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 8.34 4.32) (size 3 3) (drill 3) (layers *.Cu *.Mask))
)
