(footprint "M8_718_4pin_vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 8 0)
		(layer "F.SilkS")
		(uuid "b680b4a7-6cb0-40b5-a7ec-a02910a0daa4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "M8_718_4pin"
		(at 0 -7.62 0)
		(layer "F.Fab")
		(uuid "c5a1761e-3391-4e74-90c9-947fd66e1fc6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "dcaf2f58-7535-4c16-a965-c0b08929320b")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "23c79916-6723-4a1f-a564-a37aa3cd420c")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "967d72d7-8798-4823-a439-fc04a483d4ab")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr through_hole)
	(fp_arc
		(start -6 -2.5)
		(mid 0 -6.5)
		(end 6 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b287f145-851e-45cc-b200-e62677b551d5")
	)
	(fp_arc
		(start 6 2.5)
		(mid 0 6.5)
		(end -6 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a7f25f41-0b4c-4430-b6cd-b2160b2db099")
	)
	(fp_circle
		(center 0 0)
		(end 8.5 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "422b10b9-e829-44a2-8808-05edd8cb3050")
	)
	(pad "1" thru_hole circle
		(at 1.7 0.5)
		(size 1.8 1.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a1c7b1f5-f895-4192-9484-2357882c73e0")
	)
	(pad "2" thru_hole circle
		(at 1.075 -1.45)
		(size 1.8 1.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "681bd495-c396-44ce-92bd-4b397cd48c04")
	)
	(pad "3" thru_hole circle
		(at -1.7 0.5)
		(size 1.8 1.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "be0953c0-632d-4dd2-85e9-4d41239f22d2")
	)
	(pad "4" thru_hole circle
		(at -1.075 -1.45)
		(size 1.8 1.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a3668681-09b1-48f0-a7b1-f6b24183a469")
	)
	(pad "5" thru_hole circle
		(at -6.25 0)
		(size 4 4)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "563c12e4-8f8c-446c-a11f-94f5aa93b994")
	)
	(pad "5" thru_hole circle
		(at 6.25 0)
		(size 4 4)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3451168c-3c76-4628-aee4-7c231bd100c3")
	)
	(model "${KIPRJMOD}/Symbol_Libraries/FaSTTUBe_connectors_3dmodels/M8_718_4pin_vertical.stp"
		(offset
			(xyz 0 0 0.6)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 90 90)
		)
	)
)