(footprint "TLE9351VSJ" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 62937963)
  (descr "Infineon  PG-DSO, 8 Pin (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-8-27), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "Infineon PG-DSO SO")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.4) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b10a9f8e-4d37-49e3-bac3-1deccafc7947)
  )
  (fp_text value "TLE9351VSJ" (at 0 3.4) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d5ee8780-f4a2-4e2a-824b-168ad13f2b6c)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 0.98 0.98) (thickness 0.15)))
    (tstamp b4ce4a40-f81c-4359-8803-a908455e31b3)
  )
  (fp_line (start 0 -2.56) (end 1.95 -2.56) (layer "F.SilkS") (width 0.12) (tstamp 11478247-3a4b-40d3-a911-168f22a0a39a))
  (fp_line (start 0 2.56) (end 1.95 2.56) (layer "F.SilkS") (width 0.12) (tstamp 19956d14-44ae-480b-89a2-5e629f4fc78e))
  (fp_line (start 0 -2.56) (end -3.45 -2.56) (layer "F.SilkS") (width 0.12) (tstamp c1f45fe7-e68e-4696-ac8f-4ad8f8605d26))
  (fp_line (start 0 2.56) (end -1.95 2.56) (layer "F.SilkS") (width 0.12) (tstamp c7092ce6-f184-4d5a-9860-06bdb325a74f))
  (fp_line (start 3.7 -2.7) (end -3.7 -2.7) (layer "F.CrtYd") (width 0.05) (tstamp 2048a23e-ab49-452b-b97d-db688cf35538))
  (fp_line (start 3.7 2.7) (end 3.7 -2.7) (layer "F.CrtYd") (width 0.05) (tstamp 843f92e2-bc29-4f1a-af3e-35ee54979cd5))
  (fp_line (start -3.7 -2.7) (end -3.7 2.7) (layer "F.CrtYd") (width 0.05) (tstamp ee0a7447-2bcf-4418-9a35-aea3cf6a1ac6))
  (fp_line (start -3.7 2.7) (end 3.7 2.7) (layer "F.CrtYd") (width 0.05) (tstamp f03795ac-b5db-4d67-91b2-e01efbb34e9b))
  (fp_line (start -1.95 -1.475) (end -0.975 -2.45) (layer "F.Fab") (width 0.1) (tstamp 3a8228ac-1433-4309-8e9f-4c8c0684d7d3))
  (fp_line (start -0.975 -2.45) (end 1.95 -2.45) (layer "F.Fab") (width 0.1) (tstamp 4b4fd3db-6628-44f5-a94d-aa7c5b13124a))
  (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer "F.Fab") (width 0.1) (tstamp 500ef03c-b1de-483a-85d9-3c094cecdc30))
  (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer "F.Fab") (width 0.1) (tstamp 62b6f3f6-f696-4e9e-b2bf-919a94efdbb1))
  (fp_line (start -1.95 2.45) (end -1.95 -1.475) (layer "F.Fab") (width 0.1) (tstamp f317e77d-64f6-4d2c-bcaf-81640935b145))
  (pad "1" smd roundrect (at -2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6571004b-fdf6-4e0a-91bc-2f03fd12b368))
  (pad "2" smd roundrect (at -2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b09dc2b9-2a48-4ca6-8464-507885d9750c))
  (pad "3" smd roundrect (at -2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b00bdeab-3b3c-4748-b9b0-8b8ea2b3b599))
  (pad "4" smd roundrect (at -2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 08ff838c-8130-4b86-9d11-08c1de7a1d5f))
  (pad "5" smd roundrect (at 2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 14f24796-5e73-4eec-8563-70846dccba31))
  (pad "6" smd roundrect (at 2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 19fa85a8-376f-4b86-a1a9-cd5914c65cf3))
  (pad "7" smd roundrect (at 2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4e773bb7-c138-4e80-8fca-56cd272e592e))
  (pad "8" smd roundrect (at 2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1f19a878-e119-4556-93b4-e0038c8f9448))
  (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/Infineon_PG-DSO-8-27_3.9x4.9mm_EP2.65x3mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
