(footprint "sumida"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0.5 0)
		(layer "F.SilkS")
		(uuid "b06ce446-c27e-47df-a4e3-d10b64552c26")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "sumida"
		(at 0 -0.5 0)
		(layer "F.Fab")
		(uuid "c9a0dd18-d945-4bfe-8921-ced29a4068d2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "sumida"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bb74db9a-3292-4844-b187-43e3b72a5a70")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "123593b4-be29-423a-ae1c-04a3be1b995d")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d71b9ca2-53f9-4bfd-a6af-fa348cd771f4")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -8.5 -9.5)
		(end 8.5 9.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "ef3c006a-93b2-4c16-9912-3eea1a3493b5")
	)
	(pad "1" thru_hole circle
		(at -6.54 7.62)
		(size 1.524 1.524)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a1c7b1f5-f895-4192-9484-2357882c73e0")
	)
	(pad "3" thru_hole circle
		(at -2.54 7.62)
		(size 1.524 1.524)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e149e0b1-47fa-4b20-b36e-2d51ee1e85c3")
	)
	(pad "4" thru_hole circle
		(at 2.54 7.62)
		(size 1.524 1.524)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "81c041f3-483e-477d-9475-d108280de2a9")
	)
	(pad "5" thru_hole circle
		(at 4.54 7.62)
		(size 1.524 1.524)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5994a946-119f-4db4-aafe-00ae73b5b800")
	)
	(pad "6" thru_hole circle
		(at 6.54 7.62)
		(size 1.524 1.524)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b680b4a7-6cb0-40b5-a7ec-a02910a0daa4")
	)
	(pad "7" thru_hole circle
		(at 6.54 -7.62)
		(size 1.524 1.524)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "eaef1172-3351-417c-bfc4-74a598f141cb")
	)
	(pad "8" thru_hole circle
		(at 4.54 -7.62)
		(size 1.524 1.524)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "08e2d62f-f99a-4268-8b33-617dfcc63e75")
	)
	(pad "9" thru_hole circle
		(at 2.54 -7.62)
		(size 1.524 1.524)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "92e8f8c3-0985-4c0d-8e38-92cbbf365409")
	)
	(pad "10" thru_hole circle
		(at -2.54 -7.62)
		(size 1.524 1.524)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e68c5170-03c3-4a20-abd0-ad610c43d035")
	)
	(pad "12" thru_hole circle
		(at -6.54 -7.62)
		(size 1.524 1.524)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f6ee98b5-4773-4eeb-a825-33c1705abace")
	)
	(model "${KIPRJMOD}/Symbol_Libraries/HV_Indicator.pretty/sumida.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
