;Proteus Design Interchange Format
(PDIF
 (vendor "SamacSys Limited")
 (version 1 0)
 (library
  (part "744228"
   (description "SMD Common-Mode Line Filter WE-SL2")
   (family "IND")
   (package "WE-SL274")
   (attribute "Datasheet Link" "")
   (attribute "Mouser Part Number" "710-744228")
   (attribute "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Wurth-Elektronik/744228?qs=PGXP4M47uW4%2FEvqlverBmg%3D%3D")
   (attribute "Manufacturer_Name" "Wurth Elektronik")
   (attribute "Manufacturer_Part_Number" "744228")
   (gate
    (symbol "744228")
    (pin "1" 1 PS)
    (pin "3" 2 PS)
    (pin "4" 3 PS)
    (pin "2" 4 PS)
   )
  )
  (symbol "744228"
   (units THOU)
   (origin (pt 0 0))
   (graphic
    (stroke 10)
    (path (pt 200 100) (pt 600 100) (pt 600 -200) (pt 200 -200) (pt 200 100) (closed))
   )
   (terminal
    (body (symbol "PIN") (pt 0 0) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 0 -100) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 800 -100) (rot 0) (mir X) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 800 0) (rot 0) (mir X) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
  )
  (symbol "PIN"
   (units THOU)
   (origin (pt 0 0))
   (graphic
    (stroke 10)
    (path (pt 0 0) (pt 200 0))))
  (symbol "PINSHORT"
   (units THOU)
   (origin (pt 0 0))
   (graphic
    (stroke 10)
    (path (pt 0 0) (pt 100 0))))
  (package "WE-SL274"
   (units MM)
   (layer TASM
    (graphic
     (stroke 0.127)
     (path
      (closed false)
      (pt 3.81 -1.27)
      (pt -3.81 -1.27))))
   (layer TASM
    (graphic
     (stroke 0.127)
     (path
      (closed false)
      (pt 3.81 1.27)
      (pt -3.81 1.27))))
   (layer TASM
    (graphic
     (stroke 0.127)
     (path
      (closed false)
      (pt 4.6 -3)
      (pt 4.6 3))))
   (layer TSLK
    (graphic
     (stroke 0.127)
     (path
      (closed false)
      (pt 4.6 3)
      (pt -4.6 3))))
   (layer TASM
    (graphic
     (stroke 0.127)
     (path
      (closed false)
      (pt -4.6 3)
      (pt -4.6 -3))))
   (layer TSLK
    (graphic
     (stroke 0.127)
     (path
      (closed false)
      (pt -4.6 -3)
      (pt 4.6 -3))))
   (layer OCCA
    (graphic
     (stroke 0.127)
     (path
      (closed false)
      (pt -5 3.25)
      (pt 5 3.25))))
   (layer OCCA
    (graphic
     (stroke 0.127)
     (path
      (closed false)
      (pt 5 3.25)
      (pt 5 -3.25))))
   (layer OCCA
    (graphic
     (stroke 0.127)
     (path
      (closed false)
      (pt 5 -3.25)
      (pt -5 -3.25))))
   (layer OCCA
    (graphic
     (stroke 0.127)
     (path
      (closed false)
      (pt -5 -3.25)
      (pt -5 3.25))))
   (leg 3 (pt 3.75 -1.34) (padstack 0))
   (leg 2 (pt -3.75 -1.34) (padstack 0))
   (leg 4 (pt 3.75 1.27) (padstack 0))
   (leg 1 (pt -3.75 1.27) (padstack 0))
   (padstack 0
    (plated false)
    (pad (layer TCOP) (rectf 1.2 2 0 0 0))
   )
   (model "744228.stp"
    (euler 90 0 0)
    (offset 0 0 3.5)
   )
  )
 )
)
