ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 1


   1              		.cpu cortex-m7
   2              		.arch armv7e-m
   3              		.fpu fpv5-d16
   4              		.eabi_attribute 28, 1
   5              		.eabi_attribute 20, 1
   6              		.eabi_attribute 21, 1
   7              		.eabi_attribute 23, 3
   8              		.eabi_attribute 24, 1
   9              		.eabi_attribute 25, 1
  10              		.eabi_attribute 26, 1
  11              		.eabi_attribute 30, 1
  12              		.eabi_attribute 34, 1
  13              		.eabi_attribute 18, 4
  14              		.file	"stm32h7xx_hal_spi.c"
  15              		.text
  16              	.Ltext0:
  17              		.cfi_sections	.debug_frame
  18              		.file 1 "Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c"
  19              		.section	.text.SPI_RxISR_8BIT,"ax",%progbits
  20              		.align	1
  21              		.syntax unified
  22              		.thumb
  23              		.thumb_func
  25              	SPI_RxISR_8BIT:
  26              	.LVL0:
  27              	.LFB375:
   1:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
   2:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   ******************************************************************************
   3:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @file    stm32h7xx_hal_spi.c
   4:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @author  MCD Application Team
   5:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief   SPI HAL module driver.
   6:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *          This file provides firmware functions to manage the following
   7:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *          functionalities of the Serial Peripheral Interface (SPI) peripheral:
   8:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *           + Initialization and de-initialization functions
   9:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *           + IO operation functions
  10:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *           + Peripheral Control functions
  11:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *           + Peripheral State functions
  12:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *
  13:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   ******************************************************************************
  14:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @attention
  15:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *
  16:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * Copyright (c) 2017 STMicroelectronics.
  17:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * All rights reserved.
  18:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *
  19:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * This software is licensed under terms that can be found in the LICENSE file
  20:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * in the root directory of this software component.
  21:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * If no LICENSE file comes with this software, it is provided AS-IS.
  22:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *
  23:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   ******************************************************************************
  24:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   @verbatim
  25:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   ==============================================================================
  26:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                         ##### How to use this driver #####
  27:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   ==============================================================================
  28:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     [..]
  29:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       The SPI HAL driver can be used as follows:
  30:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
  31:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       (#) Declare a SPI_HandleTypeDef handle structure, for example:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 2


  32:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SPI_HandleTypeDef  hspi;
  33:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
  34:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       (#)Initialize the SPI low level resources by implementing the HAL_SPI_MspInit() API:
  35:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (##) Enable the SPIx interface clock
  36:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (##) SPI pins configuration
  37:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****               (+++) Enable the clock for the SPI GPIOs
  38:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****               (+++) Configure these SPI pins as alternate function push-pull
  39:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (##) NVIC configuration if you need to use interrupt process or DMA process
  40:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****               (+++) Configure the SPIx interrupt priority
  41:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****               (+++) Enable the NVIC SPI IRQ handle
  42:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (##) DMA Configuration if you need to use DMA process
  43:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****               (+++) Declare a DMA_HandleTypeDef handle structure for the transmit or receive Stream
  44:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****               (+++) Enable the DMAx clock
  45:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****               (+++) Configure the DMA handle parameters
  46:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****               (+++) Configure the DMA Tx or Rx Stream/Channel
  47:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****               (+++) Associate the initialized hdma_tx handle to the hspi DMA Tx or Rx handle
  48:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****               (+++) Configure the priority and enable the NVIC for the transfer complete interrupt 
  49:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                     or Rx Stream/Channel
  50:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
  51:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       (#) Program the Mode, BidirectionalMode , Data size, Baudrate Prescaler, NSS
  52:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           management, Clock polarity and phase, FirstBit and CRC configuration in the hspi Init str
  53:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
  54:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       (#) Initialize the SPI registers by calling the HAL_SPI_Init() API:
  55:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (++) This API configures also the low level Hardware GPIO, CLOCK, CORTEX...etc)
  56:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****               by calling the customized HAL_SPI_MspInit() API.
  57:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****      [..]
  58:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        Callback registration:
  59:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
  60:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       (#) The compilation flag USE_HAL_SPI_REGISTER_CALLBACKS when set to 1UL
  61:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           allows the user to configure dynamically the driver callbacks.
  62:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           Use Functions HAL_SPI_RegisterCallback() to register an interrupt callback.
  63:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
  64:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           Function HAL_SPI_RegisterCallback() allows to register following callbacks:
  65:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) TxCpltCallback        : SPI Tx Completed callback
  66:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) RxCpltCallback        : SPI Rx Completed callback
  67:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) TxRxCpltCallback      : SPI TxRx Completed callback
  68:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) TxHalfCpltCallback    : SPI Tx Half Completed callback
  69:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) RxHalfCpltCallback    : SPI Rx Half Completed callback
  70:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) TxRxHalfCpltCallback  : SPI TxRx Half Completed callback
  71:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) ErrorCallback         : SPI Error callback
  72:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) AbortCpltCallback     : SPI Abort callback
  73:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) SuspendCallback       : SPI Suspend callback
  74:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) MspInitCallback       : SPI Msp Init callback
  75:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) MspDeInitCallback     : SPI Msp DeInit callback
  76:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           This function takes as parameters the HAL peripheral handle, the Callback ID
  77:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           and a pointer to the user callback function.
  78:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
  79:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
  80:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       (#) Use function HAL_SPI_UnRegisterCallback to reset a callback to the default
  81:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           weak function.
  82:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           HAL_SPI_UnRegisterCallback takes as parameters the HAL peripheral handle,
  83:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           and the Callback ID.
  84:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           This function allows to reset following callbacks:
  85:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) TxCpltCallback        : SPI Tx Completed callback
  86:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) RxCpltCallback        : SPI Rx Completed callback
  87:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) TxRxCpltCallback      : SPI TxRx Completed callback
  88:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) TxHalfCpltCallback    : SPI Tx Half Completed callback
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 3


  89:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) RxHalfCpltCallback    : SPI Rx Half Completed callback
  90:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) TxRxHalfCpltCallback  : SPI TxRx Half Completed callback
  91:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) ErrorCallback         : SPI Error callback
  92:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) AbortCpltCallback     : SPI Abort callback
  93:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) SuspendCallback       : SPI Suspend callback
  94:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) MspInitCallback       : SPI Msp Init callback
  95:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             (+) MspDeInitCallback     : SPI Msp DeInit callback
  96:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
  97:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        By default, after the HAL_SPI_Init() and when the state is HAL_SPI_STATE_RESET
  98:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        all callbacks are set to the corresponding weak functions:
  99:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        examples HAL_SPI_MasterTxCpltCallback(), HAL_SPI_MasterRxCpltCallback().
 100:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        Exception done for MspInit and MspDeInit functions that are
 101:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        reset to the legacy weak functions in the HAL_SPI_Init()/ HAL_SPI_DeInit() only when
 102:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        these callbacks are null (not registered beforehand).
 103:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        If MspInit or MspDeInit are not null, the HAL_SPI_Init()/ HAL_SPI_DeInit()
 104:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        keep and use the user MspInit/MspDeInit callbacks (registered beforehand) whatever the state
 105:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 106:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        Callbacks can be registered/unregistered in HAL_SPI_STATE_READY state only.
 107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        Exception done MspInit/MspDeInit functions that can be registered/unregistered
 108:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        in HAL_SPI_STATE_READY or HAL_SPI_STATE_RESET state,
 109:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        thus registered (user) MspInit/DeInit callbacks can be used during the Init/DeInit.
 110:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        Then, the user first registers the MspInit/MspDeInit user callbacks
 111:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        using HAL_SPI_RegisterCallback() before calling HAL_SPI_DeInit()
 112:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        or HAL_SPI_Init() function.
 113:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 114:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        When The compilation define USE_HAL_PPP_REGISTER_CALLBACKS is set to 0 or not defined,
 115:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        the callback registering feature is not available and weak callbacks are used.
 116:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 117:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        SuspendCallback restriction:
 118:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****            SuspendCallback is called only when MasterReceiverAutoSusp is enabled and
 119:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        EOT interrupt is activated. SuspendCallback is used in relation with functions
 120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        HAL_SPI_Transmit_IT, HAL_SPI_Receive_IT and HAL_SPI_TransmitReceive_IT.
 121:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 122:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     [..]
 123:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       Circular mode restriction:
 124:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       (+) The DMA circular mode cannot be used when the SPI is configured in these modes:
 125:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (++) Master 2Lines RxOnly
 126:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (++) Master 1Line Rx
 127:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       (+) The CRC feature is not managed when the DMA circular mode is enabled
 128:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       (+) The functions HAL_SPI_DMAPause()/ HAL_SPI_DMAResume() are not supported. Return always
 129:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           HAL_ERROR with ErrorCode set to HAL_SPI_ERROR_NOT_SUPPORTED.
 130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           Those functions are maintained for backward compatibility reasons.
 131:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 132:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   @endverbatim
 133:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 134:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 135:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /* Includes ------------------------------------------------------------------*/
 136:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #include "stm32h7xx_hal.h"
 137:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 138:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /** @addtogroup STM32H7xx_HAL_Driver
 139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @{
 140:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 141:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 142:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /** @defgroup SPI SPI
 143:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief SPI HAL module driver
 144:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @{
 145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 4


 146:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #ifdef HAL_SPI_MODULE_ENABLED
 147:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /* Private typedef -----------------------------------------------------------*/
 149:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /* Private defines -----------------------------------------------------------*/
 150:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /** @defgroup SPI_Private_Constants SPI Private Constants
 151:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @{
 152:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 153:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #define SPI_DEFAULT_TIMEOUT 100UL
 154:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
 155:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @}
 156:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 157:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 158:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /* Private macros ------------------------------------------------------------*/
 159:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /* Private variables ---------------------------------------------------------*/
 160:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /* Private function prototypes -----------------------------------------------*/
 161:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /** @defgroup SPI_Private_Functions SPI Private Functions
 162:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @{
 163:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 164:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMATransmitCplt(DMA_HandleTypeDef *hdma);
 165:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMAReceiveCplt(DMA_HandleTypeDef *hdma);
 166:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMATransmitReceiveCplt(DMA_HandleTypeDef *hdma);
 167:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMAHalfTransmitCplt(DMA_HandleTypeDef *hdma);
 168:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMAHalfReceiveCplt(DMA_HandleTypeDef *hdma);
 169:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMAHalfTransmitReceiveCplt(DMA_HandleTypeDef *hdma);
 170:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMAError(DMA_HandleTypeDef *hdma);
 171:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMAAbortOnError(DMA_HandleTypeDef *hdma);
 172:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMATxAbortCallback(DMA_HandleTypeDef *hdma);
 173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMARxAbortCallback(DMA_HandleTypeDef *hdma);
 174:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static HAL_StatusTypeDef SPI_WaitOnFlagUntilTimeout(const SPI_HandleTypeDef *hspi, uint32_t Flag,
 175:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                     FlagStatus FlagStatus, uint32_t Timeout, uint32
 176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_TxISR_8BIT(SPI_HandleTypeDef *hspi);
 177:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_TxISR_16BIT(SPI_HandleTypeDef *hspi);
 178:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_TxISR_32BIT(SPI_HandleTypeDef *hspi);
 179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_RxISR_8BIT(SPI_HandleTypeDef *hspi);
 180:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_RxISR_16BIT(SPI_HandleTypeDef *hspi);
 181:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_RxISR_32BIT(SPI_HandleTypeDef *hspi);
 182:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_AbortTransfer(SPI_HandleTypeDef *hspi);
 183:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_CloseTransfer(SPI_HandleTypeDef *hspi);
 184:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static uint32_t SPI_GetPacketSize(const SPI_HandleTypeDef *hspi);
 185:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 186:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 187:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
 188:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @}
 189:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 190:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 191:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /* Exported functions --------------------------------------------------------*/
 192:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /** @defgroup SPI_Exported_Functions SPI Exported Functions
 193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @{
 194:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 195:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 196:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /** @defgroup SPI_Exported_Functions_Group1 Initialization and de-initialization functions
 197:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *  @brief    Initialization and Configuration functions
 198:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *
 199:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** @verbatim
 200:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****  ===============================================================================
 201:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****               ##### Initialization and de-initialization functions #####
 202:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****  ===============================================================================
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 5


 203:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     [..]  This subsection provides a set of functions allowing to initialize and
 204:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           de-initialize the SPIx peripheral:
 205:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       (+) User must implement HAL_SPI_MspInit() function in which he configures
 207:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           all related peripherals resources (CLOCK, GPIO, DMA, IT and NVIC ).
 208:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 209:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       (+) Call the function HAL_SPI_Init() to configure the selected device with
 210:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           the selected configuration:
 211:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) Mode
 212:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) Direction
 213:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) Data Size
 214:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) Clock Polarity and Phase
 215:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) NSS Management
 216:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) BaudRate Prescaler
 217:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) FirstBit
 218:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) TIMode
 219:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) CRC Calculation
 220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) CRC Polynomial if CRC enabled
 221:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) CRC Length, used only with Data8 and Data16
 222:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) FIFO reception threshold
 223:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         (++) FIFO transmission threshold
 224:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 225:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       (+) Call the function HAL_SPI_DeInit() to restore the default configuration
 226:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           of the selected SPIx peripheral.
 227:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 228:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** @endverbatim
 229:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @{
 230:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 231:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 232:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
 233:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Initialize the SPI according to the specified parameters
 234:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         in the SPI_InitTypeDef and initialize the associated handle.
 235:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
 236:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
 237:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
 238:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Init(SPI_HandleTypeDef *hspi)
 240:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t crc_length;
 242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t packet_length;
 243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_SPI_CRC != 0UL)
 244:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t crc_poly_msb_mask;
 245:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check the SPI handle allocation */
 248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi == NULL)
 249:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 250:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 251:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 253:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check the parameters */
 254:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_ALL_INSTANCE(hspi->Instance));
 255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_MODE(hspi->Init.Mode));
 256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION(hspi->Init.Direction));
 257:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DATASIZE(hspi->Init.DataSize));
 258:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_FIFOTHRESHOLD(hspi->Init.FifoThreshold));
 259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_NSS(hspi->Init.NSS));
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 6


 260:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_NSSP(hspi->Init.NSSPMode));
 261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_BAUDRATE_PRESCALER(hspi->Init.BaudRatePrescaler));
 262:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_FIRST_BIT(hspi->Init.FirstBit));
 263:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_TIMODE(hspi->Init.TIMode));
 264:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.TIMode == SPI_TIMODE_DISABLE)
 265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 266:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     assert_param(IS_SPI_CPOL(hspi->Init.CLKPolarity));
 267:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     assert_param(IS_SPI_CPHA(hspi->Init.CLKPhase));
 268:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 269:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_SPI_CRC != 0UL)
 270:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_CRC_CALCULATION(hspi->Init.CRCCalculation));
 271:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 272:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 273:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     assert_param(IS_SPI_CRC_LENGTH(hspi->Init.CRCLength));
 274:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     assert_param(IS_SPI_CRC_POLYNOMIAL(hspi->Init.CRCPolynomial));
 275:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     assert_param(IS_SPI_CRC_INITIALIZATION_PATTERN(hspi->Init.TxCRCInitializationPattern));
 276:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     assert_param(IS_SPI_CRC_INITIALIZATION_PATTERN(hspi->Init.RxCRCInitializationPattern));
 277:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 279:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->Init.CRCCalculation = SPI_CRCCALCULATION_DISABLE;
 280:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 281:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 282:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Verify that the SPI instance supports Data Size higher than 16bits */
 283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((!IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (hspi->Init.DataSize > SPI_DATASIZE_16BIT))
 284:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 285:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 286:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 287:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 288:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Verify that the SPI instance supports requested data packing */
 289:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   packet_length = SPI_GetPacketSize(hspi);
 290:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (((!IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (packet_length > SPI_LOWEND_FIFO_SIZE)) ||
 291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (packet_length > SPI_HIGHEND_FIFO_SIZE)))
 292:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 294:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 296:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_SPI_CRC != 0UL)
 297:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 299:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Verify that the SPI instance supports CRC Length higher than 16bits */
 300:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if ((!IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (hspi->Init.CRCLength > SPI_CRC_LENGTH_16BIT)
 301:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 302:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       return HAL_ERROR;
 303:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 305:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Align the CRC Length on the data size */
 306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->Init.CRCLength == SPI_CRC_LENGTH_DATASIZE)
 307:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 308:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       crc_length = (hspi->Init.DataSize >> SPI_CFG1_DSIZE_Pos) << SPI_CFG1_CRCSIZE_Pos;
 309:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 310:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
 311:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 312:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       crc_length = hspi->Init.CRCLength;
 313:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 314:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 315:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Verify the correctness of polynom size */
 316:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     assert_param(IS_SPI_CRC_POLYNOMIAL_SIZE(hspi->Init.CRCPolynomial, crc_length));
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 7


 317:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 318:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Verify that the CRC Length is higher than DataSize */
 319:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if ((hspi->Init.DataSize >> SPI_CFG1_DSIZE_Pos) > (crc_length >> SPI_CFG1_CRCSIZE_Pos))
 320:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 321:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       return HAL_ERROR;
 322:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 323:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
 325:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 326:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     crc_length = hspi->Init.DataSize << SPI_CFG1_CRCSIZE_Pos;
 327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 328:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 329:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 330:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State == HAL_SPI_STATE_RESET)
 331:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Allocate lock resource and initialize it */
 333:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->Lock = HAL_UNLOCKED;
 334:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 335:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
 336:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Init the SPI Callback settings */
 337:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxCpltCallback       = HAL_SPI_TxCpltCallback;       /* Legacy weak TxCpltCallback       
 338:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxCpltCallback       = HAL_SPI_RxCpltCallback;       /* Legacy weak RxCpltCallback       
 339:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxRxCpltCallback     = HAL_SPI_TxRxCpltCallback;     /* Legacy weak TxRxCpltCallback     
 340:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxHalfCpltCallback   = HAL_SPI_TxHalfCpltCallback;   /* Legacy weak TxHalfCpltCallback   
 341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxHalfCpltCallback   = HAL_SPI_RxHalfCpltCallback;   /* Legacy weak RxHalfCpltCallback   
 342:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxRxHalfCpltCallback = HAL_SPI_TxRxHalfCpltCallback; /* Legacy weak TxRxHalfCpltCallback 
 343:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->ErrorCallback        = HAL_SPI_ErrorCallback;        /* Legacy weak ErrorCallback        
 344:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->AbortCpltCallback    = HAL_SPI_AbortCpltCallback;    /* Legacy weak AbortCpltCallback    
 345:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->SuspendCallback      = HAL_SPI_SuspendCallback;      /* Legacy weak SuspendCallback      
 346:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->MspInitCallback == NULL)
 348:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 349:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->MspInitCallback = HAL_SPI_MspInit; /* Legacy weak MspInit  */
 350:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 351:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 352:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Init the low level hardware : GPIO, CLOCK, NVIC... */
 353:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->MspInitCallback(hspi);
 354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 355:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Init the low level hardware : GPIO, CLOCK, NVIC... */
 356:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     HAL_SPI_MspInit(hspi);
 357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 359:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_BUSY;
 361:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 362:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable the selected SPI peripheral */
 363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
 364:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 365:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_SPI_CRC == 0)
 366:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Keep the default value of CRCSIZE in case of CRC is not used */
 367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   crc_length = hspi->Instance->CFG1 & SPI_CFG1_CRCSIZE;
 368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 369:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 370:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /*----------------------- SPIx CR1 & CR2 Configuration ---------------------*/
 371:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Configure : SPI Mode, Communication Mode, Clock polarity and phase, NSS management,
 372:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   Communication speed, First bit, CRC calculation state, CRC Length */
 373:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 8


 374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPIx NSS Software Management Configuration */
 375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((hspi->Init.NSS == SPI_NSS_SOFT) && (((hspi->Init.Mode == SPI_MODE_MASTER) &&  \
 376:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                             (hspi->Init.NSSPolarity == SPI_NSS_POLARITY_LOW)) || \
 377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                            ((hspi->Init.Mode == SPI_MODE_SLAVE) && \
 378:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                             (hspi->Init.NSSPolarity == SPI_NSS_POLARITY_HIGH))))
 379:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 380:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_SSI);
 381:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 382:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 383:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPIx Master Rx Auto Suspend Configuration */
 384:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (((hspi->Init.Mode & SPI_MODE_MASTER) == SPI_MODE_MASTER) && (hspi->Init.DataSize >= SPI_DATAS
 385:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 386:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     MODIFY_REG(hspi->Instance->CR1, SPI_CR1_MASRX, hspi->Init.MasterReceiverAutoSusp);
 387:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 388:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
 389:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 390:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR1, SPI_CR1_MASRX);
 391:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 392:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 393:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPIx CFG1 Configuration */
 394:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   WRITE_REG(hspi->Instance->CFG1, (hspi->Init.BaudRatePrescaler | hspi->Init.CRCCalculation | crc_l
 395:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                    hspi->Init.FifoThreshold     | hspi->Init.DataSize));
 396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 397:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPIx CFG2 Configuration */
 398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   WRITE_REG(hspi->Instance->CFG2, (hspi->Init.NSSPMode                | hspi->Init.TIMode    |
 399:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                    hspi->Init.NSSPolarity             | hspi->Init.NSS       |
 400:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                    hspi->Init.CLKPolarity             | hspi->Init.CLKPhase  |
 401:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                    hspi->Init.FirstBit                | hspi->Init.Mode      |
 402:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                    hspi->Init.MasterInterDataIdleness | hspi->Init.Direction |
 403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                    hspi->Init.MasterSSIdleness        | hspi->Init.IOSwap));
 404:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_SPI_CRC != 0UL)
 406:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /*---------------------------- SPIx CRCPOLY Configuration ------------------*/
 407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Configure : CRC Polynomial */
 408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 409:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 410:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Initialize TXCRC Pattern Initial Value */
 411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->Init.TxCRCInitializationPattern == SPI_CRC_INITIALIZATION_ALL_ONE_PATTERN)
 412:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 413:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_TCRCINI);
 414:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 415:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
 416:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 417:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR1, SPI_CR1_TCRCINI);
 418:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 419:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Initialize RXCRC Pattern Initial Value */
 421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->Init.RxCRCInitializationPattern == SPI_CRC_INITIALIZATION_ALL_ONE_PATTERN)
 422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 423:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_RCRCINI);
 424:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 425:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
 426:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 427:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR1, SPI_CR1_RCRCINI);
 428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 429:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 430:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Enable 33/17 bits CRC computation */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 9


 431:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (((!IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (crc_length == SPI_CRC_LENGTH_16BIT)) ||
 432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         ((IS_SPI_HIGHEND_INSTANCE(hspi->Instance))  && (crc_length == SPI_CRC_LENGTH_32BIT)))
 433:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 434:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Set SPI_CR1_CRC33_17 bit */
 435:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_CRC33_17);
 436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Write CRC polynomial in SPI Register */
 437:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       WRITE_REG(hspi->Instance->CRCPOLY, hspi->Init.CRCPolynomial);
 438:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 439:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
 440:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 441:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Clear SPI_CR1_CRC33_17 bit */
 442:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR1, SPI_CR1_CRC33_17);
 443:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Write CRC polynomial and set MSB bit at 1 in SPI Register */
 445:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Set MSB is mandatory for a correct CRC computation        */
 446:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       crc_poly_msb_mask = (0x1UL << ((crc_length >> SPI_CFG1_CRCSIZE_Pos) + 0x1U));
 447:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       WRITE_REG(hspi->Instance->CRCPOLY, (hspi->Init.CRCPolynomial) | crc_poly_msb_mask);
 448:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 449:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 450:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 451:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 452:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Insure that Underrun configuration is managed only by Salve */
 453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Mode == SPI_MODE_SLAVE)
 454:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 455:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Set Default Underrun configuration */
 456:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_SPI_CRC != 0UL)
 457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_DISABLE)
 458:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 460:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       MODIFY_REG(hspi->Instance->CFG1, SPI_CFG1_UDRDET, SPI_CFG1_UDRDET_0);
 461:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     MODIFY_REG(hspi->Instance->CFG1, SPI_CFG1_UDRCFG, SPI_CFG1_UDRCFG_1);
 463:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 464:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 465:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(SPI_I2SCFGR_I2SMOD)
 466:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Activate the SPI mode (Make sure that I2SMOD bit in I2SCFGR register is reset) */
 467:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->I2SCFGR, SPI_I2SCFGR_I2SMOD);
 468:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* SPI_I2SCFGR_I2SMOD */
 469:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 470:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Insure that AFCNTR is managed only by Master */
 471:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((hspi->Init.Mode & SPI_MODE_MASTER) == SPI_MODE_MASTER)
 472:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 473:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Alternate function GPIOs control */
 474:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     MODIFY_REG(hspi->Instance->CFG2, SPI_CFG2_AFCNTR, (hspi->Init.MasterKeepIOState));
 475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 476:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 477:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode = HAL_SPI_ERROR_NONE;
 478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State     = HAL_SPI_STATE_READY;
 479:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 480:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return HAL_OK;
 481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 482:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 483:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
 484:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  De-Initialize the SPI peripheral.
 485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
 486:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
 487:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 10


 488:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 489:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_DeInit(SPI_HandleTypeDef *hspi)
 490:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 491:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check the SPI handle allocation */
 492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi == NULL)
 493:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 494:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 495:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 497:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check SPI Instance parameter */
 498:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_ALL_INSTANCE(hspi->Instance));
 499:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_BUSY;
 501:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 502:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable the SPI Peripheral Clock */
 503:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
 504:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 505:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
 506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->MspDeInitCallback == NULL)
 507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->MspDeInitCallback = HAL_SPI_MspDeInit; /* Legacy weak MspDeInit  */
 509:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 510:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 511:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* DeInit the low level hardware: GPIO, CLOCK, NVIC... */
 512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->MspDeInitCallback(hspi);
 513:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 514:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* DeInit the low level hardware: GPIO, CLOCK, NVIC... */
 515:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_SPI_MspDeInit(hspi);
 516:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 517:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode = HAL_SPI_ERROR_NONE;
 519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_RESET;
 520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 521:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Release Lock */
 522:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
 523:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 524:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return HAL_OK;
 525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 526:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 527:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
 528:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Initialize the SPI MSP.
 529:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
 530:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
 531:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
 532:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 533:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** __weak void HAL_SPI_MspInit(SPI_HandleTypeDef *hspi)
 534:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 535:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 536:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   UNUSED(hspi);
 537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 538:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
 539:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             the HAL_SPI_MspInit should be implemented in the user file
 540:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****    */
 541:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 542:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 543:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
 544:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  De-Initialize the SPI MSP.
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 11


 545:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
 546:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
 547:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
 548:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 549:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** __weak void HAL_SPI_MspDeInit(SPI_HandleTypeDef *hspi)
 550:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 551:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 552:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   UNUSED(hspi);
 553:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 554:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
 555:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             the HAL_SPI_MspDeInit should be implemented in the user file
 556:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****    */
 557:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 558:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 559:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
 560:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
 561:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Register a User SPI Callback
 562:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         To be used instead of the weak predefined callback
 563:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi Pointer to a SPI_HandleTypeDef structure that contains
 564:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                the configuration information for the specified SPI.
 565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  CallbackID ID of the callback to be registered
 566:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pCallback pointer to the Callback function
 567:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @note   The HAL_SPI_RegisterCallback() may be called before HAL_SPI_Init() in HAL_SPI_STATE_RES
 568:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         to register callbacks for HAL_SPI_MSPINIT_CB_ID and HAL_SPI_MSPDEINIT_CB_ID
 569:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
 570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 571:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_RegisterCallback(SPI_HandleTypeDef *hspi, HAL_SPI_CallbackIDTypeDef Callb
 572:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                            pSPI_CallbackTypeDef pCallback)
 573:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_StatusTypeDef status = HAL_OK;
 575:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 576:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (pCallback == NULL)
 577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 578:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Update the error code */
 579:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->ErrorCode |= HAL_SPI_ERROR_INVALID_CALLBACK;
 580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 581:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 582:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 583:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 584:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_SPI_STATE_READY == hspi->State)
 585:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 586:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     switch (CallbackID)
 587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_TX_COMPLETE_CB_ID :
 589:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxCpltCallback = pCallback;
 590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 591:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 592:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_RX_COMPLETE_CB_ID :
 593:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxCpltCallback = pCallback;
 594:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 596:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_TX_RX_COMPLETE_CB_ID :
 597:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxRxCpltCallback = pCallback;
 598:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 599:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 600:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_TX_HALF_COMPLETE_CB_ID :
 601:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxHalfCpltCallback = pCallback;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 12


 602:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 603:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_RX_HALF_COMPLETE_CB_ID :
 605:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxHalfCpltCallback = pCallback;
 606:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 607:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 608:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_TX_RX_HALF_COMPLETE_CB_ID :
 609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxRxHalfCpltCallback = pCallback;
 610:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 612:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_ERROR_CB_ID :
 613:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->ErrorCallback = pCallback;
 614:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 615:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 616:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_ABORT_CB_ID :
 617:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->AbortCpltCallback = pCallback;
 618:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 619:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_SUSPEND_CB_ID :
 621:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->SuspendCallback = pCallback;
 622:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 623:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 624:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_MSPINIT_CB_ID :
 625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->MspInitCallback = pCallback;
 626:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 627:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_MSPDEINIT_CB_ID :
 629:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->MspDeInitCallback = pCallback;
 630:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 631:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 632:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       default :
 633:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Update the error code */
 634:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 635:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 636:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Return error status */
 637:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         status =  HAL_ERROR;
 638:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 639:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 640:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else if (HAL_SPI_STATE_RESET == hspi->State)
 642:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 643:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     switch (CallbackID)
 644:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 645:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_MSPINIT_CB_ID :
 646:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->MspInitCallback = pCallback;
 647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 648:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 649:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_MSPDEINIT_CB_ID :
 650:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->MspDeInitCallback = pCallback;
 651:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 652:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 653:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       default :
 654:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Update the error code */
 655:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 656:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 657:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Return error status */
 658:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         status =  HAL_ERROR;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 13


 659:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 660:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 662:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
 663:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 664:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Update the error code */
 665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 666:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 667:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Return error status */
 668:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     status =  HAL_ERROR;
 669:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 670:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 671:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return status;
 672:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 673:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 674:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
 675:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Unregister an SPI Callback
 676:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         SPI callback is redirected to the weak predefined callback
 677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi Pointer to a SPI_HandleTypeDef structure that contains
 678:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                the configuration information for the specified SPI.
 679:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  CallbackID ID of the callback to be unregistered
 680:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @note   The HAL_SPI_UnRegisterCallback() may be called before HAL_SPI_Init() in HAL_SPI_STATE_R
 681:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         to un-register callbacks for HAL_SPI_MSPINIT_CB_ID and HAL_SPI_MSPDEINIT_CB_ID
 682:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
 683:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 684:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_UnRegisterCallback(SPI_HandleTypeDef *hspi, HAL_SPI_CallbackIDTypeDef Cal
 685:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 686:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_StatusTypeDef status = HAL_OK;
 687:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 688:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_SPI_STATE_READY == hspi->State)
 689:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 690:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     switch (CallbackID)
 691:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 692:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_TX_COMPLETE_CB_ID :
 693:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxCpltCallback = HAL_SPI_TxCpltCallback;             /* Legacy weak TxCpltCallback   
 694:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 695:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 696:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_RX_COMPLETE_CB_ID :
 697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxCpltCallback = HAL_SPI_RxCpltCallback;             /* Legacy weak RxCpltCallback   
 698:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 699:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 700:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_TX_RX_COMPLETE_CB_ID :
 701:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxRxCpltCallback = HAL_SPI_TxRxCpltCallback;         /* Legacy weak TxRxCpltCallback 
 702:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 703:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 704:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_TX_HALF_COMPLETE_CB_ID :
 705:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxHalfCpltCallback = HAL_SPI_TxHalfCpltCallback;     /* Legacy weak TxHalfCpltCallbac
 706:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 707:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 708:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_RX_HALF_COMPLETE_CB_ID :
 709:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxHalfCpltCallback = HAL_SPI_RxHalfCpltCallback;     /* Legacy weak RxHalfCpltCallbac
 710:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 711:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 712:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_TX_RX_HALF_COMPLETE_CB_ID :
 713:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxRxHalfCpltCallback = HAL_SPI_TxRxHalfCpltCallback; /* Legacy weak TxRxHalfCpltCallb
 714:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 715:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 14


 716:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_ERROR_CB_ID :
 717:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->ErrorCallback = HAL_SPI_ErrorCallback;               /* Legacy weak ErrorCallback    
 718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 719:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 720:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_ABORT_CB_ID :
 721:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->AbortCpltCallback = HAL_SPI_AbortCpltCallback;       /* Legacy weak AbortCpltCallback
 722:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 723:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_SUSPEND_CB_ID :
 725:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->SuspendCallback = HAL_SPI_SuspendCallback;           /* Legacy weak SuspendCallback  
 726:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 727:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 728:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_MSPINIT_CB_ID :
 729:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->MspInitCallback = HAL_SPI_MspInit;                   /* Legacy weak MspInit          
 730:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 731:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 732:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_MSPDEINIT_CB_ID :
 733:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->MspDeInitCallback = HAL_SPI_MspDeInit;               /* Legacy weak MspDeInit        
 734:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 735:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 736:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       default :
 737:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Update the error code */
 738:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 739:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 740:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Return error status */
 741:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         status =  HAL_ERROR;
 742:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 743:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 744:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 745:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else if (HAL_SPI_STATE_RESET == hspi->State)
 746:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 747:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     switch (CallbackID)
 748:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 749:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_MSPINIT_CB_ID :
 750:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->MspInitCallback = HAL_SPI_MspInit;                   /* Legacy weak MspInit          
 751:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 752:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 753:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       case HAL_SPI_MSPDEINIT_CB_ID :
 754:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->MspDeInitCallback = HAL_SPI_MspDeInit;               /* Legacy weak MspDeInit        
 755:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 756:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 757:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       default :
 758:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Update the error code */
 759:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 761:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Return error status */
 762:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         status =  HAL_ERROR;
 763:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 764:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 765:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 766:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
 767:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 768:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Update the error code */
 769:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 770:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 771:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Return error status */
 772:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     status =  HAL_ERROR;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 15


 773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 774:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 775:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return status;
 776:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 777:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 778:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
 779:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @}
 780:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 781:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 782:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /** @defgroup SPI_Exported_Functions_Group2 IO operation functions
 783:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *  @brief   Data transfers functions
 784:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *
 785:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** @verbatim
 786:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   ==============================================================================
 787:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                       ##### IO operation functions #####
 788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****  ===============================================================================
 789:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****  [..]
 790:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     This subsection provides a set of functions allowing to manage the SPI
 791:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     data transfers.
 792:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 793:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     [..] The SPI supports master and slave mode :
 794:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 795:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     (#) There are two modes of transfer:
 796:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        (##) Blocking mode: The communication is performed in polling mode.
 797:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             The HAL status of all data processing is returned by the same function
 798:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             after finishing transfer.
 799:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****        (##) No-Blocking mode: The communication is performed using Interrupts
 800:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             or DMA, These APIs return the HAL status.
 801:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             The end of the data processing will be indicated through the
 802:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             dedicated SPI IRQ when using Interrupt mode or the DMA IRQ when
 803:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             using DMA mode.
 804:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             The HAL_SPI_TxCpltCallback(), HAL_SPI_RxCpltCallback() and HAL_SPI_TxRxCpltCallback() u
 805:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             will be executed respectively at the end of the transmit or Receive process
 806:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             The HAL_SPI_ErrorCallback()user callback will be executed when a communication error is
 807:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 808:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     (#) APIs provided for these 2 transfer modes (Blocking mode or Non blocking mode using either I
 809:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         exist for 1Line (simplex) and 2Lines (full duplex) modes.
 810:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 811:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** @endverbatim
 812:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @{
 813:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 814:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 815:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
 816:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Transmit an amount of data in blocking mode.
 817:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi   : pointer to a SPI_HandleTypeDef structure that contains
 818:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                  the configuration information for SPI module.
 819:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pData  : pointer to data buffer
 820:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Size   : amount of data to be sent
 821:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Timeout: Timeout duration
 822:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
 823:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
 824:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Transmit(SPI_HandleTypeDef *hspi, const uint8_t *pData, uint16_t Size, ui
 825:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 826:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 827:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint16_t *ptxdr_16bits = (__IO uint16_t *)(&(hspi->Instance->TXDR));
 828:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
 829:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 16


 830:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t tickstart;
 831:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 832:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
 833:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES_OR_1LINE_2LINES_TXONLY(hspi->Init.Direction));
 834:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 835:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Init tickstart for timeout management*/
 836:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   tickstart = HAL_GetTick();
 837:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
 839:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 840:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_BUSY;
 841:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 842:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 843:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0UL))
 844:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 845:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 846:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 848:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Lock the process */
 849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_LOCK(hspi);
 850:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 851:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the transaction information */
 852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_TX;
 853:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 854:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pData;
 855:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 856:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 858:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /*Init field not used in handle to zero */
 859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = NULL;
 860:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = (uint16_t) 0UL;
 861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t) 0UL;
 862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
 864:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Configure communication direction : 1Line */
 866:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
 867:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 868:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 869:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 870:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
 871:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 872:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_2LINES_TX(hspi);
 873:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 874:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 875:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the number of data at current transfer */
 876:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSIZE, Size);
 877:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 878:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable SPI peripheral */
 879:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE(hspi);
 880:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Mode == SPI_MODE_MASTER)
 882:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 883:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Master transfer start */
 884:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CSTART);
 885:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 886:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 17


 887:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Transmit data in 32 Bit mode */
 888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_16BIT)
 889:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 890:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Transmit data in 32 Bit mode */
 891:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     while (hspi->TxXferCount > 0UL)
 892:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 893:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Wait until TXP flag is set to send data */
 894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXP))
 895:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 896:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((__IO uint32_t *)&hspi->Instance->TXDR) = *((const uint32_t *)hspi->pTxBuffPtr);
 897:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint32_t);
 898:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount--;
 899:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       else
 901:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 902:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Timeout management */
 903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
 904:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 905:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Call standard close procedure with error check */
 906:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SPI_CloseTransfer(hspi);
 907:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 908:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_TIMEOUT);
 909:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 910:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 911:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Unlock the process */
 912:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           __HAL_UNLOCK(hspi);
 913:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 914:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           return HAL_TIMEOUT;
 915:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 916:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 917:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 918:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
 920:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
 921:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 922:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Transmit data in 16 Bit mode */
 923:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     while (hspi->TxXferCount > 0UL)
 924:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 925:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Wait until TXP flag is set to send data */
 926:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXP))
 927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if ((hspi->TxXferCount > 1UL) && (hspi->Init.FifoThreshold > SPI_FIFO_THRESHOLD_01DATA))
 929:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 930:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((__IO uint32_t *)&hspi->Instance->TXDR) = *((const uint32_t *)hspi->pTxBuffPtr);
 931:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint32_t);
 932:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount -= (uint16_t)2UL;
 933:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 934:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else
 935:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 936:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 937:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *ptxdr_16bits = *((const uint16_t *)hspi->pTxBuffPtr);
 938:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 939:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((__IO uint16_t *)&hspi->Instance->TXDR) = *((const uint16_t *)hspi->pTxBuffPtr);
 940:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
 941:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 942:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount--;
 943:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 18


 944:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 945:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       else
 946:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 947:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Timeout management */
 948:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
 949:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 950:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Call standard close procedure with error check */
 951:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SPI_CloseTransfer(hspi);
 952:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 953:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_TIMEOUT);
 954:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 955:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 956:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Unlock the process */
 957:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           __HAL_UNLOCK(hspi);
 958:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 959:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           return HAL_TIMEOUT;
 960:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 961:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 962:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 963:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 964:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Transmit data in 8 Bit mode */
 965:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
 966:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 967:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     while (hspi->TxXferCount > 0UL)
 968:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 969:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Wait until TXP flag is set to send data */
 970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXP))
 971:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if ((hspi->TxXferCount > 3UL) && (hspi->Init.FifoThreshold > SPI_FIFO_THRESHOLD_03DATA))
 973:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 974:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((__IO uint32_t *)&hspi->Instance->TXDR) = *((const uint32_t *)hspi->pTxBuffPtr);
 975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint32_t);
 976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount -= (uint16_t)4UL;
 977:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 978:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else if ((hspi->TxXferCount > 1UL) && (hspi->Init.FifoThreshold > SPI_FIFO_THRESHOLD_01DATA
 979:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 980:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 981:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *ptxdr_16bits = *((const uint16_t *)hspi->pTxBuffPtr);
 982:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 983:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((__IO uint16_t *)&hspi->Instance->TXDR) = *((const uint16_t *)hspi->pTxBuffPtr);
 984:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
 985:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 986:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount -= (uint16_t)2UL;
 987:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else
 989:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 990:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((__IO uint8_t *)&hspi->Instance->TXDR) = *((const uint8_t *)hspi->pTxBuffPtr);
 991:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint8_t);
 992:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount--;
 993:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 994:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 995:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       else
 996:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 997:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Timeout management */
 998:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
 999:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1000:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Call standard close procedure with error check */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 19


1001:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SPI_CloseTransfer(hspi);
1002:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1003:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_TIMEOUT);
1004:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
1005:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1006:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Unlock the process */
1007:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           __HAL_UNLOCK(hspi);
1008:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1009:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           return HAL_TIMEOUT;
1010:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1011:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1012:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
1013:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1014:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1015:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Wait for Tx (and CRC) data to be sent */
1016:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (SPI_WaitOnFlagUntilTimeout(hspi, SPI_FLAG_EOT, RESET, Timeout, tickstart) != HAL_OK)
1017:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1018:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
1019:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1020:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1021:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Call standard close procedure with error check */
1022:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_CloseTransfer(hspi);
1023:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1024:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
1025:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1026:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Unlock the process */
1027:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1028:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1029:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
1030:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1031:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
1032:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1033:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1034:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1035:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_OK;
1036:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1037:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
1038:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1039:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
1040:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Receive an amount of data in blocking mode.
1041:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi   : pointer to a SPI_HandleTypeDef structure that contains
1042:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                  the configuration information for SPI module.
1043:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pData  : pointer to data buffer
1044:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Size   : amount of data to be received
1045:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Timeout: Timeout duration
1046:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
1047:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
1048:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Receive(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size, uint32_t 
1049:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
1050:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t tickstart;
1051:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t temp_sr_reg;
1052:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint16_t init_max_data_in_fifo;
1053:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   init_max_data_in_fifo = (((uint16_t)(hspi->Init.FifoThreshold >> 5U) + 1U));
1054:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
1055:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint16_t *prxdr_16bits = (__IO uint16_t *)(&(hspi->Instance->RXDR));
1056:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
1057:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 20


1058:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
1059:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES_OR_1LINE_2LINES_RXONLY(hspi->Init.Direction));
1060:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1061:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Init tickstart for timeout management*/
1062:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   tickstart = HAL_GetTick();
1063:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1064:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1065:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1066:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_BUSY;
1067:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1068:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1069:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0UL))
1070:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1071:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
1072:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1073:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1074:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Lock the process */
1075:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_LOCK(hspi);
1076:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1077:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the transaction information */
1078:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_RX;
1079:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1080:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
1081:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
1082:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
1083:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1084:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /*Init field not used in handle to zero */
1085:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = NULL;
1086:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = (uint16_t) 0UL;
1087:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t) 0UL;
1088:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
1089:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
1090:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1091:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Configure communication direction: 1Line */
1092:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
1093:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1094:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
1095:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1096:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1097:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1098:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_2LINES_RX(hspi);
1099:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1100:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1101:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the number of data at current transfer */
1102:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSIZE, Size);
1103:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1104:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable SPI peripheral */
1105:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE(hspi);
1106:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Mode == SPI_MODE_MASTER)
1108:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1109:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Master transfer start */
1110:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CSTART);
1111:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1112:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1113:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Receive data in 32 Bit mode */
1114:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_16BIT)
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 21


1115:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1116:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Transfer loop */
1117:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     while (hspi->RxXferCount > 0UL)
1118:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
1119:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Evaluate state of SR register */
1120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       temp_sr_reg = hspi->Instance->SR;
1121:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1122:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Check the RXP flag */
1123:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXP))
1124:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1125:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint32_t *)hspi->pRxBuffPtr) = *((__IO uint32_t *)&hspi->Instance->RXDR);
1126:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint32_t);
1127:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
1128:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1129:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Check RXWNE flag if RXP cannot be reached */
1130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       else if ((hspi->RxXferCount < init_max_data_in_fifo) && ((temp_sr_reg & SPI_SR_RXWNE_Msk) != 
1131:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1132:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint32_t *)hspi->pRxBuffPtr) = *((__IO uint32_t *)&hspi->Instance->RXDR);
1133:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint32_t);
1134:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
1135:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1136:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       else
1137:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1138:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Timeout management */
1139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
1140:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1141:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Call standard close procedure with error check */
1142:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SPI_CloseTransfer(hspi);
1143:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1144:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_TIMEOUT);
1145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
1146:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1147:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Unlock the process */
1148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           __HAL_UNLOCK(hspi);
1149:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1150:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           return HAL_TIMEOUT;
1151:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1152:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1153:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
1154:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1155:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Receive data in 16 Bit mode */
1156:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1157:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1158:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Transfer loop */
1159:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     while (hspi->RxXferCount > 0UL)
1160:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
1161:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Evaluate state of SR register */
1162:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       temp_sr_reg = hspi->Instance->SR;
1163:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1164:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Check the RXP flag */
1165:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXP))
1166:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1167:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
1168:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint16_t *)hspi->pRxBuffPtr) = *prxdr_16bits;
1169:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
1170:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint16_t *)hspi->pRxBuffPtr) = *((__IO uint16_t *)&hspi->Instance->RXDR);
1171:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 22


1172:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
1173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
1174:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1175:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Check RXWNE flag if RXP cannot be reached */
1176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       else if ((hspi->RxXferCount < init_max_data_in_fifo) && ((temp_sr_reg & SPI_SR_RXWNE_Msk) != 
1177:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1178:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
1179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint16_t *)hspi->pRxBuffPtr) = *prxdr_16bits;
1180:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
1181:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint16_t *)hspi->pRxBuffPtr) = *((__IO uint16_t *)&hspi->Instance->RXDR);
1182:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
1183:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
1184:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
1185:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint16_t *)hspi->pRxBuffPtr) = *prxdr_16bits;
1186:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
1187:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint16_t *)hspi->pRxBuffPtr) = *((__IO uint16_t *)&hspi->Instance->RXDR);
1188:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
1189:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
1190:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount -= (uint16_t)2UL;
1191:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1192:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Check RXPLVL flags when RXWNE cannot be reached */
1193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       else if ((hspi->RxXferCount == 1UL) && ((temp_sr_reg & SPI_SR_RXPLVL_0) != 0UL))
1194:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1195:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
1196:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint16_t *)hspi->pRxBuffPtr) = *prxdr_16bits;
1197:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
1198:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint16_t *)hspi->pRxBuffPtr) = *((__IO uint16_t *)&hspi->Instance->RXDR);
1199:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
1200:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
1201:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
1202:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1203:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       else
1204:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1205:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Timeout management */
1206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
1207:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1208:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Call standard close procedure with error check */
1209:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SPI_CloseTransfer(hspi);
1210:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1211:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_TIMEOUT);
1212:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
1213:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1214:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Unlock the process */
1215:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           __HAL_UNLOCK(hspi);
1216:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1217:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           return HAL_TIMEOUT;
1218:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1219:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
1221:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1222:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Receive data in 8 Bit mode */
1223:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1224:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1225:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Transfer loop */
1226:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     while (hspi->RxXferCount > 0UL)
1227:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
1228:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Evaluate state of SR register */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 23


1229:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       temp_sr_reg = hspi->Instance->SR;
1230:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1231:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Check the RXP flag */
1232:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXP))
1233:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1234:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
1235:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
1236:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
1237:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1238:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Check RXWNE flag if RXP cannot be reached */
1239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       else if ((hspi->RxXferCount < init_max_data_in_fifo) && ((temp_sr_reg & SPI_SR_RXWNE_Msk) != 
1240:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
1242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
1243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
1244:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
1245:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
1246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
1247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
1248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
1249:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount -= (uint16_t)4UL;
1250:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1251:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Check RXPLVL flags when RXWNE cannot be reached */
1252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       else if ((hspi->RxXferCount < 4UL) && ((temp_sr_reg & SPI_SR_RXPLVL_Msk) != 0UL))
1253:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1254:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
1255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
1256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
1257:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1258:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       else
1259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1260:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Timeout management */
1261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
1262:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1263:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Call standard close procedure with error check */
1264:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SPI_CloseTransfer(hspi);
1265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1266:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_TIMEOUT);
1267:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
1268:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1269:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Unlock the process */
1270:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           __HAL_UNLOCK(hspi);
1271:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1272:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           return HAL_TIMEOUT;
1273:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1274:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1275:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
1276:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1277:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_SPI_CRC != 0UL)
1279:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1280:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1281:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Wait for crc data to be received */
1282:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (SPI_WaitOnFlagUntilTimeout(hspi, SPI_FLAG_EOT, RESET, Timeout, tickstart) != HAL_OK)
1283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
1284:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
1285:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 24


1286:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1287:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1288:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1289:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Call standard close procedure with error check */
1290:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_CloseTransfer(hspi);
1291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1292:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
1293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1294:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Unlock the process */
1295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1296:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1297:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
1299:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1300:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
1301:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1302:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1303:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_OK;
1305:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
1307:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1308:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
1309:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Transmit and Receive an amount of data in blocking mode.
1310:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi   : pointer to a SPI_HandleTypeDef structure that contains
1311:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                  the configuration information for SPI module.
1312:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pTxData: pointer to transmission data buffer
1313:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pRxData: pointer to reception data buffer
1314:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Size   : amount of data to be sent and received
1315:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Timeout: Timeout duration
1316:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
1317:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
1318:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_TransmitReceive(SPI_HandleTypeDef *hspi, const uint8_t *pTxData, uint8_t 
1319:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                           uint16_t Size, uint32_t Timeout)
1320:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
1321:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
1322:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint16_t *ptxdr_16bits = (__IO uint16_t *)(&(hspi->Instance->TXDR));
1323:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint16_t *prxdr_16bits = (__IO uint16_t *)(&(hspi->Instance->RXDR));
1324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
1325:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1326:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t   tickstart;
1327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t   fifo_length;
1328:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t   temp_sr_reg;
1329:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint16_t   initial_TxXferCount;
1330:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint16_t   initial_RxXferCount;
1331:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint16_t   init_max_data_in_fifo;
1332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   init_max_data_in_fifo = (((uint16_t)(hspi->Init.FifoThreshold >> 5U) + 1U));
1333:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1334:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
1335:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES(hspi->Init.Direction));
1336:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1337:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Init tickstart for timeout management*/
1338:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   tickstart = HAL_GetTick();
1339:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1340:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   initial_TxXferCount = Size;
1341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   initial_RxXferCount = Size;
1342:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 25


1343:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1344:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1345:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_BUSY;
1346:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1348:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((pTxData == NULL) || (pRxData == NULL) || (Size == 0UL))
1349:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1350:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
1351:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1352:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1353:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Lock the process */
1354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_LOCK(hspi);
1355:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1356:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the transaction information */
1357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_TX_RX;
1358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1359:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
1360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
1361:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
1362:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pTxData;
1363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
1364:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
1365:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1366:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /*Init field not used in handle to zero */
1367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
1368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
1369:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1370:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set Full-Duplex mode */
1371:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_2LINES(hspi);
1372:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1373:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Initialize FIFO length */
1374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (IS_SPI_HIGHEND_INSTANCE(hspi->Instance))
1375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1376:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     fifo_length = SPI_HIGHEND_FIFO_SIZE;
1377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1378:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1379:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1380:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     fifo_length = SPI_LOWEND_FIFO_SIZE;
1381:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1382:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1383:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the number of data at current transfer */
1384:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSIZE, Size);
1385:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1386:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE(hspi);
1387:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1388:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Mode == SPI_MODE_MASTER)
1389:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1390:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Master transfer start */
1391:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CSTART);
1392:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1393:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1394:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Transmit and Receive data in 32 Bit mode */
1395:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_16BIT)
1396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1397:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Adapt fifo length to 32bits data width */
1398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     fifo_length = (fifo_length / 4UL);
1399:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 26


1400:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     while ((initial_TxXferCount > 0UL) || (initial_RxXferCount > 0UL))
1401:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
1402:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Check TXP flag */
1403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if ((__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXP)) && (initial_TxXferCount > 0UL) &&
1404:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
1405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1406:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((__IO uint32_t *)&hspi->Instance->TXDR) = *((const uint32_t *)hspi->pTxBuffPtr);
1407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint32_t);
1408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount --;
1409:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         initial_TxXferCount = hspi->TxXferCount;
1410:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1412:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Evaluate state of SR register */
1413:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       temp_sr_reg = hspi->Instance->SR;
1414:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1415:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (initial_RxXferCount > 0UL)
1416:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1417:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Check the RXP flag */
1418:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXP))
1419:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint32_t *)hspi->pRxBuffPtr) = *((__IO uint32_t *)&hspi->Instance->RXDR);
1421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
1422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
1423:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
1424:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1425:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Check RXWNE flag if RXP cannot be reached */
1426:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else if ((initial_RxXferCount < init_max_data_in_fifo) && ((temp_sr_reg & SPI_SR_RXWNE_Msk)
1427:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint32_t *)hspi->pRxBuffPtr) = *((__IO uint32_t *)&hspi->Instance->RXDR);
1429:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
1430:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
1431:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
1432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1433:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else
1434:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1435:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Timeout management */
1436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout
1437:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
1438:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             /* Call standard close procedure with error check */
1439:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             SPI_CloseTransfer(hspi);
1440:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1441:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_TIMEOUT);
1442:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             hspi->State = HAL_SPI_STATE_READY;
1443:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             /* Unlock the process */
1445:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             __HAL_UNLOCK(hspi);
1446:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1447:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             return HAL_TIMEOUT;
1448:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
1449:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1450:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1451:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
1452:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Transmit and Receive data in 16 Bit mode */
1454:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1455:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1456:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Adapt fifo length to 16bits data width */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 27


1457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     fifo_length = (fifo_length / 2UL);
1458:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     while ((initial_TxXferCount > 0UL) || (initial_RxXferCount > 0UL))
1460:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
1461:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Check the TXP flag */
1462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if ((__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXP)) && (initial_TxXferCount > 0UL) &&
1463:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
1464:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1465:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
1466:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *ptxdr_16bits = *((const uint16_t *)hspi->pTxBuffPtr);
1467:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
1468:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((__IO uint16_t *)&hspi->Instance->TXDR) = *((const uint16_t *)hspi->pTxBuffPtr);
1469:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
1470:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
1471:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount--;
1472:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         initial_TxXferCount = hspi->TxXferCount;
1473:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1474:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Evaluate state of SR register */
1476:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       temp_sr_reg = hspi->Instance->SR;
1477:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (initial_RxXferCount > 0UL)
1479:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1480:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Check the RXP flag */
1481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXP))
1482:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1483:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
1484:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint16_t *)hspi->pRxBuffPtr) = *prxdr_16bits;
1485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
1486:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint16_t *)hspi->pRxBuffPtr) = *((__IO uint16_t *)&hspi->Instance->RXDR);
1487:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
1488:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
1489:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
1490:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
1491:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Check RXWNE flag if RXP cannot be reached */
1493:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else if ((initial_RxXferCount < init_max_data_in_fifo) && ((temp_sr_reg & SPI_SR_RXWNE_Msk)
1494:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1495:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
1496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint16_t *)hspi->pRxBuffPtr) = *prxdr_16bits;
1497:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
1498:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint16_t *)hspi->pRxBuffPtr) = *((__IO uint16_t *)&hspi->Instance->RXDR);
1499:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
1500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
1501:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
1502:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint16_t *)hspi->pRxBuffPtr) = *prxdr_16bits;
1503:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
1504:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint16_t *)hspi->pRxBuffPtr) = *((__IO uint16_t *)&hspi->Instance->RXDR);
1505:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
1506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
1507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount -= (uint16_t)2UL;
1508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
1509:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1510:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Check RXPLVL flags when RXWNE cannot be reached */
1511:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else if ((initial_RxXferCount == 1UL) && ((temp_sr_reg & SPI_SR_RXPLVL_0) != 0UL))
1512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1513:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 28


1514:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint16_t *)hspi->pRxBuffPtr) = *prxdr_16bits;
1515:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
1516:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint16_t *)hspi->pRxBuffPtr) = *((__IO uint16_t *)&hspi->Instance->RXDR);
1517:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
1518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
1519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
1520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
1521:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1522:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else
1523:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1524:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Timeout management */
1525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout
1526:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
1527:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             /* Call standard close procedure with error check */
1528:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             SPI_CloseTransfer(hspi);
1529:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1530:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_TIMEOUT);
1531:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             hspi->State = HAL_SPI_STATE_READY;
1532:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1533:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             /* Unlock the process */
1534:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             __HAL_UNLOCK(hspi);
1535:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1536:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             return HAL_TIMEOUT;
1537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
1538:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1539:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1540:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
1541:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1542:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Transmit and Receive data in 8 Bit mode */
1543:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1544:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1545:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     while ((initial_TxXferCount > 0UL) || (initial_RxXferCount > 0UL))
1546:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
1547:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Check the TXP flag */
1548:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if ((__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXP)) && (initial_TxXferCount > 0UL) &&
1549:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
1550:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1551:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((__IO uint8_t *)&hspi->Instance->TXDR) = *((const uint8_t *)hspi->pTxBuffPtr);
1552:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint8_t);
1553:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount--;
1554:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         initial_TxXferCount = hspi->TxXferCount;
1555:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1556:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1557:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Evaluate state of SR register */
1558:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       temp_sr_reg = hspi->Instance->SR;
1559:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1560:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (initial_RxXferCount > 0UL)
1561:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
1562:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Check the RXP flag */
1563:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXP))
1564:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
1566:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
1567:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
1568:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
1569:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Check RXWNE flag if RXP cannot be reached */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 29


1571:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else if ((initial_RxXferCount < init_max_data_in_fifo) && ((temp_sr_reg & SPI_SR_RXWNE_Msk)
1572:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1573:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
1574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
1575:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
1576:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
1577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
1578:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
1579:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
1580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
1581:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount -= (uint16_t)4UL;
1582:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
1583:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1584:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Check RXPLVL flags when RXWNE cannot be reached */
1585:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else if ((initial_RxXferCount < 4UL) && ((temp_sr_reg & SPI_SR_RXPLVL_Msk) != 0UL))
1586:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
1588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
1589:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
1590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
1591:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1592:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else
1593:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
1594:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Timeout management */
1595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout
1596:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
1597:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             /* Call standard close procedure with error check */
1598:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             SPI_CloseTransfer(hspi);
1599:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1600:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_TIMEOUT);
1601:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             hspi->State = HAL_SPI_STATE_READY;
1602:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1603:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             /* Unlock the process */
1604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             __HAL_UNLOCK(hspi);
1605:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1606:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             return HAL_TIMEOUT;
1607:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
1608:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
1609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
1610:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
1611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1612:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1613:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Wait for Tx/Rx (and CRC) data to be sent/received */
1614:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (SPI_WaitOnFlagUntilTimeout(hspi, SPI_FLAG_EOT, RESET, Timeout, tickstart) != HAL_OK)
1615:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1616:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
1617:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1618:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1619:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Call standard close procedure with error check */
1620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_CloseTransfer(hspi);
1621:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1622:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
1623:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1624:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Unlock the process */
1625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1626:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1627:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 30


1628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1629:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
1630:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1631:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1632:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1633:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_OK;
1634:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1635:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
1636:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1637:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
1638:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Transmit an amount of data in non-blocking mode with Interrupt.
1639:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi : pointer to a SPI_HandleTypeDef structure that contains
1640:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                the configuration information for SPI module.
1641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pData: pointer to data buffer
1642:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Size : amount of data to be sent
1643:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
1644:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
1645:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Transmit_IT(SPI_HandleTypeDef *hspi, const uint8_t *pData, uint16_t Size)
1646:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
1647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
1648:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES_OR_1LINE_2LINES_TXONLY(hspi->Init.Direction));
1649:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1650:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0UL))
1651:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1652:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
1653:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1654:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1655:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1656:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1657:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_BUSY;
1658:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1659:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1660:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Lock the process */
1661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_LOCK(hspi);
1662:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1663:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the transaction information */
1664:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_TX;
1665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1666:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pData;
1667:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
1668:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
1669:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1670:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Init field not used in handle to zero */
1671:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = NULL;
1672:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = (uint16_t) 0UL;
1673:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t) 0UL;
1674:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
1675:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1676:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
1677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->Reload.Requested   = 0UL;
1678:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->Reload.pTxBuffPtr  = NULL;
1679:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->Reload.TxXferSize  = NULL;
1680:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
1681:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1682:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the function for IT treatment */
1683:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_16BIT)
1684:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 31


1685:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxISR = SPI_TxISR_32BIT;
1686:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1687:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1688:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1689:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxISR = SPI_TxISR_16BIT;
1690:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1691:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1692:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1693:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxISR = SPI_TxISR_8BIT;
1694:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1695:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1696:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Configure communication direction : 1Line */
1697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
1698:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1699:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
1700:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1701:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1702:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1703:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_2LINES_TX(hspi);
1704:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1705:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1706:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the number of data at current transfer */
1707:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSIZE, Size);
1708:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1709:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable SPI peripheral */
1710:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE(hspi);
1711:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1712:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Unlock the process */
1713:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1714:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1715:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable EOT, TXP, FRE, MODF, UDR and TSERF interrupts */
1716:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_EOT | SPI_IT_TXP | SPI_IT_UDR | SPI_IT_FRE | SPI_IT_MODF | SPI_
1717:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Mode == SPI_MODE_MASTER)
1719:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1720:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Master transfer start */
1721:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CSTART);
1722:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1723:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return HAL_OK;
1725:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
1726:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1727:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
1728:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Receive an amount of data in non-blocking mode with Interrupt.
1729:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi : pointer to a SPI_HandleTypeDef structure that contains
1730:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                the configuration information for SPI module.
1731:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pData: pointer to data buffer
1732:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Size : amount of data to be sent
1733:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
1734:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
1735:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Receive_IT(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size)
1736:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
1737:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
1738:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES_OR_1LINE_2LINES_RXONLY(hspi->Init.Direction));
1739:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1740:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1741:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 32


1742:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_BUSY;
1743:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1744:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1745:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0UL))
1746:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1747:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
1748:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1749:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1750:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Lock the process */
1751:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_LOCK(hspi);
1752:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1753:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the transaction information */
1754:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_RX;
1755:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1756:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
1757:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
1758:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
1759:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Init field not used in handle to zero */
1761:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = NULL;
1762:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = (uint16_t) 0UL;
1763:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t) 0UL;
1764:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
1765:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1766:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
1767:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->Reload.Requested   = 0UL;
1768:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->Reload.pRxBuffPtr  = NULL;
1769:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->Reload.RxXferSize  = NULL;
1770:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
1771:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1772:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the function for IT treatment */
1773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_16BIT)
1774:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1775:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_32BIT;
1776:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1777:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1778:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1779:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_16BIT;
1780:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1781:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1782:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1783:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_8BIT;
1784:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1785:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1786:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Configure communication direction : 1Line */
1787:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
1788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1789:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
1790:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1791:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1792:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1793:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_2LINES_RX(hspi);
1794:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1795:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1796:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Note : The SPI must be enabled after unlocking current process
1797:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             to avoid the risk of SPI interrupt handle execution before current
1798:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             process unlock */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 33


1799:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1800:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the number of data at current transfer */
1801:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSIZE, Size);
1802:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1803:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable SPI peripheral */
1804:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE(hspi);
1805:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1806:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Unlock the process */
1807:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1808:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1809:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable EOT, RXP, OVR, FRE, MODF and TSERF interrupts */
1810:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_EOT | SPI_IT_RXP | SPI_IT_OVR | SPI_IT_FRE | SPI_IT_MODF | SPI_
1811:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1812:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Mode == SPI_MODE_MASTER)
1813:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1814:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Master transfer start */
1815:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CSTART);
1816:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1817:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1818:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return HAL_OK;
1819:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
1820:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1821:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
1822:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Transmit and Receive an amount of data in non-blocking mode with Interrupt.
1823:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi   : pointer to a SPI_HandleTypeDef structure that contains
1824:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                  the configuration information for SPI module.
1825:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pTxData: pointer to transmission data buffer
1826:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pRxData: pointer to reception data buffer
1827:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Size   : amount of data to be sent and received
1828:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
1829:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
1830:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_TransmitReceive_IT(SPI_HandleTypeDef *hspi, const uint8_t *pTxData, uint8
1831:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                              uint16_t Size)
1832:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
1833:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t tmp_TxXferCount;
1834:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
1835:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint16_t *ptxdr_16bits = (__IO uint16_t *)(&(hspi->Instance->TXDR));
1836:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
1837:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
1839:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES(hspi->Init.Direction));
1840:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1841:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1842:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1843:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_BUSY;
1844:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1845:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1846:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((pTxData == NULL) || (pRxData == NULL) || (Size == 0UL))
1847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1848:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
1849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1850:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1851:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Lock the process */
1852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_LOCK(hspi);
1853:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1854:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the transaction information */
1855:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_TX_RX;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 34


1856:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pTxData;
1858:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
1859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
1860:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
1861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
1862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
1863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   tmp_TxXferCount   = hspi->TxXferCount;
1864:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
1866:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->Reload.Requested   = 0UL;
1867:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->Reload.pRxBuffPtr  = NULL;
1868:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->Reload.RxXferSize  = NULL;
1869:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->Reload.pTxBuffPtr  = NULL;
1870:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->Reload.TxXferSize  = NULL;
1871:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
1872:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1873:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the function for IT treatment */
1874:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_16BIT)
1875:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1876:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxISR     = SPI_TxISR_32BIT;
1877:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR     = SPI_RxISR_32BIT;
1878:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1879:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1880:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR     = SPI_RxISR_16BIT;
1882:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxISR     = SPI_TxISR_16BIT;
1883:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1884:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1885:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1886:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR     = SPI_RxISR_8BIT;
1887:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxISR     = SPI_TxISR_8BIT;
1888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1889:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1890:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set Full-Duplex mode */
1891:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_2LINES(hspi);
1892:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1893:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the number of data at current transfer */
1894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSIZE, Size);
1895:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1896:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable SPI peripheral */
1897:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE(hspi);
1898:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1899:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Fill in the TxFIFO */
1900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   while ((__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXP)) && (tmp_TxXferCount != 0UL))
1901:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1902:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Transmit data in 32 Bit mode */
1903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->Init.DataSize > SPI_DATASIZE_16BIT)
1904:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
1905:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       *((__IO uint32_t *)&hspi->Instance->TXDR) = *((const uint32_t *)hspi->pTxBuffPtr);
1906:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint32_t);
1907:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount--;
1908:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       tmp_TxXferCount = hspi->TxXferCount;
1909:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
1910:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Transmit data in 16 Bit mode */
1911:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1912:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 35


1913:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
1914:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       *ptxdr_16bits = *((const uint16_t *)hspi->pTxBuffPtr);
1915:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
1916:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       *((__IO uint16_t *)&hspi->Instance->TXDR) = *((const uint16_t *)hspi->pTxBuffPtr);
1917:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
1918:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
1919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount--;
1920:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       tmp_TxXferCount = hspi->TxXferCount;
1921:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
1922:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Transmit data in 8 Bit mode */
1923:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
1924:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
1925:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       *((__IO uint8_t *)&hspi->Instance->TXDR) = *((const uint8_t *)hspi->pTxBuffPtr);
1926:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint8_t);
1927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount--;
1928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       tmp_TxXferCount = hspi->TxXferCount;
1929:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
1930:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1931:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1932:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Unlock the process */
1933:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1934:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1935:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable EOT, DXP, UDR, OVR, FRE, MODF and TSERF interrupts */
1936:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_EOT | SPI_IT_DXP | SPI_IT_UDR | SPI_IT_OVR |
1937:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                              SPI_IT_FRE | SPI_IT_MODF | SPI_IT_TSERF));
1938:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1939:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Mode == SPI_MODE_MASTER)
1940:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1941:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Start Master transfer */
1942:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CSTART);
1943:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1944:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1945:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return HAL_OK;
1946:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
1947:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1948:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
1949:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
1950:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Transmit an additional amount of data in blocking mode.
1951:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi : pointer to a SPI_HandleTypeDef structure that contains
1952:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                the configuration information for SPI module.
1953:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pData: pointer to data buffer
1954:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Size : amount of data to be sent
1955:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
1956:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
1957:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Reload_Transmit_IT(SPI_HandleTypeDef *hspi, const uint8_t *pData, uint16_
1958:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
1959:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* check if there is already a request to reload */
1960:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((hspi->Reload.Requested == 1UL) || (pData == NULL) || (Size == 0UL))
1961:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1962:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
1963:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1964:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1965:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State == HAL_SPI_STATE_BUSY_TX)
1966:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1967:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Lock the process */
1968:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_LOCK(hspi);
1969:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 36


1970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Insert the new number of data to be sent just after the current one */
1971:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSER, (Size & 0xFFFFFFFFUL) << 16UL);
1972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1973:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Set the transaction information */
1974:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->Reload.Requested   = 1UL;
1975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->Reload.pTxBuffPtr  = (const uint8_t *)pData;
1976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->Reload.TxXferSize  = Size;
1977:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1978:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Unlock the process */
1979:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_UNLOCK(hspi);
1980:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1981:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_OK;
1982:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1983:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
1984:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
1985:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
1986:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
1987:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
1988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
1989:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
1990:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
1991:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
1992:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Receive an additional amount of data in blocking mode.
1993:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi : pointer to a SPI_HandleTypeDef structure that contains
1994:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                the configuration information for SPI module.
1995:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pData: pointer to data buffer
1996:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Size : amount of data to be sent
1997:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
1998:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
1999:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Reload_Receive_IT(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size)
2000:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
2001:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* check if there is already a request to reload */
2002:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((hspi->Reload.Requested == 1UL) || (pData == NULL) || (Size == 0UL))
2003:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2004:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2005:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2006:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2007:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State == HAL_SPI_STATE_BUSY_RX)
2008:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2009:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Lock the process */
2010:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_LOCK(hspi);
2011:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2012:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Insert the new number of data that will be received just after the current one */
2013:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSER, (Size & 0xFFFFFFFFUL) << 16UL);
2014:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2015:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Set the transaction information */
2016:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->Reload.Requested   = 1UL;
2017:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->Reload.pRxBuffPtr  = (uint8_t *)pData;
2018:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->Reload.RxXferSize  = Size;
2019:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2020:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Unlock the process */
2021:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_UNLOCK(hspi);
2022:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2023:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_OK;
2024:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2025:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
2026:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 37


2027:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2028:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2029:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
2030:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
2031:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2032:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
2033:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
2034:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Transmit and receive an additional amount of data in blocking mode.
2035:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi   : pointer to a SPI_HandleTypeDef structure that contains
2036:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                  the configuration information for SPI module.
2037:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pTxData: pointer to transmission data buffer
2038:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pRxData: pointer to reception data buffer
2039:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Size   : amount of data to be sent and received
2040:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
2041:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
2042:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Reload_TransmitReceive_IT(SPI_HandleTypeDef *hspi, const uint8_t *pTxData
2043:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                     uint8_t *pRxData, uint16_t Size)
2044:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
2045:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* check if there is already a request to reload */
2046:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((hspi->Reload.Requested == 1UL) || (pTxData == NULL) || (pRxData == NULL) || (Size == 0UL))
2047:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2048:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2049:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2050:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2051:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State == HAL_SPI_STATE_BUSY_TX_RX)
2052:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2053:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Lock the process */
2054:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_LOCK(hspi);
2055:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2056:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Insert the new number of data that will be sent and received just after the current one */
2057:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSER, (Size & 0xFFFFFFFFUL) << 16UL);
2058:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2059:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Set the transaction information */
2060:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->Reload.Requested   = 1UL;
2061:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->Reload.pTxBuffPtr  = (const uint8_t *)pTxData;
2062:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->Reload.TxXferSize  = Size;
2063:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->Reload.pRxBuffPtr  = (uint8_t *)pRxData;
2064:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->Reload.RxXferSize  = Size;
2065:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2066:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Unlock the process */
2067:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_UNLOCK(hspi);
2068:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2069:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_OK;
2070:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2071:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
2072:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2073:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2074:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2075:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
2076:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
2077:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2078:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
2079:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Transmit an amount of data in non-blocking mode with DMA.
2080:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi : pointer to a SPI_HandleTypeDef structure that contains
2081:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                the configuration information for SPI module.
2082:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pData: pointer to data buffer
2083:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Size : amount of data to be sent
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 38


2084:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
2085:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
2086:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Transmit_DMA(SPI_HandleTypeDef *hspi, const uint8_t *pData, uint16_t Size
2087:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
2088:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2089:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
2090:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES_OR_1LINE_2LINES_TXONLY(hspi->Init.Direction));
2091:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2092:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
2093:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2094:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_BUSY;
2095:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2096:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2097:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0UL))
2098:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2099:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2100:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2101:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2102:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Lock the process */
2103:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_LOCK(hspi);
2104:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2105:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the transaction information */
2106:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_TX;
2107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
2108:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pData;
2109:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
2110:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
2111:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2112:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Init field not used in handle to zero */
2113:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = NULL;
2114:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
2115:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
2116:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = (uint16_t)0UL;
2117:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t)0UL;
2118:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2119:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Configure communication direction : 1Line */
2120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
2121:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2122:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
2123:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2124:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
2125:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2126:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_2LINES_TX(hspi);
2127:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2128:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2129:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Packing mode management is enabled by the DMA settings */
2130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (((hspi->Init.DataSize > SPI_DATASIZE_16BIT) && (hspi->hdmatx->Init.MemDataAlignment != DMA_MD
2131:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmatx->Init.MemDataAlignment != DMA_MD
2132:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                      (hspi->hdmatx->Init.MemDataAlignment != DMA_MD
2133:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2134:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Restriction the DMA data received is not allowed in this mode */
2135:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_UNLOCK(hspi);
2136:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2137:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2138:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Adjust XferCount according to DMA alignment / Data size */
2140:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.DataSize <= SPI_DATASIZE_8BIT)
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 39


2141:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2142:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmatx->Init.MemDataAlignment == DMA_MDATAALIGN_HALFWORD)
2143:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2144:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount + (uint16_t) 1UL) >> 1UL;
2145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2146:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmatx->Init.MemDataAlignment == DMA_MDATAALIGN_WORD)
2147:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount + (uint16_t) 3UL) >> 2UL;
2149:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2150:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2151:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else if (hspi->Init.DataSize <= SPI_DATASIZE_16BIT)
2152:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2153:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmatx->Init.MemDataAlignment == DMA_MDATAALIGN_WORD)
2154:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2155:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount + (uint16_t) 1UL) >> 1UL;
2156:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2157:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2158:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
2159:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2160:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Adjustment done */
2161:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2162:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2163:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the SPI TxDMA Half transfer complete callback */
2164:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferHalfCpltCallback = SPI_DMAHalfTransmitCplt;
2165:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2166:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the SPI TxDMA transfer complete callback */
2167:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback = SPI_DMATransmitCplt;
2168:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2169:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the DMA error callback */
2170:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferErrorCallback = SPI_DMAError;
2171:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2172:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the DMA AbortCpltCallback */
2173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback = NULL;
2174:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2175:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Clear TXDMAEN bit*/
2176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CFG1, SPI_CFG1_TXDMAEN);
2177:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2178:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable the Tx DMA Stream/Channel */
2179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_OK != HAL_DMA_Start_IT(hspi->hdmatx, (uint32_t)hspi->pTxBuffPtr, (uint32_t)&hspi->Instanc
2180:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->TxXferCount))
2181:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2182:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Update SPI error code */
2183:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2184:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
2185:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2186:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Unlock the process */
2187:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_UNLOCK(hspi);
2188:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2189:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2190:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2191:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2192:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the number of data at current transfer */
2193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->hdmatx->Init.Mode == DMA_CIRCULAR)
2194:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2195:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSIZE, 0UL);
2196:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2197:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 40


2198:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2199:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSIZE, Size);
2200:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2201:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2202:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable Tx DMA Request */
2203:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SET_BIT(hspi->Instance->CFG1, SPI_CFG1_TXDMAEN);
2204:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2205:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable the SPI Error Interrupt Bit */
2206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_UDR | SPI_IT_FRE | SPI_IT_MODF));
2207:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2208:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable SPI peripheral */
2209:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE(hspi);
2210:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2211:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Mode == SPI_MODE_MASTER)
2212:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2213:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Master transfer start */
2214:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CSTART);
2215:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2216:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2217:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Unlock the process */
2218:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
2219:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return HAL_OK;
2221:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
2222:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2223:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
2224:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Receive an amount of data in non-blocking mode with DMA.
2225:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi : pointer to a SPI_HandleTypeDef structure that contains
2226:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                the configuration information for SPI module.
2227:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pData: pointer to data buffer
2228:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Size : amount of data to be sent
2229:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @note   When the CRC feature is enabled the pData Length must be Size + 1.
2230:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
2231:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
2232:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Receive_DMA(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size)
2233:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
2234:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2235:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
2236:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES_OR_1LINE_2LINES_RXONLY(hspi->Init.Direction));
2237:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2238:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
2240:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_UNLOCK(hspi);
2242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_BUSY;
2243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2244:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2245:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0UL))
2246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_UNLOCK(hspi);
2248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2249:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2250:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2251:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Lock the process */
2252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_LOCK(hspi);
2253:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2254:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the transaction information */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 41


2255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_RX;
2256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
2257:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
2258:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
2259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
2260:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /*Init field not used in handle to zero */
2262:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
2263:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
2264:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = (uint16_t) 0UL;
2265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t) 0UL;
2266:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2267:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Configure communication direction : 1Line */
2268:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
2269:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2270:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
2271:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2272:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
2273:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2274:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_2LINES_RX(hspi);
2275:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2276:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2277:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Packing mode management is enabled by the DMA settings */
2278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (((hspi->Init.DataSize > SPI_DATASIZE_16BIT) && (hspi->hdmarx->Init.MemDataAlignment != DMA_MD
2279:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
2280:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                      (hspi->hdmarx->Init.MemDataAlignment != DMA_MD
2281:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2282:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Restriction the DMA data received is not allowed in this mode */
2283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_UNLOCK(hspi);
2284:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2285:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2286:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2287:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Clear RXDMAEN bit */
2288:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CFG1, SPI_CFG1_RXDMAEN);
2289:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2290:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Adjust XferCount according to DMA alignment / Data size */
2291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.DataSize <= SPI_DATASIZE_8BIT)
2292:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmarx->Init.MemDataAlignment == DMA_MDATAALIGN_HALFWORD)
2294:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxXferCount = (hspi->RxXferCount + (uint16_t) 1UL) >> 1UL;
2296:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2297:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmarx->Init.MemDataAlignment == DMA_MDATAALIGN_WORD)
2298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2299:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxXferCount = (hspi->RxXferCount + (uint16_t) 3UL) >> 2UL;
2300:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2301:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2302:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else if (hspi->Init.DataSize <= SPI_DATASIZE_16BIT)
2303:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmarx->Init.MemDataAlignment == DMA_MDATAALIGN_WORD)
2305:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxXferCount = (hspi->RxXferCount + (uint16_t) 1UL) >> 1UL;
2307:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2308:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2309:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
2310:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2311:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Adjustment done */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 42


2312:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2313:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2314:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the SPI RxDMA Half transfer complete callback */
2315:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmarx->XferHalfCpltCallback = SPI_DMAHalfReceiveCplt;
2316:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2317:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the SPI Rx DMA transfer complete callback */
2318:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmarx->XferCpltCallback = SPI_DMAReceiveCplt;
2319:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2320:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the DMA error callback */
2321:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmarx->XferErrorCallback = SPI_DMAError;
2322:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2323:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the DMA AbortCpltCallback */
2324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmarx->XferAbortCallback = NULL;
2325:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2326:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable the Rx DMA Stream/Channel  */
2327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_OK != HAL_DMA_Start_IT(hspi->hdmarx, (uint32_t)&hspi->Instance->RXDR, (uint32_t)hspi->pRx
2328:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->RxXferCount))
2329:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2330:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Update SPI error code */
2331:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
2333:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2334:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Unlock the process */
2335:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_UNLOCK(hspi);
2336:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2337:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2338:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2339:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2340:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the number of data at current transfer */
2341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->hdmarx->Init.Mode == DMA_CIRCULAR)
2342:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2343:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSIZE, 0UL);
2344:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2345:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
2346:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSIZE, Size);
2348:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2349:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2350:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable Rx DMA Request */
2351:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SET_BIT(hspi->Instance->CFG1, SPI_CFG1_RXDMAEN);
2352:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2353:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable the SPI Error Interrupt Bit */
2354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_OVR | SPI_IT_FRE | SPI_IT_MODF));
2355:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2356:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable SPI peripheral */
2357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE(hspi);
2358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2359:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Mode == SPI_MODE_MASTER)
2360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2361:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Master transfer start */
2362:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CSTART);
2363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2364:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2365:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Unlock the process */
2366:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
2367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return HAL_OK;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 43


2369:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
2370:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2371:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
2372:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Transmit and Receive an amount of data in non-blocking mode with DMA.
2373:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi   : pointer to a SPI_HandleTypeDef structure that contains
2374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *                  the configuration information for SPI module.
2375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pTxData: pointer to transmission data buffer
2376:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  pRxData: pointer to reception data buffer
2377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  Size   : amount of data to be sent
2378:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @note   When the CRC feature is enabled the pRxData Length must be Size + 1
2379:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
2380:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
2381:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_TransmitReceive_DMA(SPI_HandleTypeDef *hspi, const uint8_t *pTxData, uint
2382:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                               uint16_t Size)
2383:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
2384:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
2385:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES(hspi->Init.Direction));
2386:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2387:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
2388:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2389:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_BUSY;
2390:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2391:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2392:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((pTxData == NULL) || (pRxData == NULL) || (Size == 0UL))
2393:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2394:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2395:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2397:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Lock the process */
2398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_LOCK(hspi);
2399:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2400:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the transaction information */
2401:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_TX_RX;
2402:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
2403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pTxData;
2404:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
2405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
2406:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
2407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
2408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
2409:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2410:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Init field not used in handle to zero */
2411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
2412:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
2413:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2414:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set Full-Duplex mode */
2415:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_2LINES(hspi);
2416:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2417:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Reset the Tx/Rx DMA bits */
2418:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CFG1, SPI_CFG1_TXDMAEN | SPI_CFG1_RXDMAEN);
2419:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Packing mode management is enabled by the DMA settings */
2421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (((hspi->Init.DataSize > SPI_DATASIZE_16BIT) && (hspi->hdmarx->Init.MemDataAlignment != DMA_MD
2422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
2423:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                      (hspi->hdmarx->Init.MemDataAlignment != DMA_MD
2424:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2425:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Restriction the DMA data received is not allowed in this mode */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 44


2426:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Unlock the process */
2427:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_UNLOCK(hspi);
2428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2429:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2430:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2431:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Adjust XferCount according to DMA alignment / Data size */
2432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.DataSize <= SPI_DATASIZE_8BIT)
2433:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2434:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmatx->Init.MemDataAlignment == DMA_MDATAALIGN_HALFWORD)
2435:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount + (uint16_t) 1UL) >> 1UL;
2437:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2438:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmatx->Init.MemDataAlignment == DMA_MDATAALIGN_WORD)
2439:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2440:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount + (uint16_t) 3UL) >> 2UL;
2441:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2442:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmarx->Init.MemDataAlignment == DMA_MDATAALIGN_HALFWORD)
2443:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxXferCount = (hspi->RxXferCount + (uint16_t) 1UL) >> 1UL;
2445:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2446:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmarx->Init.MemDataAlignment == DMA_MDATAALIGN_WORD)
2447:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2448:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxXferCount = (hspi->RxXferCount + (uint16_t) 3UL) >> 2UL;
2449:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2450:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2451:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else if (hspi->Init.DataSize <= SPI_DATASIZE_16BIT)
2452:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmatx->Init.MemDataAlignment == DMA_MDATAALIGN_WORD)
2454:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2455:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount + (uint16_t) 1UL) >> 1UL;
2456:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmarx->Init.MemDataAlignment == DMA_MDATAALIGN_WORD)
2458:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxXferCount = (hspi->RxXferCount + (uint16_t) 1UL) >> 1UL;
2460:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2461:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
2463:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2464:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Adjustment done */
2465:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2466:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2467:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the SPI Tx/Rx DMA Half transfer complete callback */
2468:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmarx->XferHalfCpltCallback = SPI_DMAHalfTransmitReceiveCplt;
2469:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmarx->XferCpltCallback     = SPI_DMATransmitReceiveCplt;
2470:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2471:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the DMA error callback */
2472:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmarx->XferErrorCallback = SPI_DMAError;
2473:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2474:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the DMA AbortCallback */
2475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmarx->XferAbortCallback = NULL;
2476:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2477:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable the Rx DMA Stream/Channel  */
2478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_OK != HAL_DMA_Start_IT(hspi->hdmarx, (uint32_t)&hspi->Instance->RXDR, (uint32_t)hspi->pRx
2479:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->RxXferCount))
2480:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Update SPI error code */
2482:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 45


2483:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
2484:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Unlock the process */
2486:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_UNLOCK(hspi);
2487:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2488:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2489:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2490:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2491:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable Rx DMA Request */
2492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SET_BIT(hspi->Instance->CFG1, SPI_CFG1_RXDMAEN);
2493:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2494:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the SPI Tx DMA transfer complete callback as NULL because the communication closing
2495:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   is performed in DMA reception complete callback  */
2496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferHalfCpltCallback = NULL;
2497:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback     = NULL;
2498:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback    = NULL;
2499:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set the DMA error callback */
2501:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferErrorCallback    = SPI_DMAError;
2502:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2503:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable the Tx DMA Stream/Channel  */
2504:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_OK != HAL_DMA_Start_IT(hspi->hdmatx, (uint32_t)hspi->pTxBuffPtr, (uint32_t)&hspi->Instanc
2505:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->TxXferCount))
2506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Abort Rx DMA Channel already started */
2508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     (void)HAL_DMA_Abort(hspi->hdmarx);
2509:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2510:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Update SPI error code */
2511:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
2513:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2514:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Unlock the process */
2515:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_UNLOCK(hspi);
2516:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2517:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
2518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->hdmatx->Init.Mode == DMA_CIRCULAR)
2521:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2522:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSIZE, 0UL);
2523:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2524:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
2525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2526:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     MODIFY_REG(hspi->Instance->CR2, SPI_CR2_TSIZE, Size);
2527:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2528:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2529:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable Tx DMA Request */
2530:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SET_BIT(hspi->Instance->CFG1, SPI_CFG1_TXDMAEN);
2531:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2532:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable the SPI Error Interrupt Bit */
2533:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_OVR | SPI_IT_UDR | SPI_IT_FRE | SPI_IT_MODF));
2534:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2535:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Enable SPI peripheral */
2536:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_ENABLE(hspi);
2537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2538:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.Mode == SPI_MODE_MASTER)
2539:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 46


2540:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Master transfer start */
2541:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CSTART);
2542:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2543:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2544:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Unlock the process */
2545:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
2546:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2547:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return HAL_OK;
2548:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
2549:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2550:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
2551:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Abort ongoing transfer (blocking mode).
2552:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi SPI handle.
2553:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @note   This procedure could be used for aborting any ongoing transfer (Tx and Rx),
2554:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         started in Interrupt or DMA mode.
2555:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @note   This procedure performs following operations :
2556:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *          + Disable SPI Interrupts (depending of transfer direction)
2557:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *          + Disable the DMA transfer in the peripheral register (if enabled)
2558:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *          + Abort DMA transfer by calling HAL_DMA_Abort (in case of transfer in DMA mode)
2559:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *          + Set handle State to READY.
2560:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @note   This procedure is executed in blocking mode : when exiting function, Abort is considere
2561:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
2562:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
2563:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Abort(SPI_HandleTypeDef *hspi)
2564:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
2565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
2566:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2567:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint32_t count;
2568:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2569:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Lock the process */
2570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_LOCK(hspi);
2571:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2572:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set hspi->state to aborting to avoid any interaction */
2573:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_ABORT;
2574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2575:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Initialized local variable  */
2576:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   errorcode = HAL_OK;
2577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   count = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24UL / 1000UL);
2578:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2579:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* If master communication on going, make sure current frame is done before closing the connectio
2580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR1, SPI_CR1_CSTART))
2581:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2582:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Disable EOT interrupt */
2583:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_EOT);
2584:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     do
2585:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2586:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       count--;
2587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
2588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
2589:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
2591:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
2592:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     } while (HAL_IS_BIT_SET(hspi->Instance->IER, SPI_IT_EOT));
2593:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2594:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Request a Suspend transfer */
2595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CSUSP);
2596:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     do
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 47


2597:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2598:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       count--;
2599:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
2600:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
2601:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2602:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
2603:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
2604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     } while (HAL_IS_BIT_SET(hspi->Instance->CR1, SPI_CR1_CSTART));
2605:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2606:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Clear SUSP flag */
2607:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_CLEAR_SUSPFLAG(hspi);
2608:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     do
2609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2610:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       count--;
2611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
2612:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
2613:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2614:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
2615:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
2616:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     } while (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_SUSP));
2617:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2618:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2619:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable the SPI DMA Tx request if enabled */
2620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CFG1, SPI_CFG1_TXDMAEN))
2621:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2622:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmatx != NULL)
2623:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2624:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Abort the SPI DMA Tx Stream/Channel : use blocking DMA Abort API (no callback) */
2625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->hdmatx->XferAbortCallback = NULL;
2626:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2627:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Abort DMA Tx Handle linked to SPI Peripheral */
2628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (HAL_DMA_Abort(hspi->hdmatx) != HAL_OK)
2629:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
2630:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if (HAL_DMA_GetError(hspi->hdmatx) == HAL_DMA_ERROR_TIMEOUT)
2631:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
2632:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2633:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
2634:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
2635:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2636:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2637:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2638:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable the SPI DMA Rx request if enabled */
2639:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CFG1, SPI_CFG1_RXDMAEN))
2640:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmarx != NULL)
2642:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2643:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Abort the SPI DMA Rx Stream/Channel : use blocking DMA Abort API (no callback) */
2644:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->hdmarx->XferAbortCallback = NULL;
2645:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2646:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Abort DMA Rx Handle linked to SPI Peripheral */
2647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (HAL_DMA_Abort(hspi->hdmarx) != HAL_OK)
2648:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
2649:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if (HAL_DMA_GetError(hspi->hdmarx) == HAL_DMA_ERROR_TIMEOUT)
2650:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
2651:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2652:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
2653:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 48


2654:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2655:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2656:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2657:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Proceed with abort procedure */
2658:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_AbortTransfer(hspi);
2659:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2660:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check error during Abort procedure */
2661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->ErrorCode, HAL_SPI_ERROR_ABORT))
2662:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2663:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* return HAL_Error in case of error during Abort procedure */
2664:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     errorcode = HAL_ERROR;
2665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2666:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   else
2667:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2668:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Reset errorCode */
2669:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_NONE;
2670:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2671:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2672:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Restore hspi->state to ready */
2673:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
2674:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2675:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Unlock the process */
2676:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
2677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2678:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return errorcode;
2679:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
2680:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2681:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
2682:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Abort ongoing transfer (Interrupt mode).
2683:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi SPI handle.
2684:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @note   This procedure could be used for aborting any ongoing transfer (Tx and Rx),
2685:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         started in Interrupt or DMA mode.
2686:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @note   This procedure performs following operations :
2687:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *          + Disable SPI Interrupts (depending of transfer direction)
2688:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *          + Disable the DMA transfer in the peripheral register (if enabled)
2689:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *          + Abort DMA transfer by calling HAL_DMA_Abort_IT (in case of transfer in DMA mode)
2690:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *          + Set handle State to READY
2691:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *          + At abort completion, call user abort complete callback.
2692:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @note   This procedure is executed in Interrupt mode, meaning that abort procedure could be
2693:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         considered as completed only when user abort complete callback is executed (not when ex
2694:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
2695:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
2696:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Abort_IT(SPI_HandleTypeDef *hspi)
2697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
2698:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
2699:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint32_t count;
2700:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t dma_tx_abort_done = 1UL;
2701:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t dma_rx_abort_done = 1UL;
2702:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2703:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set hspi->state to aborting to avoid any interaction */
2704:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_ABORT;
2705:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2706:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Initialized local variable  */
2707:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   errorcode = HAL_OK;
2708:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   count = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24UL / 1000UL);
2709:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2710:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* If master communication on going, make sure current frame is done before closing the connectio
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 49


2711:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR1, SPI_CR1_CSTART))
2712:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2713:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Disable EOT interrupt */
2714:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_EOT);
2715:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     do
2716:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2717:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       count--;
2718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
2719:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
2720:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2721:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
2722:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
2723:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     } while (HAL_IS_BIT_SET(hspi->Instance->IER, SPI_IT_EOT));
2724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2725:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Request a Suspend transfer */
2726:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CSUSP);
2727:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     do
2728:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2729:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       count--;
2730:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
2731:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
2732:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2733:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
2734:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
2735:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     } while (HAL_IS_BIT_SET(hspi->Instance->CR1, SPI_CR1_CSTART));
2736:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2737:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Clear SUSP flag */
2738:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_CLEAR_SUSPFLAG(hspi);
2739:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     do
2740:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2741:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       count--;
2742:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
2743:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
2744:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2745:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
2746:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
2747:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     } while (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_SUSP));
2748:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2749:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2750:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* If DMA Tx and/or DMA Rx Handles are associated to SPI Handle, DMA Abort complete callbacks sho
2751:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****      before any call to DMA Abort functions */
2752:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2753:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->hdmatx != NULL)
2754:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2755:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (HAL_IS_BIT_SET(hspi->Instance->CFG1, SPI_CFG1_TXDMAEN))
2756:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2757:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Set DMA Abort Complete callback if SPI DMA Tx request if enabled */
2758:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->hdmatx->XferAbortCallback = SPI_DMATxAbortCallback;
2759:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       dma_tx_abort_done = 0UL;
2761:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2762:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Abort DMA Tx Handle linked to SPI Peripheral */
2763:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (HAL_DMA_Abort_IT(hspi->hdmatx) != HAL_OK)
2764:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
2765:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if (HAL_DMA_GetError(hspi->hdmatx) == HAL_DMA_ERROR_NO_XFER)
2766:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
2767:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           dma_tx_abort_done = 1UL;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 50


2768:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->hdmatx->XferAbortCallback = NULL;
2769:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
2770:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
2771:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2772:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
2773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2774:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->hdmatx->XferAbortCallback = NULL;
2775:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2776:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2777:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2778:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->hdmarx != NULL)
2779:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2780:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (HAL_IS_BIT_SET(hspi->Instance->CFG1, SPI_CFG1_RXDMAEN))
2781:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2782:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Set DMA Abort Complete callback if SPI DMA Rx request if enabled */
2783:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->hdmarx->XferAbortCallback = SPI_DMARxAbortCallback;
2784:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2785:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       dma_rx_abort_done = 0UL;
2786:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2787:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Abort DMA Rx Handle linked to SPI Peripheral */
2788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (HAL_DMA_Abort_IT(hspi->hdmarx) != HAL_OK)
2789:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
2790:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if (HAL_DMA_GetError(hspi->hdmarx) == HAL_DMA_ERROR_NO_XFER)
2791:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
2792:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           dma_rx_abort_done = 1UL;
2793:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->hdmarx->XferAbortCallback = NULL;
2794:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
2795:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
2796:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2797:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
2798:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2799:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->hdmarx->XferAbortCallback = NULL;
2800:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2801:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2802:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2803:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* If no running DMA transfer, finish cleanup and call callbacks */
2804:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((dma_tx_abort_done == 1UL) && (dma_rx_abort_done == 1UL))
2805:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2806:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Proceed with abort procedure */
2807:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_AbortTransfer(hspi);
2808:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2809:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Check error during Abort procedure */
2810:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (HAL_IS_BIT_SET(hspi->ErrorCode, HAL_SPI_ERROR_ABORT))
2811:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2812:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* return HAL_Error in case of error during Abort procedure */
2813:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       errorcode = HAL_ERROR;
2814:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2815:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
2816:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2817:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Reset errorCode */
2818:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->ErrorCode = HAL_SPI_ERROR_NONE;
2819:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2820:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2821:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Restore hspi->state to ready */
2822:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
2823:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2824:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Call user Abort complete callback */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 51


2825:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
2826:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->AbortCpltCallback(hspi);
2827:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
2828:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     HAL_SPI_AbortCpltCallback(hspi);
2829:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
2830:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2831:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2832:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return errorcode;
2833:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
2834:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2835:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
2836:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Pause the DMA Transfer.
2837:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         This API is not supported, it is maintained for backward compatibility.
2838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
2839:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for the specified SPI module.
2840:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL_ERROR
2841:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
2842:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_DMAPause(SPI_HandleTypeDef *hspi)
2843:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
2844:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set error code to not supported */
2845:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_NOT_SUPPORTED);
2846:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return HAL_ERROR;
2848:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
2849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2850:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
2851:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Resume the DMA Transfer.
2852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         This API is not supported, it is maintained for backward compatibility.
2853:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
2854:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for the specified SPI module.
2855:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL_ERROR
2856:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
2857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_DMAResume(SPI_HandleTypeDef *hspi)
2858:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
2859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set error code to not supported */
2860:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_NOT_SUPPORTED);
2861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return HAL_ERROR;
2863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
2864:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
2866:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Stop the DMA Transfer.
2867:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         This API is not supported, it is maintained for backward compatibility.
2868:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
2869:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for the specified SPI module.
2870:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL_ERROR
2871:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
2872:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_DMAStop(SPI_HandleTypeDef *hspi)
2873:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
2874:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set error code to not supported */
2875:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_NOT_SUPPORTED);
2876:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2877:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return HAL_ERROR;
2878:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
2879:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2880:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
2881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Handle SPI interrupt request.
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 52


2882:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
2883:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for the specified SPI module.
2884:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
2885:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
2886:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** void HAL_SPI_IRQHandler(SPI_HandleTypeDef *hspi)
2887:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
2888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t itsource = hspi->Instance->IER;
2889:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t itflag   = hspi->Instance->SR;
2890:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t trigger  = itsource & itflag;
2891:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t cfg1     = hspi->Instance->CFG1;
2892:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t handled  = 0UL;
2893:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_SPI_StateTypeDef State = hspi->State;
2895:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
2896:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint16_t *prxdr_16bits = (__IO uint16_t *)(&(hspi->Instance->RXDR));
2897:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
2898:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2899:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPI in SUSPEND mode  ----------------------------------------------------*/
2900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_IS_BIT_SET(itflag, SPI_FLAG_SUSP) && HAL_IS_BIT_SET(itsource, SPI_FLAG_EOT))
2901:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2902:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Clear the Suspend flag */
2903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_CLEAR_SUSPFLAG(hspi);
2904:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2905:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Suspend on going, Call the Suspend callback */
2906:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
2907:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->SuspendCallback(hspi);
2908:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
2909:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     HAL_SPI_SuspendCallback(hspi);
2910:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
2911:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return;
2912:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2913:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2914:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPI in mode Transmitter and Receiver ------------------------------------*/
2915:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_IS_BIT_CLR(trigger, SPI_FLAG_OVR) && HAL_IS_BIT_CLR(trigger, SPI_FLAG_UDR) && \
2916:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_IS_BIT_SET(trigger, SPI_FLAG_DXP))
2917:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2918:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxISR(hspi);
2919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR(hspi);
2920:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     handled = 1UL;
2921:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2922:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2923:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPI in mode Receiver ----------------------------------------------------*/
2924:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_IS_BIT_CLR(trigger, SPI_FLAG_OVR) && HAL_IS_BIT_SET(trigger, SPI_FLAG_RXP) && \
2925:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_IS_BIT_CLR(trigger, SPI_FLAG_DXP))
2926:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR(hspi);
2928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     handled = 1UL;
2929:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2930:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2931:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPI in mode Transmitter -------------------------------------------------*/
2932:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_IS_BIT_CLR(trigger, SPI_FLAG_UDR) && HAL_IS_BIT_SET(trigger, SPI_FLAG_TXP) && \
2933:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_IS_BIT_CLR(trigger, SPI_FLAG_DXP))
2934:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2935:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxISR(hspi);
2936:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     handled = 1UL;
2937:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2938:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 53


2939:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
2940:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPI Reload  -------------------------------------------------*/
2941:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_IS_BIT_SET(trigger, SPI_FLAG_TSERF))
2942:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2943:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_CLEAR_TSERFFLAG(hspi);
2944:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2945:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
2946:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2947:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (handled != 0UL)
2948:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2949:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return;
2950:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
2951:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2952:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPI End Of Transfer: DMA or IT based transfer */
2953:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_IS_BIT_SET(trigger, SPI_FLAG_EOT))
2954:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
2955:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Clear EOT/TXTF/SUSP flag */
2956:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_CLEAR_EOTFLAG(hspi);
2957:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_CLEAR_TXTFFLAG(hspi);
2958:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_CLEAR_SUSPFLAG(hspi);
2959:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2960:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Disable EOT interrupt */
2961:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_EOT);
2962:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2963:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* For the IT based receive extra polling maybe required for last packet */
2964:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (HAL_IS_BIT_CLR(hspi->Instance->CFG1, SPI_CFG1_TXDMAEN | SPI_CFG1_RXDMAEN))
2965:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
2966:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Pooling remaining data */
2967:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       while (hspi->RxXferCount != 0UL)
2968:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
2969:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Receive data in 32 Bit mode */
2970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if (hspi->Init.DataSize > SPI_DATASIZE_16BIT)
2971:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
2972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint32_t *)hspi->pRxBuffPtr) = *((__IO uint32_t *)&hspi->Instance->RXDR);
2973:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
2974:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
2975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Receive data in 16 Bit mode */
2976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
2977:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
2978:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
2979:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint16_t *)hspi->pRxBuffPtr) = *prxdr_16bits;
2980:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
2981:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint16_t *)hspi->pRxBuffPtr) = *((__IO uint16_t *)&hspi->Instance->RXDR);
2982:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
2983:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
2984:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
2985:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Receive data in 8 Bit mode */
2986:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         else
2987:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
2988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
2989:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
2990:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
2991:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2992:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
2993:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
2994:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
2995:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 54


2996:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Call SPI Standard close procedure */
2997:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_CloseTransfer(hspi);
2998:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
2999:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
3000:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
3001:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3002:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3003:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->ErrorCallback(hspi);
3004:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3005:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_SPI_ErrorCallback(hspi);
3006:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3007:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       return;
3008:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3009:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3010:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3011:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Call appropriate user callback */
3012:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (State == HAL_SPI_STATE_BUSY_TX_RX)
3013:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3014:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxRxCpltCallback(hspi);
3015:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3016:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else if (State == HAL_SPI_STATE_BUSY_RX)
3017:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3018:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxCpltCallback(hspi);
3019:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3020:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else if (State == HAL_SPI_STATE_BUSY_TX)
3021:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3022:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxCpltCallback(hspi);
3023:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3024:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3025:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Call appropriate user callback */
3026:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (State == HAL_SPI_STATE_BUSY_TX_RX)
3027:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3028:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_SPI_TxRxCpltCallback(hspi);
3029:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3030:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else if (State == HAL_SPI_STATE_BUSY_RX)
3031:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3032:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_SPI_RxCpltCallback(hspi);
3033:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3034:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else if (State == HAL_SPI_STATE_BUSY_TX)
3035:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3036:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_SPI_TxCpltCallback(hspi);
3037:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3038:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3039:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
3040:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3041:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* End of the appropriate call */
3042:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3043:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3044:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return;
3045:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3046:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3047:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPI in Error Treatment --------------------------------------------------*/
3048:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((trigger & (SPI_FLAG_MODF | SPI_FLAG_OVR | SPI_FLAG_FRE | SPI_FLAG_UDR)) != 0UL)
3049:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3050:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* SPI Overrun error interrupt occurred ----------------------------------*/
3051:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if ((trigger & SPI_FLAG_OVR) != 0UL)
3052:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 55


3053:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_OVR);
3054:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_CLEAR_OVRFLAG(hspi);
3055:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3056:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3057:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* SPI Mode Fault error interrupt occurred -------------------------------*/
3058:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if ((trigger & SPI_FLAG_MODF) != 0UL)
3059:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3060:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_MODF);
3061:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_CLEAR_MODFFLAG(hspi);
3062:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3063:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3064:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* SPI Frame error interrupt occurred ------------------------------------*/
3065:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if ((trigger & SPI_FLAG_FRE) != 0UL)
3066:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3067:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FRE);
3068:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_CLEAR_FREFLAG(hspi);
3069:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3070:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3071:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* SPI Underrun error interrupt occurred ------------------------------------*/
3072:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if ((trigger & SPI_FLAG_UDR) != 0UL)
3073:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3074:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_UDR);
3075:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_CLEAR_UDRFLAG(hspi);
3076:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3077:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3078:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
3079:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3080:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Disable SPI peripheral */
3081:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_DISABLE(hspi);
3082:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3083:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Disable all interrupts */
3084:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_EOT | SPI_IT_RXP | SPI_IT_TXP | SPI_IT_MODF |
3085:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                   SPI_IT_OVR | SPI_IT_FRE | SPI_IT_UDR));
3086:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3087:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Disable the SPI DMA requests if enabled */
3088:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (HAL_IS_BIT_SET(cfg1, SPI_CFG1_TXDMAEN | SPI_CFG1_RXDMAEN))
3089:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
3090:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Disable the SPI DMA requests */
3091:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         CLEAR_BIT(hspi->Instance->CFG1, SPI_CFG1_TXDMAEN | SPI_CFG1_RXDMAEN);
3092:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3093:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Abort the SPI DMA Rx channel */
3094:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if (hspi->hdmarx != NULL)
3095:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
3096:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Set the SPI DMA Abort callback :
3097:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           will lead to call HAL_SPI_ErrorCallback() at end of DMA abort procedure */
3098:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->hdmarx->XferAbortCallback = SPI_DMAAbortOnError;
3099:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmarx))
3100:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
3101:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
3102:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
3103:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
3104:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Abort the SPI DMA Tx channel */
3105:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         if (hspi->hdmatx != NULL)
3106:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
3107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           /* Set the SPI DMA Abort callback :
3108:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           will lead to call HAL_SPI_ErrorCallback() at end of DMA abort procedure */
3109:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->hdmatx->XferAbortCallback = SPI_DMAAbortOnError;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 56


3110:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmatx))
3111:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
3112:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
3113:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
3114:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
3115:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
3116:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       else
3117:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
3118:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Restore hspi->State to Ready */
3119:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
3120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3121:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         /* Call user error callback */
3122:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3123:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->ErrorCallback(hspi);
3124:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3125:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         HAL_SPI_ErrorCallback(hspi);
3126:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3127:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
3128:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3129:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return;
3130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3131:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3132:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3133:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3134:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief Tx Transfer completed callback.
3135:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3136:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3137:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3138:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** __weak void HAL_SPI_TxCpltCallback(SPI_HandleTypeDef *hspi) /* Derogation MISRAC2012-Rule-8.13 */
3140:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3141:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
3142:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   UNUSED(hspi);
3143:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3144:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
3145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             the HAL_SPI_TxCpltCallback should be implemented in the user file
3146:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****    */
3147:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3149:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3150:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief Rx Transfer completed callback.
3151:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3152:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3153:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3154:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3155:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** __weak void HAL_SPI_RxCpltCallback(SPI_HandleTypeDef *hspi) /* Derogation MISRAC2012-Rule-8.13 */
3156:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3157:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
3158:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   UNUSED(hspi);
3159:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3160:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
3161:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             the HAL_SPI_RxCpltCallback should be implemented in the user file
3162:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****    */
3163:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3164:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3165:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3166:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief Tx and Rx Transfer completed callback.
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 57


3167:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3168:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3169:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3170:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3171:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** __weak void HAL_SPI_TxRxCpltCallback(SPI_HandleTypeDef *hspi) /* Derogation MISRAC2012-Rule-8.13 */
3172:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
3174:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   UNUSED(hspi);
3175:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
3177:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             the HAL_SPI_TxRxCpltCallback should be implemented in the user file
3178:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****    */
3179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3180:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3181:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3182:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief Tx Half Transfer completed callback.
3183:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3184:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3185:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3186:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3187:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** __weak void HAL_SPI_TxHalfCpltCallback(SPI_HandleTypeDef *hspi) /* Derogation MISRAC2012-Rule-8.13 
3188:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3189:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
3190:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   UNUSED(hspi);
3191:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3192:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
3193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             the HAL_SPI_TxHalfCpltCallback should be implemented in the user file
3194:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****    */
3195:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3196:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3197:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3198:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief Rx Half Transfer completed callback.
3199:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3200:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3201:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3202:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3203:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** __weak void HAL_SPI_RxHalfCpltCallback(SPI_HandleTypeDef *hspi) /* Derogation MISRAC2012-Rule-8.13 
3204:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3205:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
3206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   UNUSED(hspi);
3207:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3208:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
3209:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             the HAL_SPI_RxHalfCpltCallback() should be implemented in the user file
3210:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****    */
3211:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3212:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3213:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3214:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief Tx and Rx Half Transfer callback.
3215:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3216:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3217:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3218:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3219:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** __weak void HAL_SPI_TxRxHalfCpltCallback(SPI_HandleTypeDef *hspi) /* Derogation MISRAC2012-Rule-8.1
3220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3221:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
3222:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   UNUSED(hspi);
3223:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 58


3224:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
3225:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             the HAL_SPI_TxRxHalfCpltCallback() should be implemented in the user file
3226:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****    */
3227:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3228:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3229:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3230:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief SPI error callback.
3231:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3232:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3233:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3234:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3235:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** __weak void HAL_SPI_ErrorCallback(SPI_HandleTypeDef *hspi) /* Derogation MISRAC2012-Rule-8.13 */
3236:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3237:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
3238:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   UNUSED(hspi);
3239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3240:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
3241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             the HAL_SPI_ErrorCallback should be implemented in the user file
3242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****    */
3243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* NOTE : The ErrorCode parameter in the hspi handle is updated by the SPI processes
3244:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             and user can use HAL_SPI_GetError() API to check the latest error occurred
3245:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****    */
3246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3249:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  SPI Abort Complete callback.
3250:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi SPI handle.
3251:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3253:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** __weak void HAL_SPI_AbortCpltCallback(SPI_HandleTypeDef *hspi) /* Derogation MISRAC2012-Rule-8.13 *
3254:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
3256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   UNUSED(hspi);
3257:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3258:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
3259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             the HAL_SPI_AbortCpltCallback can be implemented in the user file.
3260:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****    */
3261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3262:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3263:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3264:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  SPI Suspend callback.
3265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi SPI handle.
3266:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3267:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3268:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** __weak void HAL_SPI_SuspendCallback(SPI_HandleTypeDef *hspi) /* Derogation MISRAC2012-Rule-8.13 */
3269:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3270:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
3271:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   UNUSED(hspi);
3272:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3273:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
3274:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             the HAL_SPI_SuspendCallback can be implemented in the user file.
3275:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****    */
3276:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3277:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3279:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @}
3280:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 59


3281:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3282:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /** @defgroup SPI_Exported_Functions_Group3 Peripheral State and Errors functions
3283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief   SPI control functions
3284:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *
3285:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** @verbatim
3286:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****  ===============================================================================
3287:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                       ##### Peripheral State and Errors functions #####
3288:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****  ===============================================================================
3289:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     [..]
3290:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     This subsection provides a set of functions allowing to control the SPI.
3291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****      (+) HAL_SPI_GetState() API can be helpful to check in run-time the state of the SPI peripheral
3292:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****      (+) HAL_SPI_GetError() check in run-time Errors occurring during communication
3293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** @endverbatim
3294:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @{
3295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3296:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3297:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Return the SPI handle state.
3299:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3300:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3301:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval SPI state
3302:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3303:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** HAL_SPI_StateTypeDef HAL_SPI_GetState(const SPI_HandleTypeDef *hspi)
3304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3305:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Return SPI handle state */
3306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return hspi->State;
3307:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3308:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3309:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3310:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Return the SPI error code.
3311:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3312:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3313:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval SPI error code in bitmap format
3314:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3315:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** uint32_t HAL_SPI_GetError(const SPI_HandleTypeDef *hspi)
3316:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3317:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Return SPI ErrorCode */
3318:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return hspi->ErrorCode;
3319:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3320:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3321:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3322:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @}
3323:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3325:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3326:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @}
3327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3328:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3329:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /** @addtogroup SPI_Private_Functions
3330:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief   Private functions
3331:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @{
3332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3333:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3334:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3335:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief DMA SPI transmit process complete callback.
3336:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hdma: pointer to a DMA_HandleTypeDef structure that contains
3337:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 60


3338:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3339:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3340:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMATransmitCplt(DMA_HandleTypeDef *hdma)
3341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3342:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
3343:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3344:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_ABORT)
3345:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3346:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmatx->Init.Mode == DMA_CIRCULAR)
3347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3348:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3349:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxCpltCallback(hspi);
3350:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3351:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_SPI_TxCpltCallback(hspi);
3352:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3353:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
3355:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3356:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Enable EOT interrupt */
3357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_ENABLE_IT(hspi, SPI_IT_EOT);
3358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3359:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3361:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3362:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief DMA SPI receive process complete callback.
3364:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hdma: pointer to a DMA_HandleTypeDef structure that contains
3365:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3366:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMAReceiveCplt(DMA_HandleTypeDef *hdma)
3369:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3370:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
3371:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3372:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_ABORT)
3373:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmarx->Init.Mode == DMA_CIRCULAR)
3375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3376:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxCpltCallback(hspi);
3378:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3379:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_SPI_RxCpltCallback(hspi);
3380:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3381:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3382:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
3383:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3384:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Enable EOT interrupt */
3385:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_ENABLE_IT(hspi, SPI_IT_EOT);
3386:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3387:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3388:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3389:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3390:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3391:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  DMA SPI transmit receive process complete callback.
3392:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hdma: pointer to a DMA_HandleTypeDef structure that contains
3393:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3394:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 61


3395:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMATransmitReceiveCplt(DMA_HandleTypeDef *hdma)
3397:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
3399:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3400:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_ABORT)
3401:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3402:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmatx->Init.Mode == DMA_CIRCULAR)
3403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3404:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxRxCpltCallback(hspi);
3406:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_SPI_TxRxCpltCallback(hspi);
3408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3409:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3410:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
3411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3412:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Enable EOT interrupt */
3413:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_ENABLE_IT(hspi, SPI_IT_EOT);
3414:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3415:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3416:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3417:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3418:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3419:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  DMA SPI half transmit process complete callback.
3420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hdma: pointer to a DMA_HandleTypeDef structure that contains
3421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3423:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3424:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMAHalfTransmitCplt(DMA_HandleTypeDef *hdma) /* Derogation MISRAC2012-Rule-8.13 */
3425:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3426:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)
3427:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                             ((DMA_HandleTypeDef *)hdma)->Parent; /* Derogation MISRAC2012-Rule-8.13
3428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3429:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3430:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxHalfCpltCallback(hspi);
3431:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_SPI_TxHalfCpltCallback(hspi);
3433:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3434:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3435:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3437:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  DMA SPI half receive process complete callback
3438:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hdma: pointer to a DMA_HandleTypeDef structure that contains
3439:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3440:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3441:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3442:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMAHalfReceiveCplt(DMA_HandleTypeDef *hdma) /* Derogation MISRAC2012-Rule-8.13 */
3443:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)
3445:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                             ((DMA_HandleTypeDef *)hdma)->Parent; /* Derogation MISRAC2012-Rule-8.13
3446:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3447:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3448:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxHalfCpltCallback(hspi);
3449:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3450:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_SPI_RxHalfCpltCallback(hspi);
3451:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 62


3452:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3454:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3455:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  DMA SPI half transmit receive process complete callback.
3456:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hdma: pointer to a DMA_HandleTypeDef structure that contains
3457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3458:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3460:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMAHalfTransmitReceiveCplt(DMA_HandleTypeDef *hdma) /* Derogation MISRAC2012-Rule-8
3461:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)
3463:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                             ((DMA_HandleTypeDef *)hdma)->Parent; /* Derogation MISRAC2012-Rule-8.13
3464:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3465:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3466:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxRxHalfCpltCallback(hspi);
3467:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3468:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_SPI_TxRxHalfCpltCallback(hspi);
3469:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3470:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3471:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3472:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3473:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  DMA SPI communication error callback.
3474:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hdma: pointer to a DMA_HandleTypeDef structure that contains
3475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3476:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3477:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMAError(DMA_HandleTypeDef *hdma)
3479:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3480:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
3481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3482:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* if DMA error is FIFO error ignore it */
3483:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (HAL_DMA_GetError(hdma) != HAL_DMA_ERROR_FE)
3484:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Call SPI standard close procedure */
3486:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SPI_CloseTransfer(hspi);
3487:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3488:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
3489:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
3490:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3491:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->ErrorCallback(hspi);
3492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3493:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     HAL_SPI_ErrorCallback(hspi);
3494:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3495:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3497:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3498:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3499:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  DMA SPI communication abort callback, when initiated by HAL services on Error
3500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         (To be called at end of DMA Abort procedure following error occurrence).
3501:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hdma DMA handle.
3502:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3503:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3504:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMAAbortOnError(DMA_HandleTypeDef *hdma)
3505:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
3507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t) 0UL;
3508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t) 0UL;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 63


3509:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3510:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Restore hspi->State to Ready */
3511:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
3512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3513:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3514:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCallback(hspi);
3515:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3516:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_SPI_ErrorCallback(hspi);
3517:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3521:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  DMA SPI Tx communication abort callback, when initiated by user
3522:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         (To be called at end of DMA Tx Abort procedure following user abort request).
3523:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @note   When this callback is executed, User Abort complete call back is called only if no
3524:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         Abort still ongoing for Rx DMA Handle.
3525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hdma DMA handle.
3526:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3527:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3528:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMATxAbortCallback(DMA_HandleTypeDef *hdma)
3529:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3530:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
3531:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3532:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback = NULL;
3533:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3534:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check if an Abort process is still ongoing */
3535:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->hdmarx != NULL)
3536:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmarx->XferAbortCallback != NULL)
3538:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3539:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       return;
3540:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3541:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3542:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3543:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Call the Abort procedure */
3544:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_AbortTransfer(hspi);
3545:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3546:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Restore hspi->State to Ready */
3547:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
3548:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3549:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Call user Abort complete callback */
3550:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3551:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->AbortCpltCallback(hspi);
3552:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3553:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_SPI_AbortCpltCallback(hspi);
3554:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3555:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3556:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3557:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3558:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  DMA SPI Rx communication abort callback, when initiated by user
3559:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         (To be called at end of DMA Rx Abort procedure following user abort request).
3560:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @note   When this callback is executed, User Abort complete call back is called only if no
3561:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         Abort still ongoing for Tx DMA Handle.
3562:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hdma DMA handle.
3563:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3564:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_DMARxAbortCallback(DMA_HandleTypeDef *hdma)
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 64


3566:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3567:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
3568:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3569:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmarx->XferAbortCallback = NULL;
3570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3571:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check if an Abort process is still ongoing */
3572:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->hdmatx != NULL)
3573:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->hdmatx->XferAbortCallback != NULL)
3575:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3576:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       return;
3577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3578:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3579:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Call the Abort procedure */
3581:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_AbortTransfer(hspi);
3582:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3583:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Restore hspi->State to Ready */
3584:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
3585:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3586:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Call user Abort complete callback */
3587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
3588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->AbortCpltCallback(hspi);
3589:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_SPI_AbortCpltCallback(hspi);
3591:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3592:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3593:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3594:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Manage the receive 8-bit in Interrupt context.
3596:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3597:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3598:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3599:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3600:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_RxISR_8BIT(SPI_HandleTypeDef *hspi)
3601:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
  28              		.loc 1 3601 1 view -0
  29              		.cfi_startproc
  30              		@ args = 0, pretend = 0, frame = 0
  31              		@ frame_needed = 0, uses_anonymous_args = 0
  32              		@ link register save eliminated.
3602:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Receive data in 8 Bit mode */
3603:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *((uint8_t *)hspi->pRxBuffPtr) = (*(__IO uint8_t *)&hspi->Instance->RXDR);
  33              		.loc 1 3603 3 view .LVU1
  34              		.loc 1 3603 59 is_stmt 0 view .LVU2
  35 0000 0268     		ldr	r2, [r0]
  36              		.loc 1 3603 20 view .LVU3
  37 0002 436E     		ldr	r3, [r0, #100]
  38              		.loc 1 3603 37 view .LVU4
  39 0004 92F83020 		ldrb	r2, [r2, #48]	@ zero_extendqisi2
  40              		.loc 1 3603 34 view .LVU5
  41 0008 1A70     		strb	r2, [r3]
3604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint8_t);
  42              		.loc 1 3604 3 is_stmt 1 view .LVU6
  43              		.loc 1 3604 7 is_stmt 0 view .LVU7
  44 000a 436E     		ldr	r3, [r0, #100]
  45              		.loc 1 3604 20 view .LVU8
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 65


  46 000c 0133     		adds	r3, r3, #1
  47 000e 4366     		str	r3, [r0, #100]
3605:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount--;
  48              		.loc 1 3605 3 is_stmt 1 view .LVU9
  49              		.loc 1 3605 7 is_stmt 0 view .LVU10
  50 0010 B0F86A30 		ldrh	r3, [r0, #106]
  51 0014 9BB2     		uxth	r3, r3
  52              		.loc 1 3605 20 view .LVU11
  53 0016 013B     		subs	r3, r3, #1
  54 0018 9BB2     		uxth	r3, r3
  55 001a A0F86A30 		strh	r3, [r0, #106]	@ movhi
3606:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3607:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable IT if no more data excepted */
3608:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->RxXferCount == 0UL)
  56              		.loc 1 3608 3 is_stmt 1 view .LVU12
  57              		.loc 1 3608 11 is_stmt 0 view .LVU13
  58 001e B0F86A30 		ldrh	r3, [r0, #106]
  59 0022 9BB2     		uxth	r3, r3
  60              		.loc 1 3608 6 view .LVU14
  61 0024 23B9     		cbnz	r3, .L1
3609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3610:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
3611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Check if there is any request to reload */
3612:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->Reload.Requested == 1UL)
3613:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3614:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxXferSize  = hspi->Reload.RxXferSize;
3615:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxXferCount = hspi->Reload.RxXferSize;
3616:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pRxBuffPtr  = hspi->Reload.pRxBuffPtr;
3617:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->Reload.Requested = 0UL;
3618:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3619:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
3620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3621:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Disable RXP interrupts */
3622:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, SPI_IT_RXP);
3623:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3624:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Disable RXP interrupts */
3626:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_RXP);
  62              		.loc 1 3626 5 is_stmt 1 view .LVU15
  63 0026 0268     		ldr	r2, [r0]
  64 0028 1369     		ldr	r3, [r2, #16]
  65 002a 23F00103 		bic	r3, r3, #1
  66 002e 1361     		str	r3, [r2, #16]
  67              	.L1:
3627:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
3628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3629:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
  68              		.loc 1 3629 1 is_stmt 0 view .LVU16
  69 0030 7047     		bx	lr
  70              		.cfi_endproc
  71              	.LFE375:
  73              		.section	.text.SPI_RxISR_16BIT,"ax",%progbits
  74              		.align	1
  75              		.syntax unified
  76              		.thumb
  77              		.thumb_func
  79              	SPI_RxISR_16BIT:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 66


  80              	.LVL1:
  81              	.LFB376:
3630:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3631:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3632:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3633:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Manage the 16-bit receive in Interrupt context.
3634:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3635:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3636:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3637:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3638:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_RxISR_16BIT(SPI_HandleTypeDef *hspi)
3639:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
  82              		.loc 1 3639 1 is_stmt 1 view -0
  83              		.cfi_startproc
  84              		@ args = 0, pretend = 0, frame = 0
  85              		@ frame_needed = 0, uses_anonymous_args = 0
  86              		@ link register save eliminated.
3640:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Receive data in 16 Bit mode */
3641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
3642:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint16_t *prxdr_16bits = (__IO uint16_t *)(&(hspi->Instance->RXDR));
  87              		.loc 1 3642 3 view .LVU18
  88              		.loc 1 3642 57 is_stmt 0 view .LVU19
  89 0000 0268     		ldr	r2, [r0]
  90              	.LVL2:
3643:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3644:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *((uint16_t *)hspi->pRxBuffPtr) = *prxdr_16bits;
  91              		.loc 1 3644 3 is_stmt 1 view .LVU20
  92              		.loc 1 3644 21 is_stmt 0 view .LVU21
  93 0002 436E     		ldr	r3, [r0, #100]
  94              		.loc 1 3644 37 view .LVU22
  95 0004 128E     		ldrh	r2, [r2, #48]
  96              	.LVL3:
  97              		.loc 1 3644 35 view .LVU23
  98 0006 1A80     		strh	r2, [r3]	@ movhi
  99              	.LVL4:
3645:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3646:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *((uint16_t *)hspi->pRxBuffPtr) = (*(__IO uint16_t *)&hspi->Instance->RXDR);
3647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
3648:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 100              		.loc 1 3648 3 is_stmt 1 view .LVU24
 101              		.loc 1 3648 7 is_stmt 0 view .LVU25
 102 0008 436E     		ldr	r3, [r0, #100]
 103              		.loc 1 3648 20 view .LVU26
 104 000a 0233     		adds	r3, r3, #2
 105 000c 4366     		str	r3, [r0, #100]
3649:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount--;
 106              		.loc 1 3649 3 is_stmt 1 view .LVU27
 107              		.loc 1 3649 7 is_stmt 0 view .LVU28
 108 000e B0F86A30 		ldrh	r3, [r0, #106]
 109 0012 9BB2     		uxth	r3, r3
 110              		.loc 1 3649 20 view .LVU29
 111 0014 013B     		subs	r3, r3, #1
 112 0016 9BB2     		uxth	r3, r3
 113 0018 A0F86A30 		strh	r3, [r0, #106]	@ movhi
3650:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3651:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable IT if no more data excepted */
3652:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->RxXferCount == 0UL)
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 67


 114              		.loc 1 3652 3 is_stmt 1 view .LVU30
 115              		.loc 1 3652 11 is_stmt 0 view .LVU31
 116 001c B0F86A30 		ldrh	r3, [r0, #106]
 117 0020 9BB2     		uxth	r3, r3
 118              		.loc 1 3652 6 view .LVU32
 119 0022 23B9     		cbnz	r3, .L3
3653:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3654:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
3655:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Check if there is any request to reload */
3656:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->Reload.Requested == 1UL)
3657:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3658:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxXferSize  = hspi->Reload.RxXferSize;
3659:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxXferCount = hspi->Reload.RxXferSize;
3660:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pRxBuffPtr  = hspi->Reload.pRxBuffPtr;
3661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->Reload.Requested = 0UL;
3662:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3663:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
3664:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Disable RXP interrupts */
3666:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, SPI_IT_RXP);
3667:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3668:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3669:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Disable RXP interrupts */
3670:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_RXP);
 120              		.loc 1 3670 5 is_stmt 1 view .LVU33
 121 0024 0268     		ldr	r2, [r0]
 122 0026 1369     		ldr	r3, [r2, #16]
 123 0028 23F00103 		bic	r3, r3, #1
 124 002c 1361     		str	r3, [r2, #16]
 125              	.L3:
3671:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
3672:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3673:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 126              		.loc 1 3673 1 is_stmt 0 view .LVU34
 127 002e 7047     		bx	lr
 128              		.cfi_endproc
 129              	.LFE376:
 131              		.section	.text.SPI_RxISR_32BIT,"ax",%progbits
 132              		.align	1
 133              		.syntax unified
 134              		.thumb
 135              		.thumb_func
 137              	SPI_RxISR_32BIT:
 138              	.LVL5:
 139              	.LFB377:
3674:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3675:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3676:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Manage the 32-bit receive in Interrupt context.
3678:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3679:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3680:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3681:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3682:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_RxISR_32BIT(SPI_HandleTypeDef *hspi)
3683:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 140              		.loc 1 3683 1 is_stmt 1 view -0
 141              		.cfi_startproc
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 68


 142              		@ args = 0, pretend = 0, frame = 0
 143              		@ frame_needed = 0, uses_anonymous_args = 0
 144              		@ link register save eliminated.
3684:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Receive data in 32 Bit mode */
3685:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *((uint32_t *)hspi->pRxBuffPtr) = (*(__IO uint32_t *)&hspi->Instance->RXDR);
 145              		.loc 1 3685 3 view .LVU36
 146              		.loc 1 3685 61 is_stmt 0 view .LVU37
 147 0000 0268     		ldr	r2, [r0]
 148              		.loc 1 3685 21 view .LVU38
 149 0002 436E     		ldr	r3, [r0, #100]
 150              		.loc 1 3685 38 view .LVU39
 151 0004 126B     		ldr	r2, [r2, #48]
 152              		.loc 1 3685 35 view .LVU40
 153 0006 1A60     		str	r2, [r3]
3686:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint32_t);
 154              		.loc 1 3686 3 is_stmt 1 view .LVU41
 155              		.loc 1 3686 7 is_stmt 0 view .LVU42
 156 0008 436E     		ldr	r3, [r0, #100]
 157              		.loc 1 3686 20 view .LVU43
 158 000a 0433     		adds	r3, r3, #4
 159 000c 4366     		str	r3, [r0, #100]
3687:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount--;
 160              		.loc 1 3687 3 is_stmt 1 view .LVU44
 161              		.loc 1 3687 7 is_stmt 0 view .LVU45
 162 000e B0F86A30 		ldrh	r3, [r0, #106]
 163 0012 9BB2     		uxth	r3, r3
 164              		.loc 1 3687 20 view .LVU46
 165 0014 013B     		subs	r3, r3, #1
 166 0016 9BB2     		uxth	r3, r3
 167 0018 A0F86A30 		strh	r3, [r0, #106]	@ movhi
3688:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3689:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable IT if no more data excepted */
3690:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->RxXferCount == 0UL)
 168              		.loc 1 3690 3 is_stmt 1 view .LVU47
 169              		.loc 1 3690 11 is_stmt 0 view .LVU48
 170 001c B0F86A30 		ldrh	r3, [r0, #106]
 171 0020 9BB2     		uxth	r3, r3
 172              		.loc 1 3690 6 view .LVU49
 173 0022 23B9     		cbnz	r3, .L5
3691:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3692:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
3693:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Check if there is any request to reload */
3694:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->Reload.Requested == 1UL)
3695:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3696:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxXferSize  = hspi->Reload.RxXferSize;
3697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->RxXferCount = hspi->Reload.RxXferSize;
3698:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pRxBuffPtr  = hspi->Reload.pRxBuffPtr;
3699:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->Reload.Requested = 0UL;
3700:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3701:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
3702:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3703:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Disable RXP interrupts */
3704:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, SPI_IT_RXP);
3705:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3706:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3707:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Disable RXP interrupts */
3708:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_RXP);
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 69


 174              		.loc 1 3708 5 is_stmt 1 view .LVU50
 175 0024 0268     		ldr	r2, [r0]
 176 0026 1369     		ldr	r3, [r2, #16]
 177 0028 23F00103 		bic	r3, r3, #1
 178 002c 1361     		str	r3, [r2, #16]
 179              	.L5:
3709:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
3710:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3711:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 180              		.loc 1 3711 1 is_stmt 0 view .LVU51
 181 002e 7047     		bx	lr
 182              		.cfi_endproc
 183              	.LFE377:
 185              		.section	.text.SPI_TxISR_8BIT,"ax",%progbits
 186              		.align	1
 187              		.syntax unified
 188              		.thumb
 189              		.thumb_func
 191              	SPI_TxISR_8BIT:
 192              	.LVL6:
 193              	.LFB378:
3712:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3713:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3714:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3715:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Handle the data 8-bit transmit in Interrupt mode.
3716:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3717:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3719:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3720:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_TxISR_8BIT(SPI_HandleTypeDef *hspi)
3721:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 194              		.loc 1 3721 1 is_stmt 1 view -0
 195              		.cfi_startproc
 196              		@ args = 0, pretend = 0, frame = 0
 197              		@ frame_needed = 0, uses_anonymous_args = 0
 198              		@ link register save eliminated.
3722:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Transmit data in 8 Bit mode */
3723:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *(__IO uint8_t *)&hspi->Instance->TXDR = *((const uint8_t *)hspi->pTxBuffPtr);
 199              		.loc 1 3723 3 view .LVU53
 200              		.loc 1 3723 67 is_stmt 0 view .LVU54
 201 0000 C26D     		ldr	r2, [r0, #92]
 202              		.loc 1 3723 25 view .LVU55
 203 0002 0368     		ldr	r3, [r0]
 204              		.loc 1 3723 44 view .LVU56
 205 0004 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
 206              		.loc 1 3723 42 view .LVU57
 207 0006 83F82020 		strb	r2, [r3, #32]
3724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint8_t);
 208              		.loc 1 3724 3 is_stmt 1 view .LVU58
 209              		.loc 1 3724 7 is_stmt 0 view .LVU59
 210 000a C36D     		ldr	r3, [r0, #92]
 211              		.loc 1 3724 20 view .LVU60
 212 000c 0133     		adds	r3, r3, #1
 213 000e C365     		str	r3, [r0, #92]
3725:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount--;
 214              		.loc 1 3725 3 is_stmt 1 view .LVU61
 215              		.loc 1 3725 7 is_stmt 0 view .LVU62
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 70


 216 0010 B0F86230 		ldrh	r3, [r0, #98]
 217 0014 9BB2     		uxth	r3, r3
 218              		.loc 1 3725 20 view .LVU63
 219 0016 013B     		subs	r3, r3, #1
 220 0018 9BB2     		uxth	r3, r3
 221 001a A0F86230 		strh	r3, [r0, #98]	@ movhi
3726:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3727:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable IT if no more data excepted */
3728:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->TxXferCount == 0UL)
 222              		.loc 1 3728 3 is_stmt 1 view .LVU64
 223              		.loc 1 3728 11 is_stmt 0 view .LVU65
 224 001e B0F86230 		ldrh	r3, [r0, #98]
 225 0022 9BB2     		uxth	r3, r3
 226              		.loc 1 3728 6 view .LVU66
 227 0024 23B9     		cbnz	r3, .L7
3729:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3730:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
3731:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Check if there is any request to reload */
3732:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->Reload.Requested == 1UL)
3733:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3734:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferSize  = hspi->Reload.TxXferSize;
3735:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount = hspi->Reload.TxXferSize;
3736:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr  = hspi->Reload.pTxBuffPtr;
3737:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3738:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* In full duplex mode the reload request is reset in RX side */
3739:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (hspi->State == HAL_SPI_STATE_BUSY_TX)
3740:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
3741:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->Reload.Requested = 0UL;
3742:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
3743:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3744:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
3745:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3746:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Disable TXP interrupts */
3747:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXP);
3748:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3749:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3750:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Disable TXP interrupts */
3751:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXP);
 228              		.loc 1 3751 5 is_stmt 1 view .LVU67
 229 0026 0268     		ldr	r2, [r0]
 230 0028 1369     		ldr	r3, [r2, #16]
 231 002a 23F00203 		bic	r3, r3, #2
 232 002e 1361     		str	r3, [r2, #16]
 233              	.L7:
3752:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
3753:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3754:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 234              		.loc 1 3754 1 is_stmt 0 view .LVU68
 235 0030 7047     		bx	lr
 236              		.cfi_endproc
 237              	.LFE378:
 239              		.section	.text.SPI_TxISR_16BIT,"ax",%progbits
 240              		.align	1
 241              		.syntax unified
 242              		.thumb
 243              		.thumb_func
 245              	SPI_TxISR_16BIT:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 71


 246              	.LVL7:
 247              	.LFB379:
3755:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3756:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3757:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Handle the data 16-bit transmit in Interrupt mode.
3758:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3759:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3761:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3762:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_TxISR_16BIT(SPI_HandleTypeDef *hspi)
3763:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 248              		.loc 1 3763 1 is_stmt 1 view -0
 249              		.cfi_startproc
 250              		@ args = 0, pretend = 0, frame = 0
 251              		@ frame_needed = 0, uses_anonymous_args = 0
 252              		@ link register save eliminated.
3764:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
3765:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
3766:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint16_t *ptxdr_16bits = (__IO uint16_t *)(&(hspi->Instance->TXDR));
 253              		.loc 1 3766 3 view .LVU70
 254              		.loc 1 3766 57 is_stmt 0 view .LVU71
 255 0000 0368     		ldr	r3, [r0]
 256              	.LVL8:
3767:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3768:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *ptxdr_16bits = *((const uint16_t *)hspi->pTxBuffPtr);
 257              		.loc 1 3768 3 is_stmt 1 view .LVU72
 258              		.loc 1 3768 43 is_stmt 0 view .LVU73
 259 0002 C26D     		ldr	r2, [r0, #92]
 260              		.loc 1 3768 19 view .LVU74
 261 0004 1288     		ldrh	r2, [r2]
 262              		.loc 1 3768 17 view .LVU75
 263 0006 1A84     		strh	r2, [r3, #32]	@ movhi
3769:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3770:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *((__IO uint16_t *)&hspi->Instance->TXDR) = *((const uint16_t *)hspi->pTxBuffPtr);
3771:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
3772:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 264              		.loc 1 3772 3 is_stmt 1 view .LVU76
 265              		.loc 1 3772 7 is_stmt 0 view .LVU77
 266 0008 C36D     		ldr	r3, [r0, #92]
 267              	.LVL9:
 268              		.loc 1 3772 20 view .LVU78
 269 000a 0233     		adds	r3, r3, #2
 270 000c C365     		str	r3, [r0, #92]
3773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount--;
 271              		.loc 1 3773 3 is_stmt 1 view .LVU79
 272              		.loc 1 3773 7 is_stmt 0 view .LVU80
 273 000e B0F86230 		ldrh	r3, [r0, #98]
 274 0012 9BB2     		uxth	r3, r3
 275              		.loc 1 3773 20 view .LVU81
 276 0014 013B     		subs	r3, r3, #1
 277 0016 9BB2     		uxth	r3, r3
 278 0018 A0F86230 		strh	r3, [r0, #98]	@ movhi
3774:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3775:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable IT if no more data excepted */
3776:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->TxXferCount == 0UL)
 279              		.loc 1 3776 3 is_stmt 1 view .LVU82
 280              		.loc 1 3776 11 is_stmt 0 view .LVU83
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 72


 281 001c B0F86230 		ldrh	r3, [r0, #98]
 282 0020 9BB2     		uxth	r3, r3
 283              		.loc 1 3776 6 view .LVU84
 284 0022 23B9     		cbnz	r3, .L9
3777:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3778:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
3779:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Check if there is any request to reload */
3780:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->Reload.Requested == 1UL)
3781:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3782:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferSize  = hspi->Reload.TxXferSize;
3783:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount = hspi->Reload.TxXferSize;
3784:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr  = hspi->Reload.pTxBuffPtr;
3785:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3786:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* In full duplex mode the reload request is reset in RX side */
3787:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (hspi->State == HAL_SPI_STATE_BUSY_TX)
3788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
3789:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->Reload.Requested = 0UL;
3790:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
3791:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3792:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
3793:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3794:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Disable TXP interrupts */
3795:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXP);
3796:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3797:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3798:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Disable TXP interrupts */
3799:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXP);
 285              		.loc 1 3799 5 is_stmt 1 view .LVU85
 286 0024 0268     		ldr	r2, [r0]
 287 0026 1369     		ldr	r3, [r2, #16]
 288 0028 23F00203 		bic	r3, r3, #2
 289 002c 1361     		str	r3, [r2, #16]
 290              	.L9:
3800:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
3801:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3802:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 291              		.loc 1 3802 1 is_stmt 0 view .LVU86
 292 002e 7047     		bx	lr
 293              		.cfi_endproc
 294              	.LFE379:
 296              		.section	.text.SPI_TxISR_32BIT,"ax",%progbits
 297              		.align	1
 298              		.syntax unified
 299              		.thumb
 300              		.thumb_func
 302              	SPI_TxISR_32BIT:
 303              	.LVL10:
 304              	.LFB380:
3803:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3804:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3805:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Handle the data 32-bit transmit in Interrupt mode.
3806:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3807:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3808:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3809:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3810:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_TxISR_32BIT(SPI_HandleTypeDef *hspi)
3811:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 73


 305              		.loc 1 3811 1 is_stmt 1 view -0
 306              		.cfi_startproc
 307              		@ args = 0, pretend = 0, frame = 0
 308              		@ frame_needed = 0, uses_anonymous_args = 0
 309              		@ link register save eliminated.
3812:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Transmit data in 32 Bit mode */
3813:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *((__IO uint32_t *)&hspi->Instance->TXDR) = *((const uint32_t *)hspi->pTxBuffPtr);
 310              		.loc 1 3813 3 view .LVU88
 311              		.loc 1 3813 71 is_stmt 0 view .LVU89
 312 0000 C26D     		ldr	r2, [r0, #92]
 313              		.loc 1 3813 27 view .LVU90
 314 0002 0368     		ldr	r3, [r0]
 315              		.loc 1 3813 47 view .LVU91
 316 0004 1268     		ldr	r2, [r2]
 317              		.loc 1 3813 45 view .LVU92
 318 0006 1A62     		str	r2, [r3, #32]
3814:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint32_t);
 319              		.loc 1 3814 3 is_stmt 1 view .LVU93
 320              		.loc 1 3814 7 is_stmt 0 view .LVU94
 321 0008 C36D     		ldr	r3, [r0, #92]
 322              		.loc 1 3814 20 view .LVU95
 323 000a 0433     		adds	r3, r3, #4
 324 000c C365     		str	r3, [r0, #92]
3815:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount--;
 325              		.loc 1 3815 3 is_stmt 1 view .LVU96
 326              		.loc 1 3815 7 is_stmt 0 view .LVU97
 327 000e B0F86230 		ldrh	r3, [r0, #98]
 328 0012 9BB2     		uxth	r3, r3
 329              		.loc 1 3815 20 view .LVU98
 330 0014 013B     		subs	r3, r3, #1
 331 0016 9BB2     		uxth	r3, r3
 332 0018 A0F86230 		strh	r3, [r0, #98]	@ movhi
3816:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3817:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable IT if no more data excepted */
3818:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->TxXferCount == 0UL)
 333              		.loc 1 3818 3 is_stmt 1 view .LVU99
 334              		.loc 1 3818 11 is_stmt 0 view .LVU100
 335 001c B0F86230 		ldrh	r3, [r0, #98]
 336 0020 9BB2     		uxth	r3, r3
 337              		.loc 1 3818 6 view .LVU101
 338 0022 23B9     		cbnz	r3, .L11
3819:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3820:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined(USE_SPI_RELOAD_TRANSFER)
3821:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Check if there is any request to reload */
3822:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->Reload.Requested == 1UL)
3823:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3824:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferSize  = hspi->Reload.TxXferSize;
3825:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount = hspi->Reload.TxXferSize;
3826:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr  = hspi->Reload.pTxBuffPtr;
3827:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3828:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* In full duplex mode the reload request is reset in RX side */
3829:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (hspi->State == HAL_SPI_STATE_BUSY_TX)
3830:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
3831:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->Reload.Requested = 0UL;
3832:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
3833:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3834:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     else
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 74


3835:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3836:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       /* Disable TXP interrupts */
3837:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXP);
3838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3839:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
3840:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Disable TXP interrupts */
3841:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXP);
 339              		.loc 1 3841 5 is_stmt 1 view .LVU102
 340 0024 0268     		ldr	r2, [r0]
 341 0026 1369     		ldr	r3, [r2, #16]
 342 0028 23F00203 		bic	r3, r3, #2
 343 002c 1361     		str	r3, [r2, #16]
 344              	.L11:
3842:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_RELOAD_TRANSFER */
3843:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3844:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 345              		.loc 1 3844 1 is_stmt 0 view .LVU103
 346 002e 7047     		bx	lr
 347              		.cfi_endproc
 348              	.LFE380:
 350              		.section	.text.SPI_AbortTransfer,"ax",%progbits
 351              		.align	1
 352              		.syntax unified
 353              		.thumb
 354              		.thumb_func
 356              	SPI_AbortTransfer:
 357              	.LVL11:
 358              	.LFB381:
3845:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3846:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Abort Transfer and clear flags.
3848:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3850:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval None
3851:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_AbortTransfer(SPI_HandleTypeDef *hspi)
3853:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 359              		.loc 1 3853 1 is_stmt 1 view -0
 360              		.cfi_startproc
 361              		@ args = 0, pretend = 0, frame = 0
 362              		@ frame_needed = 0, uses_anonymous_args = 0
 363              		@ link register save eliminated.
3854:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable SPI peripheral */
3855:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
 364              		.loc 1 3855 3 view .LVU105
 365 0000 0268     		ldr	r2, [r0]
 366 0002 1368     		ldr	r3, [r2]
 367 0004 23F00103 		bic	r3, r3, #1
 368 0008 1360     		str	r3, [r2]
3856:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable ITs */
3858:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_EOT | SPI_IT_TXP | SPI_IT_RXP | SPI_IT_DXP | SPI_IT_UDR | SPI_
 369              		.loc 1 3858 3 view .LVU106
 370 000a 0268     		ldr	r2, [r0]
 371 000c 1169     		ldr	r1, [r2, #16]
 372 000e 184B     		ldr	r3, .L14
 373 0010 0B40     		ands	r3, r3, r1
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 75


 374 0012 1361     		str	r3, [r2, #16]
3859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                               SPI_IT_FRE | SPI_IT_MODF));
3860:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Clear the Status flags in the SR register */
3862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_CLEAR_EOTFLAG(hspi);
 375              		.loc 1 3862 3 view .LVU107
 376 0014 0268     		ldr	r2, [r0]
 377 0016 9369     		ldr	r3, [r2, #24]
 378 0018 43F00803 		orr	r3, r3, #8
 379 001c 9361     		str	r3, [r2, #24]
3863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_CLEAR_TXTFFLAG(hspi);
 380              		.loc 1 3863 3 view .LVU108
 381 001e 0268     		ldr	r2, [r0]
 382 0020 9369     		ldr	r3, [r2, #24]
 383 0022 43F01003 		orr	r3, r3, #16
 384 0026 9361     		str	r3, [r2, #24]
3864:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable Tx DMA Request */
3866:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CFG1, SPI_CFG1_TXDMAEN | SPI_CFG1_RXDMAEN);
 385              		.loc 1 3866 3 view .LVU109
 386 0028 0268     		ldr	r2, [r0]
 387 002a 9368     		ldr	r3, [r2, #8]
 388 002c 23F44043 		bic	r3, r3, #49152
 389 0030 9360     		str	r3, [r2, #8]
3867:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3868:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Clear the Error flags in the SR register */
3869:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_CLEAR_OVRFLAG(hspi);
 390              		.loc 1 3869 3 view .LVU110
 391 0032 0268     		ldr	r2, [r0]
 392 0034 9369     		ldr	r3, [r2, #24]
 393 0036 43F04003 		orr	r3, r3, #64
 394 003a 9361     		str	r3, [r2, #24]
3870:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_CLEAR_UDRFLAG(hspi);
 395              		.loc 1 3870 3 view .LVU111
 396 003c 0268     		ldr	r2, [r0]
 397 003e 9369     		ldr	r3, [r2, #24]
 398 0040 43F02003 		orr	r3, r3, #32
 399 0044 9361     		str	r3, [r2, #24]
3871:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 400              		.loc 1 3871 3 view .LVU112
 401 0046 0268     		ldr	r2, [r0]
 402 0048 9369     		ldr	r3, [r2, #24]
 403 004a 43F48073 		orr	r3, r3, #256
 404 004e 9361     		str	r3, [r2, #24]
3872:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_CLEAR_MODFFLAG(hspi);
 405              		.loc 1 3872 3 view .LVU113
 406 0050 0268     		ldr	r2, [r0]
 407 0052 9369     		ldr	r3, [r2, #24]
 408 0054 43F40073 		orr	r3, r3, #512
 409 0058 9361     		str	r3, [r2, #24]
 410              		.loc 1 3872 33 view .LVU114
3873:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_CLEAR_SUSPFLAG(hspi);
 411              		.loc 1 3873 3 view .LVU115
 412 005a 0268     		ldr	r2, [r0]
 413 005c 9369     		ldr	r3, [r2, #24]
 414 005e 43F40063 		orr	r3, r3, #2048
 415 0062 9361     		str	r3, [r2, #24]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 76


3874:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3875:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3876:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
3877:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3878:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3879:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t)0UL;
 416              		.loc 1 3879 3 view .LVU116
 417              		.loc 1 3879 21 is_stmt 0 view .LVU117
 418 0064 0023     		movs	r3, #0
 419 0066 A0F86230 		strh	r3, [r0, #98]	@ movhi
3880:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t)0UL;
 420              		.loc 1 3880 3 is_stmt 1 view .LVU118
 421              		.loc 1 3880 21 is_stmt 0 view .LVU119
 422 006a A0F86A30 		strh	r3, [r0, #106]	@ movhi
3881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 423              		.loc 1 3881 1 view .LVU120
 424 006e 7047     		bx	lr
 425              	.L15:
 426              		.align	2
 427              	.L14:
 428 0070 90FCFFFF 		.word	-880
 429              		.cfi_endproc
 430              	.LFE381:
 432              		.section	.text.SPI_CloseTransfer,"ax",%progbits
 433              		.align	1
 434              		.syntax unified
 435              		.thumb
 436              		.thumb_func
 438              	SPI_CloseTransfer:
 439              	.LVL12:
 440              	.LFB382:
3882:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3883:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3884:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3885:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Close Transfer and clear flags.
3886:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3887:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL_ERROR: if any error detected
3889:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *         HAL_OK: if nothing detected
3890:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3891:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static void SPI_CloseTransfer(SPI_HandleTypeDef *hspi)
3892:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 441              		.loc 1 3892 1 is_stmt 1 view -0
 442              		.cfi_startproc
 443              		@ args = 0, pretend = 0, frame = 0
 444              		@ frame_needed = 0, uses_anonymous_args = 0
 445              		@ link register save eliminated.
 446              		.loc 1 3892 1 is_stmt 0 view .LVU122
 447 0000 10B4     		push	{r4}
 448              		.cfi_def_cfa_offset 4
 449              		.cfi_offset 4, -4
3893:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t itflag = hspi->Instance->SR;
 450              		.loc 1 3893 3 is_stmt 1 view .LVU123
 451              		.loc 1 3893 25 is_stmt 0 view .LVU124
 452 0002 0268     		ldr	r2, [r0]
 453              		.loc 1 3893 12 view .LVU125
 454 0004 5369     		ldr	r3, [r2, #20]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 77


 455              	.LVL13:
3894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3895:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_CLEAR_EOTFLAG(hspi);
 456              		.loc 1 3895 3 is_stmt 1 view .LVU126
 457 0006 9169     		ldr	r1, [r2, #24]
 458 0008 41F00801 		orr	r1, r1, #8
 459 000c 9161     		str	r1, [r2, #24]
3896:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_CLEAR_TXTFFLAG(hspi);
 460              		.loc 1 3896 3 view .LVU127
 461 000e 0168     		ldr	r1, [r0]
 462 0010 8A69     		ldr	r2, [r1, #24]
 463 0012 42F01002 		orr	r2, r2, #16
 464 0016 8A61     		str	r2, [r1, #24]
3897:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3898:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable SPI peripheral */
3899:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
 465              		.loc 1 3899 3 view .LVU128
 466 0018 0168     		ldr	r1, [r0]
 467 001a 0A68     		ldr	r2, [r1]
 468 001c 22F00102 		bic	r2, r2, #1
 469 0020 0A60     		str	r2, [r1]
3900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3901:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable ITs */
3902:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_EOT | SPI_IT_TXP | SPI_IT_RXP | SPI_IT_DXP | SPI_IT_UDR | SPI_
 470              		.loc 1 3902 3 view .LVU129
 471 0022 0168     		ldr	r1, [r0]
 472 0024 0C69     		ldr	r4, [r1, #16]
 473 0026 284A     		ldr	r2, .L22
 474 0028 2240     		ands	r2, r2, r4
 475 002a 0A61     		str	r2, [r1, #16]
3903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                               SPI_IT_FRE | SPI_IT_MODF));
3904:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3905:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Disable Tx DMA Request */
3906:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CFG1, SPI_CFG1_TXDMAEN | SPI_CFG1_RXDMAEN);
 476              		.loc 1 3906 3 view .LVU130
 477 002c 0168     		ldr	r1, [r0]
 478 002e 8A68     		ldr	r2, [r1, #8]
 479 0030 22F44042 		bic	r2, r2, #49152
 480 0034 8A60     		str	r2, [r1, #8]
3907:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3908:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Report UnderRun error for non RX Only communication */
3909:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_BUSY_RX)
 481              		.loc 1 3909 3 view .LVU131
 482              		.loc 1 3909 11 is_stmt 0 view .LVU132
 483 0036 90F88120 		ldrb	r2, [r0, #129]	@ zero_extendqisi2
 484              		.loc 1 3909 6 view .LVU133
 485 003a 042A     		cmp	r2, #4
 486 003c 0DD0     		beq	.L17
3910:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3911:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if ((itflag & SPI_FLAG_UDR) != 0UL)
 487              		.loc 1 3911 5 is_stmt 1 view .LVU134
 488              		.loc 1 3911 8 is_stmt 0 view .LVU135
 489 003e 13F0200F 		tst	r3, #32
 490 0042 0AD0     		beq	.L17
3912:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3913:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_UDR);
 491              		.loc 1 3913 7 is_stmt 1 view .LVU136
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 78


 492 0044 D0F88420 		ldr	r2, [r0, #132]
 493 0048 42F08002 		orr	r2, r2, #128
 494 004c C0F88420 		str	r2, [r0, #132]
3914:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_CLEAR_UDRFLAG(hspi);
 495              		.loc 1 3914 7 view .LVU137
 496 0050 0168     		ldr	r1, [r0]
 497 0052 8A69     		ldr	r2, [r1, #24]
 498 0054 42F02002 		orr	r2, r2, #32
 499 0058 8A61     		str	r2, [r1, #24]
 500              	.L17:
3915:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3916:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3917:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3918:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Report OverRun error for non TX Only communication */
3919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_BUSY_TX)
 501              		.loc 1 3919 3 view .LVU138
 502              		.loc 1 3919 11 is_stmt 0 view .LVU139
 503 005a 90F88120 		ldrb	r2, [r0, #129]	@ zero_extendqisi2
 504              		.loc 1 3919 6 view .LVU140
 505 005e 032A     		cmp	r2, #3
 506 0060 0DD0     		beq	.L18
3920:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3921:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if ((itflag & SPI_FLAG_OVR) != 0UL)
 507              		.loc 1 3921 5 is_stmt 1 view .LVU141
 508              		.loc 1 3921 8 is_stmt 0 view .LVU142
 509 0062 13F0400F 		tst	r3, #64
 510 0066 0AD0     		beq	.L18
3922:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3923:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_OVR);
 511              		.loc 1 3923 7 is_stmt 1 view .LVU143
 512 0068 D0F88420 		ldr	r2, [r0, #132]
 513 006c 42F00402 		orr	r2, r2, #4
 514 0070 C0F88420 		str	r2, [r0, #132]
3924:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_CLEAR_OVRFLAG(hspi);
 515              		.loc 1 3924 7 view .LVU144
 516 0074 0168     		ldr	r1, [r0]
 517 0076 8A69     		ldr	r2, [r1, #24]
 518 0078 42F04002 		orr	r2, r2, #64
 519 007c 8A61     		str	r2, [r1, #24]
 520              	.L18:
3925:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3926:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_SPI_CRC != 0UL)
3928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Check if CRC error occurred */
3929:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3930:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3931:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if ((itflag & SPI_FLAG_CRCERR) != 0UL)
3932:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
3933:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
3934:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
3935:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
3936:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3937:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3938:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3939:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3940:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPI Mode Fault error interrupt occurred -------------------------------*/
3941:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((itflag & SPI_FLAG_MODF) != 0UL)
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 79


 521              		.loc 1 3941 3 view .LVU145
 522              		.loc 1 3941 6 is_stmt 0 view .LVU146
 523 007e 13F4007F 		tst	r3, #512
 524 0082 0AD0     		beq	.L19
3942:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3943:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_MODF);
 525              		.loc 1 3943 5 is_stmt 1 view .LVU147
 526 0084 D0F88420 		ldr	r2, [r0, #132]
 527 0088 42F00102 		orr	r2, r2, #1
 528 008c C0F88420 		str	r2, [r0, #132]
3944:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_CLEAR_MODFFLAG(hspi);
 529              		.loc 1 3944 5 view .LVU148
 530 0090 0168     		ldr	r1, [r0]
 531 0092 8A69     		ldr	r2, [r1, #24]
 532 0094 42F40072 		orr	r2, r2, #512
 533 0098 8A61     		str	r2, [r1, #24]
 534              	.L19:
 535              		.loc 1 3944 35 discriminator 1 view .LVU149
3945:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3946:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3947:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* SPI Frame error interrupt occurred ------------------------------------*/
3948:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if ((itflag & SPI_FLAG_FRE) != 0UL)
 536              		.loc 1 3948 3 view .LVU150
 537              		.loc 1 3948 6 is_stmt 0 view .LVU151
 538 009a 13F4807F 		tst	r3, #256
 539 009e 0AD0     		beq	.L20
3949:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3950:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FRE);
 540              		.loc 1 3950 5 is_stmt 1 view .LVU152
 541 00a0 D0F88430 		ldr	r3, [r0, #132]
 542              	.LVL14:
 543              		.loc 1 3950 5 is_stmt 0 view .LVU153
 544 00a4 43F00803 		orr	r3, r3, #8
 545 00a8 C0F88430 		str	r3, [r0, #132]
3951:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 546              		.loc 1 3951 5 is_stmt 1 view .LVU154
 547 00ac 0268     		ldr	r2, [r0]
 548 00ae 9369     		ldr	r3, [r2, #24]
 549 00b0 43F48073 		orr	r3, r3, #256
 550 00b4 9361     		str	r3, [r2, #24]
 551              	.L20:
3952:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3953:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3954:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t)0UL;
 552              		.loc 1 3954 3 view .LVU155
 553              		.loc 1 3954 21 is_stmt 0 view .LVU156
 554 00b6 0023     		movs	r3, #0
 555 00b8 A0F86230 		strh	r3, [r0, #98]	@ movhi
3955:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t)0UL;
 556              		.loc 1 3955 3 is_stmt 1 view .LVU157
 557              		.loc 1 3955 21 is_stmt 0 view .LVU158
 558 00bc A0F86A30 		strh	r3, [r0, #106]	@ movhi
3956:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 559              		.loc 1 3956 1 view .LVU159
 560 00c0 5DF8044B 		ldr	r4, [sp], #4
 561              		.cfi_restore 4
 562              		.cfi_def_cfa_offset 0
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 80


 563 00c4 7047     		bx	lr
 564              	.L23:
 565 00c6 00BF     		.align	2
 566              	.L22:
 567 00c8 90FCFFFF 		.word	-880
 568              		.cfi_endproc
 569              	.LFE382:
 571              		.section	.text.SPI_GetPacketSize,"ax",%progbits
 572              		.align	1
 573              		.syntax unified
 574              		.thumb
 575              		.thumb_func
 577              	SPI_GetPacketSize:
 578              	.LVL15:
 579              	.LFB384:
3957:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3958:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3959:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief Handle SPI Communication Timeout.
3960:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param hspi: pointer to a SPI_HandleTypeDef structure that contains
3961:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *              the configuration information for SPI module.
3962:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param Flag: SPI flag to check
3963:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param Status: flag state to check
3964:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param Timeout: Timeout duration
3965:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param Tickstart: Tick start value
3966:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval HAL status
3967:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3968:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static HAL_StatusTypeDef SPI_WaitOnFlagUntilTimeout(const SPI_HandleTypeDef *hspi, uint32_t Flag, F
3969:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                     uint32_t Timeout, uint32_t Tickstart)
3970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
3971:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Wait until flag is set */
3972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   while ((__HAL_SPI_GET_FLAG(hspi, Flag) ? SET : RESET) == Status)
3973:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
3974:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     /* Check for the Timeout */
3975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if ((((HAL_GetTick() - Tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout == 0U
3976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
3977:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       return HAL_TIMEOUT;
3978:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
3979:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
3980:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return HAL_OK;
3981:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
3982:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3983:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** /**
3984:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @brief  Compute configured packet size from fifo perspective.
3985:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @param  hspi: pointer to a SPI_HandleTypeDef structure that contains
3986:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   *               the configuration information for SPI module.
3987:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   * @retval Packet size occupied in the fifo
3988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   */
3989:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** static uint32_t SPI_GetPacketSize(const SPI_HandleTypeDef *hspi)
3990:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** {
 580              		.loc 1 3990 1 is_stmt 1 view -0
 581              		.cfi_startproc
 582              		@ args = 0, pretend = 0, frame = 0
 583              		@ frame_needed = 0, uses_anonymous_args = 0
 584              		@ link register save eliminated.
3991:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t fifo_threashold = (hspi->Init.FifoThreshold >> SPI_CFG1_FTHLV_Pos) + 1UL;
 585              		.loc 1 3991 3 view .LVU161
 586              		.loc 1 3991 41 is_stmt 0 view .LVU162
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 81


 587 0000 C36B     		ldr	r3, [r0, #60]
 588              		.loc 1 3991 56 view .LVU163
 589 0002 5B09     		lsrs	r3, r3, #5
 590              	.LVL16:
3992:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t data_size       = (hspi->Init.DataSize      >> SPI_CFG1_DSIZE_Pos) + 1UL;
 591              		.loc 1 3992 3 is_stmt 1 view .LVU164
 592              		.loc 1 3992 41 is_stmt 0 view .LVU165
 593 0004 C068     		ldr	r0, [r0, #12]
 594              	.LVL17:
3993:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3994:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Convert data size to Byte */
3995:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   data_size = (data_size + 7UL) / 8UL;
 595              		.loc 1 3995 3 is_stmt 1 view .LVU166
 596              		.loc 1 3995 26 is_stmt 0 view .LVU167
 597 0006 0830     		adds	r0, r0, #8
 598              	.LVL18:
 599              		.loc 1 3995 13 view .LVU168
 600 0008 C008     		lsrs	r0, r0, #3
 601              	.LVL19:
3996:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
3997:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   return data_size * fifo_threashold;
 602              		.loc 1 3997 3 is_stmt 1 view .LVU169
3998:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 603              		.loc 1 3998 1 is_stmt 0 view .LVU170
 604 000a 03FB0000 		mla	r0, r3, r0, r0
 605              	.LVL20:
 606              		.loc 1 3998 1 view .LVU171
 607 000e 7047     		bx	lr
 608              		.cfi_endproc
 609              	.LFE384:
 611              		.section	.text.SPI_WaitOnFlagUntilTimeout,"ax",%progbits
 612              		.align	1
 613              		.syntax unified
 614              		.thumb
 615              		.thumb_func
 617              	SPI_WaitOnFlagUntilTimeout:
 618              	.LVL21:
 619              	.LFB383:
3970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Wait until flag is set */
 620              		.loc 1 3970 1 is_stmt 1 view -0
 621              		.cfi_startproc
 622              		@ args = 4, pretend = 0, frame = 0
 623              		@ frame_needed = 0, uses_anonymous_args = 0
3970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Wait until flag is set */
 624              		.loc 1 3970 1 is_stmt 0 view .LVU173
 625 0000 2DE9F843 		push	{r3, r4, r5, r6, r7, r8, r9, lr}
 626              		.cfi_def_cfa_offset 32
 627              		.cfi_offset 3, -32
 628              		.cfi_offset 4, -28
 629              		.cfi_offset 5, -24
 630              		.cfi_offset 6, -20
 631              		.cfi_offset 7, -16
 632              		.cfi_offset 8, -12
 633              		.cfi_offset 9, -8
 634              		.cfi_offset 14, -4
 635 0004 8046     		mov	r8, r0
 636 0006 0F46     		mov	r7, r1
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 82


 637 0008 1646     		mov	r6, r2
 638 000a 1D46     		mov	r5, r3
 639 000c DDF82090 		ldr	r9, [sp, #32]
3972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 640              		.loc 1 3972 3 is_stmt 1 view .LVU174
3972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 641              		.loc 1 3972 9 is_stmt 0 view .LVU175
 642 0010 00E0     		b	.L26
 643              	.LVL22:
 644              	.L27:
3975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 645              		.loc 1 3975 83 discriminator 3 view .LVU176
 646 0012 BDB1     		cbz	r5, .L31
 647              	.L26:
3972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 648              		.loc 1 3972 57 is_stmt 1 view .LVU177
3972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 649              		.loc 1 3972 11 is_stmt 0 view .LVU178
 650 0014 D8F80030 		ldr	r3, [r8]
 651 0018 5C69     		ldr	r4, [r3, #20]
3972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 652              		.loc 1 3972 48 view .LVU179
 653 001a 37EA0404 		bics	r4, r7, r4
 654 001e 0CBF     		ite	eq
 655 0020 0123     		moveq	r3, #1
 656 0022 0023     		movne	r3, #0
3972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 657              		.loc 1 3972 57 view .LVU180
 658 0024 B342     		cmp	r3, r6
 659 0026 0AD1     		bne	.L33
3975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 660              		.loc 1 3975 5 is_stmt 1 view .LVU181
3975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 661              		.loc 1 3975 12 is_stmt 0 view .LVU182
 662 0028 FFF7FEFF 		bl	HAL_GetTick
 663              	.LVL23:
3975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 664              		.loc 1 3975 26 discriminator 1 view .LVU183
 665 002c A0EB0900 		sub	r0, r0, r9
3975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 666              		.loc 1 3975 8 discriminator 1 view .LVU184
 667 0030 A842     		cmp	r0, r5
 668 0032 EED3     		bcc	.L27
3975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 669              		.loc 1 3975 52 discriminator 1 view .LVU185
 670 0034 B5F1FF3F 		cmp	r5, #-1
 671 0038 EBD0     		beq	.L27
3977:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 672              		.loc 1 3977 14 view .LVU186
 673 003a 0320     		movs	r0, #3
 674 003c 00E0     		b	.L28
 675              	.L33:
3980:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 676              		.loc 1 3980 10 view .LVU187
 677 003e 0020     		movs	r0, #0
 678              	.L28:
3981:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 83


 679              		.loc 1 3981 1 view .LVU188
 680 0040 BDE8F883 		pop	{r3, r4, r5, r6, r7, r8, r9, pc}
 681              	.LVL24:
 682              	.L31:
3977:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 683              		.loc 1 3977 14 view .LVU189
 684 0044 0320     		movs	r0, #3
 685 0046 FBE7     		b	.L28
 686              		.cfi_endproc
 687              	.LFE383:
 689              		.section	.text.HAL_SPI_MspInit,"ax",%progbits
 690              		.align	1
 691              		.weak	HAL_SPI_MspInit
 692              		.syntax unified
 693              		.thumb
 694              		.thumb_func
 696              	HAL_SPI_MspInit:
 697              	.LVL25:
 698              	.LFB337:
 534:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 699              		.loc 1 534 1 is_stmt 1 view -0
 700              		.cfi_startproc
 701              		@ args = 0, pretend = 0, frame = 0
 702              		@ frame_needed = 0, uses_anonymous_args = 0
 703              		@ link register save eliminated.
 536:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 704              		.loc 1 536 3 view .LVU191
 541:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 705              		.loc 1 541 1 is_stmt 0 view .LVU192
 706 0000 7047     		bx	lr
 707              		.cfi_endproc
 708              	.LFE337:
 710              		.section	.text.HAL_SPI_Init,"ax",%progbits
 711              		.align	1
 712              		.global	HAL_SPI_Init
 713              		.syntax unified
 714              		.thumb
 715              		.thumb_func
 717              	HAL_SPI_Init:
 718              	.LVL26:
 719              	.LFB335:
 240:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t crc_length;
 720              		.loc 1 240 1 is_stmt 1 view -0
 721              		.cfi_startproc
 722              		@ args = 0, pretend = 0, frame = 0
 723              		@ frame_needed = 0, uses_anonymous_args = 0
 241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t packet_length;
 724              		.loc 1 241 3 view .LVU194
 242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_SPI_CRC != 0UL)
 725              		.loc 1 242 3 view .LVU195
 248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 726              		.loc 1 248 3 view .LVU196
 248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 727              		.loc 1 248 6 is_stmt 0 view .LVU197
 728 0000 0028     		cmp	r0, #0
 729 0002 00F0B780 		beq	.L49
 240:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t crc_length;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 84


 730              		.loc 1 240 1 view .LVU198
 731 0006 70B5     		push	{r4, r5, r6, lr}
 732              		.cfi_def_cfa_offset 16
 733              		.cfi_offset 4, -16
 734              		.cfi_offset 5, -12
 735              		.cfi_offset 6, -8
 736              		.cfi_offset 14, -4
 737 0008 0446     		mov	r4, r0
 254:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_MODE(hspi->Init.Mode));
 738              		.loc 1 254 3 is_stmt 1 view .LVU199
 255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION(hspi->Init.Direction));
 739              		.loc 1 255 3 view .LVU200
 256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_DATASIZE(hspi->Init.DataSize));
 740              		.loc 1 256 3 view .LVU201
 257:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_FIFOTHRESHOLD(hspi->Init.FifoThreshold));
 741              		.loc 1 257 3 view .LVU202
 258:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_NSS(hspi->Init.NSS));
 742              		.loc 1 258 3 view .LVU203
 259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_NSSP(hspi->Init.NSSPMode));
 743              		.loc 1 259 3 view .LVU204
 260:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_BAUDRATE_PRESCALER(hspi->Init.BaudRatePrescaler));
 744              		.loc 1 260 3 view .LVU205
 261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_FIRST_BIT(hspi->Init.FirstBit));
 745              		.loc 1 261 3 view .LVU206
 262:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   assert_param(IS_SPI_TIMODE(hspi->Init.TIMode));
 746              		.loc 1 262 3 view .LVU207
 263:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (hspi->Init.TIMode == SPI_TIMODE_DISABLE)
 747              		.loc 1 263 3 view .LVU208
 264:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 748              		.loc 1 264 3 view .LVU209
 266:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     assert_param(IS_SPI_CPHA(hspi->Init.CLKPhase));
 749              		.loc 1 266 5 view .LVU210
 267:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 750              		.loc 1 267 5 view .LVU211
 279:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 751              		.loc 1 279 3 view .LVU212
 279:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 752              		.loc 1 279 29 is_stmt 0 view .LVU213
 753 000a 0023     		movs	r3, #0
 754 000c 8362     		str	r3, [r0, #40]
 283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 755              		.loc 1 283 3 is_stmt 1 view .LVU214
 283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 756              		.loc 1 283 9 is_stmt 0 view .LVU215
 757 000e 0568     		ldr	r5, [r0]
 758 0010 5C4B     		ldr	r3, .L60
 759 0012 5D4E     		ldr	r6, .L60+4
 283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 760              		.loc 1 283 6 view .LVU216
 761 0014 9D42     		cmp	r5, r3
 762 0016 18BF     		it	ne
 763 0018 B542     		cmpne	r5, r6
 764 001a 14BF     		ite	ne
 765 001c 0126     		movne	r6, #1
 766 001e 0026     		moveq	r6, #0
 767 0020 07D0     		beq	.L37
 283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 85


 768              		.loc 1 283 8 discriminator 1 view .LVU217
 769 0022 A3F57443 		sub	r3, r3, #62464
 770 0026 9D42     		cmp	r5, r3
 771 0028 03D0     		beq	.L37
 283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 772              		.loc 1 283 64 discriminator 2 view .LVU218
 773 002a C368     		ldr	r3, [r0, #12]
 283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 774              		.loc 1 283 50 discriminator 2 view .LVU219
 775 002c 0F2B     		cmp	r3, #15
 776 002e 00F2A380 		bhi	.L50
 777              	.L37:
 289:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (((!IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (packet_length > SPI_LOWEND_FIFO_SIZE)) ||
 778              		.loc 1 289 3 is_stmt 1 view .LVU220
 289:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (((!IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (packet_length > SPI_LOWEND_FIFO_SIZE)) ||
 779              		.loc 1 289 19 is_stmt 0 view .LVU221
 780 0032 2046     		mov	r0, r4
 781              	.LVL27:
 289:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   if (((!IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (packet_length > SPI_LOWEND_FIFO_SIZE)) ||
 782              		.loc 1 289 19 view .LVU222
 783 0034 FFF7FEFF 		bl	SPI_GetPacketSize
 784              	.LVL28:
 290:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (packet_length > SPI_HIGHEND_FIFO_SIZE)))
 785              		.loc 1 290 3 is_stmt 1 view .LVU223
 290:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (packet_length > SPI_HIGHEND_FIFO_SIZE)))
 786              		.loc 1 290 6 is_stmt 0 view .LVU224
 787 0038 2EB1     		cbz	r6, .L38
 290:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (packet_length > SPI_HIGHEND_FIFO_SIZE)))
 788              		.loc 1 290 9 discriminator 1 view .LVU225
 789 003a 544B     		ldr	r3, .L60+8
 790 003c 9D42     		cmp	r5, r3
 791 003e 02D0     		beq	.L38
 290:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (packet_length > SPI_HIGHEND_FIFO_SIZE)))
 792              		.loc 1 290 51 discriminator 3 view .LVU226
 793 0040 0828     		cmp	r0, #8
 794 0042 00F29B80 		bhi	.L51
 795              	.L38:
 290:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((IS_SPI_HIGHEND_INSTANCE(hspi->Instance)) && (packet_length > SPI_HIGHEND_FIFO_SIZE)))
 796              		.loc 1 290 94 discriminator 5 view .LVU227
 797 0046 4F4A     		ldr	r2, .L60
 798 0048 4F4B     		ldr	r3, .L60+4
 799 004a 9D42     		cmp	r5, r3
 800 004c 18BF     		it	ne
 801 004e 9542     		cmpne	r5, r2
 802 0050 03D0     		beq	.L39
 291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 803              		.loc 1 291 9 view .LVU228
 804 0052 03F58063 		add	r3, r3, #1024
 805 0056 9D42     		cmp	r5, r3
 806 0058 02D1     		bne	.L40
 807              	.L39:
 291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 808              		.loc 1 291 50 discriminator 1 view .LVU229
 809 005a 1028     		cmp	r0, #16
 810 005c 00F29080 		bhi	.L52
 811              	.L40:
 330:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 86


 812              		.loc 1 330 3 is_stmt 1 view .LVU230
 330:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 813              		.loc 1 330 11 is_stmt 0 view .LVU231
 814 0060 94F88130 		ldrb	r3, [r4, #129]	@ zero_extendqisi2
 330:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 815              		.loc 1 330 6 view .LVU232
 816 0064 F3B1     		cbz	r3, .L57
 817              	.LVL29:
 818              	.L41:
 360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 819              		.loc 1 360 3 is_stmt 1 view .LVU233
 360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 820              		.loc 1 360 15 is_stmt 0 view .LVU234
 821 0066 0223     		movs	r3, #2
 822 0068 84F88130 		strb	r3, [r4, #129]
 363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 823              		.loc 1 363 3 is_stmt 1 view .LVU235
 824 006c 2268     		ldr	r2, [r4]
 825 006e 1368     		ldr	r3, [r2]
 826 0070 23F00103 		bic	r3, r3, #1
 827 0074 1360     		str	r3, [r2]
 367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 828              		.loc 1 367 3 view .LVU236
 367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 829              		.loc 1 367 20 is_stmt 0 view .LVU237
 830 0076 2368     		ldr	r3, [r4]
 367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 831              		.loc 1 367 30 view .LVU238
 832 0078 9A68     		ldr	r2, [r3, #8]
 367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 833              		.loc 1 367 14 view .LVU239
 834 007a 02F4F812 		and	r2, r2, #2031616
 835              	.LVL30:
 375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                             (hspi->Init.NSSPolarity == SPI_NSS_POLARITY_LOW)) || \
 836              		.loc 1 375 3 is_stmt 1 view .LVU240
 375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                             (hspi->Init.NSSPolarity == SPI_NSS_POLARITY_LOW)) || \
 837              		.loc 1 375 18 is_stmt 0 view .LVU241
 838 007e A169     		ldr	r1, [r4, #24]
 375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                             (hspi->Init.NSSPolarity == SPI_NSS_POLARITY_LOW)) || \
 839              		.loc 1 375 6 view .LVU242
 840 0080 B1F1806F 		cmp	r1, #67108864
 841 0084 14D0     		beq	.L58
 842              	.L42:
 384:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 843              		.loc 1 384 3 is_stmt 1 view .LVU243
 384:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 844              		.loc 1 384 19 is_stmt 0 view .LVU244
 845 0086 6368     		ldr	r3, [r4, #4]
 384:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 846              		.loc 1 384 6 view .LVU245
 847 0088 13F4800F 		tst	r3, #4194304
 848 008c 23D0     		beq	.L45
 384:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 849              		.loc 1 384 78 discriminator 1 view .LVU246
 850 008e E368     		ldr	r3, [r4, #12]
 384:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 851              		.loc 1 384 64 discriminator 1 view .LVU247
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 87


 852 0090 062B     		cmp	r3, #6
 853 0092 20D9     		bls	.L45
 386:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 854              		.loc 1 386 5 is_stmt 1 view .LVU248
 855 0094 2168     		ldr	r1, [r4]
 856 0096 0B68     		ldr	r3, [r1]
 857 0098 23F48073 		bic	r3, r3, #256
 858 009c 206D     		ldr	r0, [r4, #80]
 859 009e 0343     		orrs	r3, r3, r0
 860 00a0 0B60     		str	r3, [r1]
 861 00a2 1DE0     		b	.L46
 862              	.LVL31:
 863              	.L57:
 333:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 864              		.loc 1 333 5 view .LVU249
 333:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 865              		.loc 1 333 16 is_stmt 0 view .LVU250
 866 00a4 84F88030 		strb	r3, [r4, #128]
 356:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 867              		.loc 1 356 5 is_stmt 1 view .LVU251
 868 00a8 2046     		mov	r0, r4
 869              	.LVL32:
 356:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 870              		.loc 1 356 5 is_stmt 0 view .LVU252
 871 00aa FFF7FEFF 		bl	HAL_SPI_MspInit
 872              	.LVL33:
 873 00ae DAE7     		b	.L41
 874              	.LVL34:
 875              	.L58:
 375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                             (hspi->Init.NSSPolarity == SPI_NSS_POLARITY_LOW)) || \
 876              		.loc 1 375 56 discriminator 1 view .LVU253
 877 00b0 6168     		ldr	r1, [r4, #4]
 375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                             (hspi->Init.NSSPolarity == SPI_NSS_POLARITY_LOW)) || \
 878              		.loc 1 375 40 discriminator 1 view .LVU254
 879 00b2 B1F5800F 		cmp	r1, #4194304
 880 00b6 06D0     		beq	.L59
 881              	.L43:
 376:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                            ((hspi->Init.Mode == SPI_MODE_SLAVE) && \
 882              		.loc 1 376 95 view .LVU255
 883 00b8 0029     		cmp	r1, #0
 884 00ba E4D1     		bne	.L42
 378:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 885              		.loc 1 378 56 view .LVU256
 886 00bc A16B     		ldr	r1, [r4, #56]
 377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                             (hspi->Init.NSSPolarity == SPI_NSS_POLARITY_HIGH))))
 887              		.loc 1 377 81 view .LVU257
 888 00be B1F1805F 		cmp	r1, #268435456
 889 00c2 E0D1     		bne	.L42
 890 00c4 02E0     		b	.L44
 891              	.L59:
 376:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                            ((hspi->Init.Mode == SPI_MODE_SLAVE) && \
 892              		.loc 1 376 56 view .LVU258
 893 00c6 A06B     		ldr	r0, [r4, #56]
 375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                             (hspi->Init.NSSPolarity == SPI_NSS_POLARITY_LOW)) || \
 894              		.loc 1 375 82 discriminator 2 view .LVU259
 895 00c8 0028     		cmp	r0, #0
 896 00ca F5D1     		bne	.L43
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 88


 897              	.L44:
 380:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 898              		.loc 1 380 5 is_stmt 1 view .LVU260
 899 00cc 1968     		ldr	r1, [r3]
 900 00ce 41F48051 		orr	r1, r1, #4096
 901 00d2 1960     		str	r1, [r3]
 902 00d4 D7E7     		b	.L42
 903              	.L45:
 390:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 904              		.loc 1 390 5 view .LVU261
 905 00d6 2168     		ldr	r1, [r4]
 906 00d8 0B68     		ldr	r3, [r1]
 907 00da 23F48073 		bic	r3, r3, #256
 908 00de 0B60     		str	r3, [r1]
 909              	.L46:
 394:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                    hspi->Init.FifoThreshold     | hspi->Init.DataSize));
 910              		.loc 1 394 3 view .LVU262
 911 00e0 E369     		ldr	r3, [r4, #28]
 912 00e2 A16A     		ldr	r1, [r4, #40]
 913 00e4 0B43     		orrs	r3, r3, r1
 914 00e6 1343     		orrs	r3, r3, r2
 915 00e8 E26B     		ldr	r2, [r4, #60]
 916              	.LVL35:
 394:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                    hspi->Init.FifoThreshold     | hspi->Init.DataSize));
 917              		.loc 1 394 3 is_stmt 0 view .LVU263
 918 00ea 1343     		orrs	r3, r3, r2
 919 00ec E168     		ldr	r1, [r4, #12]
 920 00ee 2268     		ldr	r2, [r4]
 921 00f0 0B43     		orrs	r3, r3, r1
 922 00f2 9360     		str	r3, [r2, #8]
 398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                    hspi->Init.NSSPolarity             | hspi->Init.NSS       |
 923              		.loc 1 398 3 is_stmt 1 view .LVU264
 924 00f4 636B     		ldr	r3, [r4, #52]
 925 00f6 626A     		ldr	r2, [r4, #36]
 926 00f8 1343     		orrs	r3, r3, r2
 927 00fa A26B     		ldr	r2, [r4, #56]
 928 00fc 1343     		orrs	r3, r3, r2
 929 00fe A269     		ldr	r2, [r4, #24]
 930 0100 1343     		orrs	r3, r3, r2
 931 0102 2269     		ldr	r2, [r4, #16]
 932 0104 1343     		orrs	r3, r3, r2
 933 0106 6269     		ldr	r2, [r4, #20]
 934 0108 1343     		orrs	r3, r3, r2
 935 010a 226A     		ldr	r2, [r4, #32]
 936 010c 1343     		orrs	r3, r3, r2
 937 010e 6268     		ldr	r2, [r4, #4]
 938 0110 1343     		orrs	r3, r3, r2
 939 0112 E26C     		ldr	r2, [r4, #76]
 940 0114 1343     		orrs	r3, r3, r2
 941 0116 A268     		ldr	r2, [r4, #8]
 942 0118 1343     		orrs	r3, r3, r2
 943 011a A26C     		ldr	r2, [r4, #72]
 944 011c 1343     		orrs	r3, r3, r2
 945 011e A16D     		ldr	r1, [r4, #88]
 946 0120 2268     		ldr	r2, [r4]
 947 0122 0B43     		orrs	r3, r3, r1
 948 0124 D360     		str	r3, [r2, #12]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 89


 453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 949              		.loc 1 453 3 view .LVU265
 453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 950              		.loc 1 453 17 is_stmt 0 view .LVU266
 951 0126 6368     		ldr	r3, [r4, #4]
 453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 952              		.loc 1 453 6 view .LVU267
 953 0128 6BB9     		cbnz	r3, .L47
 460:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 954              		.loc 1 460 7 is_stmt 1 view .LVU268
 955 012a 2268     		ldr	r2, [r4]
 956 012c 9368     		ldr	r3, [r2, #8]
 957 012e 23F4C053 		bic	r3, r3, #6144
 958 0132 43F40063 		orr	r3, r3, #2048
 959 0136 9360     		str	r3, [r2, #8]
 462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 960              		.loc 1 462 5 view .LVU269
 961 0138 2268     		ldr	r2, [r4]
 962 013a 9368     		ldr	r3, [r2, #8]
 963 013c 23F4C063 		bic	r3, r3, #1536
 964 0140 43F48063 		orr	r3, r3, #1024
 965 0144 9360     		str	r3, [r2, #8]
 966              	.L47:
 467:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* SPI_I2SCFGR_I2SMOD */
 967              		.loc 1 467 3 view .LVU270
 968 0146 2268     		ldr	r2, [r4]
 969 0148 136D     		ldr	r3, [r2, #80]
 970 014a 23F00103 		bic	r3, r3, #1
 971 014e 1365     		str	r3, [r2, #80]
 471:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 972              		.loc 1 471 3 view .LVU271
 471:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 973              		.loc 1 471 18 is_stmt 0 view .LVU272
 974 0150 6368     		ldr	r3, [r4, #4]
 471:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 975              		.loc 1 471 6 view .LVU273
 976 0152 13F4800F 		tst	r3, #4194304
 977 0156 06D0     		beq	.L48
 474:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 978              		.loc 1 474 5 is_stmt 1 view .LVU274
 979 0158 2268     		ldr	r2, [r4]
 980 015a D368     		ldr	r3, [r2, #12]
 981 015c 23F00043 		bic	r3, r3, #-2147483648
 982 0160 616D     		ldr	r1, [r4, #84]
 983 0162 0B43     		orrs	r3, r3, r1
 984 0164 D360     		str	r3, [r2, #12]
 985              	.L48:
 477:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State     = HAL_SPI_STATE_READY;
 986              		.loc 1 477 3 view .LVU275
 477:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State     = HAL_SPI_STATE_READY;
 987              		.loc 1 477 19 is_stmt 0 view .LVU276
 988 0166 0020     		movs	r0, #0
 989 0168 C4F88400 		str	r0, [r4, #132]
 478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 990              		.loc 1 478 3 is_stmt 1 view .LVU277
 478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 991              		.loc 1 478 19 is_stmt 0 view .LVU278
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 90


 992 016c 0123     		movs	r3, #1
 993 016e 84F88130 		strb	r3, [r4, #129]
 480:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 994              		.loc 1 480 3 is_stmt 1 view .LVU279
 995              	.LVL36:
 996              	.L36:
 481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 997              		.loc 1 481 1 is_stmt 0 view .LVU280
 998 0172 70BD     		pop	{r4, r5, r6, pc}
 999              	.LVL37:
 1000              	.L49:
 1001              		.cfi_def_cfa_offset 0
 1002              		.cfi_restore 4
 1003              		.cfi_restore 5
 1004              		.cfi_restore 6
 1005              		.cfi_restore 14
 250:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1006              		.loc 1 250 12 view .LVU281
 1007 0174 0120     		movs	r0, #1
 1008              	.LVL38:
 481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1009              		.loc 1 481 1 view .LVU282
 1010 0176 7047     		bx	lr
 1011              	.LVL39:
 1012              	.L50:
 1013              		.cfi_def_cfa_offset 16
 1014              		.cfi_offset 4, -16
 1015              		.cfi_offset 5, -12
 1016              		.cfi_offset 6, -8
 1017              		.cfi_offset 14, -4
 285:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1018              		.loc 1 285 12 view .LVU283
 1019 0178 0120     		movs	r0, #1
 1020              	.LVL40:
 285:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1021              		.loc 1 285 12 view .LVU284
 1022 017a FAE7     		b	.L36
 1023              	.LVL41:
 1024              	.L51:
 293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1025              		.loc 1 293 12 view .LVU285
 1026 017c 0120     		movs	r0, #1
 1027              	.LVL42:
 293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1028              		.loc 1 293 12 view .LVU286
 1029 017e F8E7     		b	.L36
 1030              	.LVL43:
 1031              	.L52:
 293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1032              		.loc 1 293 12 view .LVU287
 1033 0180 0120     		movs	r0, #1
 1034              	.LVL44:
 293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1035              		.loc 1 293 12 view .LVU288
 1036 0182 F6E7     		b	.L36
 1037              	.L61:
 1038              		.align	2
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 91


 1039              	.L60:
 1040 0184 00300140 		.word	1073819648
 1041 0188 00380040 		.word	1073756160
 1042 018c 003C0040 		.word	1073757184
 1043              		.cfi_endproc
 1044              	.LFE335:
 1046              		.section	.text.HAL_SPI_MspDeInit,"ax",%progbits
 1047              		.align	1
 1048              		.weak	HAL_SPI_MspDeInit
 1049              		.syntax unified
 1050              		.thumb
 1051              		.thumb_func
 1053              	HAL_SPI_MspDeInit:
 1054              	.LVL45:
 1055              	.LFB338:
 550:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 1056              		.loc 1 550 1 is_stmt 1 view -0
 1057              		.cfi_startproc
 1058              		@ args = 0, pretend = 0, frame = 0
 1059              		@ frame_needed = 0, uses_anonymous_args = 0
 1060              		@ link register save eliminated.
 552:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1061              		.loc 1 552 3 view .LVU290
 557:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1062              		.loc 1 557 1 is_stmt 0 view .LVU291
 1063 0000 7047     		bx	lr
 1064              		.cfi_endproc
 1065              	.LFE338:
 1067              		.section	.text.HAL_SPI_DeInit,"ax",%progbits
 1068              		.align	1
 1069              		.global	HAL_SPI_DeInit
 1070              		.syntax unified
 1071              		.thumb
 1072              		.thumb_func
 1074              	HAL_SPI_DeInit:
 1075              	.LVL46:
 1076              	.LFB336:
 490:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check the SPI handle allocation */
 1077              		.loc 1 490 1 is_stmt 1 view -0
 1078              		.cfi_startproc
 1079              		@ args = 0, pretend = 0, frame = 0
 1080              		@ frame_needed = 0, uses_anonymous_args = 0
 492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1081              		.loc 1 492 3 view .LVU293
 492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1082              		.loc 1 492 6 is_stmt 0 view .LVU294
 1083 0000 98B1     		cbz	r0, .L65
 490:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check the SPI handle allocation */
 1084              		.loc 1 490 1 view .LVU295
 1085 0002 10B5     		push	{r4, lr}
 1086              		.cfi_def_cfa_offset 8
 1087              		.cfi_offset 4, -8
 1088              		.cfi_offset 14, -4
 1089 0004 0446     		mov	r4, r0
 498:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1090              		.loc 1 498 3 is_stmt 1 view .LVU296
 500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 92


 1091              		.loc 1 500 3 view .LVU297
 500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1092              		.loc 1 500 15 is_stmt 0 view .LVU298
 1093 0006 0223     		movs	r3, #2
 1094 0008 80F88130 		strb	r3, [r0, #129]
 503:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1095              		.loc 1 503 3 is_stmt 1 view .LVU299
 1096 000c 0268     		ldr	r2, [r0]
 1097 000e 1368     		ldr	r3, [r2]
 1098 0010 23F00103 		bic	r3, r3, #1
 1099 0014 1360     		str	r3, [r2]
 515:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 1100              		.loc 1 515 3 view .LVU300
 1101 0016 FFF7FEFF 		bl	HAL_SPI_MspDeInit
 1102              	.LVL47:
 518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_RESET;
 1103              		.loc 1 518 3 view .LVU301
 518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_RESET;
 1104              		.loc 1 518 19 is_stmt 0 view .LVU302
 1105 001a 0020     		movs	r0, #0
 1106 001c C4F88400 		str	r0, [r4, #132]
 519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1107              		.loc 1 519 3 is_stmt 1 view .LVU303
 519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1108              		.loc 1 519 15 is_stmt 0 view .LVU304
 1109 0020 84F88100 		strb	r0, [r4, #129]
 522:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1110              		.loc 1 522 3 is_stmt 1 view .LVU305
 522:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1111              		.loc 1 522 3 view .LVU306
 1112 0024 84F88000 		strb	r0, [r4, #128]
 522:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1113              		.loc 1 522 3 view .LVU307
 524:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 1114              		.loc 1 524 3 view .LVU308
 525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1115              		.loc 1 525 1 is_stmt 0 view .LVU309
 1116 0028 10BD     		pop	{r4, pc}
 1117              	.LVL48:
 1118              	.L65:
 1119              		.cfi_def_cfa_offset 0
 1120              		.cfi_restore 4
 1121              		.cfi_restore 14
 494:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1122              		.loc 1 494 12 view .LVU310
 1123 002a 0120     		movs	r0, #1
 1124              	.LVL49:
 525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1125              		.loc 1 525 1 view .LVU311
 1126 002c 7047     		bx	lr
 1127              		.cfi_endproc
 1128              	.LFE336:
 1130              		.section	.text.HAL_SPI_Transmit,"ax",%progbits
 1131              		.align	1
 1132              		.global	HAL_SPI_Transmit
 1133              		.syntax unified
 1134              		.thumb
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 93


 1135              		.thumb_func
 1137              	HAL_SPI_Transmit:
 1138              	.LVL50:
 1139              	.LFB339:
 825:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 1140              		.loc 1 825 1 is_stmt 1 view -0
 1141              		.cfi_startproc
 1142              		@ args = 0, pretend = 0, frame = 0
 1143              		@ frame_needed = 0, uses_anonymous_args = 0
 825:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 1144              		.loc 1 825 1 is_stmt 0 view .LVU313
 1145 0000 2DE9F047 		push	{r4, r5, r6, r7, r8, r9, r10, lr}
 1146              		.cfi_def_cfa_offset 32
 1147              		.cfi_offset 4, -32
 1148              		.cfi_offset 5, -28
 1149              		.cfi_offset 6, -24
 1150              		.cfi_offset 7, -20
 1151              		.cfi_offset 8, -16
 1152              		.cfi_offset 9, -12
 1153              		.cfi_offset 10, -8
 1154              		.cfi_offset 14, -4
 1155 0004 82B0     		sub	sp, sp, #8
 1156              		.cfi_def_cfa_offset 40
 1157 0006 0446     		mov	r4, r0
 1158 0008 8A46     		mov	r10, r1
 1159 000a 9146     		mov	r9, r2
 1160 000c 1D46     		mov	r5, r3
 827:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
 1161              		.loc 1 827 3 is_stmt 1 view .LVU314
 827:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
 1162              		.loc 1 827 57 is_stmt 0 view .LVU315
 1163 000e D0F80080 		ldr	r8, [r0]
 1164              	.LVL51:
 830:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1165              		.loc 1 830 3 is_stmt 1 view .LVU316
 833:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1166              		.loc 1 833 3 view .LVU317
 836:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1167              		.loc 1 836 3 view .LVU318
 836:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1168              		.loc 1 836 15 is_stmt 0 view .LVU319
 1169 0012 FFF7FEFF 		bl	HAL_GetTick
 1170              	.LVL52:
 838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1171              		.loc 1 838 3 is_stmt 1 view .LVU320
 838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1172              		.loc 1 838 11 is_stmt 0 view .LVU321
 1173 0016 94F88130 		ldrb	r3, [r4, #129]	@ zero_extendqisi2
 838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1174              		.loc 1 838 6 view .LVU322
 1175 001a 012B     		cmp	r3, #1
 1176 001c 40F04981 		bne	.L99
 1177 0020 0646     		mov	r6, r0
 1178 0022 DFB2     		uxtb	r7, r3
 843:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1179              		.loc 1 843 3 is_stmt 1 view .LVU323
 843:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 94


 1180              		.loc 1 843 6 is_stmt 0 view .LVU324
 1181 0024 B9F1000F 		cmp	r9, #0
 1182 0028 18BF     		it	ne
 1183 002a BAF1000F 		cmpne	r10, #0
 1184 002e 00F04181 		beq	.L71
 849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1185              		.loc 1 849 3 is_stmt 1 view .LVU325
 849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1186              		.loc 1 849 3 view .LVU326
 1187 0032 94F88030 		ldrb	r3, [r4, #128]	@ zero_extendqisi2
 1188 0036 012B     		cmp	r3, #1
 1189 0038 00F04081 		beq	.L100
 849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1190              		.loc 1 849 3 discriminator 2 view .LVU327
 1191 003c 0123     		movs	r3, #1
 1192 003e 84F88030 		strb	r3, [r4, #128]
 849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1193              		.loc 1 849 3 view .LVU328
 852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 1194              		.loc 1 852 3 view .LVU329
 852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 1195              		.loc 1 852 21 is_stmt 0 view .LVU330
 1196 0042 0323     		movs	r3, #3
 1197 0044 84F88130 		strb	r3, [r4, #129]
 853:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pData;
 1198              		.loc 1 853 3 is_stmt 1 view .LVU331
 853:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pData;
 1199              		.loc 1 853 21 is_stmt 0 view .LVU332
 1200 0048 0023     		movs	r3, #0
 1201 004a C4F88430 		str	r3, [r4, #132]
 854:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 1202              		.loc 1 854 3 is_stmt 1 view .LVU333
 854:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 1203              		.loc 1 854 21 is_stmt 0 view .LVU334
 1204 004e C4F85CA0 		str	r10, [r4, #92]
 855:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 1205              		.loc 1 855 3 is_stmt 1 view .LVU335
 855:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 1206              		.loc 1 855 21 is_stmt 0 view .LVU336
 1207 0052 A4F86090 		strh	r9, [r4, #96]	@ movhi
 856:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1208              		.loc 1 856 3 is_stmt 1 view .LVU337
 856:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1209              		.loc 1 856 21 is_stmt 0 view .LVU338
 1210 0056 A4F86290 		strh	r9, [r4, #98]	@ movhi
 859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = (uint16_t) 0UL;
 1211              		.loc 1 859 3 is_stmt 1 view .LVU339
 859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = (uint16_t) 0UL;
 1212              		.loc 1 859 21 is_stmt 0 view .LVU340
 1213 005a 6366     		str	r3, [r4, #100]
 860:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t) 0UL;
 1214              		.loc 1 860 3 is_stmt 1 view .LVU341
 860:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t) 0UL;
 1215              		.loc 1 860 21 is_stmt 0 view .LVU342
 1216 005c A4F86830 		strh	r3, [r4, #104]	@ movhi
 861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 1217              		.loc 1 861 3 is_stmt 1 view .LVU343
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 95


 861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 1218              		.loc 1 861 21 is_stmt 0 view .LVU344
 1219 0060 A4F86A30 		strh	r3, [r4, #106]	@ movhi
 862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
 1220              		.loc 1 862 3 is_stmt 1 view .LVU345
 862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
 1221              		.loc 1 862 21 is_stmt 0 view .LVU346
 1222 0064 6367     		str	r3, [r4, #116]
 863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1223              		.loc 1 863 3 is_stmt 1 view .LVU347
 863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1224              		.loc 1 863 21 is_stmt 0 view .LVU348
 1225 0066 2367     		str	r3, [r4, #112]
 866:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1226              		.loc 1 866 3 is_stmt 1 view .LVU349
 866:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1227              		.loc 1 866 17 is_stmt 0 view .LVU350
 1228 0068 A368     		ldr	r3, [r4, #8]
 866:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1229              		.loc 1 866 6 view .LVU351
 1230 006a B3F5C02F 		cmp	r3, #393216
 1231 006e 1CD0     		beq	.L104
 872:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1232              		.loc 1 872 5 is_stmt 1 view .LVU352
 1233 0070 2268     		ldr	r2, [r4]
 1234 0072 D368     		ldr	r3, [r2, #12]
 1235 0074 23F4C023 		bic	r3, r3, #393216
 1236 0078 43F40033 		orr	r3, r3, #131072
 1237 007c D360     		str	r3, [r2, #12]
 1238              	.L73:
 876:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1239              		.loc 1 876 3 view .LVU353
 1240 007e 2268     		ldr	r2, [r4]
 1241 0080 5368     		ldr	r3, [r2, #4]
 1242 0082 6FF30F03 		bfc	r3, #0, #16
 1243 0086 49EA0303 		orr	r3, r9, r3
 1244 008a 5360     		str	r3, [r2, #4]
 879:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1245              		.loc 1 879 3 view .LVU354
 1246 008c 2268     		ldr	r2, [r4]
 1247 008e 1368     		ldr	r3, [r2]
 1248 0090 43F00103 		orr	r3, r3, #1
 1249 0094 1360     		str	r3, [r2]
 881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1250              		.loc 1 881 3 view .LVU355
 881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1251              		.loc 1 881 17 is_stmt 0 view .LVU356
 1252 0096 6368     		ldr	r3, [r4, #4]
 881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1253              		.loc 1 881 6 view .LVU357
 1254 0098 B3F5800F 		cmp	r3, #4194304
 1255 009c 0BD0     		beq	.L105
 1256              	.L74:
 888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1257              		.loc 1 888 3 is_stmt 1 view .LVU358
 888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1258              		.loc 1 888 17 is_stmt 0 view .LVU359
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 96


 1259 009e E368     		ldr	r3, [r4, #12]
 888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1260              		.loc 1 888 6 view .LVU360
 1261 00a0 0F2B     		cmp	r3, #15
 1262 00a2 1BD8     		bhi	.L75
 920:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1263              		.loc 1 920 8 is_stmt 1 view .LVU361
 920:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1264              		.loc 1 920 11 is_stmt 0 view .LVU362
 1265 00a4 072B     		cmp	r3, #7
 1266 00a6 4DD8     		bhi	.L83
 1267 00a8 ACE0     		b	.L84
 1268              	.L104:
 868:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1269              		.loc 1 868 5 is_stmt 1 view .LVU363
 1270 00aa 2268     		ldr	r2, [r4]
 1271 00ac 1368     		ldr	r3, [r2]
 1272 00ae 43F40063 		orr	r3, r3, #2048
 1273 00b2 1360     		str	r3, [r2]
 1274 00b4 E3E7     		b	.L73
 1275              	.L105:
 884:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1276              		.loc 1 884 5 view .LVU364
 1277 00b6 2268     		ldr	r2, [r4]
 1278 00b8 1368     		ldr	r3, [r2]
 1279 00ba 43F40073 		orr	r3, r3, #512
 1280 00be 1360     		str	r3, [r2]
 1281 00c0 EDE7     		b	.L74
 1282              	.LVL53:
 1283              	.L106:
 896:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint32_t);
 1284              		.loc 1 896 9 view .LVU365
 896:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint32_t);
 1285              		.loc 1 896 77 is_stmt 0 view .LVU366
 1286 00c2 E26D     		ldr	r2, [r4, #92]
 896:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint32_t);
 1287              		.loc 1 896 53 view .LVU367
 1288 00c4 1268     		ldr	r2, [r2]
 896:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint32_t);
 1289              		.loc 1 896 51 view .LVU368
 1290 00c6 1A62     		str	r2, [r3, #32]
 897:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount--;
 1291              		.loc 1 897 9 is_stmt 1 view .LVU369
 897:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount--;
 1292              		.loc 1 897 13 is_stmt 0 view .LVU370
 1293 00c8 E36D     		ldr	r3, [r4, #92]
 897:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount--;
 1294              		.loc 1 897 26 view .LVU371
 1295 00ca 0433     		adds	r3, r3, #4
 1296 00cc E365     		str	r3, [r4, #92]
 898:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 1297              		.loc 1 898 9 is_stmt 1 view .LVU372
 898:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 1298              		.loc 1 898 13 is_stmt 0 view .LVU373
 1299 00ce B4F86220 		ldrh	r2, [r4, #98]
 1300 00d2 92B2     		uxth	r2, r2
 898:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 97


 1301              		.loc 1 898 26 view .LVU374
 1302 00d4 013A     		subs	r2, r2, #1
 1303 00d6 92B2     		uxth	r2, r2
 1304 00d8 A4F86220 		strh	r2, [r4, #98]	@ movhi
 1305              	.L75:
 891:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 1306              		.loc 1 891 30 is_stmt 1 view .LVU375
 891:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 1307              		.loc 1 891 16 is_stmt 0 view .LVU376
 1308 00dc B4F86230 		ldrh	r3, [r4, #98]
 1309 00e0 9BB2     		uxth	r3, r3
 891:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 1310              		.loc 1 891 30 view .LVU377
 1311 00e2 002B     		cmp	r3, #0
 1312 00e4 00F0C980 		beq	.L82
 894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1313              		.loc 1 894 7 is_stmt 1 view .LVU378
 894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1314              		.loc 1 894 11 is_stmt 0 view .LVU379
 1315 00e8 2368     		ldr	r3, [r4]
 1316 00ea 5A69     		ldr	r2, [r3, #20]
 894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1317              		.loc 1 894 10 view .LVU380
 1318 00ec 12F0020F 		tst	r2, #2
 1319 00f0 E7D1     		bne	.L106
 903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1320              		.loc 1 903 9 is_stmt 1 view .LVU381
 903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1321              		.loc 1 903 16 is_stmt 0 view .LVU382
 1322 00f2 FFF7FEFF 		bl	HAL_GetTick
 1323              	.LVL54:
 903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1324              		.loc 1 903 30 discriminator 1 view .LVU383
 1325 00f6 801B     		subs	r0, r0, r6
 903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1326              		.loc 1 903 12 discriminator 1 view .LVU384
 1327 00f8 A842     		cmp	r0, r5
 1328 00fa 02D3     		bcc	.L79
 903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1329              		.loc 1 903 56 discriminator 1 view .LVU385
 1330 00fc B5F1FF3F 		cmp	r5, #-1
 1331 0100 01D1     		bne	.L80
 1332              	.L79:
 903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1333              		.loc 1 903 87 discriminator 3 view .LVU386
 1334 0102 002D     		cmp	r5, #0
 1335 0104 EAD1     		bne	.L75
 1336              	.L80:
 906:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1337              		.loc 1 906 11 is_stmt 1 view .LVU387
 1338 0106 2046     		mov	r0, r4
 1339 0108 FFF7FEFF 		bl	SPI_CloseTransfer
 1340              	.LVL55:
 908:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 1341              		.loc 1 908 11 view .LVU388
 1342 010c D4F88430 		ldr	r3, [r4, #132]
 1343 0110 43F48073 		orr	r3, r3, #256
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 98


 1344 0114 C4F88430 		str	r3, [r4, #132]
 909:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1345              		.loc 1 909 11 view .LVU389
 909:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1346              		.loc 1 909 23 is_stmt 0 view .LVU390
 1347 0118 0123     		movs	r3, #1
 1348 011a 84F88130 		strb	r3, [r4, #129]
 912:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1349              		.loc 1 912 11 is_stmt 1 view .LVU391
 912:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1350              		.loc 1 912 11 view .LVU392
 1351 011e 0023     		movs	r3, #0
 1352 0120 84F88030 		strb	r3, [r4, #128]
 912:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1353              		.loc 1 912 11 view .LVU393
 914:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1354              		.loc 1 914 11 view .LVU394
 914:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1355              		.loc 1 914 18 is_stmt 0 view .LVU395
 1356 0124 0327     		movs	r7, #3
 1357 0126 C5E0     		b	.L71
 1358              	.L86:
 937:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1359              		.loc 1 937 11 is_stmt 1 view .LVU396
 937:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1360              		.loc 1 937 51 is_stmt 0 view .LVU397
 1361 0128 E36D     		ldr	r3, [r4, #92]
 937:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1362              		.loc 1 937 27 view .LVU398
 1363 012a 1B88     		ldrh	r3, [r3]
 937:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1364              		.loc 1 937 25 view .LVU399
 1365 012c A8F82030 		strh	r3, [r8, #32]	@ movhi
 941:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount--;
 1366              		.loc 1 941 11 is_stmt 1 view .LVU400
 941:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount--;
 1367              		.loc 1 941 15 is_stmt 0 view .LVU401
 1368 0130 E36D     		ldr	r3, [r4, #92]
 941:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount--;
 1369              		.loc 1 941 28 view .LVU402
 1370 0132 0233     		adds	r3, r3, #2
 1371 0134 E365     		str	r3, [r4, #92]
 942:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1372              		.loc 1 942 11 is_stmt 1 view .LVU403
 942:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1373              		.loc 1 942 15 is_stmt 0 view .LVU404
 1374 0136 B4F86230 		ldrh	r3, [r4, #98]
 1375 013a 9BB2     		uxth	r3, r3
 942:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1376              		.loc 1 942 28 view .LVU405
 1377 013c 013B     		subs	r3, r3, #1
 1378 013e 9BB2     		uxth	r3, r3
 1379 0140 A4F86230 		strh	r3, [r4, #98]	@ movhi
 1380              	.L83:
 923:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 1381              		.loc 1 923 30 is_stmt 1 view .LVU406
 923:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 99


 1382              		.loc 1 923 16 is_stmt 0 view .LVU407
 1383 0144 B4F86230 		ldrh	r3, [r4, #98]
 1384 0148 9BB2     		uxth	r3, r3
 923:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 1385              		.loc 1 923 30 view .LVU408
 1386 014a 002B     		cmp	r3, #0
 1387 014c 00F09580 		beq	.L82
 926:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1388              		.loc 1 926 7 is_stmt 1 view .LVU409
 926:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1389              		.loc 1 926 11 is_stmt 0 view .LVU410
 1390 0150 2268     		ldr	r2, [r4]
 1391 0152 5369     		ldr	r3, [r2, #20]
 926:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1392              		.loc 1 926 10 view .LVU411
 1393 0154 13F0020F 		tst	r3, #2
 1394 0158 15D0     		beq	.L85
 928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1395              		.loc 1 928 9 is_stmt 1 view .LVU412
 928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1396              		.loc 1 928 18 is_stmt 0 view .LVU413
 1397 015a B4F86230 		ldrh	r3, [r4, #98]
 1398 015e 9BB2     		uxth	r3, r3
 928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1399              		.loc 1 928 12 view .LVU414
 1400 0160 012B     		cmp	r3, #1
 1401 0162 E1D9     		bls	.L86
 928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1402              		.loc 1 928 53 discriminator 1 view .LVU415
 1403 0164 E36B     		ldr	r3, [r4, #60]
 928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1404              		.loc 1 928 39 discriminator 1 view .LVU416
 1405 0166 002B     		cmp	r3, #0
 1406 0168 DED0     		beq	.L86
 930:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint32_t);
 1407              		.loc 1 930 11 is_stmt 1 view .LVU417
 930:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint32_t);
 1408              		.loc 1 930 79 is_stmt 0 view .LVU418
 1409 016a E36D     		ldr	r3, [r4, #92]
 930:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint32_t);
 1410              		.loc 1 930 55 view .LVU419
 1411 016c 1B68     		ldr	r3, [r3]
 930:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint32_t);
 1412              		.loc 1 930 53 view .LVU420
 1413 016e 1362     		str	r3, [r2, #32]
 931:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount -= (uint16_t)2UL;
 1414              		.loc 1 931 11 is_stmt 1 view .LVU421
 931:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount -= (uint16_t)2UL;
 1415              		.loc 1 931 15 is_stmt 0 view .LVU422
 1416 0170 E36D     		ldr	r3, [r4, #92]
 931:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount -= (uint16_t)2UL;
 1417              		.loc 1 931 28 view .LVU423
 1418 0172 0433     		adds	r3, r3, #4
 1419 0174 E365     		str	r3, [r4, #92]
 932:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1420              		.loc 1 932 11 is_stmt 1 view .LVU424
 932:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 100


 1421              		.loc 1 932 15 is_stmt 0 view .LVU425
 1422 0176 B4F86230 		ldrh	r3, [r4, #98]
 1423 017a 9BB2     		uxth	r3, r3
 932:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1424              		.loc 1 932 29 view .LVU426
 1425 017c 023B     		subs	r3, r3, #2
 1426 017e 9BB2     		uxth	r3, r3
 1427 0180 A4F86230 		strh	r3, [r4, #98]	@ movhi
 1428 0184 DEE7     		b	.L83
 1429              	.L85:
 948:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1430              		.loc 1 948 9 is_stmt 1 view .LVU427
 948:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1431              		.loc 1 948 16 is_stmt 0 view .LVU428
 1432 0186 FFF7FEFF 		bl	HAL_GetTick
 1433              	.LVL56:
 948:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1434              		.loc 1 948 30 discriminator 1 view .LVU429
 1435 018a 801B     		subs	r0, r0, r6
 948:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1436              		.loc 1 948 12 discriminator 1 view .LVU430
 1437 018c A842     		cmp	r0, r5
 1438 018e 02D3     		bcc	.L88
 948:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1439              		.loc 1 948 56 discriminator 1 view .LVU431
 1440 0190 B5F1FF3F 		cmp	r5, #-1
 1441 0194 01D1     		bne	.L89
 1442              	.L88:
 948:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1443              		.loc 1 948 87 discriminator 3 view .LVU432
 1444 0196 002D     		cmp	r5, #0
 1445 0198 D4D1     		bne	.L83
 1446              	.L89:
 951:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1447              		.loc 1 951 11 is_stmt 1 view .LVU433
 1448 019a 2046     		mov	r0, r4
 1449 019c FFF7FEFF 		bl	SPI_CloseTransfer
 1450              	.LVL57:
 953:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 1451              		.loc 1 953 11 view .LVU434
 1452 01a0 D4F88430 		ldr	r3, [r4, #132]
 1453 01a4 43F48073 		orr	r3, r3, #256
 1454 01a8 C4F88430 		str	r3, [r4, #132]
 954:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1455              		.loc 1 954 11 view .LVU435
 954:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1456              		.loc 1 954 23 is_stmt 0 view .LVU436
 1457 01ac 0123     		movs	r3, #1
 1458 01ae 84F88130 		strb	r3, [r4, #129]
 957:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1459              		.loc 1 957 11 is_stmt 1 view .LVU437
 957:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1460              		.loc 1 957 11 view .LVU438
 1461 01b2 0023     		movs	r3, #0
 1462 01b4 84F88030 		strb	r3, [r4, #128]
 957:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1463              		.loc 1 957 11 view .LVU439
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 101


 959:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1464              		.loc 1 959 11 view .LVU440
 959:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1465              		.loc 1 959 18 is_stmt 0 view .LVU441
 1466 01b8 0327     		movs	r7, #3
 1467 01ba 7BE0     		b	.L71
 1468              	.L92:
 978:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1469              		.loc 1 978 14 is_stmt 1 view .LVU442
 978:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1470              		.loc 1 978 23 is_stmt 0 view .LVU443
 1471 01bc B4F86230 		ldrh	r3, [r4, #98]
 1472 01c0 9BB2     		uxth	r3, r3
 978:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1473              		.loc 1 978 17 view .LVU444
 1474 01c2 012B     		cmp	r3, #1
 1475 01c4 10D9     		bls	.L94
 978:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1476              		.loc 1 978 58 discriminator 1 view .LVU445
 1477 01c6 E36B     		ldr	r3, [r4, #60]
 978:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1478              		.loc 1 978 44 discriminator 1 view .LVU446
 1479 01c8 73B1     		cbz	r3, .L94
 981:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1480              		.loc 1 981 11 is_stmt 1 view .LVU447
 981:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1481              		.loc 1 981 51 is_stmt 0 view .LVU448
 1482 01ca E36D     		ldr	r3, [r4, #92]
 981:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1483              		.loc 1 981 27 view .LVU449
 1484 01cc 1B88     		ldrh	r3, [r3]
 981:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1485              		.loc 1 981 25 view .LVU450
 1486 01ce A8F82030 		strh	r3, [r8, #32]	@ movhi
 985:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount -= (uint16_t)2UL;
 1487              		.loc 1 985 11 is_stmt 1 view .LVU451
 985:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount -= (uint16_t)2UL;
 1488              		.loc 1 985 15 is_stmt 0 view .LVU452
 1489 01d2 E36D     		ldr	r3, [r4, #92]
 985:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount -= (uint16_t)2UL;
 1490              		.loc 1 985 28 view .LVU453
 1491 01d4 0233     		adds	r3, r3, #2
 1492 01d6 E365     		str	r3, [r4, #92]
 986:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1493              		.loc 1 986 11 is_stmt 1 view .LVU454
 986:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1494              		.loc 1 986 15 is_stmt 0 view .LVU455
 1495 01d8 B4F86230 		ldrh	r3, [r4, #98]
 1496 01dc 9BB2     		uxth	r3, r3
 986:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1497              		.loc 1 986 29 view .LVU456
 1498 01de 023B     		subs	r3, r3, #2
 1499 01e0 9BB2     		uxth	r3, r3
 1500 01e2 A4F86230 		strh	r3, [r4, #98]	@ movhi
 1501 01e6 0DE0     		b	.L84
 1502              	.L94:
 990:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint8_t);
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 102


 1503              		.loc 1 990 11 is_stmt 1 view .LVU457
 990:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint8_t);
 1504              		.loc 1 990 77 is_stmt 0 view .LVU458
 1505 01e8 E36D     		ldr	r3, [r4, #92]
 990:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint8_t);
 1506              		.loc 1 990 54 view .LVU459
 1507 01ea 1B78     		ldrb	r3, [r3]	@ zero_extendqisi2
 990:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint8_t);
 1508              		.loc 1 990 52 view .LVU460
 1509 01ec 82F82030 		strb	r3, [r2, #32]
 991:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount--;
 1510              		.loc 1 991 11 is_stmt 1 view .LVU461
 991:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount--;
 1511              		.loc 1 991 15 is_stmt 0 view .LVU462
 1512 01f0 E36D     		ldr	r3, [r4, #92]
 991:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount--;
 1513              		.loc 1 991 28 view .LVU463
 1514 01f2 0133     		adds	r3, r3, #1
 1515 01f4 E365     		str	r3, [r4, #92]
 992:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1516              		.loc 1 992 11 is_stmt 1 view .LVU464
 992:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1517              		.loc 1 992 15 is_stmt 0 view .LVU465
 1518 01f6 B4F86230 		ldrh	r3, [r4, #98]
 1519 01fa 9BB2     		uxth	r3, r3
 992:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1520              		.loc 1 992 28 view .LVU466
 1521 01fc 013B     		subs	r3, r3, #1
 1522 01fe 9BB2     		uxth	r3, r3
 1523 0200 A4F86230 		strh	r3, [r4, #98]	@ movhi
 1524              	.L84:
 967:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 1525              		.loc 1 967 30 is_stmt 1 view .LVU467
 967:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 1526              		.loc 1 967 16 is_stmt 0 view .LVU468
 1527 0204 B4F86230 		ldrh	r3, [r4, #98]
 1528 0208 9BB2     		uxth	r3, r3
 967:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 1529              		.loc 1 967 30 view .LVU469
 1530 020a 002B     		cmp	r3, #0
 1531 020c 35D0     		beq	.L82
 970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1532              		.loc 1 970 7 is_stmt 1 view .LVU470
 970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1533              		.loc 1 970 11 is_stmt 0 view .LVU471
 1534 020e 2268     		ldr	r2, [r4]
 1535 0210 5369     		ldr	r3, [r2, #20]
 970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1536              		.loc 1 970 10 view .LVU472
 1537 0212 13F0020F 		tst	r3, #2
 1538 0216 15D0     		beq	.L91
 972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1539              		.loc 1 972 9 is_stmt 1 view .LVU473
 972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1540              		.loc 1 972 18 is_stmt 0 view .LVU474
 1541 0218 B4F86230 		ldrh	r3, [r4, #98]
 1542 021c 9BB2     		uxth	r3, r3
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 103


 972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1543              		.loc 1 972 12 view .LVU475
 1544 021e 032B     		cmp	r3, #3
 1545 0220 CCD9     		bls	.L92
 972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1546              		.loc 1 972 53 discriminator 1 view .LVU476
 1547 0222 E36B     		ldr	r3, [r4, #60]
 972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1548              		.loc 1 972 39 discriminator 1 view .LVU477
 1549 0224 402B     		cmp	r3, #64
 1550 0226 C9D9     		bls	.L92
 974:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint32_t);
 1551              		.loc 1 974 11 is_stmt 1 view .LVU478
 974:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint32_t);
 1552              		.loc 1 974 79 is_stmt 0 view .LVU479
 1553 0228 E36D     		ldr	r3, [r4, #92]
 974:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint32_t);
 1554              		.loc 1 974 55 view .LVU480
 1555 022a 1B68     		ldr	r3, [r3]
 974:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint32_t);
 1556              		.loc 1 974 53 view .LVU481
 1557 022c 1362     		str	r3, [r2, #32]
 975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount -= (uint16_t)4UL;
 1558              		.loc 1 975 11 is_stmt 1 view .LVU482
 975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount -= (uint16_t)4UL;
 1559              		.loc 1 975 15 is_stmt 0 view .LVU483
 1560 022e E36D     		ldr	r3, [r4, #92]
 975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->TxXferCount -= (uint16_t)4UL;
 1561              		.loc 1 975 28 view .LVU484
 1562 0230 0433     		adds	r3, r3, #4
 1563 0232 E365     		str	r3, [r4, #92]
 976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1564              		.loc 1 976 11 is_stmt 1 view .LVU485
 976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1565              		.loc 1 976 15 is_stmt 0 view .LVU486
 1566 0234 B4F86230 		ldrh	r3, [r4, #98]
 1567 0238 9BB2     		uxth	r3, r3
 976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1568              		.loc 1 976 29 view .LVU487
 1569 023a 043B     		subs	r3, r3, #4
 1570 023c 9BB2     		uxth	r3, r3
 1571 023e A4F86230 		strh	r3, [r4, #98]	@ movhi
 1572 0242 DFE7     		b	.L84
 1573              	.L91:
 998:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1574              		.loc 1 998 9 is_stmt 1 view .LVU488
 998:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1575              		.loc 1 998 16 is_stmt 0 view .LVU489
 1576 0244 FFF7FEFF 		bl	HAL_GetTick
 1577              	.LVL58:
 998:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1578              		.loc 1 998 30 discriminator 1 view .LVU490
 1579 0248 801B     		subs	r0, r0, r6
 998:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1580              		.loc 1 998 12 discriminator 1 view .LVU491
 1581 024a A842     		cmp	r0, r5
 1582 024c 02D3     		bcc	.L95
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 104


 998:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1583              		.loc 1 998 56 discriminator 1 view .LVU492
 1584 024e B5F1FF3F 		cmp	r5, #-1
 1585 0252 01D1     		bne	.L96
 1586              	.L95:
 998:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1587              		.loc 1 998 87 discriminator 3 view .LVU493
 1588 0254 002D     		cmp	r5, #0
 1589 0256 D5D1     		bne	.L84
 1590              	.L96:
1001:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1591              		.loc 1 1001 11 is_stmt 1 view .LVU494
 1592 0258 2046     		mov	r0, r4
 1593 025a FFF7FEFF 		bl	SPI_CloseTransfer
 1594              	.LVL59:
1003:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 1595              		.loc 1 1003 11 view .LVU495
 1596 025e D4F88430 		ldr	r3, [r4, #132]
 1597 0262 43F48073 		orr	r3, r3, #256
 1598 0266 C4F88430 		str	r3, [r4, #132]
1004:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1599              		.loc 1 1004 11 view .LVU496
1004:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1600              		.loc 1 1004 23 is_stmt 0 view .LVU497
 1601 026a 0123     		movs	r3, #1
 1602 026c 84F88130 		strb	r3, [r4, #129]
1007:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1603              		.loc 1 1007 11 is_stmt 1 view .LVU498
1007:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1604              		.loc 1 1007 11 view .LVU499
 1605 0270 0023     		movs	r3, #0
 1606 0272 84F88030 		strb	r3, [r4, #128]
1007:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1607              		.loc 1 1007 11 view .LVU500
1009:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1608              		.loc 1 1009 11 view .LVU501
1009:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1609              		.loc 1 1009 18 is_stmt 0 view .LVU502
 1610 0276 0327     		movs	r7, #3
 1611 0278 1CE0     		b	.L71
 1612              	.L82:
1016:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1613              		.loc 1 1016 3 is_stmt 1 view .LVU503
1016:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1614              		.loc 1 1016 7 is_stmt 0 view .LVU504
 1615 027a 0096     		str	r6, [sp]
 1616 027c 2B46     		mov	r3, r5
 1617 027e 0022     		movs	r2, #0
 1618 0280 0821     		movs	r1, #8
 1619 0282 2046     		mov	r0, r4
 1620 0284 FFF7FEFF 		bl	SPI_WaitOnFlagUntilTimeout
 1621              	.LVL60:
1016:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1622              		.loc 1 1016 6 discriminator 1 view .LVU505
 1623 0288 28B1     		cbz	r0, .L98
1018:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1624              		.loc 1 1018 5 is_stmt 1 view .LVU506
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 105


 1625 028a D4F88430 		ldr	r3, [r4, #132]
 1626 028e 43F02003 		orr	r3, r3, #32
 1627 0292 C4F88430 		str	r3, [r4, #132]
 1628              	.L98:
1022:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1629              		.loc 1 1022 3 view .LVU507
 1630 0296 2046     		mov	r0, r4
 1631 0298 FFF7FEFF 		bl	SPI_CloseTransfer
 1632              	.LVL61:
1024:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1633              		.loc 1 1024 3 view .LVU508
1024:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1634              		.loc 1 1024 15 is_stmt 0 view .LVU509
 1635 029c 0123     		movs	r3, #1
 1636 029e 84F88130 		strb	r3, [r4, #129]
1027:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1637              		.loc 1 1027 3 is_stmt 1 view .LVU510
1027:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1638              		.loc 1 1027 3 view .LVU511
 1639 02a2 0023     		movs	r3, #0
 1640 02a4 84F88030 		strb	r3, [r4, #128]
1027:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1641              		.loc 1 1027 3 view .LVU512
1029:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1642              		.loc 1 1029 3 view .LVU513
1029:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1643              		.loc 1 1029 11 is_stmt 0 view .LVU514
 1644 02a8 D4F88430 		ldr	r3, [r4, #132]
1029:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1645              		.loc 1 1029 6 view .LVU515
 1646 02ac 13B9     		cbnz	r3, .L71
1035:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1647              		.loc 1 1035 12 view .LVU516
 1648 02ae 0027     		movs	r7, #0
 1649 02b0 00E0     		b	.L71
 1650              	.LVL62:
 1651              	.L99:
 840:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1652              		.loc 1 840 12 view .LVU517
 1653 02b2 0227     		movs	r7, #2
 1654              	.LVL63:
 1655              	.L71:
1037:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1656              		.loc 1 1037 1 view .LVU518
 1657 02b4 3846     		mov	r0, r7
 1658 02b6 02B0     		add	sp, sp, #8
 1659              		.cfi_remember_state
 1660              		.cfi_def_cfa_offset 32
 1661              		@ sp needed
 1662 02b8 BDE8F087 		pop	{r4, r5, r6, r7, r8, r9, r10, pc}
 1663              	.LVL64:
 1664              	.L100:
 1665              		.cfi_restore_state
 849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1666              		.loc 1 849 3 discriminator 1 view .LVU519
 1667 02bc 0227     		movs	r7, #2
 1668 02be F9E7     		b	.L71
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 106


 1669              		.cfi_endproc
 1670              	.LFE339:
 1672              		.section	.text.HAL_SPI_Receive,"ax",%progbits
 1673              		.align	1
 1674              		.global	HAL_SPI_Receive
 1675              		.syntax unified
 1676              		.thumb
 1677              		.thumb_func
 1679              	HAL_SPI_Receive:
 1680              	.LVL65:
 1681              	.LFB340:
1049:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t tickstart;
 1682              		.loc 1 1049 1 is_stmt 1 view -0
 1683              		.cfi_startproc
 1684              		@ args = 0, pretend = 0, frame = 0
 1685              		@ frame_needed = 0, uses_anonymous_args = 0
1049:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t tickstart;
 1686              		.loc 1 1049 1 is_stmt 0 view .LVU521
 1687 0000 2DE9F84F 		push	{r3, r4, r5, r6, r7, r8, r9, r10, fp, lr}
 1688              		.cfi_def_cfa_offset 40
 1689              		.cfi_offset 3, -40
 1690              		.cfi_offset 4, -36
 1691              		.cfi_offset 5, -32
 1692              		.cfi_offset 6, -28
 1693              		.cfi_offset 7, -24
 1694              		.cfi_offset 8, -20
 1695              		.cfi_offset 9, -16
 1696              		.cfi_offset 10, -12
 1697              		.cfi_offset 11, -8
 1698              		.cfi_offset 14, -4
 1699 0004 0446     		mov	r4, r0
 1700 0006 8B46     		mov	fp, r1
 1701 0008 9246     		mov	r10, r2
 1702 000a 1E46     		mov	r6, r3
1050:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t temp_sr_reg;
 1703              		.loc 1 1050 3 is_stmt 1 view .LVU522
1051:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint16_t init_max_data_in_fifo;
 1704              		.loc 1 1051 3 view .LVU523
1052:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   init_max_data_in_fifo = (((uint16_t)(hspi->Init.FifoThreshold >> 5U) + 1U));
 1705              		.loc 1 1052 3 view .LVU524
1053:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 1706              		.loc 1 1053 3 view .LVU525
1053:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 1707              		.loc 1 1053 50 is_stmt 0 view .LVU526
 1708 000c C56B     		ldr	r5, [r0, #60]
1053:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 1709              		.loc 1 1053 29 view .LVU527
 1710 000e C5F34F15 		ubfx	r5, r5, #5, #16
 1711              	.LVL66:
1055:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
 1712              		.loc 1 1055 3 is_stmt 1 view .LVU528
1055:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
 1713              		.loc 1 1055 57 is_stmt 0 view .LVU529
 1714 0012 D0F80090 		ldr	r9, [r0]
 1715              	.LVL67:
1059:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1716              		.loc 1 1059 3 is_stmt 1 view .LVU530
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 107


1062:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1717              		.loc 1 1062 3 view .LVU531
1062:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1718              		.loc 1 1062 15 is_stmt 0 view .LVU532
 1719 0016 FFF7FEFF 		bl	HAL_GetTick
 1720              	.LVL68:
1064:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1721              		.loc 1 1064 3 is_stmt 1 view .LVU533
1064:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1722              		.loc 1 1064 11 is_stmt 0 view .LVU534
 1723 001a 94F88130 		ldrb	r3, [r4, #129]	@ zero_extendqisi2
1064:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1724              		.loc 1 1064 6 view .LVU535
 1725 001e 012B     		cmp	r3, #1
 1726 0020 40F09081 		bne	.L137
 1727 0024 0135     		adds	r5, r5, #1
 1728              	.LVL69:
1064:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1729              		.loc 1 1064 6 view .LVU536
 1730 0026 ADB2     		uxth	r5, r5
 1731              	.LVL70:
1064:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1732              		.loc 1 1064 6 view .LVU537
 1733 0028 0746     		mov	r7, r0
 1734 002a 5FFA83F8 		uxtb	r8, r3
1069:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1735              		.loc 1 1069 3 is_stmt 1 view .LVU538
1069:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1736              		.loc 1 1069 6 is_stmt 0 view .LVU539
 1737 002e BAF1000F 		cmp	r10, #0
 1738 0032 18BF     		it	ne
 1739 0034 BBF1000F 		cmpne	fp, #0
 1740 0038 00F08681 		beq	.L108
1075:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1741              		.loc 1 1075 3 is_stmt 1 view .LVU540
1075:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1742              		.loc 1 1075 3 view .LVU541
 1743 003c 94F88030 		ldrb	r3, [r4, #128]	@ zero_extendqisi2
 1744 0040 012B     		cmp	r3, #1
 1745 0042 00F08481 		beq	.L138
1075:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1746              		.loc 1 1075 3 discriminator 2 view .LVU542
 1747 0046 0123     		movs	r3, #1
 1748 0048 84F88030 		strb	r3, [r4, #128]
1075:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1749              		.loc 1 1075 3 view .LVU543
1078:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 1750              		.loc 1 1078 3 view .LVU544
1078:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 1751              		.loc 1 1078 21 is_stmt 0 view .LVU545
 1752 004c 0423     		movs	r3, #4
 1753 004e 84F88130 		strb	r3, [r4, #129]
1079:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 1754              		.loc 1 1079 3 is_stmt 1 view .LVU546
1079:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 1755              		.loc 1 1079 21 is_stmt 0 view .LVU547
 1756 0052 0023     		movs	r3, #0
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 108


 1757 0054 C4F88430 		str	r3, [r4, #132]
1080:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 1758              		.loc 1 1080 3 is_stmt 1 view .LVU548
1080:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 1759              		.loc 1 1080 21 is_stmt 0 view .LVU549
 1760 0058 C4F864B0 		str	fp, [r4, #100]
1081:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
 1761              		.loc 1 1081 3 is_stmt 1 view .LVU550
1081:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
 1762              		.loc 1 1081 21 is_stmt 0 view .LVU551
 1763 005c A4F868A0 		strh	r10, [r4, #104]	@ movhi
1082:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1764              		.loc 1 1082 3 is_stmt 1 view .LVU552
1082:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1765              		.loc 1 1082 21 is_stmt 0 view .LVU553
 1766 0060 A4F86AA0 		strh	r10, [r4, #106]	@ movhi
1085:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = (uint16_t) 0UL;
 1767              		.loc 1 1085 3 is_stmt 1 view .LVU554
1085:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = (uint16_t) 0UL;
 1768              		.loc 1 1085 21 is_stmt 0 view .LVU555
 1769 0064 E365     		str	r3, [r4, #92]
1086:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t) 0UL;
 1770              		.loc 1 1086 3 is_stmt 1 view .LVU556
1086:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t) 0UL;
 1771              		.loc 1 1086 21 is_stmt 0 view .LVU557
 1772 0066 A4F86030 		strh	r3, [r4, #96]	@ movhi
1087:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
 1773              		.loc 1 1087 3 is_stmt 1 view .LVU558
1087:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
 1774              		.loc 1 1087 21 is_stmt 0 view .LVU559
 1775 006a A4F86230 		strh	r3, [r4, #98]	@ movhi
1088:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 1776              		.loc 1 1088 3 is_stmt 1 view .LVU560
1088:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 1777              		.loc 1 1088 21 is_stmt 0 view .LVU561
 1778 006e 2367     		str	r3, [r4, #112]
1089:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1779              		.loc 1 1089 3 is_stmt 1 view .LVU562
1089:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1780              		.loc 1 1089 21 is_stmt 0 view .LVU563
 1781 0070 6367     		str	r3, [r4, #116]
1092:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1782              		.loc 1 1092 3 is_stmt 1 view .LVU564
1092:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1783              		.loc 1 1092 17 is_stmt 0 view .LVU565
 1784 0072 A368     		ldr	r3, [r4, #8]
1092:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1785              		.loc 1 1092 6 view .LVU566
 1786 0074 B3F5C02F 		cmp	r3, #393216
 1787 0078 1DD0     		beq	.L142
1098:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1788              		.loc 1 1098 5 is_stmt 1 view .LVU567
 1789 007a 2268     		ldr	r2, [r4]
 1790 007c D368     		ldr	r3, [r2, #12]
 1791 007e 23F4C023 		bic	r3, r3, #393216
 1792 0082 43F48023 		orr	r3, r3, #262144
 1793 0086 D360     		str	r3, [r2, #12]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 109


 1794              	.L110:
1102:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1795              		.loc 1 1102 3 view .LVU568
 1796 0088 2268     		ldr	r2, [r4]
 1797 008a 5368     		ldr	r3, [r2, #4]
 1798 008c 6FF30F03 		bfc	r3, #0, #16
 1799 0090 4AEA0303 		orr	r3, r10, r3
 1800 0094 5360     		str	r3, [r2, #4]
1105:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1801              		.loc 1 1105 3 view .LVU569
 1802 0096 2268     		ldr	r2, [r4]
 1803 0098 1368     		ldr	r3, [r2]
 1804 009a 43F00103 		orr	r3, r3, #1
 1805 009e 1360     		str	r3, [r2]
1107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1806              		.loc 1 1107 3 view .LVU570
1107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1807              		.loc 1 1107 17 is_stmt 0 view .LVU571
 1808 00a0 6368     		ldr	r3, [r4, #4]
1107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1809              		.loc 1 1107 6 view .LVU572
 1810 00a2 B3F5800F 		cmp	r3, #4194304
 1811 00a6 0CD0     		beq	.L143
 1812              	.L111:
1114:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1813              		.loc 1 1114 3 is_stmt 1 view .LVU573
1114:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1814              		.loc 1 1114 17 is_stmt 0 view .LVU574
 1815 00a8 E368     		ldr	r3, [r4, #12]
1114:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1816              		.loc 1 1114 6 view .LVU575
 1817 00aa 0F2B     		cmp	r3, #15
 1818 00ac 2ED8     		bhi	.L112
1156:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1819              		.loc 1 1156 8 is_stmt 1 view .LVU576
1156:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 1820              		.loc 1 1156 11 is_stmt 0 view .LVU577
 1821 00ae 072B     		cmp	r3, #7
 1822 00b0 00F29580 		bhi	.L121
 1823 00b4 0CE1     		b	.L122
 1824              	.L142:
1094:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1825              		.loc 1 1094 5 is_stmt 1 view .LVU578
 1826 00b6 2268     		ldr	r2, [r4]
 1827 00b8 1368     		ldr	r3, [r2]
 1828 00ba 23F40063 		bic	r3, r3, #2048
 1829 00be 1360     		str	r3, [r2]
 1830 00c0 E2E7     		b	.L110
 1831              	.L143:
1110:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 1832              		.loc 1 1110 5 view .LVU579
 1833 00c2 2268     		ldr	r2, [r4]
 1834 00c4 1368     		ldr	r3, [r2]
 1835 00c6 43F40073 		orr	r3, r3, #512
 1836 00ca 1360     		str	r3, [r2]
 1837 00cc ECE7     		b	.L111
 1838              	.LVL71:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 110


 1839              	.L114:
1130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1840              		.loc 1 1130 12 view .LVU580
1130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1841              		.loc 1 1130 21 is_stmt 0 view .LVU581
 1842 00ce B4F86A20 		ldrh	r2, [r4, #106]
 1843 00d2 92B2     		uxth	r2, r2
1130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1844              		.loc 1 1130 15 view .LVU582
 1845 00d4 AA42     		cmp	r2, r5
 1846 00d6 10D2     		bcs	.L116
1130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1847              		.loc 1 1130 60 discriminator 1 view .LVU583
 1848 00d8 11F4004F 		tst	r1, #32768
 1849 00dc 0DD0     		beq	.L116
1132:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint32_t);
 1850              		.loc 1 1132 9 is_stmt 1 view .LVU584
1132:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint32_t);
 1851              		.loc 1 1132 27 is_stmt 0 view .LVU585
 1852 00de 626E     		ldr	r2, [r4, #100]
1132:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint32_t);
 1853              		.loc 1 1132 43 view .LVU586
 1854 00e0 1B6B     		ldr	r3, [r3, #48]
1132:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint32_t);
 1855              		.loc 1 1132 41 view .LVU587
 1856 00e2 1360     		str	r3, [r2]
1133:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 1857              		.loc 1 1133 9 is_stmt 1 view .LVU588
1133:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 1858              		.loc 1 1133 13 is_stmt 0 view .LVU589
 1859 00e4 636E     		ldr	r3, [r4, #100]
1133:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 1860              		.loc 1 1133 26 view .LVU590
 1861 00e6 0433     		adds	r3, r3, #4
 1862 00e8 6366     		str	r3, [r4, #100]
1134:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 1863              		.loc 1 1134 9 is_stmt 1 view .LVU591
1134:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 1864              		.loc 1 1134 13 is_stmt 0 view .LVU592
 1865 00ea B4F86A30 		ldrh	r3, [r4, #106]
 1866 00ee 9BB2     		uxth	r3, r3
1134:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 1867              		.loc 1 1134 26 view .LVU593
 1868 00f0 013B     		subs	r3, r3, #1
 1869 00f2 9BB2     		uxth	r3, r3
 1870 00f4 A4F86A30 		strh	r3, [r4, #106]	@ movhi
 1871 00f8 08E0     		b	.L112
 1872              	.L116:
1139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1873              		.loc 1 1139 9 is_stmt 1 view .LVU594
1139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1874              		.loc 1 1139 16 is_stmt 0 view .LVU595
 1875 00fa FFF7FEFF 		bl	HAL_GetTick
 1876              	.LVL72:
1139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1877              		.loc 1 1139 30 discriminator 1 view .LVU596
 1878 00fe C01B     		subs	r0, r0, r7
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 111


1139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1879              		.loc 1 1139 12 discriminator 1 view .LVU597
 1880 0100 B042     		cmp	r0, r6
 1881 0102 02D3     		bcc	.L117
1139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1882              		.loc 1 1139 56 discriminator 1 view .LVU598
 1883 0104 B6F1FF3F 		cmp	r6, #-1
 1884 0108 1AD1     		bne	.L118
 1885              	.L117:
1139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 1886              		.loc 1 1139 87 discriminator 3 view .LVU599
 1887 010a CEB1     		cbz	r6, .L118
 1888              	.LVL73:
 1889              	.L112:
1117:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 1890              		.loc 1 1117 30 is_stmt 1 view .LVU600
1117:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 1891              		.loc 1 1117 16 is_stmt 0 view .LVU601
 1892 010c B4F86A20 		ldrh	r2, [r4, #106]
 1893 0110 92B2     		uxth	r2, r2
1117:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 1894              		.loc 1 1117 30 view .LVU602
 1895 0112 002A     		cmp	r2, #0
 1896 0114 00F00781 		beq	.L120
1120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1897              		.loc 1 1120 7 is_stmt 1 view .LVU603
1120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1898              		.loc 1 1120 25 is_stmt 0 view .LVU604
 1899 0118 2368     		ldr	r3, [r4]
1120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1900              		.loc 1 1120 19 view .LVU605
 1901 011a 5969     		ldr	r1, [r3, #20]
 1902              	.LVL74:
1123:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1903              		.loc 1 1123 7 is_stmt 1 view .LVU606
1123:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1904              		.loc 1 1123 11 is_stmt 0 view .LVU607
 1905 011c 5A69     		ldr	r2, [r3, #20]
1123:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1906              		.loc 1 1123 10 view .LVU608
 1907 011e 12F0010F 		tst	r2, #1
 1908 0122 D4D0     		beq	.L114
1125:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint32_t);
 1909              		.loc 1 1125 9 is_stmt 1 view .LVU609
1125:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint32_t);
 1910              		.loc 1 1125 27 is_stmt 0 view .LVU610
 1911 0124 626E     		ldr	r2, [r4, #100]
1125:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint32_t);
 1912              		.loc 1 1125 43 view .LVU611
 1913 0126 1B6B     		ldr	r3, [r3, #48]
1125:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint32_t);
 1914              		.loc 1 1125 41 view .LVU612
 1915 0128 1360     		str	r3, [r2]
1126:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 1916              		.loc 1 1126 9 is_stmt 1 view .LVU613
1126:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 1917              		.loc 1 1126 13 is_stmt 0 view .LVU614
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 112


 1918 012a 636E     		ldr	r3, [r4, #100]
1126:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 1919              		.loc 1 1126 26 view .LVU615
 1920 012c 0433     		adds	r3, r3, #4
 1921 012e 6366     		str	r3, [r4, #100]
1127:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 1922              		.loc 1 1127 9 is_stmt 1 view .LVU616
1127:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 1923              		.loc 1 1127 13 is_stmt 0 view .LVU617
 1924 0130 B4F86A20 		ldrh	r2, [r4, #106]
 1925 0134 92B2     		uxth	r2, r2
1127:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 1926              		.loc 1 1127 26 view .LVU618
 1927 0136 013A     		subs	r2, r2, #1
 1928 0138 92B2     		uxth	r2, r2
 1929 013a A4F86A20 		strh	r2, [r4, #106]	@ movhi
 1930 013e E5E7     		b	.L112
 1931              	.LVL75:
 1932              	.L118:
1142:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1933              		.loc 1 1142 11 is_stmt 1 view .LVU619
 1934 0140 2046     		mov	r0, r4
 1935 0142 FFF7FEFF 		bl	SPI_CloseTransfer
 1936              	.LVL76:
1144:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 1937              		.loc 1 1144 11 view .LVU620
 1938 0146 D4F88430 		ldr	r3, [r4, #132]
 1939 014a 43F48073 		orr	r3, r3, #256
 1940 014e C4F88430 		str	r3, [r4, #132]
1145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1941              		.loc 1 1145 11 view .LVU621
1145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1942              		.loc 1 1145 23 is_stmt 0 view .LVU622
 1943 0152 0123     		movs	r3, #1
 1944 0154 84F88130 		strb	r3, [r4, #129]
1148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1945              		.loc 1 1148 11 is_stmt 1 view .LVU623
1148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1946              		.loc 1 1148 11 view .LVU624
 1947 0158 0023     		movs	r3, #0
 1948 015a 84F88030 		strb	r3, [r4, #128]
1148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 1949              		.loc 1 1148 11 view .LVU625
1150:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1950              		.loc 1 1150 11 view .LVU626
1150:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 1951              		.loc 1 1150 18 is_stmt 0 view .LVU627
 1952 015e 4FF00308 		mov	r8, #3
 1953 0162 F1E0     		b	.L108
 1954              	.LVL77:
 1955              	.L123:
1176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1956              		.loc 1 1176 12 is_stmt 1 view .LVU628
1176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1957              		.loc 1 1176 21 is_stmt 0 view .LVU629
 1958 0164 B4F86A30 		ldrh	r3, [r4, #106]
 1959 0168 9BB2     		uxth	r3, r3
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 113


1176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1960              		.loc 1 1176 15 view .LVU630
 1961 016a AB42     		cmp	r3, r5
 1962 016c 17D2     		bcs	.L125
1176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 1963              		.loc 1 1176 60 discriminator 1 view .LVU631
 1964 016e 12F4004F 		tst	r2, #32768
 1965 0172 14D0     		beq	.L125
1179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1966              		.loc 1 1179 9 is_stmt 1 view .LVU632
1179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1967              		.loc 1 1179 27 is_stmt 0 view .LVU633
 1968 0174 636E     		ldr	r3, [r4, #100]
1179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1969              		.loc 1 1179 43 view .LVU634
 1970 0176 B9F83020 		ldrh	r2, [r9, #48]
 1971              	.LVL78:
1179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1972              		.loc 1 1179 41 view .LVU635
 1973 017a 1A80     		strh	r2, [r3]	@ movhi
1183:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 1974              		.loc 1 1183 9 is_stmt 1 view .LVU636
1183:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 1975              		.loc 1 1183 13 is_stmt 0 view .LVU637
 1976 017c 636E     		ldr	r3, [r4, #100]
1183:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 1977              		.loc 1 1183 26 view .LVU638
 1978 017e 9A1C     		adds	r2, r3, #2
 1979 0180 6266     		str	r2, [r4, #100]
1185:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1980              		.loc 1 1185 9 is_stmt 1 view .LVU639
1185:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1981              		.loc 1 1185 43 is_stmt 0 view .LVU640
 1982 0182 B9F83020 		ldrh	r2, [r9, #48]
1185:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 1983              		.loc 1 1185 41 view .LVU641
 1984 0186 5A80     		strh	r2, [r3, #2]	@ movhi
1189:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount -= (uint16_t)2UL;
 1985              		.loc 1 1189 9 is_stmt 1 view .LVU642
1189:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount -= (uint16_t)2UL;
 1986              		.loc 1 1189 13 is_stmt 0 view .LVU643
 1987 0188 636E     		ldr	r3, [r4, #100]
1189:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount -= (uint16_t)2UL;
 1988              		.loc 1 1189 26 view .LVU644
 1989 018a 0233     		adds	r3, r3, #2
 1990 018c 6366     		str	r3, [r4, #100]
1190:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 1991              		.loc 1 1190 9 is_stmt 1 view .LVU645
1190:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 1992              		.loc 1 1190 13 is_stmt 0 view .LVU646
 1993 018e B4F86A30 		ldrh	r3, [r4, #106]
 1994 0192 9BB2     		uxth	r3, r3
1190:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 1995              		.loc 1 1190 27 view .LVU647
 1996 0194 023B     		subs	r3, r3, #2
 1997 0196 9BB2     		uxth	r3, r3
 1998 0198 A4F86A30 		strh	r3, [r4, #106]	@ movhi
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 114


 1999 019c 1FE0     		b	.L121
 2000              	.LVL79:
 2001              	.L125:
1193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2002              		.loc 1 1193 12 is_stmt 1 view .LVU648
1193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2003              		.loc 1 1193 21 is_stmt 0 view .LVU649
 2004 019e B4F86A30 		ldrh	r3, [r4, #106]
 2005 01a2 9BB2     		uxth	r3, r3
1193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2006              		.loc 1 1193 15 view .LVU650
 2007 01a4 012B     		cmp	r3, #1
 2008 01a6 11D1     		bne	.L126
1193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2009              		.loc 1 1193 43 discriminator 1 view .LVU651
 2010 01a8 12F4005F 		tst	r2, #8192
 2011 01ac 0ED0     		beq	.L126
1196:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2012              		.loc 1 1196 9 is_stmt 1 view .LVU652
1196:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2013              		.loc 1 1196 27 is_stmt 0 view .LVU653
 2014 01ae 636E     		ldr	r3, [r4, #100]
1196:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2015              		.loc 1 1196 43 view .LVU654
 2016 01b0 B9F83020 		ldrh	r2, [r9, #48]
 2017              	.LVL80:
1196:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2018              		.loc 1 1196 41 view .LVU655
 2019 01b4 1A80     		strh	r2, [r3]	@ movhi
1200:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 2020              		.loc 1 1200 9 is_stmt 1 view .LVU656
1200:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 2021              		.loc 1 1200 13 is_stmt 0 view .LVU657
 2022 01b6 636E     		ldr	r3, [r4, #100]
1200:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 2023              		.loc 1 1200 26 view .LVU658
 2024 01b8 0233     		adds	r3, r3, #2
 2025 01ba 6366     		str	r3, [r4, #100]
1201:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2026              		.loc 1 1201 9 is_stmt 1 view .LVU659
1201:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2027              		.loc 1 1201 13 is_stmt 0 view .LVU660
 2028 01bc B4F86A30 		ldrh	r3, [r4, #106]
 2029 01c0 9BB2     		uxth	r3, r3
1201:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2030              		.loc 1 1201 26 view .LVU661
 2031 01c2 013B     		subs	r3, r3, #1
 2032 01c4 9BB2     		uxth	r3, r3
 2033 01c6 A4F86A30 		strh	r3, [r4, #106]	@ movhi
 2034 01ca 08E0     		b	.L121
 2035              	.LVL81:
 2036              	.L126:
1206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2037              		.loc 1 1206 9 is_stmt 1 view .LVU662
1206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2038              		.loc 1 1206 16 is_stmt 0 view .LVU663
 2039 01cc FFF7FEFF 		bl	HAL_GetTick
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 115


 2040              	.LVL82:
1206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2041              		.loc 1 1206 30 discriminator 1 view .LVU664
 2042 01d0 C01B     		subs	r0, r0, r7
1206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2043              		.loc 1 1206 12 discriminator 1 view .LVU665
 2044 01d2 B042     		cmp	r0, r6
 2045 01d4 02D3     		bcc	.L127
1206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2046              		.loc 1 1206 56 discriminator 1 view .LVU666
 2047 01d6 B6F1FF3F 		cmp	r6, #-1
 2048 01da 1BD1     		bne	.L128
 2049              	.L127:
1206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2050              		.loc 1 1206 87 discriminator 3 view .LVU667
 2051 01dc D6B1     		cbz	r6, .L128
 2052              	.LVL83:
 2053              	.L121:
1159:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 2054              		.loc 1 1159 30 is_stmt 1 view .LVU668
1159:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 2055              		.loc 1 1159 16 is_stmt 0 view .LVU669
 2056 01de B4F86A30 		ldrh	r3, [r4, #106]
 2057 01e2 9BB2     		uxth	r3, r3
1159:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 2058              		.loc 1 1159 30 view .LVU670
 2059 01e4 002B     		cmp	r3, #0
 2060 01e6 00F09E80 		beq	.L120
1162:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2061              		.loc 1 1162 7 is_stmt 1 view .LVU671
1162:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2062              		.loc 1 1162 25 is_stmt 0 view .LVU672
 2063 01ea 2368     		ldr	r3, [r4]
1162:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2064              		.loc 1 1162 19 view .LVU673
 2065 01ec 5A69     		ldr	r2, [r3, #20]
 2066              	.LVL84:
1165:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2067              		.loc 1 1165 7 is_stmt 1 view .LVU674
1165:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2068              		.loc 1 1165 11 is_stmt 0 view .LVU675
 2069 01ee 5B69     		ldr	r3, [r3, #20]
1165:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2070              		.loc 1 1165 10 view .LVU676
 2071 01f0 13F0010F 		tst	r3, #1
 2072 01f4 B6D0     		beq	.L123
1168:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2073              		.loc 1 1168 9 is_stmt 1 view .LVU677
1168:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2074              		.loc 1 1168 27 is_stmt 0 view .LVU678
 2075 01f6 636E     		ldr	r3, [r4, #100]
1168:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2076              		.loc 1 1168 43 view .LVU679
 2077 01f8 B9F83020 		ldrh	r2, [r9, #48]
 2078              	.LVL85:
1168:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2079              		.loc 1 1168 41 view .LVU680
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 116


 2080 01fc 1A80     		strh	r2, [r3]	@ movhi
1172:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 2081              		.loc 1 1172 9 is_stmt 1 view .LVU681
1172:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 2082              		.loc 1 1172 13 is_stmt 0 view .LVU682
 2083 01fe 636E     		ldr	r3, [r4, #100]
1172:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 2084              		.loc 1 1172 26 view .LVU683
 2085 0200 0233     		adds	r3, r3, #2
 2086 0202 6366     		str	r3, [r4, #100]
1173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2087              		.loc 1 1173 9 is_stmt 1 view .LVU684
1173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2088              		.loc 1 1173 13 is_stmt 0 view .LVU685
 2089 0204 B4F86A30 		ldrh	r3, [r4, #106]
 2090 0208 9BB2     		uxth	r3, r3
1173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2091              		.loc 1 1173 26 view .LVU686
 2092 020a 013B     		subs	r3, r3, #1
 2093 020c 9BB2     		uxth	r3, r3
 2094 020e A4F86A30 		strh	r3, [r4, #106]	@ movhi
 2095 0212 E4E7     		b	.L121
 2096              	.L128:
1209:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2097              		.loc 1 1209 11 is_stmt 1 view .LVU687
 2098 0214 2046     		mov	r0, r4
 2099 0216 FFF7FEFF 		bl	SPI_CloseTransfer
 2100              	.LVL86:
1211:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 2101              		.loc 1 1211 11 view .LVU688
 2102 021a D4F88430 		ldr	r3, [r4, #132]
 2103 021e 43F48073 		orr	r3, r3, #256
 2104 0222 C4F88430 		str	r3, [r4, #132]
1212:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2105              		.loc 1 1212 11 view .LVU689
1212:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2106              		.loc 1 1212 23 is_stmt 0 view .LVU690
 2107 0226 0123     		movs	r3, #1
 2108 0228 84F88130 		strb	r3, [r4, #129]
1215:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2109              		.loc 1 1215 11 is_stmt 1 view .LVU691
1215:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2110              		.loc 1 1215 11 view .LVU692
 2111 022c 0023     		movs	r3, #0
 2112 022e 84F88030 		strb	r3, [r4, #128]
1215:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2113              		.loc 1 1215 11 view .LVU693
1217:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2114              		.loc 1 1217 11 view .LVU694
1217:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2115              		.loc 1 1217 18 is_stmt 0 view .LVU695
 2116 0232 4FF00308 		mov	r8, #3
 2117 0236 87E0     		b	.L108
 2118              	.LVL87:
 2119              	.L130:
1239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2120              		.loc 1 1239 12 is_stmt 1 view .LVU696
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 117


1239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2121              		.loc 1 1239 21 is_stmt 0 view .LVU697
 2122 0238 B4F86A20 		ldrh	r2, [r4, #106]
 2123 023c 92B2     		uxth	r2, r2
1239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2124              		.loc 1 1239 15 view .LVU698
 2125 023e AA42     		cmp	r2, r5
 2126 0240 26D2     		bcs	.L132
1239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2127              		.loc 1 1239 60 discriminator 1 view .LVU699
 2128 0242 11F4004F 		tst	r1, #32768
 2129 0246 23D0     		beq	.L132
1241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2130              		.loc 1 1241 9 is_stmt 1 view .LVU700
1241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2131              		.loc 1 1241 26 is_stmt 0 view .LVU701
 2132 0248 626E     		ldr	r2, [r4, #100]
1241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2133              		.loc 1 1241 42 view .LVU702
 2134 024a 93F83030 		ldrb	r3, [r3, #48]	@ zero_extendqisi2
1241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2135              		.loc 1 1241 40 view .LVU703
 2136 024e 1370     		strb	r3, [r2]
1242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 2137              		.loc 1 1242 9 is_stmt 1 view .LVU704
1242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 2138              		.loc 1 1242 13 is_stmt 0 view .LVU705
 2139 0250 636E     		ldr	r3, [r4, #100]
1242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 2140              		.loc 1 1242 26 view .LVU706
 2141 0252 5A1C     		adds	r2, r3, #1
 2142 0254 6266     		str	r2, [r4, #100]
1243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2143              		.loc 1 1243 9 is_stmt 1 view .LVU707
1243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2144              		.loc 1 1243 65 is_stmt 0 view .LVU708
 2145 0256 2268     		ldr	r2, [r4]
1243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2146              		.loc 1 1243 42 view .LVU709
 2147 0258 92F83020 		ldrb	r2, [r2, #48]	@ zero_extendqisi2
1243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2148              		.loc 1 1243 40 view .LVU710
 2149 025c 5A70     		strb	r2, [r3, #1]
1244:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 2150              		.loc 1 1244 9 is_stmt 1 view .LVU711
1244:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 2151              		.loc 1 1244 13 is_stmt 0 view .LVU712
 2152 025e 636E     		ldr	r3, [r4, #100]
1244:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 2153              		.loc 1 1244 26 view .LVU713
 2154 0260 5A1C     		adds	r2, r3, #1
 2155 0262 6266     		str	r2, [r4, #100]
1245:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2156              		.loc 1 1245 9 is_stmt 1 view .LVU714
1245:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2157              		.loc 1 1245 65 is_stmt 0 view .LVU715
 2158 0264 2268     		ldr	r2, [r4]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 118


1245:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2159              		.loc 1 1245 42 view .LVU716
 2160 0266 92F83020 		ldrb	r2, [r2, #48]	@ zero_extendqisi2
1245:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2161              		.loc 1 1245 40 view .LVU717
 2162 026a 5A70     		strb	r2, [r3, #1]
1246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 2163              		.loc 1 1246 9 is_stmt 1 view .LVU718
1246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 2164              		.loc 1 1246 13 is_stmt 0 view .LVU719
 2165 026c 636E     		ldr	r3, [r4, #100]
1246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 2166              		.loc 1 1246 26 view .LVU720
 2167 026e 5A1C     		adds	r2, r3, #1
 2168 0270 6266     		str	r2, [r4, #100]
1247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2169              		.loc 1 1247 9 is_stmt 1 view .LVU721
1247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2170              		.loc 1 1247 65 is_stmt 0 view .LVU722
 2171 0272 2268     		ldr	r2, [r4]
1247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2172              		.loc 1 1247 42 view .LVU723
 2173 0274 92F83020 		ldrb	r2, [r2, #48]	@ zero_extendqisi2
1247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2174              		.loc 1 1247 40 view .LVU724
 2175 0278 5A70     		strb	r2, [r3, #1]
1248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount -= (uint16_t)4UL;
 2176              		.loc 1 1248 9 is_stmt 1 view .LVU725
1248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount -= (uint16_t)4UL;
 2177              		.loc 1 1248 13 is_stmt 0 view .LVU726
 2178 027a 636E     		ldr	r3, [r4, #100]
1248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount -= (uint16_t)4UL;
 2179              		.loc 1 1248 26 view .LVU727
 2180 027c 0133     		adds	r3, r3, #1
 2181 027e 6366     		str	r3, [r4, #100]
1249:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2182              		.loc 1 1249 9 is_stmt 1 view .LVU728
1249:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2183              		.loc 1 1249 13 is_stmt 0 view .LVU729
 2184 0280 B4F86A30 		ldrh	r3, [r4, #106]
 2185 0284 9BB2     		uxth	r3, r3
1249:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2186              		.loc 1 1249 27 view .LVU730
 2187 0286 043B     		subs	r3, r3, #4
 2188 0288 9BB2     		uxth	r3, r3
 2189 028a A4F86A30 		strh	r3, [r4, #106]	@ movhi
 2190 028e 1FE0     		b	.L122
 2191              	.L132:
1252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2192              		.loc 1 1252 12 is_stmt 1 view .LVU731
1252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2193              		.loc 1 1252 21 is_stmt 0 view .LVU732
 2194 0290 B4F86A20 		ldrh	r2, [r4, #106]
 2195 0294 92B2     		uxth	r2, r2
1252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2196              		.loc 1 1252 15 view .LVU733
 2197 0296 032A     		cmp	r2, #3
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 119


 2198 0298 11D8     		bhi	.L133
1252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2199              		.loc 1 1252 42 discriminator 1 view .LVU734
 2200 029a 11F4C04F 		tst	r1, #24576
 2201 029e 0ED0     		beq	.L133
1254:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2202              		.loc 1 1254 9 is_stmt 1 view .LVU735
1254:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2203              		.loc 1 1254 26 is_stmt 0 view .LVU736
 2204 02a0 626E     		ldr	r2, [r4, #100]
1254:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2205              		.loc 1 1254 42 view .LVU737
 2206 02a2 93F83030 		ldrb	r3, [r3, #48]	@ zero_extendqisi2
1254:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2207              		.loc 1 1254 40 view .LVU738
 2208 02a6 1370     		strb	r3, [r2]
1255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 2209              		.loc 1 1255 9 is_stmt 1 view .LVU739
1255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 2210              		.loc 1 1255 13 is_stmt 0 view .LVU740
 2211 02a8 636E     		ldr	r3, [r4, #100]
1255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 2212              		.loc 1 1255 26 view .LVU741
 2213 02aa 0133     		adds	r3, r3, #1
 2214 02ac 6366     		str	r3, [r4, #100]
1256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2215              		.loc 1 1256 9 is_stmt 1 view .LVU742
1256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2216              		.loc 1 1256 13 is_stmt 0 view .LVU743
 2217 02ae B4F86A30 		ldrh	r3, [r4, #106]
 2218 02b2 9BB2     		uxth	r3, r3
1256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2219              		.loc 1 1256 26 view .LVU744
 2220 02b4 013B     		subs	r3, r3, #1
 2221 02b6 9BB2     		uxth	r3, r3
 2222 02b8 A4F86A30 		strh	r3, [r4, #106]	@ movhi
 2223 02bc 08E0     		b	.L122
 2224              	.L133:
1261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2225              		.loc 1 1261 9 is_stmt 1 view .LVU745
1261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2226              		.loc 1 1261 16 is_stmt 0 view .LVU746
 2227 02be FFF7FEFF 		bl	HAL_GetTick
 2228              	.LVL88:
1261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2229              		.loc 1 1261 30 discriminator 1 view .LVU747
 2230 02c2 C01B     		subs	r0, r0, r7
1261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2231              		.loc 1 1261 12 discriminator 1 view .LVU748
 2232 02c4 B042     		cmp	r0, r6
 2233 02c6 02D3     		bcc	.L134
1261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2234              		.loc 1 1261 56 discriminator 1 view .LVU749
 2235 02c8 B6F1FF3F 		cmp	r6, #-1
 2236 02cc 19D1     		bne	.L135
 2237              	.L134:
1261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 120


 2238              		.loc 1 1261 87 discriminator 3 view .LVU750
 2239 02ce C6B1     		cbz	r6, .L135
 2240              	.LVL89:
 2241              	.L122:
1226:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 2242              		.loc 1 1226 30 is_stmt 1 view .LVU751
1226:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 2243              		.loc 1 1226 16 is_stmt 0 view .LVU752
 2244 02d0 B4F86A30 		ldrh	r3, [r4, #106]
 2245 02d4 9BB2     		uxth	r3, r3
1226:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 2246              		.loc 1 1226 30 view .LVU753
 2247 02d6 33B3     		cbz	r3, .L120
1229:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2248              		.loc 1 1229 7 is_stmt 1 view .LVU754
1229:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2249              		.loc 1 1229 25 is_stmt 0 view .LVU755
 2250 02d8 2368     		ldr	r3, [r4]
1229:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2251              		.loc 1 1229 19 view .LVU756
 2252 02da 5969     		ldr	r1, [r3, #20]
 2253              	.LVL90:
1232:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2254              		.loc 1 1232 7 is_stmt 1 view .LVU757
1232:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2255              		.loc 1 1232 11 is_stmt 0 view .LVU758
 2256 02dc 5A69     		ldr	r2, [r3, #20]
1232:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2257              		.loc 1 1232 10 view .LVU759
 2258 02de 12F0010F 		tst	r2, #1
 2259 02e2 A9D0     		beq	.L130
1234:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2260              		.loc 1 1234 9 is_stmt 1 view .LVU760
1234:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2261              		.loc 1 1234 26 is_stmt 0 view .LVU761
 2262 02e4 626E     		ldr	r2, [r4, #100]
1234:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2263              		.loc 1 1234 42 view .LVU762
 2264 02e6 93F83030 		ldrb	r3, [r3, #48]	@ zero_extendqisi2
1234:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2265              		.loc 1 1234 40 view .LVU763
 2266 02ea 1370     		strb	r3, [r2]
1235:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 2267              		.loc 1 1235 9 is_stmt 1 view .LVU764
1235:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 2268              		.loc 1 1235 13 is_stmt 0 view .LVU765
 2269 02ec 636E     		ldr	r3, [r4, #100]
1235:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->RxXferCount--;
 2270              		.loc 1 1235 26 view .LVU766
 2271 02ee 0133     		adds	r3, r3, #1
 2272 02f0 6366     		str	r3, [r4, #100]
1236:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2273              		.loc 1 1236 9 is_stmt 1 view .LVU767
1236:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2274              		.loc 1 1236 13 is_stmt 0 view .LVU768
 2275 02f2 B4F86A30 		ldrh	r3, [r4, #106]
 2276 02f6 9BB2     		uxth	r3, r3
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 121


1236:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2277              		.loc 1 1236 26 view .LVU769
 2278 02f8 013B     		subs	r3, r3, #1
 2279 02fa 9BB2     		uxth	r3, r3
 2280 02fc A4F86A30 		strh	r3, [r4, #106]	@ movhi
 2281 0300 E6E7     		b	.L122
 2282              	.LVL91:
 2283              	.L135:
1264:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2284              		.loc 1 1264 11 is_stmt 1 view .LVU770
 2285 0302 2046     		mov	r0, r4
 2286 0304 FFF7FEFF 		bl	SPI_CloseTransfer
 2287              	.LVL92:
1266:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->State = HAL_SPI_STATE_READY;
 2288              		.loc 1 1266 11 view .LVU771
 2289 0308 D4F88430 		ldr	r3, [r4, #132]
 2290 030c 43F48073 		orr	r3, r3, #256
 2291 0310 C4F88430 		str	r3, [r4, #132]
1267:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2292              		.loc 1 1267 11 view .LVU772
1267:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2293              		.loc 1 1267 23 is_stmt 0 view .LVU773
 2294 0314 0123     		movs	r3, #1
 2295 0316 84F88130 		strb	r3, [r4, #129]
1270:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2296              		.loc 1 1270 11 is_stmt 1 view .LVU774
1270:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2297              		.loc 1 1270 11 view .LVU775
 2298 031a 0023     		movs	r3, #0
 2299 031c 84F88030 		strb	r3, [r4, #128]
1270:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2300              		.loc 1 1270 11 view .LVU776
1272:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2301              		.loc 1 1272 11 view .LVU777
1272:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2302              		.loc 1 1272 18 is_stmt 0 view .LVU778
 2303 0320 4FF00308 		mov	r8, #3
 2304 0324 10E0     		b	.L108
 2305              	.LVL93:
 2306              	.L120:
1290:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2307              		.loc 1 1290 3 is_stmt 1 view .LVU779
 2308 0326 2046     		mov	r0, r4
 2309 0328 FFF7FEFF 		bl	SPI_CloseTransfer
 2310              	.LVL94:
1292:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2311              		.loc 1 1292 3 view .LVU780
1292:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2312              		.loc 1 1292 15 is_stmt 0 view .LVU781
 2313 032c 0123     		movs	r3, #1
 2314 032e 84F88130 		strb	r3, [r4, #129]
1295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2315              		.loc 1 1295 3 is_stmt 1 view .LVU782
1295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2316              		.loc 1 1295 3 view .LVU783
 2317 0332 0023     		movs	r3, #0
 2318 0334 84F88030 		strb	r3, [r4, #128]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 122


1295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2319              		.loc 1 1295 3 view .LVU784
1298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2320              		.loc 1 1298 3 view .LVU785
1298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2321              		.loc 1 1298 11 is_stmt 0 view .LVU786
 2322 0338 D4F88430 		ldr	r3, [r4, #132]
1298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2323              		.loc 1 1298 6 view .LVU787
 2324 033c 23B9     		cbnz	r3, .L108
1304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 2325              		.loc 1 1304 12 view .LVU788
 2326 033e 4FF00008 		mov	r8, #0
 2327 0342 01E0     		b	.L108
 2328              	.LVL95:
 2329              	.L137:
1066:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 2330              		.loc 1 1066 12 view .LVU789
 2331 0344 4FF00208 		mov	r8, #2
 2332              	.LVL96:
 2333              	.L108:
1306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2334              		.loc 1 1306 1 view .LVU790
 2335 0348 4046     		mov	r0, r8
 2336 034a BDE8F88F 		pop	{r3, r4, r5, r6, r7, r8, r9, r10, fp, pc}
 2337              	.LVL97:
 2338              	.L138:
1075:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2339              		.loc 1 1075 3 discriminator 1 view .LVU791
 2340 034e 4FF00208 		mov	r8, #2
 2341 0352 F9E7     		b	.L108
 2342              		.cfi_endproc
 2343              	.LFE340:
 2345              		.section	.text.HAL_SPI_TransmitReceive,"ax",%progbits
 2346              		.align	1
 2347              		.global	HAL_SPI_TransmitReceive
 2348              		.syntax unified
 2349              		.thumb
 2350              		.thumb_func
 2352              	HAL_SPI_TransmitReceive:
 2353              	.LVL98:
 2354              	.LFB341:
1320:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 2355              		.loc 1 1320 1 is_stmt 1 view -0
 2356              		.cfi_startproc
 2357              		@ args = 4, pretend = 0, frame = 0
 2358              		@ frame_needed = 0, uses_anonymous_args = 0
1320:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 2359              		.loc 1 1320 1 is_stmt 0 view .LVU793
 2360 0000 2DE9F04F 		push	{r4, r5, r6, r7, r8, r9, r10, fp, lr}
 2361              		.cfi_def_cfa_offset 36
 2362              		.cfi_offset 4, -36
 2363              		.cfi_offset 5, -32
 2364              		.cfi_offset 6, -28
 2365              		.cfi_offset 7, -24
 2366              		.cfi_offset 8, -20
 2367              		.cfi_offset 9, -16
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 123


 2368              		.cfi_offset 10, -12
 2369              		.cfi_offset 11, -8
 2370              		.cfi_offset 14, -4
 2371 0004 83B0     		sub	sp, sp, #12
 2372              		.cfi_def_cfa_offset 48
 2373 0006 0446     		mov	r4, r0
 2374 0008 8946     		mov	r9, r1
 2375 000a 9046     		mov	r8, r2
 2376 000c 1D46     		mov	r5, r3
1322:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint16_t *prxdr_16bits = (__IO uint16_t *)(&(hspi->Instance->RXDR));
 2377              		.loc 1 1322 3 is_stmt 1 view .LVU794
1322:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint16_t *prxdr_16bits = (__IO uint16_t *)(&(hspi->Instance->RXDR));
 2378              		.loc 1 1322 57 is_stmt 0 view .LVU795
 2379 000e D0F800B0 		ldr	fp, [r0]
 2380              	.LVL99:
1323:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
 2381              		.loc 1 1323 3 is_stmt 1 view .LVU796
1326:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t   fifo_length;
 2382              		.loc 1 1326 3 view .LVU797
1327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t   temp_sr_reg;
 2383              		.loc 1 1327 3 view .LVU798
1328:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint16_t   initial_TxXferCount;
 2384              		.loc 1 1328 3 view .LVU799
1329:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint16_t   initial_RxXferCount;
 2385              		.loc 1 1329 3 view .LVU800
1330:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint16_t   init_max_data_in_fifo;
 2386              		.loc 1 1330 3 view .LVU801
1331:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   init_max_data_in_fifo = (((uint16_t)(hspi->Init.FifoThreshold >> 5U) + 1U));
 2387              		.loc 1 1331 3 view .LVU802
1332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2388              		.loc 1 1332 3 view .LVU803
1332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2389              		.loc 1 1332 50 is_stmt 0 view .LVU804
 2390 0012 C66B     		ldr	r6, [r0, #60]
1332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2391              		.loc 1 1332 29 view .LVU805
 2392 0014 C6F34F16 		ubfx	r6, r6, #5, #16
 2393              	.LVL100:
1335:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2394              		.loc 1 1335 3 is_stmt 1 view .LVU806
1338:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2395              		.loc 1 1338 3 view .LVU807
1338:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2396              		.loc 1 1338 15 is_stmt 0 view .LVU808
 2397 0018 FFF7FEFF 		bl	HAL_GetTick
 2398              	.LVL101:
1340:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   initial_RxXferCount = Size;
 2399              		.loc 1 1340 3 is_stmt 1 view .LVU809
1341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2400              		.loc 1 1341 3 view .LVU810
1343:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2401              		.loc 1 1343 3 view .LVU811
1343:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2402              		.loc 1 1343 11 is_stmt 0 view .LVU812
 2403 001c 94F88130 		ldrb	r3, [r4, #129]	@ zero_extendqisi2
1343:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2404              		.loc 1 1343 6 view .LVU813
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 124


 2405 0020 012B     		cmp	r3, #1
 2406 0022 40F03082 		bne	.L177
 2407 0026 0136     		adds	r6, r6, #1
 2408              	.LVL102:
1343:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2409              		.loc 1 1343 6 view .LVU814
 2410 0028 B6B2     		uxth	r6, r6
 2411              	.LVL103:
1343:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2412              		.loc 1 1343 6 view .LVU815
 2413 002a 0746     		mov	r7, r0
 2414 002c 5FFA83FA 		uxtb	r10, r3
1348:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2415              		.loc 1 1348 3 is_stmt 1 view .LVU816
1348:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2416              		.loc 1 1348 6 is_stmt 0 view .LVU817
 2417 0030 B8F1000F 		cmp	r8, #0
 2418 0034 18BF     		it	ne
 2419 0036 B9F1000F 		cmpne	r9, #0
 2420 003a 00F02682 		beq	.L145
1348:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2421              		.loc 1 1348 46 discriminator 1 view .LVU818
 2422 003e 002D     		cmp	r5, #0
 2423 0040 00F02382 		beq	.L145
1354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2424              		.loc 1 1354 3 is_stmt 1 view .LVU819
1354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2425              		.loc 1 1354 3 view .LVU820
 2426 0044 94F88030 		ldrb	r3, [r4, #128]	@ zero_extendqisi2
 2427 0048 012B     		cmp	r3, #1
 2428 004a 00F02282 		beq	.L178
1354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2429              		.loc 1 1354 3 discriminator 2 view .LVU821
 2430 004e 0123     		movs	r3, #1
 2431 0050 84F88030 		strb	r3, [r4, #128]
1354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2432              		.loc 1 1354 3 view .LVU822
1357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 2433              		.loc 1 1357 3 view .LVU823
1357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 2434              		.loc 1 1357 21 is_stmt 0 view .LVU824
 2435 0054 0523     		movs	r3, #5
 2436 0056 84F88130 		strb	r3, [r4, #129]
1358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 2437              		.loc 1 1358 3 is_stmt 1 view .LVU825
1358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 2438              		.loc 1 1358 21 is_stmt 0 view .LVU826
 2439 005a 0023     		movs	r3, #0
 2440 005c C4F88430 		str	r3, [r4, #132]
1359:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
 2441              		.loc 1 1359 3 is_stmt 1 view .LVU827
1359:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
 2442              		.loc 1 1359 21 is_stmt 0 view .LVU828
 2443 0060 C4F86480 		str	r8, [r4, #100]
1360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 2444              		.loc 1 1360 3 is_stmt 1 view .LVU829
1360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 125


 2445              		.loc 1 1360 21 is_stmt 0 view .LVU830
 2446 0064 A4F86A50 		strh	r5, [r4, #106]	@ movhi
1361:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pTxData;
 2447              		.loc 1 1361 3 is_stmt 1 view .LVU831
1361:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pTxData;
 2448              		.loc 1 1361 21 is_stmt 0 view .LVU832
 2449 0068 A4F86850 		strh	r5, [r4, #104]	@ movhi
1362:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 2450              		.loc 1 1362 3 is_stmt 1 view .LVU833
1362:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 2451              		.loc 1 1362 21 is_stmt 0 view .LVU834
 2452 006c C4F85C90 		str	r9, [r4, #92]
1363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 2453              		.loc 1 1363 3 is_stmt 1 view .LVU835
1363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 2454              		.loc 1 1363 21 is_stmt 0 view .LVU836
 2455 0070 A4F86250 		strh	r5, [r4, #98]	@ movhi
1364:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2456              		.loc 1 1364 3 is_stmt 1 view .LVU837
1364:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2457              		.loc 1 1364 21 is_stmt 0 view .LVU838
 2458 0074 A4F86050 		strh	r5, [r4, #96]	@ movhi
1367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 2459              		.loc 1 1367 3 is_stmt 1 view .LVU839
1367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 2460              		.loc 1 1367 21 is_stmt 0 view .LVU840
 2461 0078 2367     		str	r3, [r4, #112]
1368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2462              		.loc 1 1368 3 is_stmt 1 view .LVU841
1368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2463              		.loc 1 1368 21 is_stmt 0 view .LVU842
 2464 007a 6367     		str	r3, [r4, #116]
1371:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2465              		.loc 1 1371 3 is_stmt 1 view .LVU843
 2466 007c 2268     		ldr	r2, [r4]
 2467 007e D368     		ldr	r3, [r2, #12]
 2468 0080 23F4C023 		bic	r3, r3, #393216
 2469 0084 D360     		str	r3, [r2, #12]
1374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2470              		.loc 1 1374 3 view .LVU844
1374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2471              		.loc 1 1374 7 is_stmt 0 view .LVU845
 2472 0086 2268     		ldr	r2, [r4]
1374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2473              		.loc 1 1374 6 view .LVU846
 2474 0088 9C49     		ldr	r1, .L186
 2475 008a 9D4B     		ldr	r3, .L186+4
 2476 008c 9A42     		cmp	r2, r3
 2477 008e 18BF     		it	ne
 2478 0090 8A42     		cmpne	r2, r1
 2479 0092 09D0     		beq	.L179
1374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2480              		.loc 1 1374 7 discriminator 1 view .LVU847
 2481 0094 03F58063 		add	r3, r3, #1024
 2482 0098 9A42     		cmp	r2, r3
 2483 009a 02D0     		beq	.L184
1380:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 126


 2484              		.loc 1 1380 17 view .LVU848
 2485 009c 4FF00808 		mov	r8, #8
 2486              	.LVL104:
1380:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 2487              		.loc 1 1380 17 view .LVU849
 2488 00a0 04E0     		b	.L146
 2489              	.LVL105:
 2490              	.L184:
1376:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 2491              		.loc 1 1376 17 view .LVU850
 2492 00a2 4FF01008 		mov	r8, #16
 2493              	.LVL106:
1376:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 2494              		.loc 1 1376 17 view .LVU851
 2495 00a6 01E0     		b	.L146
 2496              	.LVL107:
 2497              	.L179:
1376:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 2498              		.loc 1 1376 17 view .LVU852
 2499 00a8 4FF01008 		mov	r8, #16
 2500              	.LVL108:
 2501              	.L146:
1384:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2502              		.loc 1 1384 3 is_stmt 1 view .LVU853
 2503 00ac 5368     		ldr	r3, [r2, #4]
 2504 00ae 6FF30F03 		bfc	r3, #0, #16
 2505 00b2 2B43     		orrs	r3, r3, r5
 2506 00b4 5360     		str	r3, [r2, #4]
1386:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2507              		.loc 1 1386 3 view .LVU854
 2508 00b6 2268     		ldr	r2, [r4]
 2509 00b8 1368     		ldr	r3, [r2]
 2510 00ba 43F00103 		orr	r3, r3, #1
 2511 00be 1360     		str	r3, [r2]
1388:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2512              		.loc 1 1388 3 view .LVU855
1388:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2513              		.loc 1 1388 17 is_stmt 0 view .LVU856
 2514 00c0 6368     		ldr	r3, [r4, #4]
1388:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2515              		.loc 1 1388 6 view .LVU857
 2516 00c2 B3F5800F 		cmp	r3, #4194304
 2517 00c6 06D0     		beq	.L185
 2518              	.L147:
1395:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2519              		.loc 1 1395 3 is_stmt 1 view .LVU858
1395:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2520              		.loc 1 1395 17 is_stmt 0 view .LVU859
 2521 00c8 E368     		ldr	r3, [r4, #12]
1395:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2522              		.loc 1 1395 6 view .LVU860
 2523 00ca 0F2B     		cmp	r3, #15
 2524 00cc 7AD9     		bls	.L148
1398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2525              		.loc 1 1398 5 is_stmt 1 view .LVU861
1398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2526              		.loc 1 1398 17 is_stmt 0 view .LVU862
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 127


 2527 00ce 4FEA980B 		lsr	fp, r8, #2
 2528              	.LVL109:
1400:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 2529              		.loc 1 1400 5 is_stmt 1 view .LVU863
1341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2530              		.loc 1 1341 23 is_stmt 0 view .LVU864
 2531 00d2 A846     		mov	r8, r5
1400:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 2532              		.loc 1 1400 11 view .LVU865
 2533 00d4 1FE0     		b	.L149
 2534              	.LVL110:
 2535              	.L185:
1391:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 2536              		.loc 1 1391 5 is_stmt 1 view .LVU866
 2537 00d6 2268     		ldr	r2, [r4]
 2538 00d8 1368     		ldr	r3, [r2]
 2539 00da 43F40073 		orr	r3, r3, #512
 2540 00de 1360     		str	r3, [r2]
 2541 00e0 F2E7     		b	.L147
 2542              	.LVL111:
 2543              	.L150:
1413:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2544              		.loc 1 1413 7 view .LVU867
1413:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2545              		.loc 1 1413 25 is_stmt 0 view .LVU868
 2546 00e2 2368     		ldr	r3, [r4]
1413:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2547              		.loc 1 1413 19 view .LVU869
 2548 00e4 5A69     		ldr	r2, [r3, #20]
 2549              	.LVL112:
1415:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2550              		.loc 1 1415 7 is_stmt 1 view .LVU870
1415:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2551              		.loc 1 1415 10 is_stmt 0 view .LVU871
 2552 00e6 B8F1000F 		cmp	r8, #0
 2553 00ea 14D0     		beq	.L149
1418:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2554              		.loc 1 1418 9 is_stmt 1 view .LVU872
1418:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2555              		.loc 1 1418 13 is_stmt 0 view .LVU873
 2556 00ec 5969     		ldr	r1, [r3, #20]
1418:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2557              		.loc 1 1418 12 view .LVU874
 2558 00ee 11F0010F 		tst	r1, #1
 2559 00f2 32D0     		beq	.L152
1420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
 2560              		.loc 1 1420 11 is_stmt 1 view .LVU875
1420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
 2561              		.loc 1 1420 29 is_stmt 0 view .LVU876
 2562 00f4 626E     		ldr	r2, [r4, #100]
 2563              	.LVL113:
1420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
 2564              		.loc 1 1420 45 view .LVU877
 2565 00f6 1B6B     		ldr	r3, [r3, #48]
1420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
 2566              		.loc 1 1420 43 view .LVU878
 2567 00f8 1360     		str	r3, [r2]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 128


1421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2568              		.loc 1 1421 11 is_stmt 1 view .LVU879
1421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2569              		.loc 1 1421 15 is_stmt 0 view .LVU880
 2570 00fa 636E     		ldr	r3, [r4, #100]
1421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2571              		.loc 1 1421 28 view .LVU881
 2572 00fc 0433     		adds	r3, r3, #4
 2573 00fe 6366     		str	r3, [r4, #100]
1422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2574              		.loc 1 1422 11 is_stmt 1 view .LVU882
1422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2575              		.loc 1 1422 15 is_stmt 0 view .LVU883
 2576 0100 B4F86A30 		ldrh	r3, [r4, #106]
 2577 0104 9BB2     		uxth	r3, r3
1422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2578              		.loc 1 1422 28 view .LVU884
 2579 0106 013B     		subs	r3, r3, #1
 2580 0108 9BB2     		uxth	r3, r3
 2581 010a A4F86A30 		strh	r3, [r4, #106]	@ movhi
1423:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2582              		.loc 1 1423 11 is_stmt 1 view .LVU885
1423:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2583              		.loc 1 1423 31 is_stmt 0 view .LVU886
 2584 010e B4F86A80 		ldrh	r8, [r4, #106]
 2585              	.LVL114:
1423:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2586              		.loc 1 1423 31 view .LVU887
 2587 0112 1FFA88F8 		uxth	r8, r8
 2588              	.LVL115:
 2589              	.L149:
1400:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 2590              		.loc 1 1400 40 is_stmt 1 view .LVU888
 2591 0116 45EA0803 		orr	r3, r5, r8
 2592 011a 9BB2     		uxth	r3, r3
 2593 011c 002B     		cmp	r3, #0
 2594 011e 00F09581 		beq	.L157
1403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 2595              		.loc 1 1403 7 view .LVU889
1403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 2596              		.loc 1 1403 12 is_stmt 0 view .LVU890
 2597 0122 2368     		ldr	r3, [r4]
 2598 0124 5A69     		ldr	r2, [r3, #20]
1403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 2599              		.loc 1 1403 10 view .LVU891
 2600 0126 12F0020F 		tst	r2, #2
 2601 012a DAD0     		beq	.L150
1403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 2602              		.loc 1 1403 52 discriminator 1 view .LVU892
 2603 012c 002D     		cmp	r5, #0
 2604 012e D8D0     		beq	.L150
1404:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2605              		.loc 1 1404 56 view .LVU893
 2606 0130 05EB0B02 		add	r2, r5, fp
1403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 2607              		.loc 1 1403 83 discriminator 2 view .LVU894
 2608 0134 9045     		cmp	r8, r2
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 129


 2609 0136 D4D2     		bcs	.L150
1406:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint32_t);
 2610              		.loc 1 1406 9 is_stmt 1 view .LVU895
1406:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint32_t);
 2611              		.loc 1 1406 77 is_stmt 0 view .LVU896
 2612 0138 E26D     		ldr	r2, [r4, #92]
1406:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint32_t);
 2613              		.loc 1 1406 53 view .LVU897
 2614 013a 1268     		ldr	r2, [r2]
1406:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint32_t);
 2615              		.loc 1 1406 51 view .LVU898
 2616 013c 1A62     		str	r2, [r3, #32]
1407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount --;
 2617              		.loc 1 1407 9 is_stmt 1 view .LVU899
1407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount --;
 2618              		.loc 1 1407 13 is_stmt 0 view .LVU900
 2619 013e E36D     		ldr	r3, [r4, #92]
1407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount --;
 2620              		.loc 1 1407 26 view .LVU901
 2621 0140 0433     		adds	r3, r3, #4
 2622 0142 E365     		str	r3, [r4, #92]
1408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         initial_TxXferCount = hspi->TxXferCount;
 2623              		.loc 1 1408 9 is_stmt 1 view .LVU902
1408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         initial_TxXferCount = hspi->TxXferCount;
 2624              		.loc 1 1408 13 is_stmt 0 view .LVU903
 2625 0144 B4F86230 		ldrh	r3, [r4, #98]
 2626 0148 9BB2     		uxth	r3, r3
1408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         initial_TxXferCount = hspi->TxXferCount;
 2627              		.loc 1 1408 27 view .LVU904
 2628 014a 013B     		subs	r3, r3, #1
 2629 014c 9BB2     		uxth	r3, r3
 2630 014e A4F86230 		strh	r3, [r4, #98]	@ movhi
1409:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2631              		.loc 1 1409 9 is_stmt 1 view .LVU905
1409:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2632              		.loc 1 1409 29 is_stmt 0 view .LVU906
 2633 0152 B4F86250 		ldrh	r5, [r4, #98]
 2634              	.LVL116:
1409:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2635              		.loc 1 1409 29 view .LVU907
 2636 0156 ADB2     		uxth	r5, r5
 2637 0158 C3E7     		b	.L150
 2638              	.LVL117:
 2639              	.L152:
1426:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2640              		.loc 1 1426 14 is_stmt 1 view .LVU908
1426:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2641              		.loc 1 1426 17 is_stmt 0 view .LVU909
 2642 015a B045     		cmp	r8, r6
 2643 015c 14D2     		bcs	.L153
1426:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2644              		.loc 1 1426 64 discriminator 1 view .LVU910
 2645 015e 12F4004F 		tst	r2, #32768
 2646 0162 11D0     		beq	.L153
1428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
 2647              		.loc 1 1428 11 is_stmt 1 view .LVU911
1428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 130


 2648              		.loc 1 1428 29 is_stmt 0 view .LVU912
 2649 0164 626E     		ldr	r2, [r4, #100]
 2650              	.LVL118:
1428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
 2651              		.loc 1 1428 45 view .LVU913
 2652 0166 1B6B     		ldr	r3, [r3, #48]
1428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
 2653              		.loc 1 1428 43 view .LVU914
 2654 0168 1360     		str	r3, [r2]
1429:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2655              		.loc 1 1429 11 is_stmt 1 view .LVU915
1429:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2656              		.loc 1 1429 15 is_stmt 0 view .LVU916
 2657 016a 636E     		ldr	r3, [r4, #100]
1429:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2658              		.loc 1 1429 28 view .LVU917
 2659 016c 0433     		adds	r3, r3, #4
 2660 016e 6366     		str	r3, [r4, #100]
1430:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2661              		.loc 1 1430 11 is_stmt 1 view .LVU918
1430:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2662              		.loc 1 1430 15 is_stmt 0 view .LVU919
 2663 0170 B4F86A30 		ldrh	r3, [r4, #106]
 2664 0174 9BB2     		uxth	r3, r3
1430:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2665              		.loc 1 1430 28 view .LVU920
 2666 0176 013B     		subs	r3, r3, #1
 2667 0178 9BB2     		uxth	r3, r3
 2668 017a A4F86A30 		strh	r3, [r4, #106]	@ movhi
1431:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2669              		.loc 1 1431 11 is_stmt 1 view .LVU921
1431:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2670              		.loc 1 1431 31 is_stmt 0 view .LVU922
 2671 017e B4F86A80 		ldrh	r8, [r4, #106]
 2672              	.LVL119:
1431:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2673              		.loc 1 1431 31 view .LVU923
 2674 0182 1FFA88F8 		uxth	r8, r8
 2675              	.LVL120:
1431:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2676              		.loc 1 1431 31 view .LVU924
 2677 0186 C6E7     		b	.L149
 2678              	.LVL121:
 2679              	.L153:
1436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 2680              		.loc 1 1436 11 is_stmt 1 view .LVU925
1436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 2681              		.loc 1 1436 18 is_stmt 0 view .LVU926
 2682 0188 FFF7FEFF 		bl	HAL_GetTick
 2683              	.LVL122:
1436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 2684              		.loc 1 1436 32 discriminator 1 view .LVU927
 2685 018c C01B     		subs	r0, r0, r7
1436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 2686              		.loc 1 1436 14 discriminator 1 view .LVU928
 2687 018e 0C9B     		ldr	r3, [sp, #48]
 2688 0190 9842     		cmp	r0, r3
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 131


 2689 0192 02D3     		bcc	.L154
1436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 2690              		.loc 1 1436 58 discriminator 1 view .LVU929
 2691 0194 B3F1FF3F 		cmp	r3, #-1
 2692 0198 02D1     		bne	.L155
 2693              	.L154:
1436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 2694              		.loc 1 1436 89 discriminator 3 view .LVU930
 2695 019a 0C9B     		ldr	r3, [sp, #48]
 2696 019c 002B     		cmp	r3, #0
 2697 019e BAD1     		bne	.L149
 2698              	.L155:
1439:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2699              		.loc 1 1439 13 is_stmt 1 view .LVU931
 2700 01a0 2046     		mov	r0, r4
 2701 01a2 FFF7FEFF 		bl	SPI_CloseTransfer
 2702              	.LVL123:
1441:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             hspi->State = HAL_SPI_STATE_READY;
 2703              		.loc 1 1441 13 view .LVU932
 2704 01a6 D4F88430 		ldr	r3, [r4, #132]
 2705 01aa 43F48073 		orr	r3, r3, #256
 2706 01ae C4F88430 		str	r3, [r4, #132]
1442:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2707              		.loc 1 1442 13 view .LVU933
1442:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2708              		.loc 1 1442 25 is_stmt 0 view .LVU934
 2709 01b2 0123     		movs	r3, #1
 2710 01b4 84F88130 		strb	r3, [r4, #129]
1445:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2711              		.loc 1 1445 13 is_stmt 1 view .LVU935
1445:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2712              		.loc 1 1445 13 view .LVU936
 2713 01b8 0023     		movs	r3, #0
 2714 01ba 84F88030 		strb	r3, [r4, #128]
1445:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2715              		.loc 1 1445 13 view .LVU937
1447:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
 2716              		.loc 1 1447 13 view .LVU938
1447:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
 2717              		.loc 1 1447 20 is_stmt 0 view .LVU939
 2718 01be 4FF0030A 		mov	r10, #3
 2719 01c2 62E1     		b	.L145
 2720              	.LVL124:
 2721              	.L148:
1454:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2722              		.loc 1 1454 8 is_stmt 1 view .LVU940
1454:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 2723              		.loc 1 1454 11 is_stmt 0 view .LVU941
 2724 01c4 072B     		cmp	r3, #7
 2725 01c6 40F23F81 		bls	.L181
1457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2726              		.loc 1 1457 5 is_stmt 1 view .LVU942
1457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2727              		.loc 1 1457 17 is_stmt 0 view .LVU943
 2728 01ca 4FEA5803 		lsr	r3, r8, #1
 2729 01ce 9946     		mov	r9, r3
 2730              	.LVL125:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 132


1459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 2731              		.loc 1 1459 5 is_stmt 1 view .LVU944
1341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2732              		.loc 1 1341 23 is_stmt 0 view .LVU945
 2733 01d0 A846     		mov	r8, r5
1459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 2734              		.loc 1 1459 11 view .LVU946
 2735 01d2 1AE0     		b	.L159
 2736              	.LVL126:
 2737              	.L160:
1476:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2738              		.loc 1 1476 7 is_stmt 1 view .LVU947
1476:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2739              		.loc 1 1476 25 is_stmt 0 view .LVU948
 2740 01d4 2368     		ldr	r3, [r4]
1476:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2741              		.loc 1 1476 19 view .LVU949
 2742 01d6 5A69     		ldr	r2, [r3, #20]
 2743              	.LVL127:
1478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2744              		.loc 1 1478 7 is_stmt 1 view .LVU950
1478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2745              		.loc 1 1478 10 is_stmt 0 view .LVU951
 2746 01d8 B8F1000F 		cmp	r8, #0
 2747 01dc 15D0     		beq	.L159
1481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2748              		.loc 1 1481 9 is_stmt 1 view .LVU952
1481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2749              		.loc 1 1481 13 is_stmt 0 view .LVU953
 2750 01de 5B69     		ldr	r3, [r3, #20]
1481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2751              		.loc 1 1481 12 view .LVU954
 2752 01e0 13F0010F 		tst	r3, #1
 2753 01e4 34D0     		beq	.L162
1484:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2754              		.loc 1 1484 11 is_stmt 1 view .LVU955
1484:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2755              		.loc 1 1484 29 is_stmt 0 view .LVU956
 2756 01e6 636E     		ldr	r3, [r4, #100]
1484:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2757              		.loc 1 1484 45 view .LVU957
 2758 01e8 BBF83020 		ldrh	r2, [fp, #48]
 2759              	.LVL128:
1484:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2760              		.loc 1 1484 43 view .LVU958
 2761 01ec 1A80     		strh	r2, [r3]	@ movhi
1488:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2762              		.loc 1 1488 11 is_stmt 1 view .LVU959
1488:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2763              		.loc 1 1488 15 is_stmt 0 view .LVU960
 2764 01ee 636E     		ldr	r3, [r4, #100]
1488:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2765              		.loc 1 1488 28 view .LVU961
 2766 01f0 0233     		adds	r3, r3, #2
 2767 01f2 6366     		str	r3, [r4, #100]
1489:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2768              		.loc 1 1489 11 is_stmt 1 view .LVU962
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 133


1489:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2769              		.loc 1 1489 15 is_stmt 0 view .LVU963
 2770 01f4 B4F86A30 		ldrh	r3, [r4, #106]
 2771 01f8 9BB2     		uxth	r3, r3
1489:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2772              		.loc 1 1489 28 view .LVU964
 2773 01fa 013B     		subs	r3, r3, #1
 2774 01fc 9BB2     		uxth	r3, r3
 2775 01fe A4F86A30 		strh	r3, [r4, #106]	@ movhi
1490:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2776              		.loc 1 1490 11 is_stmt 1 view .LVU965
1490:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2777              		.loc 1 1490 31 is_stmt 0 view .LVU966
 2778 0202 B4F86A80 		ldrh	r8, [r4, #106]
 2779              	.LVL129:
1490:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2780              		.loc 1 1490 31 view .LVU967
 2781 0206 1FFA88F8 		uxth	r8, r8
 2782              	.LVL130:
 2783              	.L159:
1459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 2784              		.loc 1 1459 40 is_stmt 1 view .LVU968
 2785 020a 45EA0803 		orr	r3, r5, r8
 2786 020e 9BB2     		uxth	r3, r3
 2787 0210 002B     		cmp	r3, #0
 2788 0212 00F01B81 		beq	.L157
1462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 2789              		.loc 1 1462 7 view .LVU969
1462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 2790              		.loc 1 1462 12 is_stmt 0 view .LVU970
 2791 0216 2368     		ldr	r3, [r4]
 2792 0218 5B69     		ldr	r3, [r3, #20]
1462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 2793              		.loc 1 1462 10 view .LVU971
 2794 021a 13F0020F 		tst	r3, #2
 2795 021e D9D0     		beq	.L160
1462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 2796              		.loc 1 1462 52 discriminator 1 view .LVU972
 2797 0220 002D     		cmp	r5, #0
 2798 0222 D7D0     		beq	.L160
1463:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2799              		.loc 1 1463 56 view .LVU973
 2800 0224 4B46     		mov	r3, r9
 2801 0226 EB18     		adds	r3, r5, r3
1462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 2802              		.loc 1 1462 83 discriminator 2 view .LVU974
 2803 0228 9845     		cmp	r8, r3
 2804 022a D3D2     		bcs	.L160
1466:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2805              		.loc 1 1466 9 is_stmt 1 view .LVU975
1466:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2806              		.loc 1 1466 49 is_stmt 0 view .LVU976
 2807 022c E36D     		ldr	r3, [r4, #92]
1466:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2808              		.loc 1 1466 25 view .LVU977
 2809 022e 1B88     		ldrh	r3, [r3]
1466:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 134


 2810              		.loc 1 1466 23 view .LVU978
 2811 0230 ABF82030 		strh	r3, [fp, #32]	@ movhi
1470:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount--;
 2812              		.loc 1 1470 9 is_stmt 1 view .LVU979
1470:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount--;
 2813              		.loc 1 1470 13 is_stmt 0 view .LVU980
 2814 0234 E36D     		ldr	r3, [r4, #92]
1470:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount--;
 2815              		.loc 1 1470 26 view .LVU981
 2816 0236 0233     		adds	r3, r3, #2
 2817 0238 E365     		str	r3, [r4, #92]
1471:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         initial_TxXferCount = hspi->TxXferCount;
 2818              		.loc 1 1471 9 is_stmt 1 view .LVU982
1471:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         initial_TxXferCount = hspi->TxXferCount;
 2819              		.loc 1 1471 13 is_stmt 0 view .LVU983
 2820 023a B4F86230 		ldrh	r3, [r4, #98]
 2821 023e 9BB2     		uxth	r3, r3
1471:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         initial_TxXferCount = hspi->TxXferCount;
 2822              		.loc 1 1471 26 view .LVU984
 2823 0240 013B     		subs	r3, r3, #1
 2824 0242 9BB2     		uxth	r3, r3
 2825 0244 A4F86230 		strh	r3, [r4, #98]	@ movhi
1472:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2826              		.loc 1 1472 9 is_stmt 1 view .LVU985
1472:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2827              		.loc 1 1472 29 is_stmt 0 view .LVU986
 2828 0248 B4F86250 		ldrh	r5, [r4, #98]
 2829              	.LVL131:
1472:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 2830              		.loc 1 1472 29 view .LVU987
 2831 024c ADB2     		uxth	r5, r5
 2832 024e C1E7     		b	.L160
 2833              	.LVL132:
 2834              	.L162:
1493:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2835              		.loc 1 1493 14 is_stmt 1 view .LVU988
1493:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2836              		.loc 1 1493 17 is_stmt 0 view .LVU989
 2837 0250 B045     		cmp	r8, r6
 2838 0252 1BD2     		bcs	.L163
1493:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2839              		.loc 1 1493 64 discriminator 1 view .LVU990
 2840 0254 12F4004F 		tst	r2, #32768
 2841 0258 18D0     		beq	.L163
1496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2842              		.loc 1 1496 11 is_stmt 1 view .LVU991
1496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2843              		.loc 1 1496 29 is_stmt 0 view .LVU992
 2844 025a 636E     		ldr	r3, [r4, #100]
1496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2845              		.loc 1 1496 45 view .LVU993
 2846 025c BBF83020 		ldrh	r2, [fp, #48]
 2847              	.LVL133:
1496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2848              		.loc 1 1496 43 view .LVU994
 2849 0260 1A80     		strh	r2, [r3]	@ movhi
1500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 135


 2850              		.loc 1 1500 11 is_stmt 1 view .LVU995
1500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 2851              		.loc 1 1500 15 is_stmt 0 view .LVU996
 2852 0262 636E     		ldr	r3, [r4, #100]
1500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 2853              		.loc 1 1500 28 view .LVU997
 2854 0264 9A1C     		adds	r2, r3, #2
 2855 0266 6266     		str	r2, [r4, #100]
1502:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2856              		.loc 1 1502 11 is_stmt 1 view .LVU998
1502:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2857              		.loc 1 1502 45 is_stmt 0 view .LVU999
 2858 0268 BBF83020 		ldrh	r2, [fp, #48]
1502:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2859              		.loc 1 1502 43 view .LVU1000
 2860 026c 5A80     		strh	r2, [r3, #2]	@ movhi
1506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount -= (uint16_t)2UL;
 2861              		.loc 1 1506 11 is_stmt 1 view .LVU1001
1506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount -= (uint16_t)2UL;
 2862              		.loc 1 1506 15 is_stmt 0 view .LVU1002
 2863 026e 636E     		ldr	r3, [r4, #100]
1506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount -= (uint16_t)2UL;
 2864              		.loc 1 1506 28 view .LVU1003
 2865 0270 0233     		adds	r3, r3, #2
 2866 0272 6366     		str	r3, [r4, #100]
1507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2867              		.loc 1 1507 11 is_stmt 1 view .LVU1004
1507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2868              		.loc 1 1507 15 is_stmt 0 view .LVU1005
 2869 0274 B4F86A30 		ldrh	r3, [r4, #106]
 2870 0278 9BB2     		uxth	r3, r3
1507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2871              		.loc 1 1507 29 view .LVU1006
 2872 027a 023B     		subs	r3, r3, #2
 2873 027c 9BB2     		uxth	r3, r3
 2874 027e A4F86A30 		strh	r3, [r4, #106]	@ movhi
1508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2875              		.loc 1 1508 11 is_stmt 1 view .LVU1007
1508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2876              		.loc 1 1508 31 is_stmt 0 view .LVU1008
 2877 0282 B4F86A80 		ldrh	r8, [r4, #106]
 2878              	.LVL134:
1508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2879              		.loc 1 1508 31 view .LVU1009
 2880 0286 1FFA88F8 		uxth	r8, r8
 2881              	.LVL135:
1508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2882              		.loc 1 1508 31 view .LVU1010
 2883 028a BEE7     		b	.L159
 2884              	.LVL136:
 2885              	.L163:
1511:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2886              		.loc 1 1511 14 is_stmt 1 view .LVU1011
1511:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2887              		.loc 1 1511 17 is_stmt 0 view .LVU1012
 2888 028c B8F1010F 		cmp	r8, #1
 2889 0290 15D1     		bne	.L164
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 136


1511:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2890              		.loc 1 1511 47 discriminator 1 view .LVU1013
 2891 0292 12F4005F 		tst	r2, #8192
 2892 0296 12D0     		beq	.L164
1514:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2893              		.loc 1 1514 11 is_stmt 1 view .LVU1014
1514:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2894              		.loc 1 1514 29 is_stmt 0 view .LVU1015
 2895 0298 636E     		ldr	r3, [r4, #100]
1514:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2896              		.loc 1 1514 45 view .LVU1016
 2897 029a BBF83020 		ldrh	r2, [fp, #48]
 2898              	.LVL137:
1514:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 2899              		.loc 1 1514 43 view .LVU1017
 2900 029e 1A80     		strh	r2, [r3]	@ movhi
1518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2901              		.loc 1 1518 11 is_stmt 1 view .LVU1018
1518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2902              		.loc 1 1518 15 is_stmt 0 view .LVU1019
 2903 02a0 636E     		ldr	r3, [r4, #100]
1518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2904              		.loc 1 1518 28 view .LVU1020
 2905 02a2 0233     		adds	r3, r3, #2
 2906 02a4 6366     		str	r3, [r4, #100]
1519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2907              		.loc 1 1519 11 is_stmt 1 view .LVU1021
1519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2908              		.loc 1 1519 15 is_stmt 0 view .LVU1022
 2909 02a6 B4F86A30 		ldrh	r3, [r4, #106]
 2910 02aa 9BB2     		uxth	r3, r3
1519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 2911              		.loc 1 1519 28 view .LVU1023
 2912 02ac 013B     		subs	r3, r3, #1
 2913 02ae 9BB2     		uxth	r3, r3
 2914 02b0 A4F86A30 		strh	r3, [r4, #106]	@ movhi
1520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2915              		.loc 1 1520 11 is_stmt 1 view .LVU1024
1520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2916              		.loc 1 1520 31 is_stmt 0 view .LVU1025
 2917 02b4 B4F86A80 		ldrh	r8, [r4, #106]
 2918              	.LVL138:
1520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2919              		.loc 1 1520 31 view .LVU1026
 2920 02b8 1FFA88F8 		uxth	r8, r8
 2921              	.LVL139:
1520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 2922              		.loc 1 1520 31 view .LVU1027
 2923 02bc A5E7     		b	.L159
 2924              	.LVL140:
 2925              	.L164:
1525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 2926              		.loc 1 1525 11 is_stmt 1 view .LVU1028
1525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 2927              		.loc 1 1525 18 is_stmt 0 view .LVU1029
 2928 02be FFF7FEFF 		bl	HAL_GetTick
 2929              	.LVL141:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 137


1525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 2930              		.loc 1 1525 32 discriminator 1 view .LVU1030
 2931 02c2 C01B     		subs	r0, r0, r7
1525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 2932              		.loc 1 1525 14 discriminator 1 view .LVU1031
 2933 02c4 0C9B     		ldr	r3, [sp, #48]
 2934 02c6 9842     		cmp	r0, r3
 2935 02c8 02D3     		bcc	.L165
1525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 2936              		.loc 1 1525 58 discriminator 1 view .LVU1032
 2937 02ca B3F1FF3F 		cmp	r3, #-1
 2938 02ce 02D1     		bne	.L166
 2939              	.L165:
1525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 2940              		.loc 1 1525 89 discriminator 3 view .LVU1033
 2941 02d0 0C9B     		ldr	r3, [sp, #48]
 2942 02d2 002B     		cmp	r3, #0
 2943 02d4 99D1     		bne	.L159
 2944              	.L166:
1528:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2945              		.loc 1 1528 13 is_stmt 1 view .LVU1034
 2946 02d6 2046     		mov	r0, r4
 2947 02d8 FFF7FEFF 		bl	SPI_CloseTransfer
 2948              	.LVL142:
1530:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             hspi->State = HAL_SPI_STATE_READY;
 2949              		.loc 1 1530 13 view .LVU1035
 2950 02dc D4F88430 		ldr	r3, [r4, #132]
 2951 02e0 43F48073 		orr	r3, r3, #256
 2952 02e4 C4F88430 		str	r3, [r4, #132]
1531:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2953              		.loc 1 1531 13 view .LVU1036
1531:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2954              		.loc 1 1531 25 is_stmt 0 view .LVU1037
 2955 02e8 0123     		movs	r3, #1
 2956 02ea 84F88130 		strb	r3, [r4, #129]
1534:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2957              		.loc 1 1534 13 is_stmt 1 view .LVU1038
1534:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2958              		.loc 1 1534 13 view .LVU1039
 2959 02ee 0023     		movs	r3, #0
 2960 02f0 84F88030 		strb	r3, [r4, #128]
1534:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2961              		.loc 1 1534 13 view .LVU1040
1536:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
 2962              		.loc 1 1536 13 view .LVU1041
1536:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
 2963              		.loc 1 1536 20 is_stmt 0 view .LVU1042
 2964 02f4 4FF0030A 		mov	r10, #3
 2965 02f8 C7E0     		b	.L145
 2966              	.L187:
 2967 02fa 00BF     		.align	2
 2968              	.L186:
 2969 02fc 00300140 		.word	1073819648
 2970 0300 00380040 		.word	1073756160
 2971              	.LVL143:
 2972              	.L168:
1558:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 138


 2973              		.loc 1 1558 7 is_stmt 1 view .LVU1043
1558:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2974              		.loc 1 1558 25 is_stmt 0 view .LVU1044
 2975 0304 2368     		ldr	r3, [r4]
1558:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 2976              		.loc 1 1558 19 view .LVU1045
 2977 0306 5A69     		ldr	r2, [r3, #20]
 2978              	.LVL144:
1560:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2979              		.loc 1 1560 7 is_stmt 1 view .LVU1046
1560:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 2980              		.loc 1 1560 10 is_stmt 0 view .LVU1047
 2981 0308 BBF1000F 		cmp	fp, #0
 2982 030c 15D0     		beq	.L158
1563:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2983              		.loc 1 1563 9 is_stmt 1 view .LVU1048
1563:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2984              		.loc 1 1563 13 is_stmt 0 view .LVU1049
 2985 030e 5969     		ldr	r1, [r3, #20]
1563:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 2986              		.loc 1 1563 12 view .LVU1050
 2987 0310 11F0010F 		tst	r1, #1
 2988 0314 34D0     		beq	.L170
1565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 2989              		.loc 1 1565 11 is_stmt 1 view .LVU1051
1565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 2990              		.loc 1 1565 28 is_stmt 0 view .LVU1052
 2991 0316 626E     		ldr	r2, [r4, #100]
 2992              	.LVL145:
1565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 2993              		.loc 1 1565 44 view .LVU1053
 2994 0318 93F83030 		ldrb	r3, [r3, #48]	@ zero_extendqisi2
1565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 2995              		.loc 1 1565 42 view .LVU1054
 2996 031c 1370     		strb	r3, [r2]
1566:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2997              		.loc 1 1566 11 is_stmt 1 view .LVU1055
1566:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 2998              		.loc 1 1566 15 is_stmt 0 view .LVU1056
 2999 031e 636E     		ldr	r3, [r4, #100]
1566:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 3000              		.loc 1 1566 28 view .LVU1057
 3001 0320 0133     		adds	r3, r3, #1
 3002 0322 6366     		str	r3, [r4, #100]
1567:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 3003              		.loc 1 1567 11 is_stmt 1 view .LVU1058
1567:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 3004              		.loc 1 1567 15 is_stmt 0 view .LVU1059
 3005 0324 B4F86A30 		ldrh	r3, [r4, #106]
 3006 0328 9BB2     		uxth	r3, r3
1567:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 3007              		.loc 1 1567 28 view .LVU1060
 3008 032a 013B     		subs	r3, r3, #1
 3009 032c 9BB2     		uxth	r3, r3
 3010 032e A4F86A30 		strh	r3, [r4, #106]	@ movhi
1568:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 3011              		.loc 1 1568 11 is_stmt 1 view .LVU1061
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 139


1568:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 3012              		.loc 1 1568 31 is_stmt 0 view .LVU1062
 3013 0332 B4F86AB0 		ldrh	fp, [r4, #106]
 3014              	.LVL146:
1568:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 3015              		.loc 1 1568 31 view .LVU1063
 3016 0336 1FFA8BFB 		uxth	fp, fp
 3017              	.LVL147:
 3018              	.L158:
1545:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 3019              		.loc 1 1545 40 is_stmt 1 view .LVU1064
 3020 033a 45EA0B03 		orr	r3, r5, fp
 3021 033e 9BB2     		uxth	r3, r3
 3022 0340 002B     		cmp	r3, #0
 3023 0342 00F08380 		beq	.L157
1548:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 3024              		.loc 1 1548 7 view .LVU1065
1548:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 3025              		.loc 1 1548 12 is_stmt 0 view .LVU1066
 3026 0346 2368     		ldr	r3, [r4]
 3027 0348 5A69     		ldr	r2, [r3, #20]
1548:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 3028              		.loc 1 1548 10 view .LVU1067
 3029 034a 12F0020F 		tst	r2, #2
 3030 034e D9D0     		beq	.L168
1548:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 3031              		.loc 1 1548 52 discriminator 1 view .LVU1068
 3032 0350 002D     		cmp	r5, #0
 3033 0352 D7D0     		beq	.L168
1549:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 3034              		.loc 1 1549 56 view .LVU1069
 3035 0354 05EB0802 		add	r2, r5, r8
1548:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           (initial_RxXferCount  < (initial_TxXferCount + fifo_length)))
 3036              		.loc 1 1548 83 discriminator 2 view .LVU1070
 3037 0358 9345     		cmp	fp, r2
 3038 035a D3D2     		bcs	.L168
1551:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint8_t);
 3039              		.loc 1 1551 9 is_stmt 1 view .LVU1071
1551:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint8_t);
 3040              		.loc 1 1551 75 is_stmt 0 view .LVU1072
 3041 035c E26D     		ldr	r2, [r4, #92]
1551:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint8_t);
 3042              		.loc 1 1551 52 view .LVU1073
 3043 035e 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
1551:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint8_t);
 3044              		.loc 1 1551 50 view .LVU1074
 3045 0360 83F82020 		strb	r2, [r3, #32]
1552:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount--;
 3046              		.loc 1 1552 9 is_stmt 1 view .LVU1075
1552:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount--;
 3047              		.loc 1 1552 13 is_stmt 0 view .LVU1076
 3048 0364 E36D     		ldr	r3, [r4, #92]
1552:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         hspi->TxXferCount--;
 3049              		.loc 1 1552 26 view .LVU1077
 3050 0366 0133     		adds	r3, r3, #1
 3051 0368 E365     		str	r3, [r4, #92]
1553:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         initial_TxXferCount = hspi->TxXferCount;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 140


 3052              		.loc 1 1553 9 is_stmt 1 view .LVU1078
1553:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         initial_TxXferCount = hspi->TxXferCount;
 3053              		.loc 1 1553 13 is_stmt 0 view .LVU1079
 3054 036a B4F86230 		ldrh	r3, [r4, #98]
 3055 036e 9BB2     		uxth	r3, r3
1553:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         initial_TxXferCount = hspi->TxXferCount;
 3056              		.loc 1 1553 26 view .LVU1080
 3057 0370 013B     		subs	r3, r3, #1
 3058 0372 9BB2     		uxth	r3, r3
 3059 0374 A4F86230 		strh	r3, [r4, #98]	@ movhi
1554:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 3060              		.loc 1 1554 9 is_stmt 1 view .LVU1081
1554:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 3061              		.loc 1 1554 29 is_stmt 0 view .LVU1082
 3062 0378 B4F86250 		ldrh	r5, [r4, #98]
 3063              	.LVL148:
1554:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 3064              		.loc 1 1554 29 view .LVU1083
 3065 037c ADB2     		uxth	r5, r5
 3066 037e C1E7     		b	.L168
 3067              	.LVL149:
 3068              	.L170:
1571:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 3069              		.loc 1 1571 14 is_stmt 1 view .LVU1084
1571:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 3070              		.loc 1 1571 17 is_stmt 0 view .LVU1085
 3071 0380 B345     		cmp	fp, r6
 3072 0382 2AD2     		bcs	.L171
1571:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 3073              		.loc 1 1571 64 discriminator 1 view .LVU1086
 3074 0384 12F4004F 		tst	r2, #32768
 3075 0388 27D0     		beq	.L171
1573:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3076              		.loc 1 1573 11 is_stmt 1 view .LVU1087
1573:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3077              		.loc 1 1573 28 is_stmt 0 view .LVU1088
 3078 038a 626E     		ldr	r2, [r4, #100]
 3079              	.LVL150:
1573:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3080              		.loc 1 1573 44 view .LVU1089
 3081 038c 93F83030 		ldrb	r3, [r3, #48]	@ zero_extendqisi2
1573:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3082              		.loc 1 1573 42 view .LVU1090
 3083 0390 1370     		strb	r3, [r2]
1574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 3084              		.loc 1 1574 11 is_stmt 1 view .LVU1091
1574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 3085              		.loc 1 1574 15 is_stmt 0 view .LVU1092
 3086 0392 636E     		ldr	r3, [r4, #100]
1574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 3087              		.loc 1 1574 28 view .LVU1093
 3088 0394 5A1C     		adds	r2, r3, #1
 3089 0396 6266     		str	r2, [r4, #100]
1575:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3090              		.loc 1 1575 11 is_stmt 1 view .LVU1094
1575:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3091              		.loc 1 1575 67 is_stmt 0 view .LVU1095
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 141


 3092 0398 2268     		ldr	r2, [r4]
1575:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3093              		.loc 1 1575 44 view .LVU1096
 3094 039a 92F83020 		ldrb	r2, [r2, #48]	@ zero_extendqisi2
1575:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3095              		.loc 1 1575 42 view .LVU1097
 3096 039e 5A70     		strb	r2, [r3, #1]
1576:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 3097              		.loc 1 1576 11 is_stmt 1 view .LVU1098
1576:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 3098              		.loc 1 1576 15 is_stmt 0 view .LVU1099
 3099 03a0 636E     		ldr	r3, [r4, #100]
1576:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 3100              		.loc 1 1576 28 view .LVU1100
 3101 03a2 5A1C     		adds	r2, r3, #1
 3102 03a4 6266     		str	r2, [r4, #100]
1577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3103              		.loc 1 1577 11 is_stmt 1 view .LVU1101
1577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3104              		.loc 1 1577 67 is_stmt 0 view .LVU1102
 3105 03a6 2268     		ldr	r2, [r4]
1577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3106              		.loc 1 1577 44 view .LVU1103
 3107 03a8 92F83020 		ldrb	r2, [r2, #48]	@ zero_extendqisi2
1577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3108              		.loc 1 1577 42 view .LVU1104
 3109 03ac 5A70     		strb	r2, [r3, #1]
1578:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 3110              		.loc 1 1578 11 is_stmt 1 view .LVU1105
1578:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 3111              		.loc 1 1578 15 is_stmt 0 view .LVU1106
 3112 03ae 636E     		ldr	r3, [r4, #100]
1578:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           *((uint8_t *)hspi->pRxBuffPtr) = *((__IO uint8_t *)&hspi->Instance->RXDR);
 3113              		.loc 1 1578 28 view .LVU1107
 3114 03b0 5A1C     		adds	r2, r3, #1
 3115 03b2 6266     		str	r2, [r4, #100]
1579:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3116              		.loc 1 1579 11 is_stmt 1 view .LVU1108
1579:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3117              		.loc 1 1579 67 is_stmt 0 view .LVU1109
 3118 03b4 2268     		ldr	r2, [r4]
1579:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3119              		.loc 1 1579 44 view .LVU1110
 3120 03b6 92F83020 		ldrb	r2, [r2, #48]	@ zero_extendqisi2
1579:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3121              		.loc 1 1579 42 view .LVU1111
 3122 03ba 5A70     		strb	r2, [r3, #1]
1580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount -= (uint16_t)4UL;
 3123              		.loc 1 1580 11 is_stmt 1 view .LVU1112
1580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount -= (uint16_t)4UL;
 3124              		.loc 1 1580 15 is_stmt 0 view .LVU1113
 3125 03bc 636E     		ldr	r3, [r4, #100]
1580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount -= (uint16_t)4UL;
 3126              		.loc 1 1580 28 view .LVU1114
 3127 03be 0133     		adds	r3, r3, #1
 3128 03c0 6366     		str	r3, [r4, #100]
1581:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 142


 3129              		.loc 1 1581 11 is_stmt 1 view .LVU1115
1581:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 3130              		.loc 1 1581 15 is_stmt 0 view .LVU1116
 3131 03c2 B4F86A30 		ldrh	r3, [r4, #106]
 3132 03c6 9BB2     		uxth	r3, r3
1581:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 3133              		.loc 1 1581 29 view .LVU1117
 3134 03c8 043B     		subs	r3, r3, #4
 3135 03ca 9BB2     		uxth	r3, r3
 3136 03cc A4F86A30 		strh	r3, [r4, #106]	@ movhi
1582:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 3137              		.loc 1 1582 11 is_stmt 1 view .LVU1118
1582:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 3138              		.loc 1 1582 31 is_stmt 0 view .LVU1119
 3139 03d0 B4F86AB0 		ldrh	fp, [r4, #106]
 3140              	.LVL151:
1582:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 3141              		.loc 1 1582 31 view .LVU1120
 3142 03d4 1FFA8BFB 		uxth	fp, fp
 3143              	.LVL152:
1582:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 3144              		.loc 1 1582 31 view .LVU1121
 3145 03d8 AFE7     		b	.L158
 3146              	.LVL153:
 3147              	.L171:
1585:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 3148              		.loc 1 1585 14 is_stmt 1 view .LVU1122
1585:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 3149              		.loc 1 1585 17 is_stmt 0 view .LVU1123
 3150 03da BBF1030F 		cmp	fp, #3
 3151 03de 15D8     		bhi	.L172
1585:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 3152              		.loc 1 1585 46 discriminator 1 view .LVU1124
 3153 03e0 12F4C04F 		tst	r2, #24576
 3154 03e4 12D0     		beq	.L172
1587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3155              		.loc 1 1587 11 is_stmt 1 view .LVU1125
1587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3156              		.loc 1 1587 28 is_stmt 0 view .LVU1126
 3157 03e6 626E     		ldr	r2, [r4, #100]
 3158              	.LVL154:
1587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3159              		.loc 1 1587 44 view .LVU1127
 3160 03e8 93F83030 		ldrb	r3, [r3, #48]	@ zero_extendqisi2
1587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 3161              		.loc 1 1587 42 view .LVU1128
 3162 03ec 1370     		strb	r3, [r2]
1588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 3163              		.loc 1 1588 11 is_stmt 1 view .LVU1129
1588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 3164              		.loc 1 1588 15 is_stmt 0 view .LVU1130
 3165 03ee 636E     		ldr	r3, [r4, #100]
1588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->RxXferCount--;
 3166              		.loc 1 1588 28 view .LVU1131
 3167 03f0 0133     		adds	r3, r3, #1
 3168 03f2 6366     		str	r3, [r4, #100]
1589:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 143


 3169              		.loc 1 1589 11 is_stmt 1 view .LVU1132
1589:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 3170              		.loc 1 1589 15 is_stmt 0 view .LVU1133
 3171 03f4 B4F86A30 		ldrh	r3, [r4, #106]
 3172 03f8 9BB2     		uxth	r3, r3
1589:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           initial_RxXferCount = hspi->RxXferCount;
 3173              		.loc 1 1589 28 view .LVU1134
 3174 03fa 013B     		subs	r3, r3, #1
 3175 03fc 9BB2     		uxth	r3, r3
 3176 03fe A4F86A30 		strh	r3, [r4, #106]	@ movhi
1590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 3177              		.loc 1 1590 11 is_stmt 1 view .LVU1135
1590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 3178              		.loc 1 1590 31 is_stmt 0 view .LVU1136
 3179 0402 B4F86AB0 		ldrh	fp, [r4, #106]
 3180              	.LVL155:
1590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 3181              		.loc 1 1590 31 view .LVU1137
 3182 0406 1FFA8BFB 		uxth	fp, fp
 3183              	.LVL156:
1590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 3184              		.loc 1 1590 31 view .LVU1138
 3185 040a 96E7     		b	.L158
 3186              	.LVL157:
 3187              	.L172:
1595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 3188              		.loc 1 1595 11 is_stmt 1 view .LVU1139
1595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 3189              		.loc 1 1595 18 is_stmt 0 view .LVU1140
 3190 040c FFF7FEFF 		bl	HAL_GetTick
 3191              	.LVL158:
1595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 3192              		.loc 1 1595 32 discriminator 1 view .LVU1141
 3193 0410 C01B     		subs	r0, r0, r7
1595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 3194              		.loc 1 1595 14 discriminator 1 view .LVU1142
 3195 0412 0C9B     		ldr	r3, [sp, #48]
 3196 0414 9842     		cmp	r0, r3
 3197 0416 02D3     		bcc	.L173
1595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 3198              		.loc 1 1595 58 discriminator 1 view .LVU1143
 3199 0418 B3F1FF3F 		cmp	r3, #-1
 3200 041c 02D1     		bne	.L174
 3201              	.L173:
1595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 3202              		.loc 1 1595 89 discriminator 3 view .LVU1144
 3203 041e 0C9B     		ldr	r3, [sp, #48]
 3204 0420 002B     		cmp	r3, #0
 3205 0422 8AD1     		bne	.L158
 3206              	.L174:
1598:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3207              		.loc 1 1598 13 is_stmt 1 view .LVU1145
 3208 0424 2046     		mov	r0, r4
 3209 0426 FFF7FEFF 		bl	SPI_CloseTransfer
 3210              	.LVL159:
1600:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****             hspi->State = HAL_SPI_STATE_READY;
 3211              		.loc 1 1600 13 view .LVU1146
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 144


 3212 042a D4F88430 		ldr	r3, [r4, #132]
 3213 042e 43F48073 		orr	r3, r3, #256
 3214 0432 C4F88430 		str	r3, [r4, #132]
1601:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3215              		.loc 1 1601 13 view .LVU1147
1601:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3216              		.loc 1 1601 25 is_stmt 0 view .LVU1148
 3217 0436 0123     		movs	r3, #1
 3218 0438 84F88130 		strb	r3, [r4, #129]
1604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3219              		.loc 1 1604 13 is_stmt 1 view .LVU1149
1604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3220              		.loc 1 1604 13 view .LVU1150
 3221 043c 0023     		movs	r3, #0
 3222 043e 84F88030 		strb	r3, [r4, #128]
1604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3223              		.loc 1 1604 13 view .LVU1151
1606:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
 3224              		.loc 1 1606 13 view .LVU1152
1606:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
 3225              		.loc 1 1606 20 is_stmt 0 view .LVU1153
 3226 0442 4FF0030A 		mov	r10, #3
 3227 0446 20E0     		b	.L145
 3228              	.LVL160:
 3229              	.L181:
1341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3230              		.loc 1 1341 23 view .LVU1154
 3231 0448 AB46     		mov	fp, r5
 3232              	.LVL161:
1341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3233              		.loc 1 1341 23 view .LVU1155
 3234 044a 76E7     		b	.L158
 3235              	.LVL162:
 3236              	.L157:
1614:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3237              		.loc 1 1614 3 is_stmt 1 view .LVU1156
1614:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3238              		.loc 1 1614 7 is_stmt 0 view .LVU1157
 3239 044c 0097     		str	r7, [sp]
 3240 044e 0C9B     		ldr	r3, [sp, #48]
 3241 0450 0022     		movs	r2, #0
 3242 0452 0821     		movs	r1, #8
 3243 0454 2046     		mov	r0, r4
 3244 0456 FFF7FEFF 		bl	SPI_WaitOnFlagUntilTimeout
 3245              	.LVL163:
1614:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3246              		.loc 1 1614 6 discriminator 1 view .LVU1158
 3247 045a 28B1     		cbz	r0, .L176
1616:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3248              		.loc 1 1616 5 is_stmt 1 view .LVU1159
 3249 045c D4F88430 		ldr	r3, [r4, #132]
 3250 0460 43F02003 		orr	r3, r3, #32
 3251 0464 C4F88430 		str	r3, [r4, #132]
 3252              	.L176:
1620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3253              		.loc 1 1620 3 view .LVU1160
 3254 0468 2046     		mov	r0, r4
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 145


 3255 046a FFF7FEFF 		bl	SPI_CloseTransfer
 3256              	.LVL164:
1622:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3257              		.loc 1 1622 3 view .LVU1161
1622:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3258              		.loc 1 1622 15 is_stmt 0 view .LVU1162
 3259 046e 0123     		movs	r3, #1
 3260 0470 84F88130 		strb	r3, [r4, #129]
1625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3261              		.loc 1 1625 3 is_stmt 1 view .LVU1163
1625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3262              		.loc 1 1625 3 view .LVU1164
 3263 0474 0023     		movs	r3, #0
 3264 0476 84F88030 		strb	r3, [r4, #128]
1625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3265              		.loc 1 1625 3 view .LVU1165
1627:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3266              		.loc 1 1627 3 view .LVU1166
1627:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3267              		.loc 1 1627 11 is_stmt 0 view .LVU1167
 3268 047a D4F88430 		ldr	r3, [r4, #132]
1627:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3269              		.loc 1 1627 6 view .LVU1168
 3270 047e 23B9     		cbnz	r3, .L145
1633:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3271              		.loc 1 1633 12 view .LVU1169
 3272 0480 4FF0000A 		mov	r10, #0
 3273 0484 01E0     		b	.L145
 3274              	.LVL165:
 3275              	.L177:
1345:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3276              		.loc 1 1345 12 view .LVU1170
 3277 0486 4FF0020A 		mov	r10, #2
 3278              	.LVL166:
 3279              	.L145:
1635:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3280              		.loc 1 1635 1 view .LVU1171
 3281 048a 5046     		mov	r0, r10
 3282 048c 03B0     		add	sp, sp, #12
 3283              		.cfi_remember_state
 3284              		.cfi_def_cfa_offset 36
 3285              		@ sp needed
 3286 048e BDE8F08F 		pop	{r4, r5, r6, r7, r8, r9, r10, fp, pc}
 3287              	.LVL167:
 3288              	.L178:
 3289              		.cfi_restore_state
1354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3290              		.loc 1 1354 3 discriminator 1 view .LVU1172
 3291 0492 4FF0020A 		mov	r10, #2
 3292 0496 F8E7     		b	.L145
 3293              		.cfi_endproc
 3294              	.LFE341:
 3296              		.section	.text.HAL_SPI_Transmit_IT,"ax",%progbits
 3297              		.align	1
 3298              		.global	HAL_SPI_Transmit_IT
 3299              		.syntax unified
 3300              		.thumb
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 146


 3301              		.thumb_func
 3303              	HAL_SPI_Transmit_IT:
 3304              	.LVL168:
 3305              	.LFB342:
1646:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
 3306              		.loc 1 1646 1 is_stmt 1 view -0
 3307              		.cfi_startproc
 3308              		@ args = 0, pretend = 0, frame = 0
 3309              		@ frame_needed = 0, uses_anonymous_args = 0
 3310              		@ link register save eliminated.
1648:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3311              		.loc 1 1648 3 view .LVU1174
1650:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3312              		.loc 1 1650 3 view .LVU1175
1650:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3313              		.loc 1 1650 6 is_stmt 0 view .LVU1176
 3314 0000 002A     		cmp	r2, #0
 3315 0002 18BF     		it	ne
 3316 0004 0029     		cmpne	r1, #0
 3317 0006 5AD0     		beq	.L195
1655:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3318              		.loc 1 1655 3 is_stmt 1 view .LVU1177
1655:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3319              		.loc 1 1655 11 is_stmt 0 view .LVU1178
 3320 0008 90F88130 		ldrb	r3, [r0, #129]	@ zero_extendqisi2
1655:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3321              		.loc 1 1655 6 view .LVU1179
 3322 000c 012B     		cmp	r3, #1
 3323 000e 58D1     		bne	.L196
1661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3324              		.loc 1 1661 3 is_stmt 1 view .LVU1180
1661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3325              		.loc 1 1661 3 view .LVU1181
 3326 0010 90F88030 		ldrb	r3, [r0, #128]	@ zero_extendqisi2
 3327 0014 012B     		cmp	r3, #1
 3328 0016 56D0     		beq	.L197
1661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3329              		.loc 1 1661 3 discriminator 2 view .LVU1182
 3330 0018 0123     		movs	r3, #1
 3331 001a 80F88030 		strb	r3, [r0, #128]
1661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3332              		.loc 1 1661 3 view .LVU1183
1664:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3333              		.loc 1 1664 3 view .LVU1184
1664:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3334              		.loc 1 1664 21 is_stmt 0 view .LVU1185
 3335 001e 0323     		movs	r3, #3
 3336 0020 80F88130 		strb	r3, [r0, #129]
1665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pData;
 3337              		.loc 1 1665 3 is_stmt 1 view .LVU1186
1665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pData;
 3338              		.loc 1 1665 21 is_stmt 0 view .LVU1187
 3339 0024 0023     		movs	r3, #0
 3340 0026 C0F88430 		str	r3, [r0, #132]
1666:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3341              		.loc 1 1666 3 is_stmt 1 view .LVU1188
1666:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 147


 3342              		.loc 1 1666 21 is_stmt 0 view .LVU1189
 3343 002a C165     		str	r1, [r0, #92]
1667:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3344              		.loc 1 1667 3 is_stmt 1 view .LVU1190
1667:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3345              		.loc 1 1667 21 is_stmt 0 view .LVU1191
 3346 002c A0F86020 		strh	r2, [r0, #96]	@ movhi
1668:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3347              		.loc 1 1668 3 is_stmt 1 view .LVU1192
1668:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3348              		.loc 1 1668 21 is_stmt 0 view .LVU1193
 3349 0030 A0F86220 		strh	r2, [r0, #98]	@ movhi
1671:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = (uint16_t) 0UL;
 3350              		.loc 1 1671 3 is_stmt 1 view .LVU1194
1671:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = (uint16_t) 0UL;
 3351              		.loc 1 1671 21 is_stmt 0 view .LVU1195
 3352 0034 4366     		str	r3, [r0, #100]
1672:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t) 0UL;
 3353              		.loc 1 1672 3 is_stmt 1 view .LVU1196
1672:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t) 0UL;
 3354              		.loc 1 1672 21 is_stmt 0 view .LVU1197
 3355 0036 A0F86830 		strh	r3, [r0, #104]	@ movhi
1673:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
 3356              		.loc 1 1673 3 is_stmt 1 view .LVU1198
1673:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
 3357              		.loc 1 1673 21 is_stmt 0 view .LVU1199
 3358 003a A0F86A30 		strh	r3, [r0, #106]	@ movhi
1674:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3359              		.loc 1 1674 3 is_stmt 1 view .LVU1200
1674:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3360              		.loc 1 1674 21 is_stmt 0 view .LVU1201
 3361 003e 0367     		str	r3, [r0, #112]
1683:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3362              		.loc 1 1683 3 is_stmt 1 view .LVU1202
1683:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3363              		.loc 1 1683 17 is_stmt 0 view .LVU1203
 3364 0040 C368     		ldr	r3, [r0, #12]
1683:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3365              		.loc 1 1683 6 view .LVU1204
 3366 0042 0F2B     		cmp	r3, #15
 3367 0044 26D9     		bls	.L190
1685:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3368              		.loc 1 1685 5 is_stmt 1 view .LVU1205
1685:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3369              		.loc 1 1685 17 is_stmt 0 view .LVU1206
 3370 0046 214B     		ldr	r3, .L201
 3371 0048 4367     		str	r3, [r0, #116]
 3372              	.L191:
1697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3373              		.loc 1 1697 3 is_stmt 1 view .LVU1207
1697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3374              		.loc 1 1697 17 is_stmt 0 view .LVU1208
 3375 004a 8368     		ldr	r3, [r0, #8]
1697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3376              		.loc 1 1697 6 view .LVU1209
 3377 004c B3F5C02F 		cmp	r3, #393216
 3378 0050 28D0     		beq	.L199
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 148


1703:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3379              		.loc 1 1703 5 is_stmt 1 view .LVU1210
 3380 0052 0168     		ldr	r1, [r0]
 3381              	.LVL169:
1703:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3382              		.loc 1 1703 5 is_stmt 0 view .LVU1211
 3383 0054 CB68     		ldr	r3, [r1, #12]
 3384 0056 23F4C023 		bic	r3, r3, #393216
 3385 005a 43F40033 		orr	r3, r3, #131072
 3386 005e CB60     		str	r3, [r1, #12]
 3387              	.LVL170:
 3388              	.L194:
1707:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3389              		.loc 1 1707 3 is_stmt 1 view .LVU1212
 3390 0060 0168     		ldr	r1, [r0]
 3391 0062 4B68     		ldr	r3, [r1, #4]
 3392 0064 6FF30F03 		bfc	r3, #0, #16
 3393 0068 1A43     		orrs	r2, r2, r3
 3394              	.LVL171:
1707:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3395              		.loc 1 1707 3 is_stmt 0 view .LVU1213
 3396 006a 4A60     		str	r2, [r1, #4]
1710:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3397              		.loc 1 1710 3 is_stmt 1 view .LVU1214
 3398 006c 0268     		ldr	r2, [r0]
 3399 006e 1368     		ldr	r3, [r2]
 3400 0070 43F00103 		orr	r3, r3, #1
 3401 0074 1360     		str	r3, [r2]
1713:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3402              		.loc 1 1713 3 view .LVU1215
1713:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3403              		.loc 1 1713 3 view .LVU1216
 3404 0076 0023     		movs	r3, #0
 3405 0078 80F88030 		strb	r3, [r0, #128]
1713:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3406              		.loc 1 1713 3 view .LVU1217
1716:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3407              		.loc 1 1716 3 view .LVU1218
 3408 007c 0268     		ldr	r2, [r0]
 3409 007e 1169     		ldr	r1, [r2, #16]
 3410 0080 40F22A73 		movw	r3, #1834
 3411 0084 0B43     		orrs	r3, r3, r1
 3412 0086 1361     		str	r3, [r2, #16]
1718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3413              		.loc 1 1718 3 view .LVU1219
1718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3414              		.loc 1 1718 17 is_stmt 0 view .LVU1220
 3415 0088 4368     		ldr	r3, [r0, #4]
1718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3416              		.loc 1 1718 6 view .LVU1221
 3417 008a B3F5800F 		cmp	r3, #4194304
 3418 008e 0FD0     		beq	.L200
1724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 3419              		.loc 1 1724 10 view .LVU1222
 3420 0090 0020     		movs	r0, #0
 3421              	.LVL172:
1725:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 149


 3422              		.loc 1 1725 1 view .LVU1223
 3423 0092 7047     		bx	lr
 3424              	.LVL173:
 3425              	.L190:
1687:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3426              		.loc 1 1687 8 is_stmt 1 view .LVU1224
1687:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3427              		.loc 1 1687 11 is_stmt 0 view .LVU1225
 3428 0094 072B     		cmp	r3, #7
 3429 0096 02D9     		bls	.L192
1689:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3430              		.loc 1 1689 5 is_stmt 1 view .LVU1226
1689:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3431              		.loc 1 1689 17 is_stmt 0 view .LVU1227
 3432 0098 0D4B     		ldr	r3, .L201+4
 3433 009a 4367     		str	r3, [r0, #116]
 3434 009c D5E7     		b	.L191
 3435              	.L192:
1693:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3436              		.loc 1 1693 5 is_stmt 1 view .LVU1228
1693:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3437              		.loc 1 1693 17 is_stmt 0 view .LVU1229
 3438 009e 0D4B     		ldr	r3, .L201+8
 3439 00a0 4367     		str	r3, [r0, #116]
 3440 00a2 D2E7     		b	.L191
 3441              	.L199:
1699:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3442              		.loc 1 1699 5 is_stmt 1 view .LVU1230
 3443 00a4 0168     		ldr	r1, [r0]
 3444              	.LVL174:
1699:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3445              		.loc 1 1699 5 is_stmt 0 view .LVU1231
 3446 00a6 0B68     		ldr	r3, [r1]
 3447 00a8 43F40063 		orr	r3, r3, #2048
 3448 00ac 0B60     		str	r3, [r1]
 3449              	.LVL175:
1699:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3450              		.loc 1 1699 5 view .LVU1232
 3451 00ae D7E7     		b	.L194
 3452              	.LVL176:
 3453              	.L200:
1721:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3454              		.loc 1 1721 5 is_stmt 1 view .LVU1233
 3455 00b0 0268     		ldr	r2, [r0]
 3456 00b2 1368     		ldr	r3, [r2]
 3457 00b4 43F40073 		orr	r3, r3, #512
 3458 00b8 1360     		str	r3, [r2]
1724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 3459              		.loc 1 1724 10 is_stmt 0 view .LVU1234
 3460 00ba 0020     		movs	r0, #0
 3461              	.LVL177:
1724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 3462              		.loc 1 1724 10 view .LVU1235
 3463 00bc 7047     		bx	lr
 3464              	.LVL178:
 3465              	.L195:
1652:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 150


 3466              		.loc 1 1652 12 view .LVU1236
 3467 00be 0120     		movs	r0, #1
 3468              	.LVL179:
1652:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3469              		.loc 1 1652 12 view .LVU1237
 3470 00c0 7047     		bx	lr
 3471              	.LVL180:
 3472              	.L196:
1657:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3473              		.loc 1 1657 12 view .LVU1238
 3474 00c2 0220     		movs	r0, #2
 3475              	.LVL181:
1657:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3476              		.loc 1 1657 12 view .LVU1239
 3477 00c4 7047     		bx	lr
 3478              	.LVL182:
 3479              	.L197:
1661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3480              		.loc 1 1661 3 discriminator 1 view .LVU1240
 3481 00c6 0220     		movs	r0, #2
 3482              	.LVL183:
1661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3483              		.loc 1 1661 3 discriminator 1 view .LVU1241
 3484 00c8 7047     		bx	lr
 3485              	.L202:
 3486 00ca 00BF     		.align	2
 3487              	.L201:
 3488 00cc 00000000 		.word	SPI_TxISR_32BIT
 3489 00d0 00000000 		.word	SPI_TxISR_16BIT
 3490 00d4 00000000 		.word	SPI_TxISR_8BIT
 3491              		.cfi_endproc
 3492              	.LFE342:
 3494              		.section	.text.HAL_SPI_Receive_IT,"ax",%progbits
 3495              		.align	1
 3496              		.global	HAL_SPI_Receive_IT
 3497              		.syntax unified
 3498              		.thumb
 3499              		.thumb_func
 3501              	HAL_SPI_Receive_IT:
 3502              	.LVL184:
 3503              	.LFB343:
1736:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
 3504              		.loc 1 1736 1 is_stmt 1 view -0
 3505              		.cfi_startproc
 3506              		@ args = 0, pretend = 0, frame = 0
 3507              		@ frame_needed = 0, uses_anonymous_args = 0
 3508              		@ link register save eliminated.
1736:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
 3509              		.loc 1 1736 1 is_stmt 0 view .LVU1243
 3510 0000 0346     		mov	r3, r0
1738:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3511              		.loc 1 1738 3 is_stmt 1 view .LVU1244
1740:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3512              		.loc 1 1740 3 view .LVU1245
1740:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3513              		.loc 1 1740 11 is_stmt 0 view .LVU1246
 3514 0002 90F881C0 		ldrb	ip, [r0, #129]	@ zero_extendqisi2
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 151


 3515 0006 5FFA8CF0 		uxtb	r0, ip
 3516              	.LVL185:
1740:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3517              		.loc 1 1740 6 view .LVU1247
 3518 000a BCF1010F 		cmp	ip, #1
 3519 000e 5AD1     		bne	.L210
1745:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3520              		.loc 1 1745 3 is_stmt 1 view .LVU1248
1745:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3521              		.loc 1 1745 6 is_stmt 0 view .LVU1249
 3522 0010 002A     		cmp	r2, #0
 3523 0012 18BF     		it	ne
 3524 0014 0029     		cmpne	r1, #0
 3525 0016 40D0     		beq	.L204
1751:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3526              		.loc 1 1751 3 is_stmt 1 view .LVU1250
1751:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3527              		.loc 1 1751 3 view .LVU1251
 3528 0018 93F88000 		ldrb	r0, [r3, #128]	@ zero_extendqisi2
 3529 001c 0128     		cmp	r0, #1
 3530 001e 54D0     		beq	.L211
1751:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3531              		.loc 1 1751 3 discriminator 2 view .LVU1252
 3532 0020 0120     		movs	r0, #1
 3533 0022 83F88000 		strb	r0, [r3, #128]
1751:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3534              		.loc 1 1751 3 view .LVU1253
1754:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3535              		.loc 1 1754 3 view .LVU1254
1754:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3536              		.loc 1 1754 21 is_stmt 0 view .LVU1255
 3537 0026 0420     		movs	r0, #4
 3538 0028 83F88100 		strb	r0, [r3, #129]
1755:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 3539              		.loc 1 1755 3 is_stmt 1 view .LVU1256
1755:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 3540              		.loc 1 1755 21 is_stmt 0 view .LVU1257
 3541 002c 0020     		movs	r0, #0
 3542 002e C3F88400 		str	r0, [r3, #132]
1756:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3543              		.loc 1 1756 3 is_stmt 1 view .LVU1258
1756:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3544              		.loc 1 1756 21 is_stmt 0 view .LVU1259
 3545 0032 5966     		str	r1, [r3, #100]
1757:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3546              		.loc 1 1757 3 is_stmt 1 view .LVU1260
1757:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3547              		.loc 1 1757 21 is_stmt 0 view .LVU1261
 3548 0034 A3F86820 		strh	r2, [r3, #104]	@ movhi
1758:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3549              		.loc 1 1758 3 is_stmt 1 view .LVU1262
1758:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3550              		.loc 1 1758 21 is_stmt 0 view .LVU1263
 3551 0038 A3F86A20 		strh	r2, [r3, #106]	@ movhi
1761:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = (uint16_t) 0UL;
 3552              		.loc 1 1761 3 is_stmt 1 view .LVU1264
1761:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = (uint16_t) 0UL;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 152


 3553              		.loc 1 1761 21 is_stmt 0 view .LVU1265
 3554 003c D865     		str	r0, [r3, #92]
1762:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t) 0UL;
 3555              		.loc 1 1762 3 is_stmt 1 view .LVU1266
1762:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t) 0UL;
 3556              		.loc 1 1762 21 is_stmt 0 view .LVU1267
 3557 003e A3F86000 		strh	r0, [r3, #96]	@ movhi
1763:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3558              		.loc 1 1763 3 is_stmt 1 view .LVU1268
1763:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3559              		.loc 1 1763 21 is_stmt 0 view .LVU1269
 3560 0042 A3F86200 		strh	r0, [r3, #98]	@ movhi
1764:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3561              		.loc 1 1764 3 is_stmt 1 view .LVU1270
1764:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3562              		.loc 1 1764 21 is_stmt 0 view .LVU1271
 3563 0046 5867     		str	r0, [r3, #116]
1773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3564              		.loc 1 1773 3 is_stmt 1 view .LVU1272
1773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3565              		.loc 1 1773 17 is_stmt 0 view .LVU1273
 3566 0048 D968     		ldr	r1, [r3, #12]
 3567              	.LVL186:
1773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3568              		.loc 1 1773 6 view .LVU1274
 3569 004a 0F29     		cmp	r1, #15
 3570 004c 26D9     		bls	.L205
1775:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3571              		.loc 1 1775 5 is_stmt 1 view .LVU1275
1775:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3572              		.loc 1 1775 17 is_stmt 0 view .LVU1276
 3573 004e 2049     		ldr	r1, .L215
 3574 0050 1967     		str	r1, [r3, #112]
 3575              	.L206:
1787:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3576              		.loc 1 1787 3 is_stmt 1 view .LVU1277
1787:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3577              		.loc 1 1787 17 is_stmt 0 view .LVU1278
 3578 0052 9968     		ldr	r1, [r3, #8]
1787:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3579              		.loc 1 1787 6 view .LVU1279
 3580 0054 B1F5C02F 		cmp	r1, #393216
 3581 0058 28D0     		beq	.L213
1793:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3582              		.loc 1 1793 5 is_stmt 1 view .LVU1280
 3583 005a 1868     		ldr	r0, [r3]
 3584 005c C168     		ldr	r1, [r0, #12]
 3585 005e 21F4C021 		bic	r1, r1, #393216
 3586 0062 41F48021 		orr	r1, r1, #262144
 3587 0066 C160     		str	r1, [r0, #12]
 3588              	.LVL187:
 3589              	.L209:
1801:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3590              		.loc 1 1801 3 view .LVU1281
 3591 0068 1868     		ldr	r0, [r3]
 3592 006a 4168     		ldr	r1, [r0, #4]
 3593 006c 6FF30F01 		bfc	r1, #0, #16
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 153


 3594 0070 0A43     		orrs	r2, r2, r1
 3595              	.LVL188:
1801:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3596              		.loc 1 1801 3 is_stmt 0 view .LVU1282
 3597 0072 4260     		str	r2, [r0, #4]
1804:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3598              		.loc 1 1804 3 is_stmt 1 view .LVU1283
 3599 0074 1968     		ldr	r1, [r3]
 3600 0076 0A68     		ldr	r2, [r1]
 3601 0078 42F00102 		orr	r2, r2, #1
 3602 007c 0A60     		str	r2, [r1]
1807:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3603              		.loc 1 1807 3 view .LVU1284
1807:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3604              		.loc 1 1807 3 view .LVU1285
 3605 007e 0022     		movs	r2, #0
 3606 0080 83F88020 		strb	r2, [r3, #128]
1807:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3607              		.loc 1 1807 3 view .LVU1286
1810:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3608              		.loc 1 1810 3 view .LVU1287
 3609 0084 1968     		ldr	r1, [r3]
 3610 0086 0869     		ldr	r0, [r1, #16]
 3611 0088 40F24972 		movw	r2, #1865
 3612 008c 0243     		orrs	r2, r2, r0
 3613 008e 0A61     		str	r2, [r1, #16]
1812:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3614              		.loc 1 1812 3 view .LVU1288
1812:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3615              		.loc 1 1812 17 is_stmt 0 view .LVU1289
 3616 0090 5A68     		ldr	r2, [r3, #4]
1812:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3617              		.loc 1 1812 6 view .LVU1290
 3618 0092 B2F5800F 		cmp	r2, #4194304
 3619 0096 0FD0     		beq	.L214
1818:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 3620              		.loc 1 1818 10 view .LVU1291
 3621 0098 0020     		movs	r0, #0
 3622              	.L204:
1819:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3623              		.loc 1 1819 1 view .LVU1292
 3624 009a 7047     		bx	lr
 3625              	.LVL189:
 3626              	.L205:
1777:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3627              		.loc 1 1777 8 is_stmt 1 view .LVU1293
1777:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3628              		.loc 1 1777 11 is_stmt 0 view .LVU1294
 3629 009c 0729     		cmp	r1, #7
 3630 009e 02D9     		bls	.L207
1779:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3631              		.loc 1 1779 5 is_stmt 1 view .LVU1295
1779:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3632              		.loc 1 1779 17 is_stmt 0 view .LVU1296
 3633 00a0 0C49     		ldr	r1, .L215+4
 3634 00a2 1967     		str	r1, [r3, #112]
 3635 00a4 D5E7     		b	.L206
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 154


 3636              	.L207:
1783:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3637              		.loc 1 1783 5 is_stmt 1 view .LVU1297
1783:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3638              		.loc 1 1783 17 is_stmt 0 view .LVU1298
 3639 00a6 0C49     		ldr	r1, .L215+8
 3640 00a8 1967     		str	r1, [r3, #112]
 3641 00aa D2E7     		b	.L206
 3642              	.L213:
1789:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3643              		.loc 1 1789 5 is_stmt 1 view .LVU1299
 3644 00ac 1868     		ldr	r0, [r3]
 3645 00ae 0168     		ldr	r1, [r0]
 3646 00b0 21F40061 		bic	r1, r1, #2048
 3647 00b4 0160     		str	r1, [r0]
 3648              	.LVL190:
1789:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3649              		.loc 1 1789 5 is_stmt 0 view .LVU1300
 3650 00b6 D7E7     		b	.L209
 3651              	.LVL191:
 3652              	.L214:
1815:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3653              		.loc 1 1815 5 is_stmt 1 view .LVU1301
 3654 00b8 1A68     		ldr	r2, [r3]
 3655 00ba 1368     		ldr	r3, [r2]
 3656              	.LVL192:
1815:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3657              		.loc 1 1815 5 is_stmt 0 view .LVU1302
 3658 00bc 43F40073 		orr	r3, r3, #512
 3659 00c0 1360     		str	r3, [r2]
1818:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 3660              		.loc 1 1818 10 view .LVU1303
 3661 00c2 0020     		movs	r0, #0
 3662 00c4 7047     		bx	lr
 3663              	.LVL193:
 3664              	.L210:
1742:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3665              		.loc 1 1742 12 view .LVU1304
 3666 00c6 0220     		movs	r0, #2
 3667 00c8 7047     		bx	lr
 3668              	.L211:
1751:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3669              		.loc 1 1751 3 discriminator 1 view .LVU1305
 3670 00ca 0220     		movs	r0, #2
 3671 00cc 7047     		bx	lr
 3672              	.L216:
 3673 00ce 00BF     		.align	2
 3674              	.L215:
 3675 00d0 00000000 		.word	SPI_RxISR_32BIT
 3676 00d4 00000000 		.word	SPI_RxISR_16BIT
 3677 00d8 00000000 		.word	SPI_RxISR_8BIT
 3678              		.cfi_endproc
 3679              	.LFE343:
 3681              		.section	.text.HAL_SPI_TransmitReceive_IT,"ax",%progbits
 3682              		.align	1
 3683              		.global	HAL_SPI_TransmitReceive_IT
 3684              		.syntax unified
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 155


 3685              		.thumb
 3686              		.thumb_func
 3688              	HAL_SPI_TransmitReceive_IT:
 3689              	.LVL194:
 3690              	.LFB344:
1832:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t tmp_TxXferCount;
 3691              		.loc 1 1832 1 is_stmt 1 view -0
 3692              		.cfi_startproc
 3693              		@ args = 0, pretend = 0, frame = 0
 3694              		@ frame_needed = 0, uses_anonymous_args = 0
1832:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t tmp_TxXferCount;
 3695              		.loc 1 1832 1 is_stmt 0 view .LVU1307
 3696 0000 10B5     		push	{r4, lr}
 3697              		.cfi_def_cfa_offset 8
 3698              		.cfi_offset 4, -8
 3699              		.cfi_offset 14, -4
1833:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 3700              		.loc 1 1833 3 is_stmt 1 view .LVU1308
1835:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
 3701              		.loc 1 1835 3 view .LVU1309
1835:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
 3702              		.loc 1 1835 57 is_stmt 0 view .LVU1310
 3703 0002 0468     		ldr	r4, [r0]
 3704              	.LVL195:
1839:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3705              		.loc 1 1839 3 is_stmt 1 view .LVU1311
1841:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3706              		.loc 1 1841 3 view .LVU1312
1841:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3707              		.loc 1 1841 11 is_stmt 0 view .LVU1313
 3708 0004 90F881E0 		ldrb	lr, [r0, #129]	@ zero_extendqisi2
1841:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3709              		.loc 1 1841 6 view .LVU1314
 3710 0008 BEF1010F 		cmp	lr, #1
 3711 000c 40F0B480 		bne	.L228
 3712 0010 8446     		mov	ip, r0
 3713 0012 5FFA8EF0 		uxtb	r0, lr
 3714              	.LVL196:
1846:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3715              		.loc 1 1846 3 is_stmt 1 view .LVU1315
1846:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3716              		.loc 1 1846 6 is_stmt 0 view .LVU1316
 3717 0016 002A     		cmp	r2, #0
 3718 0018 18BF     		it	ne
 3719 001a 0029     		cmpne	r1, #0
 3720 001c 00F0AD80 		beq	.L218
1846:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3721              		.loc 1 1846 46 discriminator 1 view .LVU1317
 3722 0020 002B     		cmp	r3, #0
 3723 0022 00F0AA80 		beq	.L218
1852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3724              		.loc 1 1852 3 is_stmt 1 view .LVU1318
1852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3725              		.loc 1 1852 3 view .LVU1319
 3726 0026 9CF88000 		ldrb	r0, [ip, #128]	@ zero_extendqisi2
 3727 002a 0128     		cmp	r0, #1
 3728 002c 00F0A680 		beq	.L229
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 156


1852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3729              		.loc 1 1852 3 discriminator 2 view .LVU1320
 3730 0030 0120     		movs	r0, #1
 3731 0032 8CF88000 		strb	r0, [ip, #128]
1852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3732              		.loc 1 1852 3 view .LVU1321
1855:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3733              		.loc 1 1855 3 view .LVU1322
1855:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3734              		.loc 1 1855 21 is_stmt 0 view .LVU1323
 3735 0036 0520     		movs	r0, #5
 3736 0038 8CF88100 		strb	r0, [ip, #129]
1856:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pTxData;
 3737              		.loc 1 1856 3 is_stmt 1 view .LVU1324
1856:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pTxData;
 3738              		.loc 1 1856 21 is_stmt 0 view .LVU1325
 3739 003c 0020     		movs	r0, #0
 3740 003e CCF88400 		str	r0, [ip, #132]
1857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3741              		.loc 1 1857 3 is_stmt 1 view .LVU1326
1857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3742              		.loc 1 1857 21 is_stmt 0 view .LVU1327
 3743 0042 CCF85C10 		str	r1, [ip, #92]
1858:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3744              		.loc 1 1858 3 is_stmt 1 view .LVU1328
1858:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3745              		.loc 1 1858 21 is_stmt 0 view .LVU1329
 3746 0046 ACF86030 		strh	r3, [ip, #96]	@ movhi
1859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 3747              		.loc 1 1859 3 is_stmt 1 view .LVU1330
1859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 3748              		.loc 1 1859 21 is_stmt 0 view .LVU1331
 3749 004a ACF86230 		strh	r3, [ip, #98]	@ movhi
1860:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3750              		.loc 1 1860 3 is_stmt 1 view .LVU1332
1860:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3751              		.loc 1 1860 21 is_stmt 0 view .LVU1333
 3752 004e CCF86420 		str	r2, [ip, #100]
1861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3753              		.loc 1 1861 3 is_stmt 1 view .LVU1334
1861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3754              		.loc 1 1861 21 is_stmt 0 view .LVU1335
 3755 0052 ACF86830 		strh	r3, [ip, #104]	@ movhi
1862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   tmp_TxXferCount   = hspi->TxXferCount;
 3756              		.loc 1 1862 3 is_stmt 1 view .LVU1336
1862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   tmp_TxXferCount   = hspi->TxXferCount;
 3757              		.loc 1 1862 21 is_stmt 0 view .LVU1337
 3758 0056 ACF86A30 		strh	r3, [ip, #106]	@ movhi
1863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3759              		.loc 1 1863 3 is_stmt 1 view .LVU1338
1863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3760              		.loc 1 1863 27 is_stmt 0 view .LVU1339
 3761 005a BCF86220 		ldrh	r2, [ip, #98]
 3762              	.LVL197:
1863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3763              		.loc 1 1863 27 view .LVU1340
 3764 005e 92B2     		uxth	r2, r2
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 157


 3765              	.LVL198:
1874:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3766              		.loc 1 1874 3 is_stmt 1 view .LVU1341
1874:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3767              		.loc 1 1874 17 is_stmt 0 view .LVU1342
 3768 0060 DCF80C10 		ldr	r1, [ip, #12]
 3769              	.LVL199:
1874:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3770              		.loc 1 1874 6 view .LVU1343
 3771 0064 0F29     		cmp	r1, #15
 3772 0066 17D9     		bls	.L219
1876:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR     = SPI_RxISR_32BIT;
 3773              		.loc 1 1876 5 is_stmt 1 view .LVU1344
1876:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR     = SPI_RxISR_32BIT;
 3774              		.loc 1 1876 21 is_stmt 0 view .LVU1345
 3775 0068 4549     		ldr	r1, .L233
 3776 006a CCF87410 		str	r1, [ip, #116]
1877:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3777              		.loc 1 1877 5 is_stmt 1 view .LVU1346
1877:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3778              		.loc 1 1877 21 is_stmt 0 view .LVU1347
 3779 006e 4549     		ldr	r1, .L233+4
 3780 0070 CCF87010 		str	r1, [ip, #112]
 3781              	.L220:
1891:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3782              		.loc 1 1891 3 is_stmt 1 view .LVU1348
 3783 0074 E168     		ldr	r1, [r4, #12]
 3784 0076 21F4C021 		bic	r1, r1, #393216
 3785 007a E160     		str	r1, [r4, #12]
 3786              	.LVL200:
1894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3787              		.loc 1 1894 3 view .LVU1349
 3788 007c DCF80000 		ldr	r0, [ip]
 3789 0080 4168     		ldr	r1, [r0, #4]
 3790 0082 6FF30F01 		bfc	r1, #0, #16
 3791 0086 0B43     		orrs	r3, r3, r1
 3792              	.LVL201:
1894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3793              		.loc 1 1894 3 is_stmt 0 view .LVU1350
 3794 0088 4360     		str	r3, [r0, #4]
1897:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3795              		.loc 1 1897 3 is_stmt 1 view .LVU1351
 3796 008a DCF80010 		ldr	r1, [ip]
 3797 008e 0B68     		ldr	r3, [r1]
 3798 0090 43F00103 		orr	r3, r3, #1
 3799 0094 0B60     		str	r3, [r1]
1900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3800              		.loc 1 1900 3 view .LVU1352
1900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3801              		.loc 1 1900 9 is_stmt 0 view .LVU1353
 3802 0096 24E0     		b	.L222
 3803              	.LVL202:
 3804              	.L219:
1879:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3805              		.loc 1 1879 8 is_stmt 1 view .LVU1354
1879:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3806              		.loc 1 1879 11 is_stmt 0 view .LVU1355
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 158


 3807 0098 0729     		cmp	r1, #7
 3808 009a 06D9     		bls	.L221
1881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxISR     = SPI_TxISR_16BIT;
 3809              		.loc 1 1881 5 is_stmt 1 view .LVU1356
1881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxISR     = SPI_TxISR_16BIT;
 3810              		.loc 1 1881 21 is_stmt 0 view .LVU1357
 3811 009c 3A49     		ldr	r1, .L233+8
 3812 009e CCF87010 		str	r1, [ip, #112]
1882:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3813              		.loc 1 1882 5 is_stmt 1 view .LVU1358
1882:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3814              		.loc 1 1882 21 is_stmt 0 view .LVU1359
 3815 00a2 3A49     		ldr	r1, .L233+12
 3816 00a4 CCF87410 		str	r1, [ip, #116]
 3817 00a8 E4E7     		b	.L220
 3818              	.L221:
1886:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxISR     = SPI_TxISR_8BIT;
 3819              		.loc 1 1886 5 is_stmt 1 view .LVU1360
1886:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->TxISR     = SPI_TxISR_8BIT;
 3820              		.loc 1 1886 21 is_stmt 0 view .LVU1361
 3821 00aa 3949     		ldr	r1, .L233+16
 3822 00ac CCF87010 		str	r1, [ip, #112]
1887:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3823              		.loc 1 1887 5 is_stmt 1 view .LVU1362
1887:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3824              		.loc 1 1887 21 is_stmt 0 view .LVU1363
 3825 00b0 3849     		ldr	r1, .L233+20
 3826 00b2 CCF87410 		str	r1, [ip, #116]
 3827 00b6 DDE7     		b	.L220
 3828              	.LVL203:
 3829              	.L223:
1911:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 3830              		.loc 1 1911 10 is_stmt 1 view .LVU1364
1911:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 3831              		.loc 1 1911 13 is_stmt 0 view .LVU1365
 3832 00b8 072A     		cmp	r2, #7
 3833 00ba 31D9     		bls	.L225
1914:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 3834              		.loc 1 1914 7 is_stmt 1 view .LVU1366
1914:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 3835              		.loc 1 1914 47 is_stmt 0 view .LVU1367
 3836 00bc DCF85C30 		ldr	r3, [ip, #92]
1914:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 3837              		.loc 1 1914 23 view .LVU1368
 3838 00c0 1B88     		ldrh	r3, [r3]
1914:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 3839              		.loc 1 1914 21 view .LVU1369
 3840 00c2 2384     		strh	r3, [r4, #32]	@ movhi
1918:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount--;
 3841              		.loc 1 1918 7 is_stmt 1 view .LVU1370
1918:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount--;
 3842              		.loc 1 1918 11 is_stmt 0 view .LVU1371
 3843 00c4 DCF85C30 		ldr	r3, [ip, #92]
1918:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount--;
 3844              		.loc 1 1918 24 view .LVU1372
 3845 00c8 0233     		adds	r3, r3, #2
 3846 00ca CCF85C30 		str	r3, [ip, #92]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 159


1919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       tmp_TxXferCount = hspi->TxXferCount;
 3847              		.loc 1 1919 7 is_stmt 1 view .LVU1373
1919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       tmp_TxXferCount = hspi->TxXferCount;
 3848              		.loc 1 1919 11 is_stmt 0 view .LVU1374
 3849 00ce BCF86230 		ldrh	r3, [ip, #98]
 3850 00d2 9BB2     		uxth	r3, r3
1919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       tmp_TxXferCount = hspi->TxXferCount;
 3851              		.loc 1 1919 24 view .LVU1375
 3852 00d4 013B     		subs	r3, r3, #1
 3853 00d6 9BB2     		uxth	r3, r3
 3854 00d8 ACF86230 		strh	r3, [ip, #98]	@ movhi
1920:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 3855              		.loc 1 1920 7 is_stmt 1 view .LVU1376
1920:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 3856              		.loc 1 1920 29 is_stmt 0 view .LVU1377
 3857 00dc BCF86220 		ldrh	r2, [ip, #98]
 3858 00e0 92B2     		uxth	r2, r2
 3859              	.LVL204:
 3860              	.L222:
1900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3861              		.loc 1 1900 51 is_stmt 1 view .LVU1378
1900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3862              		.loc 1 1900 11 is_stmt 0 view .LVU1379
 3863 00e2 DCF80030 		ldr	r3, [ip]
 3864 00e6 5969     		ldr	r1, [r3, #20]
1900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3865              		.loc 1 1900 51 view .LVU1380
 3866 00e8 11F0020F 		tst	r1, #2
 3867 00ec 2DD0     		beq	.L226
1900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3868              		.loc 1 1900 51 discriminator 1 view .LVU1381
 3869 00ee 62B3     		cbz	r2, .L226
1903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 3870              		.loc 1 1903 5 is_stmt 1 view .LVU1382
1903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 3871              		.loc 1 1903 19 is_stmt 0 view .LVU1383
 3872 00f0 DCF80C20 		ldr	r2, [ip, #12]
 3873              	.LVL205:
1903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 3874              		.loc 1 1903 8 view .LVU1384
 3875 00f4 0F2A     		cmp	r2, #15
 3876 00f6 DFD9     		bls	.L223
1905:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint32_t);
 3877              		.loc 1 1905 7 is_stmt 1 view .LVU1385
1905:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint32_t);
 3878              		.loc 1 1905 75 is_stmt 0 view .LVU1386
 3879 00f8 DCF85C20 		ldr	r2, [ip, #92]
1905:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint32_t);
 3880              		.loc 1 1905 51 view .LVU1387
 3881 00fc 1268     		ldr	r2, [r2]
1905:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint32_t);
 3882              		.loc 1 1905 49 view .LVU1388
 3883 00fe 1A62     		str	r2, [r3, #32]
1906:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount--;
 3884              		.loc 1 1906 7 is_stmt 1 view .LVU1389
1906:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount--;
 3885              		.loc 1 1906 11 is_stmt 0 view .LVU1390
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 160


 3886 0100 DCF85C30 		ldr	r3, [ip, #92]
1906:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount--;
 3887              		.loc 1 1906 24 view .LVU1391
 3888 0104 0433     		adds	r3, r3, #4
 3889 0106 CCF85C30 		str	r3, [ip, #92]
1907:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       tmp_TxXferCount = hspi->TxXferCount;
 3890              		.loc 1 1907 7 is_stmt 1 view .LVU1392
1907:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       tmp_TxXferCount = hspi->TxXferCount;
 3891              		.loc 1 1907 11 is_stmt 0 view .LVU1393
 3892 010a BCF86230 		ldrh	r3, [ip, #98]
 3893 010e 9BB2     		uxth	r3, r3
1907:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       tmp_TxXferCount = hspi->TxXferCount;
 3894              		.loc 1 1907 24 view .LVU1394
 3895 0110 013B     		subs	r3, r3, #1
 3896 0112 9BB2     		uxth	r3, r3
 3897 0114 ACF86230 		strh	r3, [ip, #98]	@ movhi
1908:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 3898              		.loc 1 1908 7 is_stmt 1 view .LVU1395
1908:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 3899              		.loc 1 1908 29 is_stmt 0 view .LVU1396
 3900 0118 BCF86220 		ldrh	r2, [ip, #98]
 3901 011c 92B2     		uxth	r2, r2
 3902              	.LVL206:
1908:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 3903              		.loc 1 1908 29 view .LVU1397
 3904 011e E0E7     		b	.L222
 3905              	.LVL207:
 3906              	.L225:
1925:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint8_t);
 3907              		.loc 1 1925 7 is_stmt 1 view .LVU1398
1925:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint8_t);
 3908              		.loc 1 1925 73 is_stmt 0 view .LVU1399
 3909 0120 DCF85C20 		ldr	r2, [ip, #92]
1925:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint8_t);
 3910              		.loc 1 1925 50 view .LVU1400
 3911 0124 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
1925:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint8_t);
 3912              		.loc 1 1925 48 view .LVU1401
 3913 0126 83F82020 		strb	r2, [r3, #32]
1926:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount--;
 3914              		.loc 1 1926 7 is_stmt 1 view .LVU1402
1926:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount--;
 3915              		.loc 1 1926 11 is_stmt 0 view .LVU1403
 3916 012a DCF85C30 		ldr	r3, [ip, #92]
1926:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       hspi->TxXferCount--;
 3917              		.loc 1 1926 24 view .LVU1404
 3918 012e 0133     		adds	r3, r3, #1
 3919 0130 CCF85C30 		str	r3, [ip, #92]
1927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       tmp_TxXferCount = hspi->TxXferCount;
 3920              		.loc 1 1927 7 is_stmt 1 view .LVU1405
1927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       tmp_TxXferCount = hspi->TxXferCount;
 3921              		.loc 1 1927 11 is_stmt 0 view .LVU1406
 3922 0134 BCF86230 		ldrh	r3, [ip, #98]
 3923 0138 9BB2     		uxth	r3, r3
1927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       tmp_TxXferCount = hspi->TxXferCount;
 3924              		.loc 1 1927 24 view .LVU1407
 3925 013a 013B     		subs	r3, r3, #1
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 161


 3926 013c 9BB2     		uxth	r3, r3
 3927 013e ACF86230 		strh	r3, [ip, #98]	@ movhi
1928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 3928              		.loc 1 1928 7 is_stmt 1 view .LVU1408
1928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 3929              		.loc 1 1928 29 is_stmt 0 view .LVU1409
 3930 0142 BCF86220 		ldrh	r2, [ip, #98]
 3931 0146 92B2     		uxth	r2, r2
 3932 0148 CBE7     		b	.L222
 3933              	.LVL208:
 3934              	.L226:
1933:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3935              		.loc 1 1933 3 is_stmt 1 view .LVU1410
1933:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3936              		.loc 1 1933 3 view .LVU1411
 3937 014a 0022     		movs	r2, #0
 3938              	.LVL209:
1933:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3939              		.loc 1 1933 3 is_stmt 0 view .LVU1412
 3940 014c 8CF88020 		strb	r2, [ip, #128]
1933:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3941              		.loc 1 1933 3 is_stmt 1 view .LVU1413
1936:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                              SPI_IT_FRE | SPI_IT_MODF | SPI_IT_TSERF));
 3942              		.loc 1 1936 3 view .LVU1414
 3943 0150 1969     		ldr	r1, [r3, #16]
 3944 0152 40F26C72 		movw	r2, #1900
 3945 0156 0A43     		orrs	r2, r2, r1
 3946 0158 1A61     		str	r2, [r3, #16]
1939:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3947              		.loc 1 1939 3 view .LVU1415
1939:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3948              		.loc 1 1939 17 is_stmt 0 view .LVU1416
 3949 015a DCF80430 		ldr	r3, [ip, #4]
1939:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 3950              		.loc 1 1939 6 view .LVU1417
 3951 015e B3F5800F 		cmp	r3, #4194304
 3952 0162 01D0     		beq	.L232
1945:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 3953              		.loc 1 1945 10 view .LVU1418
 3954 0164 0020     		movs	r0, #0
 3955 0166 08E0     		b	.L218
 3956              	.L232:
1942:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3957              		.loc 1 1942 5 is_stmt 1 view .LVU1419
 3958 0168 DCF80020 		ldr	r2, [ip]
 3959 016c 1368     		ldr	r3, [r2]
 3960 016e 43F40073 		orr	r3, r3, #512
 3961 0172 1360     		str	r3, [r2]
1945:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 3962              		.loc 1 1945 10 is_stmt 0 view .LVU1420
 3963 0174 0020     		movs	r0, #0
 3964 0176 00E0     		b	.L218
 3965              	.LVL210:
 3966              	.L228:
1843:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 3967              		.loc 1 1843 12 view .LVU1421
 3968 0178 0220     		movs	r0, #2
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 162


 3969              	.LVL211:
 3970              	.L218:
1946:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3971              		.loc 1 1946 1 view .LVU1422
 3972 017a 10BD     		pop	{r4, pc}
 3973              	.LVL212:
 3974              	.L229:
1852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 3975              		.loc 1 1852 3 discriminator 1 view .LVU1423
 3976 017c 0220     		movs	r0, #2
 3977 017e FCE7     		b	.L218
 3978              	.L234:
 3979              		.align	2
 3980              	.L233:
 3981 0180 00000000 		.word	SPI_TxISR_32BIT
 3982 0184 00000000 		.word	SPI_RxISR_32BIT
 3983 0188 00000000 		.word	SPI_RxISR_16BIT
 3984 018c 00000000 		.word	SPI_TxISR_16BIT
 3985 0190 00000000 		.word	SPI_RxISR_8BIT
 3986 0194 00000000 		.word	SPI_TxISR_8BIT
 3987              		.cfi_endproc
 3988              	.LFE344:
 3990              		.section	.text.HAL_SPI_Transmit_DMA,"ax",%progbits
 3991              		.align	1
 3992              		.global	HAL_SPI_Transmit_DMA
 3993              		.syntax unified
 3994              		.thumb
 3995              		.thumb_func
 3997              	HAL_SPI_Transmit_DMA:
 3998              	.LVL213:
 3999              	.LFB345:
2087:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4000              		.loc 1 2087 1 is_stmt 1 view -0
 4001              		.cfi_startproc
 4002              		@ args = 0, pretend = 0, frame = 0
 4003              		@ frame_needed = 0, uses_anonymous_args = 0
2087:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4004              		.loc 1 2087 1 is_stmt 0 view .LVU1425
 4005 0000 70B5     		push	{r4, r5, r6, lr}
 4006              		.cfi_def_cfa_offset 16
 4007              		.cfi_offset 4, -16
 4008              		.cfi_offset 5, -12
 4009              		.cfi_offset 6, -8
 4010              		.cfi_offset 14, -4
2090:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4011              		.loc 1 2090 3 is_stmt 1 view .LVU1426
2092:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4012              		.loc 1 2092 3 view .LVU1427
2092:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4013              		.loc 1 2092 11 is_stmt 0 view .LVU1428
 4014 0002 90F88130 		ldrb	r3, [r0, #129]	@ zero_extendqisi2
2092:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4015              		.loc 1 2092 6 view .LVU1429
 4016 0006 012B     		cmp	r3, #1
 4017 0008 40F0CC80 		bne	.L249
 4018 000c 0446     		mov	r4, r0
 4019 000e 1546     		mov	r5, r2
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 163


 4020 0010 DEB2     		uxtb	r6, r3
2097:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4021              		.loc 1 2097 3 is_stmt 1 view .LVU1430
2097:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4022              		.loc 1 2097 6 is_stmt 0 view .LVU1431
 4023 0012 002A     		cmp	r2, #0
 4024 0014 18BF     		it	ne
 4025 0016 0029     		cmpne	r1, #0
 4026 0018 00F0C580 		beq	.L236
2103:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4027              		.loc 1 2103 3 is_stmt 1 view .LVU1432
2103:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4028              		.loc 1 2103 3 view .LVU1433
 4029 001c 90F88030 		ldrb	r3, [r0, #128]	@ zero_extendqisi2
 4030 0020 012B     		cmp	r3, #1
 4031 0022 00F0C280 		beq	.L250
2103:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4032              		.loc 1 2103 3 discriminator 2 view .LVU1434
 4033 0026 0123     		movs	r3, #1
 4034 0028 80F88030 		strb	r3, [r0, #128]
2103:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4035              		.loc 1 2103 3 view .LVU1435
2106:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 4036              		.loc 1 2106 3 view .LVU1436
2106:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 4037              		.loc 1 2106 21 is_stmt 0 view .LVU1437
 4038 002c 0323     		movs	r3, #3
 4039 002e 80F88130 		strb	r3, [r0, #129]
2107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pData;
 4040              		.loc 1 2107 3 is_stmt 1 view .LVU1438
2107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pData;
 4041              		.loc 1 2107 21 is_stmt 0 view .LVU1439
 4042 0032 0023     		movs	r3, #0
 4043 0034 C0F88430 		str	r3, [r0, #132]
2108:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 4044              		.loc 1 2108 3 is_stmt 1 view .LVU1440
2108:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 4045              		.loc 1 2108 21 is_stmt 0 view .LVU1441
 4046 0038 C165     		str	r1, [r0, #92]
2109:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 4047              		.loc 1 2109 3 is_stmt 1 view .LVU1442
2109:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 4048              		.loc 1 2109 21 is_stmt 0 view .LVU1443
 4049 003a A0F86020 		strh	r2, [r0, #96]	@ movhi
2110:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4050              		.loc 1 2110 3 is_stmt 1 view .LVU1444
2110:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4051              		.loc 1 2110 21 is_stmt 0 view .LVU1445
 4052 003e A0F86220 		strh	r2, [r0, #98]	@ movhi
2113:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 4053              		.loc 1 2113 3 is_stmt 1 view .LVU1446
2113:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 4054              		.loc 1 2113 21 is_stmt 0 view .LVU1447
 4055 0042 4366     		str	r3, [r0, #100]
2114:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
 4056              		.loc 1 2114 3 is_stmt 1 view .LVU1448
2114:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxISR       = NULL;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 164


 4057              		.loc 1 2114 21 is_stmt 0 view .LVU1449
 4058 0044 4367     		str	r3, [r0, #116]
2115:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = (uint16_t)0UL;
 4059              		.loc 1 2115 3 is_stmt 1 view .LVU1450
2115:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = (uint16_t)0UL;
 4060              		.loc 1 2115 21 is_stmt 0 view .LVU1451
 4061 0046 0367     		str	r3, [r0, #112]
2116:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t)0UL;
 4062              		.loc 1 2116 3 is_stmt 1 view .LVU1452
2116:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t)0UL;
 4063              		.loc 1 2116 21 is_stmt 0 view .LVU1453
 4064 0048 A0F86830 		strh	r3, [r0, #104]	@ movhi
2117:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4065              		.loc 1 2117 3 is_stmt 1 view .LVU1454
2117:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4066              		.loc 1 2117 21 is_stmt 0 view .LVU1455
 4067 004c A0F86A30 		strh	r3, [r0, #106]	@ movhi
2120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4068              		.loc 1 2120 3 is_stmt 1 view .LVU1456
2120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4069              		.loc 1 2120 17 is_stmt 0 view .LVU1457
 4070 0050 8368     		ldr	r3, [r0, #8]
2120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4071              		.loc 1 2120 6 view .LVU1458
 4072 0052 B3F5C02F 		cmp	r3, #393216
 4073 0056 63D0     		beq	.L252
2126:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4074              		.loc 1 2126 5 is_stmt 1 view .LVU1459
 4075 0058 0268     		ldr	r2, [r0]
 4076              	.LVL214:
2126:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4077              		.loc 1 2126 5 is_stmt 0 view .LVU1460
 4078 005a D368     		ldr	r3, [r2, #12]
 4079 005c 23F4C023 		bic	r3, r3, #393216
 4080 0060 43F40033 		orr	r3, r3, #131072
 4081 0064 D360     		str	r3, [r2, #12]
 4082              	.LVL215:
 4083              	.L238:
2130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmatx->Init.MemDataAlignment != DMA_MD
 4084              		.loc 1 2130 3 is_stmt 1 view .LVU1461
2130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmatx->Init.MemDataAlignment != DMA_MD
 4085              		.loc 1 2130 19 is_stmt 0 view .LVU1462
 4086 0066 E368     		ldr	r3, [r4, #12]
2130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmatx->Init.MemDataAlignment != DMA_MD
 4087              		.loc 1 2130 6 view .LVU1463
 4088 0068 0F2B     		cmp	r3, #15
 4089 006a 04D9     		bls	.L239
2130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmatx->Init.MemDataAlignment != DMA_MD
 4090              		.loc 1 2130 59 discriminator 1 view .LVU1464
 4091 006c A26F     		ldr	r2, [r4, #120]
2130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmatx->Init.MemDataAlignment != DMA_MD
 4092              		.loc 1 2130 73 discriminator 1 view .LVU1465
 4093 006e 9269     		ldr	r2, [r2, #24]
2130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmatx->Init.MemDataAlignment != DMA_MD
 4094              		.loc 1 2130 51 discriminator 1 view .LVU1466
 4095 0070 B2F5804F 		cmp	r2, #16384
 4096 0074 5AD1     		bne	.L240
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 165


 4097              	.L239:
2130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmatx->Init.MemDataAlignment != DMA_MD
 4098              		.loc 1 2130 119 discriminator 3 view .LVU1467
 4099 0076 072B     		cmp	r3, #7
 4100 0078 07D9     		bls	.L241
2131:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                      (hspi->hdmatx->Init.MemDataAlignment != DMA_MD
 4101              		.loc 1 2131 59 view .LVU1468
 4102 007a A26F     		ldr	r2, [r4, #120]
2131:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                      (hspi->hdmatx->Init.MemDataAlignment != DMA_MD
 4103              		.loc 1 2131 73 view .LVU1469
 4104 007c 9269     		ldr	r2, [r2, #24]
2131:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                      (hspi->hdmatx->Init.MemDataAlignment != DMA_MD
 4105              		.loc 1 2131 50 view .LVU1470
 4106 007e B2F5005F 		cmp	r2, #8192
 4107 0082 18BF     		it	ne
 4108 0084 B2F5804F 		cmpne	r2, #16384
 4109 0088 50D1     		bne	.L240
 4110              	.L241:
2140:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4111              		.loc 1 2140 3 is_stmt 1 view .LVU1471
2140:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4112              		.loc 1 2140 6 is_stmt 0 view .LVU1472
 4113 008a 072B     		cmp	r3, #7
 4114 008c 62D8     		bhi	.L242
2142:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4115              		.loc 1 2142 5 is_stmt 1 view .LVU1473
2142:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4116              		.loc 1 2142 13 is_stmt 0 view .LVU1474
 4117 008e A36F     		ldr	r3, [r4, #120]
2142:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4118              		.loc 1 2142 27 view .LVU1475
 4119 0090 9A69     		ldr	r2, [r3, #24]
2142:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4120              		.loc 1 2142 8 view .LVU1476
 4121 0092 B2F5005F 		cmp	r2, #8192
 4122 0096 4DD0     		beq	.L253
 4123              	.L243:
2146:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4124              		.loc 1 2146 5 is_stmt 1 view .LVU1477
2146:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4125              		.loc 1 2146 27 is_stmt 0 view .LVU1478
 4126 0098 9B69     		ldr	r3, [r3, #24]
2146:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4127              		.loc 1 2146 8 view .LVU1479
 4128 009a B3F5804F 		cmp	r3, #16384
 4129 009e 51D0     		beq	.L254
 4130              	.L244:
2161:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4131              		.loc 1 2161 3 is_stmt 1 view .LVU1480
2164:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4132              		.loc 1 2164 3 view .LVU1481
2164:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4133              		.loc 1 2164 7 is_stmt 0 view .LVU1482
 4134 00a0 A36F     		ldr	r3, [r4, #120]
2164:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4135              		.loc 1 2164 38 view .LVU1483
 4136 00a2 434A     		ldr	r2, .L258
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 166


 4137 00a4 1A64     		str	r2, [r3, #64]
2167:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4138              		.loc 1 2167 3 is_stmt 1 view .LVU1484
2167:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4139              		.loc 1 2167 7 is_stmt 0 view .LVU1485
 4140 00a6 A36F     		ldr	r3, [r4, #120]
2167:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4141              		.loc 1 2167 34 view .LVU1486
 4142 00a8 424A     		ldr	r2, .L258+4
 4143 00aa DA63     		str	r2, [r3, #60]
2170:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4144              		.loc 1 2170 3 is_stmt 1 view .LVU1487
2170:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4145              		.loc 1 2170 7 is_stmt 0 view .LVU1488
 4146 00ac A36F     		ldr	r3, [r4, #120]
2170:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4147              		.loc 1 2170 35 view .LVU1489
 4148 00ae 424A     		ldr	r2, .L258+8
 4149 00b0 DA64     		str	r2, [r3, #76]
2173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4150              		.loc 1 2173 3 is_stmt 1 view .LVU1490
2173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4151              		.loc 1 2173 7 is_stmt 0 view .LVU1491
 4152 00b2 A36F     		ldr	r3, [r4, #120]
2173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4153              		.loc 1 2173 35 view .LVU1492
 4154 00b4 0022     		movs	r2, #0
 4155 00b6 1A65     		str	r2, [r3, #80]
2176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4156              		.loc 1 2176 3 is_stmt 1 view .LVU1493
 4157 00b8 2268     		ldr	r2, [r4]
 4158 00ba 9368     		ldr	r3, [r2, #8]
 4159 00bc 23F40043 		bic	r3, r3, #32768
 4160 00c0 9360     		str	r3, [r2, #8]
2179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->TxXferCount))
 4161              		.loc 1 2179 3 view .LVU1494
2179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->TxXferCount))
 4162              		.loc 1 2179 91 is_stmt 0 view .LVU1495
 4163 00c2 2268     		ldr	r2, [r4]
2180:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4164              		.loc 1 2180 38 view .LVU1496
 4165 00c4 B4F86230 		ldrh	r3, [r4, #98]
2179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->TxXferCount))
 4166              		.loc 1 2179 17 view .LVU1497
 4167 00c8 9BB2     		uxth	r3, r3
 4168 00ca 2032     		adds	r2, r2, #32
 4169 00cc E16D     		ldr	r1, [r4, #92]
 4170              	.LVL216:
2179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->TxXferCount))
 4171              		.loc 1 2179 17 view .LVU1498
 4172 00ce A06F     		ldr	r0, [r4, #120]
 4173              	.LVL217:
2179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->TxXferCount))
 4174              		.loc 1 2179 17 view .LVU1499
 4175 00d0 FFF7FEFF 		bl	HAL_DMA_Start_IT
 4176              	.LVL218:
2179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->TxXferCount))
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 167


 4177              		.loc 1 2179 6 discriminator 1 view .LVU1500
 4178 00d4 0146     		mov	r1, r0
 4179 00d6 0028     		cmp	r0, #0
 4180 00d8 4BD1     		bne	.L255
2193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4181              		.loc 1 2193 3 is_stmt 1 view .LVU1501
2193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4182              		.loc 1 2193 11 is_stmt 0 view .LVU1502
 4183 00da A36F     		ldr	r3, [r4, #120]
2193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4184              		.loc 1 2193 25 view .LVU1503
 4185 00dc DB69     		ldr	r3, [r3, #28]
2193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4186              		.loc 1 2193 6 view .LVU1504
 4187 00de B3F5807F 		cmp	r3, #256
 4188 00e2 53D0     		beq	.L256
2199:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4189              		.loc 1 2199 5 is_stmt 1 view .LVU1505
 4190 00e4 2268     		ldr	r2, [r4]
 4191 00e6 5368     		ldr	r3, [r2, #4]
 4192 00e8 6FF30F03 		bfc	r3, #0, #16
 4193 00ec 1D43     		orrs	r5, r5, r3
 4194              	.LVL219:
2199:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4195              		.loc 1 2199 5 is_stmt 0 view .LVU1506
 4196 00ee 5560     		str	r5, [r2, #4]
 4197              	.L247:
2203:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4198              		.loc 1 2203 3 is_stmt 1 view .LVU1507
 4199 00f0 2268     		ldr	r2, [r4]
 4200 00f2 9368     		ldr	r3, [r2, #8]
 4201 00f4 43F40043 		orr	r3, r3, #32768
 4202 00f8 9360     		str	r3, [r2, #8]
2206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4203              		.loc 1 2206 3 view .LVU1508
 4204 00fa 2268     		ldr	r2, [r4]
 4205 00fc 1369     		ldr	r3, [r2, #16]
 4206 00fe 43F44873 		orr	r3, r3, #800
 4207 0102 1361     		str	r3, [r2, #16]
2209:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4208              		.loc 1 2209 3 view .LVU1509
 4209 0104 2268     		ldr	r2, [r4]
 4210 0106 1368     		ldr	r3, [r2]
 4211 0108 43F00103 		orr	r3, r3, #1
 4212 010c 1360     		str	r3, [r2]
2211:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4213              		.loc 1 2211 3 view .LVU1510
2211:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4214              		.loc 1 2211 17 is_stmt 0 view .LVU1511
 4215 010e 6368     		ldr	r3, [r4, #4]
2211:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4216              		.loc 1 2211 6 view .LVU1512
 4217 0110 B3F5800F 		cmp	r3, #4194304
 4218 0114 40D0     		beq	.L257
 4219              	.L248:
2218:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4220              		.loc 1 2218 3 is_stmt 1 view .LVU1513
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 168


2218:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4221              		.loc 1 2218 3 view .LVU1514
 4222 0116 0023     		movs	r3, #0
 4223 0118 84F88030 		strb	r3, [r4, #128]
2218:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4224              		.loc 1 2218 3 view .LVU1515
2220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 4225              		.loc 1 2220 3 view .LVU1516
2220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 4226              		.loc 1 2220 10 is_stmt 0 view .LVU1517
 4227 011c 0E46     		mov	r6, r1
 4228 011e 42E0     		b	.L236
 4229              	.LVL220:
 4230              	.L252:
2122:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4231              		.loc 1 2122 5 is_stmt 1 view .LVU1518
 4232 0120 0268     		ldr	r2, [r0]
 4233              	.LVL221:
2122:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4234              		.loc 1 2122 5 is_stmt 0 view .LVU1519
 4235 0122 1368     		ldr	r3, [r2]
 4236 0124 43F40063 		orr	r3, r3, #2048
 4237 0128 1360     		str	r3, [r2]
 4238              	.LVL222:
2122:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4239              		.loc 1 2122 5 view .LVU1520
 4240 012a 9CE7     		b	.L238
 4241              	.L240:
2135:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 4242              		.loc 1 2135 5 is_stmt 1 view .LVU1521
2135:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 4243              		.loc 1 2135 5 view .LVU1522
 4244 012c 0023     		movs	r3, #0
 4245 012e 84F88030 		strb	r3, [r4, #128]
2135:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 4246              		.loc 1 2135 5 view .LVU1523
2136:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4247              		.loc 1 2136 5 view .LVU1524
2136:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4248              		.loc 1 2136 12 is_stmt 0 view .LVU1525
 4249 0132 38E0     		b	.L236
 4250              	.L253:
2144:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4251              		.loc 1 2144 7 is_stmt 1 view .LVU1526
2144:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4252              		.loc 1 2144 32 is_stmt 0 view .LVU1527
 4253 0134 B4F86220 		ldrh	r2, [r4, #98]
 4254 0138 92B2     		uxth	r2, r2
2144:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4255              		.loc 1 2144 46 view .LVU1528
 4256 013a 0132     		adds	r2, r2, #1
2144:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4257              		.loc 1 2144 25 view .LVU1529
 4258 013c 5208     		lsrs	r2, r2, #1
 4259 013e A4F86220 		strh	r2, [r4, #98]	@ movhi
 4260 0142 A9E7     		b	.L243
 4261              	.L254:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 169


2148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4262              		.loc 1 2148 7 is_stmt 1 view .LVU1530
2148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4263              		.loc 1 2148 32 is_stmt 0 view .LVU1531
 4264 0144 B4F86230 		ldrh	r3, [r4, #98]
 4265 0148 9BB2     		uxth	r3, r3
2148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4266              		.loc 1 2148 46 view .LVU1532
 4267 014a 0333     		adds	r3, r3, #3
2148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4268              		.loc 1 2148 25 view .LVU1533
 4269 014c 9B08     		lsrs	r3, r3, #2
 4270 014e A4F86230 		strh	r3, [r4, #98]	@ movhi
 4271 0152 A5E7     		b	.L244
 4272              	.L242:
2151:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4273              		.loc 1 2151 8 is_stmt 1 view .LVU1534
2151:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4274              		.loc 1 2151 11 is_stmt 0 view .LVU1535
 4275 0154 0F2B     		cmp	r3, #15
 4276 0156 A3D8     		bhi	.L244
2153:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4277              		.loc 1 2153 5 is_stmt 1 view .LVU1536
2153:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4278              		.loc 1 2153 13 is_stmt 0 view .LVU1537
 4279 0158 A36F     		ldr	r3, [r4, #120]
2153:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4280              		.loc 1 2153 27 view .LVU1538
 4281 015a 9B69     		ldr	r3, [r3, #24]
2153:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4282              		.loc 1 2153 8 view .LVU1539
 4283 015c B3F5804F 		cmp	r3, #16384
 4284 0160 9ED1     		bne	.L244
2155:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4285              		.loc 1 2155 7 is_stmt 1 view .LVU1540
2155:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4286              		.loc 1 2155 32 is_stmt 0 view .LVU1541
 4287 0162 B4F86230 		ldrh	r3, [r4, #98]
 4288 0166 9BB2     		uxth	r3, r3
2155:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4289              		.loc 1 2155 46 view .LVU1542
 4290 0168 0133     		adds	r3, r3, #1
2155:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4291              		.loc 1 2155 25 view .LVU1543
 4292 016a 5B08     		lsrs	r3, r3, #1
 4293 016c A4F86230 		strh	r3, [r4, #98]	@ movhi
 4294 0170 96E7     		b	.L244
 4295              	.LVL223:
 4296              	.L255:
2183:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 4297              		.loc 1 2183 5 is_stmt 1 view .LVU1544
 4298 0172 D4F88430 		ldr	r3, [r4, #132]
 4299 0176 43F01003 		orr	r3, r3, #16
 4300 017a C4F88430 		str	r3, [r4, #132]
2184:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4301              		.loc 1 2184 5 view .LVU1545
2184:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 170


 4302              		.loc 1 2184 17 is_stmt 0 view .LVU1546
 4303 017e 0123     		movs	r3, #1
 4304 0180 84F88130 		strb	r3, [r4, #129]
2187:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4305              		.loc 1 2187 5 is_stmt 1 view .LVU1547
2187:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4306              		.loc 1 2187 5 view .LVU1548
 4307 0184 0023     		movs	r3, #0
 4308 0186 84F88030 		strb	r3, [r4, #128]
2187:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4309              		.loc 1 2187 5 view .LVU1549
2189:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4310              		.loc 1 2189 5 view .LVU1550
2189:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4311              		.loc 1 2189 12 is_stmt 0 view .LVU1551
 4312 018a 0CE0     		b	.L236
 4313              	.L256:
2195:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4314              		.loc 1 2195 5 is_stmt 1 view .LVU1552
 4315 018c 2268     		ldr	r2, [r4]
 4316 018e 5368     		ldr	r3, [r2, #4]
 4317 0190 6FF30F03 		bfc	r3, #0, #16
 4318 0194 5360     		str	r3, [r2, #4]
 4319 0196 ABE7     		b	.L247
 4320              	.LVL224:
 4321              	.L257:
2214:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4322              		.loc 1 2214 5 view .LVU1553
 4323 0198 2268     		ldr	r2, [r4]
 4324 019a 1368     		ldr	r3, [r2]
 4325 019c 43F40073 		orr	r3, r3, #512
 4326 01a0 1360     		str	r3, [r2]
 4327 01a2 B8E7     		b	.L248
 4328              	.LVL225:
 4329              	.L249:
2094:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4330              		.loc 1 2094 12 is_stmt 0 view .LVU1554
 4331 01a4 0226     		movs	r6, #2
 4332              	.LVL226:
 4333              	.L236:
2221:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4334              		.loc 1 2221 1 view .LVU1555
 4335 01a6 3046     		mov	r0, r6
 4336 01a8 70BD     		pop	{r4, r5, r6, pc}
 4337              	.LVL227:
 4338              	.L250:
2103:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4339              		.loc 1 2103 3 discriminator 1 view .LVU1556
 4340 01aa 0226     		movs	r6, #2
 4341 01ac FBE7     		b	.L236
 4342              	.L259:
 4343 01ae 00BF     		.align	2
 4344              	.L258:
 4345 01b0 00000000 		.word	SPI_DMAHalfTransmitCplt
 4346 01b4 00000000 		.word	SPI_DMATransmitCplt
 4347 01b8 00000000 		.word	SPI_DMAError
 4348              		.cfi_endproc
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 171


 4349              	.LFE345:
 4351              		.section	.text.HAL_SPI_Receive_DMA,"ax",%progbits
 4352              		.align	1
 4353              		.global	HAL_SPI_Receive_DMA
 4354              		.syntax unified
 4355              		.thumb
 4356              		.thumb_func
 4358              	HAL_SPI_Receive_DMA:
 4359              	.LVL228:
 4360              	.LFB346:
2233:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4361              		.loc 1 2233 1 is_stmt 1 view -0
 4362              		.cfi_startproc
 4363              		@ args = 0, pretend = 0, frame = 0
 4364              		@ frame_needed = 0, uses_anonymous_args = 0
2233:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4365              		.loc 1 2233 1 is_stmt 0 view .LVU1558
 4366 0000 70B5     		push	{r4, r5, r6, lr}
 4367              		.cfi_def_cfa_offset 16
 4368              		.cfi_offset 4, -16
 4369              		.cfi_offset 5, -12
 4370              		.cfi_offset 6, -8
 4371              		.cfi_offset 14, -4
 4372 0002 0446     		mov	r4, r0
2236:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4373              		.loc 1 2236 3 is_stmt 1 view .LVU1559
2239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4374              		.loc 1 2239 3 view .LVU1560
2239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4375              		.loc 1 2239 11 is_stmt 0 view .LVU1561
 4376 0004 90F88130 		ldrb	r3, [r0, #129]	@ zero_extendqisi2
2239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4377              		.loc 1 2239 6 view .LVU1562
 4378 0008 012B     		cmp	r3, #1
 4379 000a 40F08980 		bne	.L278
 4380 000e 1546     		mov	r5, r2
 4381 0010 DEB2     		uxtb	r6, r3
2245:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4382              		.loc 1 2245 3 is_stmt 1 view .LVU1563
2245:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4383              		.loc 1 2245 6 is_stmt 0 view .LVU1564
 4384 0012 002A     		cmp	r2, #0
 4385 0014 18BF     		it	ne
 4386 0016 0029     		cmpne	r1, #0
 4387 0018 00F08880 		beq	.L279
2252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4388              		.loc 1 2252 3 is_stmt 1 view .LVU1565
2252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4389              		.loc 1 2252 3 view .LVU1566
 4390 001c 90F88030 		ldrb	r3, [r0, #128]	@ zero_extendqisi2
 4391 0020 012B     		cmp	r3, #1
 4392 0022 00F0C980 		beq	.L276
2252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4393              		.loc 1 2252 3 discriminator 2 view .LVU1567
 4394 0026 0123     		movs	r3, #1
 4395 0028 80F88030 		strb	r3, [r0, #128]
2252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 172


 4396              		.loc 1 2252 3 view .LVU1568
2255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 4397              		.loc 1 2255 3 view .LVU1569
2255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 4398              		.loc 1 2255 21 is_stmt 0 view .LVU1570
 4399 002c 0423     		movs	r3, #4
 4400 002e 80F88130 		strb	r3, [r0, #129]
2256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 4401              		.loc 1 2256 3 is_stmt 1 view .LVU1571
2256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 4402              		.loc 1 2256 21 is_stmt 0 view .LVU1572
 4403 0032 0023     		movs	r3, #0
 4404 0034 C0F88430 		str	r3, [r0, #132]
2257:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 4405              		.loc 1 2257 3 is_stmt 1 view .LVU1573
2257:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 4406              		.loc 1 2257 21 is_stmt 0 view .LVU1574
 4407 0038 4166     		str	r1, [r0, #100]
2258:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
 4408              		.loc 1 2258 3 is_stmt 1 view .LVU1575
2258:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
 4409              		.loc 1 2258 21 is_stmt 0 view .LVU1576
 4410 003a A4F86820 		strh	r2, [r4, #104]	@ movhi
2259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4411              		.loc 1 2259 3 is_stmt 1 view .LVU1577
2259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4412              		.loc 1 2259 21 is_stmt 0 view .LVU1578
 4413 003e A4F86A20 		strh	r2, [r4, #106]	@ movhi
2262:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 4414              		.loc 1 2262 3 is_stmt 1 view .LVU1579
2262:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 4415              		.loc 1 2262 21 is_stmt 0 view .LVU1580
 4416 0042 0367     		str	r3, [r0, #112]
2263:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = (uint16_t) 0UL;
 4417              		.loc 1 2263 3 is_stmt 1 view .LVU1581
2263:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = (uint16_t) 0UL;
 4418              		.loc 1 2263 21 is_stmt 0 view .LVU1582
 4419 0044 4367     		str	r3, [r0, #116]
2264:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t) 0UL;
 4420              		.loc 1 2264 3 is_stmt 1 view .LVU1583
2264:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t) 0UL;
 4421              		.loc 1 2264 21 is_stmt 0 view .LVU1584
 4422 0046 A0F86030 		strh	r3, [r0, #96]	@ movhi
2265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4423              		.loc 1 2265 3 is_stmt 1 view .LVU1585
2265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4424              		.loc 1 2265 21 is_stmt 0 view .LVU1586
 4425 004a A0F86230 		strh	r3, [r0, #98]	@ movhi
2268:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4426              		.loc 1 2268 3 is_stmt 1 view .LVU1587
2268:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4427              		.loc 1 2268 17 is_stmt 0 view .LVU1588
 4428 004e 8368     		ldr	r3, [r0, #8]
2268:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4429              		.loc 1 2268 6 view .LVU1589
 4430 0050 B3F5C02F 		cmp	r3, #393216
 4431 0054 6ED0     		beq	.L280
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 173


2274:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4432              		.loc 1 2274 5 is_stmt 1 view .LVU1590
 4433 0056 0268     		ldr	r2, [r0]
 4434              	.LVL229:
2274:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4435              		.loc 1 2274 5 is_stmt 0 view .LVU1591
 4436 0058 D368     		ldr	r3, [r2, #12]
 4437 005a 23F4C023 		bic	r3, r3, #393216
 4438 005e 43F48023 		orr	r3, r3, #262144
 4439 0062 D360     		str	r3, [r2, #12]
 4440              	.LVL230:
 4441              	.L265:
2278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4442              		.loc 1 2278 3 is_stmt 1 view .LVU1592
2278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4443              		.loc 1 2278 19 is_stmt 0 view .LVU1593
 4444 0064 E368     		ldr	r3, [r4, #12]
2278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4445              		.loc 1 2278 6 view .LVU1594
 4446 0066 0F2B     		cmp	r3, #15
 4447 0068 04D9     		bls	.L266
2278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4448              		.loc 1 2278 59 discriminator 1 view .LVU1595
 4449 006a E26F     		ldr	r2, [r4, #124]
2278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4450              		.loc 1 2278 73 discriminator 1 view .LVU1596
 4451 006c 9269     		ldr	r2, [r2, #24]
2278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4452              		.loc 1 2278 51 discriminator 1 view .LVU1597
 4453 006e B2F5804F 		cmp	r2, #16384
 4454 0072 65D1     		bne	.L267
 4455              	.L266:
2278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4456              		.loc 1 2278 119 discriminator 3 view .LVU1598
 4457 0074 072B     		cmp	r3, #7
 4458 0076 07D9     		bls	.L268
2279:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                      (hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4459              		.loc 1 2279 59 view .LVU1599
 4460 0078 E36F     		ldr	r3, [r4, #124]
2279:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                      (hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4461              		.loc 1 2279 73 view .LVU1600
 4462 007a 9B69     		ldr	r3, [r3, #24]
2279:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                      (hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4463              		.loc 1 2279 50 view .LVU1601
 4464 007c B3F5005F 		cmp	r3, #8192
 4465 0080 18BF     		it	ne
 4466 0082 B3F5804F 		cmpne	r3, #16384
 4467 0086 5BD1     		bne	.L267
 4468              	.L268:
2288:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4469              		.loc 1 2288 3 is_stmt 1 view .LVU1602
 4470 0088 2268     		ldr	r2, [r4]
 4471 008a 9368     		ldr	r3, [r2, #8]
 4472 008c 23F48043 		bic	r3, r3, #16384
 4473 0090 9360     		str	r3, [r2, #8]
2291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4474              		.loc 1 2291 3 view .LVU1603
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 174


2291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4475              		.loc 1 2291 17 is_stmt 0 view .LVU1604
 4476 0092 E368     		ldr	r3, [r4, #12]
2291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4477              		.loc 1 2291 6 view .LVU1605
 4478 0094 072B     		cmp	r3, #7
 4479 0096 67D8     		bhi	.L269
2293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4480              		.loc 1 2293 5 is_stmt 1 view .LVU1606
2293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4481              		.loc 1 2293 13 is_stmt 0 view .LVU1607
 4482 0098 E36F     		ldr	r3, [r4, #124]
2293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4483              		.loc 1 2293 27 view .LVU1608
 4484 009a 9A69     		ldr	r2, [r3, #24]
2293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4485              		.loc 1 2293 8 view .LVU1609
 4486 009c B2F5005F 		cmp	r2, #8192
 4487 00a0 52D0     		beq	.L281
 4488              	.L270:
2297:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4489              		.loc 1 2297 5 is_stmt 1 view .LVU1610
2297:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4490              		.loc 1 2297 27 is_stmt 0 view .LVU1611
 4491 00a2 9B69     		ldr	r3, [r3, #24]
2297:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4492              		.loc 1 2297 8 view .LVU1612
 4493 00a4 B3F5804F 		cmp	r3, #16384
 4494 00a8 56D0     		beq	.L282
 4495              	.L271:
2312:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4496              		.loc 1 2312 3 is_stmt 1 view .LVU1613
2315:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4497              		.loc 1 2315 3 view .LVU1614
2315:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4498              		.loc 1 2315 7 is_stmt 0 view .LVU1615
 4499 00aa E36F     		ldr	r3, [r4, #124]
2315:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4500              		.loc 1 2315 38 view .LVU1616
 4501 00ac 434A     		ldr	r2, .L286
 4502 00ae 1A64     		str	r2, [r3, #64]
2318:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4503              		.loc 1 2318 3 is_stmt 1 view .LVU1617
2318:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4504              		.loc 1 2318 7 is_stmt 0 view .LVU1618
 4505 00b0 E36F     		ldr	r3, [r4, #124]
2318:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4506              		.loc 1 2318 34 view .LVU1619
 4507 00b2 434A     		ldr	r2, .L286+4
 4508 00b4 DA63     		str	r2, [r3, #60]
2321:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4509              		.loc 1 2321 3 is_stmt 1 view .LVU1620
2321:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4510              		.loc 1 2321 7 is_stmt 0 view .LVU1621
 4511 00b6 E36F     		ldr	r3, [r4, #124]
2321:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4512              		.loc 1 2321 35 view .LVU1622
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 175


 4513 00b8 424A     		ldr	r2, .L286+8
 4514 00ba DA64     		str	r2, [r3, #76]
2324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4515              		.loc 1 2324 3 is_stmt 1 view .LVU1623
2324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4516              		.loc 1 2324 7 is_stmt 0 view .LVU1624
 4517 00bc E36F     		ldr	r3, [r4, #124]
2324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4518              		.loc 1 2324 35 view .LVU1625
 4519 00be 0022     		movs	r2, #0
 4520 00c0 1A65     		str	r2, [r3, #80]
2327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->RxXferCount))
 4521              		.loc 1 2327 3 is_stmt 1 view .LVU1626
2327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->RxXferCount))
 4522              		.loc 1 2327 63 is_stmt 0 view .LVU1627
 4523 00c2 2168     		ldr	r1, [r4]
 4524              	.LVL231:
2328:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4525              		.loc 1 2328 38 view .LVU1628
 4526 00c4 B4F86A30 		ldrh	r3, [r4, #106]
2327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->RxXferCount))
 4527              		.loc 1 2327 17 view .LVU1629
 4528 00c8 9BB2     		uxth	r3, r3
 4529 00ca 626E     		ldr	r2, [r4, #100]
 4530 00cc 3031     		adds	r1, r1, #48
 4531 00ce E06F     		ldr	r0, [r4, #124]
 4532              	.LVL232:
2327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->RxXferCount))
 4533              		.loc 1 2327 17 view .LVU1630
 4534 00d0 FFF7FEFF 		bl	HAL_DMA_Start_IT
 4535              	.LVL233:
2327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->RxXferCount))
 4536              		.loc 1 2327 6 discriminator 1 view .LVU1631
 4537 00d4 0146     		mov	r1, r0
 4538 00d6 0028     		cmp	r0, #0
 4539 00d8 55D1     		bne	.L283
2341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4540              		.loc 1 2341 3 is_stmt 1 view .LVU1632
2341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4541              		.loc 1 2341 11 is_stmt 0 view .LVU1633
 4542 00da E36F     		ldr	r3, [r4, #124]
2341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4543              		.loc 1 2341 25 view .LVU1634
 4544 00dc DB69     		ldr	r3, [r3, #28]
2341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4545              		.loc 1 2341 6 view .LVU1635
 4546 00de B3F5807F 		cmp	r3, #256
 4547 00e2 5DD0     		beq	.L284
2347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4548              		.loc 1 2347 5 is_stmt 1 view .LVU1636
 4549 00e4 2268     		ldr	r2, [r4]
 4550 00e6 5368     		ldr	r3, [r2, #4]
 4551 00e8 6FF30F03 		bfc	r3, #0, #16
 4552 00ec 1D43     		orrs	r5, r5, r3
 4553              	.LVL234:
2347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4554              		.loc 1 2347 5 is_stmt 0 view .LVU1637
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 176


 4555 00ee 5560     		str	r5, [r2, #4]
 4556              	.L274:
2351:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4557              		.loc 1 2351 3 is_stmt 1 view .LVU1638
 4558 00f0 2268     		ldr	r2, [r4]
 4559 00f2 9368     		ldr	r3, [r2, #8]
 4560 00f4 43F48043 		orr	r3, r3, #16384
 4561 00f8 9360     		str	r3, [r2, #8]
2354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4562              		.loc 1 2354 3 view .LVU1639
 4563 00fa 2268     		ldr	r2, [r4]
 4564 00fc 1369     		ldr	r3, [r2, #16]
 4565 00fe 43F45073 		orr	r3, r3, #832
 4566 0102 1361     		str	r3, [r2, #16]
2357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4567              		.loc 1 2357 3 view .LVU1640
 4568 0104 2268     		ldr	r2, [r4]
 4569 0106 1368     		ldr	r3, [r2]
 4570 0108 43F00103 		orr	r3, r3, #1
 4571 010c 1360     		str	r3, [r2]
2359:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4572              		.loc 1 2359 3 view .LVU1641
2359:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4573              		.loc 1 2359 17 is_stmt 0 view .LVU1642
 4574 010e 6368     		ldr	r3, [r4, #4]
2359:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4575              		.loc 1 2359 6 view .LVU1643
 4576 0110 B3F5800F 		cmp	r3, #4194304
 4577 0114 4AD0     		beq	.L285
 4578              	.L275:
2366:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4579              		.loc 1 2366 3 is_stmt 1 view .LVU1644
2366:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4580              		.loc 1 2366 3 view .LVU1645
 4581 0116 0023     		movs	r3, #0
 4582 0118 84F88030 		strb	r3, [r4, #128]
2366:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4583              		.loc 1 2366 3 view .LVU1646
2368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 4584              		.loc 1 2368 3 view .LVU1647
2368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 4585              		.loc 1 2368 10 is_stmt 0 view .LVU1648
 4586 011c 0E46     		mov	r6, r1
 4587 011e 03E0     		b	.L262
 4588              	.LVL235:
 4589              	.L278:
2241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_BUSY;
 4590              		.loc 1 2241 5 is_stmt 1 view .LVU1649
2241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_BUSY;
 4591              		.loc 1 2241 5 view .LVU1650
 4592 0120 0023     		movs	r3, #0
 4593 0122 80F88030 		strb	r3, [r0, #128]
2241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_BUSY;
 4594              		.loc 1 2241 5 view .LVU1651
2242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4595              		.loc 1 2242 5 view .LVU1652
2242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 177


 4596              		.loc 1 2242 12 is_stmt 0 view .LVU1653
 4597 0126 0226     		movs	r6, #2
 4598              	.LVL236:
 4599              	.L262:
2369:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4600              		.loc 1 2369 1 view .LVU1654
 4601 0128 3046     		mov	r0, r6
 4602 012a 70BD     		pop	{r4, r5, r6, pc}
 4603              	.LVL237:
 4604              	.L279:
2247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 4605              		.loc 1 2247 5 is_stmt 1 view .LVU1655
2247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 4606              		.loc 1 2247 5 view .LVU1656
 4607 012c 0023     		movs	r3, #0
 4608 012e 80F88030 		strb	r3, [r0, #128]
2247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 4609              		.loc 1 2247 5 view .LVU1657
2248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4610              		.loc 1 2248 5 view .LVU1658
2248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4611              		.loc 1 2248 12 is_stmt 0 view .LVU1659
 4612 0132 F9E7     		b	.L262
 4613              	.L280:
2270:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4614              		.loc 1 2270 5 is_stmt 1 view .LVU1660
 4615 0134 0268     		ldr	r2, [r0]
 4616              	.LVL238:
2270:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4617              		.loc 1 2270 5 is_stmt 0 view .LVU1661
 4618 0136 1368     		ldr	r3, [r2]
 4619 0138 23F40063 		bic	r3, r3, #2048
 4620 013c 1360     		str	r3, [r2]
 4621              	.LVL239:
2270:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4622              		.loc 1 2270 5 view .LVU1662
 4623 013e 91E7     		b	.L265
 4624              	.L267:
2283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 4625              		.loc 1 2283 5 is_stmt 1 view .LVU1663
2283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 4626              		.loc 1 2283 5 view .LVU1664
 4627 0140 0023     		movs	r3, #0
 4628 0142 84F88030 		strb	r3, [r4, #128]
2283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 4629              		.loc 1 2283 5 view .LVU1665
2284:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4630              		.loc 1 2284 5 view .LVU1666
2284:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4631              		.loc 1 2284 12 is_stmt 0 view .LVU1667
 4632 0146 EFE7     		b	.L262
 4633              	.L281:
2295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4634              		.loc 1 2295 7 is_stmt 1 view .LVU1668
2295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4635              		.loc 1 2295 32 is_stmt 0 view .LVU1669
 4636 0148 B4F86A20 		ldrh	r2, [r4, #106]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 178


 4637 014c 92B2     		uxth	r2, r2
2295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4638              		.loc 1 2295 46 view .LVU1670
 4639 014e 0132     		adds	r2, r2, #1
2295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4640              		.loc 1 2295 25 view .LVU1671
 4641 0150 5208     		lsrs	r2, r2, #1
 4642 0152 A4F86A20 		strh	r2, [r4, #106]	@ movhi
 4643 0156 A4E7     		b	.L270
 4644              	.L282:
2299:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4645              		.loc 1 2299 7 is_stmt 1 view .LVU1672
2299:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4646              		.loc 1 2299 32 is_stmt 0 view .LVU1673
 4647 0158 B4F86A30 		ldrh	r3, [r4, #106]
 4648 015c 9BB2     		uxth	r3, r3
2299:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4649              		.loc 1 2299 46 view .LVU1674
 4650 015e 0333     		adds	r3, r3, #3
2299:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4651              		.loc 1 2299 25 view .LVU1675
 4652 0160 9B08     		lsrs	r3, r3, #2
 4653 0162 A4F86A30 		strh	r3, [r4, #106]	@ movhi
 4654 0166 A0E7     		b	.L271
 4655              	.L269:
2302:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4656              		.loc 1 2302 8 is_stmt 1 view .LVU1676
2302:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4657              		.loc 1 2302 11 is_stmt 0 view .LVU1677
 4658 0168 0F2B     		cmp	r3, #15
 4659 016a 9ED8     		bhi	.L271
2304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4660              		.loc 1 2304 5 is_stmt 1 view .LVU1678
2304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4661              		.loc 1 2304 13 is_stmt 0 view .LVU1679
 4662 016c E36F     		ldr	r3, [r4, #124]
2304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4663              		.loc 1 2304 27 view .LVU1680
 4664 016e 9B69     		ldr	r3, [r3, #24]
2304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4665              		.loc 1 2304 8 view .LVU1681
 4666 0170 B3F5804F 		cmp	r3, #16384
 4667 0174 99D1     		bne	.L271
2306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4668              		.loc 1 2306 7 is_stmt 1 view .LVU1682
2306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4669              		.loc 1 2306 32 is_stmt 0 view .LVU1683
 4670 0176 B4F86A30 		ldrh	r3, [r4, #106]
 4671 017a 9BB2     		uxth	r3, r3
2306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4672              		.loc 1 2306 46 view .LVU1684
 4673 017c 0133     		adds	r3, r3, #1
2306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4674              		.loc 1 2306 25 view .LVU1685
 4675 017e 5B08     		lsrs	r3, r3, #1
 4676 0180 A4F86A30 		strh	r3, [r4, #106]	@ movhi
 4677 0184 91E7     		b	.L271
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 179


 4678              	.LVL240:
 4679              	.L283:
2331:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 4680              		.loc 1 2331 5 is_stmt 1 view .LVU1686
 4681 0186 D4F88430 		ldr	r3, [r4, #132]
 4682 018a 43F01003 		orr	r3, r3, #16
 4683 018e C4F88430 		str	r3, [r4, #132]
2332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4684              		.loc 1 2332 5 view .LVU1687
2332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4685              		.loc 1 2332 17 is_stmt 0 view .LVU1688
 4686 0192 0123     		movs	r3, #1
 4687 0194 84F88130 		strb	r3, [r4, #129]
2335:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4688              		.loc 1 2335 5 is_stmt 1 view .LVU1689
2335:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4689              		.loc 1 2335 5 view .LVU1690
 4690 0198 0023     		movs	r3, #0
 4691 019a 84F88030 		strb	r3, [r4, #128]
2335:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4692              		.loc 1 2335 5 view .LVU1691
2337:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4693              		.loc 1 2337 5 view .LVU1692
2337:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4694              		.loc 1 2337 12 is_stmt 0 view .LVU1693
 4695 019e C3E7     		b	.L262
 4696              	.L284:
2343:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4697              		.loc 1 2343 5 is_stmt 1 view .LVU1694
 4698 01a0 2268     		ldr	r2, [r4]
 4699 01a2 5368     		ldr	r3, [r2, #4]
 4700 01a4 6FF30F03 		bfc	r3, #0, #16
 4701 01a8 5360     		str	r3, [r2, #4]
 4702 01aa A1E7     		b	.L274
 4703              	.LVL241:
 4704              	.L285:
2362:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4705              		.loc 1 2362 5 view .LVU1695
 4706 01ac 2268     		ldr	r2, [r4]
 4707 01ae 1368     		ldr	r3, [r2]
 4708 01b0 43F40073 		orr	r3, r3, #512
 4709 01b4 1360     		str	r3, [r2]
 4710 01b6 AEE7     		b	.L275
 4711              	.LVL242:
 4712              	.L276:
2252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4713              		.loc 1 2252 3 is_stmt 0 discriminator 1 view .LVU1696
 4714 01b8 0226     		movs	r6, #2
 4715 01ba B5E7     		b	.L262
 4716              	.L287:
 4717              		.align	2
 4718              	.L286:
 4719 01bc 00000000 		.word	SPI_DMAHalfReceiveCplt
 4720 01c0 00000000 		.word	SPI_DMAReceiveCplt
 4721 01c4 00000000 		.word	SPI_DMAError
 4722              		.cfi_endproc
 4723              	.LFE346:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 180


 4725              		.section	.text.HAL_SPI_TransmitReceive_DMA,"ax",%progbits
 4726              		.align	1
 4727              		.global	HAL_SPI_TransmitReceive_DMA
 4728              		.syntax unified
 4729              		.thumb
 4730              		.thumb_func
 4732              	HAL_SPI_TransmitReceive_DMA:
 4733              	.LVL243:
 4734              	.LFB347:
2383:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
 4735              		.loc 1 2383 1 is_stmt 1 view -0
 4736              		.cfi_startproc
 4737              		@ args = 0, pretend = 0, frame = 0
 4738              		@ frame_needed = 0, uses_anonymous_args = 0
2383:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Check Direction parameter */
 4739              		.loc 1 2383 1 is_stmt 0 view .LVU1698
 4740 0000 70B5     		push	{r4, r5, r6, lr}
 4741              		.cfi_def_cfa_offset 16
 4742              		.cfi_offset 4, -16
 4743              		.cfi_offset 5, -12
 4744              		.cfi_offset 6, -8
 4745              		.cfi_offset 14, -4
 4746 0002 1D46     		mov	r5, r3
2385:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4747              		.loc 1 2385 3 is_stmt 1 view .LVU1699
2387:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4748              		.loc 1 2387 3 view .LVU1700
2387:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4749              		.loc 1 2387 11 is_stmt 0 view .LVU1701
 4750 0004 90F88130 		ldrb	r3, [r0, #129]	@ zero_extendqisi2
 4751              	.LVL244:
2387:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4752              		.loc 1 2387 6 view .LVU1702
 4753 0008 012B     		cmp	r3, #1
 4754 000a 40F01181 		bne	.L304
 4755 000e 0446     		mov	r4, r0
 4756 0010 DEB2     		uxtb	r6, r3
2392:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4757              		.loc 1 2392 3 is_stmt 1 view .LVU1703
2392:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4758              		.loc 1 2392 6 is_stmt 0 view .LVU1704
 4759 0012 002A     		cmp	r2, #0
 4760 0014 18BF     		it	ne
 4761 0016 0029     		cmpne	r1, #0
 4762 0018 00F00B81 		beq	.L289
2392:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4763              		.loc 1 2392 46 discriminator 1 view .LVU1705
 4764 001c 002D     		cmp	r5, #0
 4765 001e 00F00881 		beq	.L289
2398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4766              		.loc 1 2398 3 is_stmt 1 view .LVU1706
2398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4767              		.loc 1 2398 3 view .LVU1707
 4768 0022 90F88030 		ldrb	r3, [r0, #128]	@ zero_extendqisi2
 4769 0026 012B     		cmp	r3, #1
 4770 0028 00F00581 		beq	.L305
2398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 181


 4771              		.loc 1 2398 3 discriminator 2 view .LVU1708
 4772 002c 0123     		movs	r3, #1
 4773 002e 80F88030 		strb	r3, [r0, #128]
2398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4774              		.loc 1 2398 3 view .LVU1709
2401:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 4775              		.loc 1 2401 3 view .LVU1710
2401:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 4776              		.loc 1 2401 21 is_stmt 0 view .LVU1711
 4777 0032 0523     		movs	r3, #5
 4778 0034 80F88130 		strb	r3, [r0, #129]
2402:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pTxData;
 4779              		.loc 1 2402 3 is_stmt 1 view .LVU1712
2402:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pTxBuffPtr  = (const uint8_t *)pTxData;
 4780              		.loc 1 2402 21 is_stmt 0 view .LVU1713
 4781 0038 0023     		movs	r3, #0
 4782 003a C0F88430 		str	r3, [r0, #132]
2403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 4783              		.loc 1 2403 3 is_stmt 1 view .LVU1714
2403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 4784              		.loc 1 2403 21 is_stmt 0 view .LVU1715
 4785 003e C165     		str	r1, [r0, #92]
2404:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 4786              		.loc 1 2404 3 is_stmt 1 view .LVU1716
2404:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = Size;
 4787              		.loc 1 2404 21 is_stmt 0 view .LVU1717
 4788 0040 A0F86050 		strh	r5, [r0, #96]	@ movhi
2405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 4789              		.loc 1 2405 3 is_stmt 1 view .LVU1718
2405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 4790              		.loc 1 2405 21 is_stmt 0 view .LVU1719
 4791 0044 A0F86250 		strh	r5, [r0, #98]	@ movhi
2406:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 4792              		.loc 1 2406 3 is_stmt 1 view .LVU1720
2406:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 4793              		.loc 1 2406 21 is_stmt 0 view .LVU1721
 4794 0048 4266     		str	r2, [r0, #100]
2407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
 4795              		.loc 1 2407 3 is_stmt 1 view .LVU1722
2407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = Size;
 4796              		.loc 1 2407 21 is_stmt 0 view .LVU1723
 4797 004a A0F86850 		strh	r5, [r0, #104]	@ movhi
2408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4798              		.loc 1 2408 3 is_stmt 1 view .LVU1724
2408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4799              		.loc 1 2408 21 is_stmt 0 view .LVU1725
 4800 004e A0F86A50 		strh	r5, [r0, #106]	@ movhi
2411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 4801              		.loc 1 2411 3 is_stmt 1 view .LVU1726
2411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxISR       = NULL;
 4802              		.loc 1 2411 21 is_stmt 0 view .LVU1727
 4803 0052 0367     		str	r3, [r0, #112]
2412:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4804              		.loc 1 2412 3 is_stmt 1 view .LVU1728
2412:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4805              		.loc 1 2412 21 is_stmt 0 view .LVU1729
 4806 0054 4367     		str	r3, [r0, #116]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 182


2415:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4807              		.loc 1 2415 3 is_stmt 1 view .LVU1730
 4808 0056 0268     		ldr	r2, [r0]
 4809              	.LVL245:
2415:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4810              		.loc 1 2415 3 is_stmt 0 view .LVU1731
 4811 0058 D368     		ldr	r3, [r2, #12]
 4812 005a 23F4C023 		bic	r3, r3, #393216
 4813 005e D360     		str	r3, [r2, #12]
 4814              	.LVL246:
2418:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4815              		.loc 1 2418 3 is_stmt 1 view .LVU1732
 4816 0060 0268     		ldr	r2, [r0]
 4817 0062 9368     		ldr	r3, [r2, #8]
 4818 0064 23F44043 		bic	r3, r3, #49152
 4819 0068 9360     		str	r3, [r2, #8]
2421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4820              		.loc 1 2421 3 view .LVU1733
2421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4821              		.loc 1 2421 19 is_stmt 0 view .LVU1734
 4822 006a C368     		ldr	r3, [r0, #12]
2421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4823              		.loc 1 2421 6 view .LVU1735
 4824 006c 0F2B     		cmp	r3, #15
 4825 006e 04D9     		bls	.L290
2421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4826              		.loc 1 2421 59 discriminator 1 view .LVU1736
 4827 0070 C26F     		ldr	r2, [r0, #124]
2421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4828              		.loc 1 2421 73 discriminator 1 view .LVU1737
 4829 0072 9269     		ldr	r2, [r2, #24]
2421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4830              		.loc 1 2421 51 discriminator 1 view .LVU1738
 4831 0074 B2F5804F 		cmp	r2, #16384
 4832 0078 41D1     		bne	.L291
 4833              	.L290:
2421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) && ((hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4834              		.loc 1 2421 119 discriminator 3 view .LVU1739
 4835 007a 072B     		cmp	r3, #7
 4836 007c 07D9     		bls	.L292
2422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                      (hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4837              		.loc 1 2422 59 view .LVU1740
 4838 007e E26F     		ldr	r2, [r4, #124]
2422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                      (hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4839              		.loc 1 2422 73 view .LVU1741
 4840 0080 9269     		ldr	r2, [r2, #24]
2422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                                      (hspi->hdmarx->Init.MemDataAlignment != DMA_MD
 4841              		.loc 1 2422 50 view .LVU1742
 4842 0082 B2F5005F 		cmp	r2, #8192
 4843 0086 18BF     		it	ne
 4844 0088 B2F5804F 		cmpne	r2, #16384
 4845 008c 37D1     		bne	.L291
 4846              	.L292:
2432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4847              		.loc 1 2432 3 is_stmt 1 view .LVU1743
2432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4848              		.loc 1 2432 6 is_stmt 0 view .LVU1744
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 183


 4849 008e 072B     		cmp	r3, #7
 4850 0090 59D8     		bhi	.L293
2434:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4851              		.loc 1 2434 5 is_stmt 1 view .LVU1745
2434:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4852              		.loc 1 2434 13 is_stmt 0 view .LVU1746
 4853 0092 A36F     		ldr	r3, [r4, #120]
2434:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4854              		.loc 1 2434 27 view .LVU1747
 4855 0094 9A69     		ldr	r2, [r3, #24]
2434:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4856              		.loc 1 2434 8 view .LVU1748
 4857 0096 B2F5005F 		cmp	r2, #8192
 4858 009a 34D0     		beq	.L307
 4859              	.L294:
2438:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4860              		.loc 1 2438 5 is_stmt 1 view .LVU1749
2438:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4861              		.loc 1 2438 27 is_stmt 0 view .LVU1750
 4862 009c 9B69     		ldr	r3, [r3, #24]
2438:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4863              		.loc 1 2438 8 view .LVU1751
 4864 009e B3F5804F 		cmp	r3, #16384
 4865 00a2 38D0     		beq	.L308
 4866              	.L295:
2442:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4867              		.loc 1 2442 5 is_stmt 1 view .LVU1752
2442:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4868              		.loc 1 2442 13 is_stmt 0 view .LVU1753
 4869 00a4 E36F     		ldr	r3, [r4, #124]
2442:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4870              		.loc 1 2442 27 view .LVU1754
 4871 00a6 9A69     		ldr	r2, [r3, #24]
2442:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4872              		.loc 1 2442 8 view .LVU1755
 4873 00a8 B2F5005F 		cmp	r2, #8192
 4874 00ac 3BD0     		beq	.L309
 4875              	.L296:
2446:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4876              		.loc 1 2446 5 is_stmt 1 view .LVU1756
2446:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4877              		.loc 1 2446 27 is_stmt 0 view .LVU1757
 4878 00ae 9B69     		ldr	r3, [r3, #24]
2446:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 4879              		.loc 1 2446 8 view .LVU1758
 4880 00b0 B3F5804F 		cmp	r3, #16384
 4881 00b4 3FD0     		beq	.L310
 4882              	.L297:
2465:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4883              		.loc 1 2465 3 is_stmt 1 view .LVU1759
2468:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmarx->XferCpltCallback     = SPI_DMATransmitReceiveCplt;
 4884              		.loc 1 2468 3 view .LVU1760
2468:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmarx->XferCpltCallback     = SPI_DMATransmitReceiveCplt;
 4885              		.loc 1 2468 7 is_stmt 0 view .LVU1761
 4886 00b6 E36F     		ldr	r3, [r4, #124]
2468:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmarx->XferCpltCallback     = SPI_DMATransmitReceiveCplt;
 4887              		.loc 1 2468 38 view .LVU1762
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 184


 4888 00b8 604A     		ldr	r2, .L315
 4889 00ba 1A64     		str	r2, [r3, #64]
2469:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4890              		.loc 1 2469 3 is_stmt 1 view .LVU1763
2469:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4891              		.loc 1 2469 7 is_stmt 0 view .LVU1764
 4892 00bc E36F     		ldr	r3, [r4, #124]
2469:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4893              		.loc 1 2469 38 view .LVU1765
 4894 00be 604A     		ldr	r2, .L315+4
 4895 00c0 DA63     		str	r2, [r3, #60]
2472:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4896              		.loc 1 2472 3 is_stmt 1 view .LVU1766
2472:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4897              		.loc 1 2472 7 is_stmt 0 view .LVU1767
 4898 00c2 E36F     		ldr	r3, [r4, #124]
2472:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4899              		.loc 1 2472 35 view .LVU1768
 4900 00c4 5F4A     		ldr	r2, .L315+8
 4901 00c6 DA64     		str	r2, [r3, #76]
2475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4902              		.loc 1 2475 3 is_stmt 1 view .LVU1769
2475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4903              		.loc 1 2475 7 is_stmt 0 view .LVU1770
 4904 00c8 E36F     		ldr	r3, [r4, #124]
2475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4905              		.loc 1 2475 35 view .LVU1771
 4906 00ca 0022     		movs	r2, #0
 4907 00cc 1A65     		str	r2, [r3, #80]
2478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->RxXferCount))
 4908              		.loc 1 2478 3 is_stmt 1 view .LVU1772
2478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->RxXferCount))
 4909              		.loc 1 2478 63 is_stmt 0 view .LVU1773
 4910 00ce 2168     		ldr	r1, [r4]
 4911              	.LVL247:
2479:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4912              		.loc 1 2479 38 view .LVU1774
 4913 00d0 B4F86A30 		ldrh	r3, [r4, #106]
2478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->RxXferCount))
 4914              		.loc 1 2478 17 view .LVU1775
 4915 00d4 9BB2     		uxth	r3, r3
 4916 00d6 626E     		ldr	r2, [r4, #100]
 4917 00d8 3031     		adds	r1, r1, #48
 4918 00da E06F     		ldr	r0, [r4, #124]
 4919              	.LVL248:
2478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->RxXferCount))
 4920              		.loc 1 2478 17 view .LVU1776
 4921 00dc FFF7FEFF 		bl	HAL_DMA_Start_IT
 4922              	.LVL249:
2478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->RxXferCount))
 4923              		.loc 1 2478 6 discriminator 1 view .LVU1777
 4924 00e0 0028     		cmp	r0, #0
 4925 00e2 4CD0     		beq	.L299
2482:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 4926              		.loc 1 2482 5 is_stmt 1 view .LVU1778
 4927 00e4 D4F88430 		ldr	r3, [r4, #132]
 4928 00e8 43F01003 		orr	r3, r3, #16
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 185


 4929 00ec C4F88430 		str	r3, [r4, #132]
2483:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4930              		.loc 1 2483 5 view .LVU1779
2483:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4931              		.loc 1 2483 17 is_stmt 0 view .LVU1780
 4932 00f0 0123     		movs	r3, #1
 4933 00f2 84F88130 		strb	r3, [r4, #129]
2486:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4934              		.loc 1 2486 5 is_stmt 1 view .LVU1781
2486:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4935              		.loc 1 2486 5 view .LVU1782
 4936 00f6 0023     		movs	r3, #0
 4937 00f8 84F88030 		strb	r3, [r4, #128]
2486:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 4938              		.loc 1 2486 5 view .LVU1783
2488:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4939              		.loc 1 2488 5 view .LVU1784
2488:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4940              		.loc 1 2488 12 is_stmt 0 view .LVU1785
 4941 00fc 99E0     		b	.L289
 4942              	.LVL250:
 4943              	.L291:
2427:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 4944              		.loc 1 2427 5 is_stmt 1 view .LVU1786
2427:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 4945              		.loc 1 2427 5 view .LVU1787
 4946 00fe 0023     		movs	r3, #0
 4947 0100 84F88030 		strb	r3, [r4, #128]
2427:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     return HAL_ERROR;
 4948              		.loc 1 2427 5 view .LVU1788
2428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4949              		.loc 1 2428 5 view .LVU1789
2428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 4950              		.loc 1 2428 12 is_stmt 0 view .LVU1790
 4951 0104 95E0     		b	.L289
 4952              	.L307:
2436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4953              		.loc 1 2436 7 is_stmt 1 view .LVU1791
2436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4954              		.loc 1 2436 32 is_stmt 0 view .LVU1792
 4955 0106 B4F86220 		ldrh	r2, [r4, #98]
 4956 010a 92B2     		uxth	r2, r2
2436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4957              		.loc 1 2436 46 view .LVU1793
 4958 010c 0132     		adds	r2, r2, #1
2436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4959              		.loc 1 2436 25 view .LVU1794
 4960 010e 5208     		lsrs	r2, r2, #1
 4961 0110 A4F86220 		strh	r2, [r4, #98]	@ movhi
 4962 0114 C2E7     		b	.L294
 4963              	.L308:
2440:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4964              		.loc 1 2440 7 is_stmt 1 view .LVU1795
2440:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4965              		.loc 1 2440 32 is_stmt 0 view .LVU1796
 4966 0116 B4F86230 		ldrh	r3, [r4, #98]
 4967 011a 9BB2     		uxth	r3, r3
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 186


2440:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4968              		.loc 1 2440 46 view .LVU1797
 4969 011c 0333     		adds	r3, r3, #3
2440:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4970              		.loc 1 2440 25 view .LVU1798
 4971 011e 9B08     		lsrs	r3, r3, #2
 4972 0120 A4F86230 		strh	r3, [r4, #98]	@ movhi
 4973 0124 BEE7     		b	.L295
 4974              	.L309:
2444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4975              		.loc 1 2444 7 is_stmt 1 view .LVU1799
2444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4976              		.loc 1 2444 32 is_stmt 0 view .LVU1800
 4977 0126 B4F86A20 		ldrh	r2, [r4, #106]
 4978 012a 92B2     		uxth	r2, r2
2444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4979              		.loc 1 2444 46 view .LVU1801
 4980 012c 0132     		adds	r2, r2, #1
2444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4981              		.loc 1 2444 25 view .LVU1802
 4982 012e 5208     		lsrs	r2, r2, #1
 4983 0130 A4F86A20 		strh	r2, [r4, #106]	@ movhi
 4984 0134 BBE7     		b	.L296
 4985              	.L310:
2448:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4986              		.loc 1 2448 7 is_stmt 1 view .LVU1803
2448:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4987              		.loc 1 2448 32 is_stmt 0 view .LVU1804
 4988 0136 B4F86A30 		ldrh	r3, [r4, #106]
 4989 013a 9BB2     		uxth	r3, r3
2448:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4990              		.loc 1 2448 46 view .LVU1805
 4991 013c 0333     		adds	r3, r3, #3
2448:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 4992              		.loc 1 2448 25 view .LVU1806
 4993 013e 9B08     		lsrs	r3, r3, #2
 4994 0140 A4F86A30 		strh	r3, [r4, #106]	@ movhi
 4995 0144 B7E7     		b	.L297
 4996              	.L293:
2451:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4997              		.loc 1 2451 8 is_stmt 1 view .LVU1807
2451:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 4998              		.loc 1 2451 11 is_stmt 0 view .LVU1808
 4999 0146 0F2B     		cmp	r3, #15
 5000 0148 B5D8     		bhi	.L297
2453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5001              		.loc 1 2453 5 is_stmt 1 view .LVU1809
2453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5002              		.loc 1 2453 13 is_stmt 0 view .LVU1810
 5003 014a A36F     		ldr	r3, [r4, #120]
2453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5004              		.loc 1 2453 27 view .LVU1811
 5005 014c 9B69     		ldr	r3, [r3, #24]
2453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5006              		.loc 1 2453 8 view .LVU1812
 5007 014e B3F5804F 		cmp	r3, #16384
 5008 0152 0CD0     		beq	.L311
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 187


 5009              	.L298:
2457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5010              		.loc 1 2457 5 is_stmt 1 view .LVU1813
2457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5011              		.loc 1 2457 13 is_stmt 0 view .LVU1814
 5012 0154 E36F     		ldr	r3, [r4, #124]
2457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5013              		.loc 1 2457 27 view .LVU1815
 5014 0156 9B69     		ldr	r3, [r3, #24]
2457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5015              		.loc 1 2457 8 view .LVU1816
 5016 0158 B3F5804F 		cmp	r3, #16384
 5017 015c ABD1     		bne	.L297
2459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 5018              		.loc 1 2459 7 is_stmt 1 view .LVU1817
2459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 5019              		.loc 1 2459 32 is_stmt 0 view .LVU1818
 5020 015e B4F86A30 		ldrh	r3, [r4, #106]
 5021 0162 9BB2     		uxth	r3, r3
2459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 5022              		.loc 1 2459 46 view .LVU1819
 5023 0164 0133     		adds	r3, r3, #1
2459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 5024              		.loc 1 2459 25 view .LVU1820
 5025 0166 5B08     		lsrs	r3, r3, #1
 5026 0168 A4F86A30 		strh	r3, [r4, #106]	@ movhi
 5027 016c A3E7     		b	.L297
 5028              	.L311:
2455:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 5029              		.loc 1 2455 7 is_stmt 1 view .LVU1821
2455:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 5030              		.loc 1 2455 32 is_stmt 0 view .LVU1822
 5031 016e B4F86230 		ldrh	r3, [r4, #98]
 5032 0172 9BB2     		uxth	r3, r3
2455:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 5033              		.loc 1 2455 46 view .LVU1823
 5034 0174 0133     		adds	r3, r3, #1
2455:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 5035              		.loc 1 2455 25 view .LVU1824
 5036 0176 5B08     		lsrs	r3, r3, #1
 5037 0178 A4F86230 		strh	r3, [r4, #98]	@ movhi
 5038 017c EAE7     		b	.L298
 5039              	.LVL251:
 5040              	.L299:
2492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5041              		.loc 1 2492 3 is_stmt 1 view .LVU1825
 5042 017e 2268     		ldr	r2, [r4]
 5043 0180 9368     		ldr	r3, [r2, #8]
 5044 0182 43F48043 		orr	r3, r3, #16384
 5045 0186 9360     		str	r3, [r2, #8]
2496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback     = NULL;
 5046              		.loc 1 2496 3 view .LVU1826
2496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback     = NULL;
 5047              		.loc 1 2496 7 is_stmt 0 view .LVU1827
 5048 0188 A26F     		ldr	r2, [r4, #120]
2496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback     = NULL;
 5049              		.loc 1 2496 38 view .LVU1828
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 188


 5050 018a 0023     		movs	r3, #0
 5051 018c 1364     		str	r3, [r2, #64]
2497:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback    = NULL;
 5052              		.loc 1 2497 3 is_stmt 1 view .LVU1829
2497:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback    = NULL;
 5053              		.loc 1 2497 7 is_stmt 0 view .LVU1830
 5054 018e A26F     		ldr	r2, [r4, #120]
2497:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback    = NULL;
 5055              		.loc 1 2497 38 view .LVU1831
 5056 0190 D363     		str	r3, [r2, #60]
2498:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5057              		.loc 1 2498 3 is_stmt 1 view .LVU1832
2498:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5058              		.loc 1 2498 7 is_stmt 0 view .LVU1833
 5059 0192 A26F     		ldr	r2, [r4, #120]
2498:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5060              		.loc 1 2498 38 view .LVU1834
 5061 0194 1365     		str	r3, [r2, #80]
2501:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5062              		.loc 1 2501 3 is_stmt 1 view .LVU1835
2501:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5063              		.loc 1 2501 7 is_stmt 0 view .LVU1836
 5064 0196 A36F     		ldr	r3, [r4, #120]
2501:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5065              		.loc 1 2501 38 view .LVU1837
 5066 0198 2A4A     		ldr	r2, .L315+8
 5067 019a DA64     		str	r2, [r3, #76]
2504:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->TxXferCount))
 5068              		.loc 1 2504 3 is_stmt 1 view .LVU1838
2504:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->TxXferCount))
 5069              		.loc 1 2504 91 is_stmt 0 view .LVU1839
 5070 019c 2268     		ldr	r2, [r4]
2505:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5071              		.loc 1 2505 38 view .LVU1840
 5072 019e B4F86230 		ldrh	r3, [r4, #98]
2504:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->TxXferCount))
 5073              		.loc 1 2504 17 view .LVU1841
 5074 01a2 9BB2     		uxth	r3, r3
 5075 01a4 2032     		adds	r2, r2, #32
 5076 01a6 E16D     		ldr	r1, [r4, #92]
 5077 01a8 A06F     		ldr	r0, [r4, #120]
 5078 01aa FFF7FEFF 		bl	HAL_DMA_Start_IT
 5079              	.LVL252:
2504:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                  hspi->TxXferCount))
 5080              		.loc 1 2504 6 discriminator 1 view .LVU1842
 5081 01ae 0146     		mov	r1, r0
 5082 01b0 10BB     		cbnz	r0, .L312
2520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5083              		.loc 1 2520 3 is_stmt 1 view .LVU1843
2520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5084              		.loc 1 2520 11 is_stmt 0 view .LVU1844
 5085 01b2 A36F     		ldr	r3, [r4, #120]
2520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5086              		.loc 1 2520 25 view .LVU1845
 5087 01b4 DB69     		ldr	r3, [r3, #28]
2520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5088              		.loc 1 2520 6 view .LVU1846
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 189


 5089 01b6 B3F5807F 		cmp	r3, #256
 5090 01ba 2DD0     		beq	.L313
2526:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 5091              		.loc 1 2526 5 is_stmt 1 view .LVU1847
 5092 01bc 2268     		ldr	r2, [r4]
 5093 01be 5368     		ldr	r3, [r2, #4]
 5094 01c0 6FF30F03 		bfc	r3, #0, #16
 5095 01c4 1D43     		orrs	r5, r5, r3
 5096              	.LVL253:
2526:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 5097              		.loc 1 2526 5 is_stmt 0 view .LVU1848
 5098 01c6 5560     		str	r5, [r2, #4]
 5099              	.L302:
2530:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5100              		.loc 1 2530 3 is_stmt 1 view .LVU1849
 5101 01c8 2268     		ldr	r2, [r4]
 5102 01ca 9368     		ldr	r3, [r2, #8]
 5103 01cc 43F40043 		orr	r3, r3, #32768
 5104 01d0 9360     		str	r3, [r2, #8]
2533:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5105              		.loc 1 2533 3 view .LVU1850
 5106 01d2 2268     		ldr	r2, [r4]
 5107 01d4 1369     		ldr	r3, [r2, #16]
 5108 01d6 43F45873 		orr	r3, r3, #864
 5109 01da 1361     		str	r3, [r2, #16]
2536:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5110              		.loc 1 2536 3 view .LVU1851
 5111 01dc 2268     		ldr	r2, [r4]
 5112 01de 1368     		ldr	r3, [r2]
 5113 01e0 43F00103 		orr	r3, r3, #1
 5114 01e4 1360     		str	r3, [r2]
2538:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5115              		.loc 1 2538 3 view .LVU1852
2538:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5116              		.loc 1 2538 17 is_stmt 0 view .LVU1853
 5117 01e6 6368     		ldr	r3, [r4, #4]
2538:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5118              		.loc 1 2538 6 view .LVU1854
 5119 01e8 B3F5800F 		cmp	r3, #4194304
 5120 01ec 1AD0     		beq	.L314
 5121              	.L303:
2545:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5122              		.loc 1 2545 3 is_stmt 1 view .LVU1855
2545:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5123              		.loc 1 2545 3 view .LVU1856
 5124 01ee 0023     		movs	r3, #0
 5125 01f0 84F88030 		strb	r3, [r4, #128]
2545:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5126              		.loc 1 2545 3 view .LVU1857
2547:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 5127              		.loc 1 2547 3 view .LVU1858
2547:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 5128              		.loc 1 2547 10 is_stmt 0 view .LVU1859
 5129 01f4 0E46     		mov	r6, r1
 5130 01f6 1CE0     		b	.L289
 5131              	.L312:
2508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 190


 5132              		.loc 1 2508 5 is_stmt 1 view .LVU1860
2508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5133              		.loc 1 2508 11 is_stmt 0 view .LVU1861
 5134 01f8 E06F     		ldr	r0, [r4, #124]
 5135 01fa FFF7FEFF 		bl	HAL_DMA_Abort
 5136              	.LVL254:
2511:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 5137              		.loc 1 2511 5 is_stmt 1 view .LVU1862
 5138 01fe D4F88430 		ldr	r3, [r4, #132]
 5139 0202 43F01003 		orr	r3, r3, #16
 5140 0206 C4F88430 		str	r3, [r4, #132]
2512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5141              		.loc 1 2512 5 view .LVU1863
2512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5142              		.loc 1 2512 17 is_stmt 0 view .LVU1864
 5143 020a 0123     		movs	r3, #1
 5144 020c 84F88130 		strb	r3, [r4, #129]
2515:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5145              		.loc 1 2515 5 is_stmt 1 view .LVU1865
2515:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5146              		.loc 1 2515 5 view .LVU1866
 5147 0210 0023     		movs	r3, #0
 5148 0212 84F88030 		strb	r3, [r4, #128]
2515:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5149              		.loc 1 2515 5 view .LVU1867
2517:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 5150              		.loc 1 2517 5 view .LVU1868
2517:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 5151              		.loc 1 2517 12 is_stmt 0 view .LVU1869
 5152 0216 0CE0     		b	.L289
 5153              	.L313:
2522:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 5154              		.loc 1 2522 5 is_stmt 1 view .LVU1870
 5155 0218 2268     		ldr	r2, [r4]
 5156 021a 5368     		ldr	r3, [r2, #4]
 5157 021c 6FF30F03 		bfc	r3, #0, #16
 5158 0220 5360     		str	r3, [r2, #4]
 5159 0222 D1E7     		b	.L302
 5160              	.L314:
2541:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 5161              		.loc 1 2541 5 view .LVU1871
 5162 0224 2268     		ldr	r2, [r4]
 5163 0226 1368     		ldr	r3, [r2]
 5164 0228 43F40073 		orr	r3, r3, #512
 5165 022c 1360     		str	r3, [r2]
 5166 022e DEE7     		b	.L303
 5167              	.LVL255:
 5168              	.L304:
2389:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 5169              		.loc 1 2389 12 is_stmt 0 view .LVU1872
 5170 0230 0226     		movs	r6, #2
 5171              	.LVL256:
 5172              	.L289:
2548:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5173              		.loc 1 2548 1 view .LVU1873
 5174 0232 3046     		mov	r0, r6
 5175 0234 70BD     		pop	{r4, r5, r6, pc}
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 191


 5176              	.LVL257:
 5177              	.L305:
2398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5178              		.loc 1 2398 3 discriminator 1 view .LVU1874
 5179 0236 0226     		movs	r6, #2
 5180 0238 FBE7     		b	.L289
 5181              	.L316:
 5182 023a 00BF     		.align	2
 5183              	.L315:
 5184 023c 00000000 		.word	SPI_DMAHalfTransmitReceiveCplt
 5185 0240 00000000 		.word	SPI_DMATransmitReceiveCplt
 5186 0244 00000000 		.word	SPI_DMAError
 5187              		.cfi_endproc
 5188              	.LFE347:
 5190              		.section	.text.HAL_SPI_Abort,"ax",%progbits
 5191              		.align	1
 5192              		.global	HAL_SPI_Abort
 5193              		.syntax unified
 5194              		.thumb
 5195              		.thumb_func
 5197              	HAL_SPI_Abort:
 5198              	.LVL258:
 5199              	.LFB348:
2564:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
 5200              		.loc 1 2564 1 is_stmt 1 view -0
 5201              		.cfi_startproc
 5202              		@ args = 0, pretend = 0, frame = 8
 5203              		@ frame_needed = 0, uses_anonymous_args = 0
2565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5204              		.loc 1 2565 3 view .LVU1876
2567:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5205              		.loc 1 2567 3 view .LVU1877
2570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5206              		.loc 1 2570 3 view .LVU1878
2570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5207              		.loc 1 2570 3 view .LVU1879
 5208 0000 90F88030 		ldrb	r3, [r0, #128]	@ zero_extendqisi2
 5209 0004 012B     		cmp	r3, #1
 5210 0006 00F09A80 		beq	.L331
2564:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
 5211              		.loc 1 2564 1 is_stmt 0 view .LVU1880
 5212 000a 10B5     		push	{r4, lr}
 5213              		.cfi_def_cfa_offset 8
 5214              		.cfi_offset 4, -8
 5215              		.cfi_offset 14, -4
 5216 000c 82B0     		sub	sp, sp, #8
 5217              		.cfi_def_cfa_offset 16
 5218 000e 0446     		mov	r4, r0
2570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5219              		.loc 1 2570 3 is_stmt 1 discriminator 2 view .LVU1881
 5220 0010 0123     		movs	r3, #1
 5221 0012 80F88030 		strb	r3, [r0, #128]
2570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5222              		.loc 1 2570 3 view .LVU1882
2573:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5223              		.loc 1 2573 3 view .LVU1883
2573:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 192


 5224              		.loc 1 2573 15 is_stmt 0 view .LVU1884
 5225 0016 0723     		movs	r3, #7
 5226 0018 80F88130 		strb	r3, [r0, #129]
2576:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   count = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24UL / 1000UL);
 5227              		.loc 1 2576 3 is_stmt 1 view .LVU1885
 5228              	.LVL259:
2577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5229              		.loc 1 2577 3 view .LVU1886
2577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5230              		.loc 1 2577 57 is_stmt 0 view .LVU1887
 5231 001c 494B     		ldr	r3, .L342
 5232 001e 1B68     		ldr	r3, [r3]
 5233 0020 494A     		ldr	r2, .L342+4
 5234 0022 A2FB0323 		umull	r2, r3, r2, r3
 5235 0026 5B0A     		lsrs	r3, r3, #9
2577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5236              		.loc 1 2577 31 view .LVU1888
 5237 0028 6422     		movs	r2, #100
 5238 002a 02FB03F3 		mul	r3, r2, r3
2577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5239              		.loc 1 2577 9 view .LVU1889
 5240 002e 0193     		str	r3, [sp, #4]
2580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5241              		.loc 1 2580 3 is_stmt 1 view .LVU1890
2580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5242              		.loc 1 2580 7 is_stmt 0 view .LVU1891
 5243 0030 0368     		ldr	r3, [r0]
 5244 0032 1A68     		ldr	r2, [r3]
2580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5245              		.loc 1 2580 6 view .LVU1892
 5246 0034 12F4007F 		tst	r2, #512
 5247 0038 40D0     		beq	.L319
2583:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     do
 5248              		.loc 1 2583 5 is_stmt 1 view .LVU1893
 5249 003a 1A69     		ldr	r2, [r3, #16]
 5250 003c 22F00802 		bic	r2, r2, #8
 5251 0040 1A61     		str	r2, [r3, #16]
 5252              	.L322:
2584:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5253              		.loc 1 2584 5 view .LVU1894
2586:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
 5254              		.loc 1 2586 7 view .LVU1895
2586:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
 5255              		.loc 1 2586 12 is_stmt 0 view .LVU1896
 5256 0042 019B     		ldr	r3, [sp, #4]
 5257 0044 013B     		subs	r3, r3, #1
 5258 0046 0193     		str	r3, [sp, #4]
2587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5259              		.loc 1 2587 7 is_stmt 1 view .LVU1897
2587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5260              		.loc 1 2587 17 is_stmt 0 view .LVU1898
 5261 0048 019B     		ldr	r3, [sp, #4]
2587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5262              		.loc 1 2587 10 view .LVU1899
 5263 004a 2BB1     		cbz	r3, .L337
2592:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5264              		.loc 1 2592 14 is_stmt 1 view .LVU1900
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 193


 5265 004c 2368     		ldr	r3, [r4]
 5266 004e 1B69     		ldr	r3, [r3, #16]
 5267 0050 13F0080F 		tst	r3, #8
 5268 0054 F5D1     		bne	.L322
 5269 0056 05E0     		b	.L321
 5270              	.L337:
2589:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 5271              		.loc 1 2589 9 view .LVU1901
 5272 0058 D4F88430 		ldr	r3, [r4, #132]
 5273 005c 43F04003 		orr	r3, r3, #64
 5274 0060 C4F88430 		str	r3, [r4, #132]
2590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 5275              		.loc 1 2590 9 view .LVU1902
 5276              	.L321:
2595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     do
 5277              		.loc 1 2595 5 view .LVU1903
 5278 0064 2268     		ldr	r2, [r4]
 5279 0066 1368     		ldr	r3, [r2]
 5280 0068 43F48063 		orr	r3, r3, #1024
 5281 006c 1360     		str	r3, [r2]
 5282              	.L325:
2596:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5283              		.loc 1 2596 5 view .LVU1904
2598:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
 5284              		.loc 1 2598 7 view .LVU1905
2598:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
 5285              		.loc 1 2598 12 is_stmt 0 view .LVU1906
 5286 006e 019B     		ldr	r3, [sp, #4]
 5287 0070 013B     		subs	r3, r3, #1
 5288 0072 0193     		str	r3, [sp, #4]
2599:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5289              		.loc 1 2599 7 is_stmt 1 view .LVU1907
2599:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5290              		.loc 1 2599 17 is_stmt 0 view .LVU1908
 5291 0074 019B     		ldr	r3, [sp, #4]
2599:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5292              		.loc 1 2599 10 view .LVU1909
 5293 0076 2BB1     		cbz	r3, .L338
2604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5294              		.loc 1 2604 14 is_stmt 1 view .LVU1910
 5295 0078 2368     		ldr	r3, [r4]
 5296 007a 1B68     		ldr	r3, [r3]
 5297 007c 13F4007F 		tst	r3, #512
 5298 0080 F5D1     		bne	.L325
 5299 0082 05E0     		b	.L324
 5300              	.L338:
2601:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 5301              		.loc 1 2601 9 view .LVU1911
 5302 0084 D4F88430 		ldr	r3, [r4, #132]
 5303 0088 43F04003 		orr	r3, r3, #64
 5304 008c C4F88430 		str	r3, [r4, #132]
2602:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 5305              		.loc 1 2602 9 view .LVU1912
 5306              	.L324:
2607:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     do
 5307              		.loc 1 2607 5 view .LVU1913
 5308 0090 2268     		ldr	r2, [r4]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 194


 5309 0092 9369     		ldr	r3, [r2, #24]
 5310 0094 43F40063 		orr	r3, r3, #2048
 5311 0098 9361     		str	r3, [r2, #24]
 5312              	.L327:
2608:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5313              		.loc 1 2608 5 view .LVU1914
2610:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
 5314              		.loc 1 2610 7 view .LVU1915
2610:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
 5315              		.loc 1 2610 12 is_stmt 0 view .LVU1916
 5316 009a 019B     		ldr	r3, [sp, #4]
 5317 009c 013B     		subs	r3, r3, #1
 5318 009e 0193     		str	r3, [sp, #4]
2611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5319              		.loc 1 2611 7 is_stmt 1 view .LVU1917
2611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5320              		.loc 1 2611 17 is_stmt 0 view .LVU1918
 5321 00a0 019B     		ldr	r3, [sp, #4]
2611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5322              		.loc 1 2611 10 view .LVU1919
 5323 00a2 2BB1     		cbz	r3, .L339
2616:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 5324              		.loc 1 2616 14 is_stmt 1 view .LVU1920
 5325 00a4 2368     		ldr	r3, [r4]
 5326 00a6 5B69     		ldr	r3, [r3, #20]
 5327 00a8 13F4006F 		tst	r3, #2048
 5328 00ac F5D1     		bne	.L327
 5329 00ae 05E0     		b	.L319
 5330              	.L339:
2613:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 5331              		.loc 1 2613 9 view .LVU1921
 5332 00b0 D4F88430 		ldr	r3, [r4, #132]
 5333 00b4 43F04003 		orr	r3, r3, #64
 5334 00b8 C4F88430 		str	r3, [r4, #132]
2614:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 5335              		.loc 1 2614 9 view .LVU1922
 5336              	.L319:
2620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5337              		.loc 1 2620 3 view .LVU1923
2620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5338              		.loc 1 2620 7 is_stmt 0 view .LVU1924
 5339 00bc 2368     		ldr	r3, [r4]
 5340 00be 9B68     		ldr	r3, [r3, #8]
2620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5341              		.loc 1 2620 6 view .LVU1925
 5342 00c0 13F4004F 		tst	r3, #32768
 5343 00c4 07D0     		beq	.L328
2622:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5344              		.loc 1 2622 5 is_stmt 1 view .LVU1926
2622:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5345              		.loc 1 2622 13 is_stmt 0 view .LVU1927
 5346 00c6 A36F     		ldr	r3, [r4, #120]
2622:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5347              		.loc 1 2622 8 view .LVU1928
 5348 00c8 2BB1     		cbz	r3, .L328
2625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5349              		.loc 1 2625 7 is_stmt 1 view .LVU1929
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 195


2625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5350              		.loc 1 2625 39 is_stmt 0 view .LVU1930
 5351 00ca 0022     		movs	r2, #0
 5352 00cc 1A65     		str	r2, [r3, #80]
2628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5353              		.loc 1 2628 7 is_stmt 1 view .LVU1931
2628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5354              		.loc 1 2628 11 is_stmt 0 view .LVU1932
 5355 00ce A06F     		ldr	r0, [r4, #120]
 5356              	.LVL260:
2628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5357              		.loc 1 2628 11 view .LVU1933
 5358 00d0 FFF7FEFF 		bl	HAL_DMA_Abort
 5359              	.LVL261:
2628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5360              		.loc 1 2628 10 discriminator 1 view .LVU1934
 5361 00d4 F8B9     		cbnz	r0, .L340
 5362              	.L328:
2639:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5363              		.loc 1 2639 3 is_stmt 1 view .LVU1935
2639:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5364              		.loc 1 2639 7 is_stmt 0 view .LVU1936
 5365 00d6 2368     		ldr	r3, [r4]
 5366 00d8 9B68     		ldr	r3, [r3, #8]
2639:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5367              		.loc 1 2639 6 view .LVU1937
 5368 00da 13F4804F 		tst	r3, #16384
 5369 00de 07D0     		beq	.L329
2641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5370              		.loc 1 2641 5 is_stmt 1 view .LVU1938
2641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5371              		.loc 1 2641 13 is_stmt 0 view .LVU1939
 5372 00e0 E36F     		ldr	r3, [r4, #124]
2641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5373              		.loc 1 2641 8 view .LVU1940
 5374 00e2 2BB1     		cbz	r3, .L329
2644:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5375              		.loc 1 2644 7 is_stmt 1 view .LVU1941
2644:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5376              		.loc 1 2644 39 is_stmt 0 view .LVU1942
 5377 00e4 0022     		movs	r2, #0
 5378 00e6 1A65     		str	r2, [r3, #80]
2647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5379              		.loc 1 2647 7 is_stmt 1 view .LVU1943
2647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5380              		.loc 1 2647 11 is_stmt 0 view .LVU1944
 5381 00e8 E06F     		ldr	r0, [r4, #124]
 5382 00ea FFF7FEFF 		bl	HAL_DMA_Abort
 5383              	.LVL262:
2647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 5384              		.loc 1 2647 10 discriminator 1 view .LVU1945
 5385 00ee D8B9     		cbnz	r0, .L341
 5386              	.L329:
2658:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5387              		.loc 1 2658 3 is_stmt 1 view .LVU1946
 5388 00f0 2046     		mov	r0, r4
 5389 00f2 FFF7FEFF 		bl	SPI_AbortTransfer
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 196


 5390              	.LVL263:
2661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5391              		.loc 1 2661 3 view .LVU1947
2661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5392              		.loc 1 2661 7 is_stmt 0 view .LVU1948
 5393 00f6 D4F88430 		ldr	r3, [r4, #132]
2661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5394              		.loc 1 2661 6 view .LVU1949
 5395 00fa 13F0400F 		tst	r3, #64
 5396 00fe 1CD1     		bne	.L332
2669:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 5397              		.loc 1 2669 5 is_stmt 1 view .LVU1950
2669:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 5398              		.loc 1 2669 21 is_stmt 0 view .LVU1951
 5399 0100 0020     		movs	r0, #0
 5400 0102 C4F88400 		str	r0, [r4, #132]
 5401              	.L330:
 5402              	.LVL264:
2673:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5403              		.loc 1 2673 3 is_stmt 1 view .LVU1952
2673:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5404              		.loc 1 2673 15 is_stmt 0 view .LVU1953
 5405 0106 0123     		movs	r3, #1
 5406 0108 84F88130 		strb	r3, [r4, #129]
2676:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5407              		.loc 1 2676 3 is_stmt 1 view .LVU1954
2676:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5408              		.loc 1 2676 3 view .LVU1955
 5409 010c 0023     		movs	r3, #0
 5410 010e 84F88030 		strb	r3, [r4, #128]
2676:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5411              		.loc 1 2676 3 view .LVU1956
2678:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 5412              		.loc 1 2678 3 view .LVU1957
2679:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5413              		.loc 1 2679 1 is_stmt 0 view .LVU1958
 5414 0112 02B0     		add	sp, sp, #8
 5415              		.cfi_remember_state
 5416              		.cfi_def_cfa_offset 8
 5417              		@ sp needed
 5418 0114 10BD     		pop	{r4, pc}
 5419              	.LVL265:
 5420              	.L340:
 5421              		.cfi_restore_state
2630:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 5422              		.loc 1 2630 9 is_stmt 1 view .LVU1959
2630:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 5423              		.loc 1 2630 13 is_stmt 0 view .LVU1960
 5424 0116 A06F     		ldr	r0, [r4, #120]
 5425 0118 FFF7FEFF 		bl	HAL_DMA_GetError
 5426              	.LVL266:
2630:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 5427              		.loc 1 2630 12 discriminator 1 view .LVU1961
 5428 011c 2028     		cmp	r0, #32
 5429 011e DAD1     		bne	.L328
2632:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 5430              		.loc 1 2632 11 is_stmt 1 view .LVU1962
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 197


2632:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 5431              		.loc 1 2632 27 is_stmt 0 view .LVU1963
 5432 0120 4023     		movs	r3, #64
 5433 0122 C4F88430 		str	r3, [r4, #132]
 5434 0126 D6E7     		b	.L328
 5435              	.L341:
2649:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 5436              		.loc 1 2649 9 is_stmt 1 view .LVU1964
2649:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 5437              		.loc 1 2649 13 is_stmt 0 view .LVU1965
 5438 0128 E06F     		ldr	r0, [r4, #124]
 5439 012a FFF7FEFF 		bl	HAL_DMA_GetError
 5440              	.LVL267:
2649:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 5441              		.loc 1 2649 12 discriminator 1 view .LVU1966
 5442 012e 2028     		cmp	r0, #32
 5443 0130 DED1     		bne	.L329
2651:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 5444              		.loc 1 2651 11 is_stmt 1 view .LVU1967
2651:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 5445              		.loc 1 2651 27 is_stmt 0 view .LVU1968
 5446 0132 4023     		movs	r3, #64
 5447 0134 C4F88430 		str	r3, [r4, #132]
 5448 0138 DAE7     		b	.L329
 5449              	.L332:
2664:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 5450              		.loc 1 2664 15 view .LVU1969
 5451 013a 0120     		movs	r0, #1
 5452 013c E3E7     		b	.L330
 5453              	.LVL268:
 5454              	.L331:
 5455              		.cfi_def_cfa_offset 0
 5456              		.cfi_restore 4
 5457              		.cfi_restore 14
2570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5458              		.loc 1 2570 3 discriminator 1 view .LVU1970
 5459 013e 0220     		movs	r0, #2
 5460              	.LVL269:
2679:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5461              		.loc 1 2679 1 view .LVU1971
 5462 0140 7047     		bx	lr
 5463              	.L343:
 5464 0142 00BF     		.align	2
 5465              	.L342:
 5466 0144 00000000 		.word	SystemCoreClock
 5467 0148 F1197605 		.word	91625969
 5468              		.cfi_endproc
 5469              	.LFE348:
 5471              		.section	.text.HAL_SPI_DMAPause,"ax",%progbits
 5472              		.align	1
 5473              		.global	HAL_SPI_DMAPause
 5474              		.syntax unified
 5475              		.thumb
 5476              		.thumb_func
 5478              	HAL_SPI_DMAPause:
 5479              	.LVL270:
 5480              	.LFB350:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 198


2843:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set error code to not supported */
 5481              		.loc 1 2843 1 is_stmt 1 view -0
 5482              		.cfi_startproc
 5483              		@ args = 0, pretend = 0, frame = 0
 5484              		@ frame_needed = 0, uses_anonymous_args = 0
 5485              		@ link register save eliminated.
2845:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5486              		.loc 1 2845 3 view .LVU1973
 5487 0000 D0F88430 		ldr	r3, [r0, #132]
 5488 0004 43F48063 		orr	r3, r3, #1024
 5489 0008 C0F88430 		str	r3, [r0, #132]
2847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 5490              		.loc 1 2847 3 view .LVU1974
2848:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5491              		.loc 1 2848 1 is_stmt 0 view .LVU1975
 5492 000c 0120     		movs	r0, #1
 5493              	.LVL271:
2848:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5494              		.loc 1 2848 1 view .LVU1976
 5495 000e 7047     		bx	lr
 5496              		.cfi_endproc
 5497              	.LFE350:
 5499              		.section	.text.HAL_SPI_DMAResume,"ax",%progbits
 5500              		.align	1
 5501              		.global	HAL_SPI_DMAResume
 5502              		.syntax unified
 5503              		.thumb
 5504              		.thumb_func
 5506              	HAL_SPI_DMAResume:
 5507              	.LVL272:
 5508              	.LFB351:
2858:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set error code to not supported */
 5509              		.loc 1 2858 1 is_stmt 1 view -0
 5510              		.cfi_startproc
 5511              		@ args = 0, pretend = 0, frame = 0
 5512              		@ frame_needed = 0, uses_anonymous_args = 0
 5513              		@ link register save eliminated.
2860:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5514              		.loc 1 2860 3 view .LVU1978
 5515 0000 D0F88430 		ldr	r3, [r0, #132]
 5516 0004 43F48063 		orr	r3, r3, #1024
 5517 0008 C0F88430 		str	r3, [r0, #132]
2862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 5518              		.loc 1 2862 3 view .LVU1979
2863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5519              		.loc 1 2863 1 is_stmt 0 view .LVU1980
 5520 000c 0120     		movs	r0, #1
 5521              	.LVL273:
2863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5522              		.loc 1 2863 1 view .LVU1981
 5523 000e 7047     		bx	lr
 5524              		.cfi_endproc
 5525              	.LFE351:
 5527              		.section	.text.HAL_SPI_DMAStop,"ax",%progbits
 5528              		.align	1
 5529              		.global	HAL_SPI_DMAStop
 5530              		.syntax unified
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 199


 5531              		.thumb
 5532              		.thumb_func
 5534              	HAL_SPI_DMAStop:
 5535              	.LVL274:
 5536              	.LFB352:
2873:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Set error code to not supported */
 5537              		.loc 1 2873 1 is_stmt 1 view -0
 5538              		.cfi_startproc
 5539              		@ args = 0, pretend = 0, frame = 0
 5540              		@ frame_needed = 0, uses_anonymous_args = 0
 5541              		@ link register save eliminated.
2875:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5542              		.loc 1 2875 3 view .LVU1983
 5543 0000 D0F88430 		ldr	r3, [r0, #132]
 5544 0004 43F48063 		orr	r3, r3, #1024
 5545 0008 C0F88430 		str	r3, [r0, #132]
2877:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 5546              		.loc 1 2877 3 view .LVU1984
2878:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5547              		.loc 1 2878 1 is_stmt 0 view .LVU1985
 5548 000c 0120     		movs	r0, #1
 5549              	.LVL275:
2878:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5550              		.loc 1 2878 1 view .LVU1986
 5551 000e 7047     		bx	lr
 5552              		.cfi_endproc
 5553              	.LFE352:
 5555              		.section	.text.HAL_SPI_TxCpltCallback,"ax",%progbits
 5556              		.align	1
 5557              		.weak	HAL_SPI_TxCpltCallback
 5558              		.syntax unified
 5559              		.thumb
 5560              		.thumb_func
 5562              	HAL_SPI_TxCpltCallback:
 5563              	.LVL276:
 5564              	.LFB354:
3140:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5565              		.loc 1 3140 1 is_stmt 1 view -0
 5566              		.cfi_startproc
 5567              		@ args = 0, pretend = 0, frame = 0
 5568              		@ frame_needed = 0, uses_anonymous_args = 0
 5569              		@ link register save eliminated.
3142:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5570              		.loc 1 3142 3 view .LVU1988
3147:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5571              		.loc 1 3147 1 is_stmt 0 view .LVU1989
 5572 0000 7047     		bx	lr
 5573              		.cfi_endproc
 5574              	.LFE354:
 5576              		.section	.text.SPI_DMATransmitCplt,"ax",%progbits
 5577              		.align	1
 5578              		.syntax unified
 5579              		.thumb
 5580              		.thumb_func
 5582              	SPI_DMATransmitCplt:
 5583              	.LVL277:
 5584              	.LFB365:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 200


3341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 5585              		.loc 1 3341 1 is_stmt 1 view -0
 5586              		.cfi_startproc
 5587              		@ args = 0, pretend = 0, frame = 0
 5588              		@ frame_needed = 0, uses_anonymous_args = 0
3341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 5589              		.loc 1 3341 1 is_stmt 0 view .LVU1991
 5590 0000 08B5     		push	{r3, lr}
 5591              		.cfi_def_cfa_offset 8
 5592              		.cfi_offset 3, -8
 5593              		.cfi_offset 14, -4
3342:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5594              		.loc 1 3342 3 is_stmt 1 view .LVU1992
3342:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5595              		.loc 1 3342 22 is_stmt 0 view .LVU1993
 5596 0002 806B     		ldr	r0, [r0, #56]
 5597              	.LVL278:
3344:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5598              		.loc 1 3344 3 is_stmt 1 view .LVU1994
3344:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5599              		.loc 1 3344 11 is_stmt 0 view .LVU1995
 5600 0004 90F88130 		ldrb	r3, [r0, #129]	@ zero_extendqisi2
3344:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5601              		.loc 1 3344 6 view .LVU1996
 5602 0008 072B     		cmp	r3, #7
 5603 000a 09D0     		beq	.L348
3346:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5604              		.loc 1 3346 5 is_stmt 1 view .LVU1997
3346:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5605              		.loc 1 3346 13 is_stmt 0 view .LVU1998
 5606 000c 836F     		ldr	r3, [r0, #120]
3346:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5607              		.loc 1 3346 27 view .LVU1999
 5608 000e DB69     		ldr	r3, [r3, #28]
3346:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5609              		.loc 1 3346 8 view .LVU2000
 5610 0010 B3F5807F 		cmp	r3, #256
 5611 0014 05D0     		beq	.L352
3357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 5612              		.loc 1 3357 7 is_stmt 1 view .LVU2001
 5613 0016 0268     		ldr	r2, [r0]
 5614 0018 1369     		ldr	r3, [r2, #16]
 5615 001a 43F00803 		orr	r3, r3, #8
 5616 001e 1361     		str	r3, [r2, #16]
 5617              	.LVL279:
 5618              	.L348:
3360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5619              		.loc 1 3360 1 is_stmt 0 view .LVU2002
 5620 0020 08BD     		pop	{r3, pc}
 5621              	.LVL280:
 5622              	.L352:
3351:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5623              		.loc 1 3351 7 is_stmt 1 view .LVU2003
 5624 0022 FFF7FEFF 		bl	HAL_SPI_TxCpltCallback
 5625              	.LVL281:
3351:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5626              		.loc 1 3351 7 is_stmt 0 view .LVU2004
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 201


 5627 0026 FBE7     		b	.L348
 5628              		.cfi_endproc
 5629              	.LFE365:
 5631              		.section	.text.HAL_SPI_RxCpltCallback,"ax",%progbits
 5632              		.align	1
 5633              		.weak	HAL_SPI_RxCpltCallback
 5634              		.syntax unified
 5635              		.thumb
 5636              		.thumb_func
 5638              	HAL_SPI_RxCpltCallback:
 5639              	.LVL282:
 5640              	.LFB355:
3156:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5641              		.loc 1 3156 1 is_stmt 1 view -0
 5642              		.cfi_startproc
 5643              		@ args = 0, pretend = 0, frame = 0
 5644              		@ frame_needed = 0, uses_anonymous_args = 0
 5645              		@ link register save eliminated.
3158:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5646              		.loc 1 3158 3 view .LVU2006
3163:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5647              		.loc 1 3163 1 is_stmt 0 view .LVU2007
 5648 0000 7047     		bx	lr
 5649              		.cfi_endproc
 5650              	.LFE355:
 5652              		.section	.text.SPI_DMAReceiveCplt,"ax",%progbits
 5653              		.align	1
 5654              		.syntax unified
 5655              		.thumb
 5656              		.thumb_func
 5658              	SPI_DMAReceiveCplt:
 5659              	.LVL283:
 5660              	.LFB366:
3369:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 5661              		.loc 1 3369 1 is_stmt 1 view -0
 5662              		.cfi_startproc
 5663              		@ args = 0, pretend = 0, frame = 0
 5664              		@ frame_needed = 0, uses_anonymous_args = 0
3369:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 5665              		.loc 1 3369 1 is_stmt 0 view .LVU2009
 5666 0000 08B5     		push	{r3, lr}
 5667              		.cfi_def_cfa_offset 8
 5668              		.cfi_offset 3, -8
 5669              		.cfi_offset 14, -4
3370:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5670              		.loc 1 3370 3 is_stmt 1 view .LVU2010
3370:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5671              		.loc 1 3370 22 is_stmt 0 view .LVU2011
 5672 0002 806B     		ldr	r0, [r0, #56]
 5673              	.LVL284:
3372:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5674              		.loc 1 3372 3 is_stmt 1 view .LVU2012
3372:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5675              		.loc 1 3372 11 is_stmt 0 view .LVU2013
 5676 0004 90F88130 		ldrb	r3, [r0, #129]	@ zero_extendqisi2
3372:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5677              		.loc 1 3372 6 view .LVU2014
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 202


 5678 0008 072B     		cmp	r3, #7
 5679 000a 09D0     		beq	.L354
3374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5680              		.loc 1 3374 5 is_stmt 1 view .LVU2015
3374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5681              		.loc 1 3374 13 is_stmt 0 view .LVU2016
 5682 000c C36F     		ldr	r3, [r0, #124]
3374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5683              		.loc 1 3374 27 view .LVU2017
 5684 000e DB69     		ldr	r3, [r3, #28]
3374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5685              		.loc 1 3374 8 view .LVU2018
 5686 0010 B3F5807F 		cmp	r3, #256
 5687 0014 05D0     		beq	.L358
3385:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 5688              		.loc 1 3385 7 is_stmt 1 view .LVU2019
 5689 0016 0268     		ldr	r2, [r0]
 5690 0018 1369     		ldr	r3, [r2, #16]
 5691 001a 43F00803 		orr	r3, r3, #8
 5692 001e 1361     		str	r3, [r2, #16]
 5693              	.LVL285:
 5694              	.L354:
3388:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5695              		.loc 1 3388 1 is_stmt 0 view .LVU2020
 5696 0020 08BD     		pop	{r3, pc}
 5697              	.LVL286:
 5698              	.L358:
3379:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5699              		.loc 1 3379 7 is_stmt 1 view .LVU2021
 5700 0022 FFF7FEFF 		bl	HAL_SPI_RxCpltCallback
 5701              	.LVL287:
3379:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5702              		.loc 1 3379 7 is_stmt 0 view .LVU2022
 5703 0026 FBE7     		b	.L354
 5704              		.cfi_endproc
 5705              	.LFE366:
 5707              		.section	.text.HAL_SPI_TxRxCpltCallback,"ax",%progbits
 5708              		.align	1
 5709              		.weak	HAL_SPI_TxRxCpltCallback
 5710              		.syntax unified
 5711              		.thumb
 5712              		.thumb_func
 5714              	HAL_SPI_TxRxCpltCallback:
 5715              	.LVL288:
 5716              	.LFB356:
3172:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5717              		.loc 1 3172 1 is_stmt 1 view -0
 5718              		.cfi_startproc
 5719              		@ args = 0, pretend = 0, frame = 0
 5720              		@ frame_needed = 0, uses_anonymous_args = 0
 5721              		@ link register save eliminated.
3174:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5722              		.loc 1 3174 3 view .LVU2024
3179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5723              		.loc 1 3179 1 is_stmt 0 view .LVU2025
 5724 0000 7047     		bx	lr
 5725              		.cfi_endproc
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 203


 5726              	.LFE356:
 5728              		.section	.text.SPI_DMATransmitReceiveCplt,"ax",%progbits
 5729              		.align	1
 5730              		.syntax unified
 5731              		.thumb
 5732              		.thumb_func
 5734              	SPI_DMATransmitReceiveCplt:
 5735              	.LVL289:
 5736              	.LFB367:
3397:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 5737              		.loc 1 3397 1 is_stmt 1 view -0
 5738              		.cfi_startproc
 5739              		@ args = 0, pretend = 0, frame = 0
 5740              		@ frame_needed = 0, uses_anonymous_args = 0
3397:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 5741              		.loc 1 3397 1 is_stmt 0 view .LVU2027
 5742 0000 08B5     		push	{r3, lr}
 5743              		.cfi_def_cfa_offset 8
 5744              		.cfi_offset 3, -8
 5745              		.cfi_offset 14, -4
3398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5746              		.loc 1 3398 3 is_stmt 1 view .LVU2028
3398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5747              		.loc 1 3398 22 is_stmt 0 view .LVU2029
 5748 0002 806B     		ldr	r0, [r0, #56]
 5749              	.LVL290:
3400:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5750              		.loc 1 3400 3 is_stmt 1 view .LVU2030
3400:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5751              		.loc 1 3400 11 is_stmt 0 view .LVU2031
 5752 0004 90F88130 		ldrb	r3, [r0, #129]	@ zero_extendqisi2
3400:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5753              		.loc 1 3400 6 view .LVU2032
 5754 0008 072B     		cmp	r3, #7
 5755 000a 09D0     		beq	.L360
3402:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5756              		.loc 1 3402 5 is_stmt 1 view .LVU2033
3402:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5757              		.loc 1 3402 13 is_stmt 0 view .LVU2034
 5758 000c 836F     		ldr	r3, [r0, #120]
3402:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5759              		.loc 1 3402 27 view .LVU2035
 5760 000e DB69     		ldr	r3, [r3, #28]
3402:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 5761              		.loc 1 3402 8 view .LVU2036
 5762 0010 B3F5807F 		cmp	r3, #256
 5763 0014 05D0     		beq	.L364
3413:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 5764              		.loc 1 3413 7 is_stmt 1 view .LVU2037
 5765 0016 0268     		ldr	r2, [r0]
 5766 0018 1369     		ldr	r3, [r2, #16]
 5767 001a 43F00803 		orr	r3, r3, #8
 5768 001e 1361     		str	r3, [r2, #16]
 5769              	.LVL291:
 5770              	.L360:
3416:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5771              		.loc 1 3416 1 is_stmt 0 view .LVU2038
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 204


 5772 0020 08BD     		pop	{r3, pc}
 5773              	.LVL292:
 5774              	.L364:
3407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5775              		.loc 1 3407 7 is_stmt 1 view .LVU2039
 5776 0022 FFF7FEFF 		bl	HAL_SPI_TxRxCpltCallback
 5777              	.LVL293:
3407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5778              		.loc 1 3407 7 is_stmt 0 view .LVU2040
 5779 0026 FBE7     		b	.L360
 5780              		.cfi_endproc
 5781              	.LFE367:
 5783              		.section	.text.HAL_SPI_TxHalfCpltCallback,"ax",%progbits
 5784              		.align	1
 5785              		.weak	HAL_SPI_TxHalfCpltCallback
 5786              		.syntax unified
 5787              		.thumb
 5788              		.thumb_func
 5790              	HAL_SPI_TxHalfCpltCallback:
 5791              	.LVL294:
 5792              	.LFB357:
3188:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5793              		.loc 1 3188 1 is_stmt 1 view -0
 5794              		.cfi_startproc
 5795              		@ args = 0, pretend = 0, frame = 0
 5796              		@ frame_needed = 0, uses_anonymous_args = 0
 5797              		@ link register save eliminated.
3190:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5798              		.loc 1 3190 3 view .LVU2042
3195:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5799              		.loc 1 3195 1 is_stmt 0 view .LVU2043
 5800 0000 7047     		bx	lr
 5801              		.cfi_endproc
 5802              	.LFE357:
 5804              		.section	.text.SPI_DMAHalfTransmitCplt,"ax",%progbits
 5805              		.align	1
 5806              		.syntax unified
 5807              		.thumb
 5808              		.thumb_func
 5810              	SPI_DMAHalfTransmitCplt:
 5811              	.LVL295:
 5812              	.LFB368:
3425:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)
 5813              		.loc 1 3425 1 is_stmt 1 view -0
 5814              		.cfi_startproc
 5815              		@ args = 0, pretend = 0, frame = 0
 5816              		@ frame_needed = 0, uses_anonymous_args = 0
3425:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)
 5817              		.loc 1 3425 1 is_stmt 0 view .LVU2045
 5818 0000 08B5     		push	{r3, lr}
 5819              		.cfi_def_cfa_offset 8
 5820              		.cfi_offset 3, -8
 5821              		.cfi_offset 14, -4
3426:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                             ((DMA_HandleTypeDef *)hdma)->Parent; /* Derogation MISRAC2012-Rule-8.13
 5822              		.loc 1 3426 3 is_stmt 1 view .LVU2046
 5823              	.LVL296:
3432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 205


 5824              		.loc 1 3432 3 view .LVU2047
 5825 0002 806B     		ldr	r0, [r0, #56]
 5826              	.LVL297:
3432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5827              		.loc 1 3432 3 is_stmt 0 view .LVU2048
 5828 0004 FFF7FEFF 		bl	HAL_SPI_TxHalfCpltCallback
 5829              	.LVL298:
3434:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5830              		.loc 1 3434 1 view .LVU2049
 5831 0008 08BD     		pop	{r3, pc}
 5832              		.cfi_endproc
 5833              	.LFE368:
 5835              		.section	.text.HAL_SPI_RxHalfCpltCallback,"ax",%progbits
 5836              		.align	1
 5837              		.weak	HAL_SPI_RxHalfCpltCallback
 5838              		.syntax unified
 5839              		.thumb
 5840              		.thumb_func
 5842              	HAL_SPI_RxHalfCpltCallback:
 5843              	.LVL299:
 5844              	.LFB358:
3204:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5845              		.loc 1 3204 1 is_stmt 1 view -0
 5846              		.cfi_startproc
 5847              		@ args = 0, pretend = 0, frame = 0
 5848              		@ frame_needed = 0, uses_anonymous_args = 0
 5849              		@ link register save eliminated.
3206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5850              		.loc 1 3206 3 view .LVU2051
3211:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5851              		.loc 1 3211 1 is_stmt 0 view .LVU2052
 5852 0000 7047     		bx	lr
 5853              		.cfi_endproc
 5854              	.LFE358:
 5856              		.section	.text.SPI_DMAHalfReceiveCplt,"ax",%progbits
 5857              		.align	1
 5858              		.syntax unified
 5859              		.thumb
 5860              		.thumb_func
 5862              	SPI_DMAHalfReceiveCplt:
 5863              	.LVL300:
 5864              	.LFB369:
3443:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)
 5865              		.loc 1 3443 1 is_stmt 1 view -0
 5866              		.cfi_startproc
 5867              		@ args = 0, pretend = 0, frame = 0
 5868              		@ frame_needed = 0, uses_anonymous_args = 0
3443:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)
 5869              		.loc 1 3443 1 is_stmt 0 view .LVU2054
 5870 0000 08B5     		push	{r3, lr}
 5871              		.cfi_def_cfa_offset 8
 5872              		.cfi_offset 3, -8
 5873              		.cfi_offset 14, -4
3444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                             ((DMA_HandleTypeDef *)hdma)->Parent; /* Derogation MISRAC2012-Rule-8.13
 5874              		.loc 1 3444 3 is_stmt 1 view .LVU2055
 5875              	.LVL301:
3450:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 206


 5876              		.loc 1 3450 3 view .LVU2056
 5877 0002 806B     		ldr	r0, [r0, #56]
 5878              	.LVL302:
3450:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5879              		.loc 1 3450 3 is_stmt 0 view .LVU2057
 5880 0004 FFF7FEFF 		bl	HAL_SPI_RxHalfCpltCallback
 5881              	.LVL303:
3452:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5882              		.loc 1 3452 1 view .LVU2058
 5883 0008 08BD     		pop	{r3, pc}
 5884              		.cfi_endproc
 5885              	.LFE369:
 5887              		.section	.text.HAL_SPI_TxRxHalfCpltCallback,"ax",%progbits
 5888              		.align	1
 5889              		.weak	HAL_SPI_TxRxHalfCpltCallback
 5890              		.syntax unified
 5891              		.thumb
 5892              		.thumb_func
 5894              	HAL_SPI_TxRxHalfCpltCallback:
 5895              	.LVL304:
 5896              	.LFB359:
3220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5897              		.loc 1 3220 1 is_stmt 1 view -0
 5898              		.cfi_startproc
 5899              		@ args = 0, pretend = 0, frame = 0
 5900              		@ frame_needed = 0, uses_anonymous_args = 0
 5901              		@ link register save eliminated.
3222:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5902              		.loc 1 3222 3 view .LVU2060
3227:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5903              		.loc 1 3227 1 is_stmt 0 view .LVU2061
 5904 0000 7047     		bx	lr
 5905              		.cfi_endproc
 5906              	.LFE359:
 5908              		.section	.text.SPI_DMAHalfTransmitReceiveCplt,"ax",%progbits
 5909              		.align	1
 5910              		.syntax unified
 5911              		.thumb
 5912              		.thumb_func
 5914              	SPI_DMAHalfTransmitReceiveCplt:
 5915              	.LVL305:
 5916              	.LFB370:
3461:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)
 5917              		.loc 1 3461 1 is_stmt 1 view -0
 5918              		.cfi_startproc
 5919              		@ args = 0, pretend = 0, frame = 0
 5920              		@ frame_needed = 0, uses_anonymous_args = 0
3461:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)
 5921              		.loc 1 3461 1 is_stmt 0 view .LVU2063
 5922 0000 08B5     		push	{r3, lr}
 5923              		.cfi_def_cfa_offset 8
 5924              		.cfi_offset 3, -8
 5925              		.cfi_offset 14, -4
3462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                             ((DMA_HandleTypeDef *)hdma)->Parent; /* Derogation MISRAC2012-Rule-8.13
 5926              		.loc 1 3462 3 is_stmt 1 view .LVU2064
 5927              	.LVL306:
3468:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 207


 5928              		.loc 1 3468 3 view .LVU2065
 5929 0002 806B     		ldr	r0, [r0, #56]
 5930              	.LVL307:
3468:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5931              		.loc 1 3468 3 is_stmt 0 view .LVU2066
 5932 0004 FFF7FEFF 		bl	HAL_SPI_TxRxHalfCpltCallback
 5933              	.LVL308:
3470:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5934              		.loc 1 3470 1 view .LVU2067
 5935 0008 08BD     		pop	{r3, pc}
 5936              		.cfi_endproc
 5937              	.LFE370:
 5939              		.section	.text.HAL_SPI_ErrorCallback,"ax",%progbits
 5940              		.align	1
 5941              		.weak	HAL_SPI_ErrorCallback
 5942              		.syntax unified
 5943              		.thumb
 5944              		.thumb_func
 5946              	HAL_SPI_ErrorCallback:
 5947              	.LVL309:
 5948              	.LFB360:
3236:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5949              		.loc 1 3236 1 is_stmt 1 view -0
 5950              		.cfi_startproc
 5951              		@ args = 0, pretend = 0, frame = 0
 5952              		@ frame_needed = 0, uses_anonymous_args = 0
 5953              		@ link register save eliminated.
3238:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5954              		.loc 1 3238 3 view .LVU2069
3246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5955              		.loc 1 3246 1 is_stmt 0 view .LVU2070
 5956 0000 7047     		bx	lr
 5957              		.cfi_endproc
 5958              	.LFE360:
 5960              		.section	.text.SPI_DMAError,"ax",%progbits
 5961              		.align	1
 5962              		.syntax unified
 5963              		.thumb
 5964              		.thumb_func
 5966              	SPI_DMAError:
 5967              	.LVL310:
 5968              	.LFB371:
3479:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 5969              		.loc 1 3479 1 is_stmt 1 view -0
 5970              		.cfi_startproc
 5971              		@ args = 0, pretend = 0, frame = 0
 5972              		@ frame_needed = 0, uses_anonymous_args = 0
3479:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 5973              		.loc 1 3479 1 is_stmt 0 view .LVU2072
 5974 0000 10B5     		push	{r4, lr}
 5975              		.cfi_def_cfa_offset 8
 5976              		.cfi_offset 4, -8
 5977              		.cfi_offset 14, -4
3480:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5978              		.loc 1 3480 3 is_stmt 1 view .LVU2073
3480:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5979              		.loc 1 3480 22 is_stmt 0 view .LVU2074
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 208


 5980 0002 846B     		ldr	r4, [r0, #56]
 5981              	.LVL311:
3483:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5982              		.loc 1 3483 3 is_stmt 1 view .LVU2075
3483:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5983              		.loc 1 3483 7 is_stmt 0 view .LVU2076
 5984 0004 FFF7FEFF 		bl	HAL_DMA_GetError
 5985              	.LVL312:
3483:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 5986              		.loc 1 3483 6 discriminator 1 view .LVU2077
 5987 0008 0228     		cmp	r0, #2
 5988 000a 00D1     		bne	.L378
 5989              	.L375:
3496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5990              		.loc 1 3496 1 view .LVU2078
 5991 000c 10BD     		pop	{r4, pc}
 5992              	.LVL313:
 5993              	.L378:
3486:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 5994              		.loc 1 3486 5 is_stmt 1 view .LVU2079
 5995 000e 2046     		mov	r0, r4
 5996 0010 FFF7FEFF 		bl	SPI_CloseTransfer
 5997              	.LVL314:
3488:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 5998              		.loc 1 3488 5 view .LVU2080
 5999 0014 D4F88430 		ldr	r3, [r4, #132]
 6000 0018 43F01003 		orr	r3, r3, #16
 6001 001c C4F88430 		str	r3, [r4, #132]
3489:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
 6002              		.loc 1 3489 5 view .LVU2081
3489:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1UL)
 6003              		.loc 1 3489 17 is_stmt 0 view .LVU2082
 6004 0020 0123     		movs	r3, #1
 6005 0022 84F88130 		strb	r3, [r4, #129]
3493:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6006              		.loc 1 3493 5 is_stmt 1 view .LVU2083
 6007 0026 2046     		mov	r0, r4
 6008 0028 FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6009              	.LVL315:
3496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6010              		.loc 1 3496 1 is_stmt 0 view .LVU2084
 6011 002c EEE7     		b	.L375
 6012              		.cfi_endproc
 6013              	.LFE371:
 6015              		.section	.text.SPI_DMAAbortOnError,"ax",%progbits
 6016              		.align	1
 6017              		.syntax unified
 6018              		.thumb
 6019              		.thumb_func
 6021              	SPI_DMAAbortOnError:
 6022              	.LVL316:
 6023              	.LFB372:
3505:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 6024              		.loc 1 3505 1 is_stmt 1 view -0
 6025              		.cfi_startproc
 6026              		@ args = 0, pretend = 0, frame = 0
 6027              		@ frame_needed = 0, uses_anonymous_args = 0
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 209


3505:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 6028              		.loc 1 3505 1 is_stmt 0 view .LVU2086
 6029 0000 08B5     		push	{r3, lr}
 6030              		.cfi_def_cfa_offset 8
 6031              		.cfi_offset 3, -8
 6032              		.cfi_offset 14, -4
3506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t) 0UL;
 6033              		.loc 1 3506 3 is_stmt 1 view .LVU2087
3506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->RxXferCount = (uint16_t) 0UL;
 6034              		.loc 1 3506 22 is_stmt 0 view .LVU2088
 6035 0002 806B     		ldr	r0, [r0, #56]
 6036              	.LVL317:
3507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t) 0UL;
 6037              		.loc 1 3507 3 is_stmt 1 view .LVU2089
3507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   hspi->TxXferCount = (uint16_t) 0UL;
 6038              		.loc 1 3507 21 is_stmt 0 view .LVU2090
 6039 0004 0023     		movs	r3, #0
 6040 0006 A0F86A30 		strh	r3, [r0, #106]	@ movhi
3508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6041              		.loc 1 3508 3 is_stmt 1 view .LVU2091
3508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6042              		.loc 1 3508 21 is_stmt 0 view .LVU2092
 6043 000a A0F86230 		strh	r3, [r0, #98]	@ movhi
3511:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6044              		.loc 1 3511 3 is_stmt 1 view .LVU2093
3511:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6045              		.loc 1 3511 15 is_stmt 0 view .LVU2094
 6046 000e 0123     		movs	r3, #1
 6047 0010 80F88130 		strb	r3, [r0, #129]
3516:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6048              		.loc 1 3516 3 is_stmt 1 view .LVU2095
 6049 0014 FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6050              	.LVL318:
3518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6051              		.loc 1 3518 1 is_stmt 0 view .LVU2096
 6052 0018 08BD     		pop	{r3, pc}
 6053              		.cfi_endproc
 6054              	.LFE372:
 6056              		.section	.text.HAL_SPI_AbortCpltCallback,"ax",%progbits
 6057              		.align	1
 6058              		.weak	HAL_SPI_AbortCpltCallback
 6059              		.syntax unified
 6060              		.thumb
 6061              		.thumb_func
 6063              	HAL_SPI_AbortCpltCallback:
 6064              	.LVL319:
 6065              	.LFB361:
3254:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 6066              		.loc 1 3254 1 is_stmt 1 view -0
 6067              		.cfi_startproc
 6068              		@ args = 0, pretend = 0, frame = 0
 6069              		@ frame_needed = 0, uses_anonymous_args = 0
 6070              		@ link register save eliminated.
3256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6071              		.loc 1 3256 3 view .LVU2098
3261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6072              		.loc 1 3261 1 is_stmt 0 view .LVU2099
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 210


 6073 0000 7047     		bx	lr
 6074              		.cfi_endproc
 6075              	.LFE361:
 6077              		.section	.text.HAL_SPI_Abort_IT,"ax",%progbits
 6078              		.align	1
 6079              		.global	HAL_SPI_Abort_IT
 6080              		.syntax unified
 6081              		.thumb
 6082              		.thumb_func
 6084              	HAL_SPI_Abort_IT:
 6085              	.LVL320:
 6086              	.LFB349:
2697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
 6087              		.loc 1 2697 1 is_stmt 1 view -0
 6088              		.cfi_startproc
 6089              		@ args = 0, pretend = 0, frame = 8
 6090              		@ frame_needed = 0, uses_anonymous_args = 0
2697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
 6091              		.loc 1 2697 1 is_stmt 0 view .LVU2101
 6092 0000 30B5     		push	{r4, r5, lr}
 6093              		.cfi_def_cfa_offset 12
 6094              		.cfi_offset 4, -12
 6095              		.cfi_offset 5, -8
 6096              		.cfi_offset 14, -4
 6097 0002 83B0     		sub	sp, sp, #12
 6098              		.cfi_def_cfa_offset 24
 6099 0004 0446     		mov	r4, r0
2698:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   __IO uint32_t count;
 6100              		.loc 1 2698 3 is_stmt 1 view .LVU2102
2699:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t dma_tx_abort_done = 1UL;
 6101              		.loc 1 2699 3 view .LVU2103
2700:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t dma_rx_abort_done = 1UL;
 6102              		.loc 1 2700 3 view .LVU2104
 6103              	.LVL321:
2701:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6104              		.loc 1 2701 3 view .LVU2105
2704:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6105              		.loc 1 2704 3 view .LVU2106
2704:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6106              		.loc 1 2704 15 is_stmt 0 view .LVU2107
 6107 0006 0723     		movs	r3, #7
 6108 0008 80F88130 		strb	r3, [r0, #129]
2707:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   count = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24UL / 1000UL);
 6109              		.loc 1 2707 3 is_stmt 1 view .LVU2108
 6110              	.LVL322:
2708:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6111              		.loc 1 2708 3 view .LVU2109
2708:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6112              		.loc 1 2708 57 is_stmt 0 view .LVU2110
 6113 000c 554B     		ldr	r3, .L417
 6114 000e 1B68     		ldr	r3, [r3]
 6115 0010 554A     		ldr	r2, .L417+4
 6116 0012 A2FB0323 		umull	r2, r3, r2, r3
 6117 0016 5B0A     		lsrs	r3, r3, #9
2708:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6118              		.loc 1 2708 31 view .LVU2111
 6119 0018 6422     		movs	r2, #100
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 211


 6120 001a 02FB03F3 		mul	r3, r2, r3
2708:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6121              		.loc 1 2708 9 view .LVU2112
 6122 001e 0193     		str	r3, [sp, #4]
2711:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6123              		.loc 1 2711 3 is_stmt 1 view .LVU2113
2711:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6124              		.loc 1 2711 7 is_stmt 0 view .LVU2114
 6125 0020 0368     		ldr	r3, [r0]
 6126 0022 1A68     		ldr	r2, [r3]
2711:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6127              		.loc 1 2711 6 view .LVU2115
 6128 0024 12F4007F 		tst	r2, #512
 6129 0028 40D0     		beq	.L383
2714:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     do
 6130              		.loc 1 2714 5 is_stmt 1 view .LVU2116
 6131 002a 1A69     		ldr	r2, [r3, #16]
 6132 002c 22F00802 		bic	r2, r2, #8
 6133 0030 1A61     		str	r2, [r3, #16]
 6134              	.L386:
2715:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6135              		.loc 1 2715 5 view .LVU2117
2717:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
 6136              		.loc 1 2717 7 view .LVU2118
2717:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
 6137              		.loc 1 2717 12 is_stmt 0 view .LVU2119
 6138 0032 019B     		ldr	r3, [sp, #4]
 6139 0034 013B     		subs	r3, r3, #1
 6140 0036 0193     		str	r3, [sp, #4]
2718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6141              		.loc 1 2718 7 is_stmt 1 view .LVU2120
2718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6142              		.loc 1 2718 17 is_stmt 0 view .LVU2121
 6143 0038 019B     		ldr	r3, [sp, #4]
2718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6144              		.loc 1 2718 10 view .LVU2122
 6145 003a 2BB1     		cbz	r3, .L407
2723:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6146              		.loc 1 2723 14 is_stmt 1 view .LVU2123
 6147 003c 2368     		ldr	r3, [r4]
 6148 003e 1B69     		ldr	r3, [r3, #16]
 6149 0040 13F0080F 		tst	r3, #8
 6150 0044 F5D1     		bne	.L386
 6151 0046 05E0     		b	.L385
 6152              	.L407:
2720:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 6153              		.loc 1 2720 9 view .LVU2124
 6154 0048 D4F88430 		ldr	r3, [r4, #132]
 6155 004c 43F04003 		orr	r3, r3, #64
 6156 0050 C4F88430 		str	r3, [r4, #132]
2721:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 6157              		.loc 1 2721 9 view .LVU2125
 6158              	.L385:
2726:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     do
 6159              		.loc 1 2726 5 view .LVU2126
 6160 0054 2268     		ldr	r2, [r4]
 6161 0056 1368     		ldr	r3, [r2]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 212


 6162 0058 43F48063 		orr	r3, r3, #1024
 6163 005c 1360     		str	r3, [r2]
 6164              	.L389:
2727:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6165              		.loc 1 2727 5 view .LVU2127
2729:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
 6166              		.loc 1 2729 7 view .LVU2128
2729:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
 6167              		.loc 1 2729 12 is_stmt 0 view .LVU2129
 6168 005e 019B     		ldr	r3, [sp, #4]
 6169 0060 013B     		subs	r3, r3, #1
 6170 0062 0193     		str	r3, [sp, #4]
2730:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6171              		.loc 1 2730 7 is_stmt 1 view .LVU2130
2730:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6172              		.loc 1 2730 17 is_stmt 0 view .LVU2131
 6173 0064 019B     		ldr	r3, [sp, #4]
2730:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6174              		.loc 1 2730 10 view .LVU2132
 6175 0066 2BB1     		cbz	r3, .L408
2735:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6176              		.loc 1 2735 14 is_stmt 1 view .LVU2133
 6177 0068 2368     		ldr	r3, [r4]
 6178 006a 1B68     		ldr	r3, [r3]
 6179 006c 13F4007F 		tst	r3, #512
 6180 0070 F5D1     		bne	.L389
 6181 0072 05E0     		b	.L388
 6182              	.L408:
2732:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 6183              		.loc 1 2732 9 view .LVU2134
 6184 0074 D4F88430 		ldr	r3, [r4, #132]
 6185 0078 43F04003 		orr	r3, r3, #64
 6186 007c C4F88430 		str	r3, [r4, #132]
2733:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 6187              		.loc 1 2733 9 view .LVU2135
 6188              	.L388:
2738:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     do
 6189              		.loc 1 2738 5 view .LVU2136
 6190 0080 2268     		ldr	r2, [r4]
 6191 0082 9369     		ldr	r3, [r2, #24]
 6192 0084 43F40063 		orr	r3, r3, #2048
 6193 0088 9361     		str	r3, [r2, #24]
 6194              	.L391:
2739:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6195              		.loc 1 2739 5 view .LVU2137
2741:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
 6196              		.loc 1 2741 7 view .LVU2138
2741:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       if (count == 0UL)
 6197              		.loc 1 2741 12 is_stmt 0 view .LVU2139
 6198 008a 019B     		ldr	r3, [sp, #4]
 6199 008c 013B     		subs	r3, r3, #1
 6200 008e 0193     		str	r3, [sp, #4]
2742:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6201              		.loc 1 2742 7 is_stmt 1 view .LVU2140
2742:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6202              		.loc 1 2742 17 is_stmt 0 view .LVU2141
 6203 0090 019B     		ldr	r3, [sp, #4]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 213


2742:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6204              		.loc 1 2742 10 view .LVU2142
 6205 0092 2BB1     		cbz	r3, .L409
2747:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 6206              		.loc 1 2747 14 is_stmt 1 view .LVU2143
 6207 0094 2368     		ldr	r3, [r4]
 6208 0096 5B69     		ldr	r3, [r3, #20]
 6209 0098 13F4006F 		tst	r3, #2048
 6210 009c F5D1     		bne	.L391
 6211 009e 05E0     		b	.L383
 6212              	.L409:
2744:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         break;
 6213              		.loc 1 2744 9 view .LVU2144
 6214 00a0 D4F88430 		ldr	r3, [r4, #132]
 6215 00a4 43F04003 		orr	r3, r3, #64
 6216 00a8 C4F88430 		str	r3, [r4, #132]
2745:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 6217              		.loc 1 2745 9 view .LVU2145
 6218              	.L383:
2753:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6219              		.loc 1 2753 3 view .LVU2146
2753:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6220              		.loc 1 2753 11 is_stmt 0 view .LVU2147
 6221 00ac A36F     		ldr	r3, [r4, #120]
2753:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6222              		.loc 1 2753 6 view .LVU2148
 6223 00ae 63B3     		cbz	r3, .L398
2755:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6224              		.loc 1 2755 5 is_stmt 1 view .LVU2149
2755:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6225              		.loc 1 2755 9 is_stmt 0 view .LVU2150
 6226 00b0 2268     		ldr	r2, [r4]
 6227 00b2 9268     		ldr	r2, [r2, #8]
2755:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6228              		.loc 1 2755 8 view .LVU2151
 6229 00b4 12F4004F 		tst	r2, #32768
 6230 00b8 13D1     		bne	.L410
2774:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6231              		.loc 1 2774 7 is_stmt 1 view .LVU2152
2774:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6232              		.loc 1 2774 39 is_stmt 0 view .LVU2153
 6233 00ba 0022     		movs	r2, #0
 6234 00bc 1A65     		str	r2, [r3, #80]
2700:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t dma_rx_abort_done = 1UL;
 6235              		.loc 1 2700 12 view .LVU2154
 6236 00be 0125     		movs	r5, #1
 6237              	.LVL323:
 6238              	.L392:
2778:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6239              		.loc 1 2778 3 is_stmt 1 view .LVU2155
2778:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6240              		.loc 1 2778 11 is_stmt 0 view .LVU2156
 6241 00c0 E36F     		ldr	r3, [r4, #124]
2778:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6242              		.loc 1 2778 6 view .LVU2157
 6243 00c2 002B     		cmp	r3, #0
 6244 00c4 37D0     		beq	.L401
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 214


2780:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6245              		.loc 1 2780 5 is_stmt 1 view .LVU2158
2780:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6246              		.loc 1 2780 9 is_stmt 0 view .LVU2159
 6247 00c6 2268     		ldr	r2, [r4]
 6248 00c8 9268     		ldr	r2, [r2, #8]
2780:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6249              		.loc 1 2780 8 view .LVU2160
 6250 00ca 12F4804F 		tst	r2, #16384
 6251 00ce 1ED1     		bne	.L411
2799:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6252              		.loc 1 2799 7 is_stmt 1 view .LVU2161
2799:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6253              		.loc 1 2799 39 is_stmt 0 view .LVU2162
 6254 00d0 0022     		movs	r2, #0
 6255 00d2 1A65     		str	r2, [r3, #80]
2701:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6256              		.loc 1 2701 12 view .LVU2163
 6257 00d4 0123     		movs	r3, #1
 6258              	.LVL324:
 6259              	.L394:
2804:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6260              		.loc 1 2804 3 is_stmt 1 view .LVU2164
2804:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6261              		.loc 1 2804 6 is_stmt 0 view .LVU2165
 6262 00d6 1D42     		tst	r5, r3
 6263 00d8 2FD1     		bne	.L412
2707:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   count = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24UL / 1000UL);
 6264              		.loc 1 2707 13 view .LVU2166
 6265 00da 0025     		movs	r5, #0
 6266              	.LVL325:
 6267              	.L396:
2832:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 6268              		.loc 1 2832 3 is_stmt 1 view .LVU2167
2833:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6269              		.loc 1 2833 1 is_stmt 0 view .LVU2168
 6270 00dc 2846     		mov	r0, r5
 6271 00de 03B0     		add	sp, sp, #12
 6272              		.cfi_remember_state
 6273              		.cfi_def_cfa_offset 12
 6274              		@ sp needed
 6275 00e0 30BD     		pop	{r4, r5, pc}
 6276              	.LVL326:
 6277              	.L410:
 6278              		.cfi_restore_state
2758:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6279              		.loc 1 2758 7 is_stmt 1 view .LVU2169
2758:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6280              		.loc 1 2758 39 is_stmt 0 view .LVU2170
 6281 00e2 224A     		ldr	r2, .L417+8
 6282 00e4 1A65     		str	r2, [r3, #80]
2760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6283              		.loc 1 2760 7 is_stmt 1 view .LVU2171
 6284              	.LVL327:
2763:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6285              		.loc 1 2763 7 view .LVU2172
2763:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 215


 6286              		.loc 1 2763 11 is_stmt 0 view .LVU2173
 6287 00e6 A06F     		ldr	r0, [r4, #120]
 6288              	.LVL328:
2763:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6289              		.loc 1 2763 11 view .LVU2174
 6290 00e8 FFF7FEFF 		bl	HAL_DMA_Abort_IT
 6291              	.LVL329:
2763:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6292              		.loc 1 2763 10 discriminator 1 view .LVU2175
 6293 00ec 08B9     		cbnz	r0, .L413
2760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6294              		.loc 1 2760 25 view .LVU2176
 6295 00ee 0025     		movs	r5, #0
 6296 00f0 E6E7     		b	.L392
 6297              	.L413:
2765:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6298              		.loc 1 2765 9 is_stmt 1 view .LVU2177
2765:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6299              		.loc 1 2765 13 is_stmt 0 view .LVU2178
 6300 00f2 A06F     		ldr	r0, [r4, #120]
 6301 00f4 FFF7FEFF 		bl	HAL_DMA_GetError
 6302              	.LVL330:
2765:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6303              		.loc 1 2765 12 discriminator 1 view .LVU2179
 6304 00f8 8028     		cmp	r0, #128
 6305 00fa 01D0     		beq	.L414
2760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6306              		.loc 1 2760 25 view .LVU2180
 6307 00fc 0025     		movs	r5, #0
 6308 00fe DFE7     		b	.L392
 6309              	.L414:
2767:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->hdmatx->XferAbortCallback = NULL;
 6310              		.loc 1 2767 11 is_stmt 1 view .LVU2181
 6311              	.LVL331:
2768:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6312              		.loc 1 2768 11 view .LVU2182
2768:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6313              		.loc 1 2768 15 is_stmt 0 view .LVU2183
 6314 0100 A36F     		ldr	r3, [r4, #120]
2768:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6315              		.loc 1 2768 43 view .LVU2184
 6316 0102 0022     		movs	r2, #0
 6317 0104 1A65     		str	r2, [r3, #80]
2767:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->hdmatx->XferAbortCallback = NULL;
 6318              		.loc 1 2767 29 view .LVU2185
 6319 0106 0125     		movs	r5, #1
 6320 0108 DAE7     		b	.L392
 6321              	.LVL332:
 6322              	.L398:
2700:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t dma_rx_abort_done = 1UL;
 6323              		.loc 1 2700 12 view .LVU2186
 6324 010a 0125     		movs	r5, #1
 6325 010c D8E7     		b	.L392
 6326              	.LVL333:
 6327              	.L411:
2783:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6328              		.loc 1 2783 7 is_stmt 1 view .LVU2187
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 216


2783:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6329              		.loc 1 2783 39 is_stmt 0 view .LVU2188
 6330 010e 184A     		ldr	r2, .L417+12
 6331 0110 1A65     		str	r2, [r3, #80]
2785:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6332              		.loc 1 2785 7 is_stmt 1 view .LVU2189
 6333              	.LVL334:
2788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6334              		.loc 1 2788 7 view .LVU2190
2788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6335              		.loc 1 2788 11 is_stmt 0 view .LVU2191
 6336 0112 E06F     		ldr	r0, [r4, #124]
 6337 0114 FFF7FEFF 		bl	HAL_DMA_Abort_IT
 6338              	.LVL335:
2788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6339              		.loc 1 2788 10 discriminator 1 view .LVU2192
 6340 0118 08B9     		cbnz	r0, .L415
2785:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6341              		.loc 1 2785 25 view .LVU2193
 6342 011a 0023     		movs	r3, #0
 6343 011c DBE7     		b	.L394
 6344              	.L415:
2790:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6345              		.loc 1 2790 9 is_stmt 1 view .LVU2194
2790:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6346              		.loc 1 2790 13 is_stmt 0 view .LVU2195
 6347 011e E06F     		ldr	r0, [r4, #124]
 6348 0120 FFF7FEFF 		bl	HAL_DMA_GetError
 6349              	.LVL336:
2790:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6350              		.loc 1 2790 12 discriminator 1 view .LVU2196
 6351 0124 8028     		cmp	r0, #128
 6352 0126 01D0     		beq	.L416
2785:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6353              		.loc 1 2785 25 view .LVU2197
 6354 0128 0023     		movs	r3, #0
 6355 012a D4E7     		b	.L394
 6356              	.L416:
2792:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->hdmarx->XferAbortCallback = NULL;
 6357              		.loc 1 2792 11 is_stmt 1 view .LVU2198
 6358              	.LVL337:
2793:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6359              		.loc 1 2793 11 view .LVU2199
2793:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6360              		.loc 1 2793 15 is_stmt 0 view .LVU2200
 6361 012c E36F     		ldr	r3, [r4, #124]
2793:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6362              		.loc 1 2793 43 view .LVU2201
 6363 012e 0022     		movs	r2, #0
 6364 0130 1A65     		str	r2, [r3, #80]
2792:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->hdmarx->XferAbortCallback = NULL;
 6365              		.loc 1 2792 29 view .LVU2202
 6366 0132 0123     		movs	r3, #1
 6367 0134 CFE7     		b	.L394
 6368              	.L401:
2701:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6369              		.loc 1 2701 12 view .LVU2203
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 217


 6370 0136 0123     		movs	r3, #1
 6371 0138 CDE7     		b	.L394
 6372              	.LVL338:
 6373              	.L412:
2807:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6374              		.loc 1 2807 5 is_stmt 1 view .LVU2204
 6375 013a 2046     		mov	r0, r4
 6376 013c FFF7FEFF 		bl	SPI_AbortTransfer
 6377              	.LVL339:
2810:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6378              		.loc 1 2810 5 view .LVU2205
2810:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6379              		.loc 1 2810 9 is_stmt 0 view .LVU2206
 6380 0140 D4F88430 		ldr	r3, [r4, #132]
2810:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6381              		.loc 1 2810 8 view .LVU2207
 6382 0144 13F0400F 		tst	r3, #64
 6383 0148 09D1     		bne	.L405
2818:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6384              		.loc 1 2818 7 is_stmt 1 view .LVU2208
2818:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6385              		.loc 1 2818 23 is_stmt 0 view .LVU2209
 6386 014a 0025     		movs	r5, #0
 6387              	.LVL340:
2818:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6388              		.loc 1 2818 23 view .LVU2210
 6389 014c C4F88450 		str	r5, [r4, #132]
 6390              	.L397:
 6391              	.LVL341:
2822:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6392              		.loc 1 2822 5 is_stmt 1 view .LVU2211
2822:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6393              		.loc 1 2822 17 is_stmt 0 view .LVU2212
 6394 0150 0123     		movs	r3, #1
 6395 0152 84F88130 		strb	r3, [r4, #129]
2828:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6396              		.loc 1 2828 5 is_stmt 1 view .LVU2213
 6397 0156 2046     		mov	r0, r4
 6398 0158 FFF7FEFF 		bl	HAL_SPI_AbortCpltCallback
 6399              	.LVL342:
 6400 015c BEE7     		b	.L396
 6401              	.LVL343:
 6402              	.L405:
2813:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6403              		.loc 1 2813 17 is_stmt 0 view .LVU2214
 6404 015e 0125     		movs	r5, #1
 6405              	.LVL344:
2813:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6406              		.loc 1 2813 17 view .LVU2215
 6407 0160 F6E7     		b	.L397
 6408              	.L418:
 6409 0162 00BF     		.align	2
 6410              	.L417:
 6411 0164 00000000 		.word	SystemCoreClock
 6412 0168 F1197605 		.word	91625969
 6413 016c 00000000 		.word	SPI_DMATxAbortCallback
 6414 0170 00000000 		.word	SPI_DMARxAbortCallback
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 218


 6415              		.cfi_endproc
 6416              	.LFE349:
 6418              		.section	.text.SPI_DMARxAbortCallback,"ax",%progbits
 6419              		.align	1
 6420              		.syntax unified
 6421              		.thumb
 6422              		.thumb_func
 6424              	SPI_DMARxAbortCallback:
 6425              	.LVL345:
 6426              	.LFB374:
3566:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 6427              		.loc 1 3566 1 is_stmt 1 view -0
 6428              		.cfi_startproc
 6429              		@ args = 0, pretend = 0, frame = 0
 6430              		@ frame_needed = 0, uses_anonymous_args = 0
3566:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 6431              		.loc 1 3566 1 is_stmt 0 view .LVU2217
 6432 0000 10B5     		push	{r4, lr}
 6433              		.cfi_def_cfa_offset 8
 6434              		.cfi_offset 4, -8
 6435              		.cfi_offset 14, -4
3567:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6436              		.loc 1 3567 3 is_stmt 1 view .LVU2218
3567:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6437              		.loc 1 3567 22 is_stmt 0 view .LVU2219
 6438 0002 846B     		ldr	r4, [r0, #56]
 6439              	.LVL346:
3569:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6440              		.loc 1 3569 3 is_stmt 1 view .LVU2220
3569:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6441              		.loc 1 3569 7 is_stmt 0 view .LVU2221
 6442 0004 E36F     		ldr	r3, [r4, #124]
3569:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6443              		.loc 1 3569 35 view .LVU2222
 6444 0006 0022     		movs	r2, #0
 6445 0008 1A65     		str	r2, [r3, #80]
3572:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6446              		.loc 1 3572 3 is_stmt 1 view .LVU2223
3572:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6447              		.loc 1 3572 11 is_stmt 0 view .LVU2224
 6448 000a A36F     		ldr	r3, [r4, #120]
3572:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6449              		.loc 1 3572 6 view .LVU2225
 6450 000c 0BB1     		cbz	r3, .L420
3574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6451              		.loc 1 3574 5 is_stmt 1 view .LVU2226
3574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6452              		.loc 1 3574 21 is_stmt 0 view .LVU2227
 6453 000e 1B6D     		ldr	r3, [r3, #80]
3574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6454              		.loc 1 3574 8 view .LVU2228
 6455 0010 43B9     		cbnz	r3, .L419
 6456              	.L420:
3581:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6457              		.loc 1 3581 3 is_stmt 1 view .LVU2229
 6458 0012 2046     		mov	r0, r4
 6459              	.LVL347:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 219


3581:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6460              		.loc 1 3581 3 is_stmt 0 view .LVU2230
 6461 0014 FFF7FEFF 		bl	SPI_AbortTransfer
 6462              	.LVL348:
3584:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6463              		.loc 1 3584 3 is_stmt 1 view .LVU2231
3584:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6464              		.loc 1 3584 15 is_stmt 0 view .LVU2232
 6465 0018 0123     		movs	r3, #1
 6466 001a 84F88130 		strb	r3, [r4, #129]
3590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6467              		.loc 1 3590 3 is_stmt 1 view .LVU2233
 6468 001e 2046     		mov	r0, r4
 6469 0020 FFF7FEFF 		bl	HAL_SPI_AbortCpltCallback
 6470              	.LVL349:
 6471              	.L419:
3592:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6472              		.loc 1 3592 1 is_stmt 0 view .LVU2234
 6473 0024 10BD     		pop	{r4, pc}
3592:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6474              		.loc 1 3592 1 view .LVU2235
 6475              		.cfi_endproc
 6476              	.LFE374:
 6478              		.section	.text.SPI_DMATxAbortCallback,"ax",%progbits
 6479              		.align	1
 6480              		.syntax unified
 6481              		.thumb
 6482              		.thumb_func
 6484              	SPI_DMATxAbortCallback:
 6485              	.LVL350:
 6486              	.LFB373:
3529:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 6487              		.loc 1 3529 1 is_stmt 1 view -0
 6488              		.cfi_startproc
 6489              		@ args = 0, pretend = 0, frame = 0
 6490              		@ frame_needed = 0, uses_anonymous_args = 0
3529:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)((DMA_HandleTypeDef *)hdma)->Parent;
 6491              		.loc 1 3529 1 is_stmt 0 view .LVU2237
 6492 0000 10B5     		push	{r4, lr}
 6493              		.cfi_def_cfa_offset 8
 6494              		.cfi_offset 4, -8
 6495              		.cfi_offset 14, -4
3530:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6496              		.loc 1 3530 3 is_stmt 1 view .LVU2238
3530:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6497              		.loc 1 3530 22 is_stmt 0 view .LVU2239
 6498 0002 846B     		ldr	r4, [r0, #56]
 6499              	.LVL351:
3532:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6500              		.loc 1 3532 3 is_stmt 1 view .LVU2240
3532:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6501              		.loc 1 3532 7 is_stmt 0 view .LVU2241
 6502 0004 A36F     		ldr	r3, [r4, #120]
3532:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6503              		.loc 1 3532 35 view .LVU2242
 6504 0006 0022     		movs	r2, #0
 6505 0008 1A65     		str	r2, [r3, #80]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 220


3535:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6506              		.loc 1 3535 3 is_stmt 1 view .LVU2243
3535:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6507              		.loc 1 3535 11 is_stmt 0 view .LVU2244
 6508 000a E36F     		ldr	r3, [r4, #124]
3535:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6509              		.loc 1 3535 6 view .LVU2245
 6510 000c 0BB1     		cbz	r3, .L424
3537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6511              		.loc 1 3537 5 is_stmt 1 view .LVU2246
3537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6512              		.loc 1 3537 21 is_stmt 0 view .LVU2247
 6513 000e 1B6D     		ldr	r3, [r3, #80]
3537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6514              		.loc 1 3537 8 view .LVU2248
 6515 0010 43B9     		cbnz	r3, .L423
 6516              	.L424:
3544:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6517              		.loc 1 3544 3 is_stmt 1 view .LVU2249
 6518 0012 2046     		mov	r0, r4
 6519              	.LVL352:
3544:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6520              		.loc 1 3544 3 is_stmt 0 view .LVU2250
 6521 0014 FFF7FEFF 		bl	SPI_AbortTransfer
 6522              	.LVL353:
3547:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6523              		.loc 1 3547 3 is_stmt 1 view .LVU2251
3547:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6524              		.loc 1 3547 15 is_stmt 0 view .LVU2252
 6525 0018 0123     		movs	r3, #1
 6526 001a 84F88130 		strb	r3, [r4, #129]
3553:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6527              		.loc 1 3553 3 is_stmt 1 view .LVU2253
 6528 001e 2046     		mov	r0, r4
 6529 0020 FFF7FEFF 		bl	HAL_SPI_AbortCpltCallback
 6530              	.LVL354:
 6531              	.L423:
3555:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6532              		.loc 1 3555 1 is_stmt 0 view .LVU2254
 6533 0024 10BD     		pop	{r4, pc}
3555:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6534              		.loc 1 3555 1 view .LVU2255
 6535              		.cfi_endproc
 6536              	.LFE373:
 6538              		.section	.text.HAL_SPI_SuspendCallback,"ax",%progbits
 6539              		.align	1
 6540              		.weak	HAL_SPI_SuspendCallback
 6541              		.syntax unified
 6542              		.thumb
 6543              		.thumb_func
 6545              	HAL_SPI_SuspendCallback:
 6546              	.LVL355:
 6547              	.LFB362:
3269:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 6548              		.loc 1 3269 1 is_stmt 1 view -0
 6549              		.cfi_startproc
 6550              		@ args = 0, pretend = 0, frame = 0
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 221


 6551              		@ frame_needed = 0, uses_anonymous_args = 0
 6552              		@ link register save eliminated.
3271:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6553              		.loc 1 3271 3 view .LVU2257
3276:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6554              		.loc 1 3276 1 is_stmt 0 view .LVU2258
 6555 0000 7047     		bx	lr
 6556              		.cfi_endproc
 6557              	.LFE362:
 6559              		.section	.text.HAL_SPI_IRQHandler,"ax",%progbits
 6560              		.align	1
 6561              		.global	HAL_SPI_IRQHandler
 6562              		.syntax unified
 6563              		.thumb
 6564              		.thumb_func
 6566              	HAL_SPI_IRQHandler:
 6567              	.LVL356:
 6568              	.LFB353:
2887:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t itsource = hspi->Instance->IER;
 6569              		.loc 1 2887 1 is_stmt 1 view -0
 6570              		.cfi_startproc
 6571              		@ args = 0, pretend = 0, frame = 0
 6572              		@ frame_needed = 0, uses_anonymous_args = 0
2887:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t itsource = hspi->Instance->IER;
 6573              		.loc 1 2887 1 is_stmt 0 view .LVU2260
 6574 0000 2DE9F843 		push	{r3, r4, r5, r6, r7, r8, r9, lr}
 6575              		.cfi_def_cfa_offset 32
 6576              		.cfi_offset 3, -32
 6577              		.cfi_offset 4, -28
 6578              		.cfi_offset 5, -24
 6579              		.cfi_offset 6, -20
 6580              		.cfi_offset 7, -16
 6581              		.cfi_offset 8, -12
 6582              		.cfi_offset 9, -8
 6583              		.cfi_offset 14, -4
 6584 0004 0446     		mov	r4, r0
2888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t itflag   = hspi->Instance->SR;
 6585              		.loc 1 2888 3 is_stmt 1 view .LVU2261
2888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t itflag   = hspi->Instance->SR;
 6586              		.loc 1 2888 27 is_stmt 0 view .LVU2262
 6587 0006 0668     		ldr	r6, [r0]
2888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t itflag   = hspi->Instance->SR;
 6588              		.loc 1 2888 12 view .LVU2263
 6589 0008 3269     		ldr	r2, [r6, #16]
 6590              	.LVL357:
2889:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t trigger  = itsource & itflag;
 6591              		.loc 1 2889 3 is_stmt 1 view .LVU2264
2889:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t trigger  = itsource & itflag;
 6592              		.loc 1 2889 12 is_stmt 0 view .LVU2265
 6593 000a 7369     		ldr	r3, [r6, #20]
 6594              	.LVL358:
2890:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t cfg1     = hspi->Instance->CFG1;
 6595              		.loc 1 2890 3 is_stmt 1 view .LVU2266
2890:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t cfg1     = hspi->Instance->CFG1;
 6596              		.loc 1 2890 12 is_stmt 0 view .LVU2267
 6597 000c 02EA0305 		and	r5, r2, r3
 6598              	.LVL359:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 222


2891:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t handled  = 0UL;
 6599              		.loc 1 2891 3 is_stmt 1 view .LVU2268
2891:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   uint32_t handled  = 0UL;
 6600              		.loc 1 2891 12 is_stmt 0 view .LVU2269
 6601 0010 D6F80890 		ldr	r9, [r6, #8]
 6602              	.LVL360:
2892:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6603              		.loc 1 2892 3 is_stmt 1 view .LVU2270
2894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 6604              		.loc 1 2894 3 view .LVU2271
2894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #if defined (__GNUC__)
 6605              		.loc 1 2894 24 is_stmt 0 view .LVU2272
 6606 0014 90F88170 		ldrb	r7, [r0, #129]	@ zero_extendqisi2
 6607 0018 FFB2     		uxtb	r7, r7
 6608              	.LVL361:
2896:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* __GNUC__ */
 6609              		.loc 1 2896 3 is_stmt 1 view .LVU2273
2900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6610              		.loc 1 2900 3 view .LVU2274
2900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6611              		.loc 1 2900 6 is_stmt 0 view .LVU2275
 6612 001a 13F4006F 		tst	r3, #2048
 6613 001e 02D0     		beq	.L429
2900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6614              		.loc 1 2900 45 discriminator 1 view .LVU2276
 6615 0020 12F0080F 		tst	r2, #8
 6616 0024 3FD1     		bne	.L456
 6617              	.L429:
2915:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_IS_BIT_SET(trigger, SPI_FLAG_DXP))
 6618              		.loc 1 2915 3 is_stmt 1 view .LVU2277
2915:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_IS_BIT_SET(trigger, SPI_FLAG_DXP))
 6619              		.loc 1 2915 86 is_stmt 0 view .LVU2278
 6620 0026 05F06403 		and	r3, r5, #100
 6621              	.LVL362:
2915:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_IS_BIT_SET(trigger, SPI_FLAG_DXP))
 6622              		.loc 1 2915 6 view .LVU2279
 6623 002a 042B     		cmp	r3, #4
 6624 002c 42D0     		beq	.L457
2892:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6625              		.loc 1 2892 12 view .LVU2280
 6626 002e 0023     		movs	r3, #0
 6627              	.LVL363:
 6628              	.L431:
2924:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_IS_BIT_CLR(trigger, SPI_FLAG_DXP))
 6629              		.loc 1 2924 3 is_stmt 1 view .LVU2281
2924:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_IS_BIT_CLR(trigger, SPI_FLAG_DXP))
 6630              		.loc 1 2924 86 is_stmt 0 view .LVU2282
 6631 0030 05F04508 		and	r8, r5, #69
2924:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_IS_BIT_CLR(trigger, SPI_FLAG_DXP))
 6632              		.loc 1 2924 6 view .LVU2283
 6633 0034 B8F1010F 		cmp	r8, #1
 6634 0038 44D0     		beq	.L458
 6635              	.LVL364:
 6636              	.L432:
2932:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_IS_BIT_CLR(trigger, SPI_FLAG_DXP))
 6637              		.loc 1 2932 3 is_stmt 1 view .LVU2284
2932:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_IS_BIT_CLR(trigger, SPI_FLAG_DXP))
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 223


 6638              		.loc 1 2932 86 is_stmt 0 view .LVU2285
 6639 003a 05F02602 		and	r2, r5, #38
2932:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       HAL_IS_BIT_CLR(trigger, SPI_FLAG_DXP))
 6640              		.loc 1 2932 6 view .LVU2286
 6641 003e 022A     		cmp	r2, #2
 6642 0040 45D0     		beq	.L459
2947:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6643              		.loc 1 2947 3 is_stmt 1 view .LVU2287
2947:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6644              		.loc 1 2947 6 is_stmt 0 view .LVU2288
 6645 0042 002B     		cmp	r3, #0
 6646 0044 46D1     		bne	.L428
2953:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6647              		.loc 1 2953 3 is_stmt 1 view .LVU2289
2953:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6648              		.loc 1 2953 6 is_stmt 0 view .LVU2290
 6649 0046 15F0080F 		tst	r5, #8
 6650 004a 79D0     		beq	.L436
2956:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_CLEAR_TXTFFLAG(hspi);
 6651              		.loc 1 2956 5 is_stmt 1 view .LVU2291
 6652 004c 2268     		ldr	r2, [r4]
 6653 004e 9369     		ldr	r3, [r2, #24]
 6654              	.LVL365:
2956:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_CLEAR_TXTFFLAG(hspi);
 6655              		.loc 1 2956 5 is_stmt 0 view .LVU2292
 6656 0050 43F00803 		orr	r3, r3, #8
 6657 0054 9361     		str	r3, [r2, #24]
2957:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     __HAL_SPI_CLEAR_SUSPFLAG(hspi);
 6658              		.loc 1 2957 5 is_stmt 1 view .LVU2293
 6659 0056 2268     		ldr	r2, [r4]
 6660 0058 9369     		ldr	r3, [r2, #24]
 6661 005a 43F01003 		orr	r3, r3, #16
 6662 005e 9361     		str	r3, [r2, #24]
2958:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6663              		.loc 1 2958 5 view .LVU2294
 6664 0060 2268     		ldr	r2, [r4]
 6665 0062 9369     		ldr	r3, [r2, #24]
 6666 0064 43F40063 		orr	r3, r3, #2048
 6667 0068 9361     		str	r3, [r2, #24]
2961:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6668              		.loc 1 2961 5 view .LVU2295
 6669 006a 2268     		ldr	r2, [r4]
 6670 006c 1369     		ldr	r3, [r2, #16]
 6671 006e 23F00803 		bic	r3, r3, #8
 6672 0072 1361     		str	r3, [r2, #16]
2964:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6673              		.loc 1 2964 5 view .LVU2296
2964:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6674              		.loc 1 2964 9 is_stmt 0 view .LVU2297
 6675 0074 2368     		ldr	r3, [r4]
 6676 0076 9B68     		ldr	r3, [r3, #8]
2964:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6677              		.loc 1 2964 8 view .LVU2298
 6678 0078 13F4404F 		tst	r3, #49152
 6679 007c 3BD0     		beq	.L437
 6680              	.L438:
2997:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 224


 6681              		.loc 1 2997 5 is_stmt 1 view .LVU2299
 6682 007e 2046     		mov	r0, r4
 6683 0080 FFF7FEFF 		bl	SPI_CloseTransfer
 6684              	.LVL366:
2999:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
 6685              		.loc 1 2999 5 view .LVU2300
2999:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
 6686              		.loc 1 2999 17 is_stmt 0 view .LVU2301
 6687 0084 0123     		movs	r3, #1
 6688 0086 84F88130 		strb	r3, [r4, #129]
3000:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6689              		.loc 1 3000 5 is_stmt 1 view .LVU2302
3000:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6690              		.loc 1 3000 13 is_stmt 0 view .LVU2303
 6691 008a D4F88430 		ldr	r3, [r4, #132]
3000:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6692              		.loc 1 3000 8 view .LVU2304
 6693 008e 002B     		cmp	r3, #0
 6694 0090 4AD1     		bne	.L460
3026:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6695              		.loc 1 3026 5 is_stmt 1 view .LVU2305
3026:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6696              		.loc 1 3026 8 is_stmt 0 view .LVU2306
 6697 0092 052F     		cmp	r7, #5
 6698 0094 4CD0     		beq	.L461
3030:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6699              		.loc 1 3030 10 is_stmt 1 view .LVU2307
3030:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6700              		.loc 1 3030 13 is_stmt 0 view .LVU2308
 6701 0096 042F     		cmp	r7, #4
 6702 0098 4ED0     		beq	.L462
3034:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6703              		.loc 1 3034 10 is_stmt 1 view .LVU2309
3034:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6704              		.loc 1 3034 13 is_stmt 0 view .LVU2310
 6705 009a 032F     		cmp	r7, #3
 6706 009c 1AD1     		bne	.L428
3036:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6707              		.loc 1 3036 7 is_stmt 1 view .LVU2311
 6708 009e 2046     		mov	r0, r4
 6709 00a0 FFF7FEFF 		bl	HAL_SPI_TxCpltCallback
 6710              	.LVL367:
3042:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6711              		.loc 1 3042 5 view .LVU2312
3044:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 6712              		.loc 1 3044 5 view .LVU2313
 6713 00a4 16E0     		b	.L428
 6714              	.LVL368:
 6715              	.L456:
2903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6716              		.loc 1 2903 5 view .LVU2314
 6717 00a6 B369     		ldr	r3, [r6, #24]
 6718              	.LVL369:
2903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6719              		.loc 1 2903 5 is_stmt 0 view .LVU2315
 6720 00a8 43F40063 		orr	r3, r3, #2048
 6721 00ac B361     		str	r3, [r6, #24]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 225


2909:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6722              		.loc 1 2909 5 is_stmt 1 view .LVU2316
 6723 00ae FFF7FEFF 		bl	HAL_SPI_SuspendCallback
 6724              	.LVL370:
2911:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 6725              		.loc 1 2911 5 view .LVU2317
 6726 00b2 0FE0     		b	.L428
 6727              	.LVL371:
 6728              	.L457:
2918:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR(hspi);
 6729              		.loc 1 2918 5 view .LVU2318
2918:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR(hspi);
 6730              		.loc 1 2918 9 is_stmt 0 view .LVU2319
 6731 00b4 636F     		ldr	r3, [r4, #116]
2918:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR(hspi);
 6732              		.loc 1 2918 5 view .LVU2320
 6733 00b6 2046     		mov	r0, r4
 6734              	.LVL372:
2918:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     hspi->RxISR(hspi);
 6735              		.loc 1 2918 5 view .LVU2321
 6736 00b8 9847     		blx	r3
 6737              	.LVL373:
2919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     handled = 1UL;
 6738              		.loc 1 2919 5 is_stmt 1 view .LVU2322
2919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     handled = 1UL;
 6739              		.loc 1 2919 9 is_stmt 0 view .LVU2323
 6740 00ba 236F     		ldr	r3, [r4, #112]
2919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     handled = 1UL;
 6741              		.loc 1 2919 5 view .LVU2324
 6742 00bc 2046     		mov	r0, r4
 6743 00be 9847     		blx	r3
 6744              	.LVL374:
2920:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 6745              		.loc 1 2920 5 is_stmt 1 view .LVU2325
2920:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 6746              		.loc 1 2920 13 is_stmt 0 view .LVU2326
 6747 00c0 0123     		movs	r3, #1
 6748 00c2 B5E7     		b	.L431
 6749              	.LVL375:
 6750              	.L458:
2927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     handled = 1UL;
 6751              		.loc 1 2927 5 is_stmt 1 view .LVU2327
2927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     handled = 1UL;
 6752              		.loc 1 2927 9 is_stmt 0 view .LVU2328
 6753 00c4 236F     		ldr	r3, [r4, #112]
 6754              	.LVL376:
2927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     handled = 1UL;
 6755              		.loc 1 2927 5 view .LVU2329
 6756 00c6 2046     		mov	r0, r4
 6757 00c8 9847     		blx	r3
 6758              	.LVL377:
2928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 6759              		.loc 1 2928 5 is_stmt 1 view .LVU2330
2928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 6760              		.loc 1 2928 13 is_stmt 0 view .LVU2331
 6761 00ca 4346     		mov	r3, r8
 6762 00cc B5E7     		b	.L432
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 226


 6763              	.LVL378:
 6764              	.L459:
2935:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     handled = 1UL;
 6765              		.loc 1 2935 5 is_stmt 1 view .LVU2332
2935:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     handled = 1UL;
 6766              		.loc 1 2935 9 is_stmt 0 view .LVU2333
 6767 00ce 636F     		ldr	r3, [r4, #116]
 6768              	.LVL379:
2935:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     handled = 1UL;
 6769              		.loc 1 2935 5 view .LVU2334
 6770 00d0 2046     		mov	r0, r4
 6771 00d2 9847     		blx	r3
 6772              	.LVL380:
2936:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 6773              		.loc 1 2936 5 is_stmt 1 view .LVU2335
2947:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6774              		.loc 1 2947 3 view .LVU2336
 6775              	.L428:
3131:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6776              		.loc 1 3131 1 is_stmt 0 view .LVU2337
 6777 00d4 BDE8F883 		pop	{r3, r4, r5, r6, r7, r8, r9, pc}
 6778              	.LVL381:
 6779              	.L439:
2976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6780              		.loc 1 2976 14 is_stmt 1 view .LVU2338
2976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6781              		.loc 1 2976 17 is_stmt 0 view .LVU2339
 6782 00d8 072B     		cmp	r3, #7
 6783 00da 1CD9     		bls	.L441
2979:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 6784              		.loc 1 2979 11 is_stmt 1 view .LVU2340
2979:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 6785              		.loc 1 2979 29 is_stmt 0 view .LVU2341
 6786 00dc 636E     		ldr	r3, [r4, #100]
2979:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 6787              		.loc 1 2979 45 view .LVU2342
 6788 00de 328E     		ldrh	r2, [r6, #48]
2979:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #else
 6789              		.loc 1 2979 43 view .LVU2343
 6790 00e0 1A80     		strh	r2, [r3]	@ movhi
2983:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6791              		.loc 1 2983 11 is_stmt 1 view .LVU2344
2983:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6792              		.loc 1 2983 15 is_stmt 0 view .LVU2345
 6793 00e2 636E     		ldr	r3, [r4, #100]
2983:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6794              		.loc 1 2983 28 view .LVU2346
 6795 00e4 0233     		adds	r3, r3, #2
 6796 00e6 6366     		str	r3, [r4, #100]
 6797              	.L440:
2992:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 6798              		.loc 1 2992 9 is_stmt 1 view .LVU2347
2992:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
 6799              		.loc 1 2992 13 is_stmt 0 view .LVU2348
 6800 00e8 B4F86A30 		ldrh	r3, [r4, #106]
 6801 00ec 9BB2     		uxth	r3, r3
2992:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 227


 6802              		.loc 1 2992 26 view .LVU2349
 6803 00ee 013B     		subs	r3, r3, #1
 6804 00f0 9BB2     		uxth	r3, r3
 6805 00f2 A4F86A30 		strh	r3, [r4, #106]	@ movhi
 6806              	.L437:
2967:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6807              		.loc 1 2967 32 is_stmt 1 view .LVU2350
2967:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6808              		.loc 1 2967 18 is_stmt 0 view .LVU2351
 6809 00f6 B4F86A30 		ldrh	r3, [r4, #106]
 6810 00fa 9BB2     		uxth	r3, r3
2967:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6811              		.loc 1 2967 32 view .LVU2352
 6812 00fc 002B     		cmp	r3, #0
 6813 00fe BED0     		beq	.L438
2970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6814              		.loc 1 2970 9 is_stmt 1 view .LVU2353
2970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6815              		.loc 1 2970 23 is_stmt 0 view .LVU2354
 6816 0100 E368     		ldr	r3, [r4, #12]
2970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6817              		.loc 1 2970 12 view .LVU2355
 6818 0102 0F2B     		cmp	r3, #15
 6819 0104 E8D9     		bls	.L439
2972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
 6820              		.loc 1 2972 11 is_stmt 1 view .LVU2356
2972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
 6821              		.loc 1 2972 69 is_stmt 0 view .LVU2357
 6822 0106 2268     		ldr	r2, [r4]
2972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
 6823              		.loc 1 2972 29 view .LVU2358
 6824 0108 636E     		ldr	r3, [r4, #100]
2972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
 6825              		.loc 1 2972 45 view .LVU2359
 6826 010a 126B     		ldr	r2, [r2, #48]
2972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint32_t);
 6827              		.loc 1 2972 43 view .LVU2360
 6828 010c 1A60     		str	r2, [r3]
2973:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6829              		.loc 1 2973 11 is_stmt 1 view .LVU2361
2973:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6830              		.loc 1 2973 15 is_stmt 0 view .LVU2362
 6831 010e 636E     		ldr	r3, [r4, #100]
2973:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6832              		.loc 1 2973 28 view .LVU2363
 6833 0110 0433     		adds	r3, r3, #4
 6834 0112 6366     		str	r3, [r4, #100]
 6835 0114 E8E7     		b	.L440
 6836              	.L441:
2988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 6837              		.loc 1 2988 11 is_stmt 1 view .LVU2364
2988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 6838              		.loc 1 2988 67 is_stmt 0 view .LVU2365
 6839 0116 2268     		ldr	r2, [r4]
2988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 6840              		.loc 1 2988 28 view .LVU2366
 6841 0118 636E     		ldr	r3, [r4, #100]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 228


2988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 6842              		.loc 1 2988 44 view .LVU2367
 6843 011a 92F83020 		ldrb	r2, [r2, #48]	@ zero_extendqisi2
2988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint8_t);
 6844              		.loc 1 2988 42 view .LVU2368
 6845 011e 1A70     		strb	r2, [r3]
2989:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6846              		.loc 1 2989 11 is_stmt 1 view .LVU2369
2989:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6847              		.loc 1 2989 15 is_stmt 0 view .LVU2370
 6848 0120 636E     		ldr	r3, [r4, #100]
2989:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         }
 6849              		.loc 1 2989 28 view .LVU2371
 6850 0122 0133     		adds	r3, r3, #1
 6851 0124 6366     		str	r3, [r4, #100]
 6852 0126 DFE7     		b	.L440
 6853              	.L460:
3005:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6854              		.loc 1 3005 7 is_stmt 1 view .LVU2372
 6855 0128 2046     		mov	r0, r4
 6856 012a FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6857              	.LVL382:
3007:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6858              		.loc 1 3007 7 view .LVU2373
 6859 012e D1E7     		b	.L428
 6860              	.L461:
3028:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6861              		.loc 1 3028 7 view .LVU2374
 6862 0130 2046     		mov	r0, r4
 6863 0132 FFF7FEFF 		bl	HAL_SPI_TxRxCpltCallback
 6864              	.LVL383:
 6865 0136 CDE7     		b	.L428
 6866              	.L462:
3032:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6867              		.loc 1 3032 7 view .LVU2375
 6868 0138 2046     		mov	r0, r4
 6869 013a FFF7FEFF 		bl	HAL_SPI_RxCpltCallback
 6870              	.LVL384:
 6871 013e C9E7     		b	.L428
 6872              	.LVL385:
 6873              	.L436:
3048:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6874              		.loc 1 3048 3 view .LVU2376
3048:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   {
 6875              		.loc 1 3048 6 is_stmt 0 view .LVU2377
 6876 0140 15F4587F 		tst	r5, #864
 6877 0144 C6D0     		beq	.L428
3051:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6878              		.loc 1 3051 5 is_stmt 1 view .LVU2378
3051:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6879              		.loc 1 3051 8 is_stmt 0 view .LVU2379
 6880 0146 15F0400F 		tst	r5, #64
 6881 014a 0AD0     		beq	.L447
3053:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_CLEAR_OVRFLAG(hspi);
 6882              		.loc 1 3053 7 is_stmt 1 view .LVU2380
 6883 014c D4F88430 		ldr	r3, [r4, #132]
 6884              	.LVL386:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 229


3053:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_CLEAR_OVRFLAG(hspi);
 6885              		.loc 1 3053 7 is_stmt 0 view .LVU2381
 6886 0150 43F00403 		orr	r3, r3, #4
 6887 0154 C4F88430 		str	r3, [r4, #132]
3054:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6888              		.loc 1 3054 7 is_stmt 1 view .LVU2382
 6889 0158 2268     		ldr	r2, [r4]
 6890 015a 9369     		ldr	r3, [r2, #24]
 6891 015c 43F04003 		orr	r3, r3, #64
 6892 0160 9361     		str	r3, [r2, #24]
 6893              	.L447:
3058:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6894              		.loc 1 3058 5 view .LVU2383
3058:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6895              		.loc 1 3058 8 is_stmt 0 view .LVU2384
 6896 0162 15F4007F 		tst	r5, #512
 6897 0166 0AD0     		beq	.L448
3060:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_CLEAR_MODFFLAG(hspi);
 6898              		.loc 1 3060 7 is_stmt 1 view .LVU2385
 6899 0168 D4F88430 		ldr	r3, [r4, #132]
 6900 016c 43F00103 		orr	r3, r3, #1
 6901 0170 C4F88430 		str	r3, [r4, #132]
3061:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6902              		.loc 1 3061 7 view .LVU2386
 6903 0174 2268     		ldr	r2, [r4]
 6904 0176 9369     		ldr	r3, [r2, #24]
 6905 0178 43F40073 		orr	r3, r3, #512
 6906 017c 9361     		str	r3, [r2, #24]
 6907              	.L448:
3061:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6908              		.loc 1 3061 37 discriminator 1 view .LVU2387
3065:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6909              		.loc 1 3065 5 view .LVU2388
3065:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6910              		.loc 1 3065 8 is_stmt 0 view .LVU2389
 6911 017e 15F4807F 		tst	r5, #256
 6912 0182 0AD0     		beq	.L449
3067:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_CLEAR_FREFLAG(hspi);
 6913              		.loc 1 3067 7 is_stmt 1 view .LVU2390
 6914 0184 D4F88430 		ldr	r3, [r4, #132]
 6915 0188 43F00803 		orr	r3, r3, #8
 6916 018c C4F88430 		str	r3, [r4, #132]
3068:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6917              		.loc 1 3068 7 view .LVU2391
 6918 0190 2268     		ldr	r2, [r4]
 6919 0192 9369     		ldr	r3, [r2, #24]
 6920 0194 43F48073 		orr	r3, r3, #256
 6921 0198 9361     		str	r3, [r2, #24]
 6922              	.L449:
3072:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6923              		.loc 1 3072 5 view .LVU2392
3072:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6924              		.loc 1 3072 8 is_stmt 0 view .LVU2393
 6925 019a 15F0200F 		tst	r5, #32
 6926 019e 0AD0     		beq	.L450
3074:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       __HAL_SPI_CLEAR_UDRFLAG(hspi);
 6927              		.loc 1 3074 7 is_stmt 1 view .LVU2394
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 230


 6928 01a0 D4F88430 		ldr	r3, [r4, #132]
 6929 01a4 43F08003 		orr	r3, r3, #128
 6930 01a8 C4F88430 		str	r3, [r4, #132]
3075:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     }
 6931              		.loc 1 3075 7 view .LVU2395
 6932 01ac 2268     		ldr	r2, [r4]
 6933 01ae 9369     		ldr	r3, [r2, #24]
 6934 01b0 43F02003 		orr	r3, r3, #32
 6935 01b4 9361     		str	r3, [r2, #24]
 6936              	.L450:
3078:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6937              		.loc 1 3078 5 view .LVU2396
3078:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6938              		.loc 1 3078 13 is_stmt 0 view .LVU2397
 6939 01b6 D4F88430 		ldr	r3, [r4, #132]
3078:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****     {
 6940              		.loc 1 3078 8 view .LVU2398
 6941 01ba 002B     		cmp	r3, #0
 6942 01bc 8AD0     		beq	.L428
3081:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6943              		.loc 1 3081 7 is_stmt 1 view .LVU2399
 6944 01be 2268     		ldr	r2, [r4]
 6945 01c0 1368     		ldr	r3, [r2]
 6946 01c2 23F00103 		bic	r3, r3, #1
 6947 01c6 1360     		str	r3, [r2]
3084:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****                                   SPI_IT_OVR | SPI_IT_FRE | SPI_IT_UDR));
 6948              		.loc 1 3084 7 view .LVU2400
 6949 01c8 2268     		ldr	r2, [r4]
 6950 01ca 1169     		ldr	r1, [r2, #16]
 6951 01cc 1A4B     		ldr	r3, .L463
 6952 01ce 0B40     		ands	r3, r3, r1
 6953 01d0 1361     		str	r3, [r2, #16]
3088:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6954              		.loc 1 3088 7 view .LVU2401
3088:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6955              		.loc 1 3088 11 is_stmt 0 view .LVU2402
 6956 01d2 09F44049 		and	r9, r9, #49152
 6957              	.LVL387:
3088:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****       {
 6958              		.loc 1 3088 10 view .LVU2403
 6959 01d6 B9F5404F 		cmp	r9, #49152
 6960 01da 25D1     		bne	.L452
3091:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 6961              		.loc 1 3091 9 is_stmt 1 view .LVU2404
 6962 01dc 2268     		ldr	r2, [r4]
 6963 01de 9368     		ldr	r3, [r2, #8]
 6964 01e0 23F44043 		bic	r3, r3, #49152
 6965 01e4 9360     		str	r3, [r2, #8]
3094:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6966              		.loc 1 3094 9 view .LVU2405
3094:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6967              		.loc 1 3094 17 is_stmt 0 view .LVU2406
 6968 01e6 E36F     		ldr	r3, [r4, #124]
3094:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6969              		.loc 1 3094 12 view .LVU2407
 6970 01e8 5BB1     		cbz	r3, .L453
3098:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmarx))
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 231


 6971              		.loc 1 3098 11 is_stmt 1 view .LVU2408
3098:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmarx))
 6972              		.loc 1 3098 43 is_stmt 0 view .LVU2409
 6973 01ea 144A     		ldr	r2, .L463+4
 6974 01ec 1A65     		str	r2, [r3, #80]
3099:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 6975              		.loc 1 3099 11 is_stmt 1 view .LVU2410
3099:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 6976              		.loc 1 3099 25 is_stmt 0 view .LVU2411
 6977 01ee E06F     		ldr	r0, [r4, #124]
 6978 01f0 FFF7FEFF 		bl	HAL_DMA_Abort_IT
 6979              	.LVL388:
3099:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 6980              		.loc 1 3099 14 discriminator 1 view .LVU2412
 6981 01f4 28B1     		cbz	r0, .L453
3101:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
 6982              		.loc 1 3101 13 is_stmt 1 view .LVU2413
 6983 01f6 D4F88430 		ldr	r3, [r4, #132]
 6984 01fa 43F04003 		orr	r3, r3, #64
 6985 01fe C4F88430 		str	r3, [r4, #132]
 6986              	.L453:
3105:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6987              		.loc 1 3105 9 view .LVU2414
3105:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6988              		.loc 1 3105 17 is_stmt 0 view .LVU2415
 6989 0202 A36F     		ldr	r3, [r4, #120]
3105:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****         {
 6990              		.loc 1 3105 12 view .LVU2416
 6991 0204 002B     		cmp	r3, #0
 6992 0206 3FF465AF 		beq	.L428
3109:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmatx))
 6993              		.loc 1 3109 11 is_stmt 1 view .LVU2417
3109:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmatx))
 6994              		.loc 1 3109 43 is_stmt 0 view .LVU2418
 6995 020a 0C4A     		ldr	r2, .L463+4
 6996 020c 1A65     		str	r2, [r3, #80]
3110:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 6997              		.loc 1 3110 11 is_stmt 1 view .LVU2419
3110:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 6998              		.loc 1 3110 25 is_stmt 0 view .LVU2420
 6999 020e A06F     		ldr	r0, [r4, #120]
 7000 0210 FFF7FEFF 		bl	HAL_DMA_Abort_IT
 7001              	.LVL389:
3110:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           {
 7002              		.loc 1 3110 14 discriminator 1 view .LVU2421
 7003 0214 0028     		cmp	r0, #0
 7004 0216 3FF45DAF 		beq	.L428
3112:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****           }
 7005              		.loc 1 3112 13 is_stmt 1 view .LVU2422
 7006 021a D4F88430 		ldr	r3, [r4, #132]
 7007 021e 43F04003 		orr	r3, r3, #64
 7008 0222 C4F88430 		str	r3, [r4, #132]
 7009 0226 55E7     		b	.L428
 7010              	.L452:
3119:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 7011              		.loc 1 3119 9 view .LVU2423
3119:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 232


 7012              		.loc 1 3119 21 is_stmt 0 view .LVU2424
 7013 0228 0123     		movs	r3, #1
 7014 022a 84F88130 		strb	r3, [r4, #129]
3125:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 7015              		.loc 1 3125 9 is_stmt 1 view .LVU2425
 7016 022e 2046     		mov	r0, r4
 7017 0230 FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 7018              	.LVL390:
3129:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   }
 7019              		.loc 1 3129 5 view .LVU2426
 7020 0234 4EE7     		b	.L428
 7021              	.L464:
 7022 0236 00BF     		.align	2
 7023              	.L463:
 7024 0238 94FCFFFF 		.word	-876
 7025 023c 00000000 		.word	SPI_DMAAbortOnError
 7026              		.cfi_endproc
 7027              	.LFE353:
 7029              		.section	.text.HAL_SPI_GetState,"ax",%progbits
 7030              		.align	1
 7031              		.global	HAL_SPI_GetState
 7032              		.syntax unified
 7033              		.thumb
 7034              		.thumb_func
 7036              	HAL_SPI_GetState:
 7037              	.LVL391:
 7038              	.LFB363:
3304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Return SPI handle state */
 7039              		.loc 1 3304 1 view -0
 7040              		.cfi_startproc
 7041              		@ args = 0, pretend = 0, frame = 0
 7042              		@ frame_needed = 0, uses_anonymous_args = 0
 7043              		@ link register save eliminated.
3306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 7044              		.loc 1 3306 3 view .LVU2428
3306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 7045              		.loc 1 3306 14 is_stmt 0 view .LVU2429
 7046 0000 90F88100 		ldrb	r0, [r0, #129]	@ zero_extendqisi2
 7047              	.LVL392:
3307:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 7048              		.loc 1 3307 1 view .LVU2430
 7049 0004 7047     		bx	lr
 7050              		.cfi_endproc
 7051              	.LFE363:
 7053              		.section	.text.HAL_SPI_GetError,"ax",%progbits
 7054              		.align	1
 7055              		.global	HAL_SPI_GetError
 7056              		.syntax unified
 7057              		.thumb
 7058              		.thumb_func
 7060              	HAL_SPI_GetError:
 7061              	.LVL393:
 7062              	.LFB364:
3316:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c ****   /* Return SPI ErrorCode */
 7063              		.loc 1 3316 1 is_stmt 1 view -0
 7064              		.cfi_startproc
 7065              		@ args = 0, pretend = 0, frame = 0
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 233


 7066              		@ frame_needed = 0, uses_anonymous_args = 0
 7067              		@ link register save eliminated.
3318:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 7068              		.loc 1 3318 3 view .LVU2432
3318:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** }
 7069              		.loc 1 3318 14 is_stmt 0 view .LVU2433
 7070 0000 D0F88400 		ldr	r0, [r0, #132]
 7071              	.LVL394:
3319:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_spi.c **** 
 7072              		.loc 1 3319 1 view .LVU2434
 7073 0004 7047     		bx	lr
 7074              		.cfi_endproc
 7075              	.LFE364:
 7077              		.text
 7078              	.Letext0:
 7079              		.file 2 "C:/Users/lenex/AppData/Roaming/Code/User/globalStorage/bmd.stm32-for-vscode/@xpack-dev-to
 7080              		.file 3 "C:/Users/lenex/AppData/Roaming/Code/User/globalStorage/bmd.stm32-for-vscode/@xpack-dev-to
 7081              		.file 4 "Drivers/CMSIS/Device/ST/STM32H7xx/Include/stm32h7a3xx.h"
 7082              		.file 5 "Drivers/CMSIS/Device/ST/STM32H7xx/Include/stm32h7xx.h"
 7083              		.file 6 "Drivers/STM32H7xx_HAL_Driver/Inc/stm32h7xx_hal_def.h"
 7084              		.file 7 "Drivers/STM32H7xx_HAL_Driver/Inc/stm32h7xx_hal_dma.h"
 7085              		.file 8 "Drivers/STM32H7xx_HAL_Driver/Inc/stm32h7xx_hal_spi.h"
 7086              		.file 9 "Drivers/CMSIS/Device/ST/STM32H7xx/Include/system_stm32h7xx.h"
 7087              		.file 10 "Drivers/STM32H7xx_HAL_Driver/Inc/stm32h7xx_hal.h"
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 234


DEFINED SYMBOLS
                            *ABS*:00000000 stm32h7xx_hal_spi.c
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:20     .text.SPI_RxISR_8BIT:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:25     .text.SPI_RxISR_8BIT:00000000 SPI_RxISR_8BIT
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:74     .text.SPI_RxISR_16BIT:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:79     .text.SPI_RxISR_16BIT:00000000 SPI_RxISR_16BIT
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:132    .text.SPI_RxISR_32BIT:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:137    .text.SPI_RxISR_32BIT:00000000 SPI_RxISR_32BIT
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:186    .text.SPI_TxISR_8BIT:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:191    .text.SPI_TxISR_8BIT:00000000 SPI_TxISR_8BIT
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:240    .text.SPI_TxISR_16BIT:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:245    .text.SPI_TxISR_16BIT:00000000 SPI_TxISR_16BIT
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:297    .text.SPI_TxISR_32BIT:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:302    .text.SPI_TxISR_32BIT:00000000 SPI_TxISR_32BIT
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:351    .text.SPI_AbortTransfer:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:356    .text.SPI_AbortTransfer:00000000 SPI_AbortTransfer
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:428    .text.SPI_AbortTransfer:00000070 $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:433    .text.SPI_CloseTransfer:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:438    .text.SPI_CloseTransfer:00000000 SPI_CloseTransfer
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:567    .text.SPI_CloseTransfer:000000c8 $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:572    .text.SPI_GetPacketSize:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:577    .text.SPI_GetPacketSize:00000000 SPI_GetPacketSize
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:612    .text.SPI_WaitOnFlagUntilTimeout:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:617    .text.SPI_WaitOnFlagUntilTimeout:00000000 SPI_WaitOnFlagUntilTimeout
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:690    .text.HAL_SPI_MspInit:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:696    .text.HAL_SPI_MspInit:00000000 HAL_SPI_MspInit
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:711    .text.HAL_SPI_Init:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:717    .text.HAL_SPI_Init:00000000 HAL_SPI_Init
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:1040   .text.HAL_SPI_Init:00000184 $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:1047   .text.HAL_SPI_MspDeInit:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:1053   .text.HAL_SPI_MspDeInit:00000000 HAL_SPI_MspDeInit
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:1068   .text.HAL_SPI_DeInit:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:1074   .text.HAL_SPI_DeInit:00000000 HAL_SPI_DeInit
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:1131   .text.HAL_SPI_Transmit:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:1137   .text.HAL_SPI_Transmit:00000000 HAL_SPI_Transmit
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:1673   .text.HAL_SPI_Receive:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:1679   .text.HAL_SPI_Receive:00000000 HAL_SPI_Receive
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:2346   .text.HAL_SPI_TransmitReceive:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:2352   .text.HAL_SPI_TransmitReceive:00000000 HAL_SPI_TransmitReceive
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:2969   .text.HAL_SPI_TransmitReceive:000002fc $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:2975   .text.HAL_SPI_TransmitReceive:00000304 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:3297   .text.HAL_SPI_Transmit_IT:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:3303   .text.HAL_SPI_Transmit_IT:00000000 HAL_SPI_Transmit_IT
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:3488   .text.HAL_SPI_Transmit_IT:000000cc $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:3495   .text.HAL_SPI_Receive_IT:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:3501   .text.HAL_SPI_Receive_IT:00000000 HAL_SPI_Receive_IT
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:3675   .text.HAL_SPI_Receive_IT:000000d0 $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:3682   .text.HAL_SPI_TransmitReceive_IT:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:3688   .text.HAL_SPI_TransmitReceive_IT:00000000 HAL_SPI_TransmitReceive_IT
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:3981   .text.HAL_SPI_TransmitReceive_IT:00000180 $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:3991   .text.HAL_SPI_Transmit_DMA:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:3997   .text.HAL_SPI_Transmit_DMA:00000000 HAL_SPI_Transmit_DMA
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:4345   .text.HAL_SPI_Transmit_DMA:000001b0 $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5810   .text.SPI_DMAHalfTransmitCplt:00000000 SPI_DMAHalfTransmitCplt
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5582   .text.SPI_DMATransmitCplt:00000000 SPI_DMATransmitCplt
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5966   .text.SPI_DMAError:00000000 SPI_DMAError
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:4352   .text.HAL_SPI_Receive_DMA:00000000 $t
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 235


C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:4358   .text.HAL_SPI_Receive_DMA:00000000 HAL_SPI_Receive_DMA
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:4719   .text.HAL_SPI_Receive_DMA:000001bc $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5862   .text.SPI_DMAHalfReceiveCplt:00000000 SPI_DMAHalfReceiveCplt
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5658   .text.SPI_DMAReceiveCplt:00000000 SPI_DMAReceiveCplt
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:4726   .text.HAL_SPI_TransmitReceive_DMA:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:4732   .text.HAL_SPI_TransmitReceive_DMA:00000000 HAL_SPI_TransmitReceive_DMA
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5184   .text.HAL_SPI_TransmitReceive_DMA:0000023c $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5914   .text.SPI_DMAHalfTransmitReceiveCplt:00000000 SPI_DMAHalfTransmitReceiveCplt
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5734   .text.SPI_DMATransmitReceiveCplt:00000000 SPI_DMATransmitReceiveCplt
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5191   .text.HAL_SPI_Abort:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5197   .text.HAL_SPI_Abort:00000000 HAL_SPI_Abort
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5466   .text.HAL_SPI_Abort:00000144 $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5472   .text.HAL_SPI_DMAPause:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5478   .text.HAL_SPI_DMAPause:00000000 HAL_SPI_DMAPause
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5500   .text.HAL_SPI_DMAResume:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5506   .text.HAL_SPI_DMAResume:00000000 HAL_SPI_DMAResume
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5528   .text.HAL_SPI_DMAStop:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5534   .text.HAL_SPI_DMAStop:00000000 HAL_SPI_DMAStop
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5556   .text.HAL_SPI_TxCpltCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5562   .text.HAL_SPI_TxCpltCallback:00000000 HAL_SPI_TxCpltCallback
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5577   .text.SPI_DMATransmitCplt:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5632   .text.HAL_SPI_RxCpltCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5638   .text.HAL_SPI_RxCpltCallback:00000000 HAL_SPI_RxCpltCallback
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5653   .text.SPI_DMAReceiveCplt:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5708   .text.HAL_SPI_TxRxCpltCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5714   .text.HAL_SPI_TxRxCpltCallback:00000000 HAL_SPI_TxRxCpltCallback
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5729   .text.SPI_DMATransmitReceiveCplt:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5784   .text.HAL_SPI_TxHalfCpltCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5790   .text.HAL_SPI_TxHalfCpltCallback:00000000 HAL_SPI_TxHalfCpltCallback
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5805   .text.SPI_DMAHalfTransmitCplt:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5836   .text.HAL_SPI_RxHalfCpltCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5842   .text.HAL_SPI_RxHalfCpltCallback:00000000 HAL_SPI_RxHalfCpltCallback
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5857   .text.SPI_DMAHalfReceiveCplt:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5888   .text.HAL_SPI_TxRxHalfCpltCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5894   .text.HAL_SPI_TxRxHalfCpltCallback:00000000 HAL_SPI_TxRxHalfCpltCallback
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5909   .text.SPI_DMAHalfTransmitReceiveCplt:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5940   .text.HAL_SPI_ErrorCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5946   .text.HAL_SPI_ErrorCallback:00000000 HAL_SPI_ErrorCallback
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:5961   .text.SPI_DMAError:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6016   .text.SPI_DMAAbortOnError:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6021   .text.SPI_DMAAbortOnError:00000000 SPI_DMAAbortOnError
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6057   .text.HAL_SPI_AbortCpltCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6063   .text.HAL_SPI_AbortCpltCallback:00000000 HAL_SPI_AbortCpltCallback
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6078   .text.HAL_SPI_Abort_IT:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6084   .text.HAL_SPI_Abort_IT:00000000 HAL_SPI_Abort_IT
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6411   .text.HAL_SPI_Abort_IT:00000164 $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6484   .text.SPI_DMATxAbortCallback:00000000 SPI_DMATxAbortCallback
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6424   .text.SPI_DMARxAbortCallback:00000000 SPI_DMARxAbortCallback
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6419   .text.SPI_DMARxAbortCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6479   .text.SPI_DMATxAbortCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6539   .text.HAL_SPI_SuspendCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6545   .text.HAL_SPI_SuspendCallback:00000000 HAL_SPI_SuspendCallback
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6560   .text.HAL_SPI_IRQHandler:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:6566   .text.HAL_SPI_IRQHandler:00000000 HAL_SPI_IRQHandler
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:7024   .text.HAL_SPI_IRQHandler:00000238 $d
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:7030   .text.HAL_SPI_GetState:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:7036   .text.HAL_SPI_GetState:00000000 HAL_SPI_GetState
ARM GAS  C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s 			page 236


C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:7054   .text.HAL_SPI_GetError:00000000 $t
C:\Users\lenex\AppData\Local\Temp\cceEyfn8.s:7060   .text.HAL_SPI_GetError:00000000 HAL_SPI_GetError

UNDEFINED SYMBOLS
HAL_GetTick
HAL_DMA_Start_IT
HAL_DMA_Abort
HAL_DMA_GetError
SystemCoreClock
HAL_DMA_Abort_IT
