(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "74AHC1G4210" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -3.81 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHC1G4210" (at 7.62 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5" (at 0 -13.97 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC1G4210.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "divider oscillator" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "10-stage divider and oscillator, SOT353-1" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*353*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74AHC1G4210_0_1"
      (rectangle (start -5.08 5.08) (end 5.08 -5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74AHC1G4210_1_1"
      (pin input line (at -10.16 2.54 0) (length 5.08)
        (name "X1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 5.08)
        (name "X2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 5.08)
        (name "Q" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC1G74" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G74" (at 10.16 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single D Flip-Flop D CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single D Flip-Flop, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74AUC1G74_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74AUC1G74_1_1"
      (pin input clock (at -12.7 -5.08 0) (length 5.08)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -5.08 180) (length 5.08)
        (name "~{Q}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "Q" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -12.7 90) (length 5.08)
        (name "~{CLR}" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 12.7 270) (length 5.08)
        (name "~{PRE}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUP1G74" (extends "74AUC1G74")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G74" (at 5.08 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single D Flip-Flop D CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single D Flip-Flop, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74CBT1G125" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74CBT1G125" (at 0 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single FET Bus Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single FET Bus Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74CBT1G125_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74CBT1G125_1_1"
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "~{OE}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 5.08 180) (length 5.08)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74CB3T1G125" (extends "74CBT1G125")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74CB3T1G125" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single FET Bus Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single FET Bus Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74CBTD1G125" (extends "74CBT1G125")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74CBTD1G125" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single FET Bus Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single FET Bus Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74CBTLV1G125" (extends "74CBT1G125")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74CBTLV1G125" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single FET Bus Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single FET Bus Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74CBT1G384" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74CBT1G384" (at 0 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single FET Bus Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single FET Bus Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74CBT1G384_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74CBT1G384_1_1"
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 5.08 180) (length 5.08)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "~{OE}" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74CBTD1G384" (extends "74CBT1G384")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74CBTD1G384" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single FET Bus Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single FET Bus Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G00" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G00" (at 7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g00.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NAND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NAND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G00_0_1"
      (arc (start 0 -5.08) (mid 5.0579 0) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
          (xy -7.62 5.08)
          (xy 0 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G00_1_1"
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AHC1G00" (extends "74LVC1G00")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHC1G00" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NAND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NAND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AHCT1G00" (extends "74LVC1G00")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHCT1G00" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NAND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NAND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUC1G00" (extends "74LVC1G00")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G00" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NAND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NAND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G00" (extends "74LVC1G00")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G00" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g00.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NAND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NAND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G02" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G02" (at 7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g02.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G02_0_1"
      (arc (start -7.62 -5.08) (mid -5.838 0) (end -7.62 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -5.08) (mid 3.1986 -3.2054) (end 5.08 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -2.54)
          (xy -6.35 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 2.54)
          (xy -6.35 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 5.08)
          (xy -7.62 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (arc (start 5.08 0) (mid 3.2238 3.2304) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "74LVC1G02_1_1"
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AHC1G02" (extends "74LVC1G02")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHC1G02" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AHCT1G02" (extends "74LVC1G02")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHCT1G02" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUC1G02" (extends "74LVC1G02")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G02" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G02" (extends "74LVC1G02")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G02" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g02.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G04" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G04" (at 5.08 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g04.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G04_0_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G04_1_1"
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AHC1G04" (extends "74LVC1G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHC1G04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AHC1GU04" (extends "74LVC1G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHC1GU04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "74AHC1G04, Single NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AHCT1G04" (extends "74LVC1G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHCT1G04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AHCT1GU04" (extends "74LVC1G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHCT1GU04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "74AHCT1G04, Single NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUC1G04" (extends "74LVC1G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUC1GU04" (extends "74LVC1G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1GU04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "74AUC1G04, Single NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G04" (extends "74LVC1G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g04.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1GU04" (extends "74LVC1G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1GU04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "74AUP1G04, Single NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1GU04" (extends "74LVC1G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1GU04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "74LVC1G04, Single NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G06" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G06" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS Open Drain" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOT Gate w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G06_0_1"
      (polyline
        (pts
          (xy -3.81 -1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -3.81 0)
          (xy -2.54 -1.27)
          (xy -1.27 0)
          (xy -2.54 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G06_1_1"
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC1G06" (extends "74LVC1G06")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G06" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS Open Drain" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOT Gate w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G06" (extends "74LVC1G06")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G06" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT LVC CMOS Open Drain" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOT Gate w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G07" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G07" (at 3.81 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g07.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff LVC CMOS Open Drain" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G07_0_1"
      (polyline
        (pts
          (xy -3.81 -1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -3.81 0)
          (xy -2.54 -1.27)
          (xy -1.27 0)
          (xy -2.54 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G07_1_1"
      (pin free line (at -2.54 -10.16 90) (length 6.35)
        (name "NC" (effects (font (size 0.762 0.762))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC1G07" (extends "74LVC1G07")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G07" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff LVC CMOS Open Drain" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G07" (extends "74LVC1G07")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G07" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g07" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff LVC CMOS Open Drain" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G08" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G08" (at 7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g08.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate AND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single AND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G08_0_1"
      (arc (start 0 -5.08) (mid 5.0579 0) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
          (xy -7.62 5.08)
          (xy 0 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G08_1_1"
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AHC1G08" (extends "74LVC1G08")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHC1G08" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate AND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single AND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AHCT1G08" (extends "74LVC1G08")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHCT1G08" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate AND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single AND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUC1G08" (extends "74LVC1G08")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G08" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate AND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single AND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G08" (extends "74LVC1G08")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G08" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g08.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate AND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single AND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G0832" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -7.62 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G0832" (at 0 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate AND-OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single AND-OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G0832_0_1"
      (arc (start -3.81 -1.27) (mid -0.0166 2.54) (end -3.81 6.35)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -5.08) (mid 1.782 0) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 0)
          (xy -8.89 0)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -10.16 5.08)
          (xy -8.89 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -8.89 6.35)
          (xy -3.81 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -2.54)
          (xy 1.27 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 2.54)
          (xy 1.27 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 7.62 -5.08)
          (xy 0 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 7.62 5.08)
          (xy 0 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -8.89 6.35)
          (xy -8.89 -1.27)
          (xy -3.81 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -2.54)
          (xy -1.27 -2.54)
          (xy -1.27 -3.81)
          (xy -1.27 -5.08)
          (xy -10.16 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 7.62 -5.08) (mid 10.8186 -3.2054) (end 12.7 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 12.7 0) (mid 10.8438 3.2304) (end 7.62 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "74LVC1G0832_1_1"
      (pin input line (at -17.78 5.08 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 20.32 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 -5.08 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G10" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G10" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NAND triple LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NAND 3 Input Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G10_0_1"
      (arc (start 0 -6.35) (mid 6.3224 0) (end 0 6.35)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -6.35)
          (xy -7.62 -6.35)
          (xy -7.62 6.35)
          (xy 0 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G10_1_1"
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -5.08 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 6.35)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 5.08 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G11" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G11" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate AND triple LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single AND 3 Input Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G11_0_1"
      (arc (start 0 -6.35) (mid 6.3224 0) (end 0 6.35)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -6.35)
          (xy -7.62 -6.35)
          (xy -7.62 6.35)
          (xy 0 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G11_1_1"
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -5.08 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 6.35)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 5.08 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G123" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G123" (at 3.81 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g123.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Mono Multivibrator CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Retrigerrable Monostabile Multivibrator, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP*2.95x2.8mm*P0.65* VSSOP*2.3x2mm*P0.5mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G123_1_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -12.7 -2.54 0) (length 5.08)
        (name "~{A}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -12.7 90) (length 5.08)
        (name "~{CLR}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "Q" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 5.08)
        (name "Cext" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "RCext" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC1G123_2_1"
      (rectangle (start -5.08 7.62) (end 5.08 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G125" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -10.16 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G125" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g125.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G125_0_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G125_1_1"
      (pin input inverted (at 0 10.16 270) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AHC1G125" (extends "74LVC1G125")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHC1G125" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AHCT1G125" (extends "74LVC1G125")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHCT1G125" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUC1G125" (extends "74LVC1G125")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G125" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G125" (extends "74LVC1G125")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G125" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G126" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G126" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G126_0_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G126_1_1"
      (pin input line (at 0 10.16 270) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AHC1G126" (extends "74LVC1G126")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHC1G126" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AHCT1G126" (extends "74LVC1G126")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHCT1G126" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUC1G126" (extends "74LVC1G126")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G126" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G126" (extends "74LVC1G126")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G126" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G139" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 7.62 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G139" (at 7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Decoder LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2 to 4 Decoder, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G139_0_1"
      (rectangle (start -3.81 6.35) (end 3.81 -6.35)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G139_1_1"
      (pin input line (at -10.16 2.54 0) (length 6.25)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 6.25)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -5.08 180) (length 6.35)
        (name "Y3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 6.25)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -2.54 180) (length 6.35)
        (name "Y2" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 2.54 180) (length 6.35)
        (name "Y1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 5.08 180) (length 6.35)
        (name "Y0" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 6.25)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G14" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G14" (at 7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Schmitt NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G14_0_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy -1.27 -1.27)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -1.27)
          (xy -2.54 -1.27)
          (xy -2.54 1.27)
          (xy 0 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G14_1_1"
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AHC1G14" (extends "74LVC1G14")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHC1G14" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g14.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Schmitt NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AHCT1G14" (extends "74LVC1G14")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHCT1G14" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Schmitt NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUC1G14" (extends "74LVC1G14")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G14" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Schmitt NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G14" (extends "74LVC1G14")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G14" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Schmitt NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G17" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G17" (at 5.08 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at -2.54 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g17.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Schmitt LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Schmitt Buffer Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G17_0_1"
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -1.27 1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 1.27)
          (xy -2.54 1.27)
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G17_1_1"
      (pin free line (at -2.54 -10.16 90) (length 6.35)
        (name "NC" (effects (font (size 0.762 0.762))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC1G17" (extends "74LVC1G17")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G17" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Schmitt LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Schmitt Buffer Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G17" (extends "74LVC1G17")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G17" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff Schmitt LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Schmitt Buffer Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G175" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G175" (at 10.16 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single D Flip-Flop Clear CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single D Flip-Flop w/ Asnynchronus Clear, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G175_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G175_1_1"
      (pin input clock (at -12.7 0 0) (length 5.08)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "Q" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "~{CLR}" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G18" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 6.35 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G18" (at 7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at -2.54 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "Single Demux LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Demultiplexer, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G18_1_1"
      (polyline
        (pts
          (xy -2.54 -7.62)
          (xy 0 -7.62)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 2.54)
          (xy -2.54 -2.54)
          (xy 2.54 -5.08)
          (xy 2.54 -1.27)
          (xy 2.54 0)
          (xy 2.54 1.27)
          (xy 2.54 5.08)
          (xy -2.54 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -10.16 -7.62 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 -2.54 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 2.54 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC1G18_2_1"
      (rectangle (start -5.08 5.08) (end 5.08 -5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin power_in line (at 0 -12.7 90) (length 7.62)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC1G18" (extends "74LVC1G18")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G18" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Demux LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Demultiplexer, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G19" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G19" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Decoder LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1 of 2 Decoder, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G19_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G19_1_1"
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "~{E}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -5.08 180) (length 5.08)
        (name "Y1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "Y0" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC1G19" (extends "74LVC1G19")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G19" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Decoder LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single 1 of 2 Decoder, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G240" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G240" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff/Drv Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer/Driver Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G240_0_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G240_1_1"
      (pin input inverted (at 0 10.16 270) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC1G240" (extends "74LVC1G240")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G240" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff/Drv Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer/Driver Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G240" (extends "74LVC1G240")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G240" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff/Drv Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffer/Driver Gate Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G27" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G27" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NOR triple LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NOR 3 Input Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G27_0_1"
      (arc (start -7.62 -6.35) (mid -5.321 0) (end -7.62 6.35)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -6.35) (mid 3.9978 -3.9978) (end 6.35 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -6.35)
          (xy -7.62 -6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 6.35)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (arc (start 6.35 0) (mid 3.9978 3.9978) (end 0 6.35)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "74LVC1G27_1_1"
      (pin input line (at -12.698 0 0) (length 7.11)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.698 -5.08 0) (length 5.84)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 6.35)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.698 5.08 0) (length 5.84)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G29" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G29" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Decoder LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2 of 3 Decoder, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G29_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G29_1_1"
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "~{G}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 5.08)
        (name "Y1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 5.08)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -5.08 180) (length 5.08)
        (name "Y2" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "Y0" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G3157" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G3157" (at 10.16 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "SPDT Analog Switch CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "SPDT Analog Switch, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G3157_1_1"
      (polyline
        (pts
          (xy -7.62 -10.16)
          (xy -5.08 -10.16)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 0)
          (xy -5.08 0)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -3.81)
          (xy 0 2.032)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -5.08)
          (xy 2.54 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 5.08 5.08)
          (xy 2.54 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -2.54 -5.08)
          (xy 0 -6.35)
          (xy -2.54 -7.62)
          (xy -2.54 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -2.54)
          (xy -2.54 -5.08)
          (xy 0 -3.81)
          (xy -2.54 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 5.08)
          (xy 0 3.81)
          (xy -2.54 2.54)
          (xy -2.54 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 7.62)
          (xy 0 6.35)
          (xy -2.54 5.08)
          (xy -2.54 7.62)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -0.762)
          (xy -3.81 -0.762)
          (xy -3.81 -10.16)
          (xy -5.08 -10.16)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -5.08)
          (xy 0 -6.35)
          (xy 2.54 -7.62)
          (xy 2.54 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -2.54)
          (xy 2.54 -5.08)
          (xy 0 -3.81)
          (xy 2.54 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 5.08)
          (xy 2.54 2.54)
          (xy 0 3.81)
          (xy 2.54 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 5.08)
          (xy 2.54 7.62)
          (xy 0 6.35)
          (xy 2.54 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 5.08)
          (xy -5.08 5.08)
          (xy -5.08 0)
          (xy -5.08 -5.08)
          (xy -2.54 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (circle (center 0 2.794) (radius 0.762)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (pin bidirectional line (at 10.16 5.08 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -5.08 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 0 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -10.16 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC1G3157_2_1"
      (rectangle (start -2.54 5.08) (end 2.54 -5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G32" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G32" (at 7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G32_0_1"
      (arc (start -7.62 -5.08) (mid -5.838 0) (end -7.62 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -5.08) (mid 3.1986 -3.2054) (end 5.08 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -2.54)
          (xy -6.35 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 2.54)
          (xy -6.35 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 5.08)
          (xy -7.62 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (arc (start 5.08 0) (mid 3.2238 3.2304) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "74LVC1G32_1_1"
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AHC1G32" (extends "74LVC1G32")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHC1G32" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AHCT1G32" (extends "74LVC1G32")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHCT1G32" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUC1G32" (extends "74LVC1G32")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G32" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G32" (extends "74LVC1G32")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G32" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g32.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G3208" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -7.62 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G3208" (at 0 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate OR-AND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single OR-AND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G3208_0_1"
      (arc (start -8.89 -1.27) (mid -8.108 2.54) (end -8.89 6.35)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start -5.08 -1.27) (mid -1.8194 -0.3322) (end 0 2.54)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 0)
          (xy -8.89 0)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -10.16 5.08)
          (xy -8.89 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -5.08 -1.27)
          (xy -8.89 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -5.08 6.35)
          (xy -8.89 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 5.08)
          (xy 0 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 7.62 -5.08)
          (xy 0 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 7.62 5.08)
          (xy 0 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -2.54)
          (xy -1.27 -2.54)
          (xy -1.27 -3.81)
          (xy -1.27 -5.08)
          (xy -10.16 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 2.54) (mid -1.8444 5.3784) (end -5.08 6.35)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 7.62 -5.08) (mid 12.6779 0) (end 7.62 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "74LVC1G3208_1_1"
      (pin input line (at -17.78 5.08 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 20.32 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 -5.08 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G332" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G332" (at 10.16 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at -1.27 -20.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate OR triple LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single OR 3 Input Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G332_0_1"
      (arc (start -7.62 -6.35) (mid -5.321 0) (end -7.62 6.35)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -6.35) (mid 3.9978 -3.9978) (end 6.35 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -6.35)
          (xy -7.62 -6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 6.35)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (arc (start 6.35 0) (mid 3.9978 3.9978) (end 0 6.35)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "74LVC1G332_1_0"
      (pin input line (at -10.16 3.81 0) (length 4)
        (name "" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -3.81 0) (length 4)
        (name "" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 4.8)
        (name "" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC1G332_1_1"
      (pin power_in line (at 0 -10.16 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 6.35)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G34" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G34" (at 5.08 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g34.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffef Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G34_0_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G34_1_1"
      (pin free line (at -2.54 -10.16 90) (length 6.35)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUP1G34" (extends "74LVC1G34")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G34" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g34.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate Buff LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Buffef Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G373" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G373" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single D Latch CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single D Latch, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G373_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G373_1_1"
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "LE" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 5.08 180) (length 5.08)
        (name "Q" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -5.08 180) (length 5.08)
        (name "~{OE}" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G374" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G374" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single D Flip-Flop Tri-State CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single D Flip-Flop Tri-State Output, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G374_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G374_1_1"
      (pin input clock (at -12.7 -5.08 0) (length 5.08)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 5.08 180) (length 5.08)
        (name "Q" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -5.08 180) (length 5.08)
        (name "~{OE}" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G38" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G38" (at 7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate NAND Open Drain LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single NAND Gate Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G38_0_1"
      (arc (start 0 -5.08) (mid 5.0579 0) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -5.08 -1.27)
          (xy -2.54 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
          (xy -7.62 5.08)
          (xy 0 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 1.27)
          (xy -5.08 0)
          (xy -3.81 -1.27)
          (xy -2.54 0)
          (xy -3.81 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G38_1_1"
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G386" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G386" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate EX-OR triple LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single EX-OR 3 Input Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G386_0_1"
      (arc (start -8.89 -6.35) (mid -6.2598 0) (end -8.89 6.35)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start -7.62 -6.35) (mid -5.321 0) (end -7.62 6.35)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -6.35) (mid 3.9978 -3.9978) (end 6.35 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -6.35)
          (xy -7.62 -6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 6.35)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (arc (start 6.35 0) (mid 3.9978 3.9978) (end 0 6.35)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "74LVC1G386_1_1"
      (pin input line (at -12.698 0 0) (length 7.11)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.698 -5.08 0) (length 5.84)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 6.35)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.698 5.08 0) (length 5.84)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC1G57" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G57" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Configurable Single Gate LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G57_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G57_1_1"
      (pin input line (at -12.7 0 0) (length 5.08)
        (name "IN1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "IN0" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 5.08)
        (name "Y" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "IN2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUP1G57" (extends "74LVC1G57")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G57" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Configurable Single Gate LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G97" (extends "74LVC1G57")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G97" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Configurable Single Gate LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G97" (extends "74LVC1G57")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G97" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Configurable Single Gate LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G58" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G58" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Configurable Single Gate LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G58_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G58_1_1"
      (pin input line (at -12.7 0 0) (length 5.08)
        (name "IN1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "IN0" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 5.08)
        (name "~{Y}" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "IN2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUP1G58" (extends "74LVC1G58")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G58" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Configurable Single Gate LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "74LAUP1G58, Configurable Multi-Function Single Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G98" (extends "74LVC1G58")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G98" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Configurable Single Gate LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G98" (extends "74LVC1G58")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G98" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Configurable Single Gate LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G66" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G66" (at 7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g66.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "Single Bilateral Analog Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Bilateral Analog Switch, SOT-23-5/SC-70-5" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G66_1_1"
      (polyline
        (pts
          (xy -7.62 0)
          (xy -3.81 0)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -7.62)
          (xy 0 -7.62)
          (xy 0 -1.905)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -7.62)
          (xy -7.62 5.715)
          (xy 0 5.715)
          (xy 0 3.175)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.81 0)
          (xy 3.81 3.81)
          (xy 3.81 -3.81)
          (xy -3.81 0)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 3.81 0)
          (xy -3.81 3.81)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (circle (center 0 2.54) (radius 0.635)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (pin bidirectional line (at -12.7 0 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 0 180) (length 6.25)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.62 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC1G66_2_1"
      (rectangle (start -5.08 5.08) (end 5.08 -5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC1G66" (extends "74LVC1G66")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G66" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74auc1g66.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Bilateral Analog Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Bilateral Analog Switch, SOT-23-5/SC-70-5" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SC*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G79" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G79" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single D Flip-Flop D CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single D Flip-Flop, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G79_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G79_1_1"
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -12.7 -5.08 0) (length 5.08)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "Q" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC1G79" (extends "74LVC1G79")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G79" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single D Flip-Flop D CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single D Flip-Flop, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G79" (extends "74LVC1G79")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G79" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single D Flip-Flop D CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single D Flip-Flop, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G80" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G80" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single D Flip-Flop CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single D Flip-Flop Iverted Output, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G80_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G80_1_1"
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -12.7 -5.08 0) (length 5.08)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "~{Q}" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC1G80" (extends "74LVC1G80")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G80" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single D Flip-Flop CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single D Flip-Flop Iverted Output, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUP1G80" (extends "74LVC1G80")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUP1G80" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single D Flip-Flop CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single D Flip-Flop Iverted Output, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G86" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1G86" (at 7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate EX-OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single EX-OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G86_0_1"
      (arc (start -8.89 -5.08) (mid -6.7858 0) (end -8.89 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start -7.62 -5.08) (mid -5.838 0) (end -7.62 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -5.08) (mid 3.1986 -3.2054) (end 5.08 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -2.54)
          (xy -6.35 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 2.54)
          (xy -6.35 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 5.08)
          (xy -7.62 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (arc (start 5.08 0) (mid 3.2238 3.2304) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "74LVC1G86_1_1"
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AHC1G86" (extends "74LVC1G86")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHC1G86" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate EX-OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single EX-OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AHCT1G86" (extends "74LVC1G86")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHCT1G86" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate EX-OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single EX-OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUC1G86" (extends "74LVC1G86")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC1G86" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Gate EX-OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single EX-OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT* SG-*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1G99" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -3.81 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "74LVC1G99" (at 1.27 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/gpn/sn74lvc1g99" (at 0 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Configurable Single Gate LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1G99_0_1"
      (rectangle (start -5.08 7.62) (end 5.08 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC1G99_1_1"
      (pin input line (at -10.16 5.08 0) (length 5.08)
        (name "~{OE}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 5.08)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 5.08)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 5.08)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 5.08)
        (name "Y" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUP1G99" (extends "74LVC1G99")
    (property "Reference" "U" (at -3.81 6.985 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "74AUP1G99" (at -3.81 5.715 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Configurable Single Gate LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC1GU04DRL" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC1GU04DRL" (at 17.78 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-553" (at 0 -12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1gu04.pdf" (at -3.81 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "inverter cmos" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Inverter Gate, SOT-553" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*553*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC1GU04DRL_0_1"
      (rectangle (start -5.08 7.62) (end -5.08 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -5.08 -7.62)
          (xy 10.16 0)
          (xy -5.08 7.62)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (circle (center 11.43 0) (radius 1.27)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "74LVC1GU04DRL_1_1"
      (pin no_connect line (at 10.16 0 180) (length 5.08) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 17.78 0 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC2G00" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G00" (at 7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NAND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual NAND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G00_1_1"
      (arc (start 0 -5.08) (mid 5.0579 0) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
          (xy -7.62 5.08)
          (xy 0 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G00_2_1"
      (arc (start 0 -5.08) (mid 5.0579 0) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
          (xy -7.62 5.08)
          (xy 0 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G00_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G00_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AHC2G00" (extends "74LVC2G00")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHC2G00" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT2G00.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NAND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual NAND Gate, High-speed Si-gate CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AHCT2G00" (extends "74LVC2G00")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AHCT2G00" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT2G00.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NAND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual NAND Gate, TTL input High-speed Si-gate CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUC2G00" (extends "74LVC2G00")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G00" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NAND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual NAND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G02" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G02" (at 7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NOR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual NOR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G02_1_1"
      (arc (start -7.62 -5.08) (mid -5.838 0) (end -7.62 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -5.08) (mid 3.1986 -3.2054) (end 5.08 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -2.54)
          (xy -6.35 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 2.54)
          (xy -6.35 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 5.08)
          (xy -7.62 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (arc (start 5.08 0) (mid 3.2238 3.2304) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G02_2_1"
      (arc (start -7.62 -5.08) (mid -5.838 0) (end -7.62 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -5.08) (mid 3.1986 -3.2054) (end 5.08 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -2.54)
          (xy -6.35 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 2.54)
          (xy -6.35 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 5.08)
          (xy -7.62 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (arc (start 5.08 0) (mid 3.2238 3.2304) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G02_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G02_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G02" (extends "74LVC2G02")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G02" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NOR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual NOR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G04" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G04" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SG-* SOT*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G04_1_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G04_2_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G04_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G04_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G04" (extends "74LVC2G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SG-* SOT*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74AUC2GU04" (extends "74LVC2G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2GU04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "74AUC2G04, Dual NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SG-* SOT*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2GU04" (extends "74LVC2G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2GU04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "74LVC2G04, Dual NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SG-* SOT*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G06" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G06" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NOT Open Drain LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual NOT Gate w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SG-* SOT*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G06_1_1"
      (polyline
        (pts
          (xy -3.81 -1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -3.81 0)
          (xy -2.54 -1.27)
          (xy -1.27 0)
          (xy -2.54 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G06_2_1"
      (polyline
        (pts
          (xy -3.81 -1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -3.81 0)
          (xy -2.54 -1.27)
          (xy -1.27 0)
          (xy -2.54 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G06_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G06_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G06" (extends "74LVC2G06")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G06" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NOT Open Drain LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual NOT Gate w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SG-* SOT*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G07" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G07" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate Buffer Open Drain LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Buffer w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SG-* SOT*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G07_1_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 1.27)
          (xy -2.54 0)
          (xy -1.27 -1.27)
          (xy 0 0)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G07_2_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 1.27)
          (xy -2.54 0)
          (xy -1.27 -1.27)
          (xy 0 0)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G07_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G07_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G07" (extends "74LVC2G07")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G07" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate Buffer Open Drain LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Buffer w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SG-* SOT*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G08" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -10.16 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G08" (at -10.16 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate AND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual AND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G08_1_1"
      (arc (start 0 -5.08) (mid 5.0579 0) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
          (xy -7.62 5.08)
          (xy 0 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G08_2_1"
      (arc (start 0 -5.08) (mid 5.0579 0) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
          (xy -7.62 5.08)
          (xy 0 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G08_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G08_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G08" (extends "74LVC2G08")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G08" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate AND LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual AND Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G125" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G125" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Buffer Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G125_1_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input inverted (at 0 10.16 270) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G125_2_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin tri_state line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at 0 10.16 270) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G125_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G125_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G125" (extends "74LVC2G125")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G125" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Buffer Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G126" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G126" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Buffer Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G126_1_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at 0 7.62 270) (length 5.46)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G126_2_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin tri_state line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.46)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G126_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G126_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G126" (extends "74LVC2G126")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G126" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Buffer Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G14" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G14" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc2g14.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NOT Schmitt LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual NOT Gate Schmitt Triggered, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SG-* SOT*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G14_1_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy -1.27 -1.27)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -1.27)
          (xy -2.54 -1.27)
          (xy -2.54 1.27)
          (xy 0 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G14_2_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy -1.27 -1.27)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -1.27)
          (xy -2.54 -1.27)
          (xy -2.54 1.27)
          (xy 0 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G14_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G14_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC2G157" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G157" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single Mux CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single 2 to 1 Multiplexer, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G157_0_1"
      (rectangle (start -3.81 7.62) (end 3.81 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G157_1_1"
      (pin input line (at -10.16 5.08 0) (length 6.25)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 6.25)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -2.54 180) (length 6.35)
        (name "~{Y}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 2.54 180) (length 6.35)
        (name "Y" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 6.25)
        (name "~{A}/B" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 6.25)
        (name "~{G}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC2G17" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -1.27 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G17" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Buffer Schmitt LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Buffer Schmitt Triggered, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SG-* SOT*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G17_1_1"
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -1.27 1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 1.27)
          (xy -2.54 1.27)
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G17_2_1"
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -1.27 1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 1.27)
          (xy -2.54 1.27)
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G17_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G17_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC2G240" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G240" (at 5.08 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Inv Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Inverter Buffer Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G240_1_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input inverted (at 0 10.16 270) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G240_2_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin tri_state inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at 0 10.16 270) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G240_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G240_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G240" (extends "74LVC2G240")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G240" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Inv Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Inverter Buffer Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G241" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G241" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Buffer Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G241_1_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input inverted (at 0 10.16 270) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G241_2_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin tri_state line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at 0 10.16 270) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G241_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G241_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G241" (extends "74LVC2G241")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G241" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Buff Tri-State LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Buffer Tri-State, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G32" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -7.62 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G32" (at -7.62 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G32_1_1"
      (arc (start -7.62 -5.08) (mid -5.838 0) (end -7.62 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -5.08) (mid 3.1986 -3.2054) (end 5.08 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -2.54)
          (xy -6.35 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 2.54)
          (xy -6.35 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 5.08)
          (xy -7.62 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (arc (start 5.08 0) (mid 3.2238 3.2304) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G32_2_1"
      (arc (start -7.62 -5.08) (mid -5.838 0) (end -7.62 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -5.08) (mid 3.1986 -3.2054) (end 5.08 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -2.54)
          (xy -6.35 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 2.54)
          (xy -6.35 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 5.08)
          (xy -7.62 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (arc (start 5.08 0) (mid 3.2238 3.2304) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G32_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G32_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G32" (extends "74LVC2G32")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G32" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G34" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G34" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Buffer LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Buffer, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SG-* SOT*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G34_1_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G34_2_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G34_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G34_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G34" (extends "74LVC2G34")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G34" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Buffer LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Buffer, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SG-* SOT*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G38" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G38" (at 0 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate NAND Open Drain LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual NAND Gate w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G38_1_1"
      (arc (start 0 -5.08) (mid 5.0579 0) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
          (xy -7.62 5.08)
          (xy 0 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -3.81 0)
          (xy -2.54 -1.27)
          (xy -1.27 0)
          (xy -2.54 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G38_2_1"
      (arc (start 0 -5.08) (mid 5.0579 0) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
          (xy -7.62 5.08)
          (xy 0 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -3.81 0)
          (xy -2.54 -1.27)
          (xy -1.27 0)
          (xy -2.54 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin open_collector inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G38_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G38_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC2G53" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G53" (at 6.35 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "Analog Switch 1 to 2 CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1 to 2 Analog Switch Mux/Demux, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G53_1_1"
      (circle (center -2.54 0) (radius 0.127)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (circle (center 0 -3.556) (radius 0.254)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (circle (center 0 -0.381) (radius 0.127)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.81 -5.08)
          (xy -2.54 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 0)
          (xy -2.54 0)
        )
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 2.54 -2.54)
          (xy 1.27 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 2.54 2.54)
          (xy 1.27 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -3.81)
          (xy 0 -5.08)
          (xy 2.54 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 1.016)
          (xy 0 0)
          (xy 0 -1.905)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 -2.54)
          (xy 0 -3.175)
          (xy -1.27 -3.81)
          (xy -1.27 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 -1.27)
          (xy -1.27 -2.54)
          (xy 0 -1.905)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 2.54)
          (xy 0 1.905)
          (xy -1.27 1.27)
          (xy -1.27 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 3.81)
          (xy 0 3.175)
          (xy -1.27 2.54)
          (xy -1.27 3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -0.381)
          (xy -1.905 -0.381)
          (xy -1.905 -5.08)
          (xy -2.54 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -2.54)
          (xy 0 -3.175)
          (xy 1.27 -3.81)
          (xy 1.27 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 1.27 -1.27)
          (xy 1.27 -2.54)
          (xy 0 -1.905)
          (xy 1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 1.27 2.54)
          (xy 1.27 1.27)
          (xy 0 1.905)
          (xy 1.27 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 1.27 2.54)
          (xy 1.27 3.81)
          (xy 0 3.175)
          (xy 1.27 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 1.905 -5.08)
          (xy 1.905 5.08)
          (xy 0 5.08)
          (xy 0 3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 2.54)
          (xy -2.54 2.54)
          (xy -2.54 0)
          (xy -2.54 -2.54)
          (xy -1.27 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (circle (center 0 1.397) (radius 0.381)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (circle (center 0 3.556) (radius 0.254)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (circle (center 1.905 -5.08) (radius 0.127)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (pin bidirectional line (at -10.16 0 0) (length 6.25)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 7.62 -5.08 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 6.25)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 7.62 -2.54 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 7.62 2.54 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G53_2_1"
      (rectangle (start -5.08 5.08) (end 5.08 -5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin passive line (at 0 -10.157 90) (length 4.95) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.157 90) (length 4.95)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G53" (extends "74LVC2G53")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G53" (at 0 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Analog Switch 1 to 2 CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1 to 2 Analog Switch Mux/Demux, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G66" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G66" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "Dual Analog Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Analog Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G66_1_1"
      (circle (center -7.112 -7.62) (radius 0.254)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 0)
          (xy -5.08 0)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy 7.62 0)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 5.08 5.08)
          (xy 5.08 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -7.62)
          (xy 0 -7.62)
          (xy 0 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 -5.08)
          (xy 5.08 0)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 5.08)
          (xy -5.08 0)
          (xy 5.08 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 4.318)
          (xy 0 6.604)
          (xy -7.112 6.604)
          (xy -7.112 -7.62)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (circle (center 0 3.556) (radius 0.762)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (pin input line (at -12.7 0 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 0 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.62 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G66_2_1"
      (circle (center -7.112 -7.62) (radius 0.254)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 0)
          (xy -5.08 0)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy 7.62 0)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 5.08 5.08)
          (xy 5.08 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 -7.62)
          (xy 0 -7.62)
          (xy 0 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 -5.08)
          (xy 5.08 0)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 5.08 5.08)
          (xy -5.08 0)
          (xy 5.08 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 4.318)
          (xy 0 6.604)
          (xy -7.112 6.604)
          (xy -7.112 -7.62)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (circle (center 0 3.556) (radius 0.762)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (pin input line (at -12.7 -7.62 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 0 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G66_3_1"
      (rectangle (start -5.08 5.08) (end 5.08 -5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G66" (extends "74LVC2G66")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G66" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Analog Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Analog Switch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G74" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G74" (at 10.16 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Single D Flip-Flop D CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "74AUC1G74, Single D Flip-Flop, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G74_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G74_1_1"
      (pin input clock (at -12.7 -2.54 0) (length 5.08)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -5.08 180) (length 5.08)
        (name "~{Q}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "Q" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "~{CLR}" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "~{PRE}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC2G79" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G79" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual D Flip-Flop D CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual D Flip-Flop, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G79_1_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input clock (at -12.7 -5.08 0) (length 5.08)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "Q" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G79_2_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "Q" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -12.7 -5.08 0) (length 5.08)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G79_3_0"
      (rectangle (start -5.08 -7.62) (end 5.08 7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G79_3_1"
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G79" (extends "74LVC2G79")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G79" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual D Flip-Flop D CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual D Flip-Flop, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G80" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G80" (at 7.62 -10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual D Flip-Flop Negative CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual D Flip-Flop w/ Negative Output, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G80_1_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input clock (at -12.7 -5.08 0) (length 5.08)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "~{Q}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G80_2_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "~{Q}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -12.7 -5.08 0) (length 5.08)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G80_3_0"
      (rectangle (start -5.08 -7.62) (end 5.08 7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G80_3_1"
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G80" (extends "74LVC2G80")
    (property "Reference" "U" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G80" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual D Flip-Flop Negative CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual D Flip-Flop w/ Negative Output, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC2G86" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC2G86" (at 0 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate EX-OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual EX-OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC2G86_1_1"
      (arc (start -8.89 -5.08) (mid -7.108 0) (end -8.89 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start -7.62 -5.08) (mid -5.838 0) (end -7.62 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -5.08) (mid 3.1986 -3.2054) (end 5.08 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -2.54)
          (xy -6.35 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 2.54)
          (xy -6.35 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 5.08)
          (xy -7.62 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (arc (start 5.08 0) (mid 3.2238 3.2304) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G86_2_1"
      (arc (start -8.89 -5.08) (mid -7.108 0) (end -8.89 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start -7.62 -5.08) (mid -5.838 0) (end -7.62 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 0 -5.08) (mid 3.1986 -3.2054) (end 5.08 0)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -2.54)
          (xy -6.35 -2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 2.54)
          (xy -6.35 2.54)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy -7.62 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 5.08)
          (xy -7.62 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (arc (start 5.08 0) (mid 3.2238 3.2304) (end 0 5.08)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC2G86_3_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC2G86_3_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74AUC2G86" (extends "74LVC2G86")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74AUC2G86" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Dual Gate EX-OR LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual EX-OR Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC3G04" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC3G04" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Triple Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Triple NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC3G04_1_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G04_2_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G04_3_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G04_4_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC3G04_4_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC3GU04" (extends "74LVC3G04")
    (property "Reference" "U" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC3GU04" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Triple Gate NOT LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "74LVC3G04, Triple NOT Gate, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LVC3G06" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC3G06" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Triple Gate NOT Open Drain LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Triple NOT Gate w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC3G06_1_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 1.27)
          (xy -2.54 0)
          (xy -1.27 -1.27)
          (xy 0 0)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G06_2_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 1.27)
          (xy -2.54 0)
          (xy -1.27 -1.27)
          (xy 0 0)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin open_collector inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G06_3_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 1.27)
          (xy -2.54 0)
          (xy -1.27 -1.27)
          (xy 0 0)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G06_4_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC3G06_4_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC3G07" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC3G07" (at 1.27 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Triple Buff Open Drain LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Triple Buffer w/ Open Drain, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC3G07_1_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 1.27)
          (xy -2.54 0)
          (xy -1.27 -1.27)
          (xy 0 0)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G07_2_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 1.27)
          (xy -2.54 0)
          (xy -1.27 -1.27)
          (xy 0 0)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin open_collector line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G07_3_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 1.27)
          (xy -2.54 0)
          (xy -1.27 -1.27)
          (xy 0 0)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G07_4_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC3G07_4_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC3G14" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC3G14" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at -1.27 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc3g14.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Triple NOT Schmitt LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Triple NOT Gate Schmitt, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC3G14_1_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy -1.27 -1.27)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -1.27)
          (xy -2.54 -1.27)
          (xy -2.54 1.27)
          (xy 0 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G14_2_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy -1.27 -1.27)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -1.27)
          (xy -2.54 -1.27)
          (xy -2.54 1.27)
          (xy 0 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G14_3_1"
      (polyline
        (pts
          (xy -2.54 -1.27)
          (xy -1.27 -1.27)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -1.27)
          (xy -2.54 -1.27)
          (xy -2.54 1.27)
          (xy 0 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G14_4_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC3G14_4_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC3G17" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC3G17" (at 2.54 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Triple Buf Schmitt LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Triple Buffer Schmitt, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC3G17_1_1"
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -1.27 1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 1.27)
          (xy -2.54 1.27)
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G17_2_1"
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -1.27 1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 1.27)
          (xy -2.54 1.27)
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G17_3_1"
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -1.27 1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 1.27)
          (xy -2.54 1.27)
          (xy -2.54 -1.27)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G17_4_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC3G17_4_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "74LVC3G34" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -2.54 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LVC3G34" (at 1.27 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Triple Buf LVC CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Triple Buffer, Low-Voltage CMOS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP* VSSOP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LVC3G34_1_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G34_2_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G34_3_1"
      (polyline
        (pts
          (xy -7.62 6.35)
          (xy -7.62 -6.35)
          (xy 5.08 0)
          (xy -7.62 6.35)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -15.24 0 0) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 7.62)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LVC3G34_4_0"
      (rectangle (start -5.08 -5.08) (end 5.08 5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LVC3G34_4_1"
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "NC7SVU04P5X" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "NC7SVU04P5X" (at 15.24 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5" (at 0 -12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/NC7SVU04-D.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "inverter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "High-Speed Logic Inverter, SOT-353" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*353*SC*70*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "NC7SVU04P5X_0_1"
      (polyline
        (pts
          (xy -5.08 7.62)
          (xy -5.08 -7.62)
          (xy 10.16 0)
          (xy -5.08 7.62)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (circle (center 11.43 0) (radius 1.27)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "NC7SVU04P5X_1_1"
      (pin no_connect line (at 10.16 0 180) (length 5.08) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 17.78 0 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "NC7SZ125M5X" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "NC7SZ125M5X" (at 7.62 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (at 16.51 -6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pdf/datasheet/nc7sz125-d.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "buffer three-state" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "TinyLogic UHS Buffer with Three-State Output, SOT-23-5" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "NC7SZ125M5X_0_1"
      (rectangle (start -5.08 5.08) (end 5.08 -5.08)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "NC7SZ125M5X_1_1"
      (pin input line (at -10.16 -2.54 0) (length 5.08)
        (name "~{OE}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 5.08)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 2.54 180) (length 5.08)
        (name "Y" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "NC7SZ125P5X" (extends "NC7SZ125M5X")
    (property "Reference" "U" (at -5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "NC7SZ125P5X" (at 7.62 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5" (at 20.32 -6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pdf/datasheet/nc7sz125-d.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "buffer three-state" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "TinyLogic UHS Buffer with Three-State Output, SOT-353" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT*353*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "SN74LVC1G14DBV" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SN74LVC1G14DBV" (at 20.32 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (at 0 -12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g14.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Inverter Schmitt Trigger" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Schmitt-Trigger Inverter, SOT-23" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SN74LVC1G14DBV_0_1"
      (polyline
        (pts
          (xy -2.032 1.016)
          (xy -1.016 1.016)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -5.08 7.62)
          (xy -5.08 -7.62)
          (xy 10.16 0)
          (xy -5.08 7.62)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.048 -1.016)
          (xy -3.048 1.016)
          (xy -2.032 1.016)
          (xy -2.032 -1.016)
          (xy -4.064 -1.016)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (circle (center 11.43 0) (radius 1.27)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "SN74LVC1G14DBV_1_1"
      (pin no_connect line (at 10.16 0 180) (length 5.08) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 17.78 0 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SN74LVC1G14DRL" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SN74LVC1G14DRL" (at 20.32 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-553" (at 0 -12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g14.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Inverter Schmitt Trigger" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Single Schmitt-Trigger Inverter, SOT-553" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?553*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SN74LVC1G14DRL_0_1"
      (polyline
        (pts
          (xy -2.032 1.016)
          (xy -1.016 1.016)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -5.08 7.62)
          (xy -5.08 -7.62)
          (xy 10.16 0)
          (xy -5.08 7.62)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.048 -1.016)
          (xy -3.048 1.016)
          (xy -2.032 1.016)
          (xy -2.032 -1.016)
          (xy -4.064 -1.016)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (circle (center 11.43 0) (radius 1.27)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "SN74LVC1G14DRL_1_1"
      (pin no_connect line (at 10.16 0 180) (length 5.08) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 17.78 0 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
