(footprint "LT8315" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "TSSOP SO")
  (attr smd)
  (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b5d84bc0-4d9a-4d1d-a476-5c6b51309fca)
  )
  (fp_text value "LT8315" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b1240f00-ec43-4c0b-9a41-43264db8a893)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 60960af7-b938-44a8-82b5-e9c36f2e6817)
  )
  (fp_line (start 0 -3.385) (end -3.6 -3.385)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4be2b882-65e4-4552-9482-9d622928de2f))
  (fp_line (start 0 -3.385) (end 2.2 -3.385)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f8e92727-5789-4ef6-9dc3-be888ad72e45))
  (fp_line (start 0 3.385) (end -2.2 3.385)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 27e3c71f-5a63-4710-8adf-b600b805ce02))
  (fp_line (start 0 3.385) (end 2.2 3.385)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp de588ed9-a530-46f0-aa03-e0307ff72286))
  (fp_line (start -3.85 -3.5) (end -3.85 3.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5fba7ff8-02f1-4ac0-93c4-5bd7becbcf63))
  (fp_line (start -3.85 3.5) (end 3.85 3.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3dbc1b14-20e2-4dcb-8347-d33c13d3f0e0))
  (fp_line (start 3.85 -3.5) (end -3.85 -3.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d33c6077-a8ec-48ca-b0e0-97f3539ef54c))
  (fp_line (start 3.85 3.5) (end 3.85 -3.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4b534cd1-c414-4029-9164-e46766faf60e))
  (fp_line (start -2.2 -2.25) (end -1.2 -3.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9c2a29da-c83f-4ec8-bbcf-9d775812af04))
  (fp_line (start -2.2 3.25) (end -2.2 -2.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 19a5aacd-255a-4bf3-89c1-efd2ab61016c))
  (fp_line (start -1.2 -3.25) (end 2.2 -3.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ce3f834f-337d-4957-8d02-e900d7024614))
  (fp_line (start 2.2 -3.25) (end 2.2 3.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8fbab3d0-cb5e-47c7-8764-6fa3c0e4e5f7))
  (fp_line (start 2.2 3.25) (end -2.2 3.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a25ec672-f935-4d0c-ae67-7c3ebe078d85))
  (pad "1" smd roundrect (at -3 -2.925) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3e011a46-81bd-4ecd-b93e-57dffb1143e5))
  (pad "2" smd roundrect (at -3 -2.275) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4198eb99-d244-457e-8768-395280df1a66))
  (pad "3" smd roundrect (at -3 -1.625) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 586ec748-563a-478a-82db-706fb951336a))
  (pad "8" smd roundrect (at -3 1.625) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4b042b6c-c042-4cf1-ba6e-bd77c51dbedb))
  (pad "9" smd roundrect (at -3 2.275) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 90f2ca05-313f-4af8-87b1-a8109224a221))
  (pad "10" smd roundrect (at -3 2.925) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 056788ec-4ecf-4826-b996-bd884a6442a0))
  (pad "11" smd roundrect (at 3 2.925) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9e5fe65d-f158-4eb5-af93-2b5d0b9a0d55))
  (pad "12" smd roundrect (at 3 2.275) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a86cc026-cc17-4a81-85bf-4c26f61b9f32))
  (pad "13" smd roundrect (at 3 1.625) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 792ace59-9f73-49b7-92df-01568ab2b00b))
  (pad "14" smd roundrect (at 3 0.975) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 900cb6c8-1d05-4537-a4f0-9a7cc1a2ea1c))
  (pad "15" smd roundrect (at 3 0.325) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b500fd76-a613-4f44-aac4-99213e86ff44))
  (pad "16" smd roundrect (at 3 -0.325) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 278deae2-fb37-4957-b2cb-afac30cacb12))
  (pad "17" smd roundrect (at 3 -0.975) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bc05cdd5-f72f-4c21-b397-0fa889871114))
  (pad "18" smd roundrect (at 3 -1.625) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b4fbe1fb-a9a3-4020-9a82-d3fa1900cd85))
  (pad "19" smd roundrect (at 3 -2.275) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 31070a40-077c-4123-96dd-e39f8a0007ce))
  (pad "20" smd roundrect (at 3 -2.925) (size 1.2 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 70186eba-dcad-4878-bf16-887f6eee49df))
  (pad "21" smd roundrect (at 0.47 0) (size 1.78 5.68) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp cbfa8804-aeca-40e1-9327-c353d8ec0bf0))
  (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
